Product Specifications
SC 258 E3C – 273628000-1C

ELECTRO-HYDRAULIC COMBINATION TOOL
1. The tool is a designed hydraulically activated piston with two equal, opposite blade arms that are symmetrically opened by mechanical joints, thereby spreading, squeezing, pulling or cutting objects.
2. Electro-hydraulic devices do not need to be connected to an external hydraulic source, generation of the required hydraulic pressure takes place within the body of the device by either a quick exchange lithium-ion battery or an external power supply.
3. The electro-hydraulic tool is equipped with light-emitting diodes attached on the operating side to facilitate work under poor lighting conditions. For simplicity, the lights must be powered by the same Lithium-Ion battery that powers the electro-hydraulic tool and not a secondary battery.
4. The cylinder of the tool shall be made of anti-corrosive light aluminum alloy for its lightweight, strength and long life. The body of the tool shall have a high impact, non-metallic housing. The housing shall have ventilation holes on both sides of the unit for cooling the motor. The protective housing shall protect the battery from being damaged and protect the operator’s hand from being pinched between object and the tool.
5. The maximum spreading force shall be up to 157,000 lbf (700 kN). NFPA HSF test point produced 6,500 lbf (29 kN), the LSF test point produced 5,400 lbf (24 kN).
6. The tool shall produce a spreading distance up to 12.6 in (321 mm) measured at the blade tips.
7. The tool shall produce a maximum pulling force of 7,640 lbf (34 kN). NFPA HPF test point produced 8,320 lbf (37 kN), the LPF test point produced 6,300 lbf (28 kN).
8. To maximize the capability of the combination tool the unit should utilize an optional chain and shackle package for pulling operations, use only HURST chain set 541C068.
9. The tool shall produce a pulling distance of 13.1 in (330 mm).
10. The tips are multifunctional tips that can be used for spreading, peeling, squeezing and pulling without the need to be changed.
11. The maximum cutter opening shall be 9.2 in (233 mm).
12. The blades of the tool shall be of a straight serrated edge design for maximum cutting performance. The blades of the tool shall contain shackle holes for pulling applications. The blades of the tool should be attached to the piston rod via removable links, for ease of repair, efficient power transmission and smooth operation. The blades shall be made of heat treated, shock resistant, forged tool steel. The pivot points of the blades shall have rubber booted hand guard for safety purposes.
13. The control mechanism shall feature a star-grip control actuator for ease of operation by allowing 360 º operations in any position. The tool must provide a non-interflow shear seal “dead man” actuator, whereby the unit stops functioning when thumb pressure is released. The star grip automatically returns to the central position, guaranteeing the full load-holding.
14. The tool shall have (2) two handles for ease of operation in any position. One shall be located toward the center of the tool to create an even balance. The second handle shall be located below the control mechanism and be an integral part of the protective housing and allow for easy operation of the Star Control with the thumb of the operator.
15. The tool will be equipped with a dual pilot check valve. This is to prevent accidental movement of the arms in the event of power loss.
16. The tool shall be protected by a pressure relief valve that prevents it from being over pressurized.
17. The tool dimensions without the battery shall not be any longer than 31.2 in. (792 mm), wider than 8.27 in (210 mm) or higher than 9.96 in (253 mm).
18. The maximum operating pressure to the tool will be 10,000 psi (70 MPa).
19. The tool must be compatible with three battery options; either a 5Amp/25.2 V or a 9Amp/25.2V battery capable of freshwater submersion up to 11ft. Tool must also be compatible with a 9Amp/25.2V battery capable of saltwater submersion up to 11ft .
20. The estimated current consumption at nominal voltage is 9A DC at idle mode and 40A DC at maximum load.
21. The tool shall have a noise pressure level of 72 dB(A) at maximum load.
22. The tool shall be able to tolerate an ambient temperature range of -4ºF (-20ºC) up to +131ºF (+55ºC).
23. The tool must be NFPA 1960 2024 Edition certified and shall be labelled as such bearing the mark of the testing agency.
24. Cutting classification should be no less than A6 / B6 / C6 / D7 / E7/ F4 as defined in NFPA 1960;2024 and certified by a 3rd party testing agency.
25. The tool will not weigh more than 31.1 lbs (14.1 kg) excluding the power supply.
26. The tool shall be able to operate submerged in fresh water up to 11ft.
27. The tool shall have an IP rating of IP58 and utilize a battery with an IP rating of IP68.
28. Tool dashboard shall illuminate to notify the user of a higher than normal temperature in the main circuit board and shall discontinue the turbo feature while detected.
29. Tool dashboard shall illuminate an icon on the tools dashboard to indicate that the tool has a saltwater capable battery attached.
30. The tool dashboard shall display an indicator that illuminates when the turbo feature is active.
31. The tool dashboard shall display a pressure indicator that will continually change showing the level of pressure being produced by the tool throughout its operation.
32. The tool dashboard shall display an icon that shows the current battery state of charge for real-time awareness. The indicator lights shall consist of green, yellow, and red indication levels relative to the battery level.
33. Open and Close icons shall illuminate on the tool dashboard when the trigger control valve is actuated in their respective direction.
34. The illumination of the power ring shall change from blue to red when the tool reaches a specified parameter and the tool detects a greater than 10-degree rotation along its linear axis. This shall alert end user.
35. The tool shall be Wi-Fi enabled and compatible with a 2.4GHz network. 
36. The tool shall have a Wi-Fi indicator light and must consist of the following (3) colors, green, yellow, and red.
37. The tool shall connect to secure Wi-Fi networks to transmit tool, battery, and charger data and receive firmware updates.
38. The tool shall have the capability to create its own WLAN network to connect and transmit data.
39. The tool shall be able to collect and transmit the following data: power on time, temperature, total in use time, total runs, last activity start time, last connection, days since last upload, GPS location of last upload, battery relative state of charge (in percentage), battery state of health (in percentage), current battery voltage, battery temperature, battery serial number, battery type, charger serial number, charger type.
40. The tool shall trigger alerts to send to select recipients for any of the following incidents that occur in the field: drop alert, tool roll alert, tool submerged, tool submerged in salt water, tool improperly used in salt water, tool submerged for extended time, tool temperature reached a critical level.
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