{"text_format":"1","workbook":"xlsx","n_sheets":9,"sheets":["FrontPage","Selectable","Fixed","SolidBoreAndStackTips","Shutoffs","Multi-Purpose","BlankPage","DataSource","6-27-22 Adds"],"not_rendered":{"charts":0,"images":8,"macros":1,"external_links":0,"defined_names":547,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"FrontPage","index":0,"n_rows":59,"n_cols":29,"rows_kept":59,"cut":false,"hidden":false,"merged":[[0,4,1,4],[2,4,3,4],[4,4,5,4],[7,1,8,3],[21,2,23,3],[0,3,5,3],[10,1,12,3]]}
[null,null,null,"Reaction Force Color Chart                                                                          (refers only to the Flow and Pressure you've provided below):","This is a Low RF Nozzle (RF < 51 )",null,"<61 or <51",null,null,null,null,"<50","50-65","65-70"]
[null,null,null,null,null,null,null,null,null,null,null,"Green","Green Shading to yellow","Orange to red"]
[null,null,null,null,"This is a Nozzle with Increased RF (RF > 50 and <101 )",null,"51-70 or 61-70",{"$f":"ROUNDDOWN(SQRT(C17/(29.71*SQRT(C18))),2)","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,"5-10-20-40",null,null,null,null,null,null,40,100]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"12-23-34-53",null,null,null,null,null,null,60,100,87,75]
[null,null,null,null,"This Nozzle has a High RF (RF > 100 )",null,">70","Nozzle Line",null,null,null,null,null,null,null,null,null,null,"30-60-95-125-150"]
[null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"FP\",SUBSTITUTE(O22,\" \",\"_\"))","v":"FPA_solid_stream_of_water"},"Single-tip Solid Bore","Stack Tips","Multi-Purpose (both Fog and Solid Bore)","Saber Shutoff",null,null,null,null,null,null,"13-25-40-60"]
[null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"FP\",SUBSTITUTE(O23,\" \",\"_\"))","v":"FPThe_ability_to_change_fog_pattern"},"Selectable Gallonage","Fixed Orifice Fog","Multi-Purpose (both Fog and Solid Bore)",null,null,null,null,null,null,null,"13-25-40-60"]
[null,"This page is intended to guide you toward the correct Nozzle Type and will not provide any Part Number or List Price.  Use the Recommendation (below) to guide you to the correct tab within this spreadsheet to get detailed information.  Inputs on this page will NOT carry over to other tabs.",null,null,"Rev Date: 6/27/2022"]
[null,null,null,null,null,null,null,{"$f":"CONCATENATE(\"FP\",SUBSTITUTE(O24,\" \",\"_\"))","v":"FPMake_Selection_Above"},"Make Selection Above",null,null,null,null,null,null,null,null,null,"18-30",18,30,null,null,null,null,{"$f":"TRIM(LEFT(AA9,3))","v":"30"},"30 gpm @ 50 psi; RF 11"]
[null,null,null,null,null,null,null,null,null,"d=",{"$f":"SQRT(C17/(29.71*SQRT(C18)))","v":{"$error":"#DIV/0!"}},"SQRT([flow]/(29.71*SQRT([pressure])))",null,null,null,null,null,null,"13-23-30",13,23,30,null,null,null,{"$f":"TRIM(LEFT(AA10,3))","v":"53"},"53 gpm @ 50 psi; RF 20"]
[null,"Information regarding recommended Hose Sizes and Reaction Forces are based on general firefighting knowledge.  Actual deployment of product is the responsibility of the end user and subject to the policies and procedures of the department and/or organization deploying the product."]
[]
[]
[]
[null,null,"Make your selection(s) from the dropdown in the green cell(s) below",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18-30",null,null,null,null,null,null,"82","82 gpm @ 50 psi; RF 31"]
[null,"What are you looking for?",null,{"$f":"IF(C16=\"\",\"\",IF(C19=\"\",\"\",IFERROR(IF(H16<51,J56,IF(H16<101,J57,IF(H16>100,J58,\"\"))),\"\")))","v":""},null,null,null,{"$f":"IF(C19=O23,ROUND(0.0505*C17*SQRT(C18),0),ROUND(1.57*(SQRT(C17/(29.71*SQRT(C18)))*SQRT(C17/(29.71*SQRT(C18))))*C18,0))","v":{"$error":"#DIV/0!"}},null,null,"ROUND(1.57*(ER2*ER2)*ET$1,0)",null,null,null,null,null,null,null,"13-23-30",null,null,null,null,null,null,"118","118 gpm @ 50 psi; RF 44"]
[null,"Max Flow Needed",null,{"$f":"IF(C17=\"\",\"\",IF(C17<95,K49,IF(C17<151,K50,IF(C17<251,K51,IF(C17>250,K52,\"\")))))","v":""},null,null,null,null,null,null,null,null,null,null,null,"Solid B",null,null,"30-60-95-125",30,60,95,125,null,null,"161","161 gpm @ 50 psi; RF 60"]
[null,"Nozzle Inlet Pressure (Not all Flows are available in all Pressures)",null,{"$f":"IFERROR(CONCATENATE(IF(C18=50,\"Low Pressure Hose strongly recommended; \",\"\"),VLOOKUP(C19,O22:Q23,3,FALSE),IF(C19=O23,ROUND(0.0505*C17*SQRT(C18),0),ROUND(1.57*(SQRT(C17/(29.71*SQRT(C18)))*SQRT(C17/(29.71*SQRT(C18))))*C18,0))),\"\")","v":""},{"$f":"IF(C18=\"\",\"\",IF(C19=O23,\"\",IF(C19=O22,IFERROR(CONCATENATE(VLOOKUP(ROUNDDOWN(SQRT(C17/(29.71*SQRT(C18))),2),I20:M31,5,FALSE),\" Bore Size\"),\"Exact Bore Size Not Available; see options for the closest equivalent\"),\"\")))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,"30-60-95-125",null,null,null,null,null,null,"185","185 gpm @ 50 psi; RF 69"]
[null,"Nozzle Function",null,{"$f":"IFERROR(VLOOKUP(C19,O:P,2,FALSE),\"\")","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"95-125-150-200",95,125,150,200,null,null,"210","210 gpm @ 50 psi; RF 79"]
[null,"Nozzle Type",null,{"$f":"IFERROR(HLOOKUP(C20,H36:N37,2,FALSE),\"\")","v":""},null,null,null,null,{"$f":"ROUNDDOWN(K20,2)","v":0.37},{"$f":"VALUE(TRIM(LEFT(L20,3)))","v":30},0.375,"30 gpm @ 50 psi; RF 11","3/8\"",null,null,null,null,null,"125-150-200-250",125,150,200,250,null,null,"237","237 gpm @ 50 psi; RF 89"]
[null,null,null,null,null,null,null,null,{"$f":"ROUNDDOWN(K21,2)","v":0.5},{"$f":"VALUE(TRIM(LEFT(L21,3)))","v":53},0.5,"53 gpm @ 50 psi; RF 20","1/2\"",null,null,null,null,null,"95-125-150-200",null,null,null,null,null,null,"266","266 gpm @ 50 psi; RF 99"]
[null,"Recommendation:  ",{"$f":"IF(C16=\"\",\"\",IFERROR(IF(C16=$J$43,K38,HLOOKUP(C20,H36:M38,3,FALSE)),\"\"))","v":""},null,null,null,null,null,0.62,82,0.625,"82 gpm @ 50 psi; RF 31","5/8\"",null,"A solid stream of water","Includes Solid Bore and Stack Tips","Solid Bore Reaction Force =  ",null,"125-150-200-250",null,null,null,null,null,null,"296","296 gpm @ 50 psi; RF 111"]
[null,null,null,null,null,null,null,null,0.74,118,0.75,"118 gpm @ 50 psi; RF 44","3/4\"",null,"The ability to change fog pattern","TurboJet, Assault, ProVenger, SaberJet, UltraJet","Fog Reaction Force =  ",null,"30-95-125-150-200",null,null,null,null,null,null,"328","328 gpm @ 50 psi; RF 123"]
[null,null,null,null,null,null,null,null,0.87,161,0.875,"161 gpm @ 50 psi; RF 60","7/8\"",null,"Make Selection Above",null,"Make Selection Above",null,"30-95-125-150-200",null,null,null,null,null,null,"397","397 gpm @ 50 psi; RF 148"]
[null,null,null,null,null,null,null,null,0.93,185,0.9375,"185 gpm @ 50 psi; RF 69","15/16\""]
[null,null,null,null,null,null,null,null,0.99,210,1,"210 gpm @ 50 psi; RF 79","1\""]
[null,null,null,null,null,null,null,null,1.06,237,1.0625,"237 gpm @ 50 psi; RF 89","1-1/16\"",null,null,null,null,null,"_",{"$f":"CONCATENATE(\"FP\",S27)","v":"FP_"}]
[null,null,null,null,null,null,null,null,1.1200000000000001,266,1.125,"266 gpm @ 50 psi; RF 99","1-1/8\"",null,null,null,null,null,5,{"$f":"CONCATENATE(\"FP\",S28)","v":"FP5"},100,87,75]
[null,null,null,null,null,null,null,null,1.18,296,1.1875,"296 gpm @ 50 psi; RF 111","1-3/16\"",null,null,null,null,null,10,{"$f":"CONCATENATE(\"FP\",S29)","v":"FP10"},100,87,75]
[null,null,null,null,null,null,null,null,1.24,328,1.25,"328 gpm @ 50 psi; RF 123","1-1/4\"",null,null,null,null,null,12,"FP12",87]
[null,null,null,null,null,null,null,null,1.37,397,1.375,"397 gpm @ 50 psi; RF 148","1-3/8\"",null,null,null,null,null,13,"FP13",100,87]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,20,"FP20",100,87,75]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,23,"FP23",87]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,25,"FP25",100,87]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,30,"FP30",100,75,50]
[null,null,null,null,null,null,null,"Single-tip Solid Bore","Stack Tips","Multi-Purpose (both Fog and Solid Bore)","Saber Shutoff","Selectable Gallonage","Fixed Orifice Fog","Multi-Purpose (both Fog and Solid Bore)",null,null,null,null,34,"FP34",87,50]
[null,null,null,null,null,null,null,"Styles 416, 1417, 1499, 489, 1445, 1446","Styles 439, 1420, 1441, 1443","UltraJet or SaberJet","Style 2431 or 2433","TurboJet or ProVenger","Assault or ProVenger",null,null,null,null,null,40,"FP40",100,87,75,null,null,"296"]
[null,null,null,null,null,null,null,"Go to the blue-colored tab entitled \"SolidBoreAndStackTips\" to explore the full range of options and obtain the Akron Brass part number for the solid bore tip you configure","Go to the blue-colored tab entitled \"SolidBoreAndStackTips\" to explore the full range of options and obtain the Akron Brass part number for the stack tips you configure","Go to the purple-colored tab entitled \"Multi-Purpose\" to explore the full range of options and obtain the Akron Brass part number for the nozzle or tip you configure","Go to the green-colored tab entitled \"Shutoffs\" to explore the full range of options and obtain the Akron Brass part number for the shutoff you configure","Go to the red-colored tab entitled \"Selectable\" to explore the full range of options and obtain the Akron Brass part number for the fog nozzle or fog tip you configure","Go to the yellow-colored tab entitled \"Fixed\" to explore the full range of options and obtain the Akron Brass part number for the fog nozzle or fog tip you configure",null,null,null,null,null,53,"FP53",87,50,null,null,null,"328"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,60,"FP60",100,87,75,null,null,"397"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,82,"FP82",50]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,95,"FP95",100,87,75]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,118,"FP118",50]
[null,null,null,null,null,null,null,null,null,"Just a Shutoff",null,null,null,null,null,null,null,null,125,"FP125",100,87,75,50]
[null,null,null,null,null,null,null,null,null,"Fog Nozzle or Solid Bore Tip",null,null,null,null,null,null,null,null,150,"FP150",100,87,75,50]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,161,"FP161",50]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,175,"FP175",100,75,50]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,185,"FP185",50]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,200,"FP200",100,75]
[null,null,null,null,null,null,null,null,null,"<95","1\" or 1.5\" line recommended",null,null,null,null,null,null,null,210,"FP210",50]
[null,null,null,null,null,null,null,null,null,"30-150","1.5\" line recommended, 1.75\" acceptable",null,null,null,null,null,null,null,225,"FP225",100]
[null,null,null,null,null,null,null,null,null,"95-250","1.75\" or larger line recommended",null,null,null,null,null,null,null,237,"FP237",50]
[null,null,null,null,null,null,null,null,null,"200+","Larger than 1.75\" line recommended",null,null,null,null,null,null,null,250,"FP250",100,75,50]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,265,"FP265",50]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,266,"FP266",50]
[null,null,null,null,null,null,null,null,null,"Reaction Force Color Codes",null,null,null,null,null,null,null,null,296,"FP296",50]
[null,null,null,null,null,null,null,null,null,{"$f":"E1","v":"This is a Low RF Nozzle (RF < 51 )"},null,null,null,null,null,null,null,null,300,"FP300",100,75]
[null,null,null,null,null,null,null,null,null,{"$f":"E3","v":"This is a Nozzle with Increased RF (RF > 50 and <101 )"},null,null,null,null,null,null,null,null,328,"FP328",50]
[null,null,null,null,null,null,null,null,null,{"$f":"E5","v":"This Nozzle has a High RF (RF > 100 )"},null,null,null,null,null,null,null,null,350,"FP350",100]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,397,"FP397",50]

{"sheet":"Selectable","index":1,"n_rows":51,"n_cols":51,"rows_kept":51,"cut":false,"hidden":false,"merged":[[7,1,8,1],[7,2,8,2],[7,10,8,10],[7,9,8,9],[7,8,8,8],[7,7,8,7],[7,6,8,6],[7,5,8,5],[7,4,8,4],[7,3,8,3],[13,7,14,7],[12,2,12,6],[13,8,14,10],[13,2,14,6],[10,6,10,7],[11,3,11,4],[6,3,6,7],[15,2,17,10],[0,7,5,7],[0,8,1,10],[1,1,1,5],[2,1,2,5],[2,8,3,10],[3,1,3,5],[4,1,4,5],[4,8,5,10],[5,1,5,5],[13,1,14,1],[10,2,10,3],[11,5,11,6],[11,7,12,9],[11,10,12,10]]}
[null,"Instructions:",null,null,null,null,null,"Reaction Force Color Chart (refers to highest available Flow @ Rated Pressure):","This is a Low RF Nozzle (RF < 51 )",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"asdf",13,25,40,60,95,125,150,161,175,185,200,210,225,250,265,300,350]
[null,"Tan-colored cells are headers or describe the selection options",null,null,null,null,null,null,null,null,null,null,"Nozzle",null,"Fog Nozzle","Fog Tip",null,"5-40","125-250","13-30","13-60","18-30","30-125","30-150","30-200","95-200","12-53",null,null,null,null,null,null,null,"100 (Std)","100 (Std)","100 (Std)","100 (Std)","100 (Std)","100 (Std)","100 (Std)",50,"100 (Std)",50,"100 (Std)",50,"100 (Std)","100 (Std)",50,"100 (Std)","100 (Std)"]
[null,"Use the green-colored cells to make your selections (All cells must be filled in; information from \"FrontPage\" tab does not carry over to this page)",null,null,null,null,null,null,"This is a Nozzle with Increased RF (RF > 50 and <101 )",null,null,null,"Tip",null,"1 in","1.5 in",null,"100 (Std)","100 (Std)","100 (Std)","100 (Std)","100 (Std)","100 (Std)","100 (Std)","100 (Std)","100 (Std)","87 (CE)",null,null,null,null,null,null,null,null,null,null,75,75,75,75,null,75,null,75,null,null,75,null,75]
[null,"Blue-colored cells provide outputs based on your selections",null,null,null,null,null,null,null,null,null,null,"High Pressure",null,"1.5 in",null,null,75,75,null,null,null,75,75,75,75,null,null,null,null,null,null,null,null,null,null,null,"87 (CE)","87 (CE)",50,50,null,50,null,50,null,null,50]
[null,"This shaded cell indicates an error has ocurred and you may need to modify some of your selections or contact our Customer Care team",null,null,null,null,null,null,"This Nozzle has a High RF (RF > 100 )",null,null,null,null,null,"2 in",null,null,"87 (CE)",null,null,null,null,"87 (CE)","87 (CE)",null,null,null,null,null,"5-40","100 (Std)",{"$f":"CONCATENATE(AD5,\" \",AE5)","v":"5-40 100 (Std)"},null,null,null,null,null,null,null,"87 (CE)","87 (CE)"]
[null,"Orange-colored cell allows you to input your discount for Net Price",null,null,null,null,null,null,null,null,null,null,null,null,"2.5 in",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5-40",75,{"$f":"CONCATENATE(AD6,\" \",AE6)","v":"5-40 75"}]
[null,{"$f":"FrontPage!E8","v":"Rev Date: 6/27/2022"},null,"Selectable Gallonage Fog Nozzles",null,null,null,null,null,null,null,null,null,null,"3 in",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5-40","87 (CE)","5-40 87 (CE)"]
[null,"Nozzle or Tip","Inlet Size","Flow Range","Pressure Rating","Inlet Thread","Bumper Color",{"$f":"IF(OR(B10=\"FOG TIP\",J10=\"yes\"),\"\",\"Remove Pistol Grip?\")","v":"Remove Pistol Grip?"},"Style Number",{"$f":"IF(B10=\"FOG TIP\",\"\",\"ZT Inlet?\")","v":"ZT Inlet?"},"Custom Etch",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"125-250","100 (Std)","125-250 100 (Std)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"125-250",75,"125-250 75"]
[null,"Fog Nozzle","1.5 in","30-125",75,"NH","BLACK (Std)","No (Std)",{"$f":"IFERROR(VLOOKUP(CONCATENATE(B10,\" \",D10),Q33:R49,2,FALSE),\"Not Available\")","v":"1720"},"No (Std)","No (Std)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"13-30","100 (Std)","13-30 100 (Std)"]
[null,"List price",{"$f":"SUM(E11:J11)","v":1198},null,null,{"$f":"IF(OR(F10=\"Storz\",F10=\"BIM\"),_xlfn.XLOOKUP(\"Storz\",R:R,S:S),0)","v":0},{"$f":"IFERROR(VLOOKUP(CONCATENATE(I10,D10),AD33:AH49,K11,FALSE),\"\")","v":"RF = 13-26-42-55"},null,{"$f":"IFERROR(VLOOKUP(TRIM(I10),R33:S49,2,FALSE),\"\")","v":1198},{"$f":"IF(J8=\"\",0,IF(J10=\"Yes\",_xlfn.XLOOKUP(\"zt\",R:R,S:S),0))","v":0},{"$f":"IF(TRIM(LEFT(E10,3))=\"100\",3,IF(TRIM(LEFT(E10,3))=\"87\",4,IF(TRIM(LEFT(E10,3))=\"75\",5,0)))","v":5},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"13-60","100 (Std)","13-60 100 (Std)",null,null,null,"bmpr4116","BLACK (Std)"]
[null,"Your Discount",0.3,"Net Price",null,{"$f":"ROUND(C11*(1-C12),2)","v":838.6},null,{"$f":"IF(B10=\"fog tip\",\"\",\"Include Color Clips for Shutoff and/or Pistol Grip? (no upcharge)\")","v":"Include Color Clips for Shutoff and/or Pistol Grip? (no upcharge)"},null,null,"Yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18-30","100 (Std)","18-30 100 (Std)",null,null,null,"bmpr4802","BLACK (Std)","ORANGE","YELLOW","RED","BLUE","GREEN"]
[null,"Short Description",{"$f":"IF(B22=\"Error\",\"Fix Errors\",CONCATENATE(I10,\" \",C10,\" \",F10,\" \",D10,\" \",E10,\" \",G10,IF(B10=\"Fog Tip\",\"\",IF(J10=\"yes\",\" PG\",IF(H10=\"yes\",\" NPG\",\" PG\"))),IF(B10=\"Fog Tip\",\"\",IF(J10=\"Yes\",\" ZT\",\"\")),IF(K10=\"Yes\",\" ETCH\",\"\")))","v":"1720 1.5 in NH 30-125 75 BLACK (Std) PG"},null,null,null,null,null,null,null,null,null,"1 IN","NH",null,null,null,"1 in","1.5 in","2 in","2.5 in","3 in",null,null,null,null,null,null,null,"30-125","100 (Std)","30-125 100 (Std)",null,null,null,"bmpr4824","BLACK (Std)","ORANGE","YELLOW","RED","BLUE","GREEN"]
[null,"Long Description",{"$f":"IF(B22=\"Error\",\"Some of your selections are not compatible with others; please correct the errors highlighted in RED\",CONCATENATE(\"Style \",I10,\" \",B10,\" with \",C10,\" \",F10,\" inlet; \",VLOOKUP(CONCATENATE(I10,D10),W33:X49,2,FALSE),\" gpm @ \",E10,\" psi (\",G11,\"); \",PROPER(G10),\" bumper\",IF(B10=\"Fog Tip\",\"\",IF(J10=\"yes\",\"\",IF(H10=\"yes\",\"; NO PISTOL GRIP\",\"; pistol grip\"))),IF(B10=\"Fog Tip\",\"\",IF(J10=\"Yes\",\"; Zero-Torque Grip\",\"\")),IF(K10=\"Yes\",\"; Custom Etched\",\"\")))","v":"Style 1720 Fog Nozzle with 1.5 in NH inlet; 30-60-95-125 gpm @ 75 psi (RF = 13-26-42-55); Black (Std) bumper; pistol grip"},null,null,null,null,"Akron Brass Part Number and Description",{"$f":"IF(AND(OR(E10=\"custom\",F10=\"custom\"),K10=\"yes\"),\"Contact Customer Care to request Custom Thread and Etch (800-228-1161)\",IF(F10=\"custom\",\"Contact Customer Care to request Custom Thread (800-228-1161)\",IF(K10=\"Yes\",\"Contact Customer Care to request Custom Etch (800-228-1161)\",IF(B22=\"Error\",\"Incompatible selections; please correct errors highlighted in RED\",IFERROR(CONCATENATE(VLOOKUP(C13,DataSource!AH:AJ,2,FALSE),\"      \",VLOOKUP(C13,DataSource!AH:AJ,3,FALSE)),\"Version you've requested not yet created; contact Customer Care (800-228-1161)\")))))","v":"17204011      TBJT 1.5NH 30-125G@75P"},null,null,null,"1 IN","NPSH",null,null,"30-125","5-40","13-30","5-40","30-125","30-125",null,null,null,null,null,null,null,"30-125",75,"30-125 75",null,null,null,"bmpr4826","BLACK (Std)","ORANGE","YELLOW","RED","BLUE","GREEN"]
[null,null,null,null,null,null,null,null,null,null,null,null,"1 IN","STORZ",null,null,"30-150","13-30","13-60","13-30","30-150","30-150",null,null,null,null,null,null,null,"30-125","87 (CE)","30-125 87 (CE)",null,null,null,"bmpr4863","BLACK (Std)","ORANGE","YELLOW","RED","BLUE","GREEN"]
[null,"Notes: ","You can make any notes about what you want, or anything else, in this space",null,null,null,null,null,null,null,null,null,"1.5 in",null,null,null,"30-200","18-30","30-125","18-30","30-200","30-200",null,null,null,null,null,null,null,"30-150","100 (Std)","30-150 100 (Std)",null,null,null,"bmpr4866","BLACK (Std)","ORANGE","YELLOW","RED","BLUE","GREEN"]
[null,null,null,null,null,null,null,null,null,null,null,null,"1.5 in",null,null,null,"95-200","13-60","30-150","13-60","95-200","95-200",null,null,null,null,null,null,null,"30-150",75,"30-150 75"]
[null,null,null,null,null,null,null,null,null,null,null,null,"1.5 in",null,null,null,"125-250","12-53","30-200","30-125","125-250","125-250",null,null,null,null,null,null,null,"30-150","87 (CE)","30-150 87 (CE)"]
[null,null,null,null,null,null,null,null,null,null,null,null,"1.5 IN",null,null,null,null,null,"95-200","30-200",null,null,null,null,null,null,null,null,null,"30-200","100 (Std)","30-200 100 (Std)"]
[null,null,null,{"$f":"CONCATENATE(\"_\",SUBSTITUTE(C10,\" \",\"_\"),\"_\",SUBSTITUTE(D10,\"-\",\"_\"))","v":"_1.5_in_30_125"},null,null,null,{"$f":"VLOOKUP(C13,DataSource!AH:AJ,2,FALSE)","v":"17204011"},{"$f":"VLOOKUP(C13,DataSource!AH:AJ,3,FALSE)","v":"TBJT 1.5NH 30-125G@75P"},null,null,null,"1.5 in",null,null,null,null,null,"125-250","30-150",null,null,null,null,null,null,null,null,null,"30-200",75,"30-200 75"]
[null,null,null,{"$f":"CONCATENATE(C10,\" \",D10)","v":"1.5 in 30-125"},null,null,null,null,{"$f":"CONCATENATE(SUBSTITUTE(B10,\" \",\"_\"),\"_\",SUBSTITUTE(D10,\"-\",\"_\"))","v":"Fog_Nozzle_30_125"},null,null,null,"1.5 IN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"95-200","100 (Std)","95-200 100 (Std)",null,null,null,"Style"]
[null,{"$f":"IF(OR(C22=\"False\",D22=\"False\",E22=\"False\",H22=\"False\",J22=\"False\",F22=\"False\"),\"Error\",\"Okay\")","v":"Okay"},{"$f":"IFERROR(VLOOKUP(CONCATENATE(B10,\" \",C10),C27:C43,1,FALSE),\"False\")","v":"Fog Nozzle 1.5 in"},{"$f":"IFERROR(VLOOKUP(CONCATENATE(B10,\" \",D10),D27:D43,1,FALSE),\"False\")","v":"Fog Nozzle 30-125"},{"$f":"IFERROR(VLOOKUP(CONCATENATE(D10,\" \",E10),E27:E45,1,FALSE),\"False\")","v":"30-125 75"},{"$f":"IF(OR(C10=\"2 in\",C10=\"3 in\"),IF(F10=\"storz\",\"Okay\",\"False\"),\"Okay\")","v":"Okay"},null,{"$f":"IF($B10=\"Fog Tip\",IF(H10=\"yes\",\"False\",\"Okay\"),\"Okay\")","v":"Okay"},{"$f":"IF(OR(I10=Fog_Nozzle_30_150,I10=Fog_Tip_30_125,I10=Fog_Nozzle_30_125,I10=Fog_Nozzle_95_200,I10=Fog_Nozzle_125_250,I10=Fog_Tip_95_200,I10=Fog_Tip_95_200,I10=Fog_Tip_125_250,I10=Fog_Nozzle_30_200,I10=Fog_Tip_30_200,I10=Fog_Tip_13_60,I10=Fog_Tip_18_30,I10=Fog_Tip_13_30),IF(C10=\"1 in\",\"False\",\"Okay\"),\"Okay\")","v":"Okay"},{"$f":"IF($B10=\"Fog Tip\",IF(J10=\"yes\",\"False\",\"Okay\"),\"Okay\")","v":"Okay"},null,null,"2 IN","STORZ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"95-200",75,"95-200 75",null,null,null,"bmpr1602","BLACK (Std)"]
[null,null,null,null,null,null,null,null,null,null,null,null,"2.5 IN","NH",null,null,"BLACK (Std)","THREAD1 IN","NH","NPSH","Storz","Custom",null,null,null,null,null,null,null,"12-53","87 (CE)","12-53 87 (CE)",null,null,null,"bmpr1616","BLACK (Std)"]
[null,null,null,null,null,null,null,null,null,null,null,null,"2.5 IN","NPSH",null,null,"ORANGE","THREAD1.5 in","NH","NPSH","FDNY","NYCORP","PCT","Storz","Custom",null,null,null,null,null,null,null,null,null,null,"bmpr1702","BLACK (Std)","ORANGE","YELLOW","RED","BLUE","GREEN"]
[null,null,null,"2.5 in 30-125",null,null,null,null,null,null,null,null,"2.5 IN","FDNY",null,null,"YELLOW","THREAD2 IN","Storz",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"bmpr1703","BLACK (Std)","ORANGE","YELLOW","RED","BLUE","GREEN"]
[null,null,null,null,null,null,null,null,null,null,null,null,"2.5 IN","NYCORP",null,null,"RED","THREAD2.5 IN","NH","NPSH","FDNY","NYCORP","PITT6","BAT","CSA","QST","BIM","Storz","Custom",null,null,null,null,null,null,"bmpr1704","BLACK (Std)","ORANGE","YELLOW","RED","BLUE","GREEN"]
[null,null,{"$f":"CONCATENATE(O$2,\" \",O3)","v":"Fog Nozzle 1 in"},"Fog Nozzle 5-40","5-40 100 (Std)",null,null,null,null,null,null,null,"2.5 IN","PITT6",null,null,"BLUE","THREAD3 IN","Storz",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"bmpr1711","BLACK (Std)","ORANGE","YELLOW","RED","BLUE","GREEN"]
[null,null,{"$f":"CONCATENATE(O$2,\" \",O4)","v":"Fog Nozzle 1.5 in"},"Fog Nozzle 12-53","5-40 75",null,null,null,null,null,null,null,"2.5 IN","BAT",null,null,"GREEN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"bmpr1714","BLACK (Std)","ORANGE","YELLOW","RED","BLUE","GREEN"]
[null,null,{"$f":"CONCATENATE(O$2,\" \",O5)","v":"Fog Nozzle 2 in"},"Fog Nozzle 30-150","5-40 87 (CE)",null,null,null,null,null,null,null,"2.5 IN","CSA",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"bmpr1720","BLACK (Std)","ORANGE","YELLOW","RED","BLUE","GREEN"]
[null,null,{"$f":"CONCATENATE(O$2,\" \",O6)","v":"Fog Nozzle 2.5 in"},"Fog Nozzle 13-60","125-250 100 (Std)",null,null,null,null,null,null,null,"2.5 IN","QST",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"bmpr1723","BLACK (Std)","ORANGE","YELLOW","RED","BLUE","GREEN"]
[null,null,{"$f":"CONCATENATE(O$2,\" \",O7)","v":"Fog Nozzle 3 in"},"Fog Tip 13-60","125-250 75",null,null,null,null,null,null,null,"2.5 IN","BIM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"bmpr1733","BLACK (Std)","ORANGE","YELLOW","RED","BLUE","GREEN"]
[null,null,{"$f":"CONCATENATE(P$2,\" \",P3)","v":"Fog Tip 1.5 in"},"Fog Nozzle 18-30","13-30 100 (Std)",null,null,null,null,null,null,null,"2.5 IN","STORZ",null,null,null,"Style",null,null,{"$f":"IF(B10=\"fog tip\",\"N/A\",\"No (Std)\")","v":"No (Std)"},null,null,null,null,null,null,null,null,null,null,100,87,75,null,"bmpr1737","BLACK (Std)","ORANGE","YELLOW","RED","BLUE","GREEN"]
[null,null,{"$f":"CONCATENATE(P$2,\" \",P4)","v":"Fog Tip "},"Fog Nozzle 13-30","13-60 100 (Std)",null,null,null,null,null,null,null,"3 IN","STORZ",null,null,"Fog Nozzle 5-40","1602",672,null,{"$f":"IF(B10=\"fog tip\",\"\",\"Yes\")","v":"Yes"},4,{"$f":"CONCATENATE(R33,RIGHT(Q33,V33))","v":"16025-40"},"5-10-20-40",5,10,20,40,null,"16025-40","5-10-20-40",{"$f":"CONCATENATE(\"RF = \",ROUND(0.0505*VALUE($Y33)*SQRT(VALUE(TRIM(LEFT(AF$32,3)))),0),\"-\",ROUND(0.0505*VALUE($Z33)*SQRT(VALUE(TRIM(LEFT(AF$32,3)))),0),\"-\",ROUND(0.0505*VALUE($AA33)*SQRT(VALUE(TRIM(LEFT(AF$32,3)))),0),\"-\",ROUND(0.0505*VALUE($AB33)*SQRT(VALUE(TRIM(LEFT(AF$32,3)))),0))","v":"RF = 3-5-10-20"},{"$f":"CONCATENATE(\"RF = \",ROUND(0.0505*VALUE($Y33)*SQRT(VALUE(TRIM(LEFT(AG$32,3)))),0),\"-\",ROUND(0.0505*VALUE($Z33)*SQRT(VALUE(TRIM(LEFT(AG$32,3)))),0),\"-\",ROUND(0.0505*VALUE($AA33)*SQRT(VALUE(TRIM(LEFT(AG$32,3)))),0),\"-\",ROUND(0.0505*VALUE($AB33)*SQRT(VALUE(TRIM(LEFT(AG$32,3)))),0))","v":"RF = 2-5-9-19"},{"$f":"CONCATENATE(\"RF = \",ROUND(0.0505*VALUE($Y33)*SQRT(VALUE(TRIM(LEFT(AH$32,3)))),0),\"-\",ROUND(0.0505*VALUE($Z33)*SQRT(VALUE(TRIM(LEFT(AH$32,3)))),0),\"-\",ROUND(0.0505*VALUE($AA33)*SQRT(VALUE(TRIM(LEFT(AH$32,3)))),0),\"-\",ROUND(0.0505*VALUE($AB33)*SQRT(VALUE(TRIM(LEFT(AH$32,3)))),0))","v":"RF = 2-4-9-17"},null,"bmpr1744","BLACK (Std)","ORANGE","YELLOW","RED","BLUE","GREEN"]
[null,null,null,"Fog Tip 18-30","18-30 100 (Std)",null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle 12-53","1602",null,null,null,5,{"$f":"CONCATENATE(R34,RIGHT(Q34,V34))","v":"160212-53"},"12-23-34-53",12,23,34,53,null,"160212-53","12-23-34-53",{"$f":"CONCATENATE(\"RF = \",ROUND(0.0505*VALUE($Y34)*SQRT(VALUE(TRIM(LEFT(AF$32,3)))),0),\"-\",ROUND(0.0505*VALUE($Z34)*SQRT(VALUE(TRIM(LEFT(AF$32,3)))),0),\"-\",ROUND(0.0505*VALUE($AA34)*SQRT(VALUE(TRIM(LEFT(AF$32,3)))),0),\"-\",ROUND(0.0505*VALUE($AB34)*SQRT(VALUE(TRIM(LEFT(AF$32,3)))),0))","v":"RF = 6-12-17-27"},"RF = 6-11-16-25","RF = 5-10-15-23",null,"bmpr1763","BLACK (Std)","ORANGE","YELLOW","RED","BLUE","GREEN"]
[null,null,null,"Fog Tip 13-30","30-125 100 (Std)",null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle 30-150","1616",922,null,null,6,"161630-150","30-60-95-125-150",30,60,95,125,150,"161630-150","30-60-95-125-150",{"$f":"CONCATENATE(\"RF = \",ROUND(0.0505*VALUE($Y35)*SQRT(VALUE(TRIM(LEFT(AF$32,3)))),0),\"-\",ROUND(0.0505*VALUE($Z35)*SQRT(VALUE(TRIM(LEFT(AF$32,3)))),0),\"-\",ROUND(0.0505*VALUE($AA35)*SQRT(VALUE(TRIM(LEFT(AF$32,3)))),0),\"-\",ROUND(0.0505*VALUE($AB35)*SQRT(VALUE(TRIM(LEFT(AF$32,3)))),0),\"-\",ROUND(0.0505*VALUE($AC35)*SQRT(VALUE(TRIM(LEFT(AF$32,3)))),0))","v":"RF = 15-30-48-63-76"},{"$f":"CONCATENATE(\"RF = \",ROUND(0.0505*VALUE($Y35)*SQRT(VALUE(TRIM(LEFT(AG$32,3)))),0),\"-\",ROUND(0.0505*VALUE($Z35)*SQRT(VALUE(TRIM(LEFT(AG$32,3)))),0),\"-\",ROUND(0.0505*VALUE($AA35)*SQRT(VALUE(TRIM(LEFT(AG$32,3)))),0),\"-\",ROUND(0.0505*VALUE($AB35)*SQRT(VALUE(TRIM(LEFT(AG$32,3)))),0),\"-\",ROUND(0.0505*VALUE($AC35)*SQRT(VALUE(TRIM(LEFT(AG$32,3)))),0))","v":"RF = 14-28-45-59-71"},{"$f":"CONCATENATE(\"RF = \",ROUND(0.0505*VALUE($Y35)*SQRT(VALUE(TRIM(LEFT(AH$32,3)))),0),\"-\",ROUND(0.0505*VALUE($Z35)*SQRT(VALUE(TRIM(LEFT(AH$32,3)))),0),\"-\",ROUND(0.0505*VALUE($AA35)*SQRT(VALUE(TRIM(LEFT(AH$32,3)))),0),\"-\",ROUND(0.0505*VALUE($AB35)*SQRT(VALUE(TRIM(LEFT(AH$32,3)))),0),\"-\",ROUND(0.0505*VALUE($AC35)*SQRT(VALUE(TRIM(LEFT(AH$32,3)))),0))","v":"RF = 13-26-42-55-66"},null,"bmpr1766","BLACK (Std)","ORANGE","YELLOW","RED","BLUE","GREEN"]
[null,null,null,"Fog Tip 30-125","30-125 75",null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle 13-60","1702",1160,null,null,5,"170213-60","13-25-40-60",13,25,40,60,null,"170213-60","13-25-40-60","RF = 7-13-20-30","RF = 6-12-19-28","RF = 6-11-17-26"]
[null,null,null,"Fog Nozzle 30-125","30-125 87 (CE)",null,null,null,null,null,null,null,null,null,null,null,"Fog Tip 13-60","1703",752,null,null,5,"170313-60","13-25-40-60",13,25,40,60,null,"170313-60","13-25-40-60","RF = 7-13-20-30","RF = 6-12-19-28","RF = 6-11-17-26"]
[null,null,null,"Fog Nozzle 95-200","30-150 100 (Std)",null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle 18-30","1704",1206,null,null,5,"170418-30","18-30",18,30,null,null,null,"170418-30","18-30",{"$f":"CONCATENATE(\"RF = \",ROUND(0.0505*VALUE($Y38)*SQRT(VALUE(TRIM(LEFT(AF$32,3)))),0),\"-\",ROUND(0.0505*VALUE($Z38)*SQRT(VALUE(TRIM(LEFT(AF$32,3)))),0))","v":"RF = 9-15"},{"$f":"CONCATENATE(\"RF = \",ROUND(0.0505*VALUE($Y38)*SQRT(VALUE(TRIM(LEFT(AG$32,3)))),0),\"-\",ROUND(0.0505*VALUE($Z38)*SQRT(VALUE(TRIM(LEFT(AG$32,3)))),0))","v":"RF = 8-14"},{"$f":"CONCATENATE(\"RF = \",ROUND(0.0505*VALUE($Y38)*SQRT(VALUE(TRIM(LEFT(AH$32,3)))),0),\"-\",ROUND(0.0505*VALUE($Z38)*SQRT(VALUE(TRIM(LEFT(AH$32,3)))),0))","v":"RF = 8-13"}]
[null,null,null,"Fog Nozzle 125-250","30-150 75",null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle 13-30","1704",null,null,null,5,"170413-30","13-23-30",13,23,30,null,null,"170413-30","13-23-30",{"$f":"CONCATENATE(\"RF = \",ROUND(0.0505*VALUE($Y39)*SQRT(VALUE(TRIM(LEFT(AF$32,3)))),0),\"-\",ROUND(0.0505*VALUE($Z39)*SQRT(VALUE(TRIM(LEFT(AF$32,3)))),0),\"-\",ROUND(0.0505*VALUE($AA39)*SQRT(VALUE(TRIM(LEFT(AF$32,3)))),0))","v":"RF = 7-12-15"},{"$f":"CONCATENATE(\"RF = \",ROUND(0.0505*VALUE($Y39)*SQRT(VALUE(TRIM(LEFT(AG$32,3)))),0),\"-\",ROUND(0.0505*VALUE($Z39)*SQRT(VALUE(TRIM(LEFT(AG$32,3)))),0),\"-\",ROUND(0.0505*VALUE($AA39)*SQRT(VALUE(TRIM(LEFT(AG$32,3)))),0))","v":"RF = 6-11-14"},{"$f":"CONCATENATE(\"RF = \",ROUND(0.0505*VALUE($Y39)*SQRT(VALUE(TRIM(LEFT(AH$32,3)))),0),\"-\",ROUND(0.0505*VALUE($Z39)*SQRT(VALUE(TRIM(LEFT(AH$32,3)))),0),\"-\",ROUND(0.0505*VALUE($AA39)*SQRT(VALUE(TRIM(LEFT(AH$32,3)))),0))","v":"RF = 6-10-13"}]
[null,null,null,"Fog Tip 95-200","30-150 87 (CE)",null,null,null,null,null,null,null,null,null,null,null,"Fog Tip 18-30","1711",814,null,null,5,"171118-30","18-30",18,30,null,null,null,"171118-30","18-30",{"$f":"CONCATENATE(\"RF = \",ROUND(0.0505*VALUE($Y40)*SQRT(VALUE(TRIM(LEFT(AF$32,3)))),0),\"-\",ROUND(0.0505*VALUE($Z40)*SQRT(VALUE(TRIM(LEFT(AF$32,3)))),0))","v":"RF = 9-15"},{"$f":"CONCATENATE(\"RF = \",ROUND(0.0505*VALUE($Y40)*SQRT(VALUE(TRIM(LEFT(AG$32,3)))),0),\"-\",ROUND(0.0505*VALUE($Z40)*SQRT(VALUE(TRIM(LEFT(AG$32,3)))),0))","v":"RF = 8-14"},{"$f":"CONCATENATE(\"RF = \",ROUND(0.0505*VALUE($Y40)*SQRT(VALUE(TRIM(LEFT(AH$32,3)))),0),\"-\",ROUND(0.0505*VALUE($Z40)*SQRT(VALUE(TRIM(LEFT(AH$32,3)))),0))","v":"RF = 8-13"}]
[null,null,null,"Fog Tip 125-250","30-200 100 (Std)",null,null,null,null,null,null,null,null,{"$f":"VALUE(RIGHT(G11,IF(LEFT(RIGHT(G11,3),1)=\"-\",2,3)))","v":55},null,null,"Fog Tip 13-30","1711",null,null,null,5,"171113-30","13-23-30",13,23,30,null,null,"171113-30","13-23-30",{"$f":"CONCATENATE(\"RF = \",ROUND(0.0505*VALUE($Y41)*SQRT(VALUE(TRIM(LEFT(AF$32,3)))),0),\"-\",ROUND(0.0505*VALUE($Z41)*SQRT(VALUE(TRIM(LEFT(AF$32,3)))),0),\"-\",ROUND(0.0505*VALUE($AA41)*SQRT(VALUE(TRIM(LEFT(AF$32,3)))),0))","v":"RF = 7-12-15"},{"$f":"CONCATENATE(\"RF = \",ROUND(0.0505*VALUE($Y41)*SQRT(VALUE(TRIM(LEFT(AG$32,3)))),0),\"-\",ROUND(0.0505*VALUE($Z41)*SQRT(VALUE(TRIM(LEFT(AG$32,3)))),0),\"-\",ROUND(0.0505*VALUE($AA41)*SQRT(VALUE(TRIM(LEFT(AG$32,3)))),0))","v":"RF = 6-11-14"},{"$f":"CONCATENATE(\"RF = \",ROUND(0.0505*VALUE($Y41)*SQRT(VALUE(TRIM(LEFT(AH$32,3)))),0),\"-\",ROUND(0.0505*VALUE($Z41)*SQRT(VALUE(TRIM(LEFT(AH$32,3)))),0),\"-\",ROUND(0.0505*VALUE($AA41)*SQRT(VALUE(TRIM(LEFT(AH$32,3)))),0))","v":"RF = 6-10-13"}]
[null,null,null,"Fog Nozzle 30-200","30-200 75",null,null,null,null,null,null,null,null,"RF sufficiently low to allow single person to operate",null,null,"Fog Tip 30-125","1714",842,null,null,6,"171430-125","30-60-95-125",30,60,95,125,null,"171430-125","30-60-95-125","RF = 15-30-48-63","RF = 14-28-45-59","RF = 13-26-42-55"]
[null,null,null,"Fog Tip 30-200","95-200 100 (Std)",null,null,null,null,null,null,null,null,"Increased RF may require multiple persons to operate safely",null,null,"Fog Nozzle 30-125","1720",1198,null,null,6,"172030-125","30-60-95-125",30,60,95,125,null,"172030-125","30-60-95-125","RF = 15-30-48-63","RF = 14-28-45-59","RF = 13-26-42-55"]
[null,null,null,null,"95-200 75",null,null,null,null,null,null,null,null,"Recommend multiple persons to operate at this RF",null,null,"Fog Nozzle 95-200","1723",1372,null,null,6,"172395-200","95-125-150-200",95,125,150,200,null,"172395-200","95-125-150-200","RF = 48-63-76-101","RF = 45-59-71-94","RF = 42-55-66-87"]
[null,null,null,null,"12-53 87 (CE)",null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle 125-250","1733",1470,null,null,7,"1733125-250","125-150-200-250",125,150,200,250,null,"1733125-250","125-150-200-250","RF = 63-76-101-126","RF = 59-71-94-118","RF = 55-66-87-109"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip 95-200","1737",948,null,null,6,"173795-200","95-125-150-200",95,125,150,200,null,"173795-200","95-125-150-200","RF = 48-63-76-101","RF = 45-59-71-94","RF = 42-55-66-87"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip 125-250","1744",1002,null,null,7,"1744125-250","125-150-200-250",125,150,200,250,null,"1744125-250","125-150-200-250","RF = 63-76-101-126","RF = 59-71-94-118","RF = 55-66-87-109"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle 30-200","1763",1244,null,null,6,"176330-200","30-95-125-150-200",30,95,125,150,200,"176330-200","30-95-125-150-200",{"$f":"CONCATENATE(\"RF = \",ROUND(0.0505*VALUE($Y48)*SQRT(VALUE(TRIM(LEFT(AF$32,3)))),0),\"-\",ROUND(0.0505*VALUE($Z48)*SQRT(VALUE(TRIM(LEFT(AF$32,3)))),0),\"-\",ROUND(0.0505*VALUE($AA48)*SQRT(VALUE(TRIM(LEFT(AF$32,3)))),0),\"-\",ROUND(0.0505*VALUE($AB48)*SQRT(VALUE(TRIM(LEFT(AF$32,3)))),0),\"-\",ROUND(0.0505*VALUE($AC48)*SQRT(VALUE(TRIM(LEFT(AF$32,3)))),0))","v":"RF = 15-48-63-76-101"},"RF = 14-45-59-71-94","RF = 13-42-55-66-87"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip 30-200","1766",892,null,null,6,"176630-200","30-95-125-150-200",30,95,125,150,200,"176630-200","30-95-125-150-200","RF = 15-48-63-76-101","RF = 14-45-59-71-94","RF = 13-42-55-66-87"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Storz",88]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ZT",340]

{"sheet":"Fixed","index":2,"n_rows":92,"n_cols":102,"rows_kept":92,"cut":false,"hidden":false,"merged":[[15,2,17,10],[2,1,2,5],[3,1,3,5],[1,1,1,5],[4,1,4,5],[5,1,5,5],[0,8,1,10],[13,1,14,1],[7,10,8,10],[7,9,8,9],[7,8,8,8],[7,7,8,7],[7,6,8,6],[7,5,8,5],[7,2,8,2],[7,1,8,1],[2,8,3,10],[4,8,5,10],[0,7,5,7],[7,3,8,3],[13,2,14,6],[13,8,14,10],[12,2,12,6],[10,2,10,3],[11,5,11,6],[11,7,12,9],[11,10,12,10],[13,7,14,7],[7,4,8,4],[11,3,11,4],[6,3,6,7]]}
[null,"Instructions:",null,null,null,null,null,"Reaction Force Color Chart:","This is a Low RF Nozzle (RF < 51 )",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"asdf",null,null,"Style","Flow",null,"Flow",null,null,null,null,null,null,100,75,50,87,null,null,null,null,null,null,null,"Flow",null,null,null,"Flow","Pressure",null,null,null,null,null,null,null,"Style","Flow","Pressure",null,null,null,null,null,"Style",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Style"]
[null,"Tan-colored cells are headers or describe the selection options",null,null,null,null,null,null,null,null,null,null,"Nozzle",null,"Fog Nozzle","Fog Tip",null,"5-40","125-250","13-30","13-60","18-30","30-125","30-150","30-200","95-200","12-53",null,null,null,null,null,null,null,null,null,"4116",60,null,13,"100 (Std)",null,null,null,null,4116,60,60,null,60,null,null,null,null,null,null,"Fog Nozzle",13,"Fog Nozzle 13",null,null,13,"100 (Std)",{"$f":"CONCATENATE(BJ2,\" \",BK2)","v":"13 100 (Std)"},null,200,"100 (Std)",null,null,"Fog Nozzle",4116,60,"100 (Std)",{"$f":"CONCATENATE(BR2,\" \",BT2,\" @ \",BU2)","v":"Fog Nozzle 60 @ 100 (Std)"},null,null,null,"Fog Nozzle 125 @ 100",4116,4863,null,{"$f":"CONCATENATE($BZ2,\" \",CA2)","v":"Fog Nozzle 125 @ 100 4116"},{"$f":"CONCATENATE($BZ2,\" \",CB2)","v":"Fog Nozzle 125 @ 100 4863"},"Fog_Nozzle_125___100",null,null,"Fog Nozzle 125 @ 100 4116",null,null,null,null,null,null,"Fog Nozzle 125 @ 100",4116,null,null,"RF Chart",50,75,87,100]
[null,"Use the green-colored cells to make your selections (All cells must be filled in; information from \"FrontPage\" tab does not carry over to this page)",null,null,null,null,null,null,"This is a Nozzle with Increased RF (RF > 50 and <101 )",null,null,null,"Tip",null,"1 in","1.5 in",null,"100 (Std)","100 (Std)","100 (Std)","100 (Std)","100 (Std)","100 (Std)","100 (Std)","100 (Std)","100 (Std)","87 (CE)",null,null,null,null,null,null,null,null,null,"4116",95,null,25,"100 (Std)",null,null,null,null,4116,95,95,null,95,null,null,null,null,null,null,"Fog Nozzle",25,"Fog Nozzle 25",null,null,25,"100 (Std)",{"$f":"CONCATENATE(BJ3,\" \",BK3)","v":"25 100 (Std)"},null,250,"100 (Std)",null,null,"Fog Nozzle",4116,60,75,{"$f":"CONCATENATE(BR3,\" \",BT3,\" @ \",BU3)","v":"Fog Nozzle 60 @ 75"},null,null,null,"Fog Nozzle 125 @ 75",4116,4863,null,{"$f":"CONCATENATE($BZ3,\" \",CA3)","v":"Fog Nozzle 125 @ 75 4116"},{"$f":"CONCATENATE($BZ3,\" \",CB3)","v":"Fog Nozzle 125 @ 75 4863"},null,null,null,"Fog Nozzle 125 @ 100 4863",null,null,null,null,null,null,"Fog Nozzle 125 @ 75",4116,null,13,{"$f":"TRIM(CS3)","v":"13"},{"$f":"ROUND(0.0505*$CT3*SQRT(CU$2),0)","v":5},{"$f":"ROUND(0.0505*$CT3*SQRT(CV$2),0)","v":6},6,7]
[null,"Blue-colored cells provide outputs based on your selections",null,null,null,null,null,null,null,null,null,null,"High Pressure",null,"1.5 in",null,null,75,75,null,null,null,75,75,75,75,null,null,null,null,null,null,null,null,null,null,"4116",125,null,40,"100 (Std)",null,null,null,null,4116,125,125,null,125,null,null,null,null,null,null,"Fog Nozzle",40,"Fog Nozzle 40",null,null,40,"100 (Std)","40 100 (Std)",null,300,"100 (Std)",null,null,"Fog Nozzle",4116,60,"87 (CE)","Fog Nozzle 60 @ 87 (CE)",null,null,null,"Fog Nozzle 125 @ 87",4116,null,null,{"$f":"CONCATENATE($BZ4,\" \",CA4)","v":"Fog Nozzle 125 @ 87 4116"},null,null,null,null,"Fog Nozzle 125 @ 75 4116",null,null,null,null,null,null,"Fog Nozzle 125 @ 100",4863,null,25,{"$f":"TRIM(CS4)","v":"25"},9,11,12,13]
[null,"This shaded cell indicates an error has ocurred and you may need to modify some of your selections or contact our Customer Care team",null,null,null,null,null,null,"This Nozzle has a High RF (RF > 100 )",null,null,null,null,null,"2 in",null,null,"87 (CE)",null,null,null,null,"87 (CE)","87 (CE)",null,null,null,null,null,"5-40","100 (Std)",{"$f":"CONCATENATE(AD5,\" \",AE5)","v":"5-40 100 (Std)"},null,null,null,null,"4116",150,null,60,"100 (Std)",75,"87 (CE)",null,null,4116,150,150,null,150,null,null,null,null,null,null,"Fog Nozzle",60,"Fog Nozzle 60",null,null,60,"100 (Std)","60 100 (Std)",null,350,"100 (Std)",null,null,"Fog Nozzle",4116,95,"100 (Std)","Fog Nozzle 95 @ 100 (Std)",null,null,null,"Fog Nozzle 13 @ 100",4802,null,null,"Fog Nozzle 13 @ 100 4802",null,null,null,null,"Fog Nozzle 125 @ 75 4863",null,null,null,null,null,null,"Fog Nozzle 125 @ 75",4863,null,40,"40",14,17,19,20]
[null,"Orange-colored cell allows you to input your discount for Net Price",null,null,null,null,null,null,null,null,null,null,null,null,"2.5 in",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5-40",75,{"$f":"CONCATENATE(AD6,\" \",AE6)","v":"5-40 75"},null,null,null,null,"4802",13,null,95,"100 (Std)",75,"87 (CE)",null,null,4802,13,null,null,null,null,null,null,null,null,null,"Fog Nozzle",95,"Fog Nozzle 95",null,null,60,"87 (CE)","60 87 (CE)",null,200,75,null,null,"Fog Nozzle",4116,95,75,"Fog Nozzle 95 @ 75",null,null,null,"Fog Nozzle 150 @ 100",4116,4863,null,"Fog Nozzle 150 @ 100 4116",{"$f":"CONCATENATE($BZ6,\" \",CB6)","v":"Fog Nozzle 150 @ 100 4863"},null,null,null,"Fog Nozzle 125 @ 87 4116",null,null,null,null,null,null,"Fog Nozzle 125 @ 87",4116,null,60,"60",21,26,28,30]
[null,{"$f":"FrontPage!E8","v":"Rev Date: 6/27/2022"},null,"Fixed Orifice Fog Nozzles",null,null,null,null,null,null,null,null,null,null,"3 in",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5-40","87 (CE)","5-40 87 (CE)",null,null,null,null,"4802",25,null,125,"100 (Std)",75,"87 (CE)",null,null,4802,25,null,null,null,null,null,null,null,null,null,"Fog Nozzle",125,"Fog Nozzle 125",null,null,60,75,"60 75",null,250,75,null,null,"Fog Nozzle",4116,95,"87 (CE)","Fog Nozzle 95 @ 87 (CE)",null,null,null,"Fog Nozzle 150 @ 50",4863,null,null,"Fog Nozzle 150 @ 50 4863",null,null,null,null,"Fog Nozzle 13 @ 100 4802",null,null,null,null,null,null,"Fog Nozzle 13 @ 100",4802,null,95,"95",34,42,45,48]
[null,"Nozzle or Tip","Inlet Size","Flow Rate","Pressure Rating","Inlet Thread","Bumper Color",{"$f":"IF(OR(B10=\"FOG TIP\",J10=\"yes\"),\"\",\"Remove Pistol Grip?\")","v":"Remove Pistol Grip?"},"Style Number",{"$f":"IF(B10=\"FOG TIP\",\"\",\"ZT Inlet?\")","v":"ZT Inlet?"},"Custom Etch",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"125-250","100 (Std)","125-250 100 (Std)",null,null,null,null,"4802",40,null,150,"100 (Std)",75,50,"87 (CE)",null,4802,40,null,null,null,null,null,null,null,null,null,"Fog Nozzle",150,"Fog Nozzle 150",null,null,95,"100 (Std)","95 100 (Std)",null,300,75,null,null,"Fog Nozzle",4116,125,"100 (Std)","Fog Nozzle 125 @ 100 (Std)",null,null,null,"Fog Nozzle 150 @ 75",4116,4863,null,"Fog Nozzle 150 @ 75 4116",{"$f":"CONCATENATE($BZ8,\" \",CB8)","v":"Fog Nozzle 150 @ 75 4863"},null,null,null,"Fog Nozzle 150 @ 100 4116",null,null,null,null,null,null,"Fog Nozzle 150 @ 100",4116,null,125,"125",45,55,59,63]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"ROUND(0.0505*VALUE(D10)*SQRT(VALUE(TRIM(LEFT(E10,3)))),0)","v":101},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"125-250",75,"125-250 75",null,null,null,null,"4824",200,null,161,50,null,null,null,null,4824,200,200,null,null,null,null,null,null,null,null,"Fog Nozzle",161,"Fog Nozzle 161",null,null,95,75,"95 75",null,210,50,null,null,"Fog Nozzle",4116,125,75,"Fog Nozzle 125 @ 75",null,null,null,"Fog Nozzle 150 @ 87",4116,null,null,"Fog Nozzle 150 @ 87 4116",null,null,null,null,"Fog Nozzle 150 @ 100 4863",null,null,null,null,null,null,"Fog Nozzle 150 @ 100",4863,null,150,"150",54,66,71,76]
[null,"Fog Nozzle","1.5 in",200,"100 (Std)","NH","BLACK (Std)","No (Std)",4863,"No (Std)","No (Std)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"13-30","100 (Std)","13-30 100 (Std)",null,null,null,null,"4824",210,null,175,"100 (Std)",75,50,null,null,4824,null,null,210,null,null,null,null,null,null,null,"Fog Nozzle",175,"Fog Nozzle 175",null,null,95,"87 (CE)","95 87 (CE)",null,250,50,null,null,"Fog Nozzle",4116,125,"87 (CE)","Fog Nozzle 125 @ 87 (CE)",null,null,null,"Fog Nozzle 161 @ 50",4863,null,null,"Fog Nozzle 161 @ 50 4863",null,null,null,null,"Fog Nozzle 150 @ 50 4863",null,null,null,null,null,null,"Fog Nozzle 150 @ 50",4863,null,161,"161",57,70,76,81]
[null,"List price",{"$f":"SUM(E11:K11)","v":992},null,{"$f":"IFERROR(CONCATENATE(\"RF = \",ROUND(0.0505*VALUE(D10)*SQRT(VALUE(TRIM(LEFT(E10,3)))),0)),\"\")","v":"RF = 101"},{"$f":"IF(OR(F10=\"Storz\",F10=\"BIM\"),_xlfn.XLOOKUP(\"storz\",AF:AF,AG:AG),0)","v":0},null,null,{"$f":"IFERROR(VLOOKUP(I10,AF28:AG33,2,FALSE),\"\")","v":992},{"$f":"IF(J8=\"\",0,IF(J10=\"Yes\",_xlfn.XLOOKUP(\"zt\",AF:AF,AG:AG),0))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"13-60","100 (Std)","13-60 100 (Std)",null,null,null,null,"4824",250,null,185,50,null,null,null,null,4824,250,250,250,null,null,null,null,null,null,null,"Fog Nozzle",185,"Fog Nozzle 185",null,null,125,"100 (Std)","125 100 (Std)",null,null,null,null,null,"Fog Nozzle",4116,150,"100 (Std)","Fog Nozzle 150 @ 100 (Std)",null,null,null,"Fog Nozzle 175 @ 100",4863,null,null,"Fog Nozzle 175 @ 100 4863",null,null,null,null,"Fog Nozzle 150 @ 75 4116",null,null,null,null,null,null,"Fog Nozzle 150 @ 75",4116,null,175,"175",62,77,82,88]
[null,"Your Discount",null,"Net Price",null,{"$f":"ROUND(C11*(1-C12),2)","v":992},null,{"$f":"IF(OR(B10=\"fog tip\",TRIM(I10)=\"4116\"),\"\",\"Include Color Clips for Shutoff and/or Pistol Grip?\")","v":"Include Color Clips for Shutoff and/or Pistol Grip?"},null,null,"Yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"18-30","100 (Std)","18-30 100 (Std)",null,null,null,null,"4824",265,null,200,"100 (Std)",75,50,null,null,4824,300,300,null,null,null,null,null,null,null,null,"Fog Nozzle",200,"Fog Nozzle 200",null,null,125,75,"125 75",null,null,null,null,null,"Fog Nozzle",4116,150,75,"Fog Nozzle 150 @ 75",null,null,null,"Fog Nozzle 175 @ 50",4863,null,null,"Fog Nozzle 175 @ 50 4863",null,null,null,null,"Fog Nozzle 150 @ 75 4863",null,null,null,null,null,null,"Fog Nozzle 150 @ 75",4863,null,185,"185",66,81,87,93]
[null,"Short Description",{"$f":"IF(B24=\"Error\",\"Fix Errors\",CONCATENATE(I10,\" \",C10,\" \",F10,\" \",D10,\" \",E10,\" \",G10,IF(B10=\"Fog Tip\",\" \",IF(J10=\"yes\",\" PG\",IF(H10=\"yes\",\" NPG\",\" PG\"))),IF(B10=\"Fog Tip\",\"\",IF(J10=\"Yes\",\" ZT\",\"\")),IF(K10=\"Yes\",\" ETCH\",\"\")))","v":"4863 1.5 in NH 200 100 (Std) BLACK (Std) PG"},null,null,null,null,null,null,null,null,null,"1 IN","NH",null,null,null,"1 in","1.5 in","2 in","2.5 in","3 in",null,null,null,null,null,null,null,"30-125","100 (Std)","30-125 100 (Std)",null,null,null,null,"4824",300,null,210,50,null,null,null,null,4824,350,null,null,null,null,null,null,null,null,null,"Fog Nozzle",210,"Fog Nozzle 210",null,null,125,50,"125 50",null,null,null,null,null,"Fog Nozzle",4116,150,"87 (CE)","Fog Nozzle 150 @ 87 (CE)",null,null,null,"Fog Nozzle 175 @ 75",4863,null,null,"Fog Nozzle 175 @ 75 4863",null,null,null,null,"Fog Nozzle 150 @ 87 4116",null,null,null,null,null,null,"Fog Nozzle 150 @ 87",4116,null,200,"200",71,87,94,101]
[null,"Long Description",{"$f":"IF(B24=\"Error\",\"Some of your selections are not compatible with others; please correct the errors highlighted in RED\",CONCATENATE(\"Style \",I10,\" \",B10,\" with \",C10,\" \",F10,\" inlet; \",D10,\" gpm @ \",E10,IF(E11>\"\",CONCATENATE(\" psi (\",E11,\"); \"),\" psi; \"),PROPER(G10),\" bumper\",IF(B10=\"Fog Tip\",\"\",IF(J10=\"yes\",\"\",IF(H10=\"yes\",\"; no pistol grip\",\"; pistol grip\"))),IF(B10=\"Fog Tip\",\"\",IF(J10=\"Yes\",\"; Zero-Torque Grip\",\"\")),IF(K10=\"Yes\",\"; Custom Etched\",\"\")))","v":"Style 4863 Fog Nozzle with 1.5 in NH inlet; 200 gpm @ 100 (Std) psi (RF = 101); Black (Std) bumper; pistol grip"},null,null,null,null,"Akron Brass Part Number and Description",{"$f":"IF(AND(OR(F10=\"custom\",G10=\"custom\"),K10=\"yes\"),\"Contact Customer Care to request Custom Thread and Etch (800-228-1161)\",IF(F10=\"custom\",\"Contact Customer Care to request Custom Thread (800-228-1161)\",IF(K10=\"Yes\",\"Contact Customer Care to request Custom Etch (800-228-1161)\",IF(B24=\"Error\",\"Incompatible selections; please correct errors highlighted in RED\",IFERROR(CONCATENATE(VLOOKUP(C13,DataSource!AH:AJ,2,FALSE),\"      \",VLOOKUP(C13,DataSource!AH:AJ,3,FALSE)),\"Version you've requested not yet created; contact Customer Care (800-228-1161)\")))))","v":"48634144      ASLT 2.5NH 125G@100P FM"},null,null,null,"1 IN","NPSH",null,null,"30-125",13,60,60,60,60,null,null,null,null,null,null,null,"30-125",75,"30-125 75",null,null,null,null,"4824",350,null,225,"100 (Std)",null,null,null,null,4826,200,200,null,null,null,null,null,null,null,null,"Fog Nozzle",225,"Fog Nozzle 225",null,null,125,"87 (CE)","125 87 (CE)",null,null,null,null,null,"Fog Nozzle",4802,13,"100 (Std)","Fog Nozzle 13 @ 100 (Std)",null,null,null,"Fog Nozzle 185 @ 50",4863,null,null,"Fog Nozzle 185 @ 50 4863",null,null,null,null,"Fog Nozzle 161 @ 50 4863",null,null,null,null,null,null,"Fog Nozzle 161 @ 50",4863,null,210,"210",75,92,99,106]
[null,null,null,null,null,null,null,null,null,null,null,null,"1 IN","STORZ",null,null,"30-150",25,95,95,95,95,null,null,null,null,null,null,null,"30-125","87 (CE)","30-125 87 (CE)",null,null,null,null,"4826",200,null,250,"100 (Std)",75,50,null,null,4826,null,null,210,null,null,null,null,null,null,null,"Fog Nozzle",250,"Fog Nozzle 250",null,null,150,"100 (Std)","150 100 (Std)",null,null,null,null,null,"Fog Nozzle",4802,25,"100 (Std)","Fog Nozzle 25 @ 100 (Std)",null,null,null,"Fog Nozzle 200 @ 100",4826,4863,null,"Fog Nozzle 200 @ 100 4826",{"$f":"CONCATENATE($BZ15,\" \",CB15)","v":"Fog Nozzle 200 @ 100 4863"},null,null,null,"Fog Nozzle 175 @ 100 4863",null,null,null,null,null,null,"Fog Nozzle 175 @ 100",4863,null,225,"225",80,98,106,114]
[null,"Notes: ","You can make any notes about what you want, or anything else, in this space",null,null,null,null,null,null,null,null,null,"1.5 in",null,null,null,"30-200",40,125,125,125,125,null,null,null,null,null,null,null,"30-150","100 (Std)","30-150 100 (Std)",null,null,null,null,"4826",210,null,265,50,null,null,null,null,4826,250,250,250,null,null,null,null,null,null,null,"Fog Nozzle",265,"Fog Nozzle 265",null,null,150,75,"150 75",null,null,null,null,null,"Fog Nozzle",4802,40,"100 (Std)","Fog Nozzle 40 @ 100 (Std)",null,null,null,"Fog Nozzle 200 @ 75",4826,4863,null,"Fog Nozzle 200 @ 75 4826",{"$f":"CONCATENATE($BZ16,\" \",CB16)","v":"Fog Nozzle 200 @ 75 4863"},null,null,null,"Fog Nozzle 175 @ 50 4863",null,null,null,null,null,null,"Fog Nozzle 175 @ 50",4863,null,250,"250",89,109,118,126]
[null,null,null,null,null,null,null,null,null,null,null,null,"1.5 in",null,null,null,"95-200",null,150,150,150,150,null,null,null,null,null,null,null,"30-150",75,"30-150 75",null,null,null,null,"4826",250,null,300,"100 (Std)",75,null,null,null,4826,300,300,null,null,null,null,null,null,null,null,"Fog Nozzle",300,"Fog Nozzle 300",null,null,150,50,"150 50",null,null,null,null,null,"Fog Tip",4824,200,"100 (Std)","Fog Tip 200 @ 100 (Std)",null,null,null,"Fog Nozzle 200 @ 50",4826,4863,null,{"$f":"CONCATENATE($BZ18,\" \",CA18)","v":"Fog Nozzle 210 @ 50 4826"},null,null,null,null,"Fog Nozzle 175 @ 75 4863",null,null,null,null,null,null,"Fog Nozzle 175 @ 75",4863,null,300,"300",107,131,141,152]
[null,null,null,null,null,null,null,null,null,null,null,null,"1.5 in",null,null,null,"125-250",null,161,161,161,161,null,null,null,null,null,null,null,"30-150","87 (CE)","30-150 87 (CE)",null,null,null,null,"4826",300,null,350,"100 (Std)",null,null,null,null,4826,350,null,null,null,null,null,null,null,null,null,"Fog Nozzle",350,"Fog Nozzle 350",null,null,150,"87 (CE)","150 87 (CE)",null,null,null,null,null,"Fog Tip",4824,250,"100 (Std)","Fog Tip 250 @ 100 (Std)",null,null,null,"Fog Nozzle 210 @ 50",4826,null,null,"Fog Nozzle 225 @ 100 4863",null,null,null,null,"Fog Nozzle 185 @ 50 4863",null,null,null,null,null,null,"Fog Nozzle 185 @ 50",4863,null,350,"350",125,153,165,177]
[null,null,null,null,null,null,null,null,null,null,null,null,"1.5 IN",null,null,null,null,null,175,175,175,175,null,null,null,null,null,null,null,"30-200","100 (Std)","30-200 100 (Std)",null,null,null,null,"4826",350,null,null,null,null,null,null,null,4863,95,null,null,null,null,null,null,null,null,null,"Fog Tip",95,"Fog Tip 95",null,null,161,50,"161 50",null,null,null,null,null,"Fog Tip",4824,300,"100 (Std)","Fog Tip 300 @ 100 (Std)",null,null,null,"Fog Nozzle 225 @ 100",4863,null,null,"Fog Nozzle 25 @ 100 4802",null,null,null,null,"Fog Nozzle 200 @ 100 4826",null,null,null,null,null,null,"Fog Nozzle 200 @ 100",4826,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,"1.5 in",null,null,null,null,null,185,185,185,185,null,null,null,null,null,null,null,"30-200",75,"30-200 75",null,null,null,null,"4863",95,null,null,null,null,null,null,null,4863,125,125,125,null,null,null,null,null,null,null,"Fog Tip",125,"Fog Tip 125",null,null,175,"100 (Std)","175 100 (Std)",null,null,null,null,null,"Fog Tip",4824,350,"100 (Std)","Fog Tip 350 @ 100 (Std)",null,null,null,"Fog Nozzle 25 @ 100",4802,null,null,"Fog Nozzle 250 @ 100 4826",null,null,null,null,"Fog Nozzle 200 @ 100 4863",null,null,null,null,null,null,"Fog Nozzle 200 @ 75",4826,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,"1.5 IN",null,null,null,null,null,200,200,200,200,null,null,null,null,null,null,null,"95-200","100 (Std)","95-200 100 (Std)",null,null,null,null,"4863",125,null,null,null,null,null,null,null,4863,150,150,150,null,null,null,null,null,null,null,"Fog Tip",150,"Fog Tip 150",null,null,175,75,"175 75",null,null,null,null,null,"Fog Tip",4824,200,75,"Fog Tip 200 @ 75",null,null,null,"Fog Nozzle 250 @ 100",4826,null,null,"Fog Nozzle 250 @ 50 4826",null,null,null,null,"Fog Nozzle 200 @ 75 4826",null,null,null,null,null,null,"Fog Nozzle 200 @ 100",4863,null,null,""]
[null,null,null,{"$f":"CONCATENATE(\"_\",SUBSTITUTE(C10,\" \",\"_\"),\"_\",SUBSTITUTE(D10,\"-\",\"_\"))","v":"_1.5_in_200"},null,null,null,null,{"$f":"CONCATENATE(SUBSTITUTE(B10,\" \",\"_\"),\"_\",SUBSTITUTE(D10,\"-\",\"_\"))","v":"Fog_Nozzle_200"},null,"asdfa",null,"2 IN","STORZ",null,null,null,null,210,210,210,210,null,null,null,null,null,null,null,"95-200",75,"95-200 75",null,null,null,null,"4863",150,null,null,null,null,null,null,null,4863,175,175,175,null,null,null,null,null,null,null,"Fog Tip",161,"Fog Tip 161",null,null,175,50,"175 50",null,null,null,null,null,"Fog Tip",4824,250,75,"Fog Tip 250 @ 75",null,null,null,"Fog Nozzle 250 @ 50",4826,null,null,"Fog Nozzle 250 @ 75 4826",null,null,null,null,"Fog Nozzle 200 @ 75 4863",null,null,null,null,null,null,"Fog Nozzle 200 @ 75",4863,null,null,""]
[null,null,null,{"$f":"CONCATENATE(C10,\" \",D10)","v":"1.5 in 200"},null,null,null,null,null,null,null,null,"2.5 IN","NH",null,null,null,null,225,225,225,225,null,null,null,null,null,null,null,"12-53","87 (CE)","12-53 87 (CE)",null,null,null,null,"4863",161,null,null,null,null,null,null,null,4863,200,200,null,null,null,null,null,null,null,null,"Fog Tip",175,"Fog Tip 175",null,null,185,50,"185 50",null,null,null,null,null,"Fog Tip",4824,300,75,"Fog Tip 300 @ 75",null,null,null,"Fog Nozzle 250 @ 75",4826,null,null,"Fog Nozzle 265 @ 50 4826",null,null,null,null,"Fog Nozzle 210 @ 50 4826",null,null,null,null,null,null,"Fog Nozzle 210 @ 50",4826,null,null,""]
[null,{"$f":"IF(OR(C24=\"False\",D24=\"False\",E24=\"False\",H24=\"False\",J24=\"False\",F24=\"False\"),\"Error\",\"Okay\")","v":"Okay"},{"$f":"IFERROR(VLOOKUP(CONCATENATE(B10,\" \",C10),C29:C45,1,FALSE),\"False\")","v":"Fog Nozzle 1.5 in"},{"$f":"IFERROR(VLOOKUP(CONCATENATE(B10,\" \",D10),D29:D58,1,FALSE),\"False\")","v":"Fog Nozzle 200"},{"$f":"IFERROR(VLOOKUP(CONCATENATE(D10,\" \",E10),E29:E62,1,FALSE),\"False\")","v":"200 100 (Std)"},{"$f":"IF(OR(C10=\"2 in\",C10=\"3 in\"),IF(F10=\"storz\",\"Okay\",\"False\"),\"Okay\")","v":"Okay"},null,{"$f":"IF($B10=\"Fog Tip\",IF(H10=\"yes\",\"False\",\"Okay\"),\"Okay\")","v":"Okay"},{"$f":"IFERROR(VLOOKUP(CONCATENATE(B10,\" \",D10,\" @ \",IF(E10=\"100 (Std)\",100,IF(E10=\"87 (ce)\",87,E10)),\" \",I10),I28:I92,1,FALSE),\"False\")","v":"Fog Nozzle 200 @ 100 4863"},{"$f":"IF($B10=\"Fog Tip\",IF(J10=\"yes\",\"False\",\"Okay\"),\"Okay\")","v":"Okay"},null,null,"2.5 IN","NPSH",null,null,null,null,250,250,250,250,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4863",175,null,null,null,null,null,null,null,4863,null,null,161,null,null,null,null,null,null,null,"Fog Tip",200,"Fog Tip 200",null,null,200,"100 (Std)","200 100 (Std)",null,null,null,null,null,"Fog Tip",4824,210,50,"Fog Tip 210 @ 50",null,null,null,"Fog Nozzle 265 @ 50",4826,null,null,"Fog Nozzle 300 @ 100 4826",null,null,null,null,"Fog Nozzle 225 @ 100 4863",null,null,null,null,null,null,"Fog Nozzle 225 @ 100",4863,null,null,""]
[null,null,null,null,null,null,null,null,null,null,null,null,"2.5 IN","FDNY",null,null,null,null,300,300,300,300,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4863",185,null,null,null,null,null,null,null,4863,null,null,185,null,null,null,null,null,null,null,"Fog Tip",210,"Fog Tip 210",null,null,200,75,"200 75",null,null,null,null,null,"Fog Tip",4824,265,50,"Fog Tip 265 @ 50",null,null,null,"Fog Nozzle 300 @ 100",4826,null,null,"Fog Nozzle 300 @ 75 4826",null,null,null,null,"Fog Nozzle 25 @ 100 4802",null,null,null,null,null,null,"Fog Nozzle 25 @ 100",4802,null,null,""]
[null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(SUBSTITUTE(B10,\" \",\"_\"),\"_\",D10,\"___\",IF(E10=\"100 (Std)\",100,IF(E10=\"87 (ce)\",87,E10)),\" \",I10)","v":"Fog_Nozzle_200___100 4863"},null,null,null,"2.5 IN","NYCORP",null,null,null,null,350,350,350,350,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4863",200,null,null,null,null,null,null,null,4866,95,null,null,null,null,null,null,null,null,null,"Fog Tip",225,"Fog Tip 225",null,null,200,50,{"$f":"CONCATENATE(BJ26,\" \",BK26)","v":"200 50"},null,null,null,null,null,"Fog Tip",4824,250,50,"Fog Tip 250 @ 50",null,null,null,"Fog Nozzle 300 @ 75",4826,null,null,"Fog Nozzle 350 @ 100 4826",null,null,null,null,"Fog Nozzle 250 @ 100 4826",null,null,null,null,null,null,"Fog Nozzle 250 @ 100",4826,null,null,""]
[null,null,null,"2.5 in 30-125",null,null,null,null,null,null,null,null,"2.5 IN","PITT6",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4863",225,null,null,null,null,null,null,null,4866,125,125,125,null,null,null,null,null,null,null,"Fog Tip",250,"Fog Tip 250",null,null,210,50,"210 50",null,null,null,null,null,"Fog Nozzle",4826,200,"100 (Std)","Fog Nozzle 200 @ 100 (Std)",null,null,null,"Fog Nozzle 350 @ 100",4826,null,null,"Fog Nozzle 40 @ 100 4802",null,null,null,null,"Fog Nozzle 250 @ 50 4826",null,null,null,null,null,null,"Fog Nozzle 250 @ 50",4826,null,null,""]
[null,null,null,null,null,null,null,null,"Fog Nozzle 125 @ 100 4116",null,null,null,"2.5 IN","BAT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4116,888,null,null,null,"4866",95,null,null,null,null,null,null,null,4866,150,150,150,null,null,null,null,null,null,null,"Fog Tip",265,"Fog Tip 265",null,null,225,"100 (Std)","225 100 (Std)",null,null,null,null,null,"Fog Nozzle",4826,250,"100 (Std)","Fog Nozzle 250 @ 100 (Std)",null,null,null,"Fog Nozzle 40 @ 100",4802,null,null,"Fog Nozzle 60 @ 100 4116",null,null,null,null,"Fog Nozzle 250 @ 75 4826",null,null,null,null,null,null,"Fog Nozzle 250 @ 75",4826,null,null,""]
[null,null,{"$f":"CONCATENATE(O$2,\" \",O3)","v":"Fog Nozzle 1 in"},"Fog Nozzle 13","13 100 (Std)",null,null,null,"Fog Nozzle 125 @ 100 4863",null,null,null,"2.5 IN","CSA",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4802,996,null,null,null,"4866",125,null,null,null,null,null,null,null,4866,175,175,175,null,null,null,null,null,null,null,"Fog Tip",300,"Fog Tip 300",null,null,250,"100 (Std)","250 100 (Std)",null,null,null,null,null,"Fog Nozzle",4826,300,"100 (Std)","Fog Nozzle 300 @ 100 (Std)",null,null,null,"Fog Nozzle 60 @ 100",4116,null,null,"Fog Nozzle 60 @ 75 4116",null,null,null,null,"Fog Nozzle 265 @ 50 4826",null,null,null,null,null,null,"Fog Nozzle 265 @ 50",4826,null,null,""]
[null,null,{"$f":"CONCATENATE(O$2,\" \",O4)","v":"Fog Nozzle 1.5 in"},"Fog Nozzle 25","25 100 (Std)",null,{"$f":"VLOOKUP(C13,DataSource!AH:AJ,2,FALSE)","v":"48634144"},{"$f":"VLOOKUP(C13,DataSource!AH:AJ,3,FALSE)","v":"ASLT 2.5NH 125G@100P FM"},"Fog Nozzle 125 @ 75 4116",null,null,null,"2.5 IN","QST",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4824,902,null,null,null,"4866",150,null,null,null,null,null,null,null,4866,200,200,null,null,null,null,null,null,null,null,"Fog Tip",350,"Fog Tip 350",null,null,250,75,"250 75",null,null,null,null,null,"Fog Nozzle",4826,350,"100 (Std)","Fog Nozzle 350 @ 100 (Std)",null,null,null,"Fog Nozzle 60 @ 75",4116,null,null,"Fog Nozzle 60 @ 87 4116",null,null,null,null,"Fog Nozzle 300 @ 100 4826",null,null,null,null,null,null,"Fog Nozzle 300 @ 100",4826,null,null,""]
[null,null,{"$f":"CONCATENATE(O$2,\" \",O5)","v":"Fog Nozzle 2 in"},"Fog Nozzle 40","40 100 (Std)",null,null,null,"Fog Nozzle 125 @ 75 4863",null,null,null,"2.5 IN","BIM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4826,1278,null,null,null,"4866",161,null,null,null,null,null,null,null,4866,null,null,161,null,null,null,null,null,null,null,null,null,null,null,null,250,50,"250 50",null,null,null,null,null,"Fog Nozzle",4826,200,75,"Fog Nozzle 200 @ 75",null,null,null,"Fog Nozzle 60 @ 87",4116,null,null,"Fog Nozzle 95 @ 100 4116",{"$f":"CONCATENATE($BZ32,\" \",CB32)","v":"Fog Nozzle 95 @ 100 4863"},null,null,null,"Fog Nozzle 300 @ 75 4826",null,null,null,null,null,null,"Fog Nozzle 300 @ 75",4826,null,null,""]
[null,null,{"$f":"CONCATENATE(O$2,\" \",O6)","v":"Fog Nozzle 2.5 in"},"Fog Nozzle 60","60 100 (Std)",null,null,null,"Fog Nozzle 125 @ 87 4116",null,null,null,"2.5 IN","STORZ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4863,992,null,null,null,"4866",175,null,null,null,null,null,null,null,4866,null,null,185,null,null,null,null,null,null,null,null,null,null,null,null,265,50,"265 50",null,null,null,null,null,"Fog Nozzle",4826,265,50,"Fog Nozzle 265 @ 50",null,null,null,"Fog Nozzle 95 @ 100",4116,4863,null,"Fog Nozzle 95 @ 75 4116",null,null,null,null,"Fog Nozzle 350 @ 100 4826",null,null,null,null,null,null,"Fog Nozzle 350 @ 100",4826,null,null,""]
[null,null,{"$f":"CONCATENATE(O$2,\" \",O7)","v":"Fog Nozzle 3 in"},"Fog Nozzle 95","60 87 (CE)",null,null,null,"Fog Nozzle 13 @ 100 4802",null,null,null,"3 IN","STORZ",null,null,"BLACK (Std)","THREAD1 IN","NH","NPSH","Storz","Custom","PCT","Storz","Custom",null,null,null,null,null,null,4866,772,null,null,null,"4866",185,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,300,"100 (Std)","300 100 (Std)",null,null,null,null,null,"Fog Nozzle",4826,250,75,"Fog Nozzle 250 @ 75",null,null,null,"Fog Nozzle 95 @ 75",4116,null,null,"Fog Nozzle 95 @ 87 4116",null,null,null,null,"Fog Nozzle 40 @ 100 4802",null,null,null,null,null,null,"Fog Nozzle 40 @ 100",4802,null,null,""]
[null,null,{"$f":"CONCATENATE(P$2,\" \",P3)","v":"Fog Tip 1.5 in"},"Fog Nozzle 125","60 75",null,null,null,"Fog Nozzle 150 @ 100 4116",null,null,null,null,null,null,null,"ORANGE","THREAD1.5 in","NH","NPSH","FDNY","NYCORP","Storz","Custom",null,null,null,null,null,null,null,"Storz",88,null,null,null,"4866",200,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,300,75,"300 75",null,null,null,null,null,"Fog Nozzle",4826,300,75,"Fog Nozzle 300 @ 75",null,null,null,"Fog Nozzle 95 @ 87",4116,null,null,"Fog Tip 125 @ 100 4866",null,null,null,null,"Fog Nozzle 60 @ 100 4116",null,null,null,null,null,null,"Fog Nozzle 60 @ 100",4116,null,null,""]
[null,null,null,"Fog Nozzle 150","95 100 (Std)",null,null,null,"Fog Nozzle 150 @ 100 4863",null,null,null,null,null,null,null,"YELLOW","THREAD2 IN","Storz",null,null,null,null,null,null,null,null,null,null,null,null,"ZT",340,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,350,"100 (Std)","350 100 (Std)",null,null,null,null,null,"Fog Nozzle",4826,210,50,"Fog Nozzle 210 @ 50",null,null,null,"Fog Tip 125 @ 100",4866,null,null,"Fog Tip 125 @ 75 4866",null,null,null,null,"Fog Nozzle 60 @ 75 4116",null,null,null,null,null,null,"Fog Nozzle 60 @ 75",4116,null,null,""]
[null,null,null,"Fog Nozzle 161","95 75",null,null,null,"Fog Nozzle 150 @ 50 4863",null,null,null,null,null,null,null,"RED","THREAD2.5 IN","NH","NPSH","FDNY","NYCORP","PITT6","BAT","CSA","QST","BIM","Storz","Custom",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4826,250,50,"Fog Nozzle 250 @ 50",null,null,null,"Fog Tip 125 @ 75",4866,null,null,"Fog Tip 150 @ 100 4866",null,null,null,null,"Fog Nozzle 60 @ 87 4116",null,null,null,null,null,null,"Fog Nozzle 60 @ 87",4116,null,null,""]
[null,null,null,"Fog Nozzle 175","95 87 (CE)",null,null,null,"Fog Nozzle 150 @ 75 4116",null,null,null,null,null,null,null,"BLUE","THREAD3 IN","Storz",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4863,95,"100 (Std)","Fog Nozzle 95 @ 100 (Std)",null,null,null,"Fog Tip 150 @ 100",4866,null,null,"Fog Tip 150 @ 50 4866",null,null,null,null,"Fog Nozzle 95 @ 100 4116",null,null,null,null,null,null,"Fog Nozzle 95 @ 100",4116,null,null,""]
[null,null,null,"Fog Nozzle 185","125 100 (Std)",null,null,null,"Fog Nozzle 150 @ 75 4863",null,null,null,null,null,null,null,"GREEN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4863,125,"100 (Std)","Fog Nozzle 125 @ 100 (Std)",null,null,null,"Fog Tip 150 @ 50",4866,null,null,"Fog Tip 150 @ 75 4866",null,null,null,null,"Fog Nozzle 95 @ 100 4863",null,null,null,null,null,null,"Fog Nozzle 95 @ 100",4863,null,null,""]
[null,null,null,"Fog Nozzle 200","125 75",null,null,null,"Fog Nozzle 150 @ 87 4116",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4863,150,"100 (Std)","Fog Nozzle 150 @ 100 (Std)",null,null,null,"Fog Tip 150 @ 75",4866,null,null,"Fog Tip 161 @ 50 4866",null,null,null,null,"Fog Nozzle 95 @ 75 4116",null,null,null,null,null,null,"Fog Nozzle 95 @ 75",4116,null,null,""]
[null,null,null,"Fog Nozzle 210",null,null,null,null,"Fog Nozzle 161 @ 50 4863",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4863,175,"100 (Std)","Fog Nozzle 175 @ 100 (Std)",null,null,null,"Fog Tip 161 @ 50",4866,null,null,"Fog Tip 175 @ 100 4866",null,null,null,null,"Fog Nozzle 95 @ 87 4116",null,null,null,null,null,null,"Fog Nozzle 95 @ 87",4116,null,null,""]
[null,null,null,"Fog Nozzle 225","125 87 (CE)",null,null,null,"Fog Nozzle 175 @ 100 4863",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"bmpr4116","BLACK (Std)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4863,200,"100 (Std)","Fog Nozzle 200 @ 100 (Std)",null,null,null,"Fog Tip 175 @ 100",4866,null,null,"Fog Tip 175 @ 50 4866",null,null,null,null,"Fog Tip 125 @ 100 4866",null,null,null,null,null,null,"Fog Tip 125 @ 100",4866,null,null,""]
[null,null,null,"Fog Nozzle 250","150 100 (Std)",null,null,null,"Fog Nozzle 175 @ 50 4863",null,null,null,null,null,null,null,null,"Style",null,null,{"$f":"IF(B10=\"fog tip\",\"N/A\",\"No (Std)\")","v":"No (Std)"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"bmpr4802","BLACK (Std)","ORANGE","YELLOW","RED","BLUE","GREEN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4863,125,75,"Fog Nozzle 125 @ 75",null,null,null,"Fog Tip 175 @ 50",4866,null,null,"Fog Tip 175 @ 75 4866",null,null,null,null,"Fog Tip 125 @ 75 4866",null,null,null,null,null,null,"Fog Tip 125 @ 75",4866,null,null,""]
[null,null,null,"Fog Nozzle 265","150 75",null,null,null,"Fog Nozzle 175 @ 75 4863",null,null,null,null,null,null,null,"Fog Nozzle 5-40","1602",null,null,{"$f":"IF(B10=\"fog tip\",\"\",\"Yes\")","v":"Yes"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"bmpr4824","BLACK (Std)","ORANGE","YELLOW","RED","BLUE","GREEN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4863,150,75,"Fog Nozzle 150 @ 75",null,null,null,"Fog Tip 175 @ 75",4866,null,null,"Fog Tip 185 @ 50 4866",null,null,null,null,"Fog Tip 150 @ 100 4866",null,null,null,null,null,null,"Fog Tip 150 @ 100",4866,null,null,""]
[null,null,null,"Fog Nozzle 300","150 50",null,null,null,"Fog Nozzle 185 @ 50 4863",null,null,null,null,13,null,null,"Fog Nozzle 12-53","1602",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"bmpr4826","BLACK (Std)","ORANGE","YELLOW","RED","BLUE","GREEN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4863,175,75,"Fog Nozzle 175 @ 75",null,null,null,"Fog Tip 185 @ 50",4866,null,null,"Fog Tip 200 @ 100 4824",{"$f":"CONCATENATE($BZ45,\" \",CB45)","v":"Fog Tip 200 @ 100 4866"},null,null,null,"Fog Tip 150 @ 50 4866",null,null,null,null,null,null,"Fog Tip 150 @ 50",4866,null,null,""]
[null,null,null,"Fog Nozzle 350","150 87 (CE)",null,null,null,"Fog Nozzle 200 @ 100 4826",null,null,null,null,25,null,null,"Fog Nozzle 30-150","1616",35,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"bmpr4863","BLACK (Std)","ORANGE","YELLOW","RED","BLUE","GREEN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4863,200,75,"Fog Nozzle 200 @ 75",null,null,null,"Fog Tip 200 @ 100",4824,4866,null,"Fog Tip 200 @ 75 4824",{"$f":"CONCATENATE($BZ46,\" \",CB46)","v":"Fog Tip 200 @ 75 4866"},null,null,null,"Fog Tip 150 @ 75 4866",null,null,null,null,null,null,"Fog Tip 150 @ 75",4866,null,null,""]
[null,null,null,"Fog Tip 95","161 50",null,null,null,"Fog Nozzle 200 @ 100 4863",null,null,null,null,40,null,null,"Fog Nozzle 13-60","1702",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"bmpr4866","BLACK (Std)","ORANGE","YELLOW","RED","BLUE","GREEN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4863,150,50,"Fog Nozzle 150 @ 50",null,null,null,"Fog Tip 200 @ 75",4824,4866,null,"Fog Tip 210 @ 50 4824",null,null,null,null,"Fog Tip 161 @ 50 4866",null,null,null,null,null,null,"Fog Tip 161 @ 50",4866,null,null,""]
[null,null,null,"Fog Tip 125","175 100 (Std)",null,null,null,"Fog Nozzle 200 @ 75 4826",null,null,null,null,60,null,null,"Fog Tip 13-60","1703",37,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4863,161,50,"Fog Nozzle 161 @ 50",null,null,null,"Fog Tip 210 @ 50",4824,null,null,"Fog Tip 225 @ 100 4866",null,null,null,null,"Fog Tip 175 @ 100 4866",null,null,null,null,null,null,"Fog Tip 175 @ 100",4866,null,null,""]
[null,null,null,"Fog Tip 150","175 75",null,null,null,"Fog Nozzle 200 @ 75 4863",null,null,null,null,95,null,null,"Fog Nozzle 18-30","1704",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4863,175,50,"Fog Nozzle 175 @ 50",null,null,null,"Fog Tip 225 @ 100",4866,null,null,"Fog Tip 250 @ 100 4824",null,null,null,null,"Fog Tip 175 @ 50 4866",null,null,null,null,null,null,"Fog Tip 175 @ 50",4866,null,null,""]
[null,null,null,"Fog Tip 161","175 50",null,null,null,"Fog Nozzle 200 @ 50 4863",null,null,null,null,125,null,null,"Fog Nozzle 13-30","1704",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4863,185,50,"Fog Nozzle 185 @ 50",null,null,null,"Fog Tip 250 @ 100",4824,null,null,"Fog Tip 250 @ 50 4824",null,null,null,null,"Fog Tip 175 @ 75 4866",null,null,null,null,null,null,"Fog Tip 175 @ 75",4866,null,null,""]
[null,null,null,"Fog Tip 175","185 50",null,null,null,"Fog Nozzle 200 @ 50 4826",null,null,null,null,150,null,null,"Fog Tip 18-30","1711",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4863,225,"100 (Std)","Fog Nozzle 225 @ 100 (Std)",null,null,null,"Fog Tip 250 @ 50",4824,null,null,"Fog Tip 250 @ 75 4824",null,null,null,null,"Fog Tip 185 @ 50 4866",null,null,null,null,null,null,"Fog Tip 185 @ 50",4866,null,null,""]
[null,null,null,"Fog Tip 185","200 100 (Std)",null,null,null,"Fog Nozzle 210 @ 50 4826",null,null,null,null,161,null,null,"Fog Tip 13-30","1711",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip",4866,95,"100 (Std)","Fog Tip 95 @ 100 (Std)",null,null,null,"Fog Tip 250 @ 75",4824,null,null,"Fog Tip 265 @ 50 4824",null,null,null,null,"Fog Tip 200 @ 100 4824",null,null,null,null,null,null,"Fog Tip 200 @ 100",4824,null,null,""]
[null,null,null,"Fog Tip 200","200 75",null,null,null,"Fog Nozzle 225 @ 100 4863",null,null,null,null,175,null,null,"Fog Tip 30-125","1714",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip",4866,125,"100 (Std)","Fog Tip 125 @ 100 (Std)",null,null,null,"Fog Tip 265 @ 50",4824,null,null,"Fog Tip 300 @ 100 4824",null,null,null,null,"Fog Tip 200 @ 100 4866",null,null,null,null,null,null,"Fog Tip 200 @ 75",4824,null,null,""]
[null,null,null,"Fog Tip 210","200 50",null,null,null,"Fog Nozzle 25 @ 100 4802",null,null,null,null,185,null,null,"Fog Nozzle 30-125","1720",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip",4866,150,"100 (Std)","Fog Tip 150 @ 100 (Std)",null,null,null,"Fog Tip 300 @ 100",4824,null,null,"Fog Tip 300 @ 75 4824",null,null,null,null,"Fog Tip 200 @ 75 4824",null,null,null,null,null,null,"Fog Tip 200 @ 100",4866,null,null,""]
[null,null,null,"Fog Tip 225","210 50",null,null,null,"Fog Nozzle 250 @ 100 4826",null,null,null,null,200,null,null,"Fog Nozzle 95-200","1723",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip",4866,175,"100 (Std)","Fog Tip 175 @ 100 (Std)",null,null,null,"Fog Tip 300 @ 75",4824,null,null,"Fog Tip 350 @ 100 4824",null,null,null,null,"Fog Tip 200 @ 75 4866",null,null,null,null,null,null,"Fog Tip 200 @ 75",4866,null,null,""]
[null,null,null,"Fog Tip 250","225 100 (Std)",null,null,null,"Fog Nozzle 250 @ 50 4826",null,null,null,null,210,null,null,"Fog Nozzle 125-250","1733",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip",4866,200,"100 (Std)","Fog Tip 200 @ 100 (Std)",null,null,null,"Fog Tip 350 @ 100",4824,null,null,"Fog Tip 95 @ 100 4866",null,null,null,null,"Fog Tip 210 @ 50 4824",null,null,null,null,null,null,"Fog Tip 210 @ 50",4824,null,null,""]
[null,null,null,"Fog Tip 265","250 100 (Std)",null,null,null,"Fog Nozzle 250 @ 75 4826",null,null,null,null,225,null,null,"Fog Tip 95-200","1737",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip",4866,125,75,"Fog Tip 125 @ 75",null,null,null,"Fog Tip 95 @ 100",4866,null,null,null,null,null,null,null,"Fog Tip 225 @ 100 4866",null,null,null,null,null,null,"Fog Tip 225 @ 100",4866,null,null,""]
[null,null,null,"Fog Tip 300","250 75",null,null,null,"Fog Nozzle 265 @ 50 4826",null,null,null,null,250,null,null,"Fog Tip 125-250","1744",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip",4866,150,75,"Fog Tip 150 @ 75",null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip 250 @ 100 4824",null,null,null,null,null,null,"Fog Tip 250 @ 100",4824,null,null,""]
[null,null,null,"Fog Tip 350","250 50",null,null,null,"Fog Nozzle 300 @ 100 4826",null,null,null,null,300,null,null,"Fog Nozzle 30-200","1763",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip",4866,175,75,"Fog Tip 175 @ 75",null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip 250 @ 50 4824",null,null,null,null,null,null,"Fog Tip 250 @ 50",4824,null,null,""]
[null,null,null,null,"265 50",null,null,null,"Fog Nozzle 300 @ 75 4826",null,null,null,null,350,null,null,"Fog Tip 30-200","1766",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip",4866,200,75,"Fog Tip 200 @ 75",null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip 250 @ 75 4824",null,null,null,null,null,null,"Fog Tip 250 @ 75",4824,null,null,""]
[null,null,null,null,"300 100 (Std)",null,null,null,"Fog Nozzle 350 @ 100 4826",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip",4866,150,50,"Fog Tip 150 @ 50",null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip 265 @ 50 4824",null,null,null,null,null,null,"Fog Tip 265 @ 50",4824,null,null,""]
[null,null,null,null,"300 75",null,null,null,"Fog Nozzle 40 @ 100 4802",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip",4866,161,50,"Fog Tip 161 @ 50",null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip 300 @ 100 4824",null,null,null,null,null,null,"Fog Tip 300 @ 100",4824,null,null,""]
[null,null,null,null,"350 100 (Std)",null,null,null,"Fog Nozzle 60 @ 100 4116",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip",4866,175,50,"Fog Tip 175 @ 50",null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip 300 @ 75 4824",null,null,null,null,null,null,"Fog Tip 300 @ 75",4824,null,null,""]
[null,null,null,null,null,null,null,null,"Fog Nozzle 60 @ 75 4116",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip",4866,185,50,"Fog Tip 185 @ 50",null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip 350 @ 100 4824",null,null,null,null,null,null,"Fog Tip 350 @ 100",4824,null,null,""]
[null,null,null,null,null,null,null,null,"Fog Nozzle 60 @ 87 4116",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip",4866,225,"100 (Std)","Fog Tip 225 @ 100 (Std)",null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip 95 @ 100 4866",null,null,null,null,null,null,"Fog Tip 95 @ 100",4866,null,null,""]
[null,null,null,null,null,null,null,null,"Fog Nozzle 95 @ 100 4116",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,"Fog Nozzle 95 @ 100 4863",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,"Fog Nozzle 95 @ 75 4116",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,"Fog Nozzle 95 @ 87 4116",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"TRIM(CS68)","v":""}]
[null,null,null,null,null,null,null,null,"Fog Tip 125 @ 100 4866",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,"Fog Tip 125 @ 75 4866",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,"Fog Tip 150 @ 100 4866",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,"Fog Tip 150 @ 50 4866",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,"Fog Tip 150 @ 75 4866",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,"Fog Tip 161 @ 50 4866",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,"Fog Tip 175 @ 100 4866",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,"Fog Tip 175 @ 50 4866",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,"Fog Tip 175 @ 75 4866",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,"Fog Tip 185 @ 50 4866",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,"Fog Tip 200 @ 100 4824",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,""]
[null,null,null,null,null,null,null,null,"Fog Tip 200 @ 100 4866",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,118,"118",{"$f":"ROUND(0.0505*$CT80*SQRT(CU$2),0)","v":42}]
[null,null,null,null,null,null,null,null,"Fog Tip 200 @ 75 4824",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,161,"161",{"$f":"ROUND(0.0505*$CT81*SQRT(CU$2),0)","v":57}]
[null,null,null,null,null,null,null,null,"Fog Tip 200 @ 75 4866",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,210,"210",{"$f":"ROUND(0.0505*$CT82*SQRT(CU$2),0)","v":75}]
[null,null,null,null,null,null,null,null,"Fog Tip 210 @ 50 4824",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,185,"185",{"$f":"ROUND(0.0505*$CT83*SQRT(CU$2),0)","v":66}]
[null,null,null,null,null,null,null,null,"Fog Tip 225 @ 100 4866"]
[null,null,null,null,null,null,null,null,"Fog Tip 250 @ 100 4824"]
[null,null,null,null,null,null,null,null,"Fog Tip 250 @ 50 4824"]
[null,null,null,null,null,null,null,null,"Fog Tip 250 @ 75 4824"]
[null,null,null,null,null,null,null,null,"Fog Tip 265 @ 50 4824"]
[null,null,null,null,null,null,null,null,"Fog Tip 300 @ 100 4824"]
[null,null,null,null,null,null,null,null,"Fog Tip 300 @ 75 4824"]
[null,null,null,null,null,null,null,null,"Fog Tip 350 @ 100 4824"]
[null,null,null,null,null,null,null,null,"Fog Tip 95 @ 100 4866"]

{"sheet":"SolidBoreAndStackTips","index":3,"n_rows":84,"n_cols":164,"rows_kept":84,"cut":false,"hidden":false,"merged":[[7,1,8,1],[7,2,8,2],[7,3,8,3],[13,1,14,1],[13,2,14,6],[10,2,10,3],[11,5,11,6],[12,2,12,6],[7,10,8,10],[11,7,12,9],[11,10,12,10],[7,4,8,4],[7,5,8,5],[7,6,8,6],[11,3,11,4],[6,3,6,7],[15,2,17,10],[0,7,5,7],[0,8,1,10],[1,1,1,5],[2,1,2,5],[2,8,3,10],[3,1,3,5],[4,1,4,5],[4,8,5,10],[5,1,5,5],[13,7,14,7],[13,8,14,10],[7,7,8,7],[7,8,8,8],[7,9,8,9]]}
[null,"Instructions:",null,null,null,null,null,"Reaction Force Color Chart (For Stack Tips RF is for Base Tip only):","This is a Low RF Nozzle (RF < 51 )",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"asdf",null,null,"Style","Flow",null,"Flow",null,null,null,null,null,null,100,75,50,87,null,null,"Bore Size","Style",null,null,null,"Flow",null,null,null,"Flow","Pressure",null,null,null,null,null,null,null,"Style","Flow","Pressure",null,null,null,null,null,"Style",null,null,null,null,null,null,null,null,null,null,null,null,"Bore Size",null,null,null,null,null,null,"Bore Size",null,null,null,null,"Bore Size",null,"Bore,Shutoff,Inlet,Remove Grip",null,null,"Bore Size","Style","Inlet","Dec Size","Shutoff","Remove PG",null,"Bore Size","Dec Size",null,"Solid Bore No 1.5 in","Solid Bore No 2.5 in","Solid Bore Yes 1.5 in","Solid Bore Yes 2.5 in","Stack Tips No 1.5 in","Stack Tips No 2.5 in","Stack Tips Yes 1.5 in","Stack Tips Yes 2.5 in",null,null,"Bore,Shutoff,Inlet,Remove Grip","Style",null,null,null,"Bore Size","Bore Size",null,null,"Bore Size","Style","Inlet","Dec Size","Shutoff",null,null,null,null,null,null,null,null,50,null,null,"Bore Size","Style",null,null,null,null,null,null,{"$f":"CONCATENATE(B10,E10,\"0439\")","v":"Solid Bore1-3/8\"0439"}]
[null,"Tan-colored cells are headers or describe the selection options",null,null,null,null,null,null,null,null,null,null,"Nozzle",null,"Fog Nozzle","Fog Tip",null,"5-40","125-250","13-30","13-60","18-30","30-125","30-150","30-200","95-200","12-53",null,null,null,null,null,null,null,null,null,"4116",60,null,13,"100 (Std)",null,null,null,null,4116,60,60,null,60,null,"Solid Bore","3/4\"","0416","1.5 in",0.75,"Fog Nozzle",13,"Fog Nozzle 13",null,null,13,"100 (Std)",{"$f":"CONCATENATE(BJ2,\" \",BK2)","v":"13 100 (Std)"},null,200,"100 (Std)",null,null,"Fog Nozzle",4116,60,"100 (Std)",{"$f":"CONCATENATE(BR2,\" \",BT2,\" @ \",BU2)","v":"Fog Nozzle 60 @ 100 (Std)"},null,null,null,"Fog Nozzle 125 @ 100",4116,4863,null,{"$f":"CONCATENATE($BZ2,\" \",CA2)","v":"Fog Nozzle 125 @ 100 4116"},{"$f":"CONCATENATE($BZ2,\" \",CB2)","v":"Fog Nozzle 125 @ 100 4863"},"Fog_Nozzle_125___100",null,null,"Fog Nozzle 125 @ 100 4116",null,null,null,"Solid Bore","3/8\"",0.375,{"$f":"CONCATENATE(CM2,\" \",CN2)","v":"Solid Bore 3/8\""},null,null,null,"Solid Bore 1.5 in","3/4\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 1.5 in","3/4\"",null,{"$f":"CONCATENATE(DD2,\" \",DI2,\" \",DG2,\" \",DE2,\" \",DJ2)","v":"Solid Bore No 1.5 in 3/4\" Yes"},{"$f":"CONCATENATE(DD2,\" \",DI2,\" \",DG2)","v":"Solid Bore No 1.5 in"},"Solid Bore","3/4\"","0416","1.5 in",0.75,"No","Yes","Solid Bore No 1.5 in",null,0.375,null,"3/8\"","7/8\"","1/2\"","7/8\"","1-1/8\"; 1/2\"","1-1/2\"; 1-1/4\"; 1\"","15/16\"; 1/2\"","1-1/8\"; 1/2\"",null,null,"Solid Bore No 1.5 in 1\" Yes","0416","1417","1499",null,"3/4\"","3_4_",null,"Solid Bore","3/4\"","0416","1.5 in",0.75,"No",{"$f":"CONCATENATE(EG2,\" \",EJ2,\" \",EL2,\" \",EH2,\" \",EI2)","v":"Solid Bore 1.5 in No 3/4\" 0416"},null,"Solid Bore 1.5 in No 3/4\" 0416",null,null,null,0.375,"3/8\"",{"$f":"CONCATENATE(ROUND(29.71*(ES2*ES2)*SQRT(EU$1),0),\" gpm @ 50 psi; RF = \",ROUND(1.57*(ES2*ES2)*EU$1,0))","v":"30 gpm @ 50 psi; RF = 11"},null,"Solid Bore","3/4\"","0416",{"$f":"_xlfn.CONCAT(EW2:EY2)","v":"Solid Bore3/4\"0416"},null,"Solid Bore3/4\"0416",null,null,{"$f":"VLOOKUP(FF7,E25:E88,1,FALSE)","v":"Stack Tips15/16\"; 1/2\"1440"},"Stack Tips15/16\"; 1/2\"0439"]
[null,"Use the green-colored cells to make your selections (All cells must be filled in; information from \"FrontPage\" tab does not carry over to this page)",null,null,null,null,null,null,"This is a Nozzle with Increased RF (RF > 50 and <101 )",null,null,null,"Tip",null,"1 in","1.5 in",null,"100 (Std)","100 (Std)","100 (Std)","100 (Std)","100 (Std)","100 (Std)","100 (Std)","100 (Std)","100 (Std)","87 (CE)",null,null,null,null,null,null,null,null,null,"4116",95,null,25,"100 (Std)",null,null,null,null,4116,95,95,null,95,null,"Solid Bore","7/8\"","0416","1.5 in",0.875,"Fog Nozzle",25,"Fog Nozzle 25",null,null,25,"100 (Std)",{"$f":"CONCATENATE(BJ3,\" \",BK3)","v":"25 100 (Std)"},null,250,"100 (Std)",null,null,"Fog Nozzle",4116,60,75,{"$f":"CONCATENATE(BR3,\" \",BT3,\" @ \",BU3)","v":"Fog Nozzle 60 @ 75"},null,null,null,"Fog Nozzle 125 @ 75",4116,4863,null,{"$f":"CONCATENATE($BZ3,\" \",CA3)","v":"Fog Nozzle 125 @ 75 4116"},{"$f":"CONCATENATE($BZ3,\" \",CB3)","v":"Fog Nozzle 125 @ 75 4863"},null,null,null,"Fog Nozzle 125 @ 100 4863",null,null,null,"Solid Bore","1/2\"",0.5,{"$f":"CONCATENATE(CM3,\" \",CN3)","v":"Solid Bore 1/2\""},null,null,null,"Solid Bore 1.5 in","7/8\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 1.5 in","7/8\"",null,{"$f":"CONCATENATE(DD3,\" \",DI3,\" \",DG3,\" \",DE3,\" \",DJ3)","v":"Solid Bore No 1.5 in 7/8\" Yes"},{"$f":"CONCATENATE(DD3,\" \",DI3,\" \",DG3)","v":"Solid Bore No 1.5 in"},"Solid Bore","7/8\"","0416","1.5 in",0.875,"No","Yes","Solid Bore No 1.5 in",null,0.5,null,"1/2\"","15/16\"","7/8\"","15/16\"","15/16\"; 1/2\"","1-1/4\"; 1-1/8\"; 1\"",null,"1-1/4\"; 1-1/8\"; 1\"",null,null,"Solid Bore No 1.5 in 1/2\" Yes","1417",null,null,null,"7/8\"","7_8_",null,"Solid Bore","7/8\"","0416","1.5 in",0.875,"No",{"$f":"CONCATENATE(EG3,\" \",EJ3,\" \",EL3,\" \",EH3,\" \",EI3)","v":"Solid Bore 1.5 in No 7/8\" 0416"},null,"Solid Bore 1.5 in No 7/8\" 0416",null,null,null,0.5,"1/2\"","53 gpm @ 50 psi; RF = 20",null,"Solid Bore","7/8\"","0416",{"$f":"_xlfn.CONCAT(EW3:EY3)","v":"Solid Bore7/8\"0416"},null,"Solid Bore7/8\"0416",null,null,null,{"$f":"FF2=FF1","v":false}]
[null,"Blue-colored cells provide outputs based on your selections",null,null,null,null,null,null,null,null,null,null,"High Pressure",null,"1.5 in",null,null,75,75,null,null,null,75,75,75,75,null,null,null,null,null,null,null,null,null,null,"4116",125,null,40,"100 (Std)",null,null,null,null,4116,125,125,null,125,null,"Solid Bore","1\"","0416","1.5 in",1,"Fog Nozzle",40,"Fog Nozzle 40",null,null,40,"100 (Std)","40 100 (Std)",null,300,"100 (Std)",null,null,"Fog Nozzle",4116,60,"87 (CE)","Fog Nozzle 60 @ 87 (CE)",null,null,null,"Fog Nozzle 125 @ 87",4116,null,null,{"$f":"CONCATENATE($BZ4,\" \",CA4)","v":"Fog Nozzle 125 @ 87 4116"},null,null,null,null,"Fog Nozzle 125 @ 75 4116",null,null,null,"Solid Bore","5/8\"",0.625,"Solid Bore 5/8\"",null,null,null,"Solid Bore 1.5 in","1\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 1.5 in","1\"",null,"Solid Bore No 1.5 in 1\" Yes","Solid Bore No 1.5 in","Solid Bore","1\"","0416","1.5 in",1,"No","Yes","Solid Bore No 1.5 in",null,0.625,null,"5/8\"","1\"","15/16\"","1\"","1-1/16\"; 15/16\"","1-3/8\"; 1-1/4\"; 1\"",null,null,null,null,"Solid Bore No 1.5 in 1-1/16\" Yes","1499",null,null,null,"1\"","1_",null,"Solid Bore","1\"","0416","1.5 in",1,"No","Solid Bore 1.5 in No 1\" 0416",null,"Solid Bore 1.5 in No 1\" 0416",null,null,null,0.625,"5/8\"","82 gpm @ 50 psi; RF = 31",null,"Solid Bore","1\"","0416","Solid Bore1\"0416",null,"Solid Bore1\"0416",null,null,null,"Stack Tips15/16\"; 1/2\"0439"]
[null,"This shaded cell indicates an error has ocurred and you may need to modify some of your selections or contact our Customer Care team",null,null,null,null,null,null,"This Nozzle has a High RF (RF > 100 )",null,null,null,null,null,"2 in",null,null,"87 (CE)",null,null,null,null,"87 (CE)","87 (CE)",null,null,null,null,null,"5-40","100 (Std)",{"$f":"CONCATENATE(AD5,\" \",AE5)","v":"5-40 100 (Std)"},null,null,null,null,"4116",150,null,60,"100 (Std)",75,"87 (CE)",null,null,4116,150,150,null,150,null,"Solid Bore","1-1/8\"","0416","1.5 in",1.125,"Fog Nozzle",60,"Fog Nozzle 60",null,null,60,"100 (Std)","60 100 (Std)",null,350,"100 (Std)",null,null,"Fog Nozzle",4116,95,"100 (Std)","Fog Nozzle 95 @ 100 (Std)",null,null,null,"Fog Nozzle 13 @ 100",4802,null,null,{"$f":"CONCATENATE($BZ5,\" \",CA5)","v":"Fog Nozzle 13 @ 100 4802"},null,null,null,null,"Fog Nozzle 125 @ 75 4863",null,null,null,"Solid Bore","3/4\"",0.75,"Solid Bore 3/4\"",null,null,null,"Solid Bore 1.5 in","1-1/8\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 1.5 in","1-1/8\"",null,"Solid Bore No 1.5 in 1-1/8\" Yes","Solid Bore No 1.5 in","Solid Bore","1-1/8\"","0416","1.5 in",1.125,"No","Yes","Solid Bore No 1.5 in",null,0.75,null,"3/4\"","1-1/8\"","1\"","1-1/16\"","1-1/4\"; 1-1/8\"; 1\"",null,null,null,null,null,"Solid Bore No 1.5 in 1-1/4\" Yes","0416","1417","1499",null,"1-1/8\"","1_1_8_",null,"Solid Bore","1-1/8\"","0416","1.5 in",1.125,"No","Solid Bore 1.5 in No 1-1/8\" 0416",null,"Solid Bore 1.5 in No 1-1/8\" 0416",null,null,null,0.75,"3/4\"","118 gpm @ 50 psi; RF = 44",null,"Solid Bore","1-1/8\"","0416","Solid Bore1-1/8\"0416",null,"Solid Bore1-1/8\"0416"]
[null,"Orange-colored cell allows you to input your discount for Net Price",null,null,null,null,null,null,null,null,null,null,null,null,"2.5 in",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5-40",75,{"$f":"CONCATENATE(AD6,\" \",AE6)","v":"5-40 75"},null,null,null,null,"4802",13,null,95,"100 (Std)",75,"87 (CE)",null,null,4802,13,null,null,null,null,"Solid Bore","1-1/4\"","0416","1.5 in",1.25,"Fog Nozzle",95,"Fog Nozzle 95",null,null,60,"87 (CE)","60 87 (CE)",null,200,75,null,null,"Fog Nozzle",4116,95,75,"Fog Nozzle 95 @ 75",null,null,null,"Fog Nozzle 150 @ 100",4116,4863,null,"Fog Nozzle 150 @ 100 4116",{"$f":"CONCATENATE($BZ6,\" \",CB6)","v":"Fog Nozzle 150 @ 100 4863"},null,null,null,"Fog Nozzle 125 @ 87 4116",null,null,null,"Solid Bore","7/8\"",0.875,"Solid Bore 7/8\"",null,null,null,"Solid Bore 1.5 in","1-1/4\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 1.5 in","1-1/4\"",null,"Solid Bore No 1.5 in 1-1/4\" Yes","Solid Bore No 1.5 in","Solid Bore","1-1/4\"","0416","1.5 in",1.25,"No","Yes","Solid Bore No 1.5 in",null,0.875,null,"7/8\"","1-1/4\"","1-1/16\"","1-1/8\"",null,null,null,null,null,null,"Solid Bore No 1.5 in 1-1/8\" Yes","0416","1417","1499",null,"1-1/4\"","1_1_4_",null,"Solid Bore","1-1/4\"","0416","1.5 in",1.25,"No","Solid Bore 1.5 in No 1-1/4\" 0416",null,"Solid Bore 1.5 in No 1-1/4\" 0416",null,null,null,0.875,"7/8\"","161 gpm @ 50 psi; RF = 60",null,"Solid Bore","1-1/4\"","0416","Solid Bore1-1/4\"0416",null,"Solid Bore1-1/4\"0416",null,null,null,"Stack Tips15/16\"; 1/2\"1440"]
[null,{"$f":"FrontPage!E8","v":"Rev Date: 6/27/2022"},null,"Solid Bore Straight and Stack Tips",null,null,null,null,null,null,null,null,null,null,"3 in",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5-40","87 (CE)","5-40 87 (CE)",null,null,null,null,"4802",25,null,125,"100 (Std)",75,50,"87 (CE)",null,4802,25,null,null,null,null,"Solid Bore","3/8\"","1417","1.5 in",0.375,"Fog Nozzle",125,"Fog Nozzle 125",null,null,60,75,"60 75",null,250,75,null,null,"Fog Nozzle",4116,95,"87 (CE)","Fog Nozzle 95 @ 87 (CE)",null,null,null,"Fog Nozzle 150 @ 50",4863,null,null,"Fog Nozzle 150 @ 50 4863",null,null,null,null,"Fog Nozzle 13 @ 100 4802",null,null,null,"Solid Bore","15/16\"",0.9375,"Solid Bore 15/16\"",null,null,null,"Solid Bore 1.5 in","3/8\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 1.5 in","3/8\"",null,"Solid Bore No 1.5 in 3/8\" Yes","Solid Bore No 1.5 in","Solid Bore","3/8\"","1417","1.5 in",0.375,"No","Yes","Solid Bore No 1.5 in",null,0.9375,null,"15/16\"","1-3/8\"","1-1/8\"","1-3/16\"",null,null,null,null,null,null,"Solid Bore No 1.5 in 1-3/16\" Yes","1499",null,null,null,"3/8\"","3_8_",null,"Solid Bore","3/8\"","1417","1.5 in",0.375,"No","Solid Bore 1.5 in No 3/8\" 1417",null,"Solid Bore 1.5 in No 3/8\" 1417",null,null,null,0.9375,"15/16\"","185 gpm @ 50 psi; RF = 69",null,"Solid Bore","3/8\"","1417","Solid Bore3/8\"1417",null,"Solid Bore3/8\"1417",null,null,null,"Stack Tips15/16\"; 1/2\"1440"]
[null,"Solid Bore or Stack Tips","Inlet Size","Include Shutoff?",{"$f":"IF(LEFT(B10,5)=\"Stack\", \"Bore Sizes\",\"Bore Size\")","v":"Bore Size"},"Inlet Thread",{"$f":"IF(OR(D10=\"Yes\",TRIM(I10)=\"0416\",B10=\"stACK TIPS\"),\"Outlet Thread\",\"\")","v":""},{"$f":"IF(D10=\"Yes\",IF(J10=\"yes\",\"\",\"Remove Pistol Grip?\"),\"\")","v":""},"Style Number",{"$f":"IF(D10=\"Yes\",IF(TRIM(I10)=\"2393\",\"\",\"ZT Inlet?\"),\"\")","v":""},"Custom Etch",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"125-250","100 (Std)","125-250 100 (Std)",null,null,null,null,"4802",40,null,150,"100 (Std)",75,50,"87 (CE)",null,4802,40,null,null,null,null,"Solid Bore","1/2\"","1417","1.5 in",0.5,"Fog Nozzle",150,"Fog Nozzle 150",null,null,95,"100 (Std)","95 100 (Std)",null,300,75,null,null,"Fog Nozzle",4116,125,"100 (Std)","Fog Nozzle 125 @ 100 (Std)",null,null,null,"Fog Nozzle 150 @ 75",4116,4863,null,"Fog Nozzle 150 @ 75 4116",{"$f":"CONCATENATE($BZ8,\" \",CB8)","v":"Fog Nozzle 150 @ 75 4863"},null,null,null,"Fog Nozzle 150 @ 100 4116",null,null,null,"Solid Bore","1\"",1,"Solid Bore 1\"",null,null,null,"Solid Bore 1.5 in","1/2\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 1.5 in","1/2\"",null,"Solid Bore No 1.5 in 1/2\" Yes","Solid Bore No 1.5 in","Solid Bore","1/2\"","1417","1.5 in",0.5,"No","Yes","Solid Bore No 1.5 in",null,1,null,"1\"",null,"1-3/16\"","1-1/4\"",null,null,null,null,null,null,"Solid Bore No 1.5 in 1-3/8\" Yes","1499",null,null,null,"1/2\"","1_2_",null,"Solid Bore","1/2\"","1417","1.5 in",0.5,"No","Solid Bore 1.5 in No 1/2\" 1417",null,"Solid Bore 1.5 in No 1/2\" 1417",null,null,null,1,"1\"","210 gpm @ 50 psi; RF = 79",null,"Solid Bore","1/2\"","1417","Solid Bore1/2\"1417",null,"Solid Bore1/2\"1417"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore","Stack Tips",null,null,null,null,null,null,null,null,null,null,null,null,null,"125-250",75,"125-250 75",null,null,null,null,"4824",200,null,161,50,null,null,null,null,4824,200,200,null,null,null,"Solid Bore","5/8\"","1417","1.5 in",0.625,"Fog Nozzle",161,"Fog Nozzle 161",null,null,95,75,"95 75",null,210,50,null,null,"Fog Nozzle",4116,125,75,"Fog Nozzle 125 @ 75",null,null,null,"Fog Nozzle 150 @ 87",4116,null,null,"Fog Nozzle 150 @ 87 4116",null,null,null,null,"Fog Nozzle 150 @ 100 4863",null,null,null,"Solid Bore","1-1/16\"",1.0625,"Solid Bore 1-1/16\"",null,null,null,"Solid Bore 1.5 in","5/8\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 1.5 in","5/8\"",null,"Solid Bore No 1.5 in 5/8\" Yes","Solid Bore No 1.5 in","Solid Bore","5/8\"","1417","1.5 in",0.625,"No","Yes","Solid Bore No 1.5 in",null,1.0625,null,"1-1/16\"",null,"1-1/4\"","1-3/8\"",null,null,null,null,null,null,"Solid Bore No 1.5 in 15/16\" Yes","1417","1499",null,null,"5/8\"","5_8_",null,"Solid Bore","5/8\"","1417","1.5 in",0.625,"No","Solid Bore 1.5 in No 5/8\" 1417",null,"Solid Bore 1.5 in No 5/8\" 1417",null,null,null,1.0625,"1-1/16\"","237 gpm @ 50 psi; RF = 89",null,"Solid Bore","5/8\"","1417","Solid Bore5/8\"1417",null,"Solid Bore5/8\"1417"]
[null,"Solid Bore","2.5 in","No","1-3/8\"","NH","NH","No (Std)","0489","No (Std)","No (Std)",null,null,null,"1.5 in","1.5 in",null,null,null,null,null,null,null,"INDIRECT(CONCATENATE(\"tHREAD\",SUBSTITUTE(B4,\" \",\"_\")))",null,null,null,null,null,"13-30","100 (Std)","13-30 100 (Std)",null,null,null,null,"4824",210,null,175,"100 (Std)",75,50,null,null,4824,null,null,210,null,null,"Solid Bore","3/4\"","1417","1.5 in",0.75,"Fog Nozzle",175,"Fog Nozzle 175",null,null,95,"87 (CE)","95 87 (CE)",null,250,50,null,null,"Fog Nozzle",4116,125,"87 (CE)","Fog Nozzle 125 @ 87 (CE)",null,null,null,"Fog Nozzle 161 @ 50",4863,null,null,"Fog Nozzle 161 @ 50 4863",null,null,null,null,"Fog Nozzle 150 @ 50 4863",null,null,null,"Solid Bore","1-1/8\"",1.125,"Solid Bore 1-1/8\"",null,null,null,"Solid Bore 1.5 in","3/4\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 1.5 in","15/16\"",null,"Solid Bore No 1.5 in 3/4\" Yes","Solid Bore No 1.5 in","Solid Bore","3/4\"","1417","1.5 in",0.75,"No","Yes","Solid Bore No 1.5 in",null,1.125,null,"1-1/8\"",null,"1-3/8\"",null,null,null,null,null,null,null,"Solid Bore No 1.5 in 3/4\" Yes","0416","1417",null,null,"3/4\"","3_4_",null,"Solid Bore","3/4\"","1417","1.5 in",0.75,"No","Solid Bore 1.5 in No 3/4\" 1417",null,"Solid Bore 1.5 in No 3/4\" 1417",null,null,null,1.125,"1-1/8\"","266 gpm @ 50 psi; RF = 99",null,"Solid Bore","3/4\"","1417","Solid Bore3/4\"1417",null,"Solid Bore3/4\"1417"]
[null,"List price",{"$f":"SUM(E11:K11)","v":546},null,{"$f":"IFERROR(VLOOKUP(E10,ET:EU,2,FALSE),\"Fix Bore Size\")","v":"397 gpm @ 50 psi; RF = 148"},{"$f":"IF(OR(F10=\"Storz\",F10=\"BIM\"),_xlfn.XLOOKUP(\"Storz\",AO:AO,AP:AP),0)","v":0},null,null,{"$f":"IFERROR(VLOOKUP(TRIM(I10),AO39:AP53,2,FALSE),\"\")","v":546},{"$f":"IF(J8=\"\",0,IF(J10=\"Yes\",_xlfn.XLOOKUP(\"ZT\",AO:AO,AP:AP),0))","v":0},null,null,null,null,"2.5 in","2.5 in",null,null,null,null,null,null,null,null,null,null,null,null,null,"13-60","100 (Std)","13-60 100 (Std)",null,null,null,null,"4824",250,null,185,50,null,null,null,null,4824,250,250,250,null,null,"Solid Bore","7/8\"","1417","1.5 in",0.875,"Fog Nozzle",200,"Fog Nozzle 200",null,null,125,"100 (Std)","125 100 (Std)",null,null,null,null,null,"Fog Nozzle",4116,150,"100 (Std)","Fog Nozzle 150 @ 100 (Std)",null,null,null,"Fog Nozzle 175 @ 100",4863,null,null,"Fog Nozzle 175 @ 100 4863",null,null,null,null,"Fog Nozzle 150 @ 75 4116",null,null,null,"Solid Bore","1-3/16\"",1.1875,"Solid Bore 1-3/16\"",null,null,null,"Solid Bore 1.5 in","7/8\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 1.5 in","1-1/16\"",null,"Solid Bore No 1.5 in 7/8\" Yes","Solid Bore No 1.5 in","Solid Bore","7/8\"","1417","1.5 in",0.875,"No","Yes","Solid Bore No 1.5 in",null,1.1875,null,"1-3/16\"",null,null,null,null,null,null,null,null,null,"Solid Bore No 1.5 in 3/8\" Yes","1417",null,null,null,"7/8\"","7_8_",null,"Solid Bore","7/8\"","1417","1.5 in",0.875,"No","Solid Bore 1.5 in No 7/8\" 1417",null,"Solid Bore 1.5 in No 7/8\" 1417",null,null,null,1.1875,"1-3/16\"","296 gpm @ 50 psi; RF = 111",null,"Solid Bore","7/8\"","1417","Solid Bore7/8\"1417",null,"Solid Bore7/8\"1417"]
[null,"Your Discount",null,"Net Price",null,{"$f":"ROUND(C11*(1-C12),2)","v":546},null,{"$f":"IF(D10=\"YES\",\"Include Color Clips for Shutoff and/or Pistol Grip?\",\"\")","v":""},null,null,"Yes",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(B10,\" \",C10,\" \",D10,\" \",E10,\" \",I10)","v":"Solid Bore 2.5 in No 1-3/8\" 0489"},null,null,null,null,null,"18-30","100 (Std)","18-30 100 (Std)",null,null,null,null,"4824",265,null,200,"100 (Std)",75,null,null,null,4824,300,300,null,null,null,"Solid Bore","15/16\"","1417","1.5 in",0.9375,"Fog Nozzle",210,"Fog Nozzle 210",null,null,125,75,"125 75",null,null,null,null,null,"Fog Nozzle",4116,150,75,"Fog Nozzle 150 @ 75",null,null,null,"Fog Nozzle 175 @ 50",4863,null,null,"Fog Nozzle 175 @ 50 4863",null,null,null,null,"Fog Nozzle 150 @ 75 4863",null,null,null,"Solid Bore","1-1/4\"",1.25,"Solid Bore 1-1/4\"",null,null,null,"Solid Bore 1.5 in","15/16\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 1.5 in","1-3/16\"",null,"Solid Bore No 1.5 in 15/16\" Yes","Solid Bore No 1.5 in","Solid Bore","15/16\"","1417","1.5 in",0.9375,"No","Yes","Solid Bore No 1.5 in",null,1.25,null,"1-1/4\"",null,null,null,null,null,null,null,null,null,"Solid Bore No 1.5 in 5/8\" Yes","1417",null,null,null,"15/16\"","15_16_",null,"Solid Bore","15/16\"","1417","1.5 in",0.9375,"No","Solid Bore 1.5 in No 15/16\" 1417",null,"Solid Bore 1.5 in No 15/16\" 1417",null,null,null,1.25,"1-1/4\"","328 gpm @ 50 psi; RF = 123",null,"Solid Bore","15/16\"","1417","Solid Bore15/16\"1417",null,"Solid Bore15/16\"1417"]
[null,"Short Description",{"$f":"IF(B23=\"Error\",\"Fix Errors\",IF(OR(B10=P9,D10=\"yes\",TRIM(I10)=\"0416\"),CONCATENATE(I10,\" \",C10,\" \",F10,\" \",CONCATENATE(IF(TRIM(I10)=\"0439\",\"1 in \",\"1.5 in \"),G10),\" \",CONCATENATE(E10,\" bore size(s)\"),\" \",IF(D10=\"no\",\"\",IF(J10=\"yes\",\"PG\",IF(H10=\"yes\",\"NPG\",IF(I10=\"2393\",\" \",\"PG\")))),IF(B10=\"Fog Tip\",\"\",IF(D10=\"no\",\"\",IF(J10=\"Yes\",\" ZT\",\"\"))),IF(K10=\"Yes\",\" ETCH\",\"\")),CONCATENATE(I10,\" \",C10,\" \",F10,\" \",CONCATENATE(E10,\" bore size(s) \"),IF(K10=\"Yes\",\" ETCH\",\"\"))))","v":"0489 2.5 in NH 1-3/8\" bore size(s) "},null,null,null,null,null,null,null,null,null,"1 IN","NH",null,null,null,"1 in","1.5 in","2 in","2.5 in","3 in",null,null,null,null,null,null,null,"30-125","100 (Std)","30-125 100 (Std)",null,null,null,null,"4824",300,null,210,50,null,null,null,null,4824,350,null,null,null,null,"Solid Bore","1\"","1417","1.5 in",1,"Fog Nozzle",225,"Fog Nozzle 225",null,null,125,50,"125 50",null,null,null,null,null,"Fog Nozzle",4116,150,"87 (CE)","Fog Nozzle 150 @ 87 (CE)",null,null,null,"Fog Nozzle 175 @ 75",4863,null,null,"Fog Nozzle 175 @ 75 4863",null,null,null,null,"Fog Nozzle 150 @ 87 4116",null,null,null,"Solid Bore","1-3/8\"",1.375,"Solid Bore 1-3/8\"",null,null,null,"Solid Bore 1.5 in","1\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 1.5 in","1-3/8\"",null,"Solid Bore No 1.5 in 1\" Yes","Solid Bore No 1.5 in","Solid Bore","1\"","1417","1.5 in",1,"No","Yes","Solid Bore No 1.5 in",null,1.375,null,"1-3/8\"",null,null,null,null,null,null,null,null,null,"Solid Bore No 1.5 in 7/8\" Yes","0416","1417","1499",null,"1\"","1_",null,"Solid Bore","1\"","1417","1.5 in",1,"No","Solid Bore 1.5 in No 1\" 1417",null,"Solid Bore 1.5 in No 1\" 1417",null,null,null,1.375,"1-3/8\"","397 gpm @ 50 psi; RF = 148",null,"Solid Bore","1\"","1417","Solid Bore1\"1417",null,"Solid Bore1\"1417"]
[null,"Long Description",{"$f":"IF(B23=\"Error\",\"Some of your selections are not compatible with others; please correct the errors highlighted in RED\",CONCATENATE(\"Style \",I10,\" \",B10,IF(D10=\"yes\",\" including Shutoff with \",\" with \"),C10,\" \",F10,\" inlet; \",IF(G8>\"\",CONCATENATE(\"1.5 in \",G10,\" outlet; \"),\"\"),E10,IF(B10=\"Solid Bore\",CONCATENATE(\" bore size \",\"(\",E11,\")\"),CONCATENATE(\" bore sizes \",\"(\",E11,\" for Base Tip)\")),IF(J10=\"yes\",\"\",IF(D10=\"No\",\"\",IF(VLOOKUP(I10,M38:N45,2,FALSE)=\"no\",IF(I10=\"2393\",\"; playpipe with D-handles\",\"; no pistol grip\"),\"; pistol grip\"))),IF(D10=\"No\",\"\",IF(J10=\"Yes\",\"; Zero-Torque Grip\",\"\")),IF(K10=\"Yes\",\"; Custom Etched\",\"\")))","v":"Style 0489 Solid Bore with 2.5 in NH inlet; 1-3/8\" bore size (397 gpm @ 50 psi; RF = 148)"},null,null,null,null,"Akron Brass Part Number and Description",{"$f":"IF(AND(OR(F10=\"custom\",G10=\"custom\"),K10=\"yes\"),\"Contact Customer Care to request Custom Thread and Etch (800-228-1161)\",IF(OR(F10=\"custom\",G10=\"custom\"),\"Contact Customer Care to request Custom Thread (800-228-1161)\",IF(K10=\"Yes\",\"Contact Customer Care to request Custom Etch (800-228-1161)\",IF(B23=\"Error\",\"Incompatible selections; please correct errors highlighted in RED\",IFERROR(CONCATENATE(VLOOKUP(C13,DataSource!AH:AJ,2,FALSE),\"      \",VLOOKUP(C13,DataSource!AH:AJ,3,FALSE)),\"Version you've requested not yet created; contact Customer Care (800-228-1161)\")))))","v":"04890501      PLAIN DELUGE TIP 2.5NH 1 3/8D POLISH"},null,null,null,"1 IN","NPSH",null,null,"30-125",13,60,60,60,60,null,"Stack_Tips_Yes_2.5_in_1_1_4___ 1_1_8___ 1__No__Std",null,null,null,null,null,"30-125",75,"30-125 75",null,null,null,null,"4824",350,null,225,"100 (Std)",null,null,null,null,4826,200,200,null,null,null,"Solid Bore","1-1/8\"","1417","1.5 in",1.125,"Fog Nozzle",250,"Fog Nozzle 250",null,null,125,"87 (CE)","125 87 (CE)",null,null,null,null,null,"Fog Nozzle",4802,13,"100 (Std)","Fog Nozzle 13 @ 100 (Std)",null,null,null,"Fog Nozzle 185 @ 50",4863,null,null,"Fog Nozzle 185 @ 50 4863",null,null,null,null,"Fog Nozzle 161 @ 50 4863",null,null,null,"Stack Tips","1-1/8\"; 1/2\"",0.5,"Stack Tips 1-1/8\"; 1/2\"",null,null,null,"Solid Bore 1.5 in","1-1/8\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 2.5 in","7/8\"",null,"Solid Bore No 1.5 in 1-1/8\" Yes","Solid Bore No 1.5 in","Solid Bore","1-1/8\"","1417","1.5 in",1.125,"No","Yes","Solid Bore No 2.5 in",null,0.875,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore No 2.5 in 1\" Yes","0489",null,null,null,"1-1/8\"","1_1_8_",null,"Solid Bore","1-1/8\"","1417","1.5 in",1.125,"No","Solid Bore 1.5 in No 1-1/8\" 1417",null,"Solid Bore 1.5 in No 1-1/8\" 1417",null,null,null,1.0625,"1-1/16\"; 15/16\"","237 gpm @ 50 psi; RF = 89",null,"Solid Bore","1-1/8\"","1417","Solid Bore1-1/8\"1417",null,"Solid Bore1-1/8\"1417"]
[null,null,null,null,null,null,null,null,null,null,null,null,"1 IN","STORZ",null,null,"30-150",25,95,95,95,95,null,"Stack_Tips_Yes_2.5_in_1_1_4___1_1_8___1__No__Std",null,null,null,null,null,"30-125","87 (CE)","30-125 87 (CE)",null,null,null,null,"4826",200,null,250,"100 (Std)",75,50,null,null,4826,null,null,210,null,null,"Solid Bore","1-1/4\"","1417","1.5 in",1.25,"Fog Nozzle",265,"Fog Nozzle 265",null,null,150,"100 (Std)","150 100 (Std)",null,null,null,null,null,"Fog Nozzle",4802,25,"100 (Std)","Fog Nozzle 25 @ 100 (Std)",null,null,null,"Fog Nozzle 200 @ 100",4826,4863,null,"Fog Nozzle 200 @ 100 4826","Fog Nozzle 200 @ 100 4863",null,null,null,"Fog Nozzle 175 @ 100 4863",null,null,null,"Stack Tips","15/16\"; 1/2\"",0.5,"Stack Tips 15/16\"; 1/2\"",null,null,null,"Solid Bore 1.5 in","1-1/4\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 2.5 in","15/16\"",null,"Solid Bore No 1.5 in 1-1/4\" Yes","Solid Bore No 1.5 in","Solid Bore","1-1/4\"","1417","1.5 in",1.25,"No","Yes","Solid Bore No 2.5 in",null,0.9375,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore No 2.5 in 1-1/4\" Yes","0489",null,null,null,"1-1/4\"","1_1_4_",null,"Solid Bore","1-1/4\"","1417","1.5 in",1.25,"No","Solid Bore 1.5 in No 1-1/4\" 1417",null,"Solid Bore 1.5 in No 1-1/4\" 1417",null,null,null,1.5,"1-1/2\"; 1-1/4\"; 1\"","473 gpm @ 50 psi; RF = 177",null,"Solid Bore","1-1/4\"","1417","Solid Bore1-1/4\"1417",null,"Solid Bore1-1/4\"1417"]
[null,"Notes: ","You can make any notes about what you want, or anything else, in this space",null,null,null,null,null,null,null,null,null,"1.5 in",null,null,null,"30-200",40,125,125,125,125,null,null,null,null,null,null,null,"30-150","100 (Std)","30-150 100 (Std)",null,null,null,null,"4826",210,null,265,50,null,null,null,null,4826,250,250,250,null,null,"Solid Bore","7/8\"","1445","1.5 in",0.875,"Fog Nozzle",300,"Fog Nozzle 300",null,null,150,75,"150 75",null,null,null,null,null,"Fog Nozzle",4802,40,"100 (Std)","Fog Nozzle 40 @ 100 (Std)",null,null,null,"Fog Nozzle 200 @ 75",4826,4863,null,"Fog Nozzle 200 @ 75 4826","Fog Nozzle 200 @ 75 4863",null,null,null,"Fog Nozzle 175 @ 50 4863",null,null,null,"Stack Tips","15/16\"; 1/2\"",0.5,"Stack Tips 15/16\"; 1/2\"",null,null,null,"Solid Bore 1.5 in","7/8\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 2.5 in","1\"",null,"Solid Bore Yes 1.5 in 7/8\" No (Std)","Solid Bore Yes 1.5 in","Solid Bore","7/8\"","1445","1.5 in",0.875,"Yes","No (Std)","Solid Bore No 2.5 in",null,1,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore No 2.5 in 1-1/8\" Yes","0489",null,null,null,"7/8\"","7_8_",null,"Solid Bore","7/8\"","1445","1.5 in",0.875,"Yes","Solid Bore 1.5 in Yes 7/8\" 1445",null,"Solid Bore 1.5 in Yes 7/8\" 1445",null,null,null,1.25,"1-1/4\"; 1-1/8\"; 1\"","328 gpm @ 50 psi; RF = 123",null,"Solid Bore","7/8\"","1445","Solid Bore7/8\"1445",null,"Solid Bore7/8\"1445"]
[null,null,null,null,null,null,null,null,null,null,null,null,"1.5 in",null,null,null,"95-200",null,150,150,150,150,null,null,null,null,null,null,null,"30-150",75,"30-150 75",null,null,null,null,"4826",250,null,300,"100 (Std)",75,null,null,null,4826,300,300,null,null,null,"Solid Bore","15/16\"","1445","1.5 in",0.9375,"Fog Nozzle",350,"Fog Nozzle 350",null,null,150,50,"150 50",null,null,null,null,null,"Fog Tip",4824,200,"100 (Std)","Fog Tip 200 @ 100 (Std)",null,null,null,"Fog Nozzle 210 @ 50",4826,null,null,"Fog Nozzle 210 @ 50 4826",null,null,null,null,"Fog Nozzle 175 @ 75 4863",null,null,null,"Stack Tips","1-1/16\"; 15/16\"",0.9375,"Stack Tips 1-1/16\"; 15/16\"",null,null,null,"Solid Bore 1.5 in","15/16\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 2.5 in","1-1/8\"",null,"Solid Bore Yes 1.5 in 15/16\" No (Std)","Solid Bore Yes 1.5 in","Solid Bore","15/16\"","1445","1.5 in",0.9375,"Yes","No (Std)","Solid Bore No 2.5 in",null,1.125,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore No 2.5 in 1-3/8\" Yes","0489",null,null,null,"15/16\"","15_16_",null,"Solid Bore","15/16\"","1445","1.5 in",0.9375,"Yes","Solid Bore 1.5 in Yes 15/16\" 1445",null,"Solid Bore 1.5 in Yes 15/16\" 1445",null,null,null,1.25,"1-1/4\"; 1-1/8\"; 1\"","328 gpm @ 50 psi; RF = 123",null,"Solid Bore","15/16\"","1445","Solid Bore15/16\"1445",null,"Solid Bore15/16\"1445"]
[null,null,null,null,null,null,null,null,null,null,null,null,"1.5 in",null,null,null,"125-250",null,161,161,161,161,null,null,null,null,null,null,null,"30-150","87 (CE)","30-150 87 (CE)",null,null,null,null,"4826",300,null,350,"100 (Std)",null,null,null,null,4826,350,null,null,null,null,"Solid Bore","1\"","1445","1.5 in",1,"Fog Tip",95,"Fog Tip 95",null,null,150,"87 (CE)","150 87 (CE)",null,null,null,null,null,"Fog Tip",4824,250,"100 (Std)","Fog Tip 250 @ 100 (Std)",null,null,null,"Fog Nozzle 225 @ 100",4863,null,null,"Fog Nozzle 225 @ 100 4863",null,null,null,null,"Fog Nozzle 185 @ 50 4863",null,null,null,"Stack Tips","1-1/4\"; 1-1/8\"; 1\"",1,"Stack Tips 1-1/4\"; 1-1/8\"; 1\"",null,null,null,"Solid Bore 1.5 in","1\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 2.5 in","1-1/4\"",null,"Solid Bore Yes 1.5 in 1\" No (Std)","Solid Bore Yes 1.5 in","Solid Bore","1\"","1445","1.5 in",1,"Yes","No (Std)","Solid Bore No 2.5 in",null,1.25,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore No 2.5 in 15/16\" Yes","0489",null,null,null,"1\"","1_",null,"Solid Bore","1\"","1445","1.5 in",1,"Yes","Solid Bore 1.5 in Yes 1\" 1445",null,"Solid Bore 1.5 in Yes 1\" 1445",null,null,null,1.25,"1-1/4\"; 1-1/8\"; 1\"","328 gpm @ 50 psi; RF = 123",null,"Solid Bore","1\"","1445","Solid Bore1\"1445",null,"Solid Bore1\"1445"]
[null,null,null,null,null,null,null,null,null,null,null,null,"1.5 IN",null,null,null,null,null,175,175,175,175,null,null,null,null,null,null,null,"30-200","100 (Std)","30-200 100 (Std)",null,null,null,null,"4826",350,null,null,null,null,null,null,null,4863,95,null,null,null,null,"Solid Bore","1-1/16\"","1445","1.5 in",1.0625,"Fog Tip",125,"Fog Tip 125",null,null,161,50,"161 50",null,null,null,null,null,"Fog Tip",4824,300,"100 (Std)","Fog Tip 300 @ 100 (Std)",null,null,null,"Fog Nozzle 25 @ 100",4802,null,null,"Fog Nozzle 25 @ 100 4802",null,null,null,null,"Fog Nozzle 200 @ 100 4826",null,null,null,"Stack Tips","1-1/2\"; 1-1/4\"; 1\"",1,"Stack Tips 1-1/2\"; 1-1/4\"; 1\"",null,null,null,"Solid Bore 1.5 in","1-1/16\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 2.5 in","1-3/8\"",null,"Solid Bore Yes 1.5 in 1-1/16\" No (Std)","Solid Bore Yes 1.5 in","Solid Bore","1-1/16\"","1445","1.5 in",1.0625,"Yes","No (Std)","Solid Bore No 2.5 in",null,1.375,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore No 2.5 in 7/8\" Yes","0489",null,null,null,"1-1/16\"","1_1_16_",null,"Solid Bore","1-1/16\"","1445","1.5 in",1.0625,"Yes","Solid Bore 1.5 in Yes 1-1/16\" 1445",null,"Solid Bore 1.5 in Yes 1-1/16\" 1445",null,null,null,1.125,"1-1/8\"; 1/2\"","266 gpm @ 50 psi; RF = 99",null,"Solid Bore","1-1/16\"","1445","Solid Bore1-1/16\"1445",null,"Solid Bore1-1/16\"1445"]
[null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(SUBSTITUTE(B10,\" \",\"_\"),\"_\",SUBSTITUTE(D10,\"-\",\"_\"))","v":"Solid_Bore_No"},null,null,null,"1.5 in",null,null,null,null,null,200,200,200,200,null,null,null,null,null,null,null,"30-200",75,"30-200 75",null,null,null,null,"4863",95,null,null,null,null,null,null,null,4863,125,125,125,null,null,"Solid Bore","1-1/8\"","1445","1.5 in",1.125,"Fog Tip",150,"Fog Tip 150",null,null,175,"100 (Std)","175 100 (Std)",null,null,null,null,null,"Fog Tip",4824,350,"100 (Std)","Fog Tip 350 @ 100 (Std)",null,null,null,"Fog Nozzle 250 @ 100",4826,null,null,"Fog Nozzle 250 @ 100 4826",null,null,null,null,"Fog Nozzle 200 @ 100 4863",null,null,null,"Stack Tips","1-3/8\"; 1-1/4\"; 1\"",1,"Stack Tips 1-3/8\"; 1-1/4\"; 1\"",null,null,null,"Solid Bore 1.5 in","1-1/8\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 2.5 in","1-1/16\"",null,"Solid Bore Yes 1.5 in 1-1/8\" No (Std)","Solid Bore Yes 1.5 in","Solid Bore","1-1/8\"","1445","1.5 in",1.125,"Yes","No (Std)","Solid Bore Yes 1.5 in",null,0.5,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 1.5 in 1\" No (Std)","1445",null,null,null,"1-1/8\"","1_1_8_",null,"Solid Bore","1-1/8\"","1445","1.5 in",1.125,"Yes","Solid Bore 1.5 in Yes 1-1/8\" 1445",null,"Solid Bore 1.5 in Yes 1-1/8\" 1445",null,null,null,1.125,"1-1/8\"; 1/2\"",{"$f":"CONCATENATE(ROUND(29.71*(ES20*ES20)*SQRT(EU$1),0),\" gpm @ 50 psi; RF \",ROUND(1.57*(ES20*ES20)*EU$1,0))","v":"266 gpm @ 50 psi; RF 99"},null,"Solid Bore","1-1/8\"","1445","Solid Bore1-1/8\"1445",null,"Solid Bore1-1/8\"1445"]
[null,null,null,null,null,null,null,null,"Bore,Shutoff,Inlet,Remove Grip",null,null,null,"1.5 IN",null,null,null,null,null,210,210,210,210,null,null,null,null,null,null,null,"95-200","100 (Std)","95-200 100 (Std)",null,null,null,null,"4863",125,null,null,null,null,null,null,null,4863,150,150,150,null,null,"Solid Bore","1-3/16\"","1445","1.5 in",1.1875,"Fog Tip",161,"Fog Tip 161",null,null,175,75,"175 75",null,null,null,null,null,"Fog Tip",4824,200,75,"Fog Tip 200 @ 75",null,null,null,"Fog Nozzle 250 @ 50",4826,null,null,"Fog Nozzle 250 @ 50 4826",null,null,null,null,"Fog Nozzle 200 @ 75 4826",null,null,null,null,null,null,null,null,null,null,"Solid Bore 1.5 in","1-3/16\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 2.5 in","1-3/16\"",null,"Solid Bore Yes 1.5 in 1-3/16\" No (Std)","Solid Bore Yes 1.5 in","Solid Bore","1-3/16\"","1445","1.5 in",1.1875,"Yes","No (Std)","Solid Bore Yes 1.5 in",null,0.875,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 1.5 in 1/2\" No (Std)","1447",null,null,null,"1-3/16\"","1_3_16_",null,"Solid Bore","1-3/16\"","1445","1.5 in",1.1875,"Yes","Solid Bore 1.5 in Yes 1-3/16\" 1445",null,"Solid Bore 1.5 in Yes 1-3/16\" 1445",null,null,null,1.125,"1-1/8\"; 1/2\"","266 gpm @ 50 psi; RF 99",null,"Solid Bore","1-3/16\"","1445","Solid Bore1-3/16\"1445",null,"Solid Bore1-3/16\"1445"]
[null,null,null,{"$f":"CONCATENATE(C10,\" \",D10)","v":"2.5 in No"},null,null,null,null,"Solid Bore No 1.5 in 1\" Yes",null,null,null,"2 IN","STORZ",null,null,null,null,225,225,225,225,null,null,null,null,null,null,null,"95-200",75,"95-200 75",null,null,null,null,"4863",150,null,null,null,null,null,null,null,4863,175,175,175,null,null,"Solid Bore","1-1/4\"","1445","1.5 in",1.25,"Fog Tip",175,"Fog Tip 175",null,null,175,50,"175 50",null,null,null,null,null,"Fog Tip",4824,250,75,"Fog Tip 250 @ 75",null,null,null,"Fog Nozzle 250 @ 75",4826,null,null,{"$f":"CONCATENATE($BZ22,\" \",CA22)","v":"Fog Nozzle 250 @ 75 4826"},null,null,null,null,"Fog Nozzle 200 @ 75 4863",null,null,null,null,null,null,null,null,null,null,"Solid Bore 1.5 in","1-1/4\"","1.5 in","Solid Bore 1.5 in",null,"Stack Tips 1.5 in","1-1/8\"; 1/2\"",null,"Solid Bore Yes 1.5 in 1-1/4\" No (Std)","Solid Bore Yes 1.5 in","Solid Bore","1-1/4\"","1445","1.5 in",1.25,"Yes","No (Std)","Solid Bore Yes 1.5 in",null,0.9375,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 1.5 in 1\" Yes","1445",null,null,null,"1-1/4\"","1_1_4_",null,"Solid Bore","1-1/4\"","1445","1.5 in",1.25,"Yes","Solid Bore 1.5 in Yes 1-1/4\" 1445",null,"Solid Bore 1.5 in Yes 1-1/4\" 1445",null,null,null,1.375,"1-3/8\"; 1-1/4\"; 1\"","397 gpm @ 50 psi; RF 148",null,"Solid Bore","1-1/4\"","1445","Solid Bore1-1/4\"1445",null,"Solid Bore1-1/4\"1445"]
[null,{"$f":"IF(OR(C23=\"False\",D23=\"False\",E23=\"False\",H23=\"False\",J23=\"False\",F23=\"False\"),\"Error\",\"Okay\")","v":"Okay"},{"$f":"IFERROR(VLOOKUP(CONCATENATE(B10,\" \",C10),C28:C44,1,FALSE),\"False\")","v":"Solid Bore 2.5 in"},{"$f":"IFERROR(VLOOKUP(CONCATENATE(B10,\" \",E10),D28:D55,1,FALSE),\"False\")","v":"Solid Bore 1-3/8\""},{"$f":"IFERROR(VLOOKUP(CONCATENATE(B10,E10,I10),E28:E84,1,FALSE),\"False\")","v":"Solid Bore1-3/8\"0489"},{"$f":"IFERROR(VLOOKUP(CONCATENATE(D10,C10,F10),F28:F62,1,FALSE),\"false\")","v":"no2.5 INNH"},null,"Okay",{"$f":"IFERROR(VLOOKUP(CONCATENATE(B10,\" \",C10,\" \",D10,\" \",E10,\" \",I10),I27:I89,1,FALSE),\"False\")","v":"Solid Bore 2.5 in No 1-3/8\" 0489"},{"$f":"IF(D10=\"No\",IF(J10=\"yes\",\"False\",\"Okay\"),\"Okay\")","v":"Okay"},null,null,"2.5 IN","NH",null,null,null,null,250,250,250,250,null,null,null,null,null,null,null,"12-53","87 (CE)","12-53 87 (CE)",null,null,null,null,"4863",161,null,null,null,null,null,null,null,4863,200,200,null,null,null,"Solid Bore","1-3/8\"","1445","1.5 in",1.375,"Fog Tip",200,"Fog Tip 200",null,null,185,50,"185 50",null,null,null,null,null,"Fog Tip",4824,300,75,"Fog Tip 300 @ 75",null,null,null,"Fog Nozzle 265 @ 50",4826,null,null,{"$f":"CONCATENATE($BZ23,\" \",CA23)","v":"Fog Nozzle 265 @ 50 4826"},null,null,null,null,"Fog Nozzle 210 @ 50 4826",null,null,null,null,null,null,null,null,null,null,"Solid Bore 1.5 in","1-3/8\"","1.5 in","Solid Bore 1.5 in",null,"Stack Tips 1.5 in","15/16\"; 1/2\"",null,"Solid Bore Yes 1.5 in 1-3/8\" No (Std)","Solid Bore Yes 1.5 in","Solid Bore","1-3/8\"","1445","1.5 in",1.375,"Yes","No (Std)","Solid Bore Yes 1.5 in",null,1,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 1.5 in 1-1/16\" Yes","1445",null,null,null,"1-3/8\"","1_3_8_",null,"Solid Bore","1-3/8\"","1445","1.5 in",1.375,"Yes","Solid Bore 1.5 in Yes 1-3/8\" 1445",null,"Solid Bore 1.5 in Yes 1-3/8\" 1445",null,null,null,0.9375,"15/16\"; 1/2\"","185 gpm @ 50 psi; RF 69",null,"Solid Bore","1-3/8\"","1445","Solid Bore1-3/8\"1445",null,"Solid Bore1-3/8\"1445"]
[null,null,null,null,{"$f":"CONCATENATE(SUBSTITUTE(B10,\" \",\"_\"),\"_\",D10,\"_\",SUBSTITUTE(C10,\" \",\"_\"))","v":"Solid_Bore_No_2.5_in"},null,null,null,{"$f":"CONCATENATE(B10,\" \",C10,\" \",D10,\" \",E10,\" \",I10)","v":"Solid Bore 2.5 in No 1-3/8\" 0489"},null,null,null,"2.5 IN","NPSH",null,null,null,null,300,300,300,300,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4863",175,null,null,null,null,null,null,null,4863,null,null,161,null,null,"Solid Bore","1/2\"","1447","1.5 in",0.5,"Fog Tip",210,"Fog Tip 210",null,null,200,"100 (Std)","200 100 (Std)",null,null,null,null,null,"Fog Tip",4824,210,50,"Fog Tip 210 @ 50",null,null,null,"Fog Nozzle 300 @ 100",4826,null,null,{"$f":"CONCATENATE($BZ24,\" \",CA24)","v":"Fog Nozzle 300 @ 100 4826"},null,null,null,null,"Fog Nozzle 225 @ 100 4863",null,null,null,null,null,null,null,null,null,null,"Solid Bore 1.5 in","1/2\"","1.5 in","Solid Bore 1.5 in",null,"Stack Tips 1.5 in","1-1/16\"; 15/16\"",null,"Solid Bore Yes 1.5 in 1/2\" No (Std)","Solid Bore Yes 1.5 in","Solid Bore","1/2\"","1447","1.5 in",0.5,"Yes","No (Std)","Solid Bore Yes 1.5 in",null,1.0625,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 1.5 in 1-1/4\" Yes","1445",null,null,null,"1/2\"","1_2_",null,"Solid Bore","1/2\"","1447","1.5 in",0.5,"Yes","Solid Bore 1.5 in Yes 1/2\" 1447",null,"Solid Bore 1.5 in Yes 1/2\" 1447",null,null,null,0.9375,"15/16\"; 1/2\"","185 gpm @ 50 psi; RF 69",null,"Solid Bore","1/2\"","1447","Solid Bore1/2\"1447",null,"Solid Bore1/2\"1447"]
[null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(SUBSTITUTE(B10,\" \",\"_\"),\"_\",D10,\"_\",SUBSTITUTE(C10,\" \",\"_\"),\"_\",VLOOKUP(E10,ED:EE,2,FALSE),\"_\",IF(D10=\"no\",\"Yes\",IF(H10=\"yes\",\"Yes\",\"No__Std\")))","v":"Solid_Bore_No_2.5_in_1_3_8__Yes"},null,null,null,"2.5 IN","FDNY",null,null,null,null,350,350,350,350,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4863",185,null,null,null,null,null,null,null,4863,null,null,185,null,null,"Solid Bore","7/8\"","1499","1.5 in",0.875,"Fog Tip",225,"Fog Tip 225",null,null,200,75,"200 75",null,null,null,null,null,"Fog Tip",4824,265,50,"Fog Tip 265 @ 50",null,null,null,"Fog Nozzle 300 @ 75",4826,null,null,"Fog Nozzle 300 @ 75 4826",null,null,null,null,"Fog Nozzle 25 @ 100 4802",null,null,null,null,null,null,null,null,null,null,"Solid Bore 1.5 in","7/8\"","1.5 in","Solid Bore 1.5 in",null,"Stack Tips 1.5 in","1-1/4\"; 1-1/8\"; 1\"",null,"Solid Bore No 1.5 in 7/8\" Yes","Solid Bore No 1.5 in","Solid Bore","7/8\"","1499","1.5 in",0.875,"No","Yes","Solid Bore Yes 1.5 in",null,1.125,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 1.5 in 1-1/8\" Yes","1445",null,null,null,"7/8\"","7_8_",null,"Solid Bore","7/8\"","1499","1.5 in",0.875,"No","Solid Bore 1.5 in No 7/8\" 1499",null,"Solid Bore 1.5 in No 7/8\" 1499",null,null,null,0.9375,"15/16\"; 1/2\"","185 gpm @ 50 psi; RF 69",null,"Solid Bore","7/8\"","1499","Solid Bore7/8\"1499",null,"Solid Bore7/8\"1499"]
[null,null,null,null,"1440 1.5 in FDNY 1.5 in FDNY 15/16\"; 1/2\" bore size(s) PG",null,null,null,"Solid_Bore_Yes_1.5_in_1__No__Std",null,null,null,"2.5 IN","NYCORP",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4863",200,null,null,null,null,null,null,null,4866,95,null,null,null,null,"Solid Bore","15/16\"","1499","1.5 in",0.9375,"Fog Tip",250,"Fog Tip 250",null,null,210,50,"210 50",null,null,null,null,null,"Fog Tip",4824,250,50,"Fog Tip 250 @ 50",null,null,null,"Fog Nozzle 350 @ 100",4826,null,null,"Fog Nozzle 350 @ 100 4826",null,null,null,null,"Fog Nozzle 250 @ 100 4826",null,null,null,null,null,null,null,null,null,null,"Solid Bore 1.5 in","15/16\"","1.5 in","Solid Bore 1.5 in",null,"Stack Tips 1.5 in","15/16\"; 1/2\"",null,"Solid Bore No 1.5 in 15/16\" Yes","Solid Bore No 1.5 in","Solid Bore","15/16\"","1499","1.5 in",0.9375,"No","Yes","Solid Bore Yes 1.5 in",null,1.1875,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 1.5 in 1-3/16\" Yes","1445",null,null,null,"15/16\"","15_16_",null,"Solid Bore","15/16\"","1499","1.5 in",0.9375,"No","Solid Bore 1.5 in No 15/16\" 1499",null,"Solid Bore 1.5 in No 15/16\" 1499",null,null,null,null,null,null,null,"Solid Bore","15/16\"","1499","Solid Bore15/16\"1499",null,"Solid Bore15/16\"1499"]
[null,null,null,null,null,null,null,null,"Solid Bore 1.5 in No 3/4\" 0416",null,null,null,"2.5 IN","PITT6",null,null,null,null,"NH","NPSH","FDNY","NYCORP","PCT","Custom",null,null,null,null,null,null,null,null,null,null,null,null,"4863",225,null,null,null,null,null,null,null,4866,125,125,125,null,null,"Solid Bore","1\"","1499","1.5 in",1,"Fog Tip",265,"Fog Tip 265",null,null,225,"100 (Std)","225 100 (Std)",null,null,null,null,null,"Fog Nozzle",4826,200,"100 (Std)","Fog Nozzle 200 @ 100 (Std)",null,null,null,"Fog Nozzle 40 @ 100",4802,null,null,"Fog Nozzle 40 @ 100 4802",null,null,null,null,"Fog Nozzle 250 @ 50 4826",null,null,null,null,null,null,null,null,null,null,"Solid Bore 1.5 in","1\"","1.5 in","Solid Bore 1.5 in",null,"Stack Tips 2.5 in","1-1/8\"; 1/2\"",null,"Solid Bore No 1.5 in 1\" Yes","Solid Bore No 1.5 in","Solid Bore","1\"","1499","1.5 in",1,"No","Yes","Solid Bore Yes 1.5 in",null,1.25,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 1.5 in 1-3/8\" Yes","1445",null,null,null,"1\"","1_",null,"Solid Bore","1\"","1499","1.5 in",1,"No","Solid Bore 1.5 in No 1\" 1499",null,"Solid Bore 1.5 in No 1\" 1499",null,null,null,null,null,null,null,"Solid Bore","1\"","1499","Solid Bore1\"1499",null,"Solid Bore1\"1499"]
[null,null,"Solid Bore 1.5 in","Solid Bore 3/8\"","Solid Bore3/4\"0416","yes1.5 inNH",null,null,"Solid Bore 1.5 in No 7/8\" 0416",null,null,null,"2.5 IN","BAT",null,null,null,"SBTHREAD1.5 in",{"$f":"IF($B10=\"Solid Bore\",IF(OR(TRIM($I10)=\"0416\",$D10=\"yes\"),S27,\"\"),S27)","v":""},"","","","","",null,null,null,null,null,null,null,null,null,null,null,null,"4866",95,null,null,null,null,null,null,null,4866,150,150,150,null,null,"Solid Bore","1-1/16\"","1499","1.5 in",1.0625,"Fog Tip",300,"Fog Tip 300",null,null,250,"100 (Std)","250 100 (Std)",null,null,null,null,null,"Fog Nozzle",4826,250,"100 (Std)","Fog Nozzle 250 @ 100 (Std)",null,null,null,"Fog Nozzle 60 @ 100",4116,null,null,"Fog Nozzle 60 @ 100 4116",null,null,null,null,"Fog Nozzle 250 @ 75 4826",null,null,null,null,null,null,null,null,null,null,"Solid Bore 1.5 in","1-1/16\"","1.5 in","Solid Bore 1.5 in",null,"Stack Tips 2.5 in","1-1/4\"; 1-1/8\"; 1\"",null,"Solid Bore No 1.5 in 1-1/16\" Yes","Solid Bore No 1.5 in","Solid Bore","1-1/16\"","1499","1.5 in",1.0625,"No","Yes","Solid Bore Yes 1.5 in",null,1.375,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 1.5 in 15/16\" Yes","1445",null,null,null,"1-1/16\"","1_1_16_",null,"Solid Bore","1-1/16\"","1499","1.5 in",1.0625,"No","Solid Bore 1.5 in No 1-1/16\" 1499",null,"Solid Bore 1.5 in No 1-1/16\" 1499",null,null,null,null,null,null,null,"Solid Bore","1-1/16\"","1499","Solid Bore1-1/16\"1499",null,"Solid Bore1-1/16\"1499"]
[null,null,"Solid Bore 2.5 in","Solid Bore 1/2\"","Solid Bore7/8\"0416","yes1.5 inNPSH",{"$f":"VLOOKUP(C13,DataSource!AH:AJ,2,FALSE)","v":"04890501"},{"$f":"VLOOKUP(C13,DataSource!AH:AJ,3,FALSE)","v":"PLAIN DELUGE TIP 2.5NH 1 3/8D POLISH"},"Solid Bore 1.5 in No 1\" 0416",null,null,null,"2.5 IN","CSA",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4866",125,null,null,null,null,null,null,null,4866,175,175,175,null,null,"Solid Bore","1-1/8\"","1499","1.5 in",1.125,"Fog Tip",350,"Fog Tip 350",null,null,250,75,"250 75",null,null,null,null,null,"Fog Nozzle",4826,300,"100 (Std)","Fog Nozzle 300 @ 100 (Std)",null,null,null,"Fog Nozzle 60 @ 75",4116,null,null,"Fog Nozzle 60 @ 75 4116",null,null,null,null,"Fog Nozzle 265 @ 50 4826",null,null,null,null,null,null,null,null,null,null,"Solid Bore 1.5 in","1-1/8\"","1.5 in","Solid Bore 1.5 in",null,"Stack Tips 2.5 in","1-1/2\"; 1-1/4\"; 1\"",null,"Solid Bore No 1.5 in 1-1/8\" Yes","Solid Bore No 1.5 in","Solid Bore","1-1/8\"","1499","1.5 in",1.125,"No","Yes","Solid Bore Yes 2.5 in",null,0.875,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 1.5 in 7/8\" Yes","1445",null,null,null,"1-1/8\"","1_1_8_",null,"Solid Bore","1-1/8\"","1499","1.5 in",1.125,"No","Solid Bore 1.5 in No 1-1/8\" 1499",null,"Solid Bore 1.5 in No 1-1/8\" 1499",null,null,null,null,null,null,null,"Solid Bore","1-1/8\"","1499","Solid Bore1-1/8\"1499",null,"Solid Bore1-1/8\"1499"]
[null,null,"Stack Tips 1.5 in","Solid Bore 5/8\"","Solid Bore1\"0416","yes1.5 inFDNY",null,null,"Solid Bore 1.5 in No 1-1/8\" 0416",null,null,null,"2.5 IN","QST",null,null,null,"1445 1.5 in NH 1.5 in NH 15/16\" bore size(s)  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4866",150,null,null,null,null,null,null,null,4866,200,200,null,null,null,"Solid Bore","1-3/16\"","1499","1.5 in",1.1875,null,null,null,null,null,250,50,"250 50",null,null,null,null,null,"Fog Nozzle",4826,350,"100 (Std)","Fog Nozzle 350 @ 100 (Std)",null,null,null,"Fog Nozzle 60 @ 87",4116,null,null,"Fog Nozzle 60 @ 87 4116",null,null,null,null,"Fog Nozzle 300 @ 100 4826",null,null,null,null,null,null,null,null,null,null,"Solid Bore 1.5 in","1-3/16\"","1.5 in","Solid Bore 1.5 in",null,"Stack Tips 2.5 in","1-3/8\"; 1-1/4\"; 1\"",null,"Solid Bore No 1.5 in 1-3/16\" Yes","Solid Bore No 1.5 in","Solid Bore","1-3/16\"","1499","1.5 in",1.1875,"No","Yes","Solid Bore Yes 2.5 in",null,0.9375,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 2.5 in 1\" Yes","1446",null,null,null,"1-3/16\"","1_3_16_",null,"Solid Bore","1-3/16\"","1499","1.5 in",1.1875,"No","Solid Bore 1.5 in No 1-3/16\" 1499",null,"Solid Bore 1.5 in No 1-3/16\" 1499",null,null,null,null,null,null,null,"Solid Bore","1-3/16\"","1499","Solid Bore1-3/16\"1499",null,"Solid Bore1-3/16\"1499"]
[null,null,"Stack Tips 2.5 in","Solid Bore 3/4\"","Solid Bore1-1/8\"0416","yes1.5 inNYCORP",null,{"$f":"IF(D10=\"no\",\"\",IF(VLOOKUP(I10,M38:N45,2,FALSE)=\"yes\",\"Yes\",IF(VLOOKUP(I10,M38:N45,2,FALSE)=\"no\",\"No\",\"\")))","v":""},"Solid Bore 1.5 in No 1-1/4\" 0416",null,null,null,"2.5 IN","BIM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4866",161,null,null,null,null,null,null,null,4866,null,null,161,null,null,"Solid Bore","1-1/4\"","1499","1.5 in",1.25,null,null,null,null,null,265,50,"265 50",null,null,null,null,null,"Fog Nozzle",4826,200,75,"Fog Nozzle 200 @ 75",null,null,null,"Fog Nozzle 95 @ 100",4116,4863,null,"Fog Nozzle 95 @ 100 4116",{"$f":"CONCATENATE($BZ31,\" \",CB31)","v":"Fog Nozzle 95 @ 100 4863"},null,null,null,"Fog Nozzle 300 @ 75 4826",null,null,null,null,null,null,null,null,null,null,"Solid Bore 1.5 in","1-1/4\"","1.5 in","Solid Bore 1.5 in",null,null,null,null,"Solid Bore No 1.5 in 1-1/4\" Yes","Solid Bore No 1.5 in","Solid Bore","1-1/4\"","1499","1.5 in",1.25,"No","Yes","Solid Bore Yes 2.5 in",null,1,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 2.5 in 1-1/16\" Yes","1446",null,null,null,"1-1/4\"","1_1_4_",null,"Solid Bore","1-1/4\"","1499","1.5 in",1.25,"No","Solid Bore 1.5 in No 1-1/4\" 1499",null,"Solid Bore 1.5 in No 1-1/4\" 1499",null,null,null,null,null,null,null,"Solid Bore","1-1/4\"","1499","Solid Bore1-1/4\"1499",null,"Solid Bore1-1/4\"1499"]
[null,null,null,"Solid Bore 7/8\"","Solid Bore1-1/4\"0416","yes1.5 inPCT",null,null,"Solid Bore 1.5 in No 3/8\" 1417",null,null,null,"2.5 IN","STORZ",null,null,"BLACK (Std)","THREAD1 IN","NH","NPSH","Storz","Custom",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4866",175,null,null,null,null,null,null,null,4866,null,null,185,null,null,"Solid Bore","1-3/8\"","1499","1.5 in",1.375,null,null,null,null,null,300,"100 (Std)","300 100 (Std)",null,null,null,null,null,"Fog Nozzle",4826,265,50,"Fog Nozzle 265 @ 50",null,null,null,"Fog Nozzle 95 @ 75",4116,null,null,"Fog Nozzle 95 @ 75 4116",null,null,null,null,"Fog Nozzle 350 @ 100 4826",null,null,null,null,null,null,null,null,null,null,"Solid Bore 1.5 in","1-3/8\"","1.5 in","Solid Bore 1.5 in",null,null,null,null,"Solid Bore No 1.5 in 1-3/8\" Yes","Solid Bore No 1.5 in","Solid Bore","1-3/8\"","1499","1.5 in",1.375,"No","Yes","Solid Bore Yes 2.5 in",null,1.0625,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 2.5 in 1-1/4\" Yes","1446",null,null,null,"1-3/8\"","1_3_8_",null,"Solid Bore","1-3/8\"","1499","1.5 in",1.375,"No","Solid Bore 1.5 in No 1-3/8\" 1499",null,"Solid Bore 1.5 in No 1-3/8\" 1499",null,null,null,null,null,null,null,"Solid Bore","1-3/8\"","1499","Solid Bore1-3/8\"1499",null,"Solid Bore1-3/8\"1499"]
[null,null,null,"Solid Bore 15/16\"","Solid Bore3/8\"1417","yes1.5 inStorz",null,null,"Solid Bore 1.5 in No 1/2\" 1417",null,null,null,"3 IN","STORZ",null,null,"ORANGE","THREAD1.5 in","NH","NPSH","FDNY","NYCORP","PCT","Storz","Custom",null,null,null,null,null,null,null,null,null,null,null,"4866",185,null,null,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore","7/8\"","0489","2.5 in",0.875,null,null,null,null,null,300,75,"300 75",null,null,null,null,null,"Fog Nozzle",4826,250,75,"Fog Nozzle 250 @ 75",null,null,null,"Fog Nozzle 95 @ 87",4116,null,null,"Fog Nozzle 95 @ 87 4116",null,null,null,null,"Fog Nozzle 40 @ 100 4802",null,null,null,null,null,null,null,null,null,null,"Solid Bore 2.5 in","7/8\"","2.5 in","Solid Bore 2.5 in",null,null,null,null,"Solid Bore No 2.5 in 7/8\" Yes","Solid Bore No 2.5 in","Solid Bore","7/8\"","0489","2.5 in",0.875,"No","Yes","Solid Bore Yes 2.5 in",null,1.125,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 2.5 in 1-1/8\" Yes","1446",null,null,null,"7/8\"","7_8_",null,"Solid Bore","7/8\"","0489","2.5 in",0.875,"No","Solid Bore 2.5 in No 7/8\" 0489",null,"Solid Bore 2.5 in No 7/8\" 0489",null,null,null,null,null,null,null,"Solid Bore","7/8\"","0489","Solid Bore7/8\"0489",null,"Solid Bore7/8\"0489"]
[null,null,null,"Solid Bore 1\"","Solid Bore1/2\"1417","yes1.5 inCustom",null,null,"Solid Bore 1.5 in No 5/8\" 1417",null,null,null,null,null,null,null,"YELLOW","THREAD2 IN","Storz",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4866",200,null,null,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore","15/16\"","0489","2.5 in",0.9375,null,null,null,null,null,350,"100 (Std)","350 100 (Std)",null,null,null,null,null,"Fog Nozzle",4826,300,75,"Fog Nozzle 300 @ 75",null,null,null,"Fog Tip 125 @ 100",4866,null,null,"Fog Tip 125 @ 100 4866",null,null,null,null,"Fog Nozzle 60 @ 100 4116",null,null,null,null,null,null,null,null,null,null,"Solid Bore 2.5 in","15/16\"","2.5 in","Solid Bore 2.5 in",null,null,null,null,"Solid Bore No 2.5 in 15/16\" Yes","Solid Bore No 2.5 in","Solid Bore","15/16\"","0489","2.5 in",0.9375,"No","Yes","Solid Bore Yes 2.5 in",null,1.1875,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 2.5 in 1-3/16\" Yes","1446",null,null,null,"15/16\"","15_16_",null,"Solid Bore","15/16\"","0489","2.5 in",0.9375,"No","Solid Bore 2.5 in No 15/16\" 0489",null,"Solid Bore 2.5 in No 15/16\" 0489",null,null,null,null,null,null,null,"Solid Bore","15/16\"","0489","Solid Bore15/16\"0489",null,"Solid Bore15/16\"0489"]
[null,null,null,"Solid Bore 1-1/16\"","Solid Bore5/8\"1417","yes2.5 inNH",null,null,"Solid Bore 1.5 in No 3/4\" 1417",null,null,null,null,null,null,null,"RED","THREAD2.5 IN","NH","NPSH","FDNY","NYCORP","PITT6","BAT","CSA","QST","BIM","Storz","Custom",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore","1\"","0489","2.5 in",1,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4826,210,50,"Fog Nozzle 210 @ 50",null,null,null,"Fog Tip 125 @ 75",4866,null,null,"Fog Tip 125 @ 75 4866",null,null,null,null,"Fog Nozzle 60 @ 75 4116",null,null,null,null,null,null,null,null,null,null,"Solid Bore 2.5 in","1\"","2.5 in","Solid Bore 2.5 in",null,null,null,null,"Solid Bore No 2.5 in 1\" Yes","Solid Bore No 2.5 in","Solid Bore","1\"","0489","2.5 in",1,"No","Yes","Solid Bore Yes 2.5 in",null,1.25,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 2.5 in 1-3/8\" Yes","1446",null,null,null,"1\"","1_",null,"Solid Bore","1\"","0489","2.5 in",1,"No","Solid Bore 2.5 in No 1\" 0489",null,"Solid Bore 2.5 in No 1\" 0489",null,null,null,null,null,null,null,"Solid Bore","1\"","0489","Solid Bore1\"0489",null,"Solid Bore1\"0489"]
[null,null,null,"Solid Bore 1-1/8\"","Solid Bore3/4\"1417","yes2.5 inNPSH",null,null,"Solid Bore 1.5 in No 7/8\" 1417",null,null,null,null,null,null,null,"BLUE","THREAD3 IN","Storz",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore","1.5 in",{"$f":"CONCATENATE(AU36,AV36)","v":"Solid Bore1.5 in"},null,null,"Solid Bore","1-1/8\"","0489","2.5 in",1.125,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4826,250,50,"Fog Nozzle 250 @ 50",null,null,null,"Fog Tip 150 @ 100",4866,null,null,"Fog Tip 150 @ 100 4866",null,null,null,null,"Fog Nozzle 60 @ 87 4116",null,null,null,null,null,null,null,null,null,null,"Solid Bore 2.5 in","1-1/8\"","2.5 in","Solid Bore 2.5 in",null,null,null,null,"Solid Bore No 2.5 in 1-1/8\" Yes","Solid Bore No 2.5 in","Solid Bore","1-1/8\"","0489","2.5 in",1.125,"No","Yes","Solid Bore Yes 2.5 in",null,1.375,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 2.5 in 15/16\" Yes","1446",null,null,null,"1-1/8\"","1_1_8_",null,"Solid Bore","1-1/8\"","0489","2.5 in",1.125,"No","Solid Bore 2.5 in No 1-1/8\" 0489",null,"Solid Bore 2.5 in No 1-1/8\" 0489",null,null,null,null,null,null,null,"Solid Bore","1-1/8\"","0489","Solid Bore1-1/8\"0489",null,"Solid Bore1-1/8\"0489"]
[null,null,null,"Solid Bore 1-3/16\"","Solid Bore7/8\"1417","yes2.5 INFDNY",null,null,"Solid Bore 1.5 in No 15/16\" 1417",null,null,null,null,null,null,null,"GREEN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore","2.5 in",{"$f":"CONCATENATE(AU37,AV37)","v":"Solid Bore2.5 in"},null,null,"Solid Bore","1-1/4\"","0489","2.5 in",1.25,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4863,95,"100 (Std)","Fog Nozzle 95 @ 100 (Std)",null,null,null,"Fog Tip 150 @ 50",4866,null,null,"Fog Tip 150 @ 50 4866",null,null,null,null,"Fog Nozzle 95 @ 100 4116",null,null,null,null,null,null,null,null,null,null,"Solid Bore 2.5 in","1-1/4\"","2.5 in","Solid Bore 2.5 in",null,null,null,null,"Solid Bore No 2.5 in 1-1/4\" Yes","Solid Bore No 2.5 in","Solid Bore","1-1/4\"","0489","2.5 in",1.25,"No","Yes","Stack Tips No 1.5 in",null,0.5,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 2.5 in 7/8\" Yes","1446",null,null,null,"1-1/4\"","1_1_4_",null,"Solid Bore","1-1/4\"","0489","2.5 in",1.25,"No","Solid Bore 2.5 in No 1-1/4\" 0489",null,"Solid Bore 2.5 in No 1-1/4\" 0489",null,null,null,null,null,null,null,"Solid Bore","1-1/4\"","0489","Solid Bore1-1/4\"0489",null,"Solid Bore1-1/4\"0489"]
[null,null,null,"Solid Bore 1-1/4\"","Solid Bore15/16\"1417","yes2.5 INNYCORP",null,null,"Solid Bore 1.5 in No 1\" 1417",null,null,null,"1440","No",{"$f":"TRIM(M38)","v":"1440"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Style","List Price",null,null,null,null,"Stack Tips","1.5 in",{"$f":"CONCATENATE(AU38,AV38)","v":"Stack Tips1.5 in"},null,null,"Solid Bore","1-3/8\"","0489","2.5 in",1.375,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4863,125,"100 (Std)","Fog Nozzle 125 @ 100 (Std)",null,null,null,"Fog Tip 150 @ 75",4866,null,null,"Fog Tip 150 @ 75 4866",null,null,null,null,"Fog Nozzle 95 @ 100 4863",null,null,null,null,null,null,null,null,null,null,"Solid Bore 2.5 in","1-3/8\"","2.5 in","Solid Bore 2.5 in",null,null,null,null,"Solid Bore No 2.5 in 1-3/8\" Yes","Solid Bore No 2.5 in","Solid Bore","1-3/8\"","0489","2.5 in",1.375,"No","Yes","Stack Tips No 1.5 in",null,0.5,null,null,null,null,null,null,null,null,null,null,null,"Stack Tips Yes 1.5 in 15/16\"; 1/2\" Yes","1441",null,null,null,"1-3/8\"","1_3_8_",null,"Solid Bore","1-3/8\"","0489","2.5 in",1.375,"No","Solid Bore 2.5 in No 1-3/8\" 0489",null,"Solid Bore 2.5 in No 1-3/8\" 0489",null,null,null,null,null,null,null,"Solid Bore","1-3/8\"","0489","Solid Bore1-3/8\"0489",null,"Solid Bore1-3/8\"0489"]
[null,null,null,"Solid Bore 1-3/8\"","Solid Bore1\"1417","yes2.5 INPITT6",null,null,"Solid Bore 1.5 in No 1-1/8\" 1417",null,null,null,"1441","Yes",{"$f":"TRIM(M39)","v":"1441"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"0416",394,null,null,null,null,"Stack Tips","2.5 in",{"$f":"CONCATENATE(AU39,AV39)","v":"Stack Tips2.5 in"},null,null,"Solid Bore","7/8\"","1446","2.5 in",0.875,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4863,150,"100 (Std)","Fog Nozzle 150 @ 100 (Std)",null,null,null,"Fog Tip 161 @ 50",4866,null,null,"Fog Tip 161 @ 50 4866",null,null,null,null,"Fog Nozzle 95 @ 75 4116",null,null,null,null,null,null,null,null,null,null,"Solid Bore 2.5 in","7/8\"","2.5 in","Solid Bore 2.5 in",null,null,null,null,"Solid Bore Yes 2.5 in 7/8\" No (Std)","Solid Bore Yes 2.5 in","Solid Bore","7/8\"","1446","2.5 in",0.875,"Yes","No (Std)","Stack Tips No 1.5 in",null,0.9375,null,null,null,null,null,null,null,null,null,null,null,"Stack Tips Yes 2.5 in 1-1/8\"; 1/2\" Yes","1443",null,null,null,"7/8\"","7_8_",null,"Solid Bore","7/8\"","1446","2.5 in",0.875,"Yes","Solid Bore 2.5 in Yes 7/8\" 1446",null,"Solid Bore 2.5 in Yes 7/8\" 1446",null,null,null,null,null,null,null,"Solid Bore","7/8\"","1446","Solid Bore7/8\"1446",null,"Solid Bore7/8\"1446"]
[null,null,null,"Stack Tips 1-1/8\"; 1/2\"","Solid Bore1-1/8\"1417","yes2.5 INBAT",null,null,"Solid Bore 1.5 in No 1-1/4\" 1417",null,null,null,"1442","No","1442",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"yes1.5 in","NH",{"$f":"CONCATENATE(AI40,AJ40)","v":"yes1.5 inNH"},null,null,null,"0439",296,null,null,null,null,null,null,null,null,null,"Solid Bore","15/16\"","1446","2.5 in",0.9375,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4863,175,"100 (Std)","Fog Nozzle 175 @ 100 (Std)",null,null,null,"Fog Tip 175 @ 100",4866,null,null,"Fog Tip 175 @ 100 4866",null,null,null,null,"Fog Nozzle 95 @ 87 4116",null,null,null,null,null,null,null,null,null,null,"Solid Bore 2.5 in","15/16\"","2.5 in","Solid Bore 2.5 in",null,null,null,null,"Solid Bore Yes 2.5 in 15/16\" No (Std)","Solid Bore Yes 2.5 in","Solid Bore","15/16\"","1446","2.5 in",0.9375,"Yes","No (Std)","Stack Tips No 1.5 in",null,1,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 1.5 in 1-1/16\" No (Std)","1445",null,null,null,"15/16\"","15_16_",null,"Solid Bore","15/16\"","1446","2.5 in",0.9375,"Yes","Solid Bore 2.5 in Yes 15/16\" 1446",null,"Solid Bore 2.5 in Yes 15/16\" 1446",null,null,null,null,null,null,null,"Solid Bore","15/16\"","1446","Solid Bore15/16\"1446",null,"Solid Bore15/16\"1446"]
[null,null,null,"Stack Tips 15/16\"; 1/2\"","Solid Bore1-1/4\"1417","yes2.5 INCSA",null,null,"Solid Bore 1.5 in Yes 7/8\" 1445",null,null,null,"1443","Yes","1443",null,null,"Style",null,null,{"$f":"IF(B10=\"fog tip\",\"N/A\",\"No (Std)\")","v":"No (Std)"},null,"yes1 IN","NH","NPSH","Storz","Custom",null,null,null,null,null,null,null,"yes1.5 in","NPSH",{"$f":"CONCATENATE(AI41,AJ41)","v":"yes1.5 inNPSH"},null,null,null,"0489",546,null,null,null,null,null,null,null,null,null,"Solid Bore","1\"","1446","2.5 in",1,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4863,200,"100 (Std)","Fog Nozzle 200 @ 100 (Std)",null,null,null,"Fog Tip 175 @ 50",4866,null,null,"Fog Tip 175 @ 50 4866",null,null,null,null,"Fog Tip 125 @ 100 4866",null,null,null,null,null,null,null,null,null,null,"Solid Bore 2.5 in","1\"","2.5 in","Solid Bore 2.5 in",null,null,null,null,"Solid Bore Yes 2.5 in 1\" No (Std)","Solid Bore Yes 2.5 in","Solid Bore","1\"","1446","2.5 in",1,"Yes","No (Std)","Stack Tips No 2.5 in",null,1,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 1.5 in 1-1/4\" No (Std)","1445",null,null,null,"1\"","1_",null,"Solid Bore","1\"","1446","2.5 in",1,"Yes","Solid Bore 2.5 in Yes 1\" 1446",null,"Solid Bore 2.5 in Yes 1\" 1446",null,null,null,null,null,null,null,"Solid Bore","1\"","1446","Solid Bore1\"1446",null,"Solid Bore1\"1446"]
[null,null,null,"Stack Tips 15/16\"; 1/2\"","Solid Bore7/8\"1445","yes2.5 INQST",null,null,"Solid Bore 1.5 in Yes 15/16\" 1445",null,null,null,"1445","Yes","1445",null,"Fog Nozzle 5-40","1602",null,null,{"$f":"IF(B10=\"fog tip\",\"\",\"Yes\")","v":"Yes"},null,"yes1.5 in","NH","NPSH","FDNY","NYCORP","PCT","Storz","Custom",null,null,null,null,"yes1.5 in","FDNY","yes1.5 inFDNY",null,null,null,"1417",164,null,null,null,null,null,null,null,null,null,"Solid Bore","1-1/16\"","1446","2.5 in",1.0625,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4863,125,75,"Fog Nozzle 125 @ 75",null,null,null,"Fog Tip 175 @ 75",4866,null,null,"Fog Tip 175 @ 75 4866",null,null,null,null,"Fog Tip 125 @ 75 4866",null,null,null,null,null,null,null,null,null,null,"Solid Bore 2.5 in","1-1/16\"","2.5 in","Solid Bore 2.5 in",null,null,null,null,"Solid Bore Yes 2.5 in 1-1/16\" No (Std)","Solid Bore Yes 2.5 in","Solid Bore","1-1/16\"","1446","2.5 in",1.0625,"Yes","No (Std)","Stack Tips No 2.5 in",null,1,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 1.5 in 1-1/8\" No (Std)","1445",null,null,null,"1-1/16\"","1_1_16_",null,"Solid Bore","1-1/16\"","1446","2.5 in",1.0625,"Yes","Solid Bore 2.5 in Yes 1-1/16\" 1446",null,"Solid Bore 2.5 in Yes 1-1/16\" 1446",null,null,null,null,null,null,null,"Solid Bore","1-1/16\"","1446","Solid Bore1-1/16\"1446",null,"Solid Bore1-1/16\"1446"]
[null,null,null,"Stack Tips 1-1/16\"; 15/16\"","Solid Bore15/16\"1445","yes2.5 INBIM",null,null,"Solid Bore 1.5 in Yes 1\" 1445",null,null,null,"1446","Yes","1446",null,"Fog Nozzle 12-53","1602",null,null,null,null,"yes2.5 IN","NH","NPSH","FDNY","NYCORP","PITT6","BAT","CSA","QST","BIM","Storz","Custom","yes1.5 in","NYCORP","yes1.5 inNYCORP",null,null,null,"1420",520,null,null,null,null,null,null,null,null,null,"Solid Bore","1-1/8\"","1446","2.5 in",1.125,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4863,150,75,"Fog Nozzle 150 @ 75",null,null,null,"Fog Tip 185 @ 50",4866,null,null,"Fog Tip 185 @ 50 4866",null,null,null,null,"Fog Tip 150 @ 100 4866",null,null,null,null,null,null,null,null,null,null,"Solid Bore 2.5 in","1-1/8\"","2.5 in","Solid Bore 2.5 in",null,null,null,null,"Solid Bore Yes 2.5 in 1-1/8\" No (Std)","Solid Bore Yes 2.5 in","Solid Bore","1-1/8\"","1446","2.5 in",1.125,"Yes","No (Std)","Stack Tips No 2.5 in",null,1,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 1.5 in 1-3/16\" No (Std)","1445",null,null,null,"1-1/8\"","1_1_8_",null,"Solid Bore","1-1/8\"","1446","2.5 in",1.125,"Yes","Solid Bore 2.5 in Yes 1-1/8\" 1446",null,"Solid Bore 2.5 in Yes 1-1/8\" 1446",null,null,null,null,null,null,null,"Solid Bore","1-1/8\"","1446","Solid Bore1-1/8\"1446",null,"Solid Bore1-1/8\"1446"]
[null,null,null,"Stack Tips 1-1/4\"; 1-1/8\"; 1\"","Solid Bore1\"1445","yes2.5 INStorz",null,null,"Solid Bore 1.5 in Yes 1-1/16\" 1445",null,null,null,"1447","Yes","1447",null,"Fog Nozzle 30-150","1616",35,null,null,null,"no1 IN","NH","NPSH","Custom",null,null,null,null,null,null,null,null,"yes1.5 in","PCT","yes1.5 inPCT",null,null,null,"1440",858,null,null,null,null,null,null,null,null,null,"Solid Bore","1-3/16\"","1446","2.5 in",1.1875,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4863,175,75,"Fog Nozzle 175 @ 75",null,null,null,"Fog Tip 200 @ 100",4824,4866,null,"Fog Tip 200 @ 100 4824","Fog Tip 200 @ 100 4866",null,null,null,"Fog Tip 150 @ 50 4866",null,null,null,null,null,null,null,null,null,null,"Solid Bore 2.5 in","1-3/16\"","2.5 in","Solid Bore 2.5 in",null,null,null,null,"Solid Bore Yes 2.5 in 1-3/16\" No (Std)","Solid Bore Yes 2.5 in","Solid Bore","1-3/16\"","1446","2.5 in",1.1875,"Yes","No (Std)","Stack Tips Yes 1.5 in",null,0.5,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 1.5 in 1-3/8\" No (Std)","1445",null,null,null,"1-3/16\"","1_3_16_",null,"Solid Bore","1-3/16\"","1446","2.5 in",1.1875,"Yes","Solid Bore 2.5 in Yes 1-3/16\" 1446",null,"Solid Bore 2.5 in Yes 1-3/16\" 1446",null,null,null,null,null,null,null,"Solid Bore","1-3/16\"","1446","Solid Bore1-3/16\"1446",null,"Solid Bore1-3/16\"1446"]
[null,null,null,"Stack Tips 1-1/2\"; 1-1/4\"; 1\"","Solid Bore1-1/16\"1445","yes2.5 INCustom",null,null,"Solid Bore 1.5 in Yes 1-1/8\" 1445",null,null,null,"2393","No","2393",null,"Fog Nozzle 13-60","1702",null,null,null,null,"no1.5 in","NH","NPSH","FDNY","NYCORP","PCT","Custom",null,null,null,null,null,"yes1.5 in","Storz","yes1.5 inStorz",null,null,null,"1441",858,null,null,null,null,null,null,null,null,null,"Solid Bore","1-1/4\"","1446","2.5 in",1.25,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4863,200,75,"Fog Nozzle 200 @ 75",null,null,null,"Fog Tip 200 @ 75",4824,4866,null,"Fog Tip 200 @ 75 4824","Fog Tip 200 @ 75 4866",null,null,null,"Fog Tip 150 @ 75 4866",null,null,null,null,null,null,null,null,null,null,"Solid Bore 2.5 in","1-1/4\"","2.5 in","Solid Bore 2.5 in",null,null,null,null,"Solid Bore Yes 2.5 in 1-1/4\" No (Std)","Solid Bore Yes 2.5 in","Solid Bore","1-1/4\"","1446","2.5 in",1.25,"Yes","No (Std)","Stack Tips Yes 2.5 in",null,0.5,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 1.5 in 15/16\" No (Std)","1445",null,null,null,"1-1/4\"","1_1_4_",null,"Solid Bore","1-1/4\"","1446","2.5 in",1.25,"Yes","Solid Bore 2.5 in Yes 1-1/4\" 1446",null,"Solid Bore 2.5 in Yes 1-1/4\" 1446",null,null,null,null,null,null,null,"Solid Bore","1-1/4\"","1446","Solid Bore1-1/4\"1446",null,"Solid Bore1-1/4\"1446"]
[null,null,null,"Stack Tips 1-3/8\"; 1-1/4\"; 1\"","Solid Bore1-1/8\"1445","no1.5 inNH",null,null,"Solid Bore 1.5 in Yes 1-3/16\" 1445",null,null,null,null,null,null,null,"Fog Tip 13-60","1703",37,null,null,null,"no2.5 IN","NH","NPSH","FDNY","NYCORP","PITT6","BAT","CSA","QST","Custom",null,null,"yes1.5 in","Custom","yes1.5 inCustom",null,null,null,"1442",994,null,null,null,null,null,null,null,null,null,"Solid Bore","1-3/8\"","1446","2.5 in",1.375,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4863,150,50,"Fog Nozzle 150 @ 50",null,null,null,"Fog Tip 210 @ 50",4824,null,null,"Fog Tip 210 @ 50 4824",null,null,null,null,"Fog Tip 161 @ 50 4866",null,null,null,null,null,null,null,null,null,null,"Solid Bore 2.5 in","1-3/8\"","2.5 in","Solid Bore 2.5 in",null,null,null,null,"Solid Bore Yes 2.5 in 1-3/8\" No (Std)","Solid Bore Yes 2.5 in","Solid Bore","1-3/8\"","1446","2.5 in",1.375,"Yes","No (Std)","Stack Tips Yes 2.5 in",null,1,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 1.5 in 7/8\" No (Std)","1445",null,null,null,"1-3/8\"","1_3_8_",null,"Solid Bore","1-3/8\"","1446","2.5 in",1.375,"Yes","Solid Bore 2.5 in Yes 1-3/8\" 1446",null,"Solid Bore 2.5 in Yes 1-3/8\" 1446",null,null,null,null,null,null,null,"Solid Bore","1-3/8\"","1446","Solid Bore1-3/8\"1446",null,"Solid Bore1-3/8\"1446"]
[null,null,null,null,"Solid Bore1-3/16\"1445","no2.5 INNPSH",null,null,"Solid Bore 1.5 in Yes 1-1/4\" 1445",null,null,null,null,null,null,null,"Fog Nozzle 18-30","1704",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"yes2.5 IN","NH","yes2.5 INNH",null,null,null,"1443",994,null,null,null,null,null,null,null,null,null,"Stack Tips","1-1/8\"; 1/2\"","0439","1.5 in",0.5,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4863,161,50,"Fog Nozzle 161 @ 50",null,null,null,"Fog Tip 225 @ 100",4866,null,null,"Fog Tip 225 @ 100 4866",null,null,null,null,"Fog Tip 175 @ 100 4866",null,null,null,null,null,null,null,null,null,null,"Stack Tips 1.5 in","1-1/8\"; 1/2\"","1.5 in","Stack Tips 1.5 in",null,null,null,null,"Stack Tips No 1.5 in 1-1/8\"; 1/2\" Yes","Stack Tips No 1.5 in","Stack Tips","1-1/8\"; 1/2\"","0439","1.5 in",0.5,"No","Yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 2.5 in 1\" No (Std)","1446",null,null,null,"1-1/8\"; 1/2\"","1_1_8___1_2_",null,"Stack Tips","1-1/8\"; 1/2\"","0439","1.5 in",0.5,"No","Stack Tips 1.5 in No 1-1/8\"; 1/2\" 0439",null,"Stack Tips 1.5 in No 1-1/8\"; 1/2\" 0439",null,null,null,null,null,null,null,"Stack Tips","1-1/8\"; 1/2\"","0439","Stack Tips1-1/8\"; 1/2\"0439",null,"Stack Tips1-1/8\"; 1/2\"0439"]
[null,null,null,null,"Solid Bore1-1/4\"1445","no2.5 INFDNY",null,null,"Solid Bore 1.5 in Yes 1-3/8\" 1445",null,null,null,null,null,null,null,"Fog Nozzle 13-30","1704",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"yes2.5 IN","NPSH","yes2.5 INNPSH",null,null,null,"1445",738,null,null,null,null,null,null,null,null,null,"Stack Tips","15/16\"; 1/2\"","0439","1.5 in",0.5,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4863,175,50,"Fog Nozzle 175 @ 50",null,null,null,"Fog Tip 250 @ 100",4824,null,null,"Fog Tip 250 @ 100 4824",null,null,null,null,"Fog Tip 175 @ 50 4866",null,null,null,null,null,null,null,null,null,null,"Stack Tips 1.5 in","15/16\"; 1/2\"","1.5 in","Stack Tips 1.5 in",null,null,null,null,"Stack Tips No 1.5 in 15/16\"; 1/2\" Yes","Stack Tips No 1.5 in","Stack Tips","15/16\"; 1/2\"","0439","1.5 in",0.5,"No","Yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 2.5 in 1-1/16\" No (Std)","1446",null,null,null,"15/16\"; 1/2\"","15_16___1_2_",null,"Stack Tips","15/16\"; 1/2\"","0439","1.5 in",0.5,"No","Stack Tips 1.5 in No 15/16\"; 1/2\" 0439",null,"Stack Tips 1.5 in No 15/16\"; 1/2\" 0439",null,null,null,null,null,null,null,"Stack Tips","15/16\"; 1/2\"","0439","Stack Tips15/16\"; 1/2\"0439",null,"Stack Tips15/16\"; 1/2\"0439"]
[null,null,null,null,"Solid Bore1-3/8\"1445","no2.5 INNYCORP",null,null,"Solid Bore 1.5 in Yes 1/2\" 1447",null,null,null,null,null,null,null,"Fog Tip 18-30","1711",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"yes2.5 IN","FDNY","yes2.5 INFDNY",null,null,null,"1446",874,null,null,null,null,null,null,null,null,null,"Stack Tips","1-1/16\"; 15/16\"","0439","1.5 in",0.9375,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4863,185,50,"Fog Nozzle 185 @ 50",null,null,null,"Fog Tip 250 @ 50",4824,null,null,"Fog Tip 250 @ 50 4824",null,null,null,null,"Fog Tip 175 @ 75 4866",null,null,null,null,null,null,null,null,null,null,"Stack Tips 1.5 in","1-1/16\"; 15/16\"","1.5 in","Stack Tips 1.5 in",null,null,null,null,"Stack Tips No 1.5 in 1-1/16\"; 15/16\" Yes","Stack Tips No 1.5 in","Stack Tips","1-1/16\"; 15/16\"","0439","1.5 in",0.9375,"No","Yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 2.5 in 1-1/4\" No (Std)","1446",null,null,null,"1-1/16\"; 15/16\"","1_1_16___15_16_",null,"Stack Tips","1-1/16\"; 15/16\"","0439","1.5 in",0.9375,"No","Stack Tips 1.5 in No 1-1/16\"; 15/16\" 0439",null,"Stack Tips 1.5 in No 1-1/16\"; 15/16\" 0439",null,null,null,null,null,null,null,"Stack Tips","1-1/16\"; 15/16\"","0439","Stack Tips1-1/16\"; 15/16\"0439",null,"Stack Tips1-1/16\"; 15/16\"0439"]
[null,null,null,null,"Solid Bore1/2\"1447","no2.5 INPCT",null,null,"Solid Bore 1.5 in No 7/8\" 1499",null,null,null,null,null,null,null,"Fog Tip 13-30","1711",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"yes2.5 IN","NYCORP","yes2.5 INNYCORP",null,null,null,"1447",{"$f":"164+562","v":726},null,null,null,null,null,null,null,null,null,"Stack Tips","1-1/4\"; 1-1/8\"; 1\"","1420","1.5 in",1,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4863,225,"100 (Std)","Fog Nozzle 225 @ 100 (Std)",null,null,null,"Fog Tip 250 @ 75",4824,null,null,"Fog Tip 250 @ 75 4824",null,null,null,null,"Fog Tip 185 @ 50 4866",null,null,null,null,null,null,null,null,null,null,"Stack Tips 1.5 in","1-1/4\"; 1-1/8\"; 1\"","1.5 in","Stack Tips 1.5 in",null,null,null,null,"Stack Tips No 1.5 in 1-1/4\"; 1-1/8\"; 1\" Yes","Stack Tips No 1.5 in","Stack Tips","1-1/4\"; 1-1/8\"; 1\"","1420","1.5 in",1,"No","Yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 2.5 in 1-1/8\" No (Std)","1446",null,null,null,"1-1/4\"; 1-1/8\"; 1\"","1_1_4___1_1_8___1_",null,"Stack Tips","1-1/4\"; 1-1/8\"; 1\"","1420","1.5 in",1,"No","Stack Tips 1.5 in No 1-1/4\"; 1-1/8\"; 1\" 1420",null,"Stack Tips 1.5 in No 1-1/4\"; 1-1/8\"; 1\" 1420",null,null,null,null,null,null,null,"Stack Tips","1-1/4\"; 1-1/8\"; 1\"","1420","Stack Tips1-1/4\"; 1-1/8\"; 1\"1420",null,"Stack Tips1-1/4\"; 1-1/8\"; 1\"1420"]
[null,null,null,null,"Solid Bore7/8\"1499","no2.5 INCustom",null,null,"Solid Bore 1.5 in No 15/16\" 1499",null,null,null,null,null,null,null,"Fog Tip 30-125","1714",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"yes2.5 IN","PITT6","yes2.5 INPITT6",null,null,null,"1499",176,null,null,null,null,null,null,null,null,null,"Stack Tips","15/16\"; 1/2\"","1440","1.5 in",0.5,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip",4866,95,"100 (Std)","Fog Tip 95 @ 100 (Std)",null,null,null,"Fog Tip 265 @ 50",4824,null,null,"Fog Tip 265 @ 50 4824",null,null,null,null,"Fog Tip 200 @ 100 4824",null,null,null,null,null,null,null,null,null,null,"Stack Tips 1.5 in","15/16\"; 1/2\"","1.5 in","Stack Tips 1.5 in",null,null,null,null,"Stack Tips Yes 1.5 in 15/16\"; 1/2\" Yes","Stack Tips Yes 1.5 in","Stack Tips","15/16\"; 1/2\"","1440","1.5 in",0.5,"Yes","Yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 2.5 in 1-3/16\" No (Std)","1446",null,null,null,"15/16\"; 1/2\"","15_16___1_2_",null,"Stack Tips","15/16\"; 1/2\"","1440","1.5 in",0.5,"Yes","Stack Tips 1.5 in Yes 15/16\"; 1/2\" 1440",null,"Stack Tips 1.5 in Yes 15/16\"; 1/2\" 1440",null,null,null,null,null,null,null,"Stack Tips","15/16\"; 1/2\"","1440","Stack Tips15/16\"; 1/2\"1440",null,"Stack Tips15/16\"; 1/2\"1440"]
[null,null,null,null,"Solid Bore15/16\"1499","no2.5 INNH",null,null,"Solid Bore 1.5 in No 1\" 1499",null,null,null,null,null,null,null,"Fog Nozzle 30-125","1720",null,null,"0489 2.5 in NH 1\" bore size(s) ",null,null,null,null,null,null,null,null,null,null,null,null,null,"yes2.5 IN","BAT","yes2.5 INBAT",null,null,null,"2393",1656,null,null,null,null,null,null,null,null,null,"Stack Tips","15/16\"; 1/2\"","1441","1.5 in",0.5,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip",4866,125,"100 (Std)","Fog Tip 125 @ 100 (Std)",null,null,null,"Fog Tip 300 @ 100",4824,null,null,"Fog Tip 300 @ 100 4824",null,null,null,null,"Fog Tip 200 @ 100 4866",null,null,null,null,null,null,null,null,null,null,"Stack Tips 1.5 in","15/16\"; 1/2\"","1.5 in","Stack Tips 1.5 in",null,null,null,null,"Stack Tips Yes 1.5 in 15/16\"; 1/2\" No (Std)","Stack Tips Yes 1.5 in","Stack Tips","15/16\"; 1/2\"","1441","1.5 in",0.5,"Yes","No (Std)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 2.5 in 1-3/8\" No (Std)","1446",null,null,null,"15/16\"; 1/2\"","15_16___1_2_",null,"Stack Tips","15/16\"; 1/2\"","1441","1.5 in",0.5,"Yes","Stack Tips 1.5 in Yes 15/16\"; 1/2\" 1441",null,"Stack Tips 1.5 in Yes 15/16\"; 1/2\" 1441",null,null,null,null,null,null,null,"Stack Tips","15/16\"; 1/2\"","1441","Stack Tips15/16\"; 1/2\"1441",null,"Stack Tips15/16\"; 1/2\"1441"]
[null,null,null,null,"Solid Bore1\"1499","no2.5 INPITT6",null,null,"Solid Bore 1.5 in No 1-1/16\" 1499",null,null,null,null,null,null,null,"Fog Nozzle 95-200","1723",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"yes2.5 IN","CSA","yes2.5 INCSA",null,null,null,"2420",640,null,null,null,null,null,null,null,null,null,"Stack Tips","1-1/8\"; 1/2\"","1442","2.5 in",0.5,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip",4866,150,"100 (Std)","Fog Tip 150 @ 100 (Std)",null,null,null,"Fog Tip 300 @ 75",4824,null,null,"Fog Tip 300 @ 75 4824",null,null,null,null,"Fog Tip 200 @ 75 4824",null,null,null,null,null,null,null,null,null,null,"Stack Tips 2.5 in","1-1/8\"; 1/2\"","2.5 in","Stack Tips 2.5 in",null,null,null,null,"Stack Tips Yes 2.5 in 1-1/8\"; 1/2\" Yes","Stack Tips Yes 2.5 in","Stack Tips","1-1/8\"; 1/2\"","1442","2.5 in",0.5,"Yes","Yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 2.5 in 15/16\" No (Std)","1446",null,null,null,"1-1/8\"; 1/2\"","1_1_8___1_2_",null,"Stack Tips","1-1/8\"; 1/2\"","1442","2.5 in",0.5,"Yes","Stack Tips 2.5 in Yes 1-1/8\"; 1/2\" 1442",null,"Stack Tips 2.5 in Yes 1-1/8\"; 1/2\" 1442",null,null,null,null,null,null,null,"Stack Tips","1-1/8\"; 1/2\"","1442","Stack Tips1-1/8\"; 1/2\"1442",null,"Stack Tips1-1/8\"; 1/2\"1442"]
[null,null,null,null,"Solid Bore1-1/16\"1499","no2.5 INBAT",null,null,"Solid Bore 1.5 in No 1-1/8\" 1499",null,null,null,null,null,null,null,"Fog Nozzle 125-250","1733",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"yes2.5 IN","QST","yes2.5 INQST",null,null,null,"Storz",88,null,null,null,null,null,null,null,null,null,"Stack Tips","1-1/8\"; 1/2\"","1443","2.5 in",0.5,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip",4866,175,"100 (Std)","Fog Tip 175 @ 100 (Std)",null,null,null,"Fog Tip 350 @ 100",4824,null,null,"Fog Tip 350 @ 100 4824",null,null,null,null,"Fog Tip 200 @ 75 4866",null,null,null,null,null,null,null,null,null,null,"Stack Tips 2.5 in","1-1/8\"; 1/2\"","2.5 in","Stack Tips 2.5 in",null,null,null,null,"Stack Tips Yes 2.5 in 1-1/8\"; 1/2\" No (Std)","Stack Tips Yes 2.5 in","Stack Tips","1-1/8\"; 1/2\"","1443","2.5 in",0.5,"Yes","No (Std)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 2.5 in 7/8\" No (Std)","1446",null,null,null,"1-1/8\"; 1/2\"","1_1_8___1_2_",null,"Stack Tips","1-1/8\"; 1/2\"","1443","2.5 in",0.5,"Yes","Stack Tips 2.5 in Yes 1-1/8\"; 1/2\" 1443",null,"Stack Tips 2.5 in Yes 1-1/8\"; 1/2\" 1443",null,null,null,null,null,null,null,"Stack Tips","1-1/8\"; 1/2\"","1443","Stack Tips1-1/8\"; 1/2\"1443",null,"Stack Tips1-1/8\"; 1/2\"1443"]
[null,null,null,null,"Solid Bore1-1/8\"1499","no2.5 INCSA",null,null,"Solid Bore 1.5 in No 1-3/16\" 1499",null,null,null,null,null,null,null,"Fog Tip 95-200","1737",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"yes2.5 IN","BIM","yes2.5 INBIM",null,null,null,"ZT",340,null,null,null,null,null,null,null,null,null,"Stack Tips","1-1/4\"; 1-1/8\"; 1\"","2393","2.5 in",1,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip",4866,200,"100 (Std)","Fog Tip 200 @ 100 (Std)",null,null,null,"Fog Tip 95 @ 100",4866,null,null,"Fog Tip 95 @ 100 4866",null,null,null,null,"Fog Tip 210 @ 50 4824",null,null,null,null,null,null,null,null,null,null,"Stack Tips 2.5 in","1-1/4\"; 1-1/8\"; 1\"","2.5 in","Stack Tips 2.5 in",null,null,null,null,"Stack Tips Yes 2.5 in 1-1/4\"; 1-1/8\"; 1\" No (Std)","Stack Tips Yes 2.5 in","Stack Tips","1-1/4\"; 1-1/8\"; 1\"","2393","2.5 in",1,"Yes","No (Std)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stack Tips No 1.5 in 1-1/16\"; 15/16\" Yes","0439",null,null,null,"1-1/4\"; 1-1/8\"; 1\"","1_1_4___1_1_8___1_",null,"Stack Tips","1-1/4\"; 1-1/8\"; 1\"","2393","2.5 in",1,"Yes","Stack Tips 2.5 in Yes 1-1/4\"; 1-1/8\"; 1\" 2393",null,"Stack Tips 2.5 in Yes 1-1/4\"; 1-1/8\"; 1\" 2393",null,null,null,null,null,null,null,"Stack Tips","1-1/4\"; 1-1/8\"; 1\"","2393","Stack Tips1-1/4\"; 1-1/8\"; 1\"2393",null,"Stack Tips1-1/4\"; 1-1/8\"; 1\"2393"]
[null,null,null,null,"Solid Bore1-3/16\"1499","no2.5 INQST",null,null,"Solid Bore 1.5 in No 1-1/4\" 1499",null,null,null,null,null,null,null,"Fog Tip 125-250","1744",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"yes2.5 IN","Storz","yes2.5 INStorz",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stack Tips","1-1/2\"; 1-1/4\"; 1\"","2420","2.5 in",1,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip",4866,125,75,"Fog Tip 125 @ 75",null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip 225 @ 100 4866",null,null,null,null,null,null,null,null,null,null,"Stack Tips 2.5 in","1-1/2\"; 1-1/4\"; 1\"","2.5 in","Stack Tips 2.5 in",null,null,null,null,"Stack Tips No 2.5 in 1-1/2\"; 1-1/4\"; 1\" Yes","Stack Tips No 2.5 in","Stack Tips","1-1/2\"; 1-1/4\"; 1\"","2420","2.5 in",1,"No","Yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stack Tips No 1.5 in 1-1/4\"; 1-1/8\"; 1\" Yes","1420",null,null,null,"1-1/2\"; 1-1/4\"; 1\"","1_1_2___1_1_4___1_",null,"Stack Tips","1-1/2\"; 1-1/4\"; 1\"","2420","2.5 in",1,"No","Stack Tips 2.5 in No 1-1/2\"; 1-1/4\"; 1\" 2420",null,"Stack Tips 2.5 in No 1-1/2\"; 1-1/4\"; 1\" 2420",null,null,null,null,null,null,null,"Stack Tips","1-1/2\"; 1-1/4\"; 1\"","2420","Stack Tips1-1/2\"; 1-1/4\"; 1\"2420",null,"Stack Tips1-1/2\"; 1-1/4\"; 1\"2420"]
[null,null,null,null,"Solid Bore1-1/4\"1499","no1.5 inNPSH",null,null,"Solid Bore 1.5 in No 1-3/8\" 1499",null,null,null,null,null,null,null,"Fog Nozzle 30-200","1763",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"yes2.5 IN","Custom","yes2.5 INCustom",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stack Tips","1-1/4\"; 1-1/8\"; 1\"","2420","2.5 in",1,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip",4866,150,75,"Fog Tip 150 @ 75",null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip 250 @ 100 4824",null,null,null,null,null,null,null,null,null,null,"Stack Tips 2.5 in","1-1/4\"; 1-1/8\"; 1\"","2.5 in","Stack Tips 2.5 in",null,null,null,null,"Stack Tips No 2.5 in 1-1/4\"; 1-1/8\"; 1\" Yes","Stack Tips No 2.5 in","Stack Tips","1-1/4\"; 1-1/8\"; 1\"","2420","2.5 in",1,"No","Yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stack Tips No 1.5 in 1-1/8\"; 1/2\" Yes","0439",null,null,null,"1-1/4\"; 1-1/8\"; 1\"","1_1_4___1_1_8___1_",null,"Stack Tips","1-1/4\"; 1-1/8\"; 1\"","2420","2.5 in",1,"No","Stack Tips 2.5 in No 1-1/4\"; 1-1/8\"; 1\" 2420",null,"Stack Tips 2.5 in No 1-1/4\"; 1-1/8\"; 1\" 2420",null,null,null,null,null,null,null,"Stack Tips","1-1/4\"; 1-1/8\"; 1\"","2420","Stack Tips1-1/4\"; 1-1/8\"; 1\"2420",null,"Stack Tips1-1/4\"; 1-1/8\"; 1\"2420"]
[null,null,null,null,"Solid Bore1-3/8\"1499","no1.5 inFDNY",null,null,"Solid Bore 2.5 in No 7/8\" 0489",null,null,null,null,null,null,null,"Fog Tip 30-200","1766",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"no1.5 in","NH","no1.5 inNH",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stack Tips","1-3/8\"; 1-1/4\"; 1\"","2420","2.5 in",1,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip",4866,175,75,"Fog Tip 175 @ 75",null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip 250 @ 50 4824",null,null,null,null,null,null,null,null,null,null,"Stack Tips 2.5 in","1-3/8\"; 1-1/4\"; 1\"","2.5 in","Stack Tips 2.5 in",null,null,null,null,"Stack Tips No 2.5 in 1-3/8\"; 1-1/4\"; 1\" Yes","Stack Tips No 2.5 in","Stack Tips","1-3/8\"; 1-1/4\"; 1\"","2420","2.5 in",1,"No","Yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stack Tips No 1.5 in 15/16\"; 1/2\" Yes","0439",null,null,null,"1-3/8\"; 1-1/4\"; 1\"","1_3_8___1_1_4___1_",null,"Stack Tips","1-3/8\"; 1-1/4\"; 1\"","2420","2.5 in",1,"No","Stack Tips 2.5 in No 1-3/8\"; 1-1/4\"; 1\" 2420",null,"Stack Tips 2.5 in No 1-3/8\"; 1-1/4\"; 1\" 2420",null,null,null,null,null,null,null,"Stack Tips","1-3/8\"; 1-1/4\"; 1\"","2420","Stack Tips1-3/8\"; 1-1/4\"; 1\"2420",null,"Stack Tips1-3/8\"; 1-1/4\"; 1\"2420"]
[null,null,null,null,"Solid Bore7/8\"0489","no1.5 inNYCORP",null,null,"Solid Bore 2.5 in No 15/16\" 0489",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"no2.5 IN","NPSH","no2.5 INNPSH",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip",4866,200,75,"Fog Tip 200 @ 75",null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip 250 @ 75 4824",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stack Tips No 2.5 in 1-1/2\"; 1-1/4\"; 1\" Yes","2420"]
[null,"y",null,null,"Solid Bore15/16\"0489","no1.5 inPCT",null,null,"Solid Bore 2.5 in No 1\" 0489",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"no2.5 IN","FDNY","no2.5 INFDNY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip",4866,150,50,"Fog Tip 150 @ 50",null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip 265 @ 50 4824",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stack Tips No 2.5 in 1-1/4\"; 1-1/8\"; 1\" Yes","2420"]
[null,{"$f":"IF(OR(B10=P9,D10=\"yes\",TRIM(I10)=\"0416\"),CONCATENATE(I10,\" \",C10,\" \",F10,\" \",CONCATENATE(\"1.5 in \",G10),\" \",CONCATENATE(E10,\" bore size(s)\"),\" \",IF(B10=\"Fog Tip\",\"\",IF(D10=\"no\",IF(TRIM(I10)=\"0416\",\"\",\" \"),IF(OR(LEFT(I10,3)=\"144\",LEFT(I10,4)=\"2393\"),\"\",IF(H10=\"yes\",\" NPG\",\" PG\")))),IF(B10=\"Fog Tip\",\"\",IF(J10=\"Yes\",\" ZT\",\"\")),IF(K10=\"Yes\",\" ETCH\",\"\")),CONCATENATE(I10,\" \",C10,\" \",F10,\" \",CONCATENATE(E10,\" bore size(s) \"),IF(K10=\"Yes\",\" ETCH\",\"\")))","v":"0489 2.5 in NH 1-3/8\" bore size(s) "},null,null,"Solid Bore1\"0489","no1.5 inStorz",null,null,"Solid Bore 2.5 in No 1-1/8\" 0489",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"no2.5 IN","NYCORP","no2.5 INNYCORP",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip",4866,161,50,"Fog Tip 161 @ 50",null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip 300 @ 100 4824",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stack Tips No 2.5 in 1-3/8\"; 1-1/4\"; 1\" Yes","2420"]
[null,null,null,null,"Solid Bore1-1/8\"0489","no1.5 inCustom",null,null,"Solid Bore 2.5 in No 1-1/4\" 0489",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"no2.5 IN","PCT","no2.5 INPCT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip",4866,175,50,"Fog Tip 175 @ 50",null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip 300 @ 75 4824",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stack Tips Yes 1.5 in 15/16\"; 1/2\" No (Std)","1441"]
[null,"0416 1.5 in NH 1.5 in NH 7/8\" bore size(s) ",null,null,"Solid Bore1-1/4\"0489",null,null,null,"Solid Bore 2.5 in No 1-3/8\" 0489",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"no2.5 IN","Custom","no2.5 INCustom",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip",4866,185,50,"Fog Tip 185 @ 50",null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip 350 @ 100 4824",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stack Tips Yes 1.5 in 15/16\"; 1/2\" Yes","1440"]
[null,null,null,null,"Solid Bore1-3/8\"0489",null,null,null,"Solid Bore 2.5 in Yes 7/8\" 1446",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"no2.5 IN","NH","no2.5 INNH",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip",4866,225,"100 (Std)","Fog Tip 225 @ 100 (Std)",null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip 95 @ 100 4866",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stack Tips Yes 2.5 in 1-1/4\"; 1-1/8\"; 1\" No (Std)","2393"]
[null,null,null,null,"Solid Bore7/8\"1446",null,null,null,"Solid Bore 2.5 in Yes 15/16\" 1446",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"no2.5 IN","NPSH","no2.5 INNPSH",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stack Tips Yes 2.5 in 1-1/8\"; 1/2\" No (Std)","1443"]
[null,null,null,null,"Solid Bore15/16\"1446",null,null,null,"Solid Bore 2.5 in Yes 1\" 1446",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"no2.5 IN","FDNY","no2.5 INFDNY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stack Tips Yes 2.5 in 1-1/8\"; 1/2\" Yes","1442"]
[null,null,null,null,"Solid Bore1\"1446",null,null,null,"Solid Bore 2.5 in Yes 1-1/16\" 1446",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"no2.5 IN","NYCORP","no2.5 INNYCORP",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stack Tips 1.5 in Yes 15/16\"; 1/2\" 1441"]
[null,null,null,null,"Solid Bore1-1/16\"1446",null,null,null,"Solid Bore 2.5 in Yes 1-1/8\" 1446",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"no2.5 IN","PITT6","no2.5 INPITT6"]
[null,null,null,null,"Solid Bore1-1/8\"1446",null,null,null,"Solid Bore 2.5 in Yes 1-3/16\" 1446",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"no2.5 IN","BAT","no2.5 INBAT"]
[null,null,null,null,"Solid Bore1-3/16\"1446",null,null,null,"Solid Bore 2.5 in Yes 1-1/4\" 1446",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"no2.5 IN","CSA","no2.5 INCSA"]
[null,null,null,null,"Solid Bore1-1/4\"1446",null,null,null,"Solid Bore 2.5 in Yes 1-3/8\" 1446",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"no2.5 IN","QST","no2.5 INQST"]
[null,null,null,null,"Solid Bore1-3/8\"1446",null,null,null,"Stack Tips 1.5 in No 1-1/8\"; 1/2\" 0439",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"no2.5 IN","Custom","no2.5 INCustom"]
[null,null,null,null,"Stack Tips1-1/8\"; 1/2\"0439",null,null,null,"Stack Tips 1.5 in No 15/16\"; 1/2\" 0439"]
[null,null,null,null,"Stack Tips15/16\"; 1/2\"0439",null,null,null,"Stack Tips 1.5 in No 1-1/16\"; 15/16\" 0439"]
[null,null,null,null,"Stack Tips1-1/16\"; 15/16\"0439",null,null,null,"Stack Tips 1.5 in No 1-1/4\"; 1-1/8\"; 1\" 1420"]
[null,null,null,null,"Stack Tips1-1/4\"; 1-1/8\"; 1\"1420",null,null,null,"Stack Tips 1.5 in Yes 15/16\"; 1/2\" 1440"]
[null,null,null,null,"Stack Tips15/16\"; 1/2\"1440",null,null,null,"Stack Tips 1.5 in Yes 15/16\"; 1/2\" 1441"]
[null,null,null,null,"Stack Tips15/16\"; 1/2\"1441",null,null,null,"Stack Tips 2.5 in Yes 1-1/8\"; 1/2\" 1442"]
[null,null,null,null,"Stack Tips1-1/8\"; 1/2\"1442",null,null,null,"Stack Tips 2.5 in Yes 1-1/8\"; 1/2\" 1443"]
[null,null,null,null,"Stack Tips1-1/8\"; 1/2\"1443",null,null,null,"Stack Tips 2.5 in Yes 1-1/4\"; 1-1/8\"; 1\" 2393"]
[null,null,null,null,"Stack Tips1-1/4\"; 1-1/8\"; 1\"2393",null,null,null,"Stack Tips 2.5 in No 1-1/2\"; 1-1/4\"; 1\" 2420"]
[null,null,null,null,"Stack Tips1-1/2\"; 1-1/4\"; 1\"2420",null,null,null,"Stack Tips 2.5 in No 1-1/4\"; 1-1/8\"; 1\" 2420"]
[null,null,null,null,"Stack Tips1-1/4\"; 1-1/8\"; 1\"2420",null,null,null,"Stack Tips 2.5 in No 1-3/8\"; 1-1/4\"; 1\" 2420"]
[null,null,null,null,"Stack Tips1-3/8\"; 1-1/4\"; 1\"2420"]

{"sheet":"Shutoffs","index":4,"n_rows":113,"n_cols":158,"rows_kept":113,"cut":false,"hidden":false,"merged":[[13,7,14,7],[13,8,14,10],[7,7,8,7],[7,8,8,8],[7,9,8,9],[7,10,8,10],[11,7,12,9],[11,10,12,10],[10,2,10,3],[11,5,11,6],[12,2,12,6],[7,1,8,1],[7,2,8,2],[7,3,8,3],[11,3,11,4],[6,3,6,7],[15,2,17,10],[0,7,5,7],[0,8,1,10],[1,1,1,5],[2,1,2,5],[2,8,3,10],[3,1,3,5],[4,1,4,5],[4,8,5,10],[5,1,5,5],[7,4,8,4],[7,5,8,5],[7,6,8,6],[13,1,14,1],[13,2,14,6]]}
[null,"Instructions:",null,null,null,null,null,"Reaction Force Color Chart:","This is a Low RF Nozzle (RF < 51 )",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"asdf",null,null,"Style","Flow",null,"Flow",null,null,null,null,null,null,100,75,50,87,null,null,"Bore Size","Style",null,null,null,"Flow",null,null,null,"Flow","Pressure",null,null,null,null,null,null,null,"Style","Flow","Pressure",null,null,null,null,null,"Style",null,null,null,null,null,null,null,null,null,null,null,null,"Bore Size",null,null,null,null,null,null,"Bore Size",null,null,null,null,"Bore Size",null,"Bore,Shutoff,Inlet,Remove Grip",null,null,"Bore Size","Style","Inlet","Dec Size","Shutoff","Remove PG",null,"Bore Size","Dec Size",null,"Solid Bore No 1.5 in","Solid Bore No 2.5 in","Solid Bore Yes 1.5 in","Solid Bore Yes 2.5 in","Stack Tips No 1.5 in","Stack Tips No 2.5 in","Stack Tips Yes 1.5 in","Stack Tips Yes 2.5 in",null,null,"Bore,Shutoff,Inlet,Remove Grip","Style",null,null,null,"Bore Size","Bore Size",null,null,"Bore Size","Style","Inlet","Dec Size","Shutoff",null,null,null,null,null,null,null,null,50,null,null,"Bore Size","Style"]
[null,"Tan-colored cells are headers or describe the selection options",null,null,null,null,null,null,null,null,null,null,"Nozzle",null,"Shutoff Only","Shutoff with Integrated Tip",null,"5-40","125-250","13-30","13-60","18-30","30-125","30-150","30-200","95-200","12-53",null,null,null,null,null,null,null,null,null,"4116",60,null,13,"100 (Std)",null,null,null,null,4116,60,60,null,60,null,"Solid Bore","3/4\"","0416","1.5 in",0.75,"Fog Nozzle",13,"Fog Nozzle 13",null,null,13,"100 (Std)",{"$f":"CONCATENATE(BJ2,\" \",BK2)","v":"13 100 (Std)"},null,200,"100 (Std)",null,null,"Fog Nozzle",4116,60,"100 (Std)",{"$f":"CONCATENATE(BR2,\" \",BT2,\" @ \",BU2)","v":"Fog Nozzle 60 @ 100 (Std)"},null,null,null,"Fog Nozzle 125 @ 100",4116,4863,null,{"$f":"CONCATENATE($BZ2,\" \",CA2)","v":"Fog Nozzle 125 @ 100 4116"},{"$f":"CONCATENATE($BZ2,\" \",CB2)","v":"Fog Nozzle 125 @ 100 4863"},"Fog_Nozzle_125___100",null,null,"Fog Nozzle 125 @ 100 4116",null,null,null,"Solid Bore","3/8\"",0.375,{"$f":"CONCATENATE(CM2,\" \",CN2)","v":"Solid Bore 3/8\""},null,null,null,"Solid Bore 1.5 in","3/4\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 1.5 in","3/4\"",null,{"$f":"CONCATENATE(DD2,\" \",DI2,\" \",DG2,\" \",DE2,\" \",DJ2)","v":"Solid Bore No 1.5 in 3/4\" Yes"},{"$f":"CONCATENATE(DD2,\" \",DI2,\" \",DG2)","v":"Solid Bore No 1.5 in"},"Solid Bore","3/4\"","0416","1.5 in",0.75,"No","Yes","Solid Bore No 1.5 in",null,0.375,null,"3/8\"","7/8\"","1/2\"","7/8\"","1-1/8\"; 1/2\"","1-1/2\"; 1-1/4\"; 1\"","15/16\"; 1/2\"","1-1/8\"; 1/2\"",null,null,"Solid Bore No 1.5 in 1\" Yes","0416","1417","1499",null,"3/4\"","3_4_",null,"Solid Bore","3/4\"","0416","1.5 in",0.75,"No",{"$f":"CONCATENATE(EG2,\" \",EJ2,\" \",EL2,\" \",EH2,\" \",EI2)","v":"Solid Bore 1.5 in No 3/4\" 0416"},null,"Solid Bore 1.5 in No 3/4\" 0416",null,null,null,0.375,"3/8\"",{"$f":"CONCATENATE(ROUND(29.71*(ES2*ES2)*SQRT(EU$1),0),\" gpm @ 50 psi; RF = \",ROUND(1.57*(ES2*ES2)*EU$1,0))","v":"30 gpm @ 50 psi; RF = 11"},null,"Solid Bore","3/4\"","0416",{"$f":"_xlfn.CONCAT(EW2:EY2)","v":"Solid Bore3/4\"0416"},null,"Solid Bore3/4\"0416"]
[null,"Use the green-colored cells to make your selections (All cells must be filled in; information from \"FrontPage\" tab does not carry over to this page)",null,null,null,null,null,null,"This is a Nozzle with Increased RF (RF > 50 and <101 )",null,null,null,"Tip",null,"1 in","1.5 in",null,"100 (Std)","100 (Std)","100 (Std)","100 (Std)","100 (Std)","100 (Std)","100 (Std)","100 (Std)","100 (Std)","87 (CE)",null,null,null,null,null,null,null,null,null,"4116",95,null,25,"100 (Std)",null,null,null,null,4116,95,95,null,95,null,"Solid Bore","7/8\"","0416","1.5 in",0.875,"Fog Nozzle",25,"Fog Nozzle 25",null,null,25,"100 (Std)",{"$f":"CONCATENATE(BJ3,\" \",BK3)","v":"25 100 (Std)"},null,250,"100 (Std)",null,null,"Fog Nozzle",4116,60,75,{"$f":"CONCATENATE(BR3,\" \",BT3,\" @ \",BU3)","v":"Fog Nozzle 60 @ 75"},null,null,null,"Fog Nozzle 125 @ 75",4116,4863,null,{"$f":"CONCATENATE($BZ3,\" \",CA3)","v":"Fog Nozzle 125 @ 75 4116"},{"$f":"CONCATENATE($BZ3,\" \",CB3)","v":"Fog Nozzle 125 @ 75 4863"},null,null,null,"Fog Nozzle 125 @ 100 4863",null,null,null,"Solid Bore","1/2\"",0.5,{"$f":"CONCATENATE(CM3,\" \",CN3)","v":"Solid Bore 1/2\""},null,null,null,"Solid Bore 1.5 in","7/8\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 1.5 in","7/8\"",null,{"$f":"CONCATENATE(DD3,\" \",DI3,\" \",DG3,\" \",DE3,\" \",DJ3)","v":"Solid Bore No 1.5 in 7/8\" Yes"},{"$f":"CONCATENATE(DD3,\" \",DI3,\" \",DG3)","v":"Solid Bore No 1.5 in"},"Solid Bore","7/8\"","0416","1.5 in",0.875,"No","Yes","Solid Bore No 1.5 in",null,0.5,null,"1/2\"","15/16\"","7/8\"","15/16\"","15-16\"; 1/2\"","1-1/4\"; 1-1/8\"; 1\"",null,"1-1/4\"; 1-1/8\"; 1\"",null,null,"Solid Bore No 1.5 in 1/2\" Yes","1417",null,null,null,"7/8\"","7_8_",null,"Solid Bore","7/8\"","0416","1.5 in",0.875,"No",{"$f":"CONCATENATE(EG3,\" \",EJ3,\" \",EL3,\" \",EH3,\" \",EI3)","v":"Solid Bore 1.5 in No 7/8\" 0416"},null,"Solid Bore 1.5 in No 7/8\" 0416",null,null,null,0.5,"1/2\"","53 gpm @ 50 psi; RF = 20",null,"Solid Bore","7/8\"","0416",{"$f":"_xlfn.CONCAT(EW3:EY3)","v":"Solid Bore7/8\"0416"},null,"Solid Bore7/8\"0416"]
[null,"Blue-colored cells provide outputs based on your selections",null,null,null,null,null,null,null,null,null,null,"High Pressure",null,"1.5 in","2 in",null,75,75,null,null,null,75,75,75,75,null,null,null,null,null,null,null,null,null,null,"4116",125,null,40,"100 (Std)",null,null,null,null,4116,125,125,null,125,null,"Solid Bore","1\"","0416","1.5 in",1,"Fog Nozzle",40,"Fog Nozzle 40",null,null,40,"100 (Std)","40 100 (Std)",null,300,"100 (Std)",null,null,"Fog Nozzle",4116,60,"87 (CE)","Fog Nozzle 60 @ 87 (CE)",null,null,null,"Fog Nozzle 125 @ 87",4116,null,null,{"$f":"CONCATENATE($BZ4,\" \",CA4)","v":"Fog Nozzle 125 @ 87 4116"},null,null,null,null,"Fog Nozzle 125 @ 75 4116",null,null,null,"Solid Bore","5/8\"",0.625,"Solid Bore 5/8\"",null,null,null,"Solid Bore 1.5 in","1\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 1.5 in","1\"",null,"Solid Bore No 1.5 in 1\" Yes","Solid Bore No 1.5 in","Solid Bore","1\"","0416","1.5 in",1,"No","Yes","Solid Bore No 1.5 in",null,0.625,null,"5/8\"","1\"","15/16\"","1\"","1-1/16\"; 15/16\"","1-3/8\"; 1-1/4\"; 1\"",null,null,null,null,"Solid Bore No 1.5 in 1-1/16\" Yes","1499",null,null,null,"1\"","1_",null,"Solid Bore","1\"","0416","1.5 in",1,"No","Solid Bore 1.5 in No 1\" 0416",null,"Solid Bore 1.5 in No 1\" 0416",null,null,null,0.625,"5/8\"","82 gpm @ 50 psi; RF = 31",null,"Solid Bore","1\"","0416","Solid Bore1\"0416",null,"Solid Bore1\"0416"]
[null,"This shaded cell indicates an error has ocurred and you may need to modify some of your selections or contact our Customer Care team",null,null,null,null,null,null,"This Nozzle has a High RF (RF > 100 )",null,null,null,null,null,"2 in","2.5 in",null,"87 (CE)",null,null,null,null,"87 (CE)","87 (CE)",null,null,null,null,null,"5-40","100 (Std)",{"$f":"CONCATENATE(AD5,\" \",AE5)","v":"5-40 100 (Std)"},null,null,null,null,"4116",150,null,60,"100 (Std)",75,"87 (CE)",null,null,4116,150,150,null,150,null,"Solid Bore","1-1/8\"","0416","1.5 in",1.125,"Fog Nozzle",60,"Fog Nozzle 60",null,null,60,"100 (Std)","60 100 (Std)",null,350,"100 (Std)",null,null,"Fog Nozzle",4116,95,"100 (Std)","Fog Nozzle 95 @ 100 (Std)",null,null,null,"Fog Nozzle 13 @ 100",4802,null,null,{"$f":"CONCATENATE($BZ5,\" \",CA5)","v":"Fog Nozzle 13 @ 100 4802"},null,null,null,null,"Fog Nozzle 125 @ 75 4863",null,null,null,"Solid Bore","3/4\"",0.75,"Solid Bore 3/4\"",null,null,null,"Solid Bore 1.5 in","1-1/8\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 1.5 in","1-1/8\"",null,"Solid Bore No 1.5 in 1-1/8\" Yes","Solid Bore No 1.5 in","Solid Bore","1-1/8\"","0416","1.5 in",1.125,"No","Yes","Solid Bore No 1.5 in",null,0.75,null,"3/4\"","1-1/8\"","1\"","1-1/16\"","1-1/4\"; 1-1/8\"; 1\"",null,null,null,null,null,"Solid Bore No 1.5 in 1-1/4\" Yes","0416","1417","1499",null,"1-1/8\"","1_1_8_",null,"Solid Bore","1-1/8\"","0416","1.5 in",1.125,"No","Solid Bore 1.5 in No 1-1/8\" 0416",null,"Solid Bore 1.5 in No 1-1/8\" 0416",null,null,null,0.75,"3/4\"","118 gpm @ 50 psi; RF = 44",null,"Solid Bore","1-1/8\"","0416","Solid Bore1-1/8\"0416",null,"Solid Bore1-1/8\"0416"]
[null,"Orange-colored cell allows you to input your discount for Net Price",null,null,null,null,null,null,null,null,null,null,null,null,"2.5 in","3 in",null,null,null,null,null,null,null,null,null,null,null,null,null,"5-40",75,{"$f":"CONCATENATE(AD6,\" \",AE6)","v":"5-40 75"},null,null,null,null,"4802",13,null,95,"100 (Std)",75,"87 (CE)",null,null,4802,13,null,null,null,null,"Solid Bore","1-1/4\"","0416","1.5 in",1.25,"Fog Nozzle",95,"Fog Nozzle 95",null,null,60,"87 (CE)","60 87 (CE)",null,200,75,null,null,"Fog Nozzle",4116,95,75,"Fog Nozzle 95 @ 75",null,null,null,"Fog Nozzle 150 @ 100",4116,4863,null,"Fog Nozzle 150 @ 100 4116",{"$f":"CONCATENATE($BZ6,\" \",CB6)","v":"Fog Nozzle 150 @ 100 4863"},null,null,null,"Fog Nozzle 125 @ 87 4116",null,null,null,"Solid Bore","7/8\"",0.875,"Solid Bore 7/8\"",null,null,null,"Solid Bore 1.5 in","1-1/4\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 1.5 in","1-1/4\"",null,"Solid Bore No 1.5 in 1-1/4\" Yes","Solid Bore No 1.5 in","Solid Bore","1-1/4\"","0416","1.5 in",1.25,"No","Yes","Solid Bore No 1.5 in",null,0.875,null,"7/8\"","1-1/4\"","1-1/16\"","1-1/8\"",null,null,null,null,null,null,"Solid Bore No 1.5 in 1-1/8\" Yes","0416","1417","1499",null,"1-1/4\"","1_1_4_",null,"Solid Bore","1-1/4\"","0416","1.5 in",1.25,"No","Solid Bore 1.5 in No 1-1/4\" 0416",null,"Solid Bore 1.5 in No 1-1/4\" 0416",null,null,null,0.875,"7/8\"","161 gpm @ 50 psi; RF = 60",null,"Solid Bore","1-1/4\"","0416","Solid Bore1-1/4\"0416",null,"Solid Bore1-1/4\"0416"]
[null,{"$f":"FrontPage!E8","v":"Rev Date: 6/27/2022"},null,"Shutoffs and Shutoffs with Integral Tips",null,null,null,null,null,null,null,null,null,null,"3 in",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5-40","87 (CE)","5-40 87 (CE)",null,null,null,null,"4802",25,null,125,"100 (Std)",75,50,"87 (CE)",null,4802,25,null,null,null,null,"Solid Bore","3/8\"","1417","1.5 in",0.375,"Fog Nozzle",125,"Fog Nozzle 125",null,null,60,75,"60 75",null,250,75,null,null,"Fog Nozzle",4116,95,"87 (CE)","Fog Nozzle 95 @ 87 (CE)",null,null,null,"Fog Nozzle 150 @ 50",4863,null,null,"Fog Nozzle 150 @ 50 4863",null,null,null,null,"Fog Nozzle 13 @ 100 4802",null,null,null,"Solid Bore","15/16\"",0.9375,"Solid Bore 15/16\"",null,null,null,"Solid Bore 1.5 in","3/8\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 1.5 in","3/8\"",null,"Solid Bore No 1.5 in 3/8\" Yes","Solid Bore No 1.5 in","Solid Bore","3/8\"","1417","1.5 in",0.375,"No","Yes","Solid Bore No 1.5 in",null,0.9375,null,"15/16\"","1-3/8\"","1-1/8\"","1-3/16\"",null,null,null,null,null,null,"Solid Bore No 1.5 in 1-3/16\" Yes","1499",null,null,null,"3/8\"","3_8_",null,"Solid Bore","3/8\"","1417","1.5 in",0.375,"No","Solid Bore 1.5 in No 3/8\" 1417",null,"Solid Bore 1.5 in No 3/8\" 1417",null,null,null,0.9375,"15/16\"","185 gpm @ 50 psi; RF = 69",null,"Solid Bore","3/8\"","1417","Solid Bore3/8\"1417",null,"Solid Bore3/8\"1417"]
[null,"Shutoff Only or Shutoff with Integrated Tip","Inlet Size","Outlet Size",{"$f":"IF(RIGHT(B10,4)=\"only\",\"\",\"Bore Size\")","v":""},"Inlet Thread","Outlet Thread",{"$f":"IF(J10=\"yes\",\"\",\"Remove Pistol Grip?\")","v":"Remove Pistol Grip?"},"Style Number",{"$f":"IF(TRIM(I10)=\"2390\",\"\",\"ZT Inlet?\")","v":"ZT Inlet?"},"Custom Etch",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"125-250","100 (Std)","125-250 100 (Std)",null,null,null,null,"4802",40,null,150,"100 (Std)",75,50,"87 (CE)",null,4802,40,null,null,null,null,"Solid Bore","1/2\"","1417","1.5 in",0.5,"Fog Nozzle",150,"Fog Nozzle 150",null,null,95,"100 (Std)","95 100 (Std)",null,300,75,null,null,"Fog Nozzle",4116,125,"100 (Std)","Fog Nozzle 125 @ 100 (Std)",null,null,null,"Fog Nozzle 150 @ 75",4116,4863,null,"Fog Nozzle 150 @ 75 4116",{"$f":"CONCATENATE($BZ8,\" \",CB8)","v":"Fog Nozzle 150 @ 75 4863"},null,null,null,"Fog Nozzle 150 @ 100 4116",null,null,null,"Solid Bore","1\"",1,"Solid Bore 1\"",null,null,null,"Solid Bore 1.5 in","1/2\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 1.5 in","1/2\"",null,"Solid Bore No 1.5 in 1/2\" Yes","Solid Bore No 1.5 in","Solid Bore","1/2\"","1417","1.5 in",0.5,"No","Yes","Solid Bore No 1.5 in",null,1,null,"1\"",null,"1-3/16\"","1-1/4\"",null,null,null,null,null,null,"Solid Bore No 1.5 in 1-3/8\" Yes","1499",null,null,null,"1/2\"","1_2_",null,"Solid Bore","1/2\"","1417","1.5 in",0.5,"No","Solid Bore 1.5 in No 1/2\" 1417",null,"Solid Bore 1.5 in No 1/2\" 1417",null,null,null,1,"1\"","210 gpm @ 50 psi; RF = 79",null,"Solid Bore","1/2\"","1417","Solid Bore1/2\"1417",null,"Solid Bore1/2\"1417"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore","Stack Tips",null,null,null,null,null,null,null,null,null,null,null,null,null,"125-250",75,"125-250 75",null,null,null,null,"4824",200,null,161,50,null,null,null,null,4824,200,200,null,null,null,"Solid Bore","5/8\"","1417","1.5 in",0.625,"Fog Nozzle",161,"Fog Nozzle 161",null,null,95,75,"95 75",null,210,50,null,null,"Fog Nozzle",4116,125,75,"Fog Nozzle 125 @ 75",null,null,null,"Fog Nozzle 150 @ 87",4116,null,null,"Fog Nozzle 150 @ 87 4116",null,null,null,null,"Fog Nozzle 150 @ 100 4863",null,null,null,"Solid Bore","1-1/16\"",1.0625,"Solid Bore 1-1/16\"",null,null,null,"Solid Bore 1.5 in","5/8\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 1.5 in","5/8\"",null,"Solid Bore No 1.5 in 5/8\" Yes","Solid Bore No 1.5 in","Solid Bore","5/8\"","1417","1.5 in",0.625,"No","Yes","Solid Bore No 1.5 in",null,1.0625,null,"1-1/16\"",null,"1-1/4\"","1-3/8\"",null,null,null,null,null,null,"Solid Bore No 1.5 in 15/16\" Yes","1417","1499",null,null,"5/8\"","5_8_",null,"Solid Bore","5/8\"","1417","1.5 in",0.625,"No","Solid Bore 1.5 in No 5/8\" 1417",null,"Solid Bore 1.5 in No 5/8\" 1417",null,null,null,1.0625,"1-1/16\"","237 gpm @ 50 psi; RF = 89",null,"Solid Bore","5/8\"","1417","Solid Bore5/8\"1417",null,"Solid Bore5/8\"1417"]
[null,"Shutoff Only","2.5 in","1.5 in","15/16\"","NH","NH","No (Std)",2126,"No (Std)","No (Std)",null,null,null,"1.5 in","1.5 in",null,null,null,null,null,null,null,"INDIRECT(CONCATENATE(\"tHREAD\",SUBSTITUTE(B4,\" \",\"_\")))",null,null,null,null,null,"13-30","100 (Std)","13-30 100 (Std)",null,null,null,null,"4824",210,null,175,"100 (Std)",75,50,null,null,4824,null,null,210,null,null,"Solid Bore","3/4\"","1417","1.5 in",0.75,"Fog Nozzle",175,"Fog Nozzle 175",null,null,95,"87 (CE)","95 87 (CE)",null,250,50,null,null,"Fog Nozzle",4116,125,"87 (CE)","Fog Nozzle 125 @ 87 (CE)",null,null,null,"Fog Nozzle 161 @ 50",4863,null,null,"Fog Nozzle 161 @ 50 4863",null,null,null,null,"Fog Nozzle 150 @ 50 4863",null,null,null,"Solid Bore","1-1/8\"",1.125,"Solid Bore 1-1/8\"",null,null,null,"Solid Bore 1.5 in","3/4\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 1.5 in","15/16\"",null,"Solid Bore No 1.5 in 3/4\" Yes","Solid Bore No 1.5 in","Solid Bore","3/4\"","1417","1.5 in",0.75,"No","Yes","Solid Bore No 1.5 in",null,1.125,null,"1-1/8\"",null,"1-3/8\"",null,null,null,null,null,null,null,"Solid Bore No 1.5 in 3/4\" Yes","0416","1417",null,null,"3/4\"","3_4_",null,"Solid Bore","3/4\"","1417","1.5 in",0.75,"No","Solid Bore 1.5 in No 3/4\" 1417",null,"Solid Bore 1.5 in No 3/4\" 1417",null,null,null,1.125,"1-1/8\"","266 gpm @ 50 psi; RF = 99",null,"Solid Bore","3/4\"","1417","Solid Bore3/4\"1417",null,"Solid Bore3/4\"1417"]
[null,"List price",{"$f":"SUM(E11:K11)","v":698},null,{"$f":"IFERROR(IF(B10=\"shutoff only\",\"\",VLOOKUP(E10,ET:EU,2,FALSE)),\"Fix Bore Size\")","v":""},{"$f":"IF(OR(F10=\"Storz\",F10=\"BIM\"),_xlfn.XLOOKUP(\"storz\",M:M,P:P),0)","v":0},null,null,{"$f":"IFERROR(VLOOKUP(TRIM(I10),M72:P78,4,FALSE),\"\")","v":698},{"$f":"IF(TRIM(I10)=\"2390\",0,IF(J8=\"\",0,IF(J10=\"Yes\",_xlfn.XLOOKUP(\"zt\",M:M,P:P),0)))","v":0},null,null,null,null,"2.5 in","2.5 in",null,null,null,null,null,null,null,null,null,null,null,null,null,"13-60","100 (Std)","13-60 100 (Std)",null,null,null,null,"4824",250,null,185,50,null,null,null,null,4824,250,250,250,null,null,"Solid Bore","7/8\"","1417","1.5 in",0.875,"Fog Nozzle",200,"Fog Nozzle 200",null,null,125,"100 (Std)","125 100 (Std)",null,null,null,null,null,"Fog Nozzle",4116,150,"100 (Std)","Fog Nozzle 150 @ 100 (Std)",null,null,null,"Fog Nozzle 175 @ 100",4863,null,null,"Fog Nozzle 175 @ 100 4863",null,null,null,null,"Fog Nozzle 150 @ 75 4116",null,null,null,"Solid Bore","1-3/16\"",1.1875,"Solid Bore 1-3/16\"",null,null,null,"Solid Bore 1.5 in","7/8\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 1.5 in","1-1/16\"",null,"Solid Bore No 1.5 in 7/8\" Yes","Solid Bore No 1.5 in","Solid Bore","7/8\"","1417","1.5 in",0.875,"No","Yes","Solid Bore No 1.5 in",null,1.1875,null,"1-3/16\"",null,null,null,null,null,null,null,null,null,"Solid Bore No 1.5 in 3/8\" Yes","1417",null,null,null,"7/8\"","7_8_",null,"Solid Bore","7/8\"","1417","1.5 in",0.875,"No","Solid Bore 1.5 in No 7/8\" 1417",null,"Solid Bore 1.5 in No 7/8\" 1417",null,null,null,1.1875,"1-3/16\"","296 gpm @ 50 psi; RF = 111",null,"Solid Bore","7/8\"","1417","Solid Bore7/8\"1417",null,"Solid Bore7/8\"1417"]
[null,"Your Discount",null,"Net Price",null,{"$f":"ROUND(C11*(1-C12),2)","v":698},null,"Include Color Clips for Shutoff and/or Pistol Grip?",null,null,"Yes",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(B10,\" \",C10,\" \",D10,\" \",E10,\" \",I10)","v":"Shutoff Only 2.5 in 1.5 in 15/16\" 2126"},null,null,null,null,null,"18-30","100 (Std)","18-30 100 (Std)",null,null,null,null,"4824",265,null,200,"100 (Std)",75,null,null,null,4824,300,300,null,null,null,"Solid Bore","15/16\"","1417","1.5 in",0.9375,"Fog Nozzle",210,"Fog Nozzle 210",null,null,125,75,"125 75",null,null,null,null,null,"Fog Nozzle",4116,150,75,"Fog Nozzle 150 @ 75",null,null,null,"Fog Nozzle 175 @ 50",4863,null,null,"Fog Nozzle 175 @ 50 4863",null,null,null,null,"Fog Nozzle 150 @ 75 4863",null,null,null,"Solid Bore","1-1/4\"",1.25,"Solid Bore 1-1/4\"",null,null,null,"Solid Bore 1.5 in","15/16\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 1.5 in","1-3/16\"",null,"Solid Bore No 1.5 in 15/16\" Yes","Solid Bore No 1.5 in","Solid Bore","15/16\"","1417","1.5 in",0.9375,"No","Yes","Solid Bore No 1.5 in",null,1.25,null,"1-1/4\"",null,null,null,null,null,null,null,null,null,"Solid Bore No 1.5 in 5/8\" Yes","1417",null,null,null,"15/16\"","15_16_",null,"Solid Bore","15/16\"","1417","1.5 in",0.9375,"No","Solid Bore 1.5 in No 15/16\" 1417",null,"Solid Bore 1.5 in No 15/16\" 1417",null,null,null,1.25,"1-1/4\"","328 gpm @ 50 psi; RF = 123",null,"Solid Bore","15/16\"","1417","Solid Bore15/16\"1417",null,"Solid Bore15/16\"1417"]
[null,"Short Description",{"$f":"IF(B23=\"Error\",\"Fix Errors\",CONCATENATE(I10,\" \",C10,\" \",F10,\" \",D10,\" \",G10,IF(B10=\"shutoff only\",\"\",CONCATENATE(\" \",E10,\" bore size(s)\")),IF(TRIM(I10)=\"2390\",\"  \",IF(J10=\"yes\", \" PG\",IF(H10=\"yes\",\" NPG\",\" PG\"))),IF(TRIM(I10)=\"2390\",\"\",IF(J10=\"Yes\",\" ZT\",\"\")),IF(K10=\"Yes\",\" ETCH\",\"\")))","v":"2126 2.5 in NH 1.5 in NH PG"},null,null,null,null,null,null,null,null,null,"1 IN","NH",null,null,null,"1 in","1.5 in","2 in","2.5 in","3 in",null,null,null,null,null,null,null,"30-125","100 (Std)","30-125 100 (Std)",null,null,null,null,"4824",300,null,210,50,null,null,null,null,4824,350,null,null,null,null,"Solid Bore","1\"","1417","1.5 in",1,"Fog Nozzle",225,"Fog Nozzle 225",null,null,125,50,"125 50",null,null,null,null,null,"Fog Nozzle",4116,150,"87 (CE)","Fog Nozzle 150 @ 87 (CE)",null,null,null,"Fog Nozzle 175 @ 75",4863,null,null,"Fog Nozzle 175 @ 75 4863",null,null,null,null,"Fog Nozzle 150 @ 87 4116",null,null,null,"Solid Bore","1-3/8\"",1.375,"Solid Bore 1-3/8\"",null,null,null,"Solid Bore 1.5 in","1\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 1.5 in","1-3/8\"",null,"Solid Bore No 1.5 in 1\" Yes","Solid Bore No 1.5 in","Solid Bore","1\"","1417","1.5 in",1,"No","Yes","Solid Bore No 1.5 in",null,1.375,null,"1-3/8\"",null,null,null,null,null,null,null,null,null,"Solid Bore No 1.5 in 7/8\" Yes","0416","1417","1499",null,"1\"","1_",null,"Solid Bore","1\"","1417","1.5 in",1,"No","Solid Bore 1.5 in No 1\" 1417",null,"Solid Bore 1.5 in No 1\" 1417",null,null,null,1.375,"1-3/8\"","397 gpm @ 50 psi; RF = 148",null,"Solid Bore","1\"","1417","Solid Bore1\"1417",null,"Solid Bore1\"1417"]
[null,"Long Description",{"$f":"IF(B23=\"Error\",\"Some of your selections are not compatible with others; please correct the errors highlighted in RED\",CONCATENATE(\"Style \",I10,\" \",B10,\" with \",C10,\" \",F10,\" inlet; \",CONCATENATE(D10,\" \",G10,\" outlet; \"),IF(B10=\"shutoff only\",\"\",CONCATENATE(E10,\" bore size (\",E11,\"); \",)),IF(TRIM(I10)=\"2390\",\"playpipe with D-handles\",IF(J10=\"yes\",\"\",IF(H10=\"yes\",\"no pistol grip\",\"pistol grip\"))),IF(TRIM(I10)=\"2390\",\"\",IF(J10=\"Yes\",\"Zero-Torque Grip\",\"\")),IF(K10=\"Yes\",\"; Custom Etched\",\"\")))","v":"Style 2126 Shutoff Only with 2.5 in NH inlet; 1.5 in NH outlet; pistol grip"},null,null,null,null,"Akron Brass Part Number and Description",{"$f":"IF(AND(OR(F10=\"custom\",G10=\"custom\"),K10=\"yes\"),\"Contact Customer Care to request Custom Thread and Etch (800-228-1161)\",IF(OR(F10=\"custom\",G10=\"custom\"),\"Contact Customer Care to request Custom Thread (800-228-1161)\",IF(K10=\"Yes\",\"Contact Customer Care to request Custom Etch (800-228-1161)\",IF(B23=\"Error\",\"Incompatible selections; please correct errors highlighted in RED\",IFERROR(CONCATENATE(VLOOKUP(C13,DataSource!AH:AJ,2,FALSE),\"      \",VLOOKUP(C13,DataSource!AH:AJ,3,FALSE)),\"Version you've requested not yet created; contact Customer Care (800-228-1161)\")))))","v":"21264001      SHUTOFF 2.5NH  X 1.5NH#"},null,null,null,"1 IN","NPSH",null,null,"30-125",13,60,60,60,60,null,"Stack_Tips_Yes_2.5_in_1_1_4___ 1_1_8___ 1__No__Std",null,null,null,null,null,"30-125",75,"30-125 75",null,null,null,null,"4824",350,null,225,"100 (Std)",null,null,null,null,4826,200,200,null,null,null,"Solid Bore","1-1/8\"","1417","1.5 in",1.125,"Fog Nozzle",250,"Fog Nozzle 250",null,null,125,"87 (CE)","125 87 (CE)",null,null,null,null,null,"Fog Nozzle",4802,13,"100 (Std)","Fog Nozzle 13 @ 100 (Std)",null,null,null,"Fog Nozzle 185 @ 50",4863,null,null,"Fog Nozzle 185 @ 50 4863",null,null,null,null,"Fog Nozzle 161 @ 50 4863",null,null,null,"Stack Tips","1-1/8\"; 1/2\"",0.5,"Stack Tips 1-1/8\"; 1/2\"",null,null,null,"Solid Bore 1.5 in","1-1/8\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 2.5 in","7/8\"",null,"Solid Bore No 1.5 in 1-1/8\" Yes","Solid Bore No 1.5 in","Solid Bore","1-1/8\"","1417","1.5 in",1.125,"No","Yes","Solid Bore No 2.5 in",null,0.875,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore No 2.5 in 1\" Yes","0489",null,null,null,"1-1/8\"","1_1_8_",null,"Solid Bore","1-1/8\"","1417","1.5 in",1.125,"No","Solid Bore 1.5 in No 1-1/8\" 1417",null,"Solid Bore 1.5 in No 1-1/8\" 1417",null,null,null,null,null,null,null,"Solid Bore","1-1/8\"","1417","Solid Bore1-1/8\"1417",null,"Solid Bore1-1/8\"1417"]
[null,null,null,null,null,null,null,null,null,null,null,null,"1 IN","STORZ",null,null,"30-150",25,95,95,95,95,null,"Stack_Tips_Yes_2.5_in_1_1_4___1_1_8___1__No__Std",null,null,null,null,null,"30-125","87 (CE)","30-125 87 (CE)",null,null,null,null,"4826",200,null,250,"100 (Std)",75,50,null,null,4826,null,null,210,null,null,"Solid Bore","1-1/4\"","1417","1.5 in",1.25,"Fog Nozzle",265,"Fog Nozzle 265",null,null,150,"100 (Std)","150 100 (Std)",null,null,null,null,null,"Fog Nozzle",4802,25,"100 (Std)","Fog Nozzle 25 @ 100 (Std)",null,null,null,"Fog Nozzle 200 @ 100",4826,4863,null,"Fog Nozzle 200 @ 100 4826","Fog Nozzle 200 @ 100 4863",null,null,null,"Fog Nozzle 175 @ 100 4863",null,null,null,"Stack Tips","15-16\"; 1/2\"",0.5,"Stack Tips 15-16\"; 1/2\"",null,null,null,"Solid Bore 1.5 in","1-1/4\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 2.5 in","15/16\"",null,"Solid Bore No 1.5 in 1-1/4\" Yes","Solid Bore No 1.5 in","Solid Bore","1-1/4\"","1417","1.5 in",1.25,"No","Yes","Solid Bore No 2.5 in",null,0.9375,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore No 2.5 in 1-1/4\" Yes","0489",null,null,null,"1-1/4\"","1_1_4_",null,"Solid Bore","1-1/4\"","1417","1.5 in",1.25,"No","Solid Bore 1.5 in No 1-1/4\" 1417",null,"Solid Bore 1.5 in No 1-1/4\" 1417",null,null,null,null,null,null,null,"Solid Bore","1-1/4\"","1417","Solid Bore1-1/4\"1417",null,"Solid Bore1-1/4\"1417"]
[null,"Notes: ","You can make any notes about what you want, or anything else, in this space",null,null,null,null,null,null,null,null,null,"1.5 in",null,null,null,"30-200",40,125,125,125,125,null,null,null,null,null,null,null,"30-150","100 (Std)","30-150 100 (Std)",null,null,null,null,"4826",210,null,265,50,null,null,null,null,4826,250,250,250,null,null,"Solid Bore","7/8\"","1445","1.5 in",0.875,"Fog Nozzle",300,"Fog Nozzle 300",null,null,150,75,"150 75",null,null,null,null,null,"Fog Nozzle",4802,40,"100 (Std)","Fog Nozzle 40 @ 100 (Std)",null,null,null,"Fog Nozzle 200 @ 75",4826,4863,null,"Fog Nozzle 200 @ 75 4826","Fog Nozzle 200 @ 75 4863",null,null,null,"Fog Nozzle 175 @ 50 4863",null,null,null,"Stack Tips","15/16\"; 1/2\"",0.5,"Stack Tips 15/16\"; 1/2\"",null,null,null,"Solid Bore 1.5 in","7/8\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 2.5 in","1\"",null,"Solid Bore Yes 1.5 in 7/8\" No (Std)","Solid Bore Yes 1.5 in","Solid Bore","7/8\"","1445","1.5 in",0.875,"Yes","No (Std)","Solid Bore No 2.5 in",null,1,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore No 2.5 in 1-1/8\" Yes","0489",null,null,null,"7/8\"","7_8_",null,"Solid Bore","7/8\"","1445","1.5 in",0.875,"Yes","Solid Bore 1.5 in Yes 7/8\" 1445",null,"Solid Bore 1.5 in Yes 7/8\" 1445",null,null,null,null,null,null,null,"Solid Bore","7/8\"","1445","Solid Bore7/8\"1445",null,"Solid Bore7/8\"1445"]
[null,null,null,null,null,null,null,null,null,null,null,null,"1.5 in",null,null,null,"95-200",null,150,150,150,150,null,null,null,null,null,null,null,"30-150",75,"30-150 75",null,null,null,null,"4826",250,null,300,"100 (Std)",75,null,null,null,4826,300,300,null,null,null,"Solid Bore","15/16\"","1445","1.5 in",0.9375,"Fog Nozzle",350,"Fog Nozzle 350",null,null,150,50,"150 50",null,null,null,null,null,"Fog Tip",4824,200,"100 (Std)","Fog Tip 200 @ 100 (Std)",null,null,null,"Fog Nozzle 210 @ 50",4826,null,null,"Fog Nozzle 210 @ 50 4826",null,null,null,null,"Fog Nozzle 175 @ 75 4863",null,null,null,"Stack Tips","1-1/16\"; 15/16\"",0.9375,"Stack Tips 1-1/16\"; 15/16\"",null,null,null,"Solid Bore 1.5 in","15/16\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 2.5 in","1-1/8\"",null,"Solid Bore Yes 1.5 in 15/16\" No (Std)","Solid Bore Yes 1.5 in","Solid Bore","15/16\"","1445","1.5 in",0.9375,"Yes","No (Std)","Solid Bore No 2.5 in",null,1.125,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore No 2.5 in 1-3/8\" Yes","0489",null,null,null,"15/16\"","15_16_",null,"Solid Bore","15/16\"","1445","1.5 in",0.9375,"Yes","Solid Bore 1.5 in Yes 15/16\" 1445",null,"Solid Bore 1.5 in Yes 15/16\" 1445",null,null,null,null,null,null,null,"Solid Bore","15/16\"","1445","Solid Bore15/16\"1445",null,"Solid Bore15/16\"1445"]
[null,null,null,null,null,null,null,null,null,null,null,null,"1.5 in",null,null,null,"125-250",null,161,161,161,161,null,null,null,null,null,null,null,"30-150","87 (CE)","30-150 87 (CE)",null,null,null,null,"4826",300,null,350,"100 (Std)",null,null,null,null,4826,350,null,null,null,null,"Solid Bore","1\"","1445","1.5 in",1,"Fog Tip",95,"Fog Tip 95",null,null,150,"87 (CE)","150 87 (CE)",null,null,null,null,null,"Fog Tip",4824,250,"100 (Std)","Fog Tip 250 @ 100 (Std)",null,null,null,"Fog Nozzle 225 @ 100",4863,null,null,"Fog Nozzle 225 @ 100 4863",null,null,null,null,"Fog Nozzle 185 @ 50 4863",null,null,null,"Stack Tips","1-1/4\"; 1-1/8\"; 1\"",1,"Stack Tips 1-1/4\"; 1-1/8\"; 1\"",null,null,null,"Solid Bore 1.5 in","1\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 2.5 in","1-1/4\"",null,"Solid Bore Yes 1.5 in 1\" No (Std)","Solid Bore Yes 1.5 in","Solid Bore","1\"","1445","1.5 in",1,"Yes","No (Std)","Solid Bore No 2.5 in",null,1.25,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore No 2.5 in 15/16\" Yes","0489",null,null,null,"1\"","1_",null,"Solid Bore","1\"","1445","1.5 in",1,"Yes","Solid Bore 1.5 in Yes 1\" 1445",null,"Solid Bore 1.5 in Yes 1\" 1445",null,null,null,null,null,null,null,"Solid Bore","1\"","1445","Solid Bore1\"1445",null,"Solid Bore1\"1445"]
[null,null,null,null,null,null,null,null,null,null,null,null,"1.5 IN",null,null,null,null,null,175,175,175,175,null,null,null,null,null,null,null,"30-200","100 (Std)","30-200 100 (Std)",null,null,null,null,"4826",350,null,null,null,null,null,null,null,4863,95,null,null,null,null,"Solid Bore","1-1/16\"","1445","1.5 in",1.0625,"Fog Tip",125,"Fog Tip 125",null,null,161,50,"161 50",null,null,null,null,null,"Fog Tip",4824,300,"100 (Std)","Fog Tip 300 @ 100 (Std)",null,null,null,"Fog Nozzle 25 @ 100",4802,null,null,"Fog Nozzle 25 @ 100 4802",null,null,null,null,"Fog Nozzle 200 @ 100 4826",null,null,null,"Stack Tips","1-1/2\"; 1-1/4\"; 1\"",1,"Stack Tips 1-1/2\"; 1-1/4\"; 1\"",null,null,null,"Solid Bore 1.5 in","1-1/16\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 2.5 in","1-3/8\"",null,"Solid Bore Yes 1.5 in 1-1/16\" No (Std)","Solid Bore Yes 1.5 in","Solid Bore","1-1/16\"","1445","1.5 in",1.0625,"Yes","No (Std)","Solid Bore No 2.5 in",null,1.375,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore No 2.5 in 7/8\" Yes","0489",null,null,null,"1-1/16\"","1_1_16_",null,"Solid Bore","1-1/16\"","1445","1.5 in",1.0625,"Yes","Solid Bore 1.5 in Yes 1-1/16\" 1445",null,"Solid Bore 1.5 in Yes 1-1/16\" 1445",null,null,null,null,null,null,null,"Solid Bore","1-1/16\"","1445","Solid Bore1-1/16\"1445",null,"Solid Bore1-1/16\"1445"]
[null,null,null,{"$f":"CONCATENATE(I10,\" \",C10,\" \",F10,\" \",D10,\" \",E10,\" \",G10,IF(B10=\"Fog Tip\",\"\",IF(D10=\"no\",\" \",IF(H10=\"yes\",\" NPG\",\" PG\"))),IF(B10=\"Fog Tip\",\"\",IF(J10=\"Yes\",\" ZT\",\"\")),IF(K10=\"Yes\",\" ETCH\",\"\"))","v":"2126 2.5 in NH 1.5 in 15/16\" NH PG"},null,null,null,null,{"$f":"CONCATENATE(SUBSTITUTE(B10,\" \",\"_\"),\"_\",SUBSTITUTE(D10,\"-\",\"_\"))","v":"Shutoff_Only_1.5 in"},null,null,null,"1.5 in",null,null,null,null,null,200,200,200,200,null,null,null,null,null,null,null,"30-200",75,"30-200 75",null,null,null,null,"4863",95,null,null,null,null,null,null,null,4863,125,125,125,null,null,"Solid Bore","1-1/8\"","1445","1.5 in",1.125,"Fog Tip",150,"Fog Tip 150",null,null,175,"100 (Std)","175 100 (Std)",null,null,null,null,null,"Fog Tip",4824,350,"100 (Std)","Fog Tip 350 @ 100 (Std)",null,null,null,"Fog Nozzle 250 @ 100",4826,null,null,"Fog Nozzle 250 @ 100 4826",null,null,null,null,"Fog Nozzle 200 @ 100 4863",null,null,null,"Stack Tips","1-3/8\"; 1-1/4\"; 1\"",1,"Stack Tips 1-3/8\"; 1-1/4\"; 1\"",null,null,null,"Solid Bore 1.5 in","1-1/8\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 2.5 in","1-1/16\"",null,"Solid Bore Yes 1.5 in 1-1/8\" No (Std)","Solid Bore Yes 1.5 in","Solid Bore","1-1/8\"","1445","1.5 in",1.125,"Yes","No (Std)","Solid Bore Yes 1.5 in",null,0.5,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 1.5 in 1\" No (Std)","1445",null,null,null,"1-1/8\"","1_1_8_",null,"Solid Bore","1-1/8\"","1445","1.5 in",1.125,"Yes","Solid Bore 1.5 in Yes 1-1/8\" 1445",null,"Solid Bore 1.5 in Yes 1-1/8\" 1445",null,null,null,null,null,null,null,"Solid Bore","1-1/8\"","1445","Solid Bore1-1/8\"1445",null,"Solid Bore1-1/8\"1445"]
[null,null,null,{"$f":"CONCATENATE(\"_\",SUBSTITUTE(C10,\" \",\"_\"),\"_\",SUBSTITUTE(D10,\"-\",\"_\"))","v":"_2.5_in_1.5 in"},"Solid Bore No 1.5 in",null,null,null,"Bore,Shutoff,Inlet,Remove Grip",null,null,null,"1.5 IN",null,null,null,null,null,210,210,210,210,null,null,null,null,null,null,null,"95-200","100 (Std)","95-200 100 (Std)",null,null,null,null,"4863",125,null,null,null,null,null,null,null,4863,150,150,150,null,null,"Solid Bore","1-3/16\"","1445","1.5 in",1.1875,"Fog Tip",161,"Fog Tip 161",null,null,175,75,"175 75",null,null,null,null,null,"Fog Tip",4824,200,75,"Fog Tip 200 @ 75",null,null,null,"Fog Nozzle 250 @ 50",4826,null,null,"Fog Nozzle 250 @ 50 4826",null,null,null,null,"Fog Nozzle 200 @ 75 4826",null,null,null,null,null,null,null,null,null,null,"Solid Bore 1.5 in","1-3/16\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 2.5 in","1-3/16\"",null,"Solid Bore Yes 1.5 in 1-3/16\" No (Std)","Solid Bore Yes 1.5 in","Solid Bore","1-3/16\"","1445","1.5 in",1.1875,"Yes","No (Std)","Solid Bore Yes 1.5 in",null,0.875,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 1.5 in 1/2\" No (Std)","1447",null,null,null,"1-3/16\"","1_3_16_",null,"Solid Bore","1-3/16\"","1445","1.5 in",1.1875,"Yes","Solid Bore 1.5 in Yes 1-3/16\" 1445",null,"Solid Bore 1.5 in Yes 1-3/16\" 1445",null,null,null,null,null,null,null,"Solid Bore","1-3/16\"","1445","Solid Bore1-3/16\"1445",null,"Solid Bore1-3/16\"1445"]
[null,null,null,{"$f":"CONCATENATE(C10,\" \",D10)","v":"2.5 in 1.5 in"},null,null,null,null,"Solid Bore No 1.5 in 1\" Yes",null,null,null,"2 IN","STORZ",null,null,null,null,225,225,225,225,null,null,null,null,null,null,null,"95-200",75,"95-200 75",null,null,null,null,"4863",150,null,null,null,null,null,null,null,4863,175,175,175,null,null,"Solid Bore","1-1/4\"","1445","1.5 in",1.25,"Fog Tip",175,"Fog Tip 175",null,null,175,50,"175 50",null,null,null,null,null,"Fog Tip",4824,250,75,"Fog Tip 250 @ 75",null,null,null,"Fog Nozzle 250 @ 75",4826,null,null,{"$f":"CONCATENATE($BZ22,\" \",CA22)","v":"Fog Nozzle 250 @ 75 4826"},null,null,null,null,"Fog Nozzle 200 @ 75 4863",null,null,null,null,null,null,null,null,null,null,"Solid Bore 1.5 in","1-1/4\"","1.5 in","Solid Bore 1.5 in",null,"Stack Tips 1.5 in","1-1/8\"; 1/2\"",null,"Solid Bore Yes 1.5 in 1-1/4\" No (Std)","Solid Bore Yes 1.5 in","Solid Bore","1-1/4\"","1445","1.5 in",1.25,"Yes","No (Std)","Solid Bore Yes 1.5 in",null,0.9375,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 1.5 in 1\" Yes","1445",null,null,null,"1-1/4\"","1_1_4_",null,"Solid Bore","1-1/4\"","1445","1.5 in",1.25,"Yes","Solid Bore 1.5 in Yes 1-1/4\" 1445",null,"Solid Bore 1.5 in Yes 1-1/4\" 1445",null,null,null,null,null,null,null,"Solid Bore","1-1/4\"","1445","Solid Bore1-1/4\"1445",null,"Solid Bore1-1/4\"1445"]
[null,{"$f":"IF(OR(C23=\"False\",D23=\"False\",E23=\"False\",H23=\"False\",J23=\"False\",F23=\"False\",I23=\"False\"),\"Error\",\"Okay\")","v":"Okay"},{"$f":"IFERROR(VLOOKUP(CONCATENATE(B10,C10),C28:C44,1,FALSE),\"False\")","v":"Shutoff Only2.5 in"},{"$f":"IFERROR(VLOOKUP(CONCATENATE(C10,D10),D28:D48,1,FALSE),\"False\")","v":"2.5 in1.5 in"},{"$f":"IF(E8=\"\",\"Okay\",IFERROR(VLOOKUP(CONCATENATE(E10,I10),E28:E84,1,FALSE),\"False\"))","v":"Okay"},{"$f":"IFERROR(VLOOKUP(CONCATENATE(C10,F10),F28:F68,1,FALSE),\"false\")","v":"2.5 inNH"},null,{"$f":"IF(D10=\"No\",IF(H10=\"yes\",IF(B10=\"stack tips\",\"okay\",\"False\"),\"Okay\"),\"Okay\")","v":"Okay"},{"$f":"IFERROR(VLOOKUP(CONCATENATE(B10,C10,D10,I10),I27:I89,1,FALSE),\"False\")","v":"shutoff only2.5 in1.5 in2126"},{"$f":"IF(D10=\"No\",IF(J10=\"yes\",\"False\",\"Okay\"),\"Okay\")","v":"Okay"},null,null,"2.5 IN","NH",null,null,null,null,250,250,250,250,null,null,null,null,null,null,null,"12-53","87 (CE)","12-53 87 (CE)",null,null,null,null,"4863",161,null,null,null,null,null,null,null,4863,200,200,null,null,null,"Solid Bore","1-3/8\"","1445","1.5 in",1.375,"Fog Tip",200,"Fog Tip 200",null,null,185,50,"185 50",null,null,null,null,null,"Fog Tip",4824,300,75,"Fog Tip 300 @ 75",null,null,null,"Fog Nozzle 265 @ 50",4826,null,null,{"$f":"CONCATENATE($BZ23,\" \",CA23)","v":"Fog Nozzle 265 @ 50 4826"},null,null,null,null,"Fog Nozzle 210 @ 50 4826",null,null,null,null,null,null,null,null,null,null,"Solid Bore 1.5 in","1-3/8\"","1.5 in","Solid Bore 1.5 in",null,"Stack Tips 1.5 in","15-16\"; 1/2\"",null,"Solid Bore Yes 1.5 in 1-3/8\" No (Std)","Solid Bore Yes 1.5 in","Solid Bore","1-3/8\"","1445","1.5 in",1.375,"Yes","No (Std)","Solid Bore Yes 1.5 in",null,1,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 1.5 in 1-1/16\" Yes","1445",null,null,null,"1-3/8\"","1_3_8_",null,"Solid Bore","1-3/8\"","1445","1.5 in",1.375,"Yes","Solid Bore 1.5 in Yes 1-3/8\" 1445",null,"Solid Bore 1.5 in Yes 1-3/8\" 1445",null,null,null,null,null,null,null,"Solid Bore","1-3/8\"","1445","Solid Bore1-3/8\"1445",null,"Solid Bore1-3/8\"1445"]
[null,null,null,null,{"$f":"CONCATENATE(SUBSTITUTE(B10,\" \",\"_\"),\"_\",D10,\"_\",SUBSTITUTE(C10,\" \",\"_\"))","v":"Shutoff_Only_1.5 in_2.5_in"},null,null,null,{"$f":"CONCATENATE(B10,\" \",C10,\" \",D10,\" \",E10,\" \",I10)","v":"Shutoff Only 2.5 in 1.5 in 15/16\" 2126"},null,null,null,"2.5 IN","NPSH",null,null,null,null,300,300,300,300,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4863",175,null,null,null,null,null,null,null,4863,null,null,161,null,null,"Solid Bore","1/2\"","1447","1.5 in",0.5,"Fog Tip",210,"Fog Tip 210",null,null,200,"100 (Std)","200 100 (Std)",null,null,null,null,null,"Fog Tip",4824,210,50,"Fog Tip 210 @ 50",null,null,null,"Fog Nozzle 300 @ 100",4826,null,null,{"$f":"CONCATENATE($BZ24,\" \",CA24)","v":"Fog Nozzle 300 @ 100 4826"},null,null,null,null,"Fog Nozzle 225 @ 100 4863",null,null,null,null,null,null,null,null,null,null,"Solid Bore 1.5 in","1/2\"","1.5 in","Solid Bore 1.5 in",null,"Stack Tips 1.5 in","1-1/16\"; 15/16\"",null,"Solid Bore Yes 1.5 in 1/2\" No (Std)","Solid Bore Yes 1.5 in","Solid Bore","1/2\"","1447","1.5 in",0.5,"Yes","No (Std)","Solid Bore Yes 1.5 in",null,1.0625,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 1.5 in 1-1/4\" Yes","1445",null,null,null,"1/2\"","1_2_",null,"Solid Bore","1/2\"","1447","1.5 in",0.5,"Yes","Solid Bore 1.5 in Yes 1/2\" 1447",null,"Solid Bore 1.5 in Yes 1/2\" 1447",null,null,null,null,null,null,null,"Solid Bore","1/2\"","1447","Solid Bore1/2\"1447",null,"Solid Bore1/2\"1447"]
[null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(SUBSTITUTE(B10,\" \",\"_\"),\"_\",D10,\"_\",SUBSTITUTE(C10,\" \",\"_\"),\"_\",VLOOKUP(E10,ED:EE,2,FALSE),\"_\",IF(D10=\"no\",\"Yes\",IF(H10=\"yes\",\"Yes\",\"No__Std\")))","v":"Shutoff_Only_1.5 in_2.5_in_15_16__No__Std"},null,null,null,"2.5 IN","FDNY",null,null,null,null,350,350,350,350,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4863",185,null,null,null,null,null,null,null,4863,null,null,185,null,null,"Solid Bore","7/8\"","1499","1.5 in",0.875,"Fog Tip",225,"Fog Tip 225",null,null,200,75,"200 75",null,null,null,null,null,"Fog Tip",4824,265,50,"Fog Tip 265 @ 50",null,null,null,"Fog Nozzle 300 @ 75",4826,null,null,"Fog Nozzle 300 @ 75 4826",null,null,null,null,"Fog Nozzle 25 @ 100 4802",null,null,null,null,null,null,null,null,null,null,"Solid Bore 1.5 in","7/8\"","1.5 in","Solid Bore 1.5 in",null,"Stack Tips 1.5 in","1-1/4\"; 1-1/8\"; 1\"",null,"Solid Bore No 1.5 in 7/8\" Yes","Solid Bore No 1.5 in","Solid Bore","7/8\"","1499","1.5 in",0.875,"No","Yes","Solid Bore Yes 1.5 in",null,1.125,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 1.5 in 1-1/8\" Yes","1445",null,null,null,"7/8\"","7_8_",null,"Solid Bore","7/8\"","1499","1.5 in",0.875,"No","Solid Bore 1.5 in No 7/8\" 1499",null,"Solid Bore 1.5 in No 7/8\" 1499",null,null,null,null,null,null,null,"Solid Bore","7/8\"","1499","Solid Bore7/8\"1499",null,"Solid Bore7/8\"1499"]
[null,null,null,null,null,null,null,null,"Solid_Bore_Yes_1.5_in_1__No__Std",null,null,null,"2.5 IN","NYCORP",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4863",200,null,null,null,null,null,null,null,4866,95,null,null,null,null,"Solid Bore","15/16\"","1499","1.5 in",0.9375,"Fog Tip",250,"Fog Tip 250",null,null,210,50,"210 50",null,null,null,null,null,"Fog Tip",4824,250,50,"Fog Tip 250 @ 50",null,null,null,"Fog Nozzle 350 @ 100",4826,null,null,"Fog Nozzle 350 @ 100 4826",null,null,null,null,"Fog Nozzle 250 @ 100 4826",null,null,null,null,null,null,null,null,null,null,"Solid Bore 1.5 in","15/16\"","1.5 in","Solid Bore 1.5 in",null,"Stack Tips 1.5 in","15/16\"; 1/2\"",null,"Solid Bore No 1.5 in 15/16\" Yes","Solid Bore No 1.5 in","Solid Bore","15/16\"","1499","1.5 in",0.9375,"No","Yes","Solid Bore Yes 1.5 in",null,1.1875,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 1.5 in 1-3/16\" Yes","1445",null,null,null,"15/16\"","15_16_",null,"Solid Bore","15/16\"","1499","1.5 in",0.9375,"No","Solid Bore 1.5 in No 15/16\" 1499",null,"Solid Bore 1.5 in No 15/16\" 1499",null,null,null,null,null,null,null,"Solid Bore","15/16\"","1499","Solid Bore15/16\"1499",null,"Solid Bore15/16\"1499"]
[null,null,null,null,null,null,null,null,"shutoff only1 in1 in2102",null,null,null,"2.5 IN","PITT6",null,null,null,null,"NH","NPSH","FDNY","NYCORP","PCT","Custom",null,null,null,null,null,null,null,null,null,null,null,null,"4863",225,null,null,null,null,null,null,null,4866,125,125,125,null,null,"Solid Bore","1\"","1499","1.5 in",1,"Fog Tip",265,"Fog Tip 265",null,null,225,"100 (Std)","225 100 (Std)",null,null,null,null,null,"Fog Nozzle",4826,200,"100 (Std)","Fog Nozzle 200 @ 100 (Std)",null,null,null,"Fog Nozzle 40 @ 100",4802,null,null,"Fog Nozzle 40 @ 100 4802",null,null,null,null,"Fog Nozzle 250 @ 50 4826",null,null,null,null,null,null,null,null,null,null,"Solid Bore 1.5 in","1\"","1.5 in","Solid Bore 1.5 in",null,"Stack Tips 2.5 in","1-1/8\"; 1/2\"",null,"Solid Bore No 1.5 in 1\" Yes","Solid Bore No 1.5 in","Solid Bore","1\"","1499","1.5 in",1,"No","Yes","Solid Bore Yes 1.5 in",null,1.25,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 1.5 in 1-3/8\" Yes","1445",null,null,null,"1\"","1_",null,"Solid Bore","1\"","1499","1.5 in",1,"No","Solid Bore 1.5 in No 1\" 1499",null,"Solid Bore 1.5 in No 1\" 1499",null,null,null,null,null,null,null,"Solid Bore","1\"","1499","Solid Bore1\"1499",null,"Solid Bore1\"1499"]
[null,null,"Shutoff Only1 in","1 in1 in","7/8\"2431","1.5 inNH",null,null,"shutoff only1.5 in1.5 in2127",null,null,null,"2.5 IN","BAT",null,null,null,"SBTHREAD1.5 in",{"$f":"IF($B10=\"Solid Bore\",IF(OR(TRIM($I10)=\"0416\",$D10=\"yes\"),S27,\"\"),S27)","v":"NH"},"NPSH","FDNY","NYCORP","PCT","Custom",null,null,null,null,null,null,null,null,null,null,null,null,"4866",95,null,null,null,null,null,null,null,4866,150,150,150,null,null,"Solid Bore","1-1/16\"","1499","1.5 in",1.0625,"Fog Tip",300,"Fog Tip 300",null,null,250,"100 (Std)","250 100 (Std)",null,null,null,null,null,"Fog Nozzle",4826,250,"100 (Std)","Fog Nozzle 250 @ 100 (Std)",null,null,null,"Fog Nozzle 60 @ 100",4116,null,null,"Fog Nozzle 60 @ 100 4116",null,null,null,null,"Fog Nozzle 250 @ 75 4826",null,null,null,null,null,null,null,null,null,null,"Solid Bore 1.5 in","1-1/16\"","1.5 in","Solid Bore 1.5 in",null,"Stack Tips 2.5 in","1-1/4\"; 1-1/8\"; 1\"",null,"Solid Bore No 1.5 in 1-1/16\" Yes","Solid Bore No 1.5 in","Solid Bore","1-1/16\"","1499","1.5 in",1.0625,"No","Yes","Solid Bore Yes 1.5 in",null,1.375,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 1.5 in 15/16\" Yes","1445",null,null,null,"1-1/16\"","1_1_16_",null,"Solid Bore","1-1/16\"","1499","1.5 in",1.0625,"No","Solid Bore 1.5 in No 1-1/16\" 1499",null,"Solid Bore 1.5 in No 1-1/16\" 1499",null,null,null,null,null,null,null,"Solid Bore","1-1/16\"","1499","Solid Bore1-1/16\"1499",null,"Solid Bore1-1/16\"1499"]
[null,null,"Shutoff Only1.5 in","1.5 in1.5 in","15/16\"2431","1.5 inNPSH",{"$f":"VLOOKUP(C13,DataSource!AH:AJ,2,FALSE)","v":"21264001"},{"$f":"VLOOKUP(C13,DataSource!AH:AJ,3,FALSE)","v":"SHUTOFF 2.5NH  X 1.5NH#"},"shutoff only2 in1.5 in2127",null,null,null,"2.5 IN","CSA",null,null,null,"SBTHREAD1 in","NH","NPSH","Custom",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4866",125,null,null,null,null,null,null,null,4866,175,175,175,null,null,"Solid Bore","1-1/8\"","1499","1.5 in",1.125,"Fog Tip",350,"Fog Tip 350",null,null,250,75,"250 75",null,null,null,null,null,"Fog Nozzle",4826,300,"100 (Std)","Fog Nozzle 300 @ 100 (Std)",null,null,null,"Fog Nozzle 60 @ 75",4116,null,null,"Fog Nozzle 60 @ 75 4116",null,null,null,null,"Fog Nozzle 265 @ 50 4826",null,null,null,null,null,null,null,null,null,null,"Solid Bore 1.5 in","1-1/8\"","1.5 in","Solid Bore 1.5 in",null,"Stack Tips 2.5 in","1-1/2\"; 1-1/4\"; 1\"",null,"Solid Bore No 1.5 in 1-1/8\" Yes","Solid Bore No 1.5 in","Solid Bore","1-1/8\"","1499","1.5 in",1.125,"No","Yes","Solid Bore Yes 2.5 in",null,0.875,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 1.5 in 7/8\" Yes","1445",null,null,null,"1-1/8\"","1_1_8_",null,"Solid Bore","1-1/8\"","1499","1.5 in",1.125,"No","Solid Bore 1.5 in No 1-1/8\" 1499",null,"Solid Bore 1.5 in No 1-1/8\" 1499",null,null,null,null,null,null,null,"Solid Bore","1-1/8\"","1499","Solid Bore1-1/8\"1499",null,"Solid Bore1-1/8\"1499"]
[null,null,"Shutoff Only2 in","2 in1.5 in","1\"2431","1.5 inFDNY",null,null,"shutoff only2.5 in1.5 in2126",null,null,null,"2.5 IN","QST",null,null,null,"SBTHREAD2.5 in","NH","NPSH","FDNY","NYCORP","PITT6","BAT","CSA","QST","Custom",null,null,null,null,null,null,null,null,null,"4866",150,null,null,null,null,null,null,null,4866,200,200,null,null,null,"Solid Bore","1-3/16\"","1499","1.5 in",1.1875,null,null,null,null,null,250,50,"250 50",null,null,null,null,null,"Fog Nozzle",4826,350,"100 (Std)","Fog Nozzle 350 @ 100 (Std)",null,null,null,"Fog Nozzle 60 @ 87",4116,null,null,"Fog Nozzle 60 @ 87 4116",null,null,null,null,"Fog Nozzle 300 @ 100 4826",null,null,null,null,null,null,null,null,null,null,"Solid Bore 1.5 in","1-3/16\"","1.5 in","Solid Bore 1.5 in",null,"Stack Tips 2.5 in","1-3/8\"; 1-1/4\"; 1\"",null,"Solid Bore No 1.5 in 1-3/16\" Yes","Solid Bore No 1.5 in","Solid Bore","1-3/16\"","1499","1.5 in",1.1875,"No","Yes","Solid Bore Yes 2.5 in",null,0.9375,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 2.5 in 1\" Yes","1446",null,null,null,"1-3/16\"","1_3_16_",null,"Solid Bore","1-3/16\"","1499","1.5 in",1.1875,"No","Solid Bore 1.5 in No 1-3/16\" 1499",null,"Solid Bore 1.5 in No 1-3/16\" 1499",null,null,null,null,null,null,null,"Solid Bore","1-3/16\"","1499","Solid Bore1-3/16\"1499",null,"Solid Bore1-3/16\"1499"]
[null,null,"Shutoff Only2.5 in","2.5 in2.5 in","1-1/8\"2431","1.5 inNYCORP",null,null,"shutoff only2.5 in2.5 in2130",null,null,null,"2.5 IN","BIM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4866",161,null,null,null,null,null,null,null,4866,null,null,161,null,null,"Solid Bore","1-1/4\"","1499","1.5 in",1.25,null,null,null,null,null,265,50,"265 50",null,null,null,null,null,"Fog Nozzle",4826,200,75,"Fog Nozzle 200 @ 75",null,null,null,"Fog Nozzle 95 @ 100",4116,4863,null,"Fog Nozzle 95 @ 100 4116",{"$f":"CONCATENATE($BZ31,\" \",CB31)","v":"Fog Nozzle 95 @ 100 4863"},null,null,null,"Fog Nozzle 300 @ 75 4826",null,null,null,null,null,null,null,null,null,null,"Solid Bore 1.5 in","1-1/4\"","1.5 in","Solid Bore 1.5 in",null,null,null,null,"Solid Bore No 1.5 in 1-1/4\" Yes","Solid Bore No 1.5 in","Solid Bore","1-1/4\"","1499","1.5 in",1.25,"No","Yes","Solid Bore Yes 2.5 in",null,1,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 2.5 in 1-1/16\" Yes","1446",null,null,null,"1-1/4\"","1_1_4_",null,"Solid Bore","1-1/4\"","1499","1.5 in",1.25,"No","Solid Bore 1.5 in No 1-1/4\" 1499",null,"Solid Bore 1.5 in No 1-1/4\" 1499",null,null,null,null,null,null,null,"Solid Bore","1-1/4\"","1499","Solid Bore1-1/4\"1499",null,"Solid Bore1-1/4\"1499"]
[null,null,"Shutoff Only3 in","3 in2.5 in","1-1/4\"2431","1.5 inPCT",null,null,"shutoff only3 in2.5 in2130",null,null,null,"2.5 IN","STORZ",null,null,"BLACK (Std)","THREAD1 IN","NH","NPSH","Storz","Custom",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4866",175,null,null,null,null,null,null,null,4866,null,null,185,null,null,"Solid Bore","1-3/8\"","1499","1.5 in",1.375,null,null,null,null,null,300,"100 (Std)","300 100 (Std)",null,null,null,null,null,"Fog Nozzle",4826,265,50,"Fog Nozzle 265 @ 50",null,null,null,"Fog Nozzle 95 @ 75",4116,null,null,"Fog Nozzle 95 @ 75 4116",null,null,null,null,"Fog Nozzle 350 @ 100 4826",null,null,null,null,null,null,null,null,null,null,"Solid Bore 1.5 in","1-3/8\"","1.5 in","Solid Bore 1.5 in",null,null,null,null,"Solid Bore No 1.5 in 1-3/8\" Yes","Solid Bore No 1.5 in","Solid Bore","1-3/8\"","1499","1.5 in",1.375,"No","Yes","Solid Bore Yes 2.5 in",null,1.0625,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 2.5 in 1-1/4\" Yes","1446",null,null,null,"1-3/8\"","1_3_8_",null,"Solid Bore","1-3/8\"","1499","1.5 in",1.375,"No","Solid Bore 1.5 in No 1-3/8\" 1499",null,"Solid Bore 1.5 in No 1-3/8\" 1499",null,null,null,null,null,null,null,"Solid Bore","1-3/8\"","1499","Solid Bore1-3/8\"1499",null,"Solid Bore1-3/8\"1499"]
[null,null,"Shutoff with Integrated Tip1.5 in","2.5 in1.5 in","7/8\"2433","1.5 inStorz",null,null,"shutoff only3 in1.5 in2126",null,null,null,"3 IN","STORZ",null,null,"ORANGE","THREAD1.5 in","NH","NPSH","FDNY","NYCORP","PCT","Storz","Custom",null,null,null,null,null,null,null,null,null,null,null,"4866",185,null,null,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore","7/8\"","0489","2.5 in",0.875,null,null,null,null,null,300,75,"300 75",null,null,null,null,null,"Fog Nozzle",4826,250,75,"Fog Nozzle 250 @ 75",null,null,null,"Fog Nozzle 95 @ 87",4116,null,null,"Fog Nozzle 95 @ 87 4116",null,null,null,null,"Fog Nozzle 40 @ 100 4802",null,null,null,null,null,null,null,null,null,null,"Solid Bore 2.5 in","7/8\"","2.5 in","Solid Bore 2.5 in",null,null,null,null,"Solid Bore No 2.5 in 7/8\" Yes","Solid Bore No 2.5 in","Solid Bore","7/8\"","0489","2.5 in",0.875,"No","Yes","Solid Bore Yes 2.5 in",null,1.125,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 2.5 in 1-1/8\" Yes","1446",null,null,null,"7/8\"","7_8_",null,"Solid Bore","7/8\"","0489","2.5 in",0.875,"No","Solid Bore 2.5 in No 7/8\" 0489",null,"Solid Bore 2.5 in No 7/8\" 0489",null,null,null,null,null,null,null,"Solid Bore","7/8\"","0489","Solid Bore7/8\"0489",null,"Solid Bore7/8\"0489"]
[null,null,"Shutoff with Integrated Tip2 in","3 in1.5 in","15/16\"2433","1.5 inCustom",null,null,"shutoff with integrated tip1.5 in1.5 in2431",null,null,null,null,null,null,null,"YELLOW","THREAD2 IN","Storz",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4866",200,null,null,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore","15/16\"","0489","2.5 in",0.9375,null,null,null,null,null,350,"100 (Std)","350 100 (Std)",null,null,null,null,null,"Fog Nozzle",4826,300,75,"Fog Nozzle 300 @ 75",null,null,null,"Fog Tip 125 @ 100",4866,null,null,"Fog Tip 125 @ 100 4866",null,null,null,null,"Fog Nozzle 60 @ 100 4116",null,null,null,null,null,null,null,null,null,null,"Solid Bore 2.5 in","15/16\"","2.5 in","Solid Bore 2.5 in",null,null,null,null,"Solid Bore No 2.5 in 15/16\" Yes","Solid Bore No 2.5 in","Solid Bore","15/16\"","0489","2.5 in",0.9375,"No","Yes","Solid Bore Yes 2.5 in",null,1.1875,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 2.5 in 1-3/16\" Yes","1446",null,null,null,"15/16\"","15_16_",null,"Solid Bore","15/16\"","0489","2.5 in",0.9375,"No","Solid Bore 2.5 in No 15/16\" 0489",null,"Solid Bore 2.5 in No 15/16\" 0489",null,null,null,null,null,null,null,"Solid Bore","15/16\"","0489","Solid Bore15/16\"0489",null,"Solid Bore15/16\"0489"]
[null,null,"Shutoff with Integrated Tip2.5 in",null,"1\"2433","2.5 inNH",null,null,"shutoff with integrated tip2 in1.5 in2431",null,null,null,null,null,null,null,"RED","THREAD2.5 IN","NH","NPSH","FDNY","NYCORP","PITT6","BAT","CSA","QST","BIM","Storz","Custom",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore","1\"","0489","2.5 in",1,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4826,210,50,"Fog Nozzle 210 @ 50",null,null,null,"Fog Tip 125 @ 75",4866,null,null,"Fog Tip 125 @ 75 4866",null,null,null,null,"Fog Nozzle 60 @ 75 4116",null,null,null,null,null,null,null,null,null,null,"Solid Bore 2.5 in","1\"","2.5 in","Solid Bore 2.5 in",null,null,null,null,"Solid Bore No 2.5 in 1\" Yes","Solid Bore No 2.5 in","Solid Bore","1\"","0489","2.5 in",1,"No","Yes","Solid Bore Yes 2.5 in",null,1.25,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 2.5 in 1-3/8\" Yes","1446",null,null,null,"1\"","1_",null,"Solid Bore","1\"","0489","2.5 in",1,"No","Solid Bore 2.5 in No 1\" 0489",null,"Solid Bore 2.5 in No 1\" 0489",null,null,null,null,null,null,null,"Solid Bore","1\"","0489","Solid Bore1\"0489",null,"Solid Bore1\"0489"]
[null,null,"Shutoff with Integrated Tip3 in",null,"1-1/8\"2433","2.5 inNPSH",null,null,"shutoff with integrated tip2.5 in1.5 in2433",null,null,null,null,null,null,null,"BLUE","THREAD3 IN","Storz",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore","1.5 in",{"$f":"CONCATENATE(AU36,AV36)","v":"Solid Bore1.5 in"},null,null,"Solid Bore","1-1/8\"","0489","2.5 in",1.125,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4826,250,50,"Fog Nozzle 250 @ 50",null,null,null,"Fog Tip 150 @ 100",4866,null,null,"Fog Tip 150 @ 100 4866",null,null,null,null,"Fog Nozzle 60 @ 87 4116",null,null,null,null,null,null,null,null,null,null,"Solid Bore 2.5 in","1-1/8\"","2.5 in","Solid Bore 2.5 in",null,null,null,null,"Solid Bore No 2.5 in 1-1/8\" Yes","Solid Bore No 2.5 in","Solid Bore","1-1/8\"","0489","2.5 in",1.125,"No","Yes","Solid Bore Yes 2.5 in",null,1.375,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 2.5 in 15/16\" Yes","1446",null,null,null,"1-1/8\"","1_1_8_",null,"Solid Bore","1-1/8\"","0489","2.5 in",1.125,"No","Solid Bore 2.5 in No 1-1/8\" 0489",null,"Solid Bore 2.5 in No 1-1/8\" 0489",null,null,null,null,null,null,null,"Solid Bore","1-1/8\"","0489","Solid Bore1-1/8\"0489",null,"Solid Bore1-1/8\"0489"]
[null,null,null,null,"1-1/4\"2433","2.5 INFDNY",null,null,"shutoff with integrated tip3 in1.5 in2433",null,null,null,null,null,null,null,"GREEN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore","2.5 in",{"$f":"CONCATENATE(AU37,AV37)","v":"Solid Bore2.5 in"},null,null,"Solid Bore","1-1/4\"","0489","2.5 in",1.25,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4863,95,"100 (Std)","Fog Nozzle 95 @ 100 (Std)",null,null,null,"Fog Tip 150 @ 50",4866,null,null,"Fog Tip 150 @ 50 4866",null,null,null,null,"Fog Nozzle 95 @ 100 4116",null,null,null,null,null,null,null,null,null,null,"Solid Bore 2.5 in","1-1/4\"","2.5 in","Solid Bore 2.5 in",null,null,null,null,"Solid Bore No 2.5 in 1-1/4\" Yes","Solid Bore No 2.5 in","Solid Bore","1-1/4\"","0489","2.5 in",1.25,"No","Yes","Stack Tips No 1.5 in",null,0.5,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 2.5 in 7/8\" Yes","1446",null,null,null,"1-1/4\"","1_1_4_",null,"Solid Bore","1-1/4\"","0489","2.5 in",1.25,"No","Solid Bore 2.5 in No 1-1/4\" 0489",null,"Solid Bore 2.5 in No 1-1/4\" 0489",null,null,null,null,null,null,null,"Solid Bore","1-1/4\"","0489","Solid Bore1-1/4\"0489",null,"Solid Bore1-1/4\"0489"]
[null,null,null,null,"1-1/16\"2431","2.5 INNYCORP",null,null,"shutoff only2.5 in1.5 in2390",null,null,null,"1440","No",{"$f":"TRIM(M38)","v":"1440"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Style","List Price",null,null,null,null,"Stack Tips","1.5 in",{"$f":"CONCATENATE(AU38,AV38)","v":"Stack Tips1.5 in"},null,null,"Solid Bore","1-3/8\"","0489","2.5 in",1.375,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4863,125,"100 (Std)","Fog Nozzle 125 @ 100 (Std)",null,null,null,"Fog Tip 150 @ 75",4866,null,null,"Fog Tip 150 @ 75 4866",null,null,null,null,"Fog Nozzle 95 @ 100 4863",null,null,null,null,null,null,null,null,null,null,"Solid Bore 2.5 in","1-3/8\"","2.5 in","Solid Bore 2.5 in",null,null,null,null,"Solid Bore No 2.5 in 1-3/8\" Yes","Solid Bore No 2.5 in","Solid Bore","1-3/8\"","0489","2.5 in",1.375,"No","Yes","Stack Tips No 1.5 in",null,0.5,null,null,null,null,null,null,null,null,null,null,null,"Stack Tips Yes 1.5 in 15/16\"; 1/2\" Yes","1441",null,null,null,"1-3/8\"","1_3_8_",null,"Solid Bore","1-3/8\"","0489","2.5 in",1.375,"No","Solid Bore 2.5 in No 1-3/8\" 0489",null,"Solid Bore 2.5 in No 1-3/8\" 0489",null,null,null,null,null,null,null,"Solid Bore","1-3/8\"","0489","Solid Bore1-3/8\"0489",null,"Solid Bore1-3/8\"0489"]
[null,null,null,null,"1-3/16\"2431","2.5 INPITT6",null,null,"shutoff only3 in1.5 in2390",null,null,null,"1441","Yes",{"$f":"TRIM(M39)","v":"1441"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"0416",378,null,null,null,null,"Stack Tips","2.5 in",{"$f":"CONCATENATE(AU39,AV39)","v":"Stack Tips2.5 in"},null,null,"Solid Bore","7/8\"","1446","2.5 in",0.875,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4863,150,"100 (Std)","Fog Nozzle 150 @ 100 (Std)",null,null,null,"Fog Tip 161 @ 50",4866,null,null,"Fog Tip 161 @ 50 4866",null,null,null,null,"Fog Nozzle 95 @ 75 4116",null,null,null,null,null,null,null,null,null,null,"Solid Bore 2.5 in","7/8\"","2.5 in","Solid Bore 2.5 in",null,null,null,null,"Solid Bore Yes 2.5 in 7/8\" No (Std)","Solid Bore Yes 2.5 in","Solid Bore","7/8\"","1446","2.5 in",0.875,"Yes","No (Std)","Stack Tips No 1.5 in",null,0.9375,null,null,null,null,null,null,null,null,null,null,null,"Stack Tips Yes 2.5 in 1-1/8\"; 1/2\" Yes","1443",null,null,null,"7/8\"","7_8_",null,"Solid Bore","7/8\"","1446","2.5 in",0.875,"Yes","Solid Bore 2.5 in Yes 7/8\" 1446",null,"Solid Bore 2.5 in Yes 7/8\" 1446",null,null,null,null,null,null,null,"Solid Bore","7/8\"","1446","Solid Bore7/8\"1446",null,"Solid Bore7/8\"1446"]
[null,null,null,null,"1-1/16\"2433","2.5 INBAT",null,null,null,null,null,null,"1442","No","1442",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"yes1.5 in","NH",{"$f":"CONCATENATE(AI40,AJ40)","v":"yes1.5 inNH"},null,null,null,"0439",284,null,null,null,null,null,null,null,null,null,"Solid Bore","15/16\"","1446","2.5 in",0.9375,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4863,175,"100 (Std)","Fog Nozzle 175 @ 100 (Std)",null,null,null,"Fog Tip 175 @ 100",4866,null,null,"Fog Tip 175 @ 100 4866",null,null,null,null,"Fog Nozzle 95 @ 87 4116",null,null,null,null,null,null,null,null,null,null,"Solid Bore 2.5 in","15/16\"","2.5 in","Solid Bore 2.5 in",null,null,null,null,"Solid Bore Yes 2.5 in 15/16\" No (Std)","Solid Bore Yes 2.5 in","Solid Bore","15/16\"","1446","2.5 in",0.9375,"Yes","No (Std)","Stack Tips No 1.5 in",null,1,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 1.5 in 1-1/16\" No (Std)","1445",null,null,null,"15/16\"","15_16_",null,"Solid Bore","15/16\"","1446","2.5 in",0.9375,"Yes","Solid Bore 2.5 in Yes 15/16\" 1446",null,"Solid Bore 2.5 in Yes 15/16\" 1446",null,null,null,null,null,null,null,"Solid Bore","15/16\"","1446","Solid Bore15/16\"1446",null,"Solid Bore15/16\"1446"]
[null,null,null,null,"1-3/16\"2433","2.5 INCSA",null,null,null,null,null,null,"1443","Yes","1443",null,null,"Style",null,null,{"$f":"IF(B10=\"fog tip\",\"N/A\",\"No (Std)\")","v":"No (Std)"},null,"yes1 IN","NH","NPSH","Storz","Custom",null,null,null,null,null,null,null,"yes1.5 in","NPSH",{"$f":"CONCATENATE(AI41,AJ41)","v":"yes1.5 inNPSH"},null,null,null,"0489",498,null,null,null,null,null,null,null,null,null,"Solid Bore","1\"","1446","2.5 in",1,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4863,200,"100 (Std)","Fog Nozzle 200 @ 100 (Std)",null,null,null,"Fog Tip 175 @ 50",4866,null,null,"Fog Tip 175 @ 50 4866",null,null,null,null,"Fog Tip 125 @ 100 4866",null,null,null,null,null,null,null,null,null,null,"Solid Bore 2.5 in","1\"","2.5 in","Solid Bore 2.5 in",null,null,null,null,"Solid Bore Yes 2.5 in 1\" No (Std)","Solid Bore Yes 2.5 in","Solid Bore","1\"","1446","2.5 in",1,"Yes","No (Std)","Stack Tips No 2.5 in",null,1,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 1.5 in 1-1/4\" No (Std)","1445",null,null,null,"1\"","1_",null,"Solid Bore","1\"","1446","2.5 in",1,"Yes","Solid Bore 2.5 in Yes 1\" 1446",null,"Solid Bore 2.5 in Yes 1\" 1446",null,null,null,null,null,null,null,"Solid Bore","1\"","1446","Solid Bore1\"1446",null,"Solid Bore1\"1446"]
[null,null,null,null,null,"2.5 INQST",null,null,null,null,null,null,"1445","Yes","1445",null,"Fog Nozzle 5-40","1602",null,null,{"$f":"IF(B10=\"fog tip\",\"\",\"Yes\")","v":"Yes"},null,"yes1.5 in","NH","NPSH","FDNY","NYCORP","PCT","Storz","Custom",null,null,null,null,"yes1.5 in","FDNY","yes1.5 inFDNY",null,null,null,"1417",156,null,null,null,null,null,null,null,null,null,"Solid Bore","1-1/16\"","1446","2.5 in",1.0625,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4863,125,75,"Fog Nozzle 125 @ 75",null,null,null,"Fog Tip 175 @ 75",4866,null,null,"Fog Tip 175 @ 75 4866",null,null,null,null,"Fog Tip 125 @ 75 4866",null,null,null,null,null,null,null,null,null,null,"Solid Bore 2.5 in","1-1/16\"","2.5 in","Solid Bore 2.5 in",null,null,null,null,"Solid Bore Yes 2.5 in 1-1/16\" No (Std)","Solid Bore Yes 2.5 in","Solid Bore","1-1/16\"","1446","2.5 in",1.0625,"Yes","No (Std)","Stack Tips No 2.5 in",null,1,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 1.5 in 1-1/8\" No (Std)","1445",null,null,null,"1-1/16\"","1_1_16_",null,"Solid Bore","1-1/16\"","1446","2.5 in",1.0625,"Yes","Solid Bore 2.5 in Yes 1-1/16\" 1446",null,"Solid Bore 2.5 in Yes 1-1/16\" 1446",null,null,null,null,null,null,null,"Solid Bore","1-1/16\"","1446","Solid Bore1-1/16\"1446",null,"Solid Bore1-1/16\"1446"]
[null,null,null,null,null,"2.5 INBIM",null,null,null,null,null,null,"1446","Yes","1446",null,"Fog Nozzle 12-53","1602",null,null,null,null,"yes2.5 IN","NH","NPSH","FDNY","NYCORP","PITT6","BAT","CSA","QST","BIM","Storz","Custom","yes1.5 in","NYCORP","yes1.5 inNYCORP",null,null,null,"1420",500,null,null,null,null,null,null,null,null,null,"Solid Bore","1-1/8\"","1446","2.5 in",1.125,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4863,150,75,"Fog Nozzle 150 @ 75",null,null,null,"Fog Tip 185 @ 50",4866,null,null,"Fog Tip 185 @ 50 4866",null,null,null,null,"Fog Tip 150 @ 100 4866",null,null,null,null,null,null,null,null,null,null,"Solid Bore 2.5 in","1-1/8\"","2.5 in","Solid Bore 2.5 in",null,null,null,null,"Solid Bore Yes 2.5 in 1-1/8\" No (Std)","Solid Bore Yes 2.5 in","Solid Bore","1-1/8\"","1446","2.5 in",1.125,"Yes","No (Std)","Stack Tips No 2.5 in",null,1,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 1.5 in 1-3/16\" No (Std)","1445",null,null,null,"1-1/8\"","1_1_8_",null,"Solid Bore","1-1/8\"","1446","2.5 in",1.125,"Yes","Solid Bore 2.5 in Yes 1-1/8\" 1446",null,"Solid Bore 2.5 in Yes 1-1/8\" 1446",null,null,null,null,null,null,null,"Solid Bore","1-1/8\"","1446","Solid Bore1-1/8\"1446",null,"Solid Bore1-1/8\"1446"]
[null,null,null,null,null,"2.5 INStorz",null,null,null,null,null,null,"1447","Yes","1447",null,"Fog Nozzle 30-150","1616",null,null,null,null,"no1 IN","NH","NPSH","Custom",null,null,null,null,null,null,null,null,"yes1.5 in","PCT","yes1.5 inPCT",null,null,null,"1440",828,null,null,null,null,null,null,null,null,null,"Solid Bore","1-3/16\"","1446","2.5 in",1.1875,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4863,175,75,"Fog Nozzle 175 @ 75",null,null,null,"Fog Tip 200 @ 100",4824,4866,null,"Fog Tip 200 @ 100 4824","Fog Tip 200 @ 100 4866",null,null,null,"Fog Tip 150 @ 50 4866",null,null,null,null,null,null,null,null,null,null,"Solid Bore 2.5 in","1-3/16\"","2.5 in","Solid Bore 2.5 in",null,null,null,null,"Solid Bore Yes 2.5 in 1-3/16\" No (Std)","Solid Bore Yes 2.5 in","Solid Bore","1-3/16\"","1446","2.5 in",1.1875,"Yes","No (Std)","Stack Tips Yes 1.5 in",null,0.5,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 1.5 in 1-3/8\" No (Std)","1445",null,null,null,"1-3/16\"","1_3_16_",null,"Solid Bore","1-3/16\"","1446","2.5 in",1.1875,"Yes","Solid Bore 2.5 in Yes 1-3/16\" 1446",null,"Solid Bore 2.5 in Yes 1-3/16\" 1446",null,null,null,null,null,null,null,"Solid Bore","1-3/16\"","1446","Solid Bore1-3/16\"1446",null,"Solid Bore1-3/16\"1446"]
[null,null,null,null,null,"2.5 INCustom",null,null,null,null,null,null,"2393","No","2393",null,"Fog Nozzle 13-60","1702",null,null,null,null,"no1.5 in","NH","NPSH","FDNY","NYCORP","PCT","Custom",null,null,null,null,null,"yes1.5 in","Storz","yes1.5 inStorz",null,null,null,"1441",828,null,null,null,null,null,null,null,null,null,"Solid Bore","1-1/4\"","1446","2.5 in",1.25,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4863,200,75,"Fog Nozzle 200 @ 75",null,null,null,"Fog Tip 200 @ 75",4824,4866,null,"Fog Tip 200 @ 75 4824","Fog Tip 200 @ 75 4866",null,null,null,"Fog Tip 150 @ 75 4866",null,null,null,null,null,null,null,null,null,null,"Solid Bore 2.5 in","1-1/4\"","2.5 in","Solid Bore 2.5 in",null,null,null,null,"Solid Bore Yes 2.5 in 1-1/4\" No (Std)","Solid Bore Yes 2.5 in","Solid Bore","1-1/4\"","1446","2.5 in",1.25,"Yes","No (Std)","Stack Tips Yes 2.5 in",null,0.5,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 1.5 in 15/16\" No (Std)","1445",null,null,null,"1-1/4\"","1_1_4_",null,"Solid Bore","1-1/4\"","1446","2.5 in",1.25,"Yes","Solid Bore 2.5 in Yes 1-1/4\" 1446",null,"Solid Bore 2.5 in Yes 1-1/4\" 1446",null,null,null,null,null,null,null,"Solid Bore","1-1/4\"","1446","Solid Bore1-1/4\"1446",null,"Solid Bore1-1/4\"1446"]
[null,null,null,null,null,"1.5 inNH",null,null,null,null,null,null,null,null,null,null,"Fog Tip 13-60","1703",null,null,null,null,"no2.5 IN","NH","NPSH","FDNY","NYCORP","PITT6","BAT","CSA","QST","Custom",null,null,"yes1.5 in","Custom","yes1.5 inCustom",null,null,null,"1442",960,null,null,null,null,null,null,null,null,null,"Solid Bore","1-3/8\"","1446","2.5 in",1.375,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4863,150,50,"Fog Nozzle 150 @ 50",null,null,null,"Fog Tip 210 @ 50",4824,null,null,"Fog Tip 210 @ 50 4824",null,null,null,null,"Fog Tip 161 @ 50 4866",null,null,null,null,null,null,null,null,null,null,"Solid Bore 2.5 in","1-3/8\"","2.5 in","Solid Bore 2.5 in",null,null,null,null,"Solid Bore Yes 2.5 in 1-3/8\" No (Std)","Solid Bore Yes 2.5 in","Solid Bore","1-3/8\"","1446","2.5 in",1.375,"Yes","No (Std)","Stack Tips Yes 2.5 in",null,1,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 1.5 in 7/8\" No (Std)","1445",null,null,null,"1-3/8\"","1_3_8_",null,"Solid Bore","1-3/8\"","1446","2.5 in",1.375,"Yes","Solid Bore 2.5 in Yes 1-3/8\" 1446",null,"Solid Bore 2.5 in Yes 1-3/8\" 1446",null,null,null,null,null,null,null,"Solid Bore","1-3/8\"","1446","Solid Bore1-3/8\"1446",null,"Solid Bore1-3/8\"1446"]
[null,null,null,null,null,"2.5 INNPSH",null,null,null,null,null,null,null,null,null,null,"Fog Nozzle 18-30","1704",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"yes2.5 IN","NH","yes2.5 INNH",null,null,null,"1443",960,null,null,null,null,null,null,null,null,null,"Stack Tips","1-1/8\"; 1/2\"","0439","1.5 in",0.5,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4863,161,50,"Fog Nozzle 161 @ 50",null,null,null,"Fog Tip 225 @ 100",4866,null,null,"Fog Tip 225 @ 100 4866",null,null,null,null,"Fog Tip 175 @ 100 4866",null,null,null,null,null,null,null,null,null,null,"Stack Tips 1.5 in","1-1/8\"; 1/2\"","1.5 in","Stack Tips 1.5 in",null,null,null,null,"Stack Tips No 1.5 in 1-1/8\"; 1/2\" Yes","Stack Tips No 1.5 in","Stack Tips","1-1/8\"; 1/2\"","0439","1.5 in",0.5,"No","Yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 2.5 in 1\" No (Std)","1446",null,null,null,"1-1/8\"; 1/2\"","1_1_8___1_2_",null,"Stack Tips","1-1/8\"; 1/2\"","0439","1.5 in",0.5,"No","Stack Tips 1.5 in No 1-1/8\"; 1/2\" 0439",null,"Stack Tips 1.5 in No 1-1/8\"; 1/2\" 0439",null,null,null,null,null,null,null,"Stack Tips","1-1/8\"; 1/2\"","0439","Stack Tips1-1/8\"; 1/2\"0439",null,"Stack Tips1-1/8\"; 1/2\"0439"]
[null,null,null,null,null,"2.5 INFDNY",null,null,null,null,null,null,null,null,null,null,"Fog Nozzle 13-30","1704",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"yes2.5 IN","NPSH","yes2.5 INNPSH",null,null,null,"1445",714,null,null,null,null,null,null,null,null,null,"Stack Tips","15-16\"; 1/2\"","0439","1.5 in",0.5,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4863,175,50,"Fog Nozzle 175 @ 50",null,null,null,"Fog Tip 250 @ 100",4824,null,null,"Fog Tip 250 @ 100 4824",null,null,null,null,"Fog Tip 175 @ 50 4866",null,null,null,null,null,null,null,null,null,null,"Stack Tips 1.5 in","15-16\"; 1/2\"","1.5 in","Stack Tips 1.5 in",null,null,null,null,"Stack Tips No 1.5 in 15-16\"; 1/2\" Yes","Stack Tips No 1.5 in","Stack Tips","15-16\"; 1/2\"","0439","1.5 in",0.5,"No","Yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 2.5 in 1-1/16\" No (Std)","1446",null,null,null,"15-16\"; 1/2\"","15_16___1_2_",null,"Stack Tips","15-16\"; 1/2\"","0439","1.5 in",0.5,"No","Stack Tips 1.5 in No 15-16\"; 1/2\" 0439",null,"Stack Tips 1.5 in No 15-16\"; 1/2\" 0439",null,null,null,null,null,null,null,"Stack Tips","15-16\"; 1/2\"","0439","Stack Tips15-16\"; 1/2\"0439",null,"Stack Tips15-16\"; 1/2\"0439"]
[null,null,null,null,null,"2.5 INNYCORP",null,null,null,null,null,null,null,null,null,null,"Fog Tip 18-30","1711",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"yes2.5 IN","FDNY","yes2.5 INFDNY",null,null,null,"1446",846,null,null,null,null,null,null,null,null,null,"Stack Tips","1-1/16\"; 15/16\"","0439","1.5 in",0.9375,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4863,185,50,"Fog Nozzle 185 @ 50",null,null,null,"Fog Tip 250 @ 50",4824,null,null,"Fog Tip 250 @ 50 4824",null,null,null,null,"Fog Tip 175 @ 75 4866",null,null,null,null,null,null,null,null,null,null,"Stack Tips 1.5 in","1-1/16\"; 15/16\"","1.5 in","Stack Tips 1.5 in",null,null,null,null,"Stack Tips No 1.5 in 1-1/16\"; 15/16\" Yes","Stack Tips No 1.5 in","Stack Tips","1-1/16\"; 15/16\"","0439","1.5 in",0.9375,"No","Yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 2.5 in 1-1/4\" No (Std)","1446",null,null,null,"1-1/16\"; 15/16\"","1_1_16___15_16_",null,"Stack Tips","1-1/16\"; 15/16\"","0439","1.5 in",0.9375,"No","Stack Tips 1.5 in No 1-1/16\"; 15/16\" 0439",null,"Stack Tips 1.5 in No 1-1/16\"; 15/16\" 0439",null,null,null,null,null,null,null,"Stack Tips","1-1/16\"; 15/16\"","0439","Stack Tips1-1/16\"; 15/16\"0439",null,"Stack Tips1-1/16\"; 15/16\"0439"]
[null,null,null,null,null,"2.5 INPCT",null,null,null,null,null,null,null,null,null,null,"Fog Tip 13-30","1711",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"yes2.5 IN","NYCORP","yes2.5 INNYCORP",null,null,null,"1447",{"$f":"156+544","v":700},null,null,null,null,null,null,null,null,null,"Stack Tips","1-1/4\"; 1-1/8\"; 1\"","1420","1.5 in",1,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4863,225,"100 (Std)","Fog Nozzle 225 @ 100 (Std)",null,null,null,"Fog Tip 250 @ 75",4824,null,null,"Fog Tip 250 @ 75 4824",null,null,null,null,"Fog Tip 185 @ 50 4866",null,null,null,null,null,null,null,null,null,null,"Stack Tips 1.5 in","1-1/4\"; 1-1/8\"; 1\"","1.5 in","Stack Tips 1.5 in",null,null,null,null,"Stack Tips No 1.5 in 1-1/4\"; 1-1/8\"; 1\" Yes","Stack Tips No 1.5 in","Stack Tips","1-1/4\"; 1-1/8\"; 1\"","1420","1.5 in",1,"No","Yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 2.5 in 1-1/8\" No (Std)","1446",null,null,null,"1-1/4\"; 1-1/8\"; 1\"","1_1_4___1_1_8___1_",null,"Stack Tips","1-1/4\"; 1-1/8\"; 1\"","1420","1.5 in",1,"No","Stack Tips 1.5 in No 1-1/4\"; 1-1/8\"; 1\" 1420",null,"Stack Tips 1.5 in No 1-1/4\"; 1-1/8\"; 1\" 1420",null,null,null,null,null,null,null,"Stack Tips","1-1/4\"; 1-1/8\"; 1\"","1420","Stack Tips1-1/4\"; 1-1/8\"; 1\"1420",null,"Stack Tips1-1/4\"; 1-1/8\"; 1\"1420"]
[null,null,null,null,null,"2.5 INCustom",null,null,null,null,null,null,null,null,null,null,"Fog Tip 30-125","1714",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"yes2.5 IN","PITT6","yes2.5 INPITT6",null,null,null,"1499",170,null,null,null,null,null,null,null,null,null,"Stack Tips","15/16\"; 1/2\"","1440","1.5 in",0.5,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip",4866,95,"100 (Std)","Fog Tip 95 @ 100 (Std)",null,null,null,"Fog Tip 265 @ 50",4824,null,null,"Fog Tip 265 @ 50 4824",null,null,null,null,"Fog Tip 200 @ 100 4824",null,null,null,null,null,null,null,null,null,null,"Stack Tips 1.5 in","15/16\"; 1/2\"","1.5 in","Stack Tips 1.5 in",null,null,null,null,"Stack Tips Yes 1.5 in 15/16\"; 1/2\" Yes","Stack Tips Yes 1.5 in","Stack Tips","15/16\"; 1/2\"","1440","1.5 in",0.5,"Yes","Yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 2.5 in 1-3/16\" No (Std)","1446",null,null,null,"15/16\"; 1/2\"","15_16___1_2_",null,"Stack Tips","15/16\"; 1/2\"","1440","1.5 in",0.5,"Yes","Stack Tips 1.5 in Yes 15/16\"; 1/2\" 1440",null,"Stack Tips 1.5 in Yes 15/16\"; 1/2\" 1440",null,null,null,null,null,null,null,"Stack Tips","15/16\"; 1/2\"","1440","Stack Tips15/16\"; 1/2\"1440",null,"Stack Tips15/16\"; 1/2\"1440"]
[null,null,null,null,null,"2.5 INNH",null,null,null,null,null,null,null,null,null,null,"Fog Nozzle 30-125","1720",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"yes2.5 IN","BAT","yes2.5 INBAT",null,null,null,"2393",1602,null,null,null,null,null,null,null,null,null,"Stack Tips","15/16\"; 1/2\"","1441","1.5 in",0.5,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip",4866,125,"100 (Std)","Fog Tip 125 @ 100 (Std)",null,null,null,"Fog Tip 300 @ 100",4824,null,null,"Fog Tip 300 @ 100 4824",null,null,null,null,"Fog Tip 200 @ 100 4866",null,null,null,null,null,null,null,null,null,null,"Stack Tips 1.5 in","15/16\"; 1/2\"","1.5 in","Stack Tips 1.5 in",null,null,null,null,"Stack Tips Yes 1.5 in 15/16\"; 1/2\" No (Std)","Stack Tips Yes 1.5 in","Stack Tips","15/16\"; 1/2\"","1441","1.5 in",0.5,"Yes","No (Std)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 2.5 in 1-3/8\" No (Std)","1446",null,null,null,"15/16\"; 1/2\"","15_16___1_2_",null,"Stack Tips","15/16\"; 1/2\"","1441","1.5 in",0.5,"Yes","Stack Tips 1.5 in Yes 15/16\"; 1/2\" 1441",null,"Stack Tips 1.5 in Yes 15/16\"; 1/2\" 1441",null,null,null,null,null,null,null,"Stack Tips","15/16\"; 1/2\"","1441","Stack Tips15/16\"; 1/2\"1441",null,"Stack Tips15/16\"; 1/2\"1441"]
[null,null,null,null,null,"2.5 INPITT6",null,null,null,null,null,null,null,null,null,null,"Fog Nozzle 95-200","1723",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"yes2.5 IN","CSA","yes2.5 INCSA",null,null,null,"2420",590,null,null,null,null,null,null,null,null,null,"Stack Tips","1-1/8\"; 1/2\"","1442","2.5 in",0.5,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip",4866,150,"100 (Std)","Fog Tip 150 @ 100 (Std)",null,null,null,"Fog Tip 300 @ 75",4824,null,null,"Fog Tip 300 @ 75 4824",null,null,null,null,"Fog Tip 200 @ 75 4824",null,null,null,null,null,null,null,null,null,null,"Stack Tips 2.5 in","1-1/8\"; 1/2\"","2.5 in","Stack Tips 2.5 in",null,null,null,null,"Stack Tips Yes 2.5 in 1-1/8\"; 1/2\" Yes","Stack Tips Yes 2.5 in","Stack Tips","1-1/8\"; 1/2\"","1442","2.5 in",0.5,"Yes","Yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 2.5 in 15/16\" No (Std)","1446",null,null,null,"1-1/8\"; 1/2\"","1_1_8___1_2_",null,"Stack Tips","1-1/8\"; 1/2\"","1442","2.5 in",0.5,"Yes","Stack Tips 2.5 in Yes 1-1/8\"; 1/2\" 1442",null,"Stack Tips 2.5 in Yes 1-1/8\"; 1/2\" 1442",null,null,null,null,null,null,null,"Stack Tips","1-1/8\"; 1/2\"","1442","Stack Tips1-1/8\"; 1/2\"1442",null,"Stack Tips1-1/8\"; 1/2\"1442"]
[null,null,null,null,null,"2.5 INBAT",null,null,null,null,null,null,null,null,null,null,"Fog Nozzle 125-250","1733",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"yes2.5 IN","QST","yes2.5 INQST",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stack Tips","1-1/8\"; 1/2\"","1443","2.5 in",0.5,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip",4866,175,"100 (Std)","Fog Tip 175 @ 100 (Std)",null,null,null,"Fog Tip 350 @ 100",4824,null,null,"Fog Tip 350 @ 100 4824",null,null,null,null,"Fog Tip 200 @ 75 4866",null,null,null,null,null,null,null,null,null,null,"Stack Tips 2.5 in","1-1/8\"; 1/2\"","2.5 in","Stack Tips 2.5 in",null,null,null,null,"Stack Tips Yes 2.5 in 1-1/8\"; 1/2\" No (Std)","Stack Tips Yes 2.5 in","Stack Tips","1-1/8\"; 1/2\"","1443","2.5 in",0.5,"Yes","No (Std)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 2.5 in 7/8\" No (Std)","1446",null,null,null,"1-1/8\"; 1/2\"","1_1_8___1_2_",null,"Stack Tips","1-1/8\"; 1/2\"","1443","2.5 in",0.5,"Yes","Stack Tips 2.5 in Yes 1-1/8\"; 1/2\" 1443",null,"Stack Tips 2.5 in Yes 1-1/8\"; 1/2\" 1443",null,null,null,null,null,null,null,"Stack Tips","1-1/8\"; 1/2\"","1443","Stack Tips1-1/8\"; 1/2\"1443",null,"Stack Tips1-1/8\"; 1/2\"1443"]
[null,null,null,null,null,"2.5 INCSA",null,null,null,null,null,null,null,null,null,null,"Fog Tip 95-200","1737",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"yes2.5 IN","BIM","yes2.5 INBIM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stack Tips","1-1/4\"; 1-1/8\"; 1\"","2393","2.5 in",1,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip",4866,200,"100 (Std)","Fog Tip 200 @ 100 (Std)",null,null,null,"Fog Tip 95 @ 100",4866,null,null,"Fog Tip 95 @ 100 4866",null,null,null,null,"Fog Tip 210 @ 50 4824",null,null,null,null,null,null,null,null,null,null,"Stack Tips 2.5 in","1-1/4\"; 1-1/8\"; 1\"","2.5 in","Stack Tips 2.5 in",null,null,null,null,"Stack Tips Yes 2.5 in 1-1/4\"; 1-1/8\"; 1\" No (Std)","Stack Tips Yes 2.5 in","Stack Tips","1-1/4\"; 1-1/8\"; 1\"","2393","2.5 in",1,"Yes","No (Std)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stack Tips No 1.5 in 1-1/16\"; 15/16\" Yes","0439",null,null,null,"1-1/4\"; 1-1/8\"; 1\"","1_1_4___1_1_8___1_",null,"Stack Tips","1-1/4\"; 1-1/8\"; 1\"","2393","2.5 in",1,"Yes","Stack Tips 2.5 in Yes 1-1/4\"; 1-1/8\"; 1\" 2393",null,"Stack Tips 2.5 in Yes 1-1/4\"; 1-1/8\"; 1\" 2393",null,null,null,null,null,null,null,"Stack Tips","1-1/4\"; 1-1/8\"; 1\"","2393","Stack Tips1-1/4\"; 1-1/8\"; 1\"2393",null,"Stack Tips1-1/4\"; 1-1/8\"; 1\"2393"]
[null,null,null,null,null,"2.5 INQST",null,null,null,null,null,null,null,null,null,null,"Fog Tip 125-250","1744",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"yes2.5 IN","Storz","yes2.5 INStorz",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stack Tips","1-1/2\"; 1-1/4\"; 1\"","2420","2.5 in",1,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip",4866,125,75,"Fog Tip 125 @ 75",null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip 225 @ 100 4866",null,null,null,null,null,null,null,null,null,null,"Stack Tips 2.5 in","1-1/2\"; 1-1/4\"; 1\"","2.5 in","Stack Tips 2.5 in",null,null,null,null,"Stack Tips No 2.5 in 1-1/2\"; 1-1/4\"; 1\" Yes","Stack Tips No 2.5 in","Stack Tips","1-1/2\"; 1-1/4\"; 1\"","2420","2.5 in",1,"No","Yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stack Tips No 1.5 in 1-1/4\"; 1-1/8\"; 1\" Yes","1420",null,null,null,"1-1/2\"; 1-1/4\"; 1\"","1_1_2___1_1_4___1_",null,"Stack Tips","1-1/2\"; 1-1/4\"; 1\"","2420","2.5 in",1,"No","Stack Tips 2.5 in No 1-1/2\"; 1-1/4\"; 1\" 2420",null,"Stack Tips 2.5 in No 1-1/2\"; 1-1/4\"; 1\" 2420",null,null,null,null,null,null,null,"Stack Tips","1-1/2\"; 1-1/4\"; 1\"","2420","Stack Tips1-1/2\"; 1-1/4\"; 1\"2420",null,"Stack Tips1-1/2\"; 1-1/4\"; 1\"2420"]
[null,null,null,null,null,"1.5 inNPSH",null,null,null,null,null,null,null,null,null,null,"Fog Nozzle 30-200","1763",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"yes2.5 IN","Custom","yes2.5 INCustom",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stack Tips","1-1/4\"; 1-1/8\"; 1\"","2420","2.5 in",1,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip",4866,150,75,"Fog Tip 150 @ 75",null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip 250 @ 100 4824",null,null,null,null,null,null,null,null,null,null,"Stack Tips 2.5 in","1-1/4\"; 1-1/8\"; 1\"","2.5 in","Stack Tips 2.5 in",null,null,null,null,"Stack Tips No 2.5 in 1-1/4\"; 1-1/8\"; 1\" Yes","Stack Tips No 2.5 in","Stack Tips","1-1/4\"; 1-1/8\"; 1\"","2420","2.5 in",1,"No","Yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stack Tips No 1.5 in 1-1/8\"; 1/2\" Yes","0439",null,null,null,"1-1/4\"; 1-1/8\"; 1\"","1_1_4___1_1_8___1_",null,"Stack Tips","1-1/4\"; 1-1/8\"; 1\"","2420","2.5 in",1,"No","Stack Tips 2.5 in No 1-1/4\"; 1-1/8\"; 1\" 2420",null,"Stack Tips 2.5 in No 1-1/4\"; 1-1/8\"; 1\" 2420",null,null,null,null,null,null,null,"Stack Tips","1-1/4\"; 1-1/8\"; 1\"","2420","Stack Tips1-1/4\"; 1-1/8\"; 1\"2420",null,"Stack Tips1-1/4\"; 1-1/8\"; 1\"2420"]
[null,null,null,null,null,"1.5 inFDNY",null,null,null,null,null,null,null,null,null,null,"Fog Tip 30-200","1766",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"no1.5 in","NH","no1.5 inNH",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stack Tips","1-3/8\"; 1-1/4\"; 1\"","2420","2.5 in",1,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip",4866,175,75,"Fog Tip 175 @ 75",null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip 250 @ 50 4824",null,null,null,null,null,null,null,null,null,null,"Stack Tips 2.5 in","1-3/8\"; 1-1/4\"; 1\"","2.5 in","Stack Tips 2.5 in",null,null,null,null,"Stack Tips No 2.5 in 1-3/8\"; 1-1/4\"; 1\" Yes","Stack Tips No 2.5 in","Stack Tips","1-3/8\"; 1-1/4\"; 1\"","2420","2.5 in",1,"No","Yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stack Tips No 1.5 in 15-16\"; 1/2\" Yes","0439",null,null,null,"1-3/8\"; 1-1/4\"; 1\"","1_3_8___1_1_4___1_",null,"Stack Tips","1-3/8\"; 1-1/4\"; 1\"","2420","2.5 in",1,"No","Stack Tips 2.5 in No 1-3/8\"; 1-1/4\"; 1\" 2420",null,"Stack Tips 2.5 in No 1-3/8\"; 1-1/4\"; 1\" 2420",null,null,null,null,null,null,null,"Stack Tips","1-3/8\"; 1-1/4\"; 1\"","2420","Stack Tips1-3/8\"; 1-1/4\"; 1\"2420",null,"Stack Tips1-3/8\"; 1-1/4\"; 1\"2420"]
[null,null,null,null,null,"1.5 inNYCORP",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"no2.5 IN","NPSH","no2.5 INNPSH",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip",4866,200,75,"Fog Tip 200 @ 75",null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip 250 @ 75 4824",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stack Tips No 2.5 in 1-1/2\"; 1-1/4\"; 1\" Yes","2420"]
[null,null,null,null,null,"1.5 inPCT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"no2.5 IN","FDNY","no2.5 INFDNY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip",4866,150,50,"Fog Tip 150 @ 50",null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip 265 @ 50 4824",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stack Tips No 2.5 in 1-1/4\"; 1-1/8\"; 1\" Yes","2420"]
[null,null,null,null,null,"1.5 inStorz",null,null,null,null,null,null,"Style","Inlet",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"no2.5 IN","NYCORP","no2.5 INNYCORP",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip",4866,161,50,"Fog Tip 161 @ 50",null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip 300 @ 100 4824",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stack Tips No 2.5 in 1-3/8\"; 1-1/4\"; 1\" Yes","2420"]
[null,null,null,null,null,"1.5 inCustom",null,null,null,null,null,null,"2102",1,{"$f":"CONCATENATE(N62,\" in\")","v":"1 in"},"1 in",null,"SOIN1 in","1 in",null,null,{"$f":"CONCATENATE(RIGHT($R62,LEN($R62)-4),S62)","v":"1 in1 in"},null,null,null,null,null,null,null,null,null,null,null,null,"no2.5 IN","PCT","no2.5 INPCT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip",4866,175,50,"Fog Tip 175 @ 50",null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip 300 @ 75 4824",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stack Tips Yes 1.5 in 15/16\"; 1/2\" No (Std)","1441"]
[null,null,null,null,null,"1 inNH",null,null,null,null,null,null,"2126",2.5,{"$f":"CONCATENATE(N63,\" in\")","v":"2.5 in"},"1.5 in",null,"SOIN1.5 in","1.5 in",null,null,{"$f":"CONCATENATE(RIGHT($R63,LEN($R63)-4),S63)","v":"1.5 in1.5 in"},null,null,null,null,null,null,null,null,null,null,null,null,"no2.5 IN","Custom","no2.5 INCustom",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip",4866,185,50,"Fog Tip 185 @ 50",null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip 350 @ 100 4824",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stack Tips Yes 1.5 in 15/16\"; 1/2\" Yes","1440"]
[null,null,null,null,null,"1 inNPSH",null,null,null,null,null,null,"2127",1.5,"1.5 in","1.5 in",null,"SOIN2 in","1.5 in",null,null,"2 in1.5 in",null,null,null,null,null,null,null,null,null,null,null,null,"no2.5 IN","NH","no2.5 INNH",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip",4866,225,"100 (Std)","Fog Tip 225 @ 100 (Std)",null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip 95 @ 100 4866",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stack Tips Yes 2.5 in 1-1/4\"; 1-1/8\"; 1\" No (Std)","2393"]
[null,null,null,null,null,"1 inStorz",null,null,null,null,null,null,"2130",2.5,"2.5 in","2.5 in",null,"SOIN2.5 in","2.5 in","1.5 in",null,"2.5 in2.5 in","2.5 in1.5 in",null,null,null,null,null,null,null,null,null,null,null,"no2.5 IN","NPSH","no2.5 INNPSH",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stack Tips Yes 2.5 in 1-1/8\"; 1/2\" No (Std)","1443"]
[null,null,null,null,null,"1 inCustom",null,null,null,null,null,null,"2390",2.5,"2.5 in","1.5 in",null,"SOIN3 in","2.5 in","1.5 in",null,"3 in2.5 in","3 in1.5 in",null,null,null,null,null,null,null,null,null,null,null,"no2.5 IN","FDNY","no2.5 INFDNY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stack Tips Yes 2.5 in 1-1/8\"; 1/2\" Yes","1442"]
[null,null,null,null,null,"2 inStorz",null,null,null,null,null,null,"2431",1.5,"1.5 in","1.5 in",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"no2.5 IN","NYCORP","no2.5 INNYCORP"]
[null,null,null,null,null,"3 inStorz",null,null,null,null,null,null,"2433",2.5,"2.5 in","1.5 in",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"no2.5 IN","PITT6","no2.5 INPITT6"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"no2.5 IN","BAT","no2.5 INBAT"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"no2.5 IN","CSA","no2.5 INCSA"]
[null,null,null,null,null,null,null,null,null,null,null,null,"Style","Outlet",null,null,"BoreShutoff Only","BoreShutoff with Integrated Tip",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"no2.5 IN","QST","no2.5 INQST"]
[null,null,null,null,null,null,null,null,null,null,null,null,"2102",1,{"$f":"CONCATENATE(N72,\" in\")","v":"1 in"},574,"N/A","7/8\"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"no2.5 IN","Custom","no2.5 INCustom"]
[null,null,null,null,null,null,null,null,null,null,null,null,"2126",1.5,"1.5 in",698,null,"15/16\""]
[null,null,null,null,null,null,null,null,null,null,null,null,"2127",1.5,"1.5 in",562,null,"1\""]
[null,null,null,null,null,null,null,null,null,null,null,null,"2130",2.5,"2.5 in",1078,null,"1-1/16\""]
[null,null,null,null,null,null,null,null,null,null,null,null,"2390",1.5,"1.5 in",1136,null,"1-1/8\""]
[null,null,null,null,null,null,null,null,null,null,null,null,"2431",1.5,"1.5 in",592,null,"1-3/16\""]
[null,null,null,null,null,null,null,null,null,null,null,null,"2433",1.5,"1.5 in",762,null,"1-1/4\""]
[null,null,null,null,null,null,null,null,null,null,null,null,"Storz",null,null,88,null,{"$f":"CONCATENATE(R72,\"2431\")","v":"7/8\"2431"},null,"Shutoff Only","Shutoff with Integrated Tip"]
[null,null,null,null,null,null,null,null,null,null,null,null,"ZT",null,null,340,null,{"$f":"CONCATENATE(R73,\"2431\")","v":"15/16\"2431"},null,"1 in","1.5 in"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(R74,\"2431\")","v":"1\"2431"},null,"1.5 in","2 in"]
[null,null,null,null,null,null,null,null,null,null,null,null,"Style","Outlet",null,null,null,{"$f":"CONCATENATE(R76,\"2431\")","v":"1-1/8\"2431"},null,"2 in","2.5 in"]
[null,null,null,null,null,null,null,null,null,null,null,null,"2102","1 in","Shutoff Only1 in2102",null,null,{"$f":"CONCATENATE(R78,\"2431\")","v":"1-1/4\"2431"},null,"2.5 in","3 in"]
[null,null,null,null,null,null,null,null,null,null,null,null,"2126","1.5 in","Shutoff Only1.5 in2126",null,null,{"$f":"CONCATENATE(R72,\"2433\")","v":"7/8\"2433"},null,"3 in"]
[null,null,null,null,null,null,null,null,null,null,null,null,"2127","1.5 in","Shutoff Only1.5 in2127",null,null,{"$f":"CONCATENATE(R73,\"2433\")","v":"15/16\"2433"}]
[null,null,null,null,null,null,null,null,null,null,null,null,"2130","2.5 in","Shutoff Only2.5 in2130",null,null,{"$f":"CONCATENATE(R74,\"2433\")","v":"1\"2433"}]
[null,null,null,null,null,null,null,null,null,null,null,null,"2390","1.5 in","Shutoff Only1.5 in2390",null,null,{"$f":"CONCATENATE(R76,\"2433\")","v":"1-1/8\"2433"},null,{"$f":"CONCATENATE(T$79,T80)","v":"Shutoff Only1 in"}]
[null,null,null,null,null,null,null,null,null,null,null,null,"2431","1.5 in","Shutoff with Integrated Tip1.5 in2431",null,null,{"$f":"CONCATENATE(R78,\"2433\")","v":"1-1/4\"2433"},null,{"$f":"CONCATENATE(T$79,T81)","v":"Shutoff Only1.5 in"}]
[null,null,null,null,null,null,null,null,null,null,null,null,"2433","1.5 in","Shutoff with Integrated Tip1.5 in2433",null,null,"1-1/16\"2431",null,{"$f":"CONCATENATE(T$79,T82)","v":"Shutoff Only2 in"}]
[null,null,null,null,null,null,null,null,null,null,null,null,"Shutoff Only1 in2102",null,null,null,null,"1-3/16\"2431",null,{"$f":"CONCATENATE(T$79,T83)","v":"Shutoff Only2.5 in"}]
[null,null,null,null,null,null,null,null,null,null,null,null,"Shutoff Only1.5 in2126",null,null,null,null,"1-1/16\"2433",null,{"$f":"CONCATENATE(T$79,T84)","v":"Shutoff Only3 in"}]
[null,null,null,null,null,null,null,null,null,null,null,null,"Shutoff Only1.5 in2127",null,null,null,null,"1-3/16\"2433",null,{"$f":"CONCATENATE(U$79,U80)","v":"Shutoff with Integrated Tip1.5 in"}]
[null,null,null,null,null,null,null,null,null,null,null,null,"Shutoff Only2.5 in2130",null,null,null,null,null,null,{"$f":"CONCATENATE(U$79,U81)","v":"Shutoff with Integrated Tip2 in"}]
[null,null,null,null,null,null,null,null,null,null,null,null,"Shutoff Only1.5 in2390",null,null,null,null,null,null,{"$f":"CONCATENATE(U$79,U82)","v":"Shutoff with Integrated Tip2.5 in"}]
[null,null,null,null,null,null,null,null,null,null,null,null,"Shutoff with Integrated Tip1.5 in2431",null,null,null,null,null,null,{"$f":"CONCATENATE(U$79,U83)","v":"Shutoff with Integrated Tip3 in"}]
[null,null,null,null,null,null,null,null,null,null,null,null,"Shutoff with Integrated Tip1.5 in2433"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,"shutoff only1 in","1 in","shutoff only1 in1 in",2102,null,null,"shutoff only1 in1 in",2102,{"$f":"CONCATENATE(S99,T99)","v":"shutoff only1 in1 in2102"}]
[null,null,null,null,null,null,null,null,null,null,null,null,"shutoff only1.5 in","1.5 in","shutoff only1.5 in1.5 in",2127,null,null,"shutoff only1.5 in1.5 in",2127,{"$f":"CONCATENATE(S100,T100)","v":"shutoff only1.5 in1.5 in2127"}]
[null,null,null,null,null,null,null,null,null,null,null,null,"shutoff only2 in","1.5 in","shutoff only2 in1.5 in",2127,null,null,"shutoff only2 in1.5 in",2127,"shutoff only2 in1.5 in2127"]
[null,null,null,null,null,null,null,null,null,null,null,null,"shutoff only2.5 in","1.5 in","shutoff only2.5 in1.5 in",2126,2390,null,"shutoff only2.5 in1.5 in",2126,"shutoff only2.5 in1.5 in2126"]
[null,null,null,null,null,null,null,null,null,null,null,null,"shutoff only2.5 in","2.5 in","shutoff only2.5 in2.5 in",2130,null,null,"shutoff only2.5 in2.5 in",2130,"shutoff only2.5 in2.5 in2130"]
[null,null,null,null,null,null,null,null,null,null,null,null,"shutoff only3 in","2.5 in","shutoff only3 in2.5 in",2130,null,null,"shutoff only3 in2.5 in",2130,"shutoff only3 in2.5 in2130"]
[null,null,null,null,null,null,null,null,null,null,null,null,"shutoff only3 in","1.5 in","shutoff only3 in1.5 in",2126,2390,null,"shutoff only3 in1.5 in",2126,"shutoff only3 in1.5 in2126"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"shutoff with integrated tip1.5 in1.5 in",2431,null,null,"shutoff with integrated tip1.5 in1.5 in",2431,"shutoff with integrated tip1.5 in1.5 in2431"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"shutoff with integrated tip2 in1.5 in",2431,null,null,"shutoff with integrated tip2 in1.5 in",2431,"shutoff with integrated tip2 in1.5 in2431"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"shutoff with integrated tip2.5 in1.5 in",2433,null,null,"shutoff with integrated tip2.5 in1.5 in",2433,"shutoff with integrated tip2.5 in1.5 in2433"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"shutoff with integrated tip3 in1.5 in",2433,null,null,"shutoff with integrated tip3 in1.5 in",2433,"shutoff with integrated tip3 in1.5 in2433"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"shutoff only2.5 in1.5 in",2390,"shutoff only2.5 in1.5 in2390"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"shutoff only3 in1.5 in",2390,"shutoff only3 in1.5 in2390"]
[null,null,null,null,null,null,null,null,null,null,null,null,2102]
[null,null,null,null,null,null,null,null,null,null,null,null,2126]

{"sheet":"Multi-Purpose","index":5,"n_rows":111,"n_cols":158,"rows_kept":111,"cut":false,"hidden":false,"merged":[[7,1,8,1],[7,2,8,2],[7,3,8,3],[13,1,14,1],[13,2,14,6],[10,2,10,3],[11,5,11,6],[12,2,12,6],[11,3,11,4],[7,10,8,10],[11,7,12,9],[11,10,12,10],[7,4,8,4],[7,5,8,5],[7,6,8,6],[6,3,6,7],[15,2,17,10],[0,7,5,7],[0,8,1,10],[1,1,1,5],[2,1,2,5],[2,8,3,10],[3,1,3,5],[4,1,4,5],[4,8,5,10],[5,1,5,5],[13,7,14,7],[13,8,14,10],[7,7,8,7],[7,8,8,8],[7,9,8,9]]}
[null,"Instructions:",null,null,null,null,null,"Reaction Force Color Chart:","This is a Low RF Nozzle (RF < 51 )",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"asdf",null,null,"Style","Flow",null,"Flow",null,null,null,null,null,null,100,75,50,87,null,null,"Bore Size","Style",null,null,null,"Flow",null,null,null,"Flow","Pressure",null,null,null,null,null,null,null,"Style","Flow","Pressure",null,null,null,null,null,"Style",null,null,null,null,null,null,null,null,null,null,null,null,"Bore Size",null,null,null,null,null,null,"Bore Size",null,null,null,null,"Bore Size",null,"Bore,Shutoff,Inlet,Remove Grip",null,null,"Bore Size","Style","Inlet","Dec Size","Shutoff","Remove PG",null,"Bore Size","Dec Size",null,"Solid Bore No 1.5 in","Solid Bore No 2.5 in","Solid Bore Yes 1.5 in","Solid Bore Yes 2.5 in","Stack Tips No 1.5 in","Stack Tips No 2.5 in","Stack Tips Yes 1.5 in","Stack Tips Yes 2.5 in",null,null,"Bore,Shutoff,Inlet,Remove Grip","Style",null,null,null,"Bore Size","Bore Size",null,null,"Bore Size","Style","Inlet","Dec Size","Shutoff",null,null,null,null,null,null,null,null,50,null,null,"Bore Size","Style"]
[null,"Tan-colored cells are headers or describe the selection options",null,null,null,null,null,null,null,null,null,null,"Nozzle",null,"SaberJet Fog Nozzle","UltraJet Fog Nozzle",null,"5-40","125-250","13-30","13-60","18-30","30-125","30-150","30-200","95-200","12-53",null,null,null,null,null,null,null,null,null,"4116",60,null,13,"100 (Std)",null,null,null,null,4116,60,60,null,60,null,"Solid Bore","3/4\"","0416","1.5 in",0.75,"Fog Nozzle",13,"Fog Nozzle 13",null,null,13,"100 (Std)",{"$f":"CONCATENATE(BJ2,\" \",BK2)","v":"13 100 (Std)"},null,200,"100 (Std)",null,null,"Fog Nozzle",4116,60,"100 (Std)",{"$f":"CONCATENATE(BR2,\" \",BT2,\" @ \",BU2)","v":"Fog Nozzle 60 @ 100 (Std)"},null,null,null,"Fog Nozzle 125 @ 100",4116,4863,null,{"$f":"CONCATENATE($BZ2,\" \",CA2)","v":"Fog Nozzle 125 @ 100 4116"},{"$f":"CONCATENATE($BZ2,\" \",CB2)","v":"Fog Nozzle 125 @ 100 4863"},"Fog_Nozzle_125___100",null,null,"Fog Nozzle 125 @ 100 4116",null,null,null,"Solid Bore","3/8\"",0.375,{"$f":"CONCATENATE(CM2,\" \",CN2)","v":"Solid Bore 3/8\""},null,null,null,"Solid Bore 1.5 in","3/4\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 1.5 in","3/4\"",null,{"$f":"CONCATENATE(DD2,\" \",DI2,\" \",DG2,\" \",DE2,\" \",DJ2)","v":"Solid Bore No 1.5 in 3/4\" Yes"},{"$f":"CONCATENATE(DD2,\" \",DI2,\" \",DG2)","v":"Solid Bore No 1.5 in"},"Solid Bore","3/4\"","0416","1.5 in",0.75,"No","Yes","Solid Bore No 1.5 in",null,0.375,null,"3/8\"","7/8\"","1/2\"","7/8\"","1-1/8\"; 1/2\"","1-1/2\"; 1-1/4\"; 1\"","15/16\"; 1/2\"","1-1/8\"; 1/2\"",null,null,"Solid Bore No 1.5 in 1\" Yes","0416","1417","1499",null,"3/4\"","3_4_",null,"Solid Bore","3/4\"","0416","1.5 in",0.75,"No",{"$f":"CONCATENATE(EG2,\" \",EJ2,\" \",EL2,\" \",EH2,\" \",EI2)","v":"Solid Bore 1.5 in No 3/4\" 0416"},null,"Solid Bore 1.5 in No 3/4\" 0416",null,null,null,0.375,"3/8\"",{"$f":"CONCATENATE(ROUND(29.71*(ES2*ES2)*SQRT(EU$1),0),\" gpm @ 50 psi; RF = \",ROUND(1.57*(ES2*ES2)*EU$1,0))","v":"30 gpm @ 50 psi; RF = 11"},null,"Solid Bore","3/4\"","0416",{"$f":"_xlfn.CONCAT(EW2:EY2)","v":"Solid Bore3/4\"0416"},null,"Solid Bore3/4\"0416"]
[null,"Use the green-colored cells to make your selections (All cells must be filled in; information from \"FrontPage\" tab does not carry over to this page)",null,null,null,null,null,null,"This is a Nozzle with Increased RF (RF > 50 and <101 )",null,null,null,"Tip",null,"1.5 in","1.5 in",null,"100 (Std)","100 (Std)","100 (Std)","100 (Std)","100 (Std)","100 (Std)","100 (Std)","100 (Std)","100 (Std)","87 (CE)",null,null,null,null,null,null,null,null,null,"4116",95,null,25,"100 (Std)",null,null,null,null,4116,95,95,null,95,null,"Solid Bore","7/8\"","0416","1.5 in",0.875,"Fog Nozzle",25,"Fog Nozzle 25",null,null,25,"100 (Std)",{"$f":"CONCATENATE(BJ3,\" \",BK3)","v":"25 100 (Std)"},null,250,"100 (Std)",null,null,"Fog Nozzle",4116,60,75,{"$f":"CONCATENATE(BR3,\" \",BT3,\" @ \",BU3)","v":"Fog Nozzle 60 @ 75"},null,null,null,"Fog Nozzle 125 @ 75",4116,4863,null,{"$f":"CONCATENATE($BZ3,\" \",CA3)","v":"Fog Nozzle 125 @ 75 4116"},{"$f":"CONCATENATE($BZ3,\" \",CB3)","v":"Fog Nozzle 125 @ 75 4863"},null,null,null,"Fog Nozzle 125 @ 100 4863",null,null,null,"Solid Bore","1/2\"",0.5,{"$f":"CONCATENATE(CM3,\" \",CN3)","v":"Solid Bore 1/2\""},null,null,null,"Solid Bore 1.5 in","7/8\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 1.5 in","7/8\"",null,{"$f":"CONCATENATE(DD3,\" \",DI3,\" \",DG3,\" \",DE3,\" \",DJ3)","v":"Solid Bore No 1.5 in 7/8\" Yes"},{"$f":"CONCATENATE(DD3,\" \",DI3,\" \",DG3)","v":"Solid Bore No 1.5 in"},"Solid Bore","7/8\"","0416","1.5 in",0.875,"No","Yes","Solid Bore No 1.5 in",null,0.5,null,"1/2\"","15/16\"","7/8\"","15/16\"","15-16\"; 1/2\"","1-1/4\"; 1-1/8\"; 1\"",null,"1-1/4\"; 1-1/8\"; 1\"",null,null,"Solid Bore No 1.5 in 1/2\" Yes","1417",null,null,null,"7/8\"","7_8_",null,"Solid Bore","7/8\"","0416","1.5 in",0.875,"No",{"$f":"CONCATENATE(EG3,\" \",EJ3,\" \",EL3,\" \",EH3,\" \",EI3)","v":"Solid Bore 1.5 in No 7/8\" 0416"},null,"Solid Bore 1.5 in No 7/8\" 0416",null,null,null,0.5,"1/2\"","53 gpm @ 50 psi; RF = 20",null,"Solid Bore","7/8\"","0416",{"$f":"_xlfn.CONCAT(EW3:EY3)","v":"Solid Bore7/8\"0416"},null,"Solid Bore7/8\"0416"]
[null,"Blue-colored cells provide outputs based on your selections",null,null,null,null,null,null,null,null,null,null,"High Pressure",null,"2 in","2 in",null,75,75,null,null,null,75,75,75,75,null,null,null,null,null,null,null,null,null,null,"4116",125,null,40,"100 (Std)",null,null,null,null,4116,125,125,null,125,null,"Solid Bore","1\"","0416","1.5 in",1,"Fog Nozzle",40,"Fog Nozzle 40",null,null,40,"100 (Std)","40 100 (Std)",null,300,"100 (Std)",null,null,"Fog Nozzle",4116,60,"87 (CE)","Fog Nozzle 60 @ 87 (CE)",null,null,null,"Fog Nozzle 125 @ 87",4116,null,null,{"$f":"CONCATENATE($BZ4,\" \",CA4)","v":"Fog Nozzle 125 @ 87 4116"},null,null,null,null,"Fog Nozzle 125 @ 75 4116",null,null,null,"Solid Bore","5/8\"",0.625,"Solid Bore 5/8\"",null,null,null,"Solid Bore 1.5 in","1\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 1.5 in","1\"",null,"Solid Bore No 1.5 in 1\" Yes","Solid Bore No 1.5 in","Solid Bore","1\"","0416","1.5 in",1,"No","Yes","Solid Bore No 1.5 in",null,0.625,null,"5/8\"","1\"","15/16\"","1\"","1-1/16\"; 15/16\"","1-3/8\"; 1-1/4\"; 1\"",null,null,null,null,"Solid Bore No 1.5 in 1-1/16\" Yes","1499",null,null,null,"1\"","1_",null,"Solid Bore","1\"","0416","1.5 in",1,"No","Solid Bore 1.5 in No 1\" 0416",null,"Solid Bore 1.5 in No 1\" 0416",null,null,null,0.625,"5/8\"","82 gpm @ 50 psi; RF = 31",null,"Solid Bore","1\"","0416","Solid Bore1\"0416",null,"Solid Bore1\"0416"]
[null,"This shaded cell indicates an error has ocurred and you may need to modify some of your selections or contact our Customer Care team",null,null,null,null,null,null,"This Nozzle has a High RF (RF > 100 )",null,null,null,null,null,"2.5 in","2.5 in",null,"87 (CE)",null,null,null,null,"87 (CE)","87 (CE)",null,null,null,null,null,"5-40","100 (Std)",{"$f":"CONCATENATE(AD5,\" \",AE5)","v":"5-40 100 (Std)"},null,null,null,null,"4116",150,null,60,"100 (Std)",75,"87 (CE)",null,null,4116,150,150,null,150,null,"Solid Bore","1-1/8\"","0416","1.5 in",1.125,"Fog Nozzle",60,"Fog Nozzle 60",null,null,60,"100 (Std)","60 100 (Std)",null,350,"100 (Std)",null,null,"Fog Nozzle",4116,95,"100 (Std)","Fog Nozzle 95 @ 100 (Std)",null,null,null,"Fog Nozzle 13 @ 100",4802,null,null,{"$f":"CONCATENATE($BZ5,\" \",CA5)","v":"Fog Nozzle 13 @ 100 4802"},null,null,null,null,"Fog Nozzle 125 @ 75 4863",null,null,null,"Solid Bore","3/4\"",0.75,"Solid Bore 3/4\"",null,null,null,"Solid Bore 1.5 in","1-1/8\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 1.5 in","1-1/8\"",null,"Solid Bore No 1.5 in 1-1/8\" Yes","Solid Bore No 1.5 in","Solid Bore","1-1/8\"","0416","1.5 in",1.125,"No","Yes","Solid Bore No 1.5 in",null,0.75,null,"3/4\"","1-1/8\"","1\"","1-1/16\"","1-1/4\"; 1-1/8\"; 1\"",null,null,null,null,null,"Solid Bore No 1.5 in 1-1/4\" Yes","0416","1417","1499",null,"1-1/8\"","1_1_8_",null,"Solid Bore","1-1/8\"","0416","1.5 in",1.125,"No","Solid Bore 1.5 in No 1-1/8\" 0416",null,"Solid Bore 1.5 in No 1-1/8\" 0416",null,null,null,0.75,"3/4\"","118 gpm @ 50 psi; RF = 44",null,"Solid Bore","1-1/8\"","0416","Solid Bore1-1/8\"0416",null,"Solid Bore1-1/8\"0416"]
[null,"Orange-colored cell allows you to input your discount for Net Price",null,null,null,null,null,null,null,null,null,null,null,null,"3 in","3 in",null,null,null,null,null,null,null,null,null,null,null,null,null,"5-40",75,{"$f":"CONCATENATE(AD6,\" \",AE6)","v":"5-40 75"},null,null,null,null,"4802",13,null,95,"100 (Std)",75,"87 (CE)",null,null,4802,13,null,null,null,null,"Solid Bore","1-1/4\"","0416","1.5 in",1.25,"Fog Nozzle",95,"Fog Nozzle 95",null,null,60,"87 (CE)","60 87 (CE)",null,200,75,null,null,"Fog Nozzle",4116,95,75,"Fog Nozzle 95 @ 75",null,null,null,"Fog Nozzle 150 @ 100",4116,4863,null,"Fog Nozzle 150 @ 100 4116",{"$f":"CONCATENATE($BZ6,\" \",CB6)","v":"Fog Nozzle 150 @ 100 4863"},null,null,null,"Fog Nozzle 125 @ 87 4116",null,null,null,"Solid Bore","7/8\"",0.875,"Solid Bore 7/8\"",null,null,null,"Solid Bore 1.5 in","1-1/4\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 1.5 in","1-1/4\"",null,"Solid Bore No 1.5 in 1-1/4\" Yes","Solid Bore No 1.5 in","Solid Bore","1-1/4\"","0416","1.5 in",1.25,"No","Yes","Solid Bore No 1.5 in",null,0.875,null,"7/8\"","1-1/4\"","1-1/16\"","1-1/8\"",null,null,null,null,null,null,"Solid Bore No 1.5 in 1-1/8\" Yes","0416","1417","1499",null,"1-1/4\"","1_1_4_",null,"Solid Bore","1-1/4\"","0416","1.5 in",1.25,"No","Solid Bore 1.5 in No 1-1/4\" 0416",null,"Solid Bore 1.5 in No 1-1/4\" 0416",null,null,null,0.875,"7/8\"","161 gpm @ 50 psi; RF = 60",null,"Solid Bore","1-1/4\"","0416","Solid Bore1-1/4\"0416",null,"Solid Bore1-1/4\"0416"]
[null,{"$f":"FrontPage!E8","v":"Rev Date: 6/27/2022"},null,"Multipurpose Fog Nozzles (UltraJet and SaberJet)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"5-40","87 (CE)","5-40 87 (CE)",null,null,null,null,"4802",25,null,125,"100 (Std)",75,50,"87 (CE)",null,4802,25,null,null,null,null,"Solid Bore","3/8\"","1417","1.5 in",0.375,"Fog Nozzle",125,"Fog Nozzle 125",null,null,60,75,"60 75",null,250,75,null,null,"Fog Nozzle",4116,95,"87 (CE)","Fog Nozzle 95 @ 87 (CE)",null,null,null,"Fog Nozzle 150 @ 50",4863,null,null,"Fog Nozzle 150 @ 50 4863",null,null,null,null,"Fog Nozzle 13 @ 100 4802",null,null,null,"Solid Bore","15/16\"",0.9375,"Solid Bore 15/16\"",null,null,null,"Solid Bore 1.5 in","3/8\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 1.5 in","3/8\"",null,"Solid Bore No 1.5 in 3/8\" Yes","Solid Bore No 1.5 in","Solid Bore","3/8\"","1417","1.5 in",0.375,"No","Yes","Solid Bore No 1.5 in",null,0.9375,null,"15/16\"","1-3/8\"","1-1/8\"","1-3/16\"",null,null,null,null,null,null,"Solid Bore No 1.5 in 1-3/16\" Yes","1499",null,null,null,"3/8\"","3_8_",null,"Solid Bore","3/8\"","1417","1.5 in",0.375,"No","Solid Bore 1.5 in No 3/8\" 1417",null,"Solid Bore 1.5 in No 3/8\" 1417",null,null,null,0.9375,"15/16\"","185 gpm @ 50 psi; RF = 69",null,"Solid Bore","3/8\"","1417","Solid Bore3/8\"1417",null,"Solid Bore3/8\"1417"]
[null,"SaberJet or UltraJet","Inlet Size",{"$f":"IF(B10=\"SaberJet Fog Nozzle\",\"Fog Flow Rate\",\"\")","v":""},"Solid Bore Size","Inlet Thread","Fog Flow Reaction Force",{"$f":"IF(J10=\"yes\",\"\",\"Remove Pistol Grip?\")","v":"Remove Pistol Grip?"},"Style Number",{"$f":"IF(TRIM(I10)=\"2390\",\"\",\"ZT Inlet?\")","v":"ZT Inlet?"},"Custom Etch",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"125-250","100 (Std)","125-250 100 (Std)",null,null,null,null,"4802",40,null,150,"100 (Std)",75,50,"87 (CE)",null,4802,40,null,null,null,null,"Solid Bore","1/2\"","1417","1.5 in",0.5,"Fog Nozzle",150,"Fog Nozzle 150",null,null,95,"100 (Std)","95 100 (Std)",null,300,75,null,null,"Fog Nozzle",4116,125,"100 (Std)","Fog Nozzle 125 @ 100 (Std)",null,null,null,"Fog Nozzle 150 @ 75",4116,4863,null,"Fog Nozzle 150 @ 75 4116",{"$f":"CONCATENATE($BZ8,\" \",CB8)","v":"Fog Nozzle 150 @ 75 4863"},null,null,null,"Fog Nozzle 150 @ 100 4116",null,null,null,"Solid Bore","1\"",1,"Solid Bore 1\"",null,null,null,"Solid Bore 1.5 in","1/2\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 1.5 in","1/2\"",null,"Solid Bore No 1.5 in 1/2\" Yes","Solid Bore No 1.5 in","Solid Bore","1/2\"","1417","1.5 in",0.5,"No","Yes","Solid Bore No 1.5 in",null,1,null,"1\"",null,"1-3/16\"","1-1/4\"",null,null,null,null,null,null,"Solid Bore No 1.5 in 1-3/8\" Yes","1499",null,null,null,"1/2\"","1_2_",null,"Solid Bore","1/2\"","1417","1.5 in",0.5,"No","Solid Bore 1.5 in No 1/2\" 1417",null,"Solid Bore 1.5 in No 1/2\" 1417",null,null,null,1,"1\"","210 gpm @ 50 psi; RF = 79",null,"Solid Bore","1/2\"","1417","Solid Bore1/2\"1417",null,"Solid Bore1/2\"1417"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore","Stack Tips",null,null,null,null,null,null,null,null,null,null,null,null,null,"125-250",75,"125-250 75",null,null,null,null,"4824",200,null,161,50,null,null,null,null,4824,200,200,null,null,null,"Solid Bore","5/8\"","1417","1.5 in",0.625,"Fog Nozzle",161,"Fog Nozzle 161",null,null,95,75,"95 75",null,210,50,null,null,"Fog Nozzle",4116,125,75,"Fog Nozzle 125 @ 75",null,null,null,"Fog Nozzle 150 @ 87",4116,null,null,"Fog Nozzle 150 @ 87 4116",null,null,null,null,"Fog Nozzle 150 @ 100 4863",null,null,null,"Solid Bore","1-1/16\"",1.0625,"Solid Bore 1-1/16\"",null,null,null,"Solid Bore 1.5 in","5/8\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 1.5 in","5/8\"",null,"Solid Bore No 1.5 in 5/8\" Yes","Solid Bore No 1.5 in","Solid Bore","5/8\"","1417","1.5 in",0.625,"No","Yes","Solid Bore No 1.5 in",null,1.0625,null,"1-1/16\"",null,"1-1/4\"","1-3/8\"",null,null,null,null,null,null,"Solid Bore No 1.5 in 15/16\" Yes","1417","1499",null,null,"5/8\"","5_8_",null,"Solid Bore","5/8\"","1417","1.5 in",0.625,"No","Solid Bore 1.5 in No 5/8\" 1417",null,"Solid Bore 1.5 in No 5/8\" 1417",null,null,null,1.0625,"1-1/16\"","237 gpm @ 50 psi; RF = 89",null,"Solid Bore","5/8\"","1417","Solid Bore5/8\"1417",null,"Solid Bore5/8\"1417"]
[null,"UltraJet Fog Nozzle","1.5 in","95 @ 100","7/8\"","NH",{"$f":"IFERROR(IF(I10=\"\",\"\",ROUND(0.0505*IF(TRIM(I10)=\"1820\",VALUE(LEFT(E11,3)),IF(I10=\"1520\",95,135))*SQRT(IF(TRIM(I10)=\"1820\",50,100)),0)),\"Fix Bore Size\")","v":57},"No (Std)",{"$f":"IF(B10=P2,\"1820\",IFERROR(VLOOKUP(CONCATENATE(B10,E10,D10),BF63:BG69,2,FALSE),\"\"))","v":"1820"},"No (Std)","No (Std)",null,null,null,"1.5 in","1.5 in",null,null,null,null,null,null,null,"INDIRECT(CONCATENATE(\"tHREAD\",SUBSTITUTE(B4,\" \",\"_\")))",null,null,null,null,null,"13-30","100 (Std)","13-30 100 (Std)",null,null,null,null,"4824",210,null,175,"100 (Std)",75,50,null,null,4824,null,null,210,null,null,"Solid Bore","3/4\"","1417","1.5 in",0.75,"Fog Nozzle",175,"Fog Nozzle 175",null,null,95,"87 (CE)","95 87 (CE)",null,250,50,null,null,"Fog Nozzle",4116,125,"87 (CE)","Fog Nozzle 125 @ 87 (CE)",null,null,null,"Fog Nozzle 161 @ 50",4863,null,null,"Fog Nozzle 161 @ 50 4863",null,null,null,null,"Fog Nozzle 150 @ 50 4863",null,null,null,"Solid Bore","1-1/8\"",1.125,"Solid Bore 1-1/8\"",null,null,null,"Solid Bore 1.5 in","3/4\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 1.5 in","15/16\"",null,"Solid Bore No 1.5 in 3/4\" Yes","Solid Bore No 1.5 in","Solid Bore","3/4\"","1417","1.5 in",0.75,"No","Yes","Solid Bore No 1.5 in",null,1.125,null,"1-1/8\"",null,"1-3/8\"",null,null,null,null,null,null,null,"Solid Bore No 1.5 in 3/4\" Yes","0416","1417",null,null,"3/4\"","3_4_",null,"Solid Bore","3/4\"","1417","1.5 in",0.75,"No","Solid Bore 1.5 in No 3/4\" 1417",null,"Solid Bore 1.5 in No 3/4\" 1417",null,null,null,1.125,"1-1/8\"","266 gpm @ 50 psi; RF = 99",null,"Solid Bore","3/4\"","1417","Solid Bore3/4\"1417",null,"Solid Bore3/4\"1417"]
[null,"List price",{"$f":"SUM(E11:K11)","v":1578},null,{"$f":"IF(E21=\"false\",\"Fix Bore Size\",VLOOKUP(E10,ET:EU,2,FALSE))","v":"161 gpm @ 50 psi; RF = 60"},{"$f":"IF(OR(F10=\"Storz\",F10=\"BIM\"),_xlfn.XLOOKUP(\"storz\",M:M,N:N),0)","v":0},null,null,{"$f":"IFERROR(VLOOKUP(TRIM(I10),M:N,2,FALSE),\"\")","v":1578},{"$f":"IF(J8=\"\",0,IF(J10=\"Yes\",_xlfn.XLOOKUP(\"zt\",M:M,N:N),0))","v":0},null,null,null,null,"2.5 in","2.5 in",null,null,null,null,null,null,null,null,null,null,null,null,null,"13-60","100 (Std)","13-60 100 (Std)",null,null,null,null,"4824",250,null,185,50,null,null,null,null,4824,250,250,250,null,null,"Solid Bore","7/8\"","1417","1.5 in",0.875,"Fog Nozzle",200,"Fog Nozzle 200",null,null,125,"100 (Std)","125 100 (Std)",null,null,null,null,null,"Fog Nozzle",4116,150,"100 (Std)","Fog Nozzle 150 @ 100 (Std)",null,null,null,"Fog Nozzle 175 @ 100",4863,null,null,"Fog Nozzle 175 @ 100 4863",null,null,null,null,"Fog Nozzle 150 @ 75 4116",null,null,null,"Solid Bore","1-3/16\"",1.1875,"Solid Bore 1-3/16\"",null,null,null,"Solid Bore 1.5 in","7/8\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 1.5 in","1-1/16\"",null,"Solid Bore No 1.5 in 7/8\" Yes","Solid Bore No 1.5 in","Solid Bore","7/8\"","1417","1.5 in",0.875,"No","Yes","Solid Bore No 1.5 in",null,1.1875,null,"1-3/16\"",null,null,null,null,null,null,null,null,null,"Solid Bore No 1.5 in 3/8\" Yes","1417",null,null,null,"7/8\"","7_8_",null,"Solid Bore","7/8\"","1417","1.5 in",0.875,"No","Solid Bore 1.5 in No 7/8\" 1417",null,"Solid Bore 1.5 in No 7/8\" 1417",null,null,null,1.1875,"1-3/16\"","296 gpm @ 50 psi; RF = 111",null,"Solid Bore","7/8\"","1417","Solid Bore7/8\"1417",null,"Solid Bore7/8\"1417"]
[null,"Your Discount",0.3,"Net Price",null,{"$f":"ROUND(C11*(1-C12),2)","v":1104.5999999999999},null,"Include Color Clips for Shutoff and/or Pistol Grip?",null,null,"Yes",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(B10,\" \",C10,\" \",D10,\" \",E10,\" \",I10)","v":"UltraJet Fog Nozzle 1.5 in 95 @ 100 7/8\" 1820"},null,null,null,null,null,"18-30","100 (Std)","18-30 100 (Std)",null,null,null,null,"4824",265,null,200,"100 (Std)",75,null,null,null,4824,300,300,null,null,null,"Solid Bore","15/16\"","1417","1.5 in",0.9375,"Fog Nozzle",210,"Fog Nozzle 210",null,null,125,75,"125 75",null,null,null,null,null,"Fog Nozzle",4116,150,75,"Fog Nozzle 150 @ 75",null,null,null,"Fog Nozzle 175 @ 50",4863,null,null,"Fog Nozzle 175 @ 50 4863",null,null,null,null,"Fog Nozzle 150 @ 75 4863",null,null,null,"Solid Bore","1-1/4\"",1.25,"Solid Bore 1-1/4\"",null,null,null,"Solid Bore 1.5 in","15/16\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 1.5 in","1-3/16\"",null,"Solid Bore No 1.5 in 15/16\" Yes","Solid Bore No 1.5 in","Solid Bore","15/16\"","1417","1.5 in",0.9375,"No","Yes","Solid Bore No 1.5 in",null,1.25,null,"1-1/4\"",null,null,null,null,null,null,null,null,null,"Solid Bore No 1.5 in 5/8\" Yes","1417",null,null,null,"15/16\"","15_16_",null,"Solid Bore","15/16\"","1417","1.5 in",0.9375,"No","Solid Bore 1.5 in No 15/16\" 1417",null,"Solid Bore 1.5 in No 15/16\" 1417",null,null,null,1.25,"1-1/4\"","328 gpm @ 50 psi; RF = 123",null,"Solid Bore","15/16\"","1417","Solid Bore15/16\"1417",null,"Solid Bore15/16\"1417"]
[null,"Short Description",{"$f":"IF(B21=\"Error\",\"Fix Errors\",CONCATENATE(I10,\" \",C10,\" \",F10,\" \",IF(I10=\"1820\",LEFT(E11,3),TRIM(LEFT(D10,3))),\" \",CONCATENATE(E10,\" bore size(s)\"),IF(I10=\"1820\",\" 50 \",\" 100 (Std) \"),Q32,IF(TRIM(I10)=\"2390\",\"  \",IF(J10=\"yes\", \" PG\",IF(H10=\"yes\",\" NPG\",\" PG\"))),IF(TRIM(I10)=\"2390\",\"\",IF(J10=\"Yes\",\" ZT\",\"\")),IF(K10=\"Yes\",\" ETCH\",\"\")))","v":"1820 1.5 in NH 161 7/8\" bore size(s) 50 BLACK (Std) PG"},null,null,null,null,null,null,null,null,null,"1 IN","NH",null,null,null,"1 in","1.5 in","2 in","2.5 in","3 in",null,null,null,null,null,null,null,"30-125","100 (Std)","30-125 100 (Std)",null,null,null,null,"4824",300,null,210,50,null,null,null,null,4824,350,null,null,null,null,"Solid Bore","1\"","1417","1.5 in",1,"Fog Nozzle",225,"Fog Nozzle 225",null,null,125,50,"125 50",null,null,null,null,null,"Fog Nozzle",4116,150,"87 (CE)","Fog Nozzle 150 @ 87 (CE)",null,null,null,"Fog Nozzle 175 @ 75",4863,null,null,"Fog Nozzle 175 @ 75 4863",null,null,null,null,"Fog Nozzle 150 @ 87 4116",null,null,null,"Solid Bore","1-3/8\"",1.375,"Solid Bore 1-3/8\"",null,null,null,"Solid Bore 1.5 in","1\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 1.5 in","1-3/8\"",null,"Solid Bore No 1.5 in 1\" Yes","Solid Bore No 1.5 in","Solid Bore","1\"","1417","1.5 in",1,"No","Yes","Solid Bore No 1.5 in",null,1.375,null,"1-3/8\"",null,null,null,null,null,null,null,null,null,"Solid Bore No 1.5 in 7/8\" Yes","0416","1417","1499",null,"1\"","1_",null,"Solid Bore","1\"","1417","1.5 in",1,"No","Solid Bore 1.5 in No 1\" 1417",null,"Solid Bore 1.5 in No 1\" 1417",null,null,null,1.375,"1-3/8\"","397 gpm @ 50 psi; RF = 148",null,"Solid Bore","1\"","1417","Solid Bore1\"1417",null,"Solid Bore1\"1417"]
[null,"Long Description",{"$f":"IF(B21=\"Error\",\"Some of your selections are not compatible with others; please correct the errors highlighted in RED\",CONCATENATE(\"Style \",I10,\" \",B10,\" with \",C10,\" \",F10,\" inlet; \",CONCATENATE(TRIM(LEFT(IF(I10=\"1820\",E11,D10),3)),\" gpm @ \",IF(I10=\"1820\",50,100),\" psi fog flow (RF = \",G10,\"); \"),IF(B10=\"shutoff only\",\"\",CONCATENATE(E10,\" solid bore tip (\",E11,\"); \",)),\"Black (Std) bumper;\",IF(J10=\"Yes\",\" Zero-Torque Grip\",\" pistol grip\"),IF(K10=\"Yes\",\"; Custom Etched\",\"\")))","v":"Style 1820 UltraJet Fog Nozzle with 1.5 in NH inlet; 161 gpm @ 50 psi fog flow (RF = 57); 7/8\" solid bore tip (161 gpm @ 50 psi; RF = 60); Black (Std) bumper; pistol grip"},null,null,null,null,"Akron Brass Part Number and Description",{"$f":"IF(AND(OR(F10=\"custom\",G10=\"custom\"),K10=\"yes\"),\"Contact Customer Care to request Custom Thread and Etch (800-228-1161)\",IF(OR(F10=\"custom\",G10=\"custom\"),\"Contact Customer Care to request Custom Thread (800-228-1161)\",IF(K10=\"Yes\",\"Contact Customer Care to request Custom Etch (800-228-1161)\",IF(B21=\"Error\",\"Incompatible selections; please correct errors highlighted in RED\",IFERROR(CONCATENATE(VLOOKUP(C13,DataSource!AH:AJ,2,FALSE),\"      \",VLOOKUP(C13,DataSource!AH:AJ,3,FALSE)),\"Version you've requested not yet created; contact Customer Care (800-228-1161)\")))))","v":"18204002      ULTRAJET 1.5NH 7/8 TIP"},null,null,null,"1 IN","NPSH",null,null,"30-125",13,60,60,60,60,null,"Stack_Tips_Yes_2.5_in_1_1_4___ 1_1_8___ 1__No__Std",null,null,null,null,null,"30-125",75,"30-125 75",null,null,null,null,"4824",350,null,225,"100 (Std)",null,null,null,null,4826,200,200,null,null,null,"Solid Bore","1-1/8\"","1417","1.5 in",1.125,"Fog Nozzle",250,"Fog Nozzle 250",null,null,125,"87 (CE)","125 87 (CE)",null,null,null,null,null,"Fog Nozzle",4802,13,"100 (Std)","Fog Nozzle 13 @ 100 (Std)",null,null,null,"Fog Nozzle 185 @ 50",4863,null,null,"Fog Nozzle 185 @ 50 4863",null,null,null,null,"Fog Nozzle 161 @ 50 4863",null,null,null,"Stack Tips","1-1/8\"; 1/2\"",0.5,"Stack Tips 1-1/8\"; 1/2\"",null,null,null,"Solid Bore 1.5 in","1-1/8\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 2.5 in","7/8\"",null,"Solid Bore No 1.5 in 1-1/8\" Yes","Solid Bore No 1.5 in","Solid Bore","1-1/8\"","1417","1.5 in",1.125,"No","Yes","Solid Bore No 2.5 in",null,0.875,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore No 2.5 in 1\" Yes","0489",null,null,null,"1-1/8\"","1_1_8_",null,"Solid Bore","1-1/8\"","1417","1.5 in",1.125,"No","Solid Bore 1.5 in No 1-1/8\" 1417",null,"Solid Bore 1.5 in No 1-1/8\" 1417",null,null,null,null,null,null,null,"Solid Bore","1-1/8\"","1417","Solid Bore1-1/8\"1417",null,"Solid Bore1-1/8\"1417"]
[null,null,null,null,null,null,null,null,null,null,null,null,"1 IN","STORZ",null,null,"30-150",25,95,95,95,95,null,"Stack_Tips_Yes_2.5_in_1_1_4___1_1_8___1__No__Std",null,null,null,null,null,"30-125","87 (CE)","30-125 87 (CE)",null,null,null,null,"4826",200,null,250,"100 (Std)",75,50,null,null,4826,null,null,210,null,null,"Solid Bore","1-1/4\"","1417","1.5 in",1.25,"Fog Nozzle",265,"Fog Nozzle 265",null,null,150,"100 (Std)","150 100 (Std)",null,null,null,null,null,"Fog Nozzle",4802,25,"100 (Std)","Fog Nozzle 25 @ 100 (Std)",null,null,null,"Fog Nozzle 200 @ 100",4826,4863,null,"Fog Nozzle 200 @ 100 4826","Fog Nozzle 200 @ 100 4863",null,null,null,"Fog Nozzle 175 @ 100 4863",null,null,null,"Stack Tips","15-16\"; 1/2\"",0.5,"Stack Tips 15-16\"; 1/2\"",null,null,null,"Solid Bore 1.5 in","1-1/4\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 2.5 in","15/16\"",null,"Solid Bore No 1.5 in 1-1/4\" Yes","Solid Bore No 1.5 in","Solid Bore","1-1/4\"","1417","1.5 in",1.25,"No","Yes","Solid Bore No 2.5 in",null,0.9375,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore No 2.5 in 1-1/4\" Yes","0489",null,null,null,"1-1/4\"","1_1_4_",null,"Solid Bore","1-1/4\"","1417","1.5 in",1.25,"No","Solid Bore 1.5 in No 1-1/4\" 1417",null,"Solid Bore 1.5 in No 1-1/4\" 1417",null,null,null,null,null,null,null,"Solid Bore","1-1/4\"","1417","Solid Bore1-1/4\"1417",null,"Solid Bore1-1/4\"1417"]
[null,"Notes: ","You can make any notes about what you want, or anything else, in this space",null,null,null,null,null,null,null,null,null,"1.5 in",null,null,null,"30-200",40,125,125,125,125,null,null,null,null,null,null,null,"30-150","100 (Std)","30-150 100 (Std)",null,null,null,null,"4826",210,null,265,50,null,null,null,null,4826,250,250,250,null,null,"Solid Bore","7/8\"","1445","1.5 in",0.875,"Fog Nozzle",300,"Fog Nozzle 300",null,null,150,75,"150 75",null,null,null,null,null,"Fog Nozzle",4802,40,"100 (Std)","Fog Nozzle 40 @ 100 (Std)",null,null,null,"Fog Nozzle 200 @ 75",4826,4863,null,"Fog Nozzle 200 @ 75 4826","Fog Nozzle 200 @ 75 4863",null,null,null,"Fog Nozzle 175 @ 50 4863",null,null,null,"Stack Tips","15/16\"; 1/2\"",0.5,"Stack Tips 15/16\"; 1/2\"",null,null,null,"Solid Bore 1.5 in","7/8\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 2.5 in","1\"",null,"Solid Bore Yes 1.5 in 7/8\" No (Std)","Solid Bore Yes 1.5 in","Solid Bore","7/8\"","1445","1.5 in",0.875,"Yes","No (Std)","Solid Bore No 2.5 in",null,1,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore No 2.5 in 1-1/8\" Yes","0489",null,null,null,"7/8\"","7_8_",null,"Solid Bore","7/8\"","1445","1.5 in",0.875,"Yes","Solid Bore 1.5 in Yes 7/8\" 1445",null,"Solid Bore 1.5 in Yes 7/8\" 1445",null,null,null,null,null,null,null,"Solid Bore","7/8\"","1445","Solid Bore7/8\"1445",null,"Solid Bore7/8\"1445"]
[null,null,null,null,null,null,null,null,null,null,null,null,"1.5 in",null,null,null,"95-200",null,150,150,150,150,null,null,null,null,null,null,null,"30-150",75,"30-150 75",null,null,null,null,"4826",250,null,300,"100 (Std)",75,null,null,null,4826,300,300,null,null,null,"Solid Bore","15/16\"","1445","1.5 in",0.9375,"Fog Nozzle",350,"Fog Nozzle 350",null,null,150,50,"150 50",null,null,null,null,null,"Fog Tip",4824,200,"100 (Std)","Fog Tip 200 @ 100 (Std)",null,null,null,"Fog Nozzle 210 @ 50",4826,null,null,"Fog Nozzle 210 @ 50 4826",null,null,null,null,"Fog Nozzle 175 @ 75 4863",null,null,null,"Stack Tips","1-1/16\"; 15/16\"",0.9375,"Stack Tips 1-1/16\"; 15/16\"",null,null,null,"Solid Bore 1.5 in","15/16\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 2.5 in","1-1/8\"",null,"Solid Bore Yes 1.5 in 15/16\" No (Std)","Solid Bore Yes 1.5 in","Solid Bore","15/16\"","1445","1.5 in",0.9375,"Yes","No (Std)","Solid Bore No 2.5 in",null,1.125,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore No 2.5 in 1-3/8\" Yes","0489",null,null,null,"15/16\"","15_16_",null,"Solid Bore","15/16\"","1445","1.5 in",0.9375,"Yes","Solid Bore 1.5 in Yes 15/16\" 1445",null,"Solid Bore 1.5 in Yes 15/16\" 1445",null,null,null,null,null,null,null,"Solid Bore","15/16\"","1445","Solid Bore15/16\"1445",null,"Solid Bore15/16\"1445"]
[null,null,null,null,null,null,null,null,null,null,null,null,"1.5 in",null,null,null,"125-250",null,161,161,161,161,null,null,null,null,null,null,null,"30-150","87 (CE)","30-150 87 (CE)",null,null,null,null,"4826",300,null,350,"100 (Std)",null,null,null,null,4826,350,null,null,null,null,"Solid Bore","1\"","1445","1.5 in",1,"Fog Tip",95,"Fog Tip 95",null,null,150,"87 (CE)","150 87 (CE)",null,null,null,null,null,"Fog Tip",4824,250,"100 (Std)","Fog Tip 250 @ 100 (Std)",null,null,null,"Fog Nozzle 225 @ 100",4863,null,null,"Fog Nozzle 225 @ 100 4863",null,null,null,null,"Fog Nozzle 185 @ 50 4863",null,null,null,"Stack Tips","1-1/4\"; 1-1/8\"; 1\"",1,"Stack Tips 1-1/4\"; 1-1/8\"; 1\"",null,null,null,"Solid Bore 1.5 in","1\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 2.5 in","1-1/4\"",null,"Solid Bore Yes 1.5 in 1\" No (Std)","Solid Bore Yes 1.5 in","Solid Bore","1\"","1445","1.5 in",1,"Yes","No (Std)","Solid Bore No 2.5 in",null,1.25,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore No 2.5 in 15/16\" Yes","0489",null,null,null,"1\"","1_",null,"Solid Bore","1\"","1445","1.5 in",1,"Yes","Solid Bore 1.5 in Yes 1\" 1445",null,"Solid Bore 1.5 in Yes 1\" 1445",null,null,null,null,null,null,null,"Solid Bore","1\"","1445","Solid Bore1\"1445",null,"Solid Bore1\"1445"]
[null,null,null,null,null,null,null,null,null,null,null,null,"1.5 IN",null,null,null,null,null,175,175,175,175,null,null,null,null,null,null,null,"30-200","100 (Std)","30-200 100 (Std)",null,null,null,null,"4826",350,null,null,null,null,null,null,null,4863,95,null,null,null,null,"Solid Bore","1-1/16\"","1445","1.5 in",1.0625,"Fog Tip",125,"Fog Tip 125",null,null,161,50,"161 50",null,null,null,null,null,"Fog Tip",4824,300,"100 (Std)","Fog Tip 300 @ 100 (Std)",null,null,null,"Fog Nozzle 25 @ 100",4802,null,null,"Fog Nozzle 25 @ 100 4802",null,null,null,null,"Fog Nozzle 200 @ 100 4826",null,null,null,"Stack Tips","1-1/2\"; 1-1/4\"; 1\"",1,"Stack Tips 1-1/2\"; 1-1/4\"; 1\"",null,null,null,"Solid Bore 1.5 in","1-1/16\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 2.5 in","1-3/8\"",null,"Solid Bore Yes 1.5 in 1-1/16\" No (Std)","Solid Bore Yes 1.5 in","Solid Bore","1-1/16\"","1445","1.5 in",1.0625,"Yes","No (Std)","Solid Bore No 2.5 in",null,1.375,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore No 2.5 in 7/8\" Yes","0489",null,null,null,"1-1/16\"","1_1_16_",null,"Solid Bore","1-1/16\"","1445","1.5 in",1.0625,"Yes","Solid Bore 1.5 in Yes 1-1/16\" 1445",null,"Solid Bore 1.5 in Yes 1-1/16\" 1445",null,null,null,null,null,null,null,"Solid Bore","1-1/16\"","1445","Solid Bore1-1/16\"1445",null,"Solid Bore1-1/16\"1445"]
[null,null,null,null,null,null,null,null,null,null,null,null,"1.5 in",null,null,null,null,null,200,200,200,200,null,null,null,null,null,null,null,"30-200",75,"30-200 75",null,null,null,null,"4863",95,null,null,null,null,null,null,null,4863,125,125,125,null,null,"Solid Bore","1-1/8\"","1445","1.5 in",1.125,"Fog Tip",150,"Fog Tip 150",null,null,175,"100 (Std)","175 100 (Std)",null,null,null,null,null,"Fog Tip",4824,350,"100 (Std)","Fog Tip 350 @ 100 (Std)",null,null,null,"Fog Nozzle 250 @ 100",4826,null,null,"Fog Nozzle 250 @ 100 4826",null,null,null,null,"Fog Nozzle 200 @ 100 4863",null,null,null,"Stack Tips","1-3/8\"; 1-1/4\"; 1\"",1,"Stack Tips 1-3/8\"; 1-1/4\"; 1\"",null,null,null,"Solid Bore 1.5 in","1-1/8\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 2.5 in","1-1/16\"",null,"Solid Bore Yes 1.5 in 1-1/8\" No (Std)","Solid Bore Yes 1.5 in","Solid Bore","1-1/8\"","1445","1.5 in",1.125,"Yes","No (Std)","Solid Bore Yes 1.5 in",null,0.5,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 1.5 in 1\" No (Std)","1445",null,null,null,"1-1/8\"","1_1_8_",null,"Solid Bore","1-1/8\"","1445","1.5 in",1.125,"Yes","Solid Bore 1.5 in Yes 1-1/8\" 1445",null,"Solid Bore 1.5 in Yes 1-1/8\" 1445",null,null,null,null,null,null,null,"Solid Bore","1-1/8\"","1445","Solid Bore1-1/8\"1445",null,"Solid Bore1-1/8\"1445"]
[null,{"$f":"IF(OR(C21=\"False\",D21=\"False\",E21=\"False\",H21=\"False\",I21=\"False\",F21=\"False\"),\"Error\",\"Okay\")","v":"Okay"},{"$f":"IFERROR(VLOOKUP(CONCATENATE(B10,C10),C26:C42,1,FALSE),\"False\")","v":"UltraJet Fog Nozzle1.5 in"},null,{"$f":"IF(E8=\"\",\"Okay\",IFERROR(VLOOKUP(CONCATENATE(E10,I10),E26:E82,1,FALSE),\"False\"))","v":"7/8\"1820"},{"$f":"IFERROR(VLOOKUP(CONCATENATE(C10,F10),F26:F66,1,FALSE),\"false\")","v":"1.5 inNH"},null,null,{"$f":"IFERROR(VLOOKUP(CONCATENATE(B10,E10,IF(B10=\"saberjet fog nozzle\",D10,\"\")),I25:I87,1,FALSE),\"False\")","v":"UltraJet Fog Nozzle7/8\""},null,null,null,"1.5 IN",null,null,null,null,null,210,210,210,210,null,null,null,null,null,null,null,"95-200","100 (Std)","95-200 100 (Std)",null,null,null,null,"4863",125,null,null,null,null,null,null,null,4863,150,150,150,null,null,"Solid Bore","1-3/16\"","1445","1.5 in",1.1875,"Fog Tip",161,"Fog Tip 161",null,null,175,75,"175 75",null,null,null,null,null,"Fog Tip",4824,200,75,"Fog Tip 200 @ 75",null,null,null,"Fog Nozzle 250 @ 50",4826,null,null,"Fog Nozzle 250 @ 50 4826",null,null,null,null,"Fog Nozzle 200 @ 75 4826",null,null,null,null,null,null,null,null,null,null,"Solid Bore 1.5 in","1-3/16\"","1.5 in","Solid Bore 1.5 in",null,"Solid Bore 2.5 in","1-3/16\"",null,"Solid Bore Yes 1.5 in 1-3/16\" No (Std)","Solid Bore Yes 1.5 in","Solid Bore","1-3/16\"","1445","1.5 in",1.1875,"Yes","No (Std)","Solid Bore Yes 1.5 in",null,0.875,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 1.5 in 1/2\" No (Std)","1447",null,null,null,"1-3/16\"","1_3_16_",null,"Solid Bore","1-3/16\"","1445","1.5 in",1.1875,"Yes","Solid Bore 1.5 in Yes 1-3/16\" 1445",null,"Solid Bore 1.5 in Yes 1-3/16\" 1445",null,null,null,null,null,null,null,"Solid Bore","1-3/16\"","1445","Solid Bore1-3/16\"1445",null,"Solid Bore1-3/16\"1445"]
[null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(B10,\" \",C10,\" \",D10,\" \",E10,\" \",I10)","v":"UltraJet Fog Nozzle 1.5 in 95 @ 100 7/8\" 1820"},null,null,null,"2 IN","STORZ",null,null,null,null,225,225,225,225,null,null,null,null,null,null,null,"95-200",75,"95-200 75",null,null,null,null,"4863",150,null,null,null,null,null,null,null,4863,175,175,175,null,null,"Solid Bore","1-1/4\"","1445","1.5 in",1.25,"Fog Tip",175,"Fog Tip 175",null,null,175,50,"175 50",null,null,null,null,null,"Fog Tip",4824,250,75,"Fog Tip 250 @ 75",null,null,null,"Fog Nozzle 250 @ 75",4826,null,null,{"$f":"CONCATENATE($BZ22,\" \",CA22)","v":"Fog Nozzle 250 @ 75 4826"},null,null,null,null,"Fog Nozzle 200 @ 75 4863",null,null,null,null,null,null,null,null,null,null,"Solid Bore 1.5 in","1-1/4\"","1.5 in","Solid Bore 1.5 in",null,"Stack Tips 1.5 in","1-1/8\"; 1/2\"",null,"Solid Bore Yes 1.5 in 1-1/4\" No (Std)","Solid Bore Yes 1.5 in","Solid Bore","1-1/4\"","1445","1.5 in",1.25,"Yes","No (Std)","Solid Bore Yes 1.5 in",null,0.9375,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 1.5 in 1\" Yes","1445",null,null,null,"1-1/4\"","1_1_4_",null,"Solid Bore","1-1/4\"","1445","1.5 in",1.25,"Yes","Solid Bore 1.5 in Yes 1-1/4\" 1445",null,"Solid Bore 1.5 in Yes 1-1/4\" 1445",null,null,null,null,null,null,null,"Solid Bore","1-1/4\"","1445","Solid Bore1-1/4\"1445",null,"Solid Bore1-1/4\"1445"]
[null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(SUBSTITUTE(B10,\" \",\"_\"),\"_\",D10,\"_\",SUBSTITUTE(C10,\" \",\"_\"),\"_\",VLOOKUP(E10,ED:EE,2,FALSE),\"_\",IF(D10=\"no\",\"Yes\",IF(H10=\"yes\",\"Yes\",\"No__Std\")))","v":"UltraJet_Fog_Nozzle_95 @ 100_1.5_in_7_8__No__Std"},null,null,null,"2.5 IN","NH",null,null,null,null,250,250,250,250,null,null,null,null,null,null,null,"12-53","87 (CE)","12-53 87 (CE)",null,null,null,null,"4863",161,null,null,null,null,null,null,null,4863,200,200,null,null,null,"Solid Bore","1-3/8\"","1445","1.5 in",1.375,"Fog Tip",200,"Fog Tip 200",null,null,185,50,"185 50",null,null,null,null,null,"Fog Tip",4824,300,75,"Fog Tip 300 @ 75",null,null,null,"Fog Nozzle 265 @ 50",4826,null,null,{"$f":"CONCATENATE($BZ23,\" \",CA23)","v":"Fog Nozzle 265 @ 50 4826"},null,null,null,null,"Fog Nozzle 210 @ 50 4826",null,null,null,null,null,null,null,null,null,null,"Solid Bore 1.5 in","1-3/8\"","1.5 in","Solid Bore 1.5 in",null,"Stack Tips 1.5 in","15-16\"; 1/2\"",null,"Solid Bore Yes 1.5 in 1-3/8\" No (Std)","Solid Bore Yes 1.5 in","Solid Bore","1-3/8\"","1445","1.5 in",1.375,"Yes","No (Std)","Solid Bore Yes 1.5 in",null,1,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 1.5 in 1-1/16\" Yes","1445",null,null,null,"1-3/8\"","1_3_8_",null,"Solid Bore","1-3/8\"","1445","1.5 in",1.375,"Yes","Solid Bore 1.5 in Yes 1-3/8\" 1445",null,"Solid Bore 1.5 in Yes 1-3/8\" 1445",null,null,null,null,null,null,null,"Solid Bore","1-3/8\"","1445","Solid Bore1-3/8\"1445",null,"Solid Bore1-3/8\"1445"]
[null,null,null,null,null,null,null,null,"Solid_Bore_Yes_1.5_in_1__No__Std",null,null,null,"2.5 IN","NPSH",null,null,null,null,300,300,300,300,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4863",175,null,null,null,null,null,null,null,4863,null,null,161,null,null,"Solid Bore","1/2\"","1447","1.5 in",0.5,"Fog Tip",210,"Fog Tip 210",null,null,200,"100 (Std)","200 100 (Std)",null,null,null,null,null,"Fog Tip",4824,210,50,"Fog Tip 210 @ 50",null,null,null,"Fog Nozzle 300 @ 100",4826,null,null,{"$f":"CONCATENATE($BZ24,\" \",CA24)","v":"Fog Nozzle 300 @ 100 4826"},null,null,null,null,"Fog Nozzle 225 @ 100 4863",null,null,null,null,null,null,null,null,null,null,"Solid Bore 1.5 in","1/2\"","1.5 in","Solid Bore 1.5 in",null,"Stack Tips 1.5 in","1-1/16\"; 15/16\"",null,"Solid Bore Yes 1.5 in 1/2\" No (Std)","Solid Bore Yes 1.5 in","Solid Bore","1/2\"","1447","1.5 in",0.5,"Yes","No (Std)","Solid Bore Yes 1.5 in",null,1.0625,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 1.5 in 1-1/4\" Yes","1445",null,null,null,"1/2\"","1_2_",null,"Solid Bore","1/2\"","1447","1.5 in",0.5,"Yes","Solid Bore 1.5 in Yes 1/2\" 1447",null,"Solid Bore 1.5 in Yes 1/2\" 1447",null,null,null,null,null,null,null,"Solid Bore","1/2\"","1447","Solid Bore1/2\"1447",null,"Solid Bore1/2\"1447"]
[null,null,null,null,null,null,null,null,"SaberJet Fog Nozzle1/2\"95 @ 100",null,null,null,"2.5 IN","FDNY",null,null,null,null,350,350,350,350,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4863",185,null,null,null,null,null,null,null,4863,null,null,185,null,null,"Solid Bore","7/8\"","1499","1.5 in",0.875,"Fog Tip",225,"Fog Tip 225",null,null,200,75,"200 75",null,null,null,null,null,"Fog Tip",4824,265,50,"Fog Tip 265 @ 50",null,null,null,"Fog Nozzle 300 @ 75",4826,null,null,"Fog Nozzle 300 @ 75 4826",null,null,null,null,"Fog Nozzle 25 @ 100 4802",null,null,null,null,null,null,null,null,null,null,"Solid Bore 1.5 in","7/8\"","1.5 in","Solid Bore 1.5 in",null,"Stack Tips 1.5 in","1-1/4\"; 1-1/8\"; 1\"",null,"Solid Bore No 1.5 in 7/8\" Yes","Solid Bore No 1.5 in","Solid Bore","7/8\"","1499","1.5 in",0.875,"No","Yes","Solid Bore Yes 1.5 in",null,1.125,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 1.5 in 1-1/8\" Yes","1445",null,null,null,"7/8\"","7_8_",null,"Solid Bore","7/8\"","1499","1.5 in",0.875,"No","Solid Bore 1.5 in No 7/8\" 1499",null,"Solid Bore 1.5 in No 7/8\" 1499",null,null,null,null,null,null,null,"Solid Bore","7/8\"","1499","Solid Bore7/8\"1499",null,"Solid Bore7/8\"1499"]
[null,null,"SaberJet Fog Nozzle1.5 in",null,"1/2\"1520","1.5 inNH",null,null,"SaberJet Fog Nozzle5/8\"95 @ 100",null,null,null,"2.5 IN","NYCORP",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4863",200,null,null,null,null,null,null,null,4866,95,null,null,null,null,"Solid Bore","15/16\"","1499","1.5 in",0.9375,"Fog Tip",250,"Fog Tip 250",null,null,210,50,"210 50",null,null,null,null,null,"Fog Tip",4824,250,50,"Fog Tip 250 @ 50",null,null,null,"Fog Nozzle 350 @ 100",4826,null,null,"Fog Nozzle 350 @ 100 4826",null,null,null,null,"Fog Nozzle 250 @ 100 4826",null,null,null,null,null,null,null,null,null,null,"Solid Bore 1.5 in","15/16\"","1.5 in","Solid Bore 1.5 in",null,"Stack Tips 1.5 in","15/16\"; 1/2\"",null,"Solid Bore No 1.5 in 15/16\" Yes","Solid Bore No 1.5 in","Solid Bore","15/16\"","1499","1.5 in",0.9375,"No","Yes","Solid Bore Yes 1.5 in",null,1.1875,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 1.5 in 1-3/16\" Yes","1445",null,null,null,"15/16\"","15_16_",null,"Solid Bore","15/16\"","1499","1.5 in",0.9375,"No","Solid Bore 1.5 in No 15/16\" 1499",null,"Solid Bore 1.5 in No 15/16\" 1499",null,null,null,null,null,null,null,"Solid Bore","15/16\"","1499","Solid Bore15/16\"1499",null,"Solid Bore15/16\"1499"]
[null,null,"SaberJet Fog Nozzle2 in",null,"5/8\"1520","1.5 inNPSH",{"$f":"VLOOKUP(C13,DataSource!AH:AJ,2,FALSE)","v":"18204002"},{"$f":"VLOOKUP(C13,DataSource!AH:AJ,3,FALSE)","v":"ULTRAJET 1.5NH 7/8 TIP"},"SaberJet Fog Nozzle3/4\"135 @ 100",null,null,null,"2.5 IN","PITT6",null,null,null,null,"NH","NPSH","FDNY","NYCORP","PCT","Custom",null,null,null,null,null,null,null,null,null,null,null,null,"4863",225,null,null,null,null,null,null,null,4866,125,125,125,null,null,"Solid Bore","1\"","1499","1.5 in",1,"Fog Tip",265,"Fog Tip 265",null,null,225,"100 (Std)","225 100 (Std)",null,null,null,null,null,"Fog Nozzle",4826,200,"100 (Std)","Fog Nozzle 200 @ 100 (Std)",null,null,null,"Fog Nozzle 40 @ 100",4802,null,null,"Fog Nozzle 40 @ 100 4802",null,null,null,null,"Fog Nozzle 250 @ 50 4826",null,null,null,null,null,null,null,null,null,null,"Solid Bore 1.5 in","1\"","1.5 in","Solid Bore 1.5 in",null,"Stack Tips 2.5 in","1-1/8\"; 1/2\"",null,"Solid Bore No 1.5 in 1\" Yes","Solid Bore No 1.5 in","Solid Bore","1\"","1499","1.5 in",1,"No","Yes","Solid Bore Yes 1.5 in",null,1.25,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 1.5 in 1-3/8\" Yes","1445",null,null,null,"1\"","1_",null,"Solid Bore","1\"","1499","1.5 in",1,"No","Solid Bore 1.5 in No 1\" 1499",null,"Solid Bore 1.5 in No 1\" 1499",null,null,null,null,null,null,null,"Solid Bore","1\"","1499","Solid Bore1\"1499",null,"Solid Bore1\"1499"]
[null,null,"SaberJet Fog Nozzle2.5 in",null,"3/4\"1523","1.5 inFDNY",null,null,"SaberJet Fog Nozzle7/8\"135 @ 100",null,null,null,"2.5 IN","BAT",null,null,null,"SBTHREAD1.5 in",{"$f":"IF($B10=\"Solid Bore\",IF(OR(TRIM($I10)=\"0416\",$D10=\"yes\"),S27,\"\"),S27)","v":"NH"},"NPSH","FDNY","NYCORP","PCT","Custom",null,null,null,null,null,null,null,null,null,null,null,null,"4866",95,null,null,null,null,null,null,null,4866,150,150,150,null,null,"Solid Bore","1-1/16\"","1499","1.5 in",1.0625,"Fog Tip",300,"Fog Tip 300",null,null,250,"100 (Std)","250 100 (Std)",null,null,null,null,null,"Fog Nozzle",4826,250,"100 (Std)","Fog Nozzle 250 @ 100 (Std)",null,null,null,"Fog Nozzle 60 @ 100",4116,null,null,"Fog Nozzle 60 @ 100 4116",null,null,null,null,"Fog Nozzle 250 @ 75 4826",null,null,null,null,null,null,null,null,null,null,"Solid Bore 1.5 in","1-1/16\"","1.5 in","Solid Bore 1.5 in",null,"Stack Tips 2.5 in","1-1/4\"; 1-1/8\"; 1\"",null,"Solid Bore No 1.5 in 1-1/16\" Yes","Solid Bore No 1.5 in","Solid Bore","1-1/16\"","1499","1.5 in",1.0625,"No","Yes","Solid Bore Yes 1.5 in",null,1.375,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 1.5 in 15/16\" Yes","1445",null,null,null,"1-1/16\"","1_1_16_",null,"Solid Bore","1-1/16\"","1499","1.5 in",1.0625,"No","Solid Bore 1.5 in No 1-1/16\" 1499",null,"Solid Bore 1.5 in No 1-1/16\" 1499",null,null,null,null,null,null,null,"Solid Bore","1-1/16\"","1499","Solid Bore1-1/16\"1499",null,"Solid Bore1-1/16\"1499"]
[null,null,"SaberJet Fog Nozzle3 in",null,"7/8\"1523","1.5 inNYCORP",null,null,"SaberJet Fog Nozzle15/16\"135 @ 100",null,null,null,"2.5 IN","CSA",null,null,null,"SBTHREAD1 in","NH","NPSH","Custom",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4866",125,null,null,null,null,null,null,null,4866,175,175,175,null,null,"Solid Bore","1-1/8\"","1499","1.5 in",1.125,"Fog Tip",350,"Fog Tip 350",null,null,250,75,"250 75",null,null,null,null,null,"Fog Nozzle",4826,300,"100 (Std)","Fog Nozzle 300 @ 100 (Std)",null,null,null,"Fog Nozzle 60 @ 75",4116,null,null,"Fog Nozzle 60 @ 75 4116",null,null,null,null,"Fog Nozzle 265 @ 50 4826",null,null,null,null,null,null,null,null,null,null,"Solid Bore 1.5 in","1-1/8\"","1.5 in","Solid Bore 1.5 in",null,"Stack Tips 2.5 in","1-1/2\"; 1-1/4\"; 1\"",null,"Solid Bore No 1.5 in 1-1/8\" Yes","Solid Bore No 1.5 in","Solid Bore","1-1/8\"","1499","1.5 in",1.125,"No","Yes","Solid Bore Yes 2.5 in",null,0.875,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 1.5 in 7/8\" Yes","1445",null,null,null,"1-1/8\"","1_1_8_",null,"Solid Bore","1-1/8\"","1499","1.5 in",1.125,"No","Solid Bore 1.5 in No 1-1/8\" 1499",null,"Solid Bore 1.5 in No 1-1/8\" 1499",null,null,null,null,null,null,null,"Solid Bore","1-1/8\"","1499","Solid Bore1-1/8\"1499",null,"Solid Bore1-1/8\"1499"]
[null,null,"UltraJet Fog Nozzle1.5 in",null,"15/16\"1523","1.5 inPCT",null,null,"SaberJet Fog Nozzle1\"135 @ 100",null,null,null,"2.5 IN","QST",null,null,null,"SBTHREAD2.5 in","NH","NPSH","FDNY","NYCORP","PITT6","BAT","CSA","QST","Custom",null,null,null,null,null,null,null,null,null,"4866",150,null,null,null,null,null,null,null,4866,200,200,null,null,null,"Solid Bore","1-3/16\"","1499","1.5 in",1.1875,null,null,null,null,null,250,50,"250 50",null,null,null,null,null,"Fog Nozzle",4826,350,"100 (Std)","Fog Nozzle 350 @ 100 (Std)",null,null,null,"Fog Nozzle 60 @ 87",4116,null,null,"Fog Nozzle 60 @ 87 4116",null,null,null,null,"Fog Nozzle 300 @ 100 4826",null,null,null,null,null,null,null,null,null,null,"Solid Bore 1.5 in","1-3/16\"","1.5 in","Solid Bore 1.5 in",null,"Stack Tips 2.5 in","1-3/8\"; 1-1/4\"; 1\"",null,"Solid Bore No 1.5 in 1-3/16\" Yes","Solid Bore No 1.5 in","Solid Bore","1-3/16\"","1499","1.5 in",1.1875,"No","Yes","Solid Bore Yes 2.5 in",null,0.9375,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 2.5 in 1\" Yes","1446",null,null,null,"1-3/16\"","1_3_16_",null,"Solid Bore","1-3/16\"","1499","1.5 in",1.1875,"No","Solid Bore 1.5 in No 1-3/16\" 1499",null,"Solid Bore 1.5 in No 1-3/16\" 1499",null,null,null,null,null,null,null,"Solid Bore","1-3/16\"","1499","Solid Bore1-3/16\"1499",null,"Solid Bore1-3/16\"1499"]
[null,null,"UltraJet Fog Nozzle2 in",null,"1\"1523","1.5 inStorz",null,null,"SaberJet Fog Nozzle1-1/8\"135 @ 100",null,null,null,"2.5 IN","BIM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4866",161,null,null,null,null,null,null,null,4866,null,null,161,null,null,"Solid Bore","1-1/4\"","1499","1.5 in",1.25,null,null,null,null,null,265,50,"265 50",null,null,null,null,null,"Fog Nozzle",4826,200,75,"Fog Nozzle 200 @ 75",null,null,null,"Fog Nozzle 95 @ 100",4116,4863,null,"Fog Nozzle 95 @ 100 4116",{"$f":"CONCATENATE($BZ31,\" \",CB31)","v":"Fog Nozzle 95 @ 100 4863"},null,null,null,"Fog Nozzle 300 @ 75 4826",null,null,null,null,null,null,null,null,null,null,"Solid Bore 1.5 in","1-1/4\"","1.5 in","Solid Bore 1.5 in",null,null,null,null,"Solid Bore No 1.5 in 1-1/4\" Yes","Solid Bore No 1.5 in","Solid Bore","1-1/4\"","1499","1.5 in",1.25,"No","Yes","Solid Bore Yes 2.5 in",null,1,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 2.5 in 1-1/16\" Yes","1446",null,null,null,"1-1/4\"","1_1_4_",null,"Solid Bore","1-1/4\"","1499","1.5 in",1.25,"No","Solid Bore 1.5 in No 1-1/4\" 1499",null,"Solid Bore 1.5 in No 1-1/4\" 1499",null,null,null,null,null,null,null,"Solid Bore","1-1/4\"","1499","Solid Bore1-1/4\"1499",null,"Solid Bore1-1/4\"1499"]
[null,null,"UltraJet Fog Nozzle2.5 in",null,"1-1/8\"1528","1.5 inCustom",null,null,"UltraJet Fog Nozzle3/4\"",null,null,null,"2.5 IN","STORZ",null,null,"BLACK (Std)","THREAD1 IN","NH","NPSH","Storz","Custom",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4866",175,null,null,null,null,null,null,null,4866,null,null,185,null,null,"Solid Bore","1-3/8\"","1499","1.5 in",1.375,null,null,null,null,null,300,"100 (Std)","300 100 (Std)",null,null,null,null,null,"Fog Nozzle",4826,265,50,"Fog Nozzle 265 @ 50",null,null,null,"Fog Nozzle 95 @ 75",4116,null,null,"Fog Nozzle 95 @ 75 4116",null,null,null,null,"Fog Nozzle 350 @ 100 4826",null,null,null,null,null,null,null,null,null,null,"Solid Bore 1.5 in","1-3/8\"","1.5 in","Solid Bore 1.5 in",null,null,null,null,"Solid Bore No 1.5 in 1-3/8\" Yes","Solid Bore No 1.5 in","Solid Bore","1-3/8\"","1499","1.5 in",1.375,"No","Yes","Solid Bore Yes 2.5 in",null,1.0625,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 2.5 in 1-1/4\" Yes","1446",null,null,null,"1-3/8\"","1_3_8_",null,"Solid Bore","1-3/8\"","1499","1.5 in",1.375,"No","Solid Bore 1.5 in No 1-3/8\" 1499",null,"Solid Bore 1.5 in No 1-3/8\" 1499",null,null,null,null,null,null,null,"Solid Bore","1-3/8\"","1499","Solid Bore1-3/8\"1499",null,"Solid Bore1-3/8\"1499"]
[null,null,"UltraJet Fog Nozzle3 in",null,"3/4\"1820","2.5 inNH",null,null,"UltraJet Fog Nozzle7/8\"",null,null,null,"3 IN","STORZ",null,null,"ORANGE","THREAD1.5 in","NH","NPSH","FDNY","NYCORP","PCT","Storz","Custom",null,null,null,null,null,null,null,null,null,null,null,"4866",185,null,null,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore","7/8\"","0489","2.5 in",0.875,null,null,null,null,null,300,75,"300 75",null,null,null,null,null,"Fog Nozzle",4826,250,75,"Fog Nozzle 250 @ 75",null,null,null,"Fog Nozzle 95 @ 87",4116,null,null,"Fog Nozzle 95 @ 87 4116",null,null,null,null,"Fog Nozzle 40 @ 100 4802",null,null,null,null,null,null,null,null,null,null,"Solid Bore 2.5 in","7/8\"","2.5 in","Solid Bore 2.5 in",null,null,null,null,"Solid Bore No 2.5 in 7/8\" Yes","Solid Bore No 2.5 in","Solid Bore","7/8\"","0489","2.5 in",0.875,"No","Yes","Solid Bore Yes 2.5 in",null,1.125,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 2.5 in 1-1/8\" Yes","1446",null,null,null,"7/8\"","7_8_",null,"Solid Bore","7/8\"","0489","2.5 in",0.875,"No","Solid Bore 2.5 in No 7/8\" 0489",null,"Solid Bore 2.5 in No 7/8\" 0489",null,null,null,null,null,null,null,"Solid Bore","7/8\"","0489","Solid Bore7/8\"0489",null,"Solid Bore7/8\"0489"]
[null,null,null,null,"7/8\"1820","2.5 inNPSH",null,null,"UltraJet Fog Nozzle15/16\"",null,null,null,null,null,null,null,"YELLOW","THREAD2 IN","Storz",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"4866",200,null,null,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore","15/16\"","0489","2.5 in",0.9375,null,null,null,null,null,350,"100 (Std)","350 100 (Std)",null,null,null,null,null,"Fog Nozzle",4826,300,75,"Fog Nozzle 300 @ 75",null,null,null,"Fog Tip 125 @ 100",4866,null,null,"Fog Tip 125 @ 100 4866",null,null,null,null,"Fog Nozzle 60 @ 100 4116",null,null,null,null,null,null,null,null,null,null,"Solid Bore 2.5 in","15/16\"","2.5 in","Solid Bore 2.5 in",null,null,null,null,"Solid Bore No 2.5 in 15/16\" Yes","Solid Bore No 2.5 in","Solid Bore","15/16\"","0489","2.5 in",0.9375,"No","Yes","Solid Bore Yes 2.5 in",null,1.1875,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 2.5 in 1-3/16\" Yes","1446",null,null,null,"15/16\"","15_16_",null,"Solid Bore","15/16\"","0489","2.5 in",0.9375,"No","Solid Bore 2.5 in No 15/16\" 0489",null,"Solid Bore 2.5 in No 15/16\" 0489",null,null,null,null,null,null,null,"Solid Bore","15/16\"","0489","Solid Bore15/16\"0489",null,"Solid Bore15/16\"0489"]
[null,null,null,null,"15/16\"1820","2.5 INFDNY",null,null,"UltraJet Fog Nozzle1\"",null,null,null,null,null,null,null,"RED","THREAD2.5 IN","NH","NPSH","FDNY","NYCORP","PITT6","BAT","CSA","QST","BIM","Storz","Custom",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore","1\"","0489","2.5 in",1,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4826,210,50,"Fog Nozzle 210 @ 50",null,null,null,"Fog Tip 125 @ 75",4866,null,null,"Fog Tip 125 @ 75 4866",null,null,null,null,"Fog Nozzle 60 @ 75 4116",null,null,null,null,null,null,null,null,null,null,"Solid Bore 2.5 in","1\"","2.5 in","Solid Bore 2.5 in",null,null,null,null,"Solid Bore No 2.5 in 1\" Yes","Solid Bore No 2.5 in","Solid Bore","1\"","0489","2.5 in",1,"No","Yes","Solid Bore Yes 2.5 in",null,1.25,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 2.5 in 1-3/8\" Yes","1446",null,null,null,"1\"","1_",null,"Solid Bore","1\"","0489","2.5 in",1,"No","Solid Bore 2.5 in No 1\" 0489",null,"Solid Bore 2.5 in No 1\" 0489",null,null,null,null,null,null,null,"Solid Bore","1\"","0489","Solid Bore1\"0489",null,"Solid Bore1\"0489"]
[null,null,null,null,"1\"1820","2.5 INNYCORP",null,null,null,null,null,null,null,null,null,null,"BLUE","THREAD3 IN","Storz",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore","1.5 in",{"$f":"CONCATENATE(AU36,AV36)","v":"Solid Bore1.5 in"},null,null,"Solid Bore","1-1/8\"","0489","2.5 in",1.125,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4826,250,50,"Fog Nozzle 250 @ 50",null,null,null,"Fog Tip 150 @ 100",4866,null,null,"Fog Tip 150 @ 100 4866",null,null,null,null,"Fog Nozzle 60 @ 87 4116",null,null,null,null,null,null,null,null,null,null,"Solid Bore 2.5 in","1-1/8\"","2.5 in","Solid Bore 2.5 in",null,null,null,null,"Solid Bore No 2.5 in 1-1/8\" Yes","Solid Bore No 2.5 in","Solid Bore","1-1/8\"","0489","2.5 in",1.125,"No","Yes","Solid Bore Yes 2.5 in",null,1.375,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 2.5 in 15/16\" Yes","1446",null,null,null,"1-1/8\"","1_1_8_",null,"Solid Bore","1-1/8\"","0489","2.5 in",1.125,"No","Solid Bore 2.5 in No 1-1/8\" 0489",null,"Solid Bore 2.5 in No 1-1/8\" 0489",null,null,null,null,null,null,null,"Solid Bore","1-1/8\"","0489","Solid Bore1-1/8\"0489",null,"Solid Bore1-1/8\"0489"]
[null,null,null,null,null,"2.5 INPITT6",null,null,null,null,null,null,null,null,null,null,"GREEN",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore","2.5 in",{"$f":"CONCATENATE(AU37,AV37)","v":"Solid Bore2.5 in"},null,null,"Solid Bore","1-1/4\"","0489","2.5 in",1.25,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4863,95,"100 (Std)","Fog Nozzle 95 @ 100 (Std)",null,null,null,"Fog Tip 150 @ 50",4866,null,null,"Fog Tip 150 @ 50 4866",null,null,null,null,"Fog Nozzle 95 @ 100 4116",null,null,null,null,null,null,null,null,null,null,"Solid Bore 2.5 in","1-1/4\"","2.5 in","Solid Bore 2.5 in",null,null,null,null,"Solid Bore No 2.5 in 1-1/4\" Yes","Solid Bore No 2.5 in","Solid Bore","1-1/4\"","0489","2.5 in",1.25,"No","Yes","Stack Tips No 1.5 in",null,0.5,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 2.5 in 7/8\" Yes","1446",null,null,null,"1-1/4\"","1_1_4_",null,"Solid Bore","1-1/4\"","0489","2.5 in",1.25,"No","Solid Bore 2.5 in No 1-1/4\" 0489",null,"Solid Bore 2.5 in No 1-1/4\" 0489",null,null,null,null,null,null,null,"Solid Bore","1-1/4\"","0489","Solid Bore1-1/4\"0489",null,"Solid Bore1-1/4\"0489"]
[null,null,null,null,null,"2.5 INBAT",null,null,null,null,null,null,"1440","No",{"$f":"TRIM(M38)","v":"1440"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Style","List Price",null,null,null,null,"Stack Tips","1.5 in",{"$f":"CONCATENATE(AU38,AV38)","v":"Stack Tips1.5 in"},null,null,"Solid Bore","1-3/8\"","0489","2.5 in",1.375,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4863,125,"100 (Std)","Fog Nozzle 125 @ 100 (Std)",null,null,null,"Fog Tip 150 @ 75",4866,null,null,"Fog Tip 150 @ 75 4866",null,null,null,null,"Fog Nozzle 95 @ 100 4863",null,null,null,null,null,null,null,null,null,null,"Solid Bore 2.5 in","1-3/8\"","2.5 in","Solid Bore 2.5 in",null,null,null,null,"Solid Bore No 2.5 in 1-3/8\" Yes","Solid Bore No 2.5 in","Solid Bore","1-3/8\"","0489","2.5 in",1.375,"No","Yes","Stack Tips No 1.5 in",null,0.5,null,null,null,null,null,null,null,null,null,null,null,"Stack Tips Yes 1.5 in 15/16\"; 1/2\" Yes","1441",null,null,null,"1-3/8\"","1_3_8_",null,"Solid Bore","1-3/8\"","0489","2.5 in",1.375,"No","Solid Bore 2.5 in No 1-3/8\" 0489",null,"Solid Bore 2.5 in No 1-3/8\" 0489",null,null,null,null,null,null,null,"Solid Bore","1-3/8\"","0489","Solid Bore1-3/8\"0489",null,"Solid Bore1-3/8\"0489"]
[null,null,null,null,null,"2.5 INCSA",null,null,null,null,null,null,"1441","Yes",{"$f":"TRIM(M39)","v":"1441"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"0416",378,null,null,null,null,"Stack Tips","2.5 in",{"$f":"CONCATENATE(AU39,AV39)","v":"Stack Tips2.5 in"},null,null,"Solid Bore","7/8\"","1446","2.5 in",0.875,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4863,150,"100 (Std)","Fog Nozzle 150 @ 100 (Std)",null,null,null,"Fog Tip 161 @ 50",4866,null,null,"Fog Tip 161 @ 50 4866",null,null,null,null,"Fog Nozzle 95 @ 75 4116",null,null,null,null,null,null,null,null,null,null,"Solid Bore 2.5 in","7/8\"","2.5 in","Solid Bore 2.5 in",null,null,null,null,"Solid Bore Yes 2.5 in 7/8\" No (Std)","Solid Bore Yes 2.5 in","Solid Bore","7/8\"","1446","2.5 in",0.875,"Yes","No (Std)","Stack Tips No 1.5 in",null,0.9375,null,null,null,null,null,null,null,null,null,null,null,"Stack Tips Yes 2.5 in 1-1/8\"; 1/2\" Yes","1443",null,null,null,"7/8\"","7_8_",null,"Solid Bore","7/8\"","1446","2.5 in",0.875,"Yes","Solid Bore 2.5 in Yes 7/8\" 1446",null,"Solid Bore 2.5 in Yes 7/8\" 1446",null,null,null,null,null,null,null,"Solid Bore","7/8\"","1446","Solid Bore7/8\"1446",null,"Solid Bore7/8\"1446"]
[null,null,null,null,null,"2.5 INQST",null,null,null,null,null,null,"1442","No","1442",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"yes1.5 in","NH",{"$f":"CONCATENATE(AI40,AJ40)","v":"yes1.5 inNH"},null,null,null,"0439",284,null,null,null,null,null,null,null,null,null,"Solid Bore","15/16\"","1446","2.5 in",0.9375,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4863,175,"100 (Std)","Fog Nozzle 175 @ 100 (Std)",null,null,null,"Fog Tip 175 @ 100",4866,null,null,"Fog Tip 175 @ 100 4866",null,null,null,null,"Fog Nozzle 95 @ 87 4116",null,null,null,null,null,null,null,null,null,null,"Solid Bore 2.5 in","15/16\"","2.5 in","Solid Bore 2.5 in",null,null,null,null,"Solid Bore Yes 2.5 in 15/16\" No (Std)","Solid Bore Yes 2.5 in","Solid Bore","15/16\"","1446","2.5 in",0.9375,"Yes","No (Std)","Stack Tips No 1.5 in",null,1,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 1.5 in 1-1/16\" No (Std)","1445",null,null,null,"15/16\"","15_16_",null,"Solid Bore","15/16\"","1446","2.5 in",0.9375,"Yes","Solid Bore 2.5 in Yes 15/16\" 1446",null,"Solid Bore 2.5 in Yes 15/16\" 1446",null,null,null,null,null,null,null,"Solid Bore","15/16\"","1446","Solid Bore15/16\"1446",null,"Solid Bore15/16\"1446"]
[null,null,null,null,null,"2.5 INBIM",null,null,null,null,null,null,"1443","Yes","1443",null,null,"Style",null,null,{"$f":"IF(B10=\"fog tip\",\"N/A\",\"No (Std)\")","v":"No (Std)"},null,"yes1 IN","NH","NPSH","Storz","Custom",null,null,null,null,null,null,null,"yes1.5 in","NPSH",{"$f":"CONCATENATE(AI41,AJ41)","v":"yes1.5 inNPSH"},null,null,null,"0489",498,null,null,null,null,null,null,null,null,null,"Solid Bore","1\"","1446","2.5 in",1,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4863,200,"100 (Std)","Fog Nozzle 200 @ 100 (Std)",null,null,null,"Fog Tip 175 @ 50",4866,null,null,"Fog Tip 175 @ 50 4866",null,null,null,null,"Fog Tip 125 @ 100 4866",null,null,null,null,null,null,null,null,null,null,"Solid Bore 2.5 in","1\"","2.5 in","Solid Bore 2.5 in",null,null,null,null,"Solid Bore Yes 2.5 in 1\" No (Std)","Solid Bore Yes 2.5 in","Solid Bore","1\"","1446","2.5 in",1,"Yes","No (Std)","Stack Tips No 2.5 in",null,1,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 1.5 in 1-1/4\" No (Std)","1445",null,null,null,"1\"","1_",null,"Solid Bore","1\"","1446","2.5 in",1,"Yes","Solid Bore 2.5 in Yes 1\" 1446",null,"Solid Bore 2.5 in Yes 1\" 1446",null,null,null,null,null,null,null,"Solid Bore","1\"","1446","Solid Bore1\"1446",null,"Solid Bore1\"1446"]
[null,null,null,null,null,"2.5 INStorz",null,null,null,null,null,null,"1445","Yes","1445",null,"Fog Nozzle 5-40","1602",null,null,{"$f":"IF(B10=\"fog tip\",\"\",\"Yes\")","v":"Yes"},null,"yes1.5 in","NH","NPSH","FDNY","NYCORP","PCT","Storz","Custom",null,null,null,null,"yes1.5 in","FDNY","yes1.5 inFDNY",null,null,null,"1417",156,null,null,null,null,null,null,null,null,null,"Solid Bore","1-1/16\"","1446","2.5 in",1.0625,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4863,125,75,"Fog Nozzle 125 @ 75",null,null,null,"Fog Tip 175 @ 75",4866,null,null,"Fog Tip 175 @ 75 4866",null,null,null,null,"Fog Tip 125 @ 75 4866",null,null,null,null,null,null,null,null,null,null,"Solid Bore 2.5 in","1-1/16\"","2.5 in","Solid Bore 2.5 in",null,null,null,null,"Solid Bore Yes 2.5 in 1-1/16\" No (Std)","Solid Bore Yes 2.5 in","Solid Bore","1-1/16\"","1446","2.5 in",1.0625,"Yes","No (Std)","Stack Tips No 2.5 in",null,1,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 1.5 in 1-1/8\" No (Std)","1445",null,null,null,"1-1/16\"","1_1_16_",null,"Solid Bore","1-1/16\"","1446","2.5 in",1.0625,"Yes","Solid Bore 2.5 in Yes 1-1/16\" 1446",null,"Solid Bore 2.5 in Yes 1-1/16\" 1446",null,null,null,null,null,null,null,"Solid Bore","1-1/16\"","1446","Solid Bore1-1/16\"1446",null,"Solid Bore1-1/16\"1446"]
[null,null,null,null,null,"2.5 INCustom",null,null,null,null,null,null,"1446","Yes","1446",null,"Fog Nozzle 12-53","1602",null,null,null,null,"yes2.5 IN","NH","NPSH","FDNY","NYCORP","PITT6","BAT","CSA","QST","BIM","Storz","Custom","yes1.5 in","NYCORP","yes1.5 inNYCORP",null,null,null,"1420",500,null,null,null,null,null,null,null,null,null,"Solid Bore","1-1/8\"","1446","2.5 in",1.125,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4863,150,75,"Fog Nozzle 150 @ 75",null,null,null,"Fog Tip 185 @ 50",4866,null,null,"Fog Tip 185 @ 50 4866",null,null,null,null,"Fog Tip 150 @ 100 4866",null,null,null,null,null,null,null,null,null,null,"Solid Bore 2.5 in","1-1/8\"","2.5 in","Solid Bore 2.5 in",null,null,null,null,"Solid Bore Yes 2.5 in 1-1/8\" No (Std)","Solid Bore Yes 2.5 in","Solid Bore","1-1/8\"","1446","2.5 in",1.125,"Yes","No (Std)","Stack Tips No 2.5 in",null,1,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 1.5 in 1-3/16\" No (Std)","1445",null,null,null,"1-1/8\"","1_1_8_",null,"Solid Bore","1-1/8\"","1446","2.5 in",1.125,"Yes","Solid Bore 2.5 in Yes 1-1/8\" 1446",null,"Solid Bore 2.5 in Yes 1-1/8\" 1446",null,null,null,null,null,null,null,"Solid Bore","1-1/8\"","1446","Solid Bore1-1/8\"1446",null,"Solid Bore1-1/8\"1446"]
[null,null,null,null,null,"1.5 inNH",null,null,null,null,null,null,"1447","Yes","1447",null,"Fog Nozzle 30-150","1616",null,null,null,null,"no1 IN","NH","NPSH","Custom",null,null,null,null,null,null,null,null,"yes1.5 in","PCT","yes1.5 inPCT",null,null,null,"1440",828,null,null,null,null,null,null,null,null,null,"Solid Bore","1-3/16\"","1446","2.5 in",1.1875,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4863,175,75,"Fog Nozzle 175 @ 75",null,null,null,"Fog Tip 200 @ 100",4824,4866,null,"Fog Tip 200 @ 100 4824","Fog Tip 200 @ 100 4866",null,null,null,"Fog Tip 150 @ 50 4866",null,null,null,null,null,null,null,null,null,null,"Solid Bore 2.5 in","1-3/16\"","2.5 in","Solid Bore 2.5 in",null,null,null,null,"Solid Bore Yes 2.5 in 1-3/16\" No (Std)","Solid Bore Yes 2.5 in","Solid Bore","1-3/16\"","1446","2.5 in",1.1875,"Yes","No (Std)","Stack Tips Yes 1.5 in",null,0.5,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 1.5 in 1-3/8\" No (Std)","1445",null,null,null,"1-3/16\"","1_3_16_",null,"Solid Bore","1-3/16\"","1446","2.5 in",1.1875,"Yes","Solid Bore 2.5 in Yes 1-3/16\" 1446",null,"Solid Bore 2.5 in Yes 1-3/16\" 1446",null,null,null,null,null,null,null,"Solid Bore","1-3/16\"","1446","Solid Bore1-3/16\"1446",null,"Solid Bore1-3/16\"1446"]
[null,null,null,null,null,"2.5 INNPSH",null,null,null,null,null,null,"2393","No","2393",null,"Fog Nozzle 13-60","1702",null,null,null,null,"no1.5 in","NH","NPSH","FDNY","NYCORP","PCT","Custom",null,null,null,null,null,"yes1.5 in","Storz","yes1.5 inStorz",null,null,null,"1441",828,null,null,null,null,null,null,null,null,null,"Solid Bore","1-1/4\"","1446","2.5 in",1.25,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4863,200,75,"Fog Nozzle 200 @ 75",null,null,null,"Fog Tip 200 @ 75",4824,4866,null,"Fog Tip 200 @ 75 4824","Fog Tip 200 @ 75 4866",null,null,null,"Fog Tip 150 @ 75 4866",null,null,null,null,null,null,null,null,null,null,"Solid Bore 2.5 in","1-1/4\"","2.5 in","Solid Bore 2.5 in",null,null,null,null,"Solid Bore Yes 2.5 in 1-1/4\" No (Std)","Solid Bore Yes 2.5 in","Solid Bore","1-1/4\"","1446","2.5 in",1.25,"Yes","No (Std)","Stack Tips Yes 2.5 in",null,0.5,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 1.5 in 15/16\" No (Std)","1445",null,null,null,"1-1/4\"","1_1_4_",null,"Solid Bore","1-1/4\"","1446","2.5 in",1.25,"Yes","Solid Bore 2.5 in Yes 1-1/4\" 1446",null,"Solid Bore 2.5 in Yes 1-1/4\" 1446",null,null,null,null,null,null,null,"Solid Bore","1-1/4\"","1446","Solid Bore1-1/4\"1446",null,"Solid Bore1-1/4\"1446"]
[null,null,null,null,null,"2.5 INFDNY",null,null,null,null,null,null,null,null,null,null,"Fog Tip 13-60","1703",null,null,null,null,"no2.5 IN","NH","NPSH","FDNY","NYCORP","PITT6","BAT","CSA","QST","Custom",null,null,"yes1.5 in","Custom","yes1.5 inCustom",null,null,null,"1442",960,null,null,null,null,null,null,null,null,null,"Solid Bore","1-3/8\"","1446","2.5 in",1.375,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4863,150,50,"Fog Nozzle 150 @ 50",null,null,null,"Fog Tip 210 @ 50",4824,null,null,"Fog Tip 210 @ 50 4824",null,null,null,null,"Fog Tip 161 @ 50 4866",null,null,null,null,null,null,null,null,null,null,"Solid Bore 2.5 in","1-3/8\"","2.5 in","Solid Bore 2.5 in",null,null,null,null,"Solid Bore Yes 2.5 in 1-3/8\" No (Std)","Solid Bore Yes 2.5 in","Solid Bore","1-3/8\"","1446","2.5 in",1.375,"Yes","No (Std)","Stack Tips Yes 2.5 in",null,1,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 1.5 in 7/8\" No (Std)","1445",null,null,null,"1-3/8\"","1_3_8_",null,"Solid Bore","1-3/8\"","1446","2.5 in",1.375,"Yes","Solid Bore 2.5 in Yes 1-3/8\" 1446",null,"Solid Bore 2.5 in Yes 1-3/8\" 1446",null,null,null,null,null,null,null,"Solid Bore","1-3/8\"","1446","Solid Bore1-3/8\"1446",null,"Solid Bore1-3/8\"1446"]
[null,null,null,null,null,"2.5 INNYCORP",null,null,null,null,null,null,null,null,null,null,"Fog Nozzle 18-30","1704",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"yes2.5 IN","NH","yes2.5 INNH",null,null,null,"1443",960,null,null,null,null,null,null,null,null,null,"Stack Tips","1-1/8\"; 1/2\"","0439","1.5 in",0.5,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4863,161,50,"Fog Nozzle 161 @ 50",null,null,null,"Fog Tip 225 @ 100",4866,null,null,"Fog Tip 225 @ 100 4866",null,null,null,null,"Fog Tip 175 @ 100 4866",null,null,null,null,null,null,null,null,null,null,"Stack Tips 1.5 in","1-1/8\"; 1/2\"","1.5 in","Stack Tips 1.5 in",null,null,null,null,"Stack Tips No 1.5 in 1-1/8\"; 1/2\" Yes","Stack Tips No 1.5 in","Stack Tips","1-1/8\"; 1/2\"","0439","1.5 in",0.5,"No","Yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 2.5 in 1\" No (Std)","1446",null,null,null,"1-1/8\"; 1/2\"","1_1_8___1_2_",null,"Stack Tips","1-1/8\"; 1/2\"","0439","1.5 in",0.5,"No","Stack Tips 1.5 in No 1-1/8\"; 1/2\" 0439",null,"Stack Tips 1.5 in No 1-1/8\"; 1/2\" 0439",null,null,null,null,null,null,null,"Stack Tips","1-1/8\"; 1/2\"","0439","Stack Tips1-1/8\"; 1/2\"0439",null,"Stack Tips1-1/8\"; 1/2\"0439"]
[null,null,null,null,null,"2.5 INPCT",null,null,null,null,null,null,"1520",1626,null,null,"Fog Nozzle 13-30","1704",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"yes2.5 IN","NPSH","yes2.5 INNPSH",null,null,null,"1445",714,null,null,null,null,null,null,null,null,null,"Stack Tips","15-16\"; 1/2\"","0439","1.5 in",0.5,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4863,175,50,"Fog Nozzle 175 @ 50",null,null,null,"Fog Tip 250 @ 100",4824,null,null,"Fog Tip 250 @ 100 4824",null,null,null,null,"Fog Tip 175 @ 50 4866",null,null,null,null,null,null,null,null,null,null,"Stack Tips 1.5 in","15-16\"; 1/2\"","1.5 in","Stack Tips 1.5 in",null,null,null,null,"Stack Tips No 1.5 in 15-16\"; 1/2\" Yes","Stack Tips No 1.5 in","Stack Tips","15-16\"; 1/2\"","0439","1.5 in",0.5,"No","Yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 2.5 in 1-1/16\" No (Std)","1446",null,null,null,"15-16\"; 1/2\"","15_16___1_2_",null,"Stack Tips","15-16\"; 1/2\"","0439","1.5 in",0.5,"No","Stack Tips 1.5 in No 15-16\"; 1/2\" 0439",null,"Stack Tips 1.5 in No 15-16\"; 1/2\" 0439",null,null,null,null,null,null,null,"Stack Tips","15-16\"; 1/2\"","0439","Stack Tips15-16\"; 1/2\"0439",null,"Stack Tips15-16\"; 1/2\"0439"]
[null,null,null,null,null,"2.5 INCustom",null,null,null,null,null,null,"1523",1644,null,null,"Fog Tip 18-30","1711",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"yes2.5 IN","FDNY","yes2.5 INFDNY",null,null,null,"1446",846,null,null,null,null,null,null,null,null,null,"Stack Tips","1-1/16\"; 15/16\"","0439","1.5 in",0.9375,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4863,185,50,"Fog Nozzle 185 @ 50",null,null,null,"Fog Tip 250 @ 50",4824,null,null,"Fog Tip 250 @ 50 4824",null,null,null,null,"Fog Tip 175 @ 75 4866",null,null,null,null,null,null,null,null,null,null,"Stack Tips 1.5 in","1-1/16\"; 15/16\"","1.5 in","Stack Tips 1.5 in",null,null,null,null,"Stack Tips No 1.5 in 1-1/16\"; 15/16\" Yes","Stack Tips No 1.5 in","Stack Tips","1-1/16\"; 15/16\"","0439","1.5 in",0.9375,"No","Yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 2.5 in 1-1/4\" No (Std)","1446",null,null,null,"1-1/16\"; 15/16\"","1_1_16___15_16_",null,"Stack Tips","1-1/16\"; 15/16\"","0439","1.5 in",0.9375,"No","Stack Tips 1.5 in No 1-1/16\"; 15/16\" 0439",null,"Stack Tips 1.5 in No 1-1/16\"; 15/16\" 0439",null,null,null,null,null,null,null,"Stack Tips","1-1/16\"; 15/16\"","0439","Stack Tips1-1/16\"; 15/16\"0439",null,"Stack Tips1-1/16\"; 15/16\"0439"]
[null,null,null,null,null,"2.5 INNH",null,null,null,null,null,null,"1528",1734,null,null,"Fog Tip 13-30","1711",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"yes2.5 IN","NYCORP","yes2.5 INNYCORP",null,null,null,"1447",{"$f":"156+544","v":700},null,null,null,null,null,null,null,null,null,"Stack Tips","1-1/4\"; 1-1/8\"; 1\"","1420","1.5 in",1,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Nozzle",4863,225,"100 (Std)","Fog Nozzle 225 @ 100 (Std)",null,null,null,"Fog Tip 250 @ 75",4824,null,null,"Fog Tip 250 @ 75 4824",null,null,null,null,"Fog Tip 185 @ 50 4866",null,null,null,null,null,null,null,null,null,null,"Stack Tips 1.5 in","1-1/4\"; 1-1/8\"; 1\"","1.5 in","Stack Tips 1.5 in",null,null,null,null,"Stack Tips No 1.5 in 1-1/4\"; 1-1/8\"; 1\" Yes","Stack Tips No 1.5 in","Stack Tips","1-1/4\"; 1-1/8\"; 1\"","1420","1.5 in",1,"No","Yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 2.5 in 1-1/8\" No (Std)","1446",null,null,null,"1-1/4\"; 1-1/8\"; 1\"","1_1_4___1_1_8___1_",null,"Stack Tips","1-1/4\"; 1-1/8\"; 1\"","1420","1.5 in",1,"No","Stack Tips 1.5 in No 1-1/4\"; 1-1/8\"; 1\" 1420",null,"Stack Tips 1.5 in No 1-1/4\"; 1-1/8\"; 1\" 1420",null,null,null,null,null,null,null,"Stack Tips","1-1/4\"; 1-1/8\"; 1\"","1420","Stack Tips1-1/4\"; 1-1/8\"; 1\"1420",null,"Stack Tips1-1/4\"; 1-1/8\"; 1\"1420"]
[null,null,null,null,null,"2.5 INPITT6",null,null,null,null,null,null,"1820",1578,null,null,"Fog Tip 30-125","1714",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"yes2.5 IN","PITT6","yes2.5 INPITT6",null,null,null,"1499",170,null,null,null,null,null,null,null,null,null,"Stack Tips","15/16\"; 1/2\"","1440","1.5 in",0.5,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip",4866,95,"100 (Std)","Fog Tip 95 @ 100 (Std)",null,null,null,"Fog Tip 265 @ 50",4824,null,null,"Fog Tip 265 @ 50 4824",null,null,null,null,"Fog Tip 200 @ 100 4824",null,null,null,null,null,null,null,null,null,null,"Stack Tips 1.5 in","15/16\"; 1/2\"","1.5 in","Stack Tips 1.5 in",null,null,null,null,"Stack Tips Yes 1.5 in 15/16\"; 1/2\" Yes","Stack Tips Yes 1.5 in","Stack Tips","15/16\"; 1/2\"","1440","1.5 in",0.5,"Yes","Yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 2.5 in 1-3/16\" No (Std)","1446",null,null,null,"15/16\"; 1/2\"","15_16___1_2_",null,"Stack Tips","15/16\"; 1/2\"","1440","1.5 in",0.5,"Yes","Stack Tips 1.5 in Yes 15/16\"; 1/2\" 1440",null,"Stack Tips 1.5 in Yes 15/16\"; 1/2\" 1440",null,null,null,null,null,null,null,"Stack Tips","15/16\"; 1/2\"","1440","Stack Tips15/16\"; 1/2\"1440",null,"Stack Tips15/16\"; 1/2\"1440"]
[null,null,null,null,null,"2.5 INBAT",null,null,null,null,null,null,"Storz",88,null,null,"Fog Nozzle 30-125","1720",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"yes2.5 IN","BAT","yes2.5 INBAT",null,null,null,"2393",1602,null,null,null,null,null,null,null,null,null,"Stack Tips","15/16\"; 1/2\"","1441","1.5 in",0.5,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip",4866,125,"100 (Std)","Fog Tip 125 @ 100 (Std)",null,null,null,"Fog Tip 300 @ 100",4824,null,null,"Fog Tip 300 @ 100 4824",null,null,null,null,"Fog Tip 200 @ 100 4866",null,null,null,null,null,null,null,null,null,null,"Stack Tips 1.5 in","15/16\"; 1/2\"","1.5 in","Stack Tips 1.5 in",null,null,null,null,"Stack Tips Yes 1.5 in 15/16\"; 1/2\" No (Std)","Stack Tips Yes 1.5 in","Stack Tips","15/16\"; 1/2\"","1441","1.5 in",0.5,"Yes","No (Std)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 2.5 in 1-3/8\" No (Std)","1446",null,null,null,"15/16\"; 1/2\"","15_16___1_2_",null,"Stack Tips","15/16\"; 1/2\"","1441","1.5 in",0.5,"Yes","Stack Tips 1.5 in Yes 15/16\"; 1/2\" 1441",null,"Stack Tips 1.5 in Yes 15/16\"; 1/2\" 1441",null,null,null,null,null,null,null,"Stack Tips","15/16\"; 1/2\"","1441","Stack Tips15/16\"; 1/2\"1441",null,"Stack Tips15/16\"; 1/2\"1441"]
[null,null,null,null,null,"2.5 INCSA",null,null,null,null,null,null,"ZT",340,null,null,"Fog Nozzle 95-200","1723",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"yes2.5 IN","CSA","yes2.5 INCSA",null,null,null,"2420",590,null,null,null,null,null,null,null,null,null,"Stack Tips","1-1/8\"; 1/2\"","1442","2.5 in",0.5,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip",4866,150,"100 (Std)","Fog Tip 150 @ 100 (Std)",null,null,null,"Fog Tip 300 @ 75",4824,null,null,"Fog Tip 300 @ 75 4824",null,null,null,null,"Fog Tip 200 @ 75 4824",null,null,null,null,null,null,null,null,null,null,"Stack Tips 2.5 in","1-1/8\"; 1/2\"","2.5 in","Stack Tips 2.5 in",null,null,null,null,"Stack Tips Yes 2.5 in 1-1/8\"; 1/2\" Yes","Stack Tips Yes 2.5 in","Stack Tips","1-1/8\"; 1/2\"","1442","2.5 in",0.5,"Yes","Yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 2.5 in 15/16\" No (Std)","1446",null,null,null,"1-1/8\"; 1/2\"","1_1_8___1_2_",null,"Stack Tips","1-1/8\"; 1/2\"","1442","2.5 in",0.5,"Yes","Stack Tips 2.5 in Yes 1-1/8\"; 1/2\" 1442",null,"Stack Tips 2.5 in Yes 1-1/8\"; 1/2\" 1442",null,null,null,null,null,null,null,"Stack Tips","1-1/8\"; 1/2\"","1442","Stack Tips1-1/8\"; 1/2\"1442",null,"Stack Tips1-1/8\"; 1/2\"1442"]
[null,null,null,null,null,"2.5 INQST",null,null,null,null,null,null,null,null,null,null,"Fog Nozzle 125-250","1733",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"yes2.5 IN","QST","yes2.5 INQST",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stack Tips","1-1/8\"; 1/2\"","1443","2.5 in",0.5,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip",4866,175,"100 (Std)","Fog Tip 175 @ 100 (Std)",null,null,null,"Fog Tip 350 @ 100",4824,null,null,"Fog Tip 350 @ 100 4824",null,null,null,null,"Fog Tip 200 @ 75 4866",null,null,null,null,null,null,null,null,null,null,"Stack Tips 2.5 in","1-1/8\"; 1/2\"","2.5 in","Stack Tips 2.5 in",null,null,null,null,"Stack Tips Yes 2.5 in 1-1/8\"; 1/2\" No (Std)","Stack Tips Yes 2.5 in","Stack Tips","1-1/8\"; 1/2\"","1443","2.5 in",0.5,"Yes","No (Std)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Solid Bore Yes 2.5 in 7/8\" No (Std)","1446",null,null,null,"1-1/8\"; 1/2\"","1_1_8___1_2_",null,"Stack Tips","1-1/8\"; 1/2\"","1443","2.5 in",0.5,"Yes","Stack Tips 2.5 in Yes 1-1/8\"; 1/2\" 1443",null,"Stack Tips 2.5 in Yes 1-1/8\"; 1/2\" 1443",null,null,null,null,null,null,null,"Stack Tips","1-1/8\"; 1/2\"","1443","Stack Tips1-1/8\"; 1/2\"1443",null,"Stack Tips1-1/8\"; 1/2\"1443"]
[null,null,null,null,null,"1.5 inNPSH",null,null,null,null,null,null,null,null,null,null,"Fog Tip 95-200","1737",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"yes2.5 IN","BIM","yes2.5 INBIM",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stack Tips","1-1/4\"; 1-1/8\"; 1\"","2393","2.5 in",1,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip",4866,200,"100 (Std)","Fog Tip 200 @ 100 (Std)",null,null,null,"Fog Tip 95 @ 100",4866,null,null,"Fog Tip 95 @ 100 4866",null,null,null,null,"Fog Tip 210 @ 50 4824",null,null,null,null,null,null,null,null,null,null,"Stack Tips 2.5 in","1-1/4\"; 1-1/8\"; 1\"","2.5 in","Stack Tips 2.5 in",null,null,null,null,"Stack Tips Yes 2.5 in 1-1/4\"; 1-1/8\"; 1\" No (Std)","Stack Tips Yes 2.5 in","Stack Tips","1-1/4\"; 1-1/8\"; 1\"","2393","2.5 in",1,"Yes","No (Std)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stack Tips No 1.5 in 1-1/16\"; 15/16\" Yes","0439",null,null,null,"1-1/4\"; 1-1/8\"; 1\"","1_1_4___1_1_8___1_",null,"Stack Tips","1-1/4\"; 1-1/8\"; 1\"","2393","2.5 in",1,"Yes","Stack Tips 2.5 in Yes 1-1/4\"; 1-1/8\"; 1\" 2393",null,"Stack Tips 2.5 in Yes 1-1/4\"; 1-1/8\"; 1\" 2393",null,null,null,null,null,null,null,"Stack Tips","1-1/4\"; 1-1/8\"; 1\"","2393","Stack Tips1-1/4\"; 1-1/8\"; 1\"2393",null,"Stack Tips1-1/4\"; 1-1/8\"; 1\"2393"]
[null,null,null,null,null,"1.5 inFDNY",null,null,null,null,null,null,null,null,null,null,"Fog Tip 125-250","1744",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"yes2.5 IN","Storz","yes2.5 INStorz",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stack Tips","1-1/2\"; 1-1/4\"; 1\"","2420","2.5 in",1,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip",4866,125,75,"Fog Tip 125 @ 75",null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip 225 @ 100 4866",null,null,null,null,null,null,null,null,null,null,"Stack Tips 2.5 in","1-1/2\"; 1-1/4\"; 1\"","2.5 in","Stack Tips 2.5 in",null,null,null,null,"Stack Tips No 2.5 in 1-1/2\"; 1-1/4\"; 1\" Yes","Stack Tips No 2.5 in","Stack Tips","1-1/2\"; 1-1/4\"; 1\"","2420","2.5 in",1,"No","Yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stack Tips No 1.5 in 1-1/4\"; 1-1/8\"; 1\" Yes","1420",null,null,null,"1-1/2\"; 1-1/4\"; 1\"","1_1_2___1_1_4___1_",null,"Stack Tips","1-1/2\"; 1-1/4\"; 1\"","2420","2.5 in",1,"No","Stack Tips 2.5 in No 1-1/2\"; 1-1/4\"; 1\" 2420",null,"Stack Tips 2.5 in No 1-1/2\"; 1-1/4\"; 1\" 2420",null,null,null,null,null,null,null,"Stack Tips","1-1/2\"; 1-1/4\"; 1\"","2420","Stack Tips1-1/2\"; 1-1/4\"; 1\"2420",null,"Stack Tips1-1/2\"; 1-1/4\"; 1\"2420"]
[null,null,null,null,null,"1.5 inNYCORP",null,null,null,null,null,null,null,null,null,null,"Fog Nozzle 30-200","1763",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"yes2.5 IN","Custom","yes2.5 INCustom",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stack Tips","1-1/4\"; 1-1/8\"; 1\"","2420","2.5 in",1,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip",4866,150,75,"Fog Tip 150 @ 75",null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip 250 @ 100 4824",null,null,null,null,null,null,null,null,null,null,"Stack Tips 2.5 in","1-1/4\"; 1-1/8\"; 1\"","2.5 in","Stack Tips 2.5 in",null,null,null,null,"Stack Tips No 2.5 in 1-1/4\"; 1-1/8\"; 1\" Yes","Stack Tips No 2.5 in","Stack Tips","1-1/4\"; 1-1/8\"; 1\"","2420","2.5 in",1,"No","Yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stack Tips No 1.5 in 1-1/8\"; 1/2\" Yes","0439",null,null,null,"1-1/4\"; 1-1/8\"; 1\"","1_1_4___1_1_8___1_",null,"Stack Tips","1-1/4\"; 1-1/8\"; 1\"","2420","2.5 in",1,"No","Stack Tips 2.5 in No 1-1/4\"; 1-1/8\"; 1\" 2420",null,"Stack Tips 2.5 in No 1-1/4\"; 1-1/8\"; 1\" 2420",null,null,null,null,null,null,null,"Stack Tips","1-1/4\"; 1-1/8\"; 1\"","2420","Stack Tips1-1/4\"; 1-1/8\"; 1\"2420",null,"Stack Tips1-1/4\"; 1-1/8\"; 1\"2420"]
[null,null,null,null,null,"1.5 inPCT",null,null,null,null,null,null,null,null,null,null,"Fog Tip 30-200","1766",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"no1.5 in","NH","no1.5 inNH",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stack Tips","1-3/8\"; 1-1/4\"; 1\"","2420","2.5 in",1,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip",4866,175,75,"Fog Tip 175 @ 75",null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip 250 @ 50 4824",null,null,null,null,null,null,null,null,null,null,"Stack Tips 2.5 in","1-3/8\"; 1-1/4\"; 1\"","2.5 in","Stack Tips 2.5 in",null,null,null,null,"Stack Tips No 2.5 in 1-3/8\"; 1-1/4\"; 1\" Yes","Stack Tips No 2.5 in","Stack Tips","1-3/8\"; 1-1/4\"; 1\"","2420","2.5 in",1,"No","Yes",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stack Tips No 1.5 in 15-16\"; 1/2\" Yes","0439",null,null,null,"1-3/8\"; 1-1/4\"; 1\"","1_3_8___1_1_4___1_",null,"Stack Tips","1-3/8\"; 1-1/4\"; 1\"","2420","2.5 in",1,"No","Stack Tips 2.5 in No 1-3/8\"; 1-1/4\"; 1\" 2420",null,"Stack Tips 2.5 in No 1-3/8\"; 1-1/4\"; 1\" 2420",null,null,null,null,null,null,null,"Stack Tips","1-3/8\"; 1-1/4\"; 1\"","2420","Stack Tips1-3/8\"; 1-1/4\"; 1\"2420",null,"Stack Tips1-3/8\"; 1-1/4\"; 1\"2420"]
[null,null,null,null,null,"1.5 inStorz",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"no2.5 IN","NPSH","no2.5 INNPSH",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip",4866,200,75,"Fog Tip 200 @ 75",null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip 250 @ 75 4824",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stack Tips No 2.5 in 1-1/2\"; 1-1/4\"; 1\" Yes","2420"]
[null,null,null,null,null,"1.5 inCustom",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"no2.5 IN","FDNY","no2.5 INFDNY",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip",4866,150,50,"Fog Tip 150 @ 50",null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip 265 @ 50 4824",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stack Tips No 2.5 in 1-1/4\"; 1-1/8\"; 1\" Yes","2420"]
[null,null,null,null,null,"1 inNH",null,null,null,null,null,null,"Style","Inlet",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"no2.5 IN","NYCORP","no2.5 INNYCORP",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip",4866,161,50,"Fog Tip 161 @ 50",null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip 300 @ 100 4824",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stack Tips No 2.5 in 1-3/8\"; 1-1/4\"; 1\" Yes","2420"]
[null,null,null,null,null,"1 inNPSH",null,null,null,null,null,null,"2102",1,{"$f":"CONCATENATE(N62,\" in\")","v":"1 in"},"1 in",null,"SOIN1 in","1 in",null,null,{"$f":"CONCATENATE(RIGHT($R62,LEN($R62)-4),S62)","v":"1 in1 in"},null,null,null,null,null,null,null,null,null,null,null,null,"no2.5 IN","PCT","no2.5 INPCT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip",4866,175,50,"Fog Tip 175 @ 50",null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip 300 @ 75 4824",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stack Tips Yes 1.5 in 15/16\"; 1/2\" No (Std)","1441"]
[null,null,null,null,null,"1 inStorz",null,null,null,null,null,null,"2126",2.5,{"$f":"CONCATENATE(N63,\" in\")","v":"2.5 in"},"1.5 in",null,"SOIN1.5 in","1.5 in",null,null,{"$f":"CONCATENATE(RIGHT($R63,LEN($R63)-4),S63)","v":"1.5 in1.5 in"},null,null,null,null,null,null,null,null,null,null,null,null,"no2.5 IN","Custom","no2.5 INCustom",null,null,null,null,null,null,null,null,null,null,null,null,null,"1520","1523","1528","1820",null,null,null,{"$f":"CONCATENATE(AX$74,AY64,AX$64)","v":"SaberJet Fog Nozzle1/2\"95 @ 100"},"1520","SaberJet Fog Nozzle1/2\"95 @ 100",null,null,null,null,null,null,null,null,null,"Fog Tip",4866,185,50,"Fog Tip 185 @ 50",null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip 350 @ 100 4824",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stack Tips Yes 1.5 in 15/16\"; 1/2\" Yes","1440"]
[null,null,null,null,null,"1 inCustom",null,null,null,null,null,null,"2127",1.5,"1.5 in","1.5 in",null,"SOIN2 in","1.5 in",null,null,"2 in1.5 in",null,null,null,null,null,null,null,null,null,null,null,null,"no2.5 IN","NH","no2.5 INNH",null,null,null,null,null,null,null,"1/2\"1520","95 @ 100","1/2\"","1520",null,"95 @ 100","1/2\"","3/4\"","1-1/8\"","3/4\"",null,null,null,{"$f":"CONCATENATE(AX$74,AY65,AX$64)","v":"SaberJet Fog Nozzle5/8\"95 @ 100"},"1520","SaberJet Fog Nozzle5/8\"95 @ 100",null,null,null,null,null,null,null,null,null,"Fog Tip",4866,225,"100 (Std)","Fog Tip 225 @ 100 (Std)",null,null,null,null,null,null,null,null,null,null,null,null,"Fog Tip 95 @ 100 4866",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stack Tips Yes 2.5 in 1-1/4\"; 1-1/8\"; 1\" No (Std)","2393"]
[null,null,null,null,null,"2 inStorz",null,null,null,null,null,null,"2130",2.5,"2.5 in","2.5 in",null,"SOIN2.5 in","2.5 in","1.5 in",null,"2.5 in2.5 in","2.5 in1.5 in",null,null,null,null,null,null,null,null,null,null,null,"no2.5 IN","NPSH","no2.5 INNPSH",null,null,null,null,null,null,null,"5/8\"1520","95 @ 100","5/8\"","1520",null,"135 @ 100","5/8\"","7/8\"",null,"7/8\"",null,null,null,{"$f":"CONCATENATE(AX$74,AZ64,AX$65)","v":"SaberJet Fog Nozzle3/4\"135 @ 100"},"1523","SaberJet Fog Nozzle3/4\"135 @ 100",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stack Tips Yes 2.5 in 1-1/8\"; 1/2\" No (Std)","1443"]
[null,null,null,null,null,"3 inStorz",null,null,null,null,null,null,"2390",2.5,"2.5 in","1.5 in",null,"SOIN3 in","2.5 in","1.5 in",null,"3 in2.5 in","3 in1.5 in",null,null,null,null,null,null,null,null,null,null,null,"no2.5 IN","FDNY","no2.5 INFDNY",null,null,null,null,null,null,null,"3/4\"1523","135 @ 100","3/4\"","1523",null,null,null,"15/16\"",null,"15/16\"",null,null,null,{"$f":"CONCATENATE(AX$74,AZ65,AX$65)","v":"SaberJet Fog Nozzle7/8\"135 @ 100"},"1523","SaberJet Fog Nozzle7/8\"135 @ 100",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Stack Tips Yes 2.5 in 1-1/8\"; 1/2\" Yes","1442"]
[null,null,null,null,null,null,null,null,null,null,null,null,"2431",1.5,"1.5 in","1.5 in",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"no2.5 IN","NYCORP","no2.5 INNYCORP",null,null,null,null,null,null,null,"7/8\"1523","135 @ 100","7/8\"","1523",null,null,null,"1\"",null,"1\"",null,null,null,{"$f":"CONCATENATE(AX$74,AZ66,AX$65)","v":"SaberJet Fog Nozzle15/16\"135 @ 100"},"1523","SaberJet Fog Nozzle15/16\"135 @ 100"]
[null,null,null,null,null,null,null,null,null,null,null,null,"2433",2.5,"2.5 in","1.5 in",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"no2.5 IN","PITT6","no2.5 INPITT6",null,null,null,null,null,null,null,"15/16\"1523","135 @ 100","15/16\"","1523",null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(AX$74,AZ67,AX$65)","v":"SaberJet Fog Nozzle1\"135 @ 100"},"1523","SaberJet Fog Nozzle1\"135 @ 100"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"no2.5 IN","BAT","no2.5 INBAT",null,null,null,null,null,null,null,"1\"1523","135 @ 100","1\"","1523",null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(AX$74,BA64,AX$65)","v":"SaberJet Fog Nozzle1-1/8\"135 @ 100"},"1528","SaberJet Fog Nozzle1-1/8\"135 @ 100"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"no2.5 IN","CSA","no2.5 INCSA",null,null,null,null,null,null,null,"1-1/8\"1528","135 @ 100","1-1/8\"","1528",null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(AY$74,AU71)","v":"UltraJet Fog Nozzle3/4\""},"1820","UltraJet Fog Nozzle3/4\""]
[null,null,null,null,null,null,null,null,null,null,null,null,"Style","Outlet",null,null,"BoreShutoff Only","BoreShutoff with Integrated Tip",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"no2.5 IN","QST","no2.5 INQST",null,null,null,null,null,null,null,"3/4\"1820",null,"3/4\"","1820",null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(AY$74,AU72)","v":"UltraJet Fog Nozzle7/8\""},"1820","UltraJet Fog Nozzle7/8\""]
[null,null,null,null,null,null,null,null,null,null,null,null,"2102",1,{"$f":"CONCATENATE(N72,\" in\")","v":"1 in"},556,"N/A","7/8\"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"no2.5 IN","Custom","no2.5 INCustom",null,null,null,null,null,null,null,"7/8\"1820",null,"7/8\"","1820",null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(AY$74,AU73)","v":"UltraJet Fog Nozzle15/16\""},"1820","UltraJet Fog Nozzle15/16\""]
[null,null,null,null,null,null,null,null,null,null,null,null,"2126",1.5,"1.5 in",676,null,"15/16\"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"15/16\"1820",null,"15/16\"","1820",null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(AY$74,AU74)","v":"UltraJet Fog Nozzle1\""},"1820","UltraJet Fog Nozzle1\""]
[null,null,null,null,null,null,null,null,null,null,null,null,"2127",1.5,"1.5 in",544,null,"1\"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1\"1820",null,"1\"","1820",null,"SaberJet Fog Nozzle","UltraJet Fog Nozzle"]
[null,null,null,null,null,null,null,null,null,null,null,null,"2130",2.5,"2.5 in",986,null,"1-1/8\"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RF Chart",50]
[null,null,null,null,null,null,null,null,null,null,null,null,"2390",1.5,"1.5 in",1102,null,"1-1/4\"",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SaberJet Fog Nozzle",null,null,null,null,null,118,"118",42]
[null,null,null,null,null,null,null,null,null,null,null,null,"2431",1.5,"1.5 in",574,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(AU64,AT64)","v":"1/2\"95 @ 100"},{"$f":"AV64","v":"1520"},null,"SaberJet Fog Nozzle",null,null,null,null,null,161,"161",57]
[null,null,null,null,null,null,null,null,null,null,null,null,"2433",1.5,"1.5 in",738,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(AU65,AT65)","v":"5/8\"95 @ 100"},{"$f":"AV65","v":"1520"},null,null,null,null,null,null,null,210,"210",75]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(R72,\"2431\")","v":"7/8\"2431"},null,"Shutoff Only","Shutoff with Integrated Tip",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3/4\"135 @ 100","1523",null,null,null,null,null,null,null,185,"185",66]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(R73,\"2431\")","v":"15/16\"2431"},null,"1 in","1.5 in",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"7/8\"135 @ 100","1523"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(R74,\"2431\")","v":"1\"2431"},null,"1.5 in","2 in",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"15/16\"135 @ 100","1523"]
[null,null,null,null,null,null,null,null,null,null,null,null,"Style","Outlet",null,null,null,{"$f":"CONCATENATE(R75,\"2431\")","v":"1-1/8\"2431"},null,"2 in","2.5 in",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1\"135 @ 100","1523"]
[null,null,null,null,null,null,null,null,null,null,null,"Shutoff Only1 in2102","2102","1 in","Shutoff Only1 in2102",null,null,{"$f":"CONCATENATE(R76,\"2431\")","v":"1-1/4\"2431"},null,"2.5 in","3 in",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1-1/8\"135 @ 100","1528"]
[null,null,null,null,null,null,null,null,null,null,null,"Shutoff Only1.5 in2126","2126","1.5 in","Shutoff Only1.5 in2126",null,null,{"$f":"CONCATENATE(R72,\"2433\")","v":"7/8\"2433"},null,"3 in"]
[null,null,null,null,null,null,null,null,null,null,null,"Shutoff Only1.5 in2127","2127","1.5 in","Shutoff Only1.5 in2127",null,null,{"$f":"CONCATENATE(R73,\"2433\")","v":"15/16\"2433"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SaberJet_Fog_Nozzle","UltraJet_Fog_Nozzle",{"$f":"CONCATENATE(AY$85,AY86)","v":"SaberJet_Fog_Nozzle1.5_in"},"1/2\"","5/8\"","3/4\"","7/8\"","15/16\"","1\"","1-1/8\""]
[null,null,null,null,null,null,null,null,null,null,null,"Shutoff Only2.5 in2130","2130","2.5 in","Shutoff Only2.5 in2130",null,null,{"$f":"CONCATENATE(R74,\"2433\")","v":"1\"2433"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"1.5_in","1.5_in",{"$f":"CONCATENATE(AY$85,AY87)","v":"SaberJet_Fog_Nozzle2_in"},"1/2\"","5/8\"","3/4\"","7/8\"","15/16\"","1\"","1-1/8\""]
[null,null,null,null,null,null,null,null,null,null,null,"Shutoff Only1.5 in2390","2390","1.5 in","Shutoff Only1.5 in2390",null,null,{"$f":"CONCATENATE(R75,\"2433\")","v":"1-1/8\"2433"},null,{"$f":"CONCATENATE(T$79,T80)","v":"Shutoff Only1 in"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2_in","2_in",{"$f":"CONCATENATE(AY$85,AY88)","v":"SaberJet_Fog_Nozzle2.5_in"},"1/2\"","5/8\"","3/4\"","7/8\"","15/16\"","1\"","1-1/8\""]
[null,null,null,null,null,null,null,null,null,null,null,"Shutoff with Integrated Tip1.5 in2431","2431","1.5 in","Shutoff with Integrated Tip1.5 in2431",null,null,{"$f":"CONCATENATE(R76,\"2433\")","v":"1-1/4\"2433"},null,{"$f":"CONCATENATE(T$79,T81)","v":"Shutoff Only1.5 in"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"2.5_in","2.5_in",{"$f":"CONCATENATE(AY$85,AY89)","v":"SaberJet_Fog_Nozzle3_in"},"1/2\"","5/8\"","3/4\"","7/8\"","15/16\"","1\"","1-1/8\""]
[null,null,null,null,null,null,null,null,null,null,null,"Shutoff with Integrated Tip1.5 in2433","2433","1.5 in","Shutoff with Integrated Tip1.5 in2433",null,null,null,null,{"$f":"CONCATENATE(T$79,T82)","v":"Shutoff Only2 in"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"3_in","3_in",{"$f":"CONCATENATE(AZ$85,AZ86)","v":"UltraJet_Fog_Nozzle1.5_in"},"3/4\"","7/8\"","15/16\"","1\""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(T$79,T83)","v":"Shutoff Only2.5 in"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(AZ$85,AZ87)","v":"UltraJet_Fog_Nozzle2_in"},"3/4\"","7/8\"","15/16\"","1\""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(T$79,T84)","v":"Shutoff Only3 in"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(AZ$85,AZ88)","v":"UltraJet_Fog_Nozzle2.5_in"},"3/4\"","7/8\"","15/16\"","1\""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(U$79,U80)","v":"Shutoff with Integrated Tip1.5 in"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(AZ$85,AZ89)","v":"UltraJet_Fog_Nozzle3_in"},"3/4\"","7/8\"","15/16\"","1\""]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(U$79,U81)","v":"Shutoff with Integrated Tip2 in"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(U$79,U82)","v":"Shutoff with Integrated Tip2.5 in"}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CONCATENATE(U$79,U83)","v":"Shutoff with Integrated Tip3 in"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"UltraJet Fog Nozzle3_in"]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,2102,"shutoff only1 in","1 in","shutoff only1 in1 in",2102,null,null,"shutoff only1 in1 in",2102,{"$f":"CONCATENATE(S99,T99)","v":"shutoff only1 in1 in2102"}]
[null,null,null,null,null,null,null,null,null,null,null,2126,"shutoff only1.5 in","1.5 in","shutoff only1.5 in1.5 in",2127,null,null,"shutoff only1.5 in1.5 in",2127,{"$f":"CONCATENATE(S100,T100)","v":"shutoff only1.5 in1.5 in2127"}]
[null,null,null,null,null,null,null,null,null,null,null,null,"shutoff only2 in","1.5 in","shutoff only2 in1.5 in",2127,null,null,"shutoff only2 in1.5 in",2127,"shutoff only2 in1.5 in2127"]
[null,null,null,null,null,null,null,null,null,null,null,null,"shutoff only2.5 in","1.5 in","shutoff only2.5 in1.5 in",2126,2390,null,"shutoff only2.5 in1.5 in",2126,"shutoff only2.5 in1.5 in2126"]
[null,null,null,null,null,null,null,null,null,null,null,null,"shutoff only2.5 in","2.5 in","shutoff only2.5 in2.5 in",2130,null,null,"shutoff only2.5 in2.5 in",2130,"shutoff only2.5 in2.5 in2130"]
[null,null,null,null,null,null,null,null,null,null,null,null,"shutoff only3 in","2.5 in","shutoff only3 in2.5 in",2130,null,null,"shutoff only3 in2.5 in",2130,"shutoff only3 in2.5 in2130"]
[null,null,null,null,null,null,null,null,null,null,null,null,"shutoff only3 in","1.5 in","shutoff only3 in1.5 in",2126,2390,null,"shutoff only3 in1.5 in",2126,"shutoff only3 in1.5 in2126"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"shutoff with integrated tip1.5 in1.5 in",2431,null,null,"shutoff with integrated tip1.5 in1.5 in",2431,"shutoff with integrated tip1.5 in1.5 in2431"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"shutoff with integrated tip2 in1.5 in",2431,null,null,"shutoff with integrated tip2 in1.5 in",2431,"shutoff with integrated tip2 in1.5 in2431"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"shutoff with integrated tip2.5 in1.5 in",2433,null,null,"shutoff with integrated tip2.5 in1.5 in",2433,"shutoff with integrated tip2.5 in1.5 in2433"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,"shutoff with integrated tip3 in1.5 in",2433,null,null,"shutoff with integrated tip3 in1.5 in",2433,"shutoff with integrated tip3 in1.5 in2433"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"shutoff only2.5 in1.5 in",2390,"shutoff only2.5 in1.5 in2390"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"shutoff only3 in1.5 in",2390,"shutoff only3 in1.5 in2390"]

{"sheet":"BlankPage","index":6,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"DataSource","index":7,"n_rows":1490,"n_cols":42,"rows_kept":1490,"cut":false,"hidden":true,"merged":[]}
["item","description",null,null,null,null,null,null,null,null,"product_code","Prod Code Description","stat","Inlet Size","Inlet Thread or Type","GPM or LPM","Flow","PSI, kPA or BAR","Bore Size","Pressure","Bumper Color","Custom Etch","Language","Category","Size Class","NPG","Quad","Qtl","Style","Outlet Size","Outlet thread","ZT",null,null,"item","description",null,null,null,null,null,"adfad"]
["17024001","TBJT 1.0 NH 13-60G@100P FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1,"NH","GPM","13-60","PSI","n/a",100,"BLACK","N","ENGLISH","Selectable","1\"","N",80,1,"1702","N/A","N/A",null,null,{"$f":"CONCATENATE(AC2,\" \",N2,\" in \",O2,\" \",IF(AD2=\"n/a\",\"\",CONCATENATE(AD2,\" in \",AE2,\" \")),IF(Q2=\"n/a\",\"\",Q2),IF(S2=\"n/a\",\"\",CONCATENATE(IF(X2=\"saber\",\" \",\"\"),S2,\" bore size(s) \")),IF(T2=\"n/a\",\"\",CONCATENATE(IF(X2=\"saber\",\"\",\" \"),T2,IF(T2=100,\" (Std) \",IF(T2=87,\" (CE) \",\" \")))),IF(U2=\"n/a\",\"\",CONCATENATE(U2,IF(U2=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X2,3)=\"tip\",IF(LEFT(X2,1)=\"s\",\"\",IF(Z2=\"n\",IF(T2=\"N/A\",\"PG\",\" PG\"),IF(Z2=\"y\",IF(T2=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z2=\"n\",IF(T2=\"N/A\",\"PG\",\" PG\"),IF(Z2=\"y\",IF(T2=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF2=\"y\",\" ZT\",\"\"),IF(V2=\"N\",\"\",IF(S2=\"n/a\",\" ETCH\",IF(T2=\"N/A\",IF(RIGHT(X2,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X2=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"1702 1 in NH 13-60 100 (Std) BLACK (Std) PG"},{"$f":"A2","v":"17024001"},{"$f":"B2","v":"TBJT 1.0 NH 13-60G@100P FM"},{"$f":"LEN(AH2)","v":43}]
["17024002","TBJT 1.0 BSP 50-230L@7b FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1,"BSP","LPM","50-230","BAR","n/a",7,"BLACK","N","ENGLISH","Selectable","1\"","N",80,1,"1702","N/A","N/A",null,null,"1702 1 in BSP 50-230 7 BLACK (Std) PG","17024002","TBJT 1.0 BSP 50-230L@7b FM",37]
["17024008","TBJT 1.0 NPSH 13-60G@100P FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1,"NPSH","GPM","13-60","PSI","n/a",100,"BLACK","N","ENGLISH","Selectable","1\"","N",80,1,"1702","N/A","N/A",null,null,"1702 1 in NPSH 13-60 100 (Std) BLACK (Std) PG","17024008","TBJT 1.0 NPSH 13-60G@100P FM",45]
["17024701","TBJT 52MM 50-230L@6b GERMAN EN",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2,"STORZ","LPM","50-230","BAR","n/a",6,"BLACK","N","GERMAN","Selectable","1\"","N",80,1,"1702","N/A","N/A",null,null,"1702 2 in STORZ 50-230 6 BLACK (Std) PG","17024701","TBJT 52MM 50-230L@6b GERMAN EN",39]
["17024003","TBJT 1.0 BSPX25MMSTZ 50-230L@7b FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1,"STORZ","LPM","50-230","BAR","n/a",7,"BLACK","N","ENGLISH","Selectable","1\"","N",20,1,"1702","N/A","N/A",null,null,"1702 1 in STORZ 50-230 7 BLACK (Std) PG","17024003","TBJT 1.0 BSPX25MMSTZ 50-230L@7b FM",39]
["17024010","TBJT 52MM 50-230L@7b FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2,"STORZ","LPM","50-230","BAR","n/a",7,"BLACK","N","ENGLISH","Selectable","1\"","N",20,1,"1702","N/A","N/A",null,null,"1702 2 in STORZ 50-230 7 BLACK (Std) PG","17024010","TBJT 52MM 50-230L@7b FM",39]
["17024702","TBJT 1.0 BSP 50-230L@6b EN",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1,"BSP","LPM","50-230","BAR","n/a",6,"BLACK","N","ENGLISH","Selectable","1\"","N",20,1,"1702","N/A","N/A",null,null,"1702 1 in BSP 50-230 6 BLACK (Std) PG","17024702","TBJT 1.0 BSP 50-230L@6b EN",37]
["17027001","TBJT NPG 1.0 NH 13-60G@100P",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1,"NH","GPM","13-60","PSI","n/a",100,"BLACK","N","ENGLISH","Selectable","1\"","Y",20,1,"1702","N/A","N/A",null,null,"1702 1 in NH 13-60 100 (Std) BLACK (Std) NPG","17027001","TBJT NPG 1.0 NH 13-60G@100P",44]
["17020705","TBJT NZ 1 BSP50-230L@6bDUTCH SER# B",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1,"BSP","LPM","50-230","BAR","N/A",6,"BLACK","N","DUTCH","Selectable","1\"","N",20,2,"1702","N/A","N/A",null,null,"1702 1 in BSP 50-230 6 BLACK (Std) PG","17020705","TBJT NZ 1 BSP50-230L@6bDUTCH SER# B",37]
["17024009","TBJT 2.5BIM 50-230L@7b FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"BIM","LPM","50-230","BAR","n/a",7,"BLACK","N","ENGLISH","Selectable","1\"","N",20,2,"1702","N/A","N/A",null,null,"1702 2.5 in BIM 50-230 7 BLACK (Std) PG","17024009","TBJT 2.5BIM 50-230L@7b FM",39,null,{"$f":"MAX(AK:AK)","v":68}]
["17027701","TBJT NPG 52MM 50-230L@6b GERMAN EN",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2,"STORZ","LPM","50-230","BAR","n/a",6,"BLACK","N","GERMAN","Selectable","1\"","Y",20,2,"1702","N/A","N/A",null,null,"1702 2 in STORZ 50-230 6 BLACK (Std) NPG","17027701","TBJT NPG 52MM 50-230L@6b GERMAN EN",40]
["17024004","TBJT 1.0 NH 50-230L@7b FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1,"NH","LPM","50-230","BAR","n/a",7,"BLACK","N","ENGLISH","Selectable","1\"","N",20,3,"1702","N/A","N/A",null,null,"1702 1 in NH 50-230 7 BLACK (Std) PG","17024004","TBJT 1.0 NH 50-230L@7b FM",36]
["17024017","TBJT 1.0 NH 13-60G@100P MT. PLEASANT",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1,"NH","GPM","13-60","PSI","N/A",100,"BLACK","Y","ENGLISH","Selectable","1\"","N",20,3,"1702","N/A","N/A",null,null,"1702 1 in NH 13-60 100 (Std) BLACK (Std) PG ETCH","17024017","TBJT 1.0 NH 13-60G@100P MT. PLEASANT",48]
["17024018","TBJT 1.0 NH 13-60G@100P RED BANKS",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1,"NH","GPM","13-60","PSI","N/A",100,"BLACK","Y","ENGLISH","Selectable","1\"","N",20,3,"1702","N/A","N/A",null,null,"1702 1 in NH 13-60 100 (Std) BLACK (Std) PG ETCH","17024018","TBJT 1.0 NH 13-60G@100P RED BANKS",48]
["17024019","TBJT 1.0 NH 13-60G@100P VICTORIA",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1,"NH","GPM","13-60","PSI","N/A",100,"BLACK","Y","ENGLISH","Selectable","1\"","N",20,3,"1702","N/A","N/A",null,null,"1702 1 in NH 13-60 100 (Std) BLACK (Std) PG ETCH","17024019","TBJT 1.0 NH 13-60G@100P VICTORIA",48]
["17024020","TBJT 1.0 NH 13-60G@100P WATSON",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1,"NH","GPM","13-60","PSI","N/A",100,"BLACK","Y","ENGLISH","Selectable","1\"","N",20,3,"1702","N/A","N/A",null,null,"1702 1 in NH 13-60 100 (Std) BLACK (Std) PG ETCH","17024020","TBJT 1.0 NH 13-60G@100P WATSON",48]
["17024021","TBJT 1.5 NH 13-60G@100P FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","13-60","PSI","n/a",100,"BLACK","N","ENGLISH","Selectable","1\"","N",20,3,"1702","N/A","N/A",null,null,"1702 1.5 in NH 13-60 100 (Std) BLACK (Std) PG","17024021","TBJT 1.5 NH 13-60G@100P FM",45]
["17024704","TBJT 1.0BSPX25MMSTZ 50-230L@6b GERMAN EN",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1,"STORZ","LPM","50-230","BAR","n/a",6,"BLACK","N","GERMAN","Selectable","1\"","N","No 2021 Sales","No 2021 Sales","1702","N/A","N/A",null,null,"1702 1 in STORZ 50-230 6 BLACK (Std) PG","17024704","TBJT 1.0BSPX25MMSTZ 50-230L@6b GERMAN EN",39]
["17027002","TBJT NPG 1.0 BSP 50-230L@7b FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1,"BSP","LPM","50-230","BAR","n/a",7,"BLACK","N","ENGLISH","Selectable","1\"","Y","No 2021 Sales","No 2021 Sales","1702","N/A","N/A",null,null,"1702 1 in BSP 50-230 7 BLACK (Std) NPG","17027002","TBJT NPG 1.0 BSP 50-230L@7b FM",38]
["17027008","TBJT NPG 1.0 NPSH 13-60G@100P FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1,"NPSH","GPM","13-60","PSI","n/a",100,"BLACK","N","ENGLISH","Selectable","1\"","Y","No 2021 Sales","No 2021 Sales","1702","N/A","N/A",null,null,"1702 1 in NPSH 13-60 100 (Std) BLACK (Std) NPG","17027008","TBJT NPG 1.0 NPSH 13-60G@100P FM",46]
["17034002","TBJT TIP 1.0 W/1.5BSP 50-230L@7b",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"BSP","LPM","50-230","BAR","n/a",7,"BLACK","N","ENGLISH","Selectable Tip","1\"","N/A",20,1,"1703","N/A","N/A",null,null,"1703 1.5 in BSP 50-230 7 BLACK (Std)","17034002","TBJT TIP 1.0 W/1.5BSP 50-230L@7b",36]
["17034003","TBJT TIP 1.0 W/1.5NH 50-230L@7b",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","LPM","50-230","BAR","n/a",7,"BLACK","N","ENGLISH","Selectable Tip","1\"","N/A",20,1,"1703","N/A","N/A",null,null,"1703 1.5 in NH 50-230 7 BLACK (Std)","17034003","TBJT TIP 1.0 W/1.5NH 50-230L@7b",35]
["17034001","TBJT TIP 1.0 W/1.5NH 13-60G@100P#",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","13-60","PSI","n/a",100,"BLACK","N","ENGLISH","Selectable Tip","1\"","N/A",20,2,"1703","N/A","N/A",null,null,"1703 1.5 in NH 13-60 100 (Std) BLACK (Std)","17034001","TBJT TIP 1.0 W/1.5NH 13-60G@100P#",42]
["17034005","TBJT TIP 1.0 W/1.5NPSH 13-60G@100P",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NPSH","GPM","13-60","PSI","n/a",100,"BLACK","N","ENGLISH","Selectable Tip","1\"","N/A",20,2,"1703","N/A","N/A",null,null,"1703 1.5 in NPSH 13-60 100 (Std) BLACK (Std)","17034005","TBJT TIP 1.0 W/1.5NPSH 13-60G@100P",44]
["17034006","TBJT TIP 1.0 W/1.5BSP 50-230L@6b ENGLISH",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"BSP","LPM","50-230","BAR","n/a",6,"BLACK","N","ENGLISH","Selectable Tip","1\"","N/A",20,1,"1703","N/A","N/A",null,null,{"$f":"CONCATENATE(AC26,\" \",N26,\" in \",O26,\" \",IF(AD26=\"n/a\",\"\",CONCATENATE(AD26,\" in \",AE26,\" \")),IF(Q26=\"n/a\",\"\",Q26),IF(S26=\"n/a\",\"\",CONCATENATE(IF(X26=\"saber\",\" \",\"\"),S26,\" bore size(s) \")),IF(T26=\"n/a\",\"\",CONCATENATE(IF(X26=\"saber\",\"\",\" \"),T26,IF(T26=100,\" (Std) \",IF(T26=87,\" (CE) \",\" \")))),IF(U26=\"n/a\",\"\",CONCATENATE(U26,IF(U26=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X26,3)=\"tip\",IF(LEFT(X26,1)=\"s\",\"\",IF(Z26=\"n\",IF(T26=\"N/A\",\"PG\",\" PG\"),IF(Z26=\"y\",IF(T26=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z26=\"n\",IF(T26=\"N/A\",\"PG\",\" PG\"),IF(Z26=\"y\",IF(T26=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF26=\"y\",\" ZT\",\"\"),IF(V26=\"N\",\"\",IF(S26=\"n/a\",\" ETCH\",IF(T26=\"N/A\",IF(RIGHT(X26,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X26=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"1703 1.5 in BSP 50-230 6 BLACK (Std)"},{"$f":"A26","v":"17034006"},{"$f":"B26","v":"TBJT TIP 1.0 W/1.5BSP 50-230L@6b ENGLISH"},{"$f":"LEN(AH26)","v":36}]
["17034004","TBJT TIP 1.0 W/1.5BSP 50-230L@6b GERMAN",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"BSP","LPM","50-30","BAR","n/a",6,"BLACK","N","GERMAN","Selectable Tip","1\"","N/A","No 2021 Sales","No 2021 Sales","1703","N/A","N/A",null,null,"1703 1.5 in BSP 50-30 6 BLACK (Std)","17034004","TBJT TIP 1.0 W/1.5BSP 50-230L@6b GERMAN",35]
["17044703","TBJT 1.0 BSP 50-115L@6b ENGLISH EN",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1,"BSP","LPM","50-115","BAR","N/A",6,"BLACK","N","ENGLISH","Selectable","1\"","N",80,1,"1704","N/A","N/A",null,null,"1704 1 in BSP 50-115 6 BLACK (Std) PG","17044703","TBJT 1.0 BSP 50-115L@6b ENGLISH EN",37]
["17044002","TBJT 1.0 NH 13-23-30G@100P",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1,"NH","GPM","13-30","PSI","n/a",100,"BLACK","N","ENGLISH","Selectable","1\"","N",20,1,"1704","N/A","N/A",null,null,"1704 1 in NH 13-30 100 (Std) BLACK (Std) PG","17044002","TBJT 1.0 NH 13-23-30G@100P",43]
["17044003","TBJT 1.0 NH 18-30G@100P",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1,"NH","GPM","18-30","PSI","n/a",100,"BLACK","N","ENGLISH","Selectable","1\"","N",20,1,"1704","N/A","N/A",null,null,"1704 1 in NH 18-30 100 (Std) BLACK (Std) PG","17044003","TBJT 1.0 NH 18-30G@100P",43]
["17044004","TBJT 1.0 NH 70-115L@7b",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1,"NH","LPM","70-115","BAR","N/A",7,"BLACK","N","ENGLISH","Selectable","1\"","N",20,1,"1704","N/A","N/A",null,null,"1704 1 in NH 70-115 7 BLACK (Std) PG","17044004","TBJT 1.0 NH 70-115L@7b",36]
["17044006","TBJT 1.0 BSP 50-90-115L@7b",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1,"BSP","LPM","50-115","BAR","N/A",7,"BLACK","N","ENGLISH","Selectable","1\"","N",20,1,"1704","N/A","N/A",null,null,"1704 1 in BSP 50-115 7 BLACK (Std) PG","17044006","TBJT 1.0 BSP 50-90-115L@7b",37]
["17044009","TBJT 1.0 NH 18-30G@100P ORGBMPR",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1,"NH","GPM","18-30","PSI","N/A",100,"ORANGE","N","ENGLISH","Selectable","1\"","N",20,2,"1704","N/A","N/A",null,null,"1704 1 in NH 18-30 100 (Std) ORANGE PG","17044009","TBJT 1.0 NH 18-30G@100P ORGBMPR",38]
["17044005","TBJT 52MM 50-115L@7b GERMAN YLWBMPR",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2,"STORZ","LPM","50-115","BAR","N/A",7,"YELLOW","N","GERMAN","Selectable","1\"","N",20,3,"1704","N/A","N/A",null,null,"1704 2 in STORZ 50-115 7 YELLOW PG","17044005","TBJT 52MM 50-115L@7b GERMAN YLWBMPR",34]
["17044007","TBJT 1.0 NH 50-90-115L@7b/700kPa",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1,"NH","LPM","50-115","BAR","N/A",7,"BLACK","N","ENGLISH","Selectable","1\"","N",20,3,"1704","N/A","N/A",null,null,"1704 1 in NH 50-115 7 BLACK (Std) PG","17044007","TBJT 1.0 NH 50-90-115L@7b/700kPa",36]
["17044008","TBJT 52MM 50-115L@7b GERMAN",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2,"STORZ","LPM","50-115","BAR","N/A",7,"BLACK","N","GERMAN","Selectable","1\"","N",20,3,"1704","N/A","N/A",null,null,"1704 2 in STORZ 50-115 7 BLACK (Std) PG","17044008","TBJT 52MM 50-115L@7b GERMAN",39]
["17044701","TBJT 1.0 BSP 50-115L@6b DUTCH BLU EN",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1,"BSP","LPM","50-115","BAR","N/A",6,"BLUE","N","DUTCH","Selectable","1\"","N",20,3,"1704","N/A","N/A",null,null,"1704 1 in BSP 50-115 6 BLUE PG","17044701","TBJT 1.0 BSP 50-115L@6b DUTCH BLU EN",30]
["17044001","TBJT 1.0 BSP 70-115L@7b",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1,"BSP","LPM","70-115","BAR","N/A",7,"BLACK","N","ENGLISH","Selectable","1\"","N","No 2021 Sales","No 2021 Sales","1704","N/A","N/A",null,null,"1704 1 in BSP 70-115 7 BLACK (Std) PG","17044001","TBJT 1.0 BSP 70-115L@7b",37]
["17044010","TBJT 1.0 BSPX25MM STZ 50-115L@7b YLWBMPR",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1,"STORZ","LPM","50-115","BAR","N/A",7,"YELLOW","N","ENGLISH","Selectable","1\"","N","No 2021 Sales","No 2021 Sales","1704","N/A","N/A",null,null,"1704 1 in STORZ 50-115 7 YELLOW PG","17044010","TBJT 1.0 BSPX25MM STZ 50-115L@7b YLWBMPR",34]
["17044702","TBJT 1.0 BSP 70-115L@6b GERMAN EN",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1,"BSP","LPM","70-115","BAR","N/A",6,"BLACK","N","GERMAN","Selectable","1\"","N","No 2021 Sales","No 2021 Sales","1704","N/A","N/A",null,null,"1704 1 in BSP 70-115 6 BLACK (Std) PG","17044702","TBJT 1.0 BSP 70-115L@6b GERMAN EN",37]
["17047002","TBJT NPG 1.0 NH 13-23-30G@100P",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1,"NH","GPM","13-30","PSI","n/a",100,"BLACK","N","ENGLISH","Selectable","1\"","Y","No 2021 Sales","No 2021 Sales","1704","N/A","N/A",null,null,"1704 1 in NH 13-30 100 (Std) BLACK (Std) NPG","17047002","TBJT NPG 1.0 NH 13-23-30G@100P",44]
["17114701","TBJT TIP 1.5BSP 50-115L@6b DUTCH BLU",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"BSP","LPM","50-115","BAR","N/A",6,"BLUE","N","DUTCH","Selectable Tip","1\"","N/A",20,1,"1711","N/A","N/A",null,null,"1711 1.5 in BSP 50-115 6 BLUE","17114701","TBJT TIP 1.5BSP 50-115L@6b DUTCH BLU",29]
["17114702","TBJT TIP 1.5BSP 70-115L@6b",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"BSP","LPM","70-115","BAR","N/A",6,"BLACK","N","ENGLISH","Selectable Tip","1\"","N/A",20,2,"1711","N/A","N/A",null,null,"1711 1.5 in BSP 70-115 6 BLACK (Std)","17114702","TBJT TIP 1.5BSP 70-115L@6b",36]
["17114001","TBJT TIP 1.5NH 13-23-30G@100P",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","13-30","PSI","n/a",100,"BLACK","N","ENGLISH","Selectable Tip","1\"","N/A","No 2021 Sales","No 2021 Sales","1711","N/A","N/A",null,null,"1711 1.5 in NH 13-30 100 (Std) BLACK (Std)","17114001","TBJT TIP 1.5NH 13-23-30G@100P",42]
["17144001","TBJT TIP 1.5NH 30-125G@100P",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","30-125","PSI","n/a",100,"BLACK","N","ENGLISH","Selectable Tip","1.5\"","N/A",80,1,"1714","N/A","N/A",null,null,"1714 1.5 in NH 30-125 100 (Std) BLACK (Std)","17144001","TBJT TIP 1.5NH 30-125G@100P",43]
["17144003","TBJT TIP 1.5NPSH 30-125G@100P",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NPSH","GPM","30-125","PSI","n/a",100,"BLACK","N","ENGLISH","Selectable Tip","1.5\"","N/A",20,1,"1714","N/A","N/A",null,null,"1714 1.5 in NPSH 30-125 100 (Std) BLACK (Std)","17144003","TBJT TIP 1.5NPSH 30-125G@100P",45]
["17144009","TBJT TIP 1.5NH 115-475L@7b",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","LPM","115-475","BAR","N/A",7,"BLACK","N","ENGLISH","Selectable Tip","1.5\"","N/A",20,2,"1714","N/A","N/A",null,null,{"$f":"CONCATENATE(AC47,\" \",N47,\" in \",O47,\" \",IF(AD47=\"n/a\",\"\",CONCATENATE(AD47,\" in \",AE47,\" \")),IF(Q47=\"n/a\",\"\",Q47),IF(S47=\"n/a\",\"\",CONCATENATE(IF(X47=\"saber\",\" \",\"\"),S47,\" bore size(s) \")),IF(T47=\"n/a\",\"\",CONCATENATE(IF(X47=\"saber\",\"\",\" \"),T47,IF(T47=100,\" (Std) \",IF(T47=87,\" (CE) \",\" \")))),IF(U47=\"n/a\",\"\",CONCATENATE(U47,IF(U47=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X47,3)=\"tip\",IF(LEFT(X47,1)=\"s\",\"\",IF(Z47=\"n\",IF(T47=\"N/A\",\"PG\",\" PG\"),IF(Z47=\"y\",IF(T47=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z47=\"n\",IF(T47=\"N/A\",\"PG\",\" PG\"),IF(Z47=\"y\",IF(T47=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF47=\"y\",\" ZT\",\"\"),IF(V47=\"N\",\"\",IF(S47=\"n/a\",\" ETCH\",IF(T47=\"N/A\",IF(RIGHT(X47,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X47=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"1714 1.5 in NH 115-475 7 BLACK (Std)"},{"$f":"A47","v":"17144009"},{"$f":"B47","v":"TBJT TIP 1.5NH 115-475L@7b"},{"$f":"LEN(AH47)","v":36}]
["17144005","TBJT TIP 1.5BSP 115-475L@6b",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"BSP","LPM","115-475","BAR","N/A",6,"BLACK","N","ENGLISH","Selectable Tip","1.5\"","N/A",20,2,"1714","N/A","N/A",null,null,"1714 1.5 in BSP 115-475 6 BLACK (Std)","17144005","TBJT TIP 1.5BSP 115-475L@6b",37]
["17144002","TBJT TIP 1.5NH 30-125G@75P",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","30-125","PSI","n/a",75,"BLACK","N","ENGLISH","Selectable Tip","1.5\"","N/A",20,3,"1714","N/A","N/A",null,null,"1714 1.5 in NH 30-125 75 BLACK (Std)","17144002","TBJT TIP 1.5NH 30-125G@75P",36]
["17144004","TBJT TIP 1.5BSP 115-475L@7b",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"BSP","LPM","115-475","BAR","N/A",7,"BLACK","N","ENGLISH","Selectable Tip","1.5\"","N/A","No 2021 Sales","No 2021 Sales","1714","N/A","N/A",null,null,"1714 1.5 in BSP 115-475 7 BLACK (Std)","17144004","TBJT TIP 1.5BSP 115-475L@7b",37]
["17170503","TBJT TIP 1.5NPSH 30-125@100**see notes**",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NPSH","GPM","30-125","PSI","n/a",100,"BLACK","N","ENGLISH","Selectable Tip","1.5\"","N/A","No 2021 Sales","No 2021 Sales","1717","N/A","N/A",null,null,"1717 1.5 in NPSH 30-125 100 (Std) BLACK (Std)","17170503","TBJT TIP 1.5NPSH 30-125@100**see notes**",45]
["17204001","TBJT 1.5NH 30-125G@100P FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","30-125","PSI","N/A",100,"BLACK","N","ENGLISH","Selectable","1.5\"","N",80,1,"1720","N/A","N/A",null,null,"1720 1.5 in NH 30-125 100 (Std) BLACK (Std) PG","17204001","TBJT 1.5NH 30-125G@100P FM",46]
["17204002","TBJT 1.5NPSH 30-125G@100P FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NPSH","GPM","30-125","PSI","N/A",100,"BLACK","N","ENGLISH","Selectable","1.5\"","N",80,1,"1720","N/A","N/A",null,null,"1720 1.5 in NPSH 30-125 100 (Std) BLACK (Std) PG","17204002","TBJT 1.5NPSH 30-125G@100P FM",48]
["17204004","TBJT 1.5BSP 115-475L@7b FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"BSP","LPM","115-475","BAR","N/A",7,"BLACK","N","ENGLISH","Selectable","1.5\"","N",80,1,"1720","N/A","N/A",null,null,"1720 1.5 in BSP 115-475 7 BLACK (Std) PG","17204004","TBJT 1.5BSP 115-475L@7b FM",40]
["17204011","TBJT 1.5NH 30-125G@75P",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","30-125","PSI","N/A",75,"BLACK","N","ENGLISH","Selectable","1.5\"","N",80,1,"1720","N/A","N/A",null,null,"1720 1.5 in NH 30-125 75 BLACK (Std) PG","17204011","TBJT 1.5NH 30-125G@75P",39]
["17204022","TBJT ZT 1.5 ADPT EXT 115-475L@7b",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"N/A","LPM","115-475","BAR","N/A",7,"BLACK","N","ENGLISH","Selectable","1.5\"","N",80,1,"1720","N/A","N/A","Y",null,"1720 1.5 in N/A 115-475 7 BLACK (Std) PG ZT","17204022","TBJT ZT 1.5 ADPT EXT 115-475L@7b",43]
["17204700","TBJT 1.5BSP100-450L@6b DUTCH SER# BLU EN",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"BSP","LPM","100-450","BAR","N/A",6,"BLUE","N","DUTCH","Selectable","1.5\"","N",80,1,"1720","N/A","N/A",null,null,"1720 1.5 in BSP 100-450 6 BLUE PG","17204700","TBJT 1.5BSP100-450L@6b DUTCH SER# BLU EN",33]
["17207001","TBJT NPG 1.5NH 30-125G@100P FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","30-125","PSI","N/A",100,"BLACK","N","ENGLISH","Selectable","1.5\"","Y",80,1,"1720","N/A","N/A",null,null,"1720 1.5 in NH 30-125 100 (Std) BLACK (Std) NPG","17207001","TBJT NPG 1.5NH 30-125G@100P FM",47]
["17204003","TBJT 2.5BIM 115-475L@7b FM#",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"BIM","LPM","115-475","BAR","N/A",7,"BLACK","N","ENGLISH","Selectable","1.5\"","N",20,1,"1720","N/A","N/A",null,null,"1720 2.5 in BIM 115-475 7 BLACK (Std) PG","17204003","TBJT 2.5BIM 115-475L@7b FM#",40]
["17204012","TBJT 52MM 115-475L@7b FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2,"STORZ","LPM","115-475","BAR","N/A",7,"BLACK","N","ENGLISH","Selectable","1.5\"","N",20,1,"1720","N/A","N/A",null,null,"1720 2 in STORZ 115-475 7 BLACK (Std) PG","17204012","TBJT 52MM 115-475L@7b FM",40]
["17204013","TBJT 65MM 115-475L@7b FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"STORZ","LPM","115-475","BAR","N/A",7,"BLACK","N","ENGLISH","Selectable","1.5\"","N",20,1,"1720","N/A","N/A",null,null,"1720 2.5 in STORZ 115-475 7 BLACK (Std) PG","17204013","TBJT 65MM 115-475L@7b FM",42]
["17204021","TBJT 1.5BSP 115-475L@7b SPANISH FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"BSP","LPM","115-475","BAR","N/A",7,"BLACK","N","SPANISH","Selectable","1.5\"","N",20,1,"1720","N/A","N/A",null,null,"1720 1.5 in BSP 115-475 7 BLACK (Std) PG","17204021","TBJT 1.5BSP 115-475L@7b SPANISH FM",40]
["17204025","TBJT 1.5BSP M 115-475L@7b FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"BSP","LPM","115-475","BAR","N/A",7,"BLACK","N","ENGLISH","Selectable","1.5\"","N",20,1,"1720","N/A","N/A",null,null,"1720 1.5 in BSP 115-475 7 BLACK (Std) PG","17204025","TBJT 1.5BSP M 115-475L@7b FM",40]
["17204037","TBJT  2.5BIM 100-450L@6b",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"BIM","LPM","100-450","BAR","N/A",6,"BLACK","N","ENGLISH","Selectable","1.5\"","N",20,1,"1720","N/A","N/A",null,null,"1720 2.5 in BIM 100-450 6 BLACK (Std) PG","17204037","TBJT  2.5BIM 100-450L@6b",40]
["17204038","TBJT 1.5NH 30-125G@100P DE STATE FS LOGO",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","30-125","PSI","N/A",100,"BLACK","Y","ENGLISH","Selectable","1.5\"","N",20,1,"1720","N/A","N/A",null,null,"1720 1.5 in NH 30-125 100 (Std) BLACK (Std) PG ETCH","17204038","TBJT 1.5NH 30-125G@100P DE STATE FS LOGO",51]
["17204046","TBJT 1.5NH 30-125G@75P YLWBMPR",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","30-125","PSI","N/A",75,"YELLOW","N","ENGLISH","Selectable","1.5\"","N",20,1,"1720","N/A","N/A",null,null,{"$f":"CONCATENATE(AC66,\" \",N66,\" in \",O66,\" \",IF(AD66=\"n/a\",\"\",CONCATENATE(AD66,\" in \",AE66,\" \")),IF(Q66=\"n/a\",\"\",Q66),IF(S66=\"n/a\",\"\",CONCATENATE(IF(X66=\"saber\",\" \",\"\"),S66,\" bore size(s) \")),IF(T66=\"n/a\",\"\",CONCATENATE(IF(X66=\"saber\",\"\",\" \"),T66,IF(T66=100,\" (Std) \",IF(T66=87,\" (CE) \",\" \")))),IF(U66=\"n/a\",\"\",CONCATENATE(U66,IF(U66=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X66,3)=\"tip\",IF(LEFT(X66,1)=\"s\",\"\",IF(Z66=\"n\",IF(T66=\"N/A\",\"PG\",\" PG\"),IF(Z66=\"y\",IF(T66=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z66=\"n\",IF(T66=\"N/A\",\"PG\",\" PG\"),IF(Z66=\"y\",IF(T66=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF66=\"y\",\" ZT\",\"\"),IF(V66=\"N\",\"\",IF(S66=\"n/a\",\" ETCH\",IF(T66=\"N/A\",IF(RIGHT(X66,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X66=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"1720 1.5 in NH 30-125 75 YELLOW PG"},{"$f":"A66","v":"17204046"},{"$f":"B66","v":"TBJT 1.5NH 30-125G@75P YLWBMPR"},{"$f":"LEN(AH66)","v":34}]
["17204047","TBJT 1.5NH 30-125G@75P REDBMPR",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","30-125","PSI","N/A",75,"RED","N","ENGLISH","Selectable","1.5\"","N",20,1,"1720","N/A","N/A",null,null,"1720 1.5 in NH 30-125 75 RED PG","17204047","TBJT 1.5NH 30-125G@75P REDBMPR",31]
["17204048","TBJT 1.5NH 30-125G@75P ORGBMPR",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","30-125","PSI","N/A",75,"ORANGE","N","ENGLISH","Selectable","1.5\"","N",20,1,"1720","N/A","N/A",null,null,{"$f":"CONCATENATE(AC68,\" \",N68,\" in \",O68,\" \",IF(AD68=\"n/a\",\"\",CONCATENATE(AD68,\" in \",AE68,\" \")),IF(Q68=\"n/a\",\"\",Q68),IF(S68=\"n/a\",\"\",CONCATENATE(IF(X68=\"saber\",\" \",\"\"),S68,\" bore size(s) \")),IF(T68=\"n/a\",\"\",CONCATENATE(IF(X68=\"saber\",\"\",\" \"),T68,IF(T68=100,\" (Std) \",IF(T68=87,\" (CE) \",\" \")))),IF(U68=\"n/a\",\"\",CONCATENATE(U68,IF(U68=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X68,3)=\"tip\",IF(LEFT(X68,1)=\"s\",\"\",IF(Z68=\"n\",IF(T68=\"N/A\",\"PG\",\" PG\"),IF(Z68=\"y\",IF(T68=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z68=\"n\",IF(T68=\"N/A\",\"PG\",\" PG\"),IF(Z68=\"y\",IF(T68=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF68=\"y\",\" ZT\",\"\"),IF(V68=\"N\",\"\",IF(S68=\"n/a\",\" ETCH\",IF(T68=\"N/A\",IF(RIGHT(X68,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X68=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"1720 1.5 in NH 30-125 75 ORANGE PG"},{"$f":"A68","v":"17204048"},{"$f":"B68","v":"TBJT 1.5NH 30-125G@75P ORGBMPR"},{"$f":"LEN(AH68)","v":34}]
["17204005","TBJT 1.5NPSH 115-475L@7b FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NPSH","LPM","115-475","BAR","N/A",7,"BLACK","N","ENGLISH","Selectable","1.5\"","N",20,2,"1720","N/A","N/A",null,null,"1720 1.5 in NPSH 115-475 7 BLACK (Std) PG","17204005","TBJT 1.5NPSH 115-475L@7b FM",41]
["17204014","TBJT 75MM 115-475L@7b FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",3,"STORZ","LPM","115-475","BAR","N/A",7,"BLACK","N","ENGLISH","Selectable","1.5\"","N",20,2,"1720","N/A","N/A",null,null,"1720 3 in STORZ 115-475 7 BLACK (Std) PG","17204014","TBJT 75MM 115-475L@7b FM",40]
["17204015","TBJT 1.5BSP M 115-475L@5b",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"BSP","LPM","115-475","BAR","n/a",5,"BLACK","N","ENGLISH","Selectable","1.5\"","N",20,2,"1720","N/A","N/A",null,null,{"$f":"CONCATENATE(AC71,\" \",N71,\" in \",O71,\" \",IF(AD71=\"n/a\",\"\",CONCATENATE(AD71,\" in \",AE71,\" \")),IF(Q71=\"n/a\",\"\",Q71),IF(S71=\"n/a\",\"\",CONCATENATE(IF(X71=\"saber\",\" \",\"\"),S71,\" bore size(s) \")),IF(T71=\"n/a\",\"\",CONCATENATE(IF(X71=\"saber\",\"\",\" \"),T71,IF(T71=100,\" (Std) \",IF(T71=87,\" (CE) \",\" \")))),IF(U71=\"n/a\",\"\",CONCATENATE(U71,IF(U71=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X71,3)=\"tip\",IF(LEFT(X71,1)=\"s\",\"\",IF(Z71=\"n\",IF(T71=\"N/A\",\"PG\",\" PG\"),IF(Z71=\"y\",IF(T71=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z71=\"n\",IF(T71=\"N/A\",\"PG\",\" PG\"),IF(Z71=\"y\",IF(T71=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF71=\"y\",\" ZT\",\"\"),IF(V71=\"N\",\"\",IF(S71=\"n/a\",\" ETCH\",IF(T71=\"N/A\",IF(RIGHT(X71,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X71=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"1720 1.5 in BSP 115-475 5 BLACK (Std) PG"},{"$f":"A71","v":"17204015"},{"$f":"B71","v":"TBJT 1.5BSP M 115-475L@5b"},{"$f":"LEN(AH71)","v":40}]
["17204023","TBJT 1.5NPSH 30-125G@75P",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NPSH","GPM","30-125","PSI","N/A",75,"BLACK","N","ENGLISH","Selectable","1.5\"","N",20,2,"1720","N/A","N/A",null,null,"1720 1.5 in NPSH 30-125 75 BLACK (Std) PG","17204023","TBJT 1.5NPSH 30-125G@75P",41]
["17204030","TBJT 1.5BSP100-450L@6b",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"BSP","LPM","100-450","BAR","N/A",6,"BLACK","N","ENGLISH","Selectable","1.5\"","N",20,2,"1720","N/A","N/A",null,null,"1720 1.5 in BSP 100-450 6 BLACK (Std) PG","17204030","TBJT 1.5BSP100-450L@6b",40]
["17204044","TBJT 52MM 30-125G@75P",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2,"STORZ","GPM","30-125","PSI","N/A",75,"BLACK","N","ENGLISH","Selectable","1.5\"","N",20,2,"1720","N/A","N/A",null,null,{"$f":"CONCATENATE(AC74,\" \",N74,\" in \",O74,\" \",IF(AD74=\"n/a\",\"\",CONCATENATE(AD74,\" in \",AE74,\" \")),IF(Q74=\"n/a\",\"\",Q74),IF(S74=\"n/a\",\"\",CONCATENATE(IF(X74=\"saber\",\" \",\"\"),S74,\" bore size(s) \")),IF(T74=\"n/a\",\"\",CONCATENATE(IF(X74=\"saber\",\"\",\" \"),T74,IF(T74=100,\" (Std) \",IF(T74=87,\" (CE) \",\" \")))),IF(U74=\"n/a\",\"\",CONCATENATE(U74,IF(U74=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X74,3)=\"tip\",IF(LEFT(X74,1)=\"s\",\"\",IF(Z74=\"n\",IF(T74=\"N/A\",\"PG\",\" PG\"),IF(Z74=\"y\",IF(T74=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z74=\"n\",IF(T74=\"N/A\",\"PG\",\" PG\"),IF(Z74=\"y\",IF(T74=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF74=\"y\",\" ZT\",\"\"),IF(V74=\"N\",\"\",IF(S74=\"n/a\",\" ETCH\",IF(T74=\"N/A\",IF(RIGHT(X74,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X74=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"1720 2 in STORZ 30-125 75 BLACK (Std) PG"},{"$f":"A74","v":"17204044"},{"$f":"B74","v":"TBJT 52MM 30-125G@75P"},{"$f":"LEN(AH74)","v":40}]
["17204032","TBJT 38MM 30-125G@100P FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"STORZ","GPM","30-125","PSI","N/A",100,"BLACK","N","ENGLISH","Selectable","1.5\"","N",20,2,"1720","N/A","N/A",null,null,"1720 1.5 in STORZ 30-125 100 (Std) BLACK (Std) PG","17204032","TBJT 38MM 30-125G@100P FM",49]
["17204039","TBJT 2.5BIM 115-475L@7b SPECIAL",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"BIM","LPM","115-475","BAR","N/A",7,"BLACK","Y","ENGLISH","Selectable","1.5\"","N",20,2,"1720","N/A","N/A",null,null,"1720 2.5 in BIM 115-475 7 BLACK (Std) PG ETCH","17204039","TBJT 2.5BIM 115-475L@7b SPECIAL",45]
["17207002","TBJT NPG 1.5NPSH 30-125G@100P FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NPSH","GPM","30-125","PSI","N/A",100,"BLACK","N","ENGLISH","Selectable","1.5\"","Y",20,2,"1720","N/A","N/A",null,null,"1720 1.5 in NPSH 30-125 100 (Std) BLACK (Std) NPG","17207002","TBJT NPG 1.5NPSH 30-125G@100P FM",49]
["17204019","TBJT 1.5NPSH 115-475L@5b",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NPSH","LPM","115-475","BAR","n/a",5,"BLACK","N","ENGLISH","Selectable","1.5\"","N",20,3,"1720","N/A","N/A",null,null,"1720 1.5 in NPSH 115-475 5 BLACK (Std) PG","17204019","TBJT 1.5NPSH 115-475L@5b",41]
["17204020","TBJT 52MM 115-475L@7b GERMAN FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2,"STORZ","LPM","115-475","BAR","N/A",7,"BLACK","N","GERMAN","Selectable","1.5\"","N",20,3,"1720","N/A","N/A",null,null,"1720 2 in STORZ 115-475 7 BLACK (Std) PG","17204020","TBJT 52MM 115-475L@7b GERMAN FM",40]
["17204026","TBJT 38MM 115-475L@7b FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"STORZ","LPM","115-475","BAR","N/A",7,"BLACK","N","ENGLISH","Selectable","1.5\"","N",20,3,"1720","N/A","N/A",null,null,"1720 1.5 in STORZ 115-475 7 BLACK (Std) PG","17204026","TBJT 38MM 115-475L@7b FM",42]
["17204035","TBJT 1.5ABX 30-125G@75P",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"ABX","GPM","30-125","PSI","N/A",75,"BLACK","N","ENGLISH","Selectable","1.5\"","N",20,3,"1720","N/A","N/A",null,null,"1720 1.5 in ABX 30-125 75 BLACK (Std) PG","17204035","TBJT 1.5ABX 30-125G@75P",40]
["17204045","TBJT 2.5BIM 115-475L@5b",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"BIM","LPM","115-475","BAR","N/A",5,"BLACK","N","ENGLISH","Selectable","1.5\"","N",20,2,"1720","N/A","N/A",null,null,{"$f":"CONCATENATE(AC82,\" \",N82,\" in \",O82,\" \",IF(AD82=\"n/a\",\"\",CONCATENATE(AD82,\" in \",AE82,\" \")),IF(Q82=\"n/a\",\"\",Q82),IF(S82=\"n/a\",\"\",CONCATENATE(IF(X82=\"saber\",\" \",\"\"),S82,\" bore size(s) \")),IF(T82=\"n/a\",\"\",CONCATENATE(IF(X82=\"saber\",\"\",\" \"),T82,IF(T82=100,\" (Std) \",IF(T82=87,\" (CE) \",\" \")))),IF(U82=\"n/a\",\"\",CONCATENATE(U82,IF(U82=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X82,3)=\"tip\",IF(LEFT(X82,1)=\"s\",\"\",IF(Z82=\"n\",IF(T82=\"N/A\",\"PG\",\" PG\"),IF(Z82=\"y\",IF(T82=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z82=\"n\",IF(T82=\"N/A\",\"PG\",\" PG\"),IF(Z82=\"y\",IF(T82=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF82=\"y\",\" ZT\",\"\"),IF(V82=\"N\",\"\",IF(S82=\"n/a\",\" ETCH\",IF(T82=\"N/A\",IF(RIGHT(X82,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X82=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"1720 2.5 in BIM 115-475 5 BLACK (Std) PG"},{"$f":"A82","v":"17204045"},{"$f":"B82","v":"TBJT 2.5BIM 115-475L@5b"},{"$f":"LEN(AH82)","v":40}]
["17204040","TBJT 2.5BIM 30-125G@100P FM#",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"BIM","GPM","30-125","PSI","N/A",100,"BLACK","N","ENGLISH","Selectable","1.5\"","N",20,3,"1720","N/A","N/A",null,null,"1720 2.5 in BIM 30-125 100 (Std) BLACK (Std) PG","17204040","TBJT 2.5BIM 30-125G@100P FM#",47]
["17204702","TBJT 2.5BIM 100-450L@6b EN",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"BIM","LPM","100-450","BAR","N/A",6,"BLACK","N","ENGLISH","Selectable","1.5\"","N",20,3,"1720","N/A","N/A",null,null,"1720 2.5 in BIM 100-450 6 BLACK (Std) PG","17204702","TBJT 2.5BIM 100-450L@6b EN",40]
["17207011","TBJT NPG 1.5NH 30-125G@75P",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","30-125","PSI","N/A",75,"BLACK","N","ENGLISH","Selectable","1.5\"","Y",20,3,"1720","N/A","N/A",null,null,"1720 1.5 in NH 30-125 75 BLACK (Std) NPG","17207011","TBJT NPG 1.5NH 30-125G@75P",40]
["17204018","TBJT ZT 1.5NH 30-125G@100P",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","30-125","PSI","N/A",100,"BLACK","N","ENGLISH","Selectable","1.5\"","N",20,4,"1720","N/A","N/A","Y",null,"1720 1.5 in NH 30-125 100 (Std) BLACK (Std) PG ZT","17204018","TBJT ZT 1.5NH 30-125G@100P",49]
["17200711","OBS TBJ NZ1.5BSP100-450L@6bDUTCH SER# BL",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"BSP","LPM","100-450","BAR","N/A",6,"BLUE","N","DUTCH","Selectable","1.5\"","N","No 2021 Sales","No 2021 Sales","1720","N/A","N/A",null,null,"1720 1.5 in BSP 100-450 6 BLUE PG","17200711","OBS TBJ NZ1.5BSP100-450L@6bDUTCH SER# BL",33]
["17204017","TBJT 1.5BIM 115-475L@7b FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"BIM","LPM","115-475","BAR","N/A",7,"BLACK","N","ENGLISH","Selectable","1.5\"","N","No 2021 Sales","No 2021 Sales","1720","N/A","N/A",null,null,"1720 1.5 in BIM 115-475 7 BLACK (Std) PG","17204017","TBJT 1.5BIM 115-475L@7b FM",40]
["17204024","TBJT ZT 2.5NH 30-125G@100P",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"NH","GPM","30-125","PSI","n/a",100,"BLACK","N","ENGLISH","Selectable","1.5\"","N","No 2021 Sales","No 2021 Sales","1720","N/A","N/A","Y",null,"1720 2.5 in NH 30-125 100 (Std) BLACK (Std) PG ZT","17204024","TBJT ZT 2.5NH 30-125G@100P",49]
["17204027","TBJT 52MM 30-125G@100P FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2,"STORZ","GPM","30-125","PSI","n/a",100,"BLACK","N","ENGLISH","Selectable","1.5\"","N","No 2021 Sales","No 2021 Sales","1720","N/A","N/A",null,null,"1720 2 in STORZ 30-125 100 (Std) BLACK (Std) PG","17204027","TBJT 52MM 30-125G@100P FM",47]
["17204028","TBJT ZT 1.5BIM 100-450L@6b",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"BIM","LPM","100-450","BAR","N/A",6,"BLACK","N","ENGLISH","Selectable","1.5\"","N","No 2021 Sales","No 2021 Sales","1720","N/A","N/A","Y",null,"1720 1.5 in BIM 100-450 6 BLACK (Std) PG ZT","17204028","TBJT ZT 1.5BIM 100-450L@6b",43]
["17204029","TBJT ZT 1.5BSP 100-450L@6b",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"BSP","LPM","100-450","BAR","N/A",6,"BLACK","N","ENGLISH","Selectable","1.5\"","N","No 2021 Sales","No 2021 Sales","1720","N/A","N/A","Y",null,"1720 1.5 in BSP 100-450 6 BLACK (Std) PG ZT","17204029","TBJT ZT 1.5BSP 100-450L@6b",43]
["17204031","TBJT ZT 1.5NH 30-125G@ 75P",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","30-125","PSI","n/a",75,"BLACK","N","ENGLISH","Selectable","1.5\"","N","No 2021 Sales","No 2021 Sales","1720","N/A","N/A","Y",null,"1720 1.5 in NH 30-125 75 BLACK (Std) PG ZT","17204031","TBJT ZT 1.5NH 30-125G@ 75P",42]
["17204036","TBJT ZT 2.5BIM 100-450L@6b",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"BIM","LPM","100-450","BAR","N/A",6,"BLACK","N","ENGLISH","Selectable","1.5\"","N","No 2021 Sales","No 2021 Sales","1720","N/A","N/A","Y",null,"1720 2.5 in BIM 100-450 6 BLACK (Std) PG ZT","17204036","TBJT ZT 2.5BIM 100-450L@6b",43]
["17204041","TBJT ZT 1.5NPSH 30-125G@100P",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NPSH","GPM","30-125","PSI","N/A",100,"BLACK","N","ENGLISH","Selectable","1.5\"","N","No 2021 Sales","No 2021 Sales","1720","N/A","N/A","Y",null,"1720 1.5 in NPSH 30-125 100 (Std) BLACK (Std) PG ZT","17204041","TBJT ZT 1.5NPSH 30-125G@100P",51]
["17204042","TBJT 1.5NH 30-125G@100P YLWBMPR FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","30-125","PSI","N/A",100,"YELLOW","N","ENGLISH","Selectable","1.5\"","N","No 2021 Sales","No 2021 Sales","1720","N/A","N/A",null,null,"1720 1.5 in NH 30-125 100 (Std) YELLOW PG","17204042","TBJT 1.5NH 30-125G@100P YLWBMPR FM",41]
["17204701","TBJT 1.5BSP 100-450L@6b EN",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"BSP","LPM","100-450","BAR","N/A",6,"BLACK","N","ENGLISH","Selectable","1.5\"","N","No 2021 Sales","No 2021 Sales","1720","N/A","N/A",null,null,"1720 1.5 in BSP 100-450 6 BLACK (Std) PG","17204701","TBJT 1.5BSP 100-450L@6b EN",40]
["17207021","TBJT NPG 1.5BSP 115-475L@7b SPANISH FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"BSP","LPM","115-475","BAR","N/A",7,"BLACK","N","SPANISH","Selectable","1.5\"","Y","No 2021 Sales","No 2021 Sales","1720","N/A","N/A",null,null,{"$f":"CONCATENATE(AC98,\" \",N98,\" in \",O98,\" \",IF(AD98=\"n/a\",\"\",CONCATENATE(AD98,\" in \",AE98,\" \")),IF(Q98=\"n/a\",\"\",Q98),IF(S98=\"n/a\",\"\",CONCATENATE(IF(X98=\"saber\",\" \",\"\"),S98,\" bore size(s) \")),IF(T98=\"n/a\",\"\",CONCATENATE(IF(X98=\"saber\",\"\",\" \"),T98,IF(T98=100,\" (Std) \",IF(T98=87,\" (CE) \",\" \")))),IF(U98=\"n/a\",\"\",CONCATENATE(U98,IF(U98=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X98,3)=\"tip\",IF(LEFT(X98,1)=\"s\",\"\",IF(Z98=\"n\",IF(T98=\"N/A\",\"PG\",\" PG\"),IF(Z98=\"y\",IF(T98=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z98=\"n\",IF(T98=\"N/A\",\"PG\",\" PG\"),IF(Z98=\"y\",IF(T98=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF98=\"y\",\" ZT\",\"\"),IF(V98=\"N\",\"\",IF(S98=\"n/a\",\" ETCH\",IF(T98=\"N/A\",IF(RIGHT(X98,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X98=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"1720 1.5 in BSP 115-475 7 BLACK (Std) NPG"},{"$f":"A98","v":"17207021"},{"$f":"B98","v":"TBJT NPG 1.5BSP 115-475L@7b SPANISH FM"},{"$f":"LEN(AH98)","v":41}]
["17204049","TBJT 1.5NH 115-475L@5b",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","LPM","115-475","BAR","N/A",5,"BLACK","N","ENGLISH","Selectable","1.5\"","N","No 2021 Sales","No 2021 Sales","1720","N/A","N/A",null,null,"1720 1.5 in NH 115-475 5 BLACK (Std) PG","17204049","TBJT 1.5NH 115-475L@5b",39]
["17234001","TBJT 1.5NH 95-200G@100P#",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","95-200","PSI","n/a",100,"BLACK","N","ENGLISH","Selectable","Mid-Range","N",80,1,"1723","N/A","N/A",null,null,"1723 1.5 in NH 95-200 100 (Std) BLACK (Std) PG","17234001","TBJT 1.5NH 95-200G@100P#",46]
["17234002","TBJT 1.5NH 95-200G@75P",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","95-200","PSI","n/a",75,"BLACK","N","ENGLISH","Selectable","Mid-Range","N",80,1,"1723","N/A","N/A",null,null,"1723 1.5 in NH 95-200 75 BLACK (Std) PG","17234002","TBJT 1.5NH 95-200G@75P",39]
["17234010","TBJT 2.5BIM 360-750L@7b",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"BIM","LPM","360-750","BAR","N/A",7,"BLACK","N","ENGLISH","Selectable","Mid-Range","N",80,1,"1723","N/A","N/A",null,null,"1723 2.5 in BIM 360-750 7 BLACK (Std) PG","17234010","TBJT 2.5BIM 360-750L@7b",40]
["17234025","TBJT 2.5NH 95-200G@75P",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"NH","GPM","95-200","PSI","N/A",75,"BLACK","N","ENGLISH","Selectable","Mid-Range","N",20,1,"1723","N/A","N/A",null,null,"1723 2.5 in NH 95-200 75 BLACK (Std) PG","17234025","TBJT 2.5NH 95-200G@75P",39]
["17237002","TBJT NPG 1.5NH 95-200G@100P#",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","95-200","PSI","n/a",100,"BLACK","N","ENGLISH","Selectable","Mid-Range","Y",20,1,"1723","N/A","N/A",null,null,"1723 1.5 in NH 95-200 100 (Std) BLACK (Std) NPG","17237002","TBJT NPG 1.5NH 95-200G@100P#",47]
["17234003","TBJT 1.5NPSH 95-200G@100P",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NPSH","GPM","95-200","PSI","n/a",100,"BLACK","N","ENGLISH","Selectable","Mid-Range","N",20,2,"1723","N/A","N/A",null,null,"1723 1.5 in NPSH 95-200 100 (Std) BLACK (Std) PG","17234003","TBJT 1.5NPSH 95-200G@100P",48]
["17234008","TBJT 1.5NPSH 95-200G@75P",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NPSH","GPM","95-200","PSI","n/a",75,"BLACK","N","ENGLISH","Selectable","Mid-Range","N",20,2,"1723","N/A","N/A",null,null,"1723 1.5 in NPSH 95-200 75 BLACK (Std) PG","17234008","TBJT 1.5NPSH 95-200G@75P",41]
["17234012","TBJT 1.5NH 95-200G@100P ORGBMPR",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","95-200","PSI","n/a",100,"ORANGE","N","ENGLISH","Selectable","Mid-Range","N",20,2,"1723","N/A","N/A",null,null,"1723 1.5 in NH 95-200 100 (Std) ORANGE PG","17234012","TBJT 1.5NH 95-200G@100P ORGBMPR",41]
["17234020","TBJT 1.5NH 95-200G@100P GRNBMPR",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","95-200","PSI","N/A",100,"GREEN","N","ENGLISH","Selectable","Mid-Range","N",20,2,"1723","N/A","N/A",null,null,"1723 1.5 in NH 95-200 100 (Std) GREEN PG","17234020","TBJT 1.5NH 95-200G@100P GRNBMPR",40]
["17234021","TBJT ZT 1.5NH 95-200G@100P",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","95-200","PSI","N/A",100,"BLACK","N","ENGLISH","Selectable","Mid-Range","N",20,2,"1723","N/A","N/A","Y",null,"1723 1.5 in NH 95-200 100 (Std) BLACK (Std) PG ZT","17234021","TBJT ZT 1.5NH 95-200G@100P",49]
["17234026","TBJT 1.5NH 95-200G@75P MT. PLEASANT",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","95-200","PSI","N/A",75,"BLACK","Y","ENGLISH","Selectable","Mid-Range","N",20,2,"1723","N/A","N/A",null,null,"1723 1.5 in NH 95-200 75 BLACK (Std) PG ETCH","17234026","TBJT 1.5NH 95-200G@75P MT. PLEASANT",44]
["17234027","TBJT 1.5NH 95-200G@75P RED BANKS",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","95-200","PSI","N/A",75,"BLACK","Y","ENGLISH","Selectable","Mid-Range","N",20,2,"1723","N/A","N/A",null,null,"1723 1.5 in NH 95-200 75 BLACK (Std) PG ETCH","17234027","TBJT 1.5NH 95-200G@75P RED BANKS",44]
["17234028","TBJT 1.5NH 95-200G@75P VICTORIA",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","95-200","PSI","N/A",75,"BLACK","Y","ENGLISH","Selectable","Mid-Range","N",20,2,"1723","N/A","N/A",null,null,"1723 1.5 in NH 95-200 75 BLACK (Std) PG ETCH","17234028","TBJT 1.5NH 95-200G@75P VICTORIA",44]
["17234029","TBJT 1.5NH 95-200G@75P WATSON",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","95-200","PSI","N/A",75,"BLACK","Y","ENGLISH","Selectable","Mid-Range","N",20,2,"1723","N/A","N/A",null,null,"1723 1.5 in NH 95-200 75 BLACK (Std) PG ETCH","17234029","TBJT 1.5NH 95-200G@75P WATSON",44]
["17237004","TBJT NPG 1.5NH 95-200G@100P REDBMPR",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","95-200","PSI","N/A",100,"RED","N","ENGLISH","Selectable","Mid-Range","Y",20,2,"1723","N/A","N/A",null,null,"1723 1.5 in NH 95-200 100 (Std) RED NPG","17237004","TBJT NPG 1.5NH 95-200G@100P REDBMPR",39]
["17234009","TBJT 1.5BSP 360-750L@7b",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"BSP","LPM","360-750","BAR","N/A",7,"BLACK","N","ENGLISH","Selectable","Mid-Range","N",20,3,"1723","N/A","N/A",null,null,"1723 1.5 in BSP 360-750 7 BLACK (Std) PG","17234009","TBJT 1.5BSP 360-750L@7b",40]
["17234022","TBJT 2.5AJD 95-200G@100P",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"AJD","GPM","95-200","PSI","N/A",100,"BLACK","N","ENGLISH","Selectable","Mid-Range","N",20,3,"1723","N/A","N/A",null,null,"1723 2.5 in AJD 95-200 100 (Std) BLACK (Std) PG","17234022","TBJT 2.5AJD 95-200G@100P",47]
["17234024","TBJT 2.5NH 95-200G@75P",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"NH","GPM","95-200","PSI","N/A",75,"BLACK","N","ENGLISH","Selectable","Mid-Range","N",20,3,"1723","N/A","N/A",null,null,"1723 2.5 in NH 95-200 75 BLACK (Std) PG","17234024","TBJT 2.5NH 95-200G@75P",39]
["17237001","TBJT NPG 1.5NH 95-200G@75P",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","95-200","PSI","n/a",75,"BLACK","N","ENGLISH","Selectable","Mid-Range","Y",20,3,"1723","N/A","N/A",null,null,"1723 1.5 in NH 95-200 75 BLACK (Std) NPG","17237001","TBJT NPG 1.5NH 95-200G@75P",40]
["17234005","TBJT 1.5NH 95-200G@100P REDBMPR",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","95-200","PSI","n/a",100,"RED","N","ENGLISH","Selectable","Mid-Range","N","No 2021 Sales","No 2021 Sales","1723","N/A","N/A",null,null,"1723 1.5 in NH 95-200 100 (Std) RED PG","17234005","TBJT 1.5NH 95-200G@100P REDBMPR",38]
["17234006","TBJT 1.5NH 95-200G@75P YLWBMPR",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","95-200","PSI","n/a",75,"YELLOW","N","ENGLISH","Selectable","Mid-Range","N","No 2021 Sales","No 2021 Sales","1723","N/A","N/A",null,null,"1723 1.5 in NH 95-200 75 YELLOW PG","17234006","TBJT 1.5NH 95-200G@75P YLWBMPR",34]
["17234011","TBJT 75MM 360-750L@7b",null,null,null,null,null,null,null,null,"0001","Turbojet","A",3,"STORZ","LPM","360-750","BAR","N/A",7,"BLACK","N","ENGLISH","Selectable","Mid-Range","N","No 2021 Sales","No 2021 Sales","1723","N/A","N/A",null,null,"1723 3 in STORZ 360-750 7 BLACK (Std) PG","17234011","TBJT 75MM 360-750L@7b",40]
["17234013","TBJT 1.5NPSH 360-750L@700K",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NPSH","LPM","360-750","kPa","n/a",700,"BLACK","N","ENGLISH","Selectable","Mid-Range","N","No 2021 Sales","No 2021 Sales","1723","N/A","N/A",null,null,"1723 1.5 in NPSH 360-750 700 BLACK (Std) PG","17234013","TBJT 1.5NPSH 360-750L@700K",43]
["17234014","TBJT ZT 1.5BSP 360-750L@7b",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"BSP","LPM","360-750","BAR","N/A",7,"BLACK","N","ENGLISH","Selectable","Mid-Range","N","No 2021 Sales","No 2021 Sales","1723","N/A","N/A","Y",null,"1723 1.5 in BSP 360-750 7 BLACK (Std) PG ZT","17234014","TBJT ZT 1.5BSP 360-750L@7b",43]
["17234015","TBJT 1.5NH 95-200G@100P YLWBMPR",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","95-200","PSI","n/a",100,"YELLOW","N","ENGLISH","Selectable","Mid-Range","N","No 2021 Sales","No 2021 Sales","1723","N/A","N/A",null,null,"1723 1.5 in NH 95-200 100 (Std) YELLOW PG","17234015","TBJT 1.5NH 95-200G@100P YLWBMPR",41]
["17234016","TBJT 1.5ABX 95-200G@100P",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"ABX","GPM","95-200","PSI","n/a",100,"BLACK","N","ENGLISH","Selectable","Mid-Range","N","No 2021 Sales","No 2021 Sales","1723","N/A","N/A",null,null,"1723 1.5 in ABX 95-200 100 (Std) BLACK (Std) PG","17234016","TBJT 1.5ABX 95-200G@100P",47]
["17234017","TBJT 1.5NH 95-200G@75P REDBMPR",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","95-200","PSI","n/a",75,"RED","N","ENGLISH","Selectable","Mid-Range","N","No 2021 Sales","No 2021 Sales","1723","N/A","N/A",null,null,"1723 1.5 in NH 95-200 75 RED PG","17234017","TBJT 1.5NH 95-200G@75P REDBMPR",31]
["17234018","TBJT 52MM 95-200G@100P",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"STORZ","GPM","95-200","PSI","n/a",100,"BLACK","N","ENGLISH","Selectable","Mid-Range","N","No 2021 Sales","No 2021 Sales","1723","N/A","N/A",null,null,"1723 2.5 in STORZ 95-200 100 (Std) BLACK (Std) PG","17234018","TBJT 52MM 95-200G@100P",49]
["17234019","TBJT 1.5NH 95-200G@100P ORGBMPR",null,null,null,null,null,null,null,null,"0001","Turbojet","O",1.5,"NH","GPM","95-200","PSI","n/a",100,"ORANGE","N","ENGLISH","Selectable","Mid-Range","N","No 2021 Sales","No 2021 Sales","1723","N/A","N/A",null,null,"1723 1.5 in NH 95-200 100 (Std) ORANGE PG","17234019","TBJT 1.5NH 95-200G@100P ORGBMPR",41]
["17234023","TBJT ZT 1.5NPSH 95-200G@100P",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NPSH","GPM","95-200","PSI","N/A",100,"BLACK","N","ENGLISH","Selectable","Mid-Range","N","No 2021 Sales","No 2021 Sales","1723","N/A","N/A","Y",null,"1723 1.5 in NPSH 95-200 100 (Std) BLACK (Std) PG ZT","17234023","TBJT ZT 1.5NPSH 95-200G@100P",51]
["17237003","TBJT NPG 1.5NPSH 95-200G@100P",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NPSH","GPM","95-200","PSI","n/a",100,"BLACK","N","ENGLISH","Selectable","Mid-Range","Y","No 2021 Sales","No 2021 Sales","1723","N/A","N/A",null,null,"1723 1.5 in NPSH 95-200 100 (Std) BLACK (Std) NPG","17237003","TBJT NPG 1.5NPSH 95-200G@100P",49]
["17270700","TBJT TIP 2.5W/1.5BSP 500-950L EN 15767**",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"BSP","LPM","500-950","BAR","N/A",6,"BLACK","N","ENGLISH","Selectable Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","1727","N/A","N/A",null,null,"1727 1.5 in BSP 500-950 6 BLACK (Std)","17270700","TBJT TIP 2.5W/1.5BSP 500-950L EN 15767**",37]
["17334002","TBJT 2.5NH 125-250G@100P FM#",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"NH","GPM","125-250","PSI","N/A",100,"BLACK","N","ENGLISH","Selectable","High-Range","N",80,1,"1733","N/A","N/A",null,null,"1733 2.5 in NH 125-250 100 (Std) BLACK (Std) PG","17334002","TBJT 2.5NH 125-250G@100P FM#",47]
["17334006","TBJT 2.5BIM 475-950L@7b FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"BIM","LPM","475-950","BAR","N/A",7,"BLACK","N","ENGLISH","Selectable","High-Range","N",80,1,"1733","N/A","N/A",null,null,"1733 2.5 in BIM 475-950 7 BLACK (Std) PG","17334006","TBJT 2.5BIM 475-950L@7b FM",40]
["17334007","TBJT 2.5NH 125-250G@75P",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"NH","GPM","125-250","PSI","N/A",100,"BLACK","N","ENGLISH","Selectable","High-Range","N",80,1,"1733","N/A","N/A",null,null,"1733 2.5 in NH 125-250 100 (Std) BLACK (Std) PG","17334007","TBJT 2.5NH 125-250G@75P",47]
["17334021","TBJT 2.5BSP 475-950L@7b FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"BSP","LPM","475-950","BAR","N/A",7,"BLACK","N","ENGLISH","Selectable","High-Range","N",80,1,"1733","N/A","N/A",null,null,"1733 2.5 in BSP 475-950 7 BLACK (Std) PG","17334021","TBJT 2.5BSP 475-950L@7b FM",40]
["17334028","TBJT 2.5NH125-250G@100P SEQ ETCH APPLING",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"NH","GPM","125-250","PSI","N/A",100,"BLACK","Y","ENGLISH","Selectable","High-Range","N",20,1,"1733","N/A","N/A",null,null,"1733 2.5 in NH 125-250 100 (Std) BLACK (Std) PG ETCH","17334028","TBJT 2.5NH125-250G@100P SEQ ETCH APPLING",52]
["17337001","TBJT NPG 2.5NH 125-250G@100P FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"NH","GPM","125-250","PSI","N/A",100,"BLACK","N","ENGLISH","Selectable","High-Range","Y",20,1,"1733","N/A","N/A",null,null,"1733 2.5 in NH 125-250 100 (Std) BLACK (Std) NPG","17337001","TBJT NPG 2.5NH 125-250G@100P FM",48]
["17337008","TBJT NPG 65MM 475-950L@7b FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"STORZ","LPM","475-950","BAR","N/A",7,"BLACK","N","ENGLISH","Selectable","High-Range","Y",20,1,"1733","N/A","N/A",null,null,{"$f":"CONCATENATE(AC138,\" \",N138,\" in \",O138,\" \",IF(AD138=\"n/a\",\"\",CONCATENATE(AD138,\" in \",AE138,\" \")),IF(Q138=\"n/a\",\"\",Q138),IF(S138=\"n/a\",\"\",CONCATENATE(IF(X138=\"saber\",\" \",\"\"),S138,\" bore size(s) \")),IF(T138=\"n/a\",\"\",CONCATENATE(IF(X138=\"saber\",\"\",\" \"),T138,IF(T138=100,\" (Std) \",IF(T138=87,\" (CE) \",\" \")))),IF(U138=\"n/a\",\"\",CONCATENATE(U138,IF(U138=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X138,3)=\"tip\",IF(LEFT(X138,1)=\"s\",\"\",IF(Z138=\"n\",IF(T138=\"N/A\",\"PG\",\" PG\"),IF(Z138=\"y\",IF(T138=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z138=\"n\",IF(T138=\"N/A\",\"PG\",\" PG\"),IF(Z138=\"y\",IF(T138=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF138=\"y\",\" ZT\",\"\"),IF(V138=\"N\",\"\",IF(S138=\"n/a\",\" ETCH\",IF(T138=\"N/A\",IF(RIGHT(X138,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X138=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"1733 2.5 in STORZ 475-950 7 BLACK (Std) NPG"},{"$f":"A138","v":"17337008"},{"$f":"B138","v":"TBJT NPG 65MM 475-950L@7b FM"},{"$f":"LEN(AH138)","v":43}]
["17337019","TBJT NPG 2.5AEF 125-250G@100P FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"AEF","GPM","125-250","PSI","N/A",100,"BLACK","N","ENGLISH","Selectable","High-Range","Y",20,1,"1733","N/A","N/A",null,null,"1733 2.5 in AEF 125-250 100 (Std) BLACK (Std) NPG","17337019","TBJT NPG 2.5AEF 125-250G@100P FM",49]
["17334005","TBJT 75MM 475-950L@7b FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",3,"STORZ","LPM","475-950","BAR","N/A",7,"BLACK","N","ENGLISH","Selectable","High-Range","N",20,2,"1733","N/A","N/A",null,null,"1733 3 in STORZ 475-950 7 BLACK (Std) PG","17334005","TBJT 75MM 475-950L@7b FM",40]
["17334009","TBJT 2.5BAF 125-250G@100P FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"BAT","GPM","125-250","PSI","N/A",100,"BLACK","N","ENGLISH","Selectable","High-Range","N",20,2,"1733","N/A","N/A",null,null,"1733 2.5 in BAT 125-250 100 (Std) BLACK (Std) PG","17334009","TBJT 2.5BAF 125-250G@100P FM",48]
["17334010","TBJT 2.5AII 125-250G@100P FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"CSA","GPM","125-250","PSI","N/A",100,"BLACK","N","ENGLISH","Selectable","High-Range","N",20,2,"1733","N/A","N/A",null,null,"1733 2.5 in CSA 125-250 100 (Std) BLACK (Std) PG","17334010","TBJT 2.5AII 125-250G@100P FM",48]
["17334011","TBJT ZT 2.5NH 125-250G@100P",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"NH","GPM","125-250","PSI","N/A",100,"BLACK","N","ENGLISH","Selectable","High-Range","N",20,2,"1733","N/A","N/A","Y",null,"1733 2.5 in NH 125-250 100 (Std) BLACK (Std) PG ZT","17334011","TBJT ZT 2.5NH 125-250G@100P",50]
["17334014","TBJT ZT 2.5BIM 475-950L@7b",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"BIM","LPM","475-950","BAR","N/A",7,"BLACK","N","ENGLISH","Selectable","High-Range","N",20,2,"1733","N/A","N/A","Y",null,"1733 2.5 in BIM 475-950 7 BLACK (Std) PG ZT","17334014","TBJT ZT 2.5BIM 475-950L@7b",43]
["17334042","TBJT ZT 65MM 475-950L@7b",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"STORZ","LPM","475-950","BAR","N/A",7,"BLACK","N","ENGLISH","Selectable","High-Range","N",20,2,"1733","N/A","N/A","Y",null,{"$f":"CONCATENATE(AC145,\" \",N145,\" in \",O145,\" \",IF(AD145=\"n/a\",\"\",CONCATENATE(AD145,\" in \",AE145,\" \")),IF(Q145=\"n/a\",\"\",Q145),IF(S145=\"n/a\",\"\",CONCATENATE(IF(X145=\"saber\",\" \",\"\"),S145,\" bore size(s) \")),IF(T145=\"n/a\",\"\",CONCATENATE(IF(X145=\"saber\",\"\",\" \"),T145,IF(T145=100,\" (Std) \",IF(T145=87,\" (CE) \",\" \")))),IF(U145=\"n/a\",\"\",CONCATENATE(U145,IF(U145=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X145,3)=\"tip\",IF(LEFT(X145,1)=\"s\",\"\",IF(Z145=\"n\",IF(T145=\"N/A\",\"PG\",\" PG\"),IF(Z145=\"y\",IF(T145=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z145=\"n\",IF(T145=\"N/A\",\"PG\",\" PG\"),IF(Z145=\"y\",IF(T145=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF145=\"y\",\" ZT\",\"\"),IF(V145=\"N\",\"\",IF(S145=\"n/a\",\" ETCH\",IF(T145=\"N/A\",IF(RIGHT(X145,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X145=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"1733 2.5 in STORZ 475-950 7 BLACK (Std) PG ZT"},{"$f":"A145","v":"17334042"},{"$f":"B145","v":"TBJT ZT 65MM 475-950L@7b"},{"$f":"LEN(AH145)","v":45}]
["17334015","TBJT 2.5AKB 125-250G@100P FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"AKB","GPM","125-250","PSI","N/A",100,"BLACK","N","ENGLISH","Selectable","High-Range","N",20,2,"1733","N/A","N/A",null,null,"1733 2.5 in AKB 125-250 100 (Std) BLACK (Std) PG","17334015","TBJT 2.5AKB 125-250G@100P FM",48]
["17334017","TBJT 2.5NH 125-250G@100P ORGBMPR FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"NH","GPM","125-250","PSI","n/a",100,"ORANGE","N","ENGLISH","Selectable","High-Range","N",20,2,"1733","N/A","N/A",null,null,"1733 2.5 in NH 125-250 100 (Std) ORANGE PG","17334017","TBJT 2.5NH 125-250G@100P ORGBMPR FM",42]
["17334019","TBJT 2.5AEF 125-250G@100P FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"NYCORP","GPM","125-250","PSI","n/a",100,"BLACK","N","ENGLISH","Selectable","High-Range","N",20,2,"1733","N/A","N/A",null,null,"1733 2.5 in NYCORP 125-250 100 (Std) BLACK (Std) PG","17334019","TBJT 2.5AEF 125-250G@100P FM",51]
["17334043","TBJT 2.5AHY 125-250G@75P",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"AHY","GPM","125-250","PSI","n/a",75,"BLACK","N","ENGLISH","Selectable","High-Range","N",20,2,"1733","N/A","N/A",null,null,{"$f":"CONCATENATE(AC149,\" \",N149,\" in \",O149,\" \",IF(AD149=\"n/a\",\"\",CONCATENATE(AD149,\" in \",AE149,\" \")),IF(Q149=\"n/a\",\"\",Q149),IF(S149=\"n/a\",\"\",CONCATENATE(IF(X149=\"saber\",\" \",\"\"),S149,\" bore size(s) \")),IF(T149=\"n/a\",\"\",CONCATENATE(IF(X149=\"saber\",\"\",\" \"),T149,IF(T149=100,\" (Std) \",IF(T149=87,\" (CE) \",\" \")))),IF(U149=\"n/a\",\"\",CONCATENATE(U149,IF(U149=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X149,3)=\"tip\",IF(LEFT(X149,1)=\"s\",\"\",IF(Z149=\"n\",IF(T149=\"N/A\",\"PG\",\" PG\"),IF(Z149=\"y\",IF(T149=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z149=\"n\",IF(T149=\"N/A\",\"PG\",\" PG\"),IF(Z149=\"y\",IF(T149=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF149=\"y\",\" ZT\",\"\"),IF(V149=\"N\",\"\",IF(S149=\"n/a\",\" ETCH\",IF(T149=\"N/A\",IF(RIGHT(X149,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X149=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"1733 2.5 in AHY 125-250 75 BLACK (Std) PG"},{"$f":"A149","v":"17334043"},{"$f":"B149","v":"TBJT 2.5AHY 125-250G@75P"},{"$f":"LEN(AH149)","v":41}]
["17334044","TBJT 2.5NH 125-250G@75P REDBMPR",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"NH","GPM","125-250","PSI","n/a",75,"RED","N","ENGLISH","Selectable","High-Range","N",20,2,"1733","N/A","N/A",null,null,{"$f":"CONCATENATE(AC150,\" \",N150,\" in \",O150,\" \",IF(AD150=\"n/a\",\"\",CONCATENATE(AD150,\" in \",AE150,\" \")),IF(Q150=\"n/a\",\"\",Q150),IF(S150=\"n/a\",\"\",CONCATENATE(IF(X150=\"saber\",\" \",\"\"),S150,\" bore size(s) \")),IF(T150=\"n/a\",\"\",CONCATENATE(IF(X150=\"saber\",\"\",\" \"),T150,IF(T150=100,\" (Std) \",IF(T150=87,\" (CE) \",\" \")))),IF(U150=\"n/a\",\"\",CONCATENATE(U150,IF(U150=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X150,3)=\"tip\",IF(LEFT(X150,1)=\"s\",\"\",IF(Z150=\"n\",IF(T150=\"N/A\",\"PG\",\" PG\"),IF(Z150=\"y\",IF(T150=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z150=\"n\",IF(T150=\"N/A\",\"PG\",\" PG\"),IF(Z150=\"y\",IF(T150=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF150=\"y\",\" ZT\",\"\"),IF(V150=\"N\",\"\",IF(S150=\"n/a\",\" ETCH\",IF(T150=\"N/A\",IF(RIGHT(X150,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X150=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"1733 2.5 in NH 125-250 75 RED PG"},{"$f":"A150","v":"17334044"},{"$f":"B150","v":"TBJT 2.5NH 125-250G@75P REDBMPR"},{"$f":"LEN(AH150)","v":32}]
["17334045","TBJT 2.5NH 125-250G@75P YLWBMPR",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"NH","GPM","125-250","PSI","n/a",75,"YELLOW","N","ENGLISH","Selectable","High-Range","N",20,2,"1733","N/A","N/A",null,null,"1733 2.5 in NH 125-250 75 YELLOW PG","17334045","TBJT 2.5NH 125-250G@75P YLWBMPR",35]
["17334023","TBJT 2.5BAF 125-250G@75P",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"BAT","GPM","125-250","PSI","n/a",75,"BLACK","N","ENGLISH","Selectable","High-Range","N",20,2,"1733","N/A","N/A",null,null,"1733 2.5 in BAT 125-250 75 BLACK (Std) PG","17334023","TBJT 2.5BAF 125-250G@75P",41]
["17334027","TBJT ZT 2.5BAF 125-250G@100P",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"BAT","GPM","125-250","PSI","N/A",100,"BLACK","N","ENGLISH","Selectable","High-Range","N",20,2,"1733","N/A","N/A","Y",null,"1733 2.5 in BAT 125-250 100 (Std) BLACK (Std) PG ZT","17334027","TBJT ZT 2.5BAF 125-250G@100P",51]
["17334029","TBJT 2.5NH125-250G@100P SEQ ETCH STA 1-8",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"NH","GPM","125-250","PSI","N/A",100,"BLACK","Y","ENGLISH","Selectable","High-Range","N",20,2,"1733","N/A","N/A",null,null,"1733 2.5 in NH 125-250 100 (Std) BLACK (Std) PG ETCH","17334029","TBJT 2.5NH125-250G@100P SEQ ETCH STA 1-8",52]
["17334030","TBJT 2.5BAF 475-900L@7b/700K FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"BAT","LPM","475-900","BAR","N/A",7,"BLACK","N","ENGLISH","Selectable","High-Range","N",20,2,"1733","N/A","N/A",null,null,"1733 2.5 in BAT 475-900 7 BLACK (Std) PG","17334030","TBJT 2.5BAF 475-900L@7b/700K FM",40]
["17334040","TBJT 2.5AJE 125-250G@100P FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"AJE","GPM","125-250","PSI","N/A",100,"BLACK","N","ENGLISH","Selectable","High-Range","N",20,2,"1733","N/A","N/A",null,null,{"$f":"CONCATENATE(AC156,\" \",N156,\" in \",O156,\" \",IF(AD156=\"n/a\",\"\",CONCATENATE(AD156,\" in \",AE156,\" \")),IF(Q156=\"n/a\",\"\",Q156),IF(S156=\"n/a\",\"\",CONCATENATE(IF(X156=\"saber\",\" \",\"\"),S156,\" bore size(s) \")),IF(T156=\"n/a\",\"\",CONCATENATE(IF(X156=\"saber\",\"\",\" \"),T156,IF(T156=100,\" (Std) \",IF(T156=87,\" (CE) \",\" \")))),IF(U156=\"n/a\",\"\",CONCATENATE(U156,IF(U156=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X156,3)=\"tip\",IF(LEFT(X156,1)=\"s\",\"\",IF(Z156=\"n\",IF(T156=\"N/A\",\"PG\",\" PG\"),IF(Z156=\"y\",IF(T156=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z156=\"n\",IF(T156=\"N/A\",\"PG\",\" PG\"),IF(Z156=\"y\",IF(T156=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF156=\"y\",\" ZT\",\"\"),IF(V156=\"N\",\"\",IF(S156=\"n/a\",\" ETCH\",IF(T156=\"N/A\",IF(RIGHT(X156,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X156=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"1733 2.5 in AJE 125-250 100 (Std) BLACK (Std) PG"},{"$f":"A156","v":"17334040"},{"$f":"B156","v":"TBJT 2.5AJE 125-250G@100P FM"},{"$f":"LEN(AH156)","v":48}]
["17334041","TBJT 2.5AJN 125-250G@100P FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"AJN","GPM","125-250","PSI","N/A",100,"BLACK","N","ENGLISH","Selectable","High-Range","N",20,2,"1733","N/A","N/A",null,null,"1733 2.5 in AJN 125-250 100 (Std) BLACK (Std) PG","17334041","TBJT 2.5AJN 125-250G@100P FM",48]
["17334032","TBJT 2.5AFD 125-250G@100P FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"QST","GPM","125-250","PSI","N/A",100,"BLACK","N","ENGLISH","Selectable","High-Range","N",20,2,"1733","N/A","N/A",null,null,"1733 2.5 in QST 125-250 100 (Std) BLACK (Std) PG","17334032","TBJT 2.5AFD 125-250G@100P FM",48]
["17334034","TBJT 2.5AGA 125-250G@100P FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"AGA","GPM","125-250","PSI","n/a",100,"BLACK","N","ENGLISH","Selectable","High-Range","N",20,2,"1733","N/A","N/A",null,null,"1733 2.5 in AGA 125-250 100 (Std) BLACK (Std) PG","17334034","TBJT 2.5AGA 125-250G@100P FM",48]
["17334031","TBJT 2.5AKA 125-250G@100P FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"AKA","GPM","125-250","PSI","N/A",100,"BLACK","N","ENGLISH","Selectable","High-Range","N",20,3,"1733","N/A","N/A",null,null,"1733 2.5 in AKA 125-250 100 (Std) BLACK (Std) PG","17334031","TBJT 2.5AKA 125-250G@100P FM",48]
["17334033","TBJT 2.5AHQ 125-250G@100P",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"AHQ","GPM","125-250","PSI","n/a",100,"BLACK","N","ENGLISH","Selectable","High-Range","N",20,3,"1733","N/A","N/A",null,null,"1733 2.5 in AHQ 125-250 100 (Std) BLACK (Std) PG","17334033","TBJT 2.5AHQ 125-250G@100P",48]
["17334035","TBJT 2.5NH 125-250G@75P MT.PLEASANT",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"NH","GPM","125-250","PSI","N/A",75,"BLACK","Y","ENGLISH","Selectable","High-Range","N",20,3,"1733","N/A","N/A",null,null,"1733 2.5 in NH 125-250 75 BLACK (Std) PG ETCH","17334035","TBJT 2.5NH 125-250G@75P MT.PLEASANT",45]
["17334036","TBJT 2.5NH 125-250G@75P RED BANKS",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"NH","GPM","125-250","PSI","N/A",75,"BLACK","Y","ENGLISH","Selectable","High-Range","N",20,3,"1733","N/A","N/A",null,null,"1733 2.5 in NH 125-250 75 BLACK (Std) PG ETCH","17334036","TBJT 2.5NH 125-250G@75P RED BANKS",45]
["17334037","TBJT 2.5NH 125-250G@75P VICTORIA",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"NH","GPM","125-250","PSI","N/A",75,"BLACK","Y","ENGLISH","Selectable","High-Range","N",20,3,"1733","N/A","N/A",null,null,"1733 2.5 in NH 125-250 75 BLACK (Std) PG ETCH","17334037","TBJT 2.5NH 125-250G@75P VICTORIA",45]
["17334038","TBJT 2.5NH 125-250G@75P WATSON",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"NH","GPM","125-250","PSI","N/A",75,"BLACK","Y","ENGLISH","Selectable","High-Range","N",20,3,"1733","N/A","N/A",null,null,"1733 2.5 in NH 125-250 75 BLACK (Std) PG ETCH","17334038","TBJT 2.5NH 125-250G@75P WATSON",45]
["17337007","TBJT NPG 2.5NH 125-250G@75P",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"NH","GPM","125-250","PSI","n/a",75,"BLACK","N","ENGLISH","Selectable","High-Range","Y",20,3,"1733","N/A","N/A",null,null,"1733 2.5 in NH 125-250 75 BLACK (Std) NPG","17337007","TBJT NPG 2.5NH 125-250G@75P",41]
["17337014","TBJT NPG 2.5AEA 125-250G@100P FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"AEA","GPM","125-250","PSI","N/A",100,"BLACK","N","ENGLISH","Selectable","High-Range","N",20,3,"1733","N/A","N/A",null,null,"1733 2.5 in AEA 125-250 100 (Std) BLACK (Std) PG","17337014","TBJT NPG 2.5AEA 125-250G@100P FM",48]
["17334003","TBJT 65MM JIM 125-250G@100P FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"JIM","GPM","125-250","PSI","N/A",100,"BLACK","N","ENGLISH","Selectable","High-Range","N","No 2021 Sales","No 2021 Sales","1733","N/A","N/A",null,null,"1733 2.5 in JIM 125-250 100 (Std) BLACK (Std) PG","17334003","TBJT 65MM JIM 125-250G@100P FM",48]
["17334039","TBJT 65MM 125-250G@75P",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"STORZ","GPM","125-250","PSI","N/A",75,"BLACK","N","ENGLISH","Selectable","High-Range","N","No 2021 Sales","No 2021 Sales","1733","N/A","N/A",null,null,{"$f":"CONCATENATE(AC169,\" \",N169,\" in \",O169,\" \",IF(AD169=\"n/a\",\"\",CONCATENATE(AD169,\" in \",AE169,\" \")),IF(Q169=\"n/a\",\"\",Q169),IF(S169=\"n/a\",\"\",CONCATENATE(IF(X169=\"saber\",\" \",\"\"),S169,\" bore size(s) \")),IF(T169=\"n/a\",\"\",CONCATENATE(IF(X169=\"saber\",\"\",\" \"),T169,IF(T169=100,\" (Std) \",IF(T169=87,\" (CE) \",\" \")))),IF(U169=\"n/a\",\"\",CONCATENATE(U169,IF(U169=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X169,3)=\"tip\",IF(LEFT(X169,1)=\"s\",\"\",IF(Z169=\"n\",IF(T169=\"N/A\",\"PG\",\" PG\"),IF(Z169=\"y\",IF(T169=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z169=\"n\",IF(T169=\"N/A\",\"PG\",\" PG\"),IF(Z169=\"y\",IF(T169=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF169=\"y\",\" ZT\",\"\"),IF(V169=\"N\",\"\",IF(S169=\"n/a\",\" ETCH\",IF(T169=\"N/A\",IF(RIGHT(X169,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X169=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"1733 2.5 in STORZ 125-250 75 BLACK (Std) PG"},{"$f":"A169","v":"17334039"},{"$f":"B169","v":"TBJT 65MM 125-250G@75P"},{"$f":"LEN(AH169)","v":43}]
["17334004","TBJT 75MM 125-250G@100P FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",3,"STORZ","GPM","125-250","PSI","N/A",100,"BLACK","N","ENGLISH","Selectable","High-Range","N","No 2021 Sales","No 2021 Sales","1733","N/A","N/A",null,null,"1733 3 in STORZ 125-250 100 (Std) BLACK (Std) PG","17334004","TBJT 75MM 125-250G@100P FM",48]
["17334013","TBJT 2.5NH 125-250G@75P ORGBMPR",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"NH","GPM","125-250","PSI","N/A",75,"ORANGE","N","ENGLISH","Selectable","High-Range","N","No 2021 Sales","No 2021 Sales","1733","N/A","N/A",null,null,"1733 2.5 in NH 125-250 75 ORANGE PG","17334013","TBJT 2.5NH 125-250G@75P ORGBMPR",35]
["17334016","TBJT 2.5AII 475-900L@7b/700K FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"CSA","LPM","475-900","BAR","n/a",700,"BLACK","N","ENGLISH","Selectable","High-Range","N","No 2021 Sales","No 2021 Sales","1733","N/A","N/A",null,null,"1733 2.5 in CSA 475-900 700 BLACK (Std) PG","17334016","TBJT 2.5AII 475-900L@7b/700K FM",42]
["17334018","TBJT 2.5AHB 125-250G@75P",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"AHB","GPM","125-250","PSI","n/a",75,"BLACK","N","ENGLISH","Selectable","High-Range","N","No 2021 Sales","No 2021 Sales","1733","N/A","N/A",null,null,"1733 2.5 in AHB 125-250 75 BLACK (Std) PG","17334018","TBJT 2.5AHB 125-250G@75P",41]
["17334020","TBJT ZT 2.5NH 125-250G@75P",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"NH","GPM","125-250","PSI","n/a",75,"BLACK","N","ENGLISH","Selectable","High-Range","N","No 2021 Sales","No 2021 Sales","1733","N/A","N/A","Y",null,"1733 2.5 in NH 125-250 75 BLACK (Std) PG ZT","17334020","TBJT ZT 2.5NH 125-250G@75P",43]
["17334022","TBJT ZT 2.5BSP 475-950L@7b",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"BSP","LPM","475-950","BAR","N/A",7,"BLACK","N","ENGLISH","Selectable","High-Range","N","No 2021 Sales","No 2021 Sales","1733","N/A","N/A","Y",null,"1733 2.5 in BSP 475-950 7 BLACK (Std) PG ZT","17334022","TBJT ZT 2.5BSP 475-950L@7b",43]
["17334024","TBJT 2.5AGZ 125-250G@100P FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"AGZ","GPM","125-250","PSI","N/A",100,"BLACK","N","ENGLISH","Selectable","High-Range","N","No 2021 Sales","No 2021 Sales","1733","N/A","N/A",null,null,"1733 2.5 in AGZ 125-250 100 (Std) BLACK (Std) PG","17334024","TBJT 2.5AGZ 125-250G@100P FM",48]
["17337002","TBJT NPG 65MM 125-250G@100P FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"STORZ","GPM","125-250","PSI","n/a",100,"BLACK","N","ENGLISH","Selectable","High-Range","Y","No 2021 Sales","No 2021 Sales","1733","N/A","N/A",null,null,"1733 2.5 in STORZ 125-250 100 (Std) BLACK (Std) NPG","17337002","TBJT NPG 65MM 125-250G@100P FM",51]
["17337003","TBJT NPG 2.5AGA 125-250G@100P FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"AGA","GPM","125-250","PSI","n/a",100,"BLACK","N","ENGLISH","Selectable","High-Range","Y","No 2021 Sales","No 2021 Sales","1733","N/A","N/A",null,null,"1733 2.5 in AGA 125-250 100 (Std) BLACK (Std) NPG","17337003","TBJT NPG 2.5AGA 125-250G@100P FM",49]
["17337009","TBJT NPG 2.5BAF 125-250G@100P FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"BAT","GPM","125-250","PSI","n/a",100,"BLACK","N","ENGLISH","Selectable","High-Range","Y","No 2021 Sales","No 2021 Sales","1733","N/A","N/A",null,null,"1733 2.5 in BAT 125-250 100 (Std) BLACK (Std) NPG","17337009","TBJT NPG 2.5BAF 125-250G@100P FM",49]
["17374002","TBJT TIP 1.5NH 95-200G@100P",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","95-200","PSI","n/a",100,"BLACK","N","ENGLISH","Selectable Tip","Mid-Range","N/A",20,1,"1737","N/A","N/A",null,null,"1737 1.5 in NH 95-200 100 (Std) BLACK (Std)","17374002","TBJT TIP 1.5NH 95-200G@100P",43]
["17374001","TBJT TIP 1.5NH 95-200G@75P",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","95-200","PSI","n/a",75,"BLACK","N","ENGLISH","Selectable Tip","Mid-Range","N/A",20,2,"1737","N/A","N/A",null,null,"1737 1.5 in NH 95-200 75 BLACK (Std)","17374001","TBJT TIP 1.5NH 95-200G@75P",36]
["17374004","TBJT TIP 1.5NPSH 95-200G@100P",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NPSH","GPM","95-200","PSI","n/a",100,"BLACK","N","ENGLISH","Selectable Tip","Mid-Range","N/A",20,3,"1737","N/A","N/A",null,null,"1737 1.5 in NPSH 95-200 100 (Std) BLACK (Std)","17374004","TBJT TIP 1.5NPSH 95-200G@100P",45]
["17374005","TBJT TIP 1.5NH 95-200G@75P REDBMPR",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","95-200","PSI","n/a",75,"RED","N","ENGLISH","Selectable Tip","Mid-Range","N/A",20,3,"1737","N/A","N/A",null,null,"1737 1.5 in NH 95-200 75 RED","17374005","TBJT TIP 1.5NH 95-200G@75P REDBMPR",28]
["17374006","TBJT TIP 1.5NH 95-200G@75P ORG BMPR",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","95-200","PSI","N/A",75,"ORANGE","N","ENGLISH","Selectable Tip","Mid-Range","N/A",20,3,"1737","N/A","N/A",null,null,"1737 1.5 in NH 95-200 75 ORANGE","17374006","TBJT TIP 1.5NH 95-200G@75P ORG BMPR",31]
["17374003","TBJT TIP 1.5NPSH 360-750L@5b/500K",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NPSH","LPM","360-750","BAR","n/a",5,"BLACK","N","ENGLISH","Selectable Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","1737","N/A","N/A",null,null,"1737 1.5 in NPSH 360-750 5 BLACK (Std)","17374003","TBJT TIP 1.5NPSH 360-750L@5b/500K",38]
["17374032","TBJT TIP 1.5NH 95-200G@100P REDBMPR",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","95-200","PSI","n/a",100,"RED","N","ENGLISH","Selectable Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","1737","N/A","N/A",null,null,"1737 1.5 in NH 95-200 100 (Std) RED","17374032","TBJT TIP 1.5NH 95-200G@100P REDBMPR",35]
["17444001","TBJT TIP 1.5NH 125-250G@100P#",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","125-250","PSI","N/A",100,"BLACK","N","ENGLISH","Selectable Tip","High-Range","N/A",80,1,"1744","N/A","N/A",null,null,"1744 1.5 in NH 125-250 100 (Std) BLACK (Std)","17444001","TBJT TIP 1.5NH 125-250G@100P#",44]
["17444003","TBJT TIP 1.5BSP 475-950L@7b",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"BSP","LPM","475-950","BAR","N/A",7,"BLACK","N","ENGLISH","Selectable Tip","High-Range","N/A",20,2,"1744","N/A","N/A",null,null,"1744 1.5 in BSP 475-950 7 BLACK (Std)","17444003","TBJT TIP 1.5BSP 475-950L@7b",37]
["17444006","TBJT TIP 1.5NH 125-250G@75P",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","125-250","PSI","N/A",75,"BLACK","N","ENGLISH","Selectable Tip","High-Range","N/A",20,2,"1744","N/A","N/A",null,null,"1744 1.5 in NH 125-250 75 BLACK (Std)","17444006","TBJT TIP 1.5NH 125-250G@75P",37]
["17444007","TBJT TIP 1.5NPSH 125-250G@100P",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NPSH","GPM","125-250","PSI","N/A",100,"BLACK","N","ENGLISH","Selectable Tip","High-Range","N/A",20,2,"1744","N/A","N/A",null,null,"1744 1.5 in NPSH 125-250 100 (Std) BLACK (Std)","17444007","TBJT TIP 1.5NPSH 125-250G@100P",46]
["17444008","TBJT TIP 1.5NPSH 125-250G@75P",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NPSH","GPM","125-250","PSI","N/A",75,"BLACK","N","ENGLISH","Selectable Tip","High-Range","N/A",20,2,"1744","N/A","N/A",null,null,"1744 1.5 in NPSH 125-250 75 BLACK (Std)","17444008","TBJT TIP 1.5NPSH 125-250G@75P",39]
["17444005","TBJT TIP 1.5NH 475-950L@7b",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","LPM","475-950","BAR","N/A",7,"BLACK","N","ENGLISH","Selectable Tip","High-Range","N/A",20,3,"1744","N/A","N/A",null,null,"1744 1.5 in NH 475-950 7 BLACK (Std)","17444005","TBJT TIP 1.5NH 475-950L@7b",36]
["17444010","TBJT TIP 1.5NH 125-250G@100P YEL BMPR",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","125-250","PSI","N/A",100,"YELLOW","N","ENGLISH","Selectable Tip","High-Range","N/A",20,3,"1744","N/A","N/A",null,null,"1744 1.5 in NH 125-250 100 (Std) YELLOW","17444010","TBJT TIP 1.5NH 125-250G@100P YEL BMPR",39]
["17444002","TBJT TIP 1.5NH 125-250G@100P REDBMPR",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","125-250","PSI","n/a",100,"RED","N","ENGLISH","Selectable Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","1744","N/A","N/A",null,null,"1744 1.5 in NH 125-250 100 (Std) RED","17444002","TBJT TIP 1.5NH 125-250G@100P REDBMPR",36]
["17444004","TBJT TIP 1.5NPSH 475-950L@5b",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NPSH","LPM","475-900","BAR","n/a",5,"BLACK","N","ENGLISH","Selectable Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","1744","N/A","N/A",null,null,"1744 1.5 in NPSH 475-900 5 BLACK (Std)","17444004","TBJT TIP 1.5NPSH 475-950L@5b",38]
["17634001","TBJT 1.5NH 30-200G@100P FM#",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","30-200","PSI","N/A",100,"BLACK","N","ENGLISH","Selectable","Mid-Range","N",80,1,"1763","N/A","N/A",null,null,"1763 1.5 in NH 30-200 100 (Std) BLACK (Std) PG","17634001","TBJT 1.5NH 30-200G@100P FM#",46]
["17634002","TBJT 2.5BIM 115-750L@7b FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"BIM","LPM","115-750","BAR","N/A",7,"BLACK","N","ENGLISH","Selectable","Mid-Range","N",80,1,"1763","N/A","N/A",null,null,"1763 2.5 in BIM 115-750 7 BLACK (Std) PG","17634002","TBJT 2.5BIM 115-750L@7b FM",40]
["17634003","TBJT 1.5NH 30-200G@75P#",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","30-200","PSI","N/A",75,"BLACK","N","ENGLISH","Selectable","Mid-Range","N",80,1,"1763","N/A","N/A",null,null,"1763 1.5 in NH 30-200 75 BLACK (Std) PG","17634003","TBJT 1.5NH 30-200G@75P#",39]
["17634016","TBJT 2.5NH 30-200G@100P FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"NH","GPM","30-200","PSI","N/A",100,"BLACK","N","ENGLISH","Selectable","Mid-Range","N",80,1,"1763","N/A","N/A",null,null,"1763 2.5 in NH 30-200 100 (Std) BLACK (Std) PG","17634016","TBJT 2.5NH 30-200G@100P FM",46]
["17634004","TBJT 52MM 115-750L@7b FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2,"STORZ","LPM","115-750","BAR","N/A",7,"BLACK","N","ENGLISH","Selectable","Mid-Range","N",20,1,"1763","N/A","N/A",null,null,"1763 2 in STORZ 115-750 7 BLACK (Std) PG","17634004","TBJT 52MM 115-750L@7b FM",40]
["17634015","TBJT 1.5NPSH 30-200G@75P",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NPSH","GPM","30-200","PSI","N/A",75,"BLACK","N","ENGLISH","Selectable","Mid-Range","N",20,1,"1763","N/A","N/A",null,null,"1763 1.5 in NPSH 30-200 75 BLACK (Std) PG","17634015","TBJT 1.5NPSH 30-200G@75P",41]
["17634020","TBJT 1.5NPSH 30-200G@100P FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NPSH","GPM","30-200","PSI","N/A",100,"BLACK","N","ENGLISH","Selectable","Mid-Range","N",20,1,"1763","N/A","N/A",null,null,"1763 1.5 in NPSH 30-200 100 (Std) BLACK (Std) PG","17634020","TBJT 1.5NPSH 30-200G@100P FM",48]
["17637001","TBJT NPG 1.5NH 30-200G@100P FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","30-200","PSI","N/A",100,"BLACK","N","ENGLISH","Selectable","Mid-Range","Y",20,1,"1763","N/A","N/A",null,null,"1763 1.5 in NH 30-200 100 (Std) BLACK (Std) NPG","17637001","TBJT NPG 1.5NH 30-200G@100P FM",47]
["17637015","TBJT NPG 1.5NPSH 30-200G@75P",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NPSH","GPM","30-200","PSI","N/A",75,"BLACK","N","ENGLISH","Selectable","Mid-Range","Y",20,1,"1763","N/A","N/A",null,null,"1763 1.5 in NPSH 30-200 75 BLACK (Std) NPG","17637015","TBJT NPG 1.5NPSH 30-200G@75P",42]
["17634011","TBJT 1.5NH 30-200G@100P REDBMPR FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","30-200","PSI","N/A",100,"RED","N","ENGLISH","Selectable","Mid-Range","N",20,2,"1763","N/A","N/A",null,null,"1763 1.5 in NH 30-200 100 (Std) RED PG","17634011","TBJT 1.5NH 30-200G@100P REDBMPR FM",38]
["17634013","TBJT 75MM 115-750L@7b FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",3,"STORZ","LPM","115-750","BAR","N/A",7,"BLACK","N","ENGLISH","Selectable","Mid-Range","N",20,2,"1763","N/A","N/A",null,null,"1763 3 in STORZ 115-750 7 BLACK (Std) PG","17634013","TBJT 75MM 115-750L@7b FM",40]
["17634022","TBJT 1.5NH 30-200G@100P YLWBMPR FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","30-200","PSI","N/A",100,"YELLOW","N","ENGLISH","Selectable","Mid-Range","N",20,2,"1763","N/A","N/A",null,null,"1763 1.5 in NH 30-200 100 (Std) YELLOW PG","17634022","TBJT 1.5NH 30-200G@100P YLWBMPR FM",41]
["17634024","TBJT ZT 1.5NH 30-200G@100P",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","30-200","PSI","N/A",100,"BLACK","N","ENGLISH","Selectable","Mid-Range","N",20,2,"1763","N/A","N/A","Y",null,"1763 1.5 in NH 30-200 100 (Std) BLACK (Std) PG ZT","17634024","TBJT ZT 1.5NH 30-200G@100P",49]
["17634026","TBJT ZT 2.5BIM 115-750L@7b",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"BIM","LPM","115-750","BAR","N/A",7,"BLACK","N","ENGLISH","Selectable","Mid-Range","N",20,2,"1763","N/A","N/A","Y",null,"1763 2.5 in BIM 115-750 7 BLACK (Std) PG ZT","17634026","TBJT ZT 2.5BIM 115-750L@7b",43]
["17634030","TBJT 1.5NH 30-200G@100P GRNBMPR FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","30-200","PSI","n/a",100,"GREEN","N","ENGLISH","Selectable","Mid-Range","N",20,2,"1763","N/A","N/A",null,null,{"$f":"CONCATENATE(AC210,\" \",N210,\" in \",O210,\" \",IF(AD210=\"n/a\",\"\",CONCATENATE(AD210,\" in \",AE210,\" \")),IF(Q210=\"n/a\",\"\",Q210),IF(S210=\"n/a\",\"\",CONCATENATE(IF(X210=\"saber\",\" \",\"\"),S210,\" bore size(s) \")),IF(T210=\"n/a\",\"\",CONCATENATE(IF(X210=\"saber\",\"\",\" \"),T210,IF(T210=100,\" (Std) \",IF(T210=87,\" (CE) \",\" \")))),IF(U210=\"n/a\",\"\",CONCATENATE(U210,IF(U210=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X210,3)=\"tip\",IF(LEFT(X210,1)=\"s\",\"\",IF(Z210=\"n\",IF(T210=\"N/A\",\"PG\",\" PG\"),IF(Z210=\"y\",IF(T210=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z210=\"n\",IF(T210=\"N/A\",\"PG\",\" PG\"),IF(Z210=\"y\",IF(T210=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF210=\"y\",\" ZT\",\"\"),IF(V210=\"N\",\"\",IF(S210=\"n/a\",\" ETCH\",IF(T210=\"N/A\",IF(RIGHT(X210,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X210=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"1763 1.5 in NH 30-200 100 (Std) GREEN PG"},{"$f":"A210","v":"17634030"},{"$f":"B210","v":"TBJT 1.5NH 30-200G@100P GRNBMPR FM"},{"$f":"LEN(AH210)","v":40}]
["17634032","TBJT 1.5NH 30-200G@100P ORGBMPR FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","30-200","PSI","N/A",100,"ORANGE","N","ENGLISH","Selectable","Mid-Range","N",20,2,"1763","N/A","N/A",null,null,"1763 1.5 in NH 30-200 100 (Std) ORANGE PG","17634032","TBJT 1.5NH 30-200G@100P ORGBMPR FM",41]
["17634034","TBJT ZT 1.5NPSH 30-200G@100P",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NPSH","GPM","30-200","PSI","N/A",100,"BLACK","N","ENGLISH","Selectable","Mid-Range","N",20,2,"1763","N/A","N/A","Y",null,"1763 1.5 in NPSH 30-200 100 (Std) BLACK (Std) PG ZT","17634034","TBJT ZT 1.5NPSH 30-200G@100P",51]
["17634036","TBJT 38MM 30-200G@75P",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"STORZ","GPM","30-200","PSI","N/A",75,"BLACK","N","ENGLISH","Selectable","Mid-Range","N",20,2,"1763","N/A","N/A",null,null,"1763 1.5 in STORZ 30-200 75 BLACK (Std) PG","17634036","TBJT 38MM 30-200G@75P",42]
["17637003","TBJT NPG 1.5NH 30-200G@75P",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","30-200","PSI","N/A",75,"BLACK","N","ENGLISH","Selectable","Mid-Range","Y",20,2,"1763","N/A","N/A",null,null,"1763 1.5 in NH 30-200 75 BLACK (Std) NPG","17637003","TBJT NPG 1.5NH 30-200G@75P",40]
["17634021","TBJT 1.5NH 30-200G@75P REDBMPR",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","30-200","PSI","n/a",75,"RED","N","ENGLISH","Selectable","Mid-Range","N",20,3,"1763","N/A","N/A",null,null,"1763 1.5 in NH 30-200 75 RED PG","17634021","TBJT 1.5NH 30-200G@75P REDBMPR",31]
["17634033","TBJT 1.5ABP 30-200G@100P FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"ABP","GPM","30-200","PSI","N/A",100,"BLACK","N","ENGLISH","Selectable","Mid-Range","N",20,3,"1763","N/A","N/A",null,null,"1763 1.5 in ABP 30-200 100 (Std) BLACK (Std) PG","17634033","TBJT 1.5ABP 30-200G@100P FM",47]
["17634005","TBJT 52MM 30-200G@100P FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2,"STORZ","GPM","30-200","PSI","N/A",100,"BLACK","N","ENGLISH","Selectable","Mid-Range","N","No 2021 Sales","No 2021 Sales","1763","N/A","N/A",null,null,"1763 2 in STORZ 30-200 100 (Std) BLACK (Std) PG","17634005","TBJT 52MM 30-200G@100P FM",47]
["17634014","TBJT 1.5 BSP 115-750L@7b FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"BSP","LPM","115-750","BAR","N/A",7,"BLACK","N","ENGLISH","Selectable","Mid-Range","N","No 2021 Sales","No 2021 Sales","1763","N/A","N/A",null,null,"1763 1.5 in BSP 115-750 7 BLACK (Std) PG","17634014","TBJT 1.5 BSP 115-750L@7b FM",40]
["17634018","TBJT 1.5NPSH 115-750L@5b/500K",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NPSH","LPM","115-750","BAR","n/a",5,"BLACK","N","ENGLISH","Selectable","Mid-Range","N","No 2021 Sales","No 2021 Sales","1763","N/A","N/A",null,null,"1763 1.5 in NPSH 115-750 5 BLACK (Std) PG","17634018","TBJT 1.5NPSH 115-750L@5b/500K",41]
["17634019","TBJT ZT 1.5NPSH 115-750L@5b",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NPSH","LPM","115-750","BAR","n/a",5,"BLACK","N","ENGLISH","Selectable","Mid-Range","N","No 2021 Sales","No 2021 Sales","1763","N/A","N/A","Y",null,"1763 1.5 in NPSH 115-750 5 BLACK (Std) PG ZT","17634019","TBJT ZT 1.5NPSH 115-750L@5b",44]
["17634023","TBJT 1.5 NPSH 115-750L@7b FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NPSH","LPM","115-750","BAR","n/a",7,"BLACK","N","ENGLISH","Selectable","Mid-Range","N","No 2021 Sales","No 2021 Sales","1763","N/A","N/A",null,null,"1763 1.5 in NPSH 115-750 7 BLACK (Std) PG","17634023","TBJT 1.5 NPSH 115-750L@7b FM",41]
["17634027","TBJT ZT 1.5NH 30-200G@75P",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","30-200","PSI","n/a",75,"BLACK","N","ENGLISH","Selectable","Mid-Range","N","No 2021 Sales","No 2021 Sales","1763","N/A","N/A","Y",null,"1763 1.5 in NH 30-200 75 BLACK (Std) PG ZT","17634027","TBJT ZT 1.5NH 30-200G@75P",42]
["17634028","TBJT 1.5NH 115-750L@7b FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","LPM","115-750","BAR","N/A",7,"BLACK","N","ENGLISH","Selectable","Mid-Range","N","No 2021 Sales","No 2021 Sales","1763","N/A","N/A",null,null,"1763 1.5 in NH 115-750 7 BLACK (Std) PG","17634028","TBJT 1.5NH 115-750L@7b FM",39]
["17634029","TBJT 75MM 30-200G@100P FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",3,"STORZ","GPM","30-200","PSI","N/A",100,"BLACK","N","ENGLISH","Selectable","Mid-Range","N","No 2021 Sales","No 2021 Sales","1763","N/A","N/A",null,null,"1763 3 in STORZ 30-200 100 (Std) BLACK (Std) PG","17634029","TBJT 75MM 30-200G@100P FM",47]
["17634031","TBJT 1.5NH 30-200G@100P BLUEBMPR FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","30-200","PSI","N/A",100,"BLUE","N","ENGLISH","Selectable","Mid-Range","N","No 2021 Sales","No 2021 Sales","1763","N/A","N/A",null,null,"1763 1.5 in NH 30-200 100 (Std) BLUE PG","17634031","TBJT 1.5NH 30-200G@100P BLUEBMPR FM",39]
["17634038","TBJT 2.5NH 30-200G@75P",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"NH","GPM","30-200","PSI","N/A",75,"BLACK","N","ENGLISH","Selectable","Mid-Range","N","No 2021 Sales","No 2021 Sales","1763","N/A","N/A",null,null,"1763 2.5 in NH 30-200 75 BLACK (Std) PG","17634038","TBJT 2.5NH 30-200G@75P",39]
["17634039","TBJT 1.5NH 30-200G@75P BLUEBMPR",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","30-200","PSI","n/a",75,"BLUE","N","ENGLISH","Selectable","Mid-Range","N","No 2021 Sales","No 2021 Sales","1763","N/A","N/A",null,null,"1763 1.5 in NH 30-200 75 BLUE PG","17634039","TBJT 1.5NH 30-200G@75P BLUEBMPR",32]
["17634040","TBJT 1.5NH 30-200G@75P ORGBMPR",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","30-200","PSI","n/a",75,"ORANGE","N","ENGLISH","Selectable","Mid-Range","N","No 2021 Sales","No 2021 Sales","1763","N/A","N/A",null,null,"1763 1.5 in NH 30-200 75 ORANGE PG","17634040","TBJT 1.5NH 30-200G@75P ORGBMPR",34]
["17634041","TBJT 1.5NH 30-200G@75P GRNBMPR",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","30-200","PSI","n/a",75,"GREEN","N","ENGLISH","Selectable","Mid-Range","N","No 2021 Sales","No 2021 Sales","1763","N/A","N/A",null,null,"1763 1.5 in NH 30-200 75 GREEN PG","17634041","TBJT 1.5NH 30-200G@75P GRNBMPR",33]
["17637011","TBJT NPG 1.5NH 30-200G@100P REDBMPR FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","30-200","PSI","N/A",100,"RED","N","ENGLISH","Selectable","Mid-Range","Y","No 2021 Sales","No 2021 Sales","1763","N/A","N/A",null,null,"1763 1.5 in NH 30-200 100 (Std) RED NPG","17637011","TBJT NPG 1.5NH 30-200G@100P REDBMPR FM",39]
["17637020","TBJT NPG 1.5NPSH 30-200G@100P FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NPSH","GPM","30-200","PSI","n/a",100,"BLACK","N","ENGLISH","Selectable","Mid-Range","Y","No 2021 Sales","No 2021 Sales","1763","N/A","N/A",null,null,"1763 1.5 in NPSH 30-200 100 (Std) BLACK (Std) NPG","17637020","TBJT NPG 1.5NPSH 30-200G@100P FM",49]
["17637022","TBJT NPG 1.5NH 30-200G@100P YLWBMPR FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","30-200","PSI","N/A",100,"YELLOW","N","ENGLISH","Selectable","Mid-Range","Y","No 2021 Sales","No 2021 Sales","1763","N/A","N/A",null,null,"1763 1.5 in NH 30-200 100 (Std) YELLOW NPG","17637022","TBJT NPG 1.5NH 30-200G@100P YLWBMPR FM",42]
["17637030","TBJT NPG 1.5NH 30-200G@100P GRNBMPR FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","30-200","PSI","N/A",100,"GREEN","N","ENGLISH","Selectable","Mid-Range","Y","No 2021 Sales","No 2021 Sales","1763","N/A","N/A",null,null,"1763 1.5 in NH 30-200 100 (Std) GREEN NPG","17637030","TBJT NPG 1.5NH 30-200G@100P GRNBMPR FM",41]
["17637031","TBJT NPG 1.5NH 30-200G@100P BLUEBMPR FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","30-200","PSI","N/A",100,"BLUE","N","ENGLISH","Selectable","Mid-Range","Y","No 2021 Sales","No 2021 Sales","1763","N/A","N/A",null,null,"1763 1.5 in NH 30-200 100 (Std) BLUE NPG","17637031","TBJT NPG 1.5NH 30-200G@100P BLUEBMPR FM",40]
["17664001","TBJT TIP 1.5NH 30-200G@100P#",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","30-200","PSI","n/a",100,"BLACK","N","ENGLISH","Selectable Tip","Mid-Range","N/A",80,1,"1766","N/A","N/A",null,null,"1766 1.5 in NH 30-200 100 (Std) BLACK (Std)","17664001","TBJT TIP 1.5NH 30-200G@100P#",43]
["17664002","TBJT TIP 1.5NH 30-200G@75P",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","30-200","PSI","n/a",75,"BLACK","N","ENGLISH","Selectable Tip","Mid-Range","N/A",20,2,"1766","N/A","N/A",null,null,"1766 1.5 in NH 30-200 75 BLACK (Std)","17664002","TBJT TIP 1.5NH 30-200G@75P",36]
["17664005","TBJT TIP 1.5NPSH 30-200G@75P",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NPSH","GPM","30-200","PSI","n/a",75,"BLACK","N","ENGLISH","Selectable Tip","Mid-Range","N/A",20,2,"1766","N/A","N/A",null,null,"1766 1.5 in NPSH 30-200 75 BLACK (Std)","17664005","TBJT TIP 1.5NPSH 30-200G@75P",38]
["17664007","TBJT TIP 1.5NPSH 30-200G@100P",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NPSH","GPM","30-200","PSI","n/a",100,"BLACK","N","ENGLISH","Selectable Tip","Mid-Range","N/A",20,3,"1766","N/A","N/A",null,null,"1766 1.5 in NPSH 30-200 100 (Std) BLACK (Std)","17664007","TBJT TIP 1.5NPSH 30-200G@100P",45]
["17664009","TBJT TIP 1.5NH 30-200G@100P RED BMPR",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","30-200","PSI","N/A",100,"RED","N","ENGLISH","Selectable Tip","Mid-Range","N/A",20,3,"1766","N/A","N/A",null,null,"1766 1.5 in NH 30-200 100 (Std) RED","17664009","TBJT TIP 1.5NH 30-200G@100P RED BMPR",35]
["17664010","TBJT TIP 1.5NH 30-200G@100P YEL BMPR",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","30-200","PSI","N/A",100,"YELLOW","N","ENGLISH","Selectable Tip","Mid-Range","N/A",20,3,"1766","N/A","N/A",null,null,"1766 1.5 in NH 30-200 100 (Std) YELLOW","17664010","TBJT TIP 1.5NH 30-200G@100P YEL BMPR",38]
["17664011","TBJT TIP 1.5NH 30-200G@100P GRN BMPR",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","30-200","PSI","N/A",100,"GREEN","N","ENGLISH","Selectable Tip","Mid-Range","N/A",20,3,"1766","N/A","N/A",null,null,"1766 1.5 in NH 30-200 100 (Std) GREEN","17664011","TBJT TIP 1.5NH 30-200G@100P GRN BMPR",37]
["17664012","TBJT TIP 1.5NH 30-200G@100P BLU BMPR",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","30-200","PSI","N/A",100,"BLUE","N","ENGLISH","Selectable Tip","Mid-Range","N/A",20,3,"1766","N/A","N/A",null,null,"1766 1.5 in NH 30-200 100 (Std) BLUE","17664012","TBJT TIP 1.5NH 30-200G@100P BLU BMPR",36]
["17664013","TBJT TIP 1.5NH 30-200G@100P ORG  BMPR",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","30-200","PSI","N/A",100,"ORANGE","N","ENGLISH","Selectable Tip","Mid-Range","N/A",20,3,"1766","N/A","N/A",null,null,"1766 1.5 in NH 30-200 100 (Std) ORANGE","17664013","TBJT TIP 1.5NH 30-200G@100P ORG  BMPR",38]
["17664014","TBJT TIP 1.5NH 30-200G@75P ORGBMPR",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","30-200","PSI","N/A",75,"ORANGE","N","ENGLISH","Selectable Tip","Mid-Range","N",20,3,"1766","N/A","N/A",null,null,"1766 1.5 in NH 30-200 75 ORANGE","17664014","TBJT TIP 1.5NH 30-200G@75P ORGBMPR",31]
["17664003","TBJT TIP 1.5BSP 115-750L@7b",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"BSP","LPM","115-750","BAR","N/A",7,"BLACK","N","ENGLISH","Selectable Tip","Mid-Range","N/A",20,4,"1766","N/A","N/A",null,null,"1766 1.5 in BSP 115-750 7 BLACK (Std)","17664003","TBJT TIP 1.5BSP 115-750L@7b",37]
["17664008","TBJT TIP 1.5NH 30-200G@100P MTLTTH",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","30-200","PSI","n/a",100,"BLACK","N","ENGLISH","Selectable Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","1766","N/A","N/A",null,null,"1766 1.5 in NH 30-200 100 (Std) BLACK (Std)","17664008","TBJT TIP 1.5NH 30-200G@100P MTLTTH",43]
["17724006","TBJT 1\"NH 13-60G@100P 180 DEG FOG",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1,"NH","GPM","13-60","PSI","N/A",100,"BLACK","N","ENGLISH","Selectable","1.5\"","N",20,2,"1772","N/A","N/A",null,null,"1772 1 in NH 13-60 100 (Std) BLACK (Std) PG","17724006","TBJT 1\"NH 13-60G@100P 180 DEG FOG",43]
["48024001","ASLT 1.0 NH 40G@100P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1,"NH","GPM",40,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","1\"","N",80,1,"4802","N/A","N/A",null,null,"4802 1 in NH 40 100 (Std) BLACK (Std) PG","48024001","ASLT 1.0 NH 40G@100P FM",40]
["48024707","ASLT 1.0 BSP 100L@6b EN",null,null,null,null,null,null,null,null,"0003","Assault","A",1,"BSP","LPM",100,"BAR","N/A",6,"BLACK","N","ENGLISH","Fixed","1\"","N",80,1,"4802","N/A","N/A",null,null,"4802 1 in BSP 100 6 BLACK (Std) PG","48024707","ASLT 1.0 BSP 100L@6b EN",34]
["48027001","ASLT NPG 1.0 NH 40G@100P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1,"NH","GPM",40,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","1\"","Y",20,1,"4802","N/A","N/A",null,null,"4802 1 in NH 40 100 (Std) BLACK (Std) NPG","48027001","ASLT NPG 1.0 NH 40G@100P FM",41]
["48024002","ASLT 1.0 NH 25G@100P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1,"NH","GPM",25,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","1\"","N",20,2,"4802","N/A","N/A",null,null,"4802 1 in NH 25 100 (Std) BLACK (Std) PG","48024002","ASLT 1.0 NH 25G@100P FM",40]
["48024003","ASLT 1.0 NH 100L@7b FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1,"NH","LPM",100,"BAR","N/A",7,"BLACK","N","ENGLISH","Fixed","1\"","N",20,2,"4802","N/A","N/A",null,null,"4802 1 in NH 100 7 BLACK (Std) PG","48024003","ASLT 1.0 NH 100L@7b FM",33]
["48024005","ASLT 1.0 BSP 100L@7b DETENT",null,null,null,null,null,null,null,null,"0003","Assault","A",1,"BSP","LPM",100,"BAR","N/A",7,"BLACK","N","ENGLISH","Fixed","1\"","N",20,2,"4802","N/A","N/A",null,null,"4802 1 in BSP 100 7 BLACK (Std) PG","48024005","ASLT 1.0 BSP 100L@7b DETENT",34]
["48024010","ASLT 1.0 BSP 150L@7b FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1,"BSP","LPM",150,"BAR","N/A",7,"BLACK","N","ENGLISH","Fixed","1\"","N",20,2,"4802","N/A","N/A",null,null,"4802 1 in BSP 150 7 BLACK (Std) PG","48024010","ASLT 1.0 BSP 150L@7b FM",34]
["48027018","ASLT NPG 1\"NH 40G@100P D.C.F.D",null,null,null,null,null,null,null,null,"0003","Assault","A",1,"NH","GPM",40,"PSI","N/A",100,"BLACK","Y","ENGLISH","Fixed","1\"","Y",20,2,"4802","N/A","N/A",null,null,"4802 1 in NH 40 100 (Std) BLACK (Std) NPG ETCH","48027018","ASLT NPG 1\"NH 40G@100P D.C.F.D",46]
["48024011","ASLT 1.0 NH 40G@100P REDBMPR FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1,"NH","GPM",40,"PSI","N/A",100,"RED","N","ENGLISH","Fixed","1\"","N",20,3,"4802","N/A","N/A",null,null,"4802 1 in NH 40 100 (Std) RED PG","48024011","ASLT 1.0 NH 40G@100P REDBMPR FM",32]
["48024019","ASLT 1.0 BSP 100L@7b",null,null,null,null,null,null,null,null,"0003","Assault","A",1,"BSP","LPM",100,"BAR","N/A",7,"BLACK","N","ENGLISH","Fixed","1\"","N",20,3,"4802","N/A","N/A",null,null,"4802 1 in BSP 100 7 BLACK (Std) PG","48024019","ASLT 1.0 BSP 100L@7b",34]
["48024020","ASLT 1.0BSP 50L@7b FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1,"BSP","LPM",50,"BAR","N/A",7,"BLACK","N","ENGLISH","Fixed","1\"","N","No 2021 Sales","No 2021 Sales","4802","N/A","N/A",null,null,{"$f":"CONCATENATE(AC258,\" \",N258,\" in \",O258,\" \",IF(AD258=\"n/a\",\"\",CONCATENATE(AD258,\" in \",AE258,\" \")),IF(Q258=\"n/a\",\"\",Q258),IF(S258=\"n/a\",\"\",CONCATENATE(IF(X258=\"saber\",\" \",\"\"),S258,\" bore size(s) \")),IF(T258=\"n/a\",\"\",CONCATENATE(IF(X258=\"saber\",\"\",\" \"),T258,IF(T258=100,\" (Std) \",IF(T258=87,\" (CE) \",\" \")))),IF(U258=\"n/a\",\"\",CONCATENATE(U258,IF(U258=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X258,3)=\"tip\",IF(LEFT(X258,1)=\"s\",\"\",IF(Z258=\"n\",IF(T258=\"N/A\",\"PG\",\" PG\"),IF(Z258=\"y\",IF(T258=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z258=\"n\",IF(T258=\"N/A\",\"PG\",\" PG\"),IF(Z258=\"y\",IF(T258=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF258=\"y\",\" ZT\",\"\"),IF(V258=\"N\",\"\",IF(S258=\"n/a\",\" ETCH\",IF(T258=\"N/A\",IF(RIGHT(X258,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X258=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"4802 1 in BSP 50 7 BLACK (Std) PG"},{"$f":"A258","v":"48024020"},{"$f":"B258","v":"ASLT 1.0BSP 50L@7b FM"},{"$f":"LEN(AH258)","v":33}]
["48024004","ASLT 1.0 NH 13G@100P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1,"NH","GPM",13,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","1\"","N","No 2021 Sales","No 2021 Sales","4802","N/A","N/A",null,null,"4802 1 in NH 13 100 (Std) BLACK (Std) PG","48024004","ASLT 1.0 NH 13G@100P FM",40]
["48024021","ASLT 1.0 NH 13G@100P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1,"NH","GPM",13,"PSI","N/A",100,"RED","N","ENGLISH","Fixed","1\"","N","No 2021 Sales","No 2021 Sales","4802","N/A","N/A",null,null,{"$f":"CONCATENATE(AC260,\" \",N260,\" in \",O260,\" \",IF(AD260=\"n/a\",\"\",CONCATENATE(AD260,\" in \",AE260,\" \")),IF(Q260=\"n/a\",\"\",Q260),IF(S260=\"n/a\",\"\",CONCATENATE(IF(X260=\"saber\",\" \",\"\"),S260,\" bore size(s) \")),IF(T260=\"n/a\",\"\",CONCATENATE(IF(X260=\"saber\",\"\",\" \"),T260,IF(T260=100,\" (Std) \",IF(T260=87,\" (CE) \",\" \")))),IF(U260=\"n/a\",\"\",CONCATENATE(U260,IF(U260=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X260,3)=\"tip\",IF(LEFT(X260,1)=\"s\",\"\",IF(Z260=\"n\",IF(T260=\"N/A\",\"PG\",\" PG\"),IF(Z260=\"y\",IF(T260=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z260=\"n\",IF(T260=\"N/A\",\"PG\",\" PG\"),IF(Z260=\"y\",IF(T260=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF260=\"y\",\" ZT\",\"\"),IF(V260=\"N\",\"\",IF(S260=\"n/a\",\" ETCH\",IF(T260=\"N/A\",IF(RIGHT(X260,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X260=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"4802 1 in NH 13 100 (Std) RED PG"},{"$f":"A260","v":"48024021"},{"$f":"B260","v":"ASLT 1.0 NH 13G@100P FM"},{"$f":"LEN(AH260)","v":32}]
["48024012","ASLT 1.0 NH 40G@100P ORGBMPR FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1,"NH","GPM",40,"PSI","N/A",100,"ORANGE","N","ENGLISH","Fixed","1\"","N","No 2021 Sales","No 2021 Sales","4802","N/A","N/A",null,null,"4802 1 in NH 40 100 (Std) ORANGE PG","48024012","ASLT 1.0 NH 40G@100P ORGBMPR FM",35]
["48024013","ASLT 1.0 NPSH 25G@100P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1,"NPSH","GPM",25,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","1\"","N","No 2021 Sales","No 2021 Sales","4802","N/A","N/A",null,null,"4802 1 in NPSH 25 100 (Std) BLACK (Std) PG","48024013","ASLT 1.0 NPSH 25G@100P FM",42]
["48024014","ASLT 1.0 NH 25G@100P YLWBMPR FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1,"NH","GPM",25,"PSI","N/A",100,"YELLOW","N","ENGLISH","Fixed","1\"","N","No 2021 Sales","No 2021 Sales","4802","N/A","N/A",null,null,"4802 1 in NH 25 100 (Std) YELLOW PG","48024014","ASLT 1.0 NH 25G@100P YLWBMPR FM",35]
["48024015","ASLT 1.0 NPSH 40G@100P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1,"NPSH","GPM",40,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","1\"","N","No 2021 Sales","No 2021 Sales","4802","N/A","N/A",null,null,"4802 1 in NPSH 40 100 (Std) BLACK (Std) PG","48024015","ASLT 1.0 NPSH 40G@100P FM",42]
["48024016","ASLT 1.0 NH 50L@7b FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1,"NH","LPM",50,"BAR","N/A",7,"BLACK","N","ENGLISH","Fixed","1\"","N","No 2021 Sales","No 2021 Sales","4802","N/A","N/A",null,null,"4802 1 in NH 50 7 BLACK (Std) PG","48024016","ASLT 1.0 NH 50L@7b FM",32]
["48024701","ASLT 1.0 BSPX25MMSTZ 150L@6b EN",null,null,null,null,null,null,null,null,"0003","Assault","A",1,"STORZ","LPM",150,"BAR","N/A",6,"BLACK","N","ENGLISH","Fixed","1\"","N","No 2021 Sales","No 2021 Sales","4802","N/A","N/A",null,null,"4802 1 in STORZ 150 6 BLACK (Std) PG","48024701","ASLT 1.0 BSPX25MMSTZ 150L@6b EN",36]
["48027013","ASLT NPG 1.0 NPSH 25G@100P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1,"NPSH","GPM",25,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","1\"","Y","No 2021 Sales","No 2021 Sales","4802","N/A","N/A",null,null,"4802 1 in NPSH 25 100 (Std) BLACK (Std) NPG","48027013","ASLT NPG 1.0 NPSH 25G@100P FM",43]
["48020505","OBS ASLT NOZ 1\" BSP100LPM@7bar PG SPTH",null,null,null,null,null,null,null,null,"0003","Assault","O",1,"BSP","LPM",100,"BAR","N/A",7,"BLACK","N","ENGLISH","Fixed","1\"","N",20,4,"4802","N/A","N/A",null,null,"4802 1 in BSP 100 7 BLACK (Std) PG","48020505","OBS ASLT NOZ 1\" BSP100LPM@7bar PG SPTH",34]
["48080026","NOZ 1\"NH UHP HD LN 15GPM@1200PSI",null,null,null,null,null,null,null,null,"0003","Assault","A",1,"NH","GPM",15,"PSI","N/A",1200,"BLACK","N","ENGLISH","Fixed","1\"","N",20,2,"4808","N/A","N/A",null,null,"4808 1 in NH 15 1200 BLACK (Std) PG","48080026","NOZ 1\"NH UHP HD LN 15GPM@1200PSI",35]
["48080027","NOZ 1\"NPT UHP HANDLINE 15G@1400P",null,null,null,null,null,null,null,null,"0003","Assault","A",1,"NPT","GPM",15,"PSI","N/A",1400,"BLACK","N","ENGLISH","Fixed","1\"","N",20,2,"4808","N/A","N/A",null,null,"4808 1 in NPT 15 1400 BLACK (Std) PG","48080027","NOZ 1\"NPT UHP HANDLINE 15G@1400P",36]
["48200203","ASLT 1.5NH 95G@75P GRAY PG&HDL",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",95,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed","1.5\"","N",20,2,"4820","N/A","N/A",null,null,"4820 1.5 in NH 95 75 BLACK (Std) PG","48200203","ASLT 1.5NH 95G@75P GRAY PG&HDL",35]
["48200560","OBSI  ASLT NOZ 2.5 52MM 230L@7bar FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2,"STORZ","LPM",230,"BAR","N/A",7,"BLACK","N","ENGLISH","Fixed","1.5\"","N","No 2021 Sales","No 2021 Sales","4820","N/A","N/A",null,null,"4820 2 in STORZ 230 7 BLACK (Std) PG","48200560","OBSI  ASLT NOZ 2.5 52MM 230L@7bar FM",36]
["48200525","OBS ASLT NOZ 1.5NPSH 150G@100P FM",null,null,null,null,null,null,null,null,"0003","Assault","O",1.5,"NPSH","GPM",150,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","1.5\"","N",20,3,"4820","N/A","N/A",null,null,"4820 1.5 in NPSH 150 100 (Std) BLACK (Std) PG","48200525","OBS ASLT NOZ 1.5NPSH 150G@100P FM",45]
["48200579","OBS ASLT NOZ 1.5 NPSH 95G@75P  LP FM",null,null,null,null,null,null,null,null,"0003","Assault","O",1.5,"NPSH","GPM",95,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed","1.5\"","N",20,3,"4820","N/A","N/A",null,null,"4820 1.5 in NPSH 95 75 BLACK (Std) PG","48200579","OBS ASLT NOZ 1.5 NPSH 95G@75P  LP FM",37]
["48244001","ASLT TIP 1.5NH 250G@50P#",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",250,"PSI","N/A",50,"BLACK","N","ENGLISH","Fixed Tip","High-Range","N/A",80,1,"4824","N/A","N/A",null,null,"4824 1.5 in NH 250 50 BLACK (Std) ","48244001","ASLT TIP 1.5NH 250G@50P#",34]
["48244008","ASLT TIP 1.5NH 250G@75P",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",250,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed Tip","High-Range","N/A",20,1,"4824","N/A","N/A",null,null,{"$f":"CONCATENATE(AC276,\" \",N276,\" in \",O276,\" \",IF(AD276=\"n/a\",\"\",CONCATENATE(AD276,\" in \",AE276,\" \")),IF(Q276=\"n/a\",\"\",Q276),IF(S276=\"n/a\",\"\",CONCATENATE(IF(X276=\"saber\",\" \",\"\"),S276,\" bore size(s) \")),IF(T276=\"n/a\",\"\",CONCATENATE(IF(X276=\"saber\",\"\",\" \"),T276,IF(T276=100,\" (Std) \",IF(T276=87,\" (CE) \",\" \")))),IF(U276=\"n/a\",\"\",CONCATENATE(U276,IF(U276=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X276,3)=\"tip\",IF(LEFT(X276,1)=\"s\",\"\",IF(Z276=\"n\",IF(T276=\"N/A\",\"PG\",\" PG\"),IF(Z276=\"y\",IF(T276=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z276=\"n\",IF(T276=\"N/A\",\"PG\",\" PG\"),IF(Z276=\"y\",IF(T276=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF276=\"y\",\" ZT\",\"\"),IF(V276=\"N\",\"\",IF(S276=\"n/a\",\" ETCH\",IF(T276=\"N/A\",IF(RIGHT(X276,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X276=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"4824 1.5 in NH 250 75 BLACK (Std) "},{"$f":"A276","v":"48244008"},{"$f":"B276","v":"ASLT TIP 1.5NH 250G@75P"},{"$f":"LEN(AH276)","v":34}]
["48244032","ASLT TIP 1.5NH 210G@50P YLWBMPR",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",210,"PSI","N/A",50,"YELLOW","N","ENGLISH","Fixed Tip","High-Range","N/A",20,1,"4824","N/A","N/A",null,null,"4824 1.5 in NH 210 50 YELLOW ","48244032","ASLT TIP 1.5NH 210G@50P YLWBMPR",29]
["48244002","ASLT TIP 1.5NH 350G@100P",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",350,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed Tip","High-Range","N/A",20,2,"4824","N/A","N/A",null,null,"4824 1.5 in NH 350 100 (Std) BLACK (Std) ","48244002","ASLT TIP 1.5NH 350G@100P",41]
["48244003","ASLT TIP 1.5NH 300G@75P",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",300,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed Tip","High-Range","N/A",20,2,"4824","N/A","N/A",null,null,"4824 1.5 in NH 300 75 BLACK (Std) ","48244003","ASLT TIP 1.5NH 300G@75P",34]
["48244013","ASLT TIP 1.5NH 300G@100P",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",300,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed Tip","High-Range","N/A",20,2,"4824","N/A","N/A",null,null,"4824 1.5 in NH 300 100 (Std) BLACK (Std) ","48244013","ASLT TIP 1.5NH 300G@100P",41]
["48244017","ASLT TIP 1.5NH 250G@100P",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",250,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed Tip","High-Range","N/A",20,2,"4824","N/A","N/A",null,null,"4824 1.5 in NH 250 100 (Std) BLACK (Std) ","48244017","ASLT TIP 1.5NH 250G@100P",41]
["48244020","ASLT TIP 1.5NPSH 250G@100P",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NPSH","GPM",250,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed Tip","High-Range","N/A",20,2,"4824","N/A","N/A",null,null,"4824 1.5 in NPSH 250 100 (Std) BLACK (Std) ","48244020","ASLT TIP 1.5NPSH 250G@100P",43]
["48244025","ASLT TIP 1.5NH 250G@50P REDBMPR",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",250,"PSI","N/A",50,"RED","N","ENGLISH","Fixed Tip","High-Range","N/A",20,2,"4824","N/A","N/A",null,null,"4824 1.5 in NH 250 50 RED ","48244025","ASLT TIP 1.5NH 250G@50P REDBMPR",26]
["48244035","ASLT TIP 1.5NH 200G@100P",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",200,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed Tip","High-Range","N/A",20,3,"4824","N/A","N/A",null,null,"4824 1.5 in NH 200 100 (Std) BLACK (Std) ","48244035","ASLT TIP 1.5NH 200G@100P",41]
["48244037","ASLT TIP 1.5ABT 250G@50P",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"PCT","GPM",250,"PSI","N/A",50,"BLACK","N","ENGLISH","Fixed Tip","High-Range","N/A",20,3,"4824","N/A","N/A",null,null,"4824 1.5 in PCT 250 50 BLACK (Std) ","48244037","ASLT TIP 1.5ABT 250G@50P",35]
["48244038","ASLT TIP 1.5ABT 210G@50P",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"PCT","GPM",210,"PSI","N/A",50,"BLACK","N","ENGLISH","Fixed Tip","High-Range","N/A",20,3,"4824","N/A","N/A",null,null,"4824 1.5 in PCT 210 50 BLACK (Std) ","48244038","ASLT TIP 1.5ABT 210G@50P",35]
["48244015","ASLT TIP 1.5NH 200G@75P",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",200,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed Tip","High-Range","N/A",20,4,"4824","N/A","N/A",null,null,"4824 1.5 in NH 200 75 BLACK (Std) ","48244015","ASLT TIP 1.5NH 200G@75P",34]
["48244004","ASLT TIP 1.5ABU 250G@100P FDNY",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"FDNY","GPM",250,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","4824","N/A","N/A",null,null,"4824 1.5 in FDNY 250 100 (Std) BLACK (Std) ","48244004","ASLT TIP 1.5ABU 250G@100P FDNY",43]
["48244009","ASLT TIP 1.5NH 250G@75P RED BMPR",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",250,"PSI","N/A",75,"RED","N","ENGLISH","Fixed Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","4824","N/A","N/A",null,null,"4824 1.5 in NH 250 75 RED ","48244009","ASLT TIP 1.5NH 250G@75P RED BMPR",26]
["48244016","ASLT TIP 1.5NPSH 250G@50P",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NPSH","GPM",250,"PSI","N/A",50,"BLACK","N","ENGLISH","Fixed Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","4824","N/A","N/A",null,null,"4824 1.5 in NPSH 250 50 BLACK (Std) ","48244016","ASLT TIP 1.5NPSH 250G@50P",36]
["48244018","ASLT TIP 1.5NPSH 300G@75P",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NPSH","GPM",300,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","4824","N/A","N/A",null,null,"4824 1.5 in NPSH 300 75 BLACK (Std) ","48244018","ASLT TIP 1.5NPSH 300G@75P",36]
["48244019","ASLT TIP 1.5BSP 1325L@7b",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"BSP","LPM",1325,"BAR","N/A",7,"BLACK","N","ENGLISH","Fixed Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","4824","N/A","N/A",null,null,"4824 1.5 in BSP 1325 7 BLACK (Std) ","48244019","ASLT TIP 1.5BSP 1325L@7b",35]
["48244021","ASLT TIP 1.5NH 250G@50P ORGBMPR RBFR",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",250,"PSI","N/A",50,"ORANGE","N","ENGLISH","Fixed Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","4824","N/A","N/A",null,null,"4824 1.5 in NH 250 50 ORANGE ","48244021","ASLT TIP 1.5NH 250G@50P ORGBMPR RBFR",29]
["48244022","ASLT TIP 1.5NH 950L@7b",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","LPM",950,"BAR","N/A",7,"BLACK","N","ENGLISH","Fixed Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","4824","N/A","N/A",null,null,"4824 1.5 in NH 950 7 BLACK (Std) ","48244022","ASLT TIP 1.5NH 950L@7b",33]
["48244023","ASLT TIP 1.5BSP 950L@7b",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"BSP","LPM",950,"BAR","N/A",7,"BLACK","N","ENGLISH","Fixed Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","4824","N/A","N/A",null,null,"4824 1.5 in BSP 950 7 BLACK (Std) ","48244023","ASLT TIP 1.5BSP 950L@7b",34]
["48244030","ASLT TIP 1.5NH 1325L@7b",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","LPM",1325,"BAR","N/A",7,"BLACK","N","ENGLISH","Fixed Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","4824","N/A","N/A",null,null,"4824 1.5 in NH 1325 7 BLACK (Std) ","48244030","ASLT TIP 1.5NH 1325L@7b",34]
["48244031","ASLT TIP 1.5NPSH 1140L@517K",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NPSH","LPM",1140,"kPa","N/A",517,"BLACK","N","ENGLISH","Fixed Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","4824","N/A","N/A",null,null,"4824 1.5 in NPSH 1140 517 BLACK (Std) ","48244031","ASLT TIP 1.5NPSH 1140L@517K",38]
["48244043","ASLT TIP 1.5NPSH 1140L@5B",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NPSH","LPM",1140,"BAR","N/A",5,"BLACK","N","ENGLISH","Fixed Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","4824","N/A","N/A",null,null,{"$f":"CONCATENATE(AC298,\" \",N298,\" in \",O298,\" \",IF(AD298=\"n/a\",\"\",CONCATENATE(AD298,\" in \",AE298,\" \")),IF(Q298=\"n/a\",\"\",Q298),IF(S298=\"n/a\",\"\",CONCATENATE(IF(X298=\"saber\",\" \",\"\"),S298,\" bore size(s) \")),IF(T298=\"n/a\",\"\",CONCATENATE(IF(X298=\"saber\",\"\",\" \"),T298,IF(T298=100,\" (Std) \",IF(T298=87,\" (CE) \",\" \")))),IF(U298=\"n/a\",\"\",CONCATENATE(U298,IF(U298=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X298,3)=\"tip\",IF(LEFT(X298,1)=\"s\",\"\",IF(Z298=\"n\",IF(T298=\"N/A\",\"PG\",\" PG\"),IF(Z298=\"y\",IF(T298=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z298=\"n\",IF(T298=\"N/A\",\"PG\",\" PG\"),IF(Z298=\"y\",IF(T298=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF298=\"y\",\" ZT\",\"\"),IF(V298=\"N\",\"\",IF(S298=\"n/a\",\" ETCH\",IF(T298=\"N/A\",IF(RIGHT(X298,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X298=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"4824 1.5 in NPSH 1140 5 BLACK (Std) "},{"$f":"A298","v":"48244043"},{"$f":"B298","v":"ASLT TIP 1.5NPSH 1140L@5B"},{"$f":"LEN(AH298)","v":36}]
["48244034","ASLT TIP 1.5NH 250G@50P YLWBMPR",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",250,"PSI","N/A",50,"YELLOW","N","ENGLISH","Fixed Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","4824","N/A","N/A",null,null,"4824 1.5 in NH 250 50 YELLOW ","48244034","ASLT TIP 1.5NH 250G@50P YLWBMPR",29]
["48244042","ASLT TIP 1.5NH 210G@50P",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",210,"PSI","N/A",50,"BLACK","N","ENGLISH","Fixed Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","4824","N/A","N/A",null,null,"4824 1.5 in NH 210 50 BLACK (Std) ","48244042","ASLT TIP 1.5NH 210G@50P",34]
["48244040","ASLT TIP 1.5NPSH 750L@7b",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NPSH","LPM",750,"BAR","N/A",7,"BLACK","N","ENGLISH","Fixed Tip","High-Range","N/A",20,4,"4824","N/A","N/A",null,null,"4824 1.5 in NPSH 750 7 BLACK (Std) ","48244040","ASLT TIP 1.5NPSH 750L@7b",35]
["48244041","ASLT TIP 1.5NPSH 300G@100P",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NPSH","GPM",300,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed Tip","High-Range","N/A",20,4,"4824","N/A","N/A",null,null,"4824 1.5 in NPSH 300 100 (Std) BLACK (Std) ","48244041","ASLT TIP 1.5NPSH 300G@100P",43]
["48260654","ASLT NOZ 2.5AFB 250G@100P PG&SPTH FDNY",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"FDNY","GPM",250,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","High-Range","N",80,1,"4826","N/A","N/A",null,null,"4826 2.5 in FDNY 250 100 (Std) BLACK (Std) PG","48260654","ASLT NOZ 2.5AFB 250G@100P PG&SPTH FDNY",45]
["48264004","ASLT 2.5BIM 950L@7b FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"BIM","LPM",950,"BAR","N/A",7,"BLACK","N","ENGLISH","Fixed","High-Range","N",80,1,"4826","N/A","N/A",null,null,"4826 2.5 in BIM 950 7 BLACK (Std) PG","48264004","ASLT 2.5BIM 950L@7b FM",36]
["48264005","ASLT 2.5NH 200G@100P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"NH","GPM",200,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","High-Range","N",80,1,"4826","N/A","N/A",null,null,"4826 2.5 in NH 200 100 (Std) BLACK (Std) PG","48264005","ASLT 2.5NH 200G@100P FM",43]
["48264002","ASLT 2.5BIM 250G@75P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"BIM","GPM",250,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed","High-Range","N",20,1,"4826","N/A","N/A",null,null,"4826 2.5 in BIM 250 75 BLACK (Std) PG","48264002","ASLT 2.5BIM 250G@75P FM",37]
["48264006","ASLT 2.5NH 250G@50P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"NH","GPM",250,"PSI","N/A",50,"BLACK","N","ENGLISH","Fixed","High-Range","N",20,1,"4826","N/A","N/A",null,null,"4826 2.5 in NH 250 50 BLACK (Std) PG","48264006","ASLT 2.5NH 250G@50P FM",36]
["48264051","ASLT 2.5AHB 250G@50P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"AHB","GPM",250,"PSI","N/A",50,"BLACK","N","ENGLISH","Fixed","High-Range","N",20,1,"4826","N/A","N/A",null,null,{"$f":"CONCATENATE(AC308,\" \",N308,\" in \",O308,\" \",IF(AD308=\"n/a\",\"\",CONCATENATE(AD308,\" in \",AE308,\" \")),IF(Q308=\"n/a\",\"\",Q308),IF(S308=\"n/a\",\"\",CONCATENATE(IF(X308=\"saber\",\" \",\"\"),S308,\" bore size(s) \")),IF(T308=\"n/a\",\"\",CONCATENATE(IF(X308=\"saber\",\"\",\" \"),T308,IF(T308=100,\" (Std) \",IF(T308=87,\" (CE) \",\" \")))),IF(U308=\"n/a\",\"\",CONCATENATE(U308,IF(U308=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X308,3)=\"tip\",IF(LEFT(X308,1)=\"s\",\"\",IF(Z308=\"n\",IF(T308=\"N/A\",\"PG\",\" PG\"),IF(Z308=\"y\",IF(T308=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z308=\"n\",IF(T308=\"N/A\",\"PG\",\" PG\"),IF(Z308=\"y\",IF(T308=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF308=\"y\",\" ZT\",\"\"),IF(V308=\"N\",\"\",IF(S308=\"n/a\",\" ETCH\",IF(T308=\"N/A\",IF(RIGHT(X308,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X308=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"4826 2.5 in AHB 250 50 BLACK (Std) PG"},{"$f":"A308","v":"48264051"},{"$f":"B308","v":"ASLT 2.5AHB 250G@50P FM"},{"$f":"LEN(AH308)","v":37}]
["48264007","ASLT 2.5NH 250G@75P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"NH","GPM",250,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed","High-Range","N",20,1,"4826","N/A","N/A",null,null,"4826 2.5 in NH 250 75 BLACK (Std) PG","48264007","ASLT 2.5NH 250G@75P FM",36]
["48264008","ASLT 2.5NH 250G@100P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"NH","GPM",250,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","High-Range","N",20,1,"4826","N/A","N/A",null,null,"4826 2.5 in NH 250 100 (Std) BLACK (Std) PG","48264008","ASLT 2.5NH 250G@100P FM",43]
["48264013","ASLT 2.5NH 300G@75P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"NH","GPM",300,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed","High-Range","N",20,1,"4826","N/A","N/A",null,null,"4826 2.5 in NH 300 75 BLACK (Std) PG","48264013","ASLT 2.5NH 300G@75P FM",36]
["48264026","ASLT 2.5NH 200G@75P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"NH","GPM",200,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed","High-Range","N",20,1,"4826","N/A","N/A",null,null,"4826 2.5 in NH 200 75 BLACK (Std) PG","48264026","ASLT 2.5NH 200G@75P FM",36]
["48264048","ASLT 2.5BSP 1140L@7b FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"BSP","LPM",1140,"BAR","N/A",7,"BLACK","N","ENGLISH","Fixed","High-Range","N",20,1,"4826","N/A","N/A",null,null,"4826 2.5 in BSP 1140 7 BLACK (Std) PG","48264048","ASLT 2.5BSP 1140L@7b FM",37]
["48264009","ASLT 2.5NH 350G@100P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"NH","GPM",350,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","High-Range","N",20,2,"4826","N/A","N/A",null,null,"4826 2.5 in NH 350 100 (Std) BLACK (Std) PG","48264009","ASLT 2.5NH 350G@100P FM",43]
["48264020","ASLT 2.5AII 950L@700K FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"CSA","LPM",950,"kPa","N/A",700,"BLACK","N","ENGLISH","Fixed","High-Range","N",20,2,"4826","N/A","N/A",null,null,"4826 2.5 in CSA 950 700 BLACK (Std) PG","48264020","ASLT 2.5AII 950L@700K FM",38]
["48264021","ASLT 2.5NH 300G@100P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"NH","GPM",300,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","High-Range","N",20,2,"4826","N/A","N/A",null,null,"4826 2.5 in NH 300 100 (Std) BLACK (Std) PG","48264021","ASLT 2.5NH 300G@100P FM",43]
["48264024","ASLT 2.5AII 950L@350K",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"CSA","LPM",950,"kPA","N/A",350,"BLACK","N","ENGLISH","Fixed","High-Range","N",20,2,"4826","N/A","N/A",null,null,"4826 2.5 in CSA 950 350 BLACK (Std) PG","48264024","ASLT 2.5AII 950L@350K",38]
["48264038","ASLT 2.5BAF 200G@75P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"BAT","GPM",200,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed","High-Range","N",20,2,"4826","N/A","N/A",null,null,"4826 2.5 in BAT 200 75 BLACK (Std) PG","48264038","ASLT 2.5BAF 200G@75P FM",37]
["48264040","ASLT ZT 1.5NH 200G@100P",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",200,"PSI","N/A",100,"Black","N","ENGLISH","Fixed","High-Range","N",20,2,"4826","N/A","N/A","Y",null,"4826 1.5 in NH 200 100 (Std) Black (Std) PG ZT","48264040","ASLT ZT 1.5NH 200G@100P",46]
["48264041","ASLT 1.5NH 200G@100P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",200,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","Mid-Range","N",20,2,"4826","N/A","N/A",null,null,"4826 1.5 in NH 200 100 (Std) BLACK (Std) PG","48264041","ASLT 1.5NH 200G@100P FM",43]
["48267006","ASLT NPG 2.5NH 250G@50P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"NH","GPM",250,"PSI","N/A",50,"BLACK","N","ENGLISH","Fixed","High-Range","Y",20,2,"4826","N/A","N/A",null,null,"4826 2.5 in NH 250 50 BLACK (Std) NPG","48267006","ASLT NPG 2.5NH 250G@50P FM",37]
["48267007","ASLT NPG 2.5NH 250G@75P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"NH","GPM",250,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed","High-Range","Y",20,2,"4826","N/A","N/A",null,null,"4826 2.5 in NH 250 75 BLACK (Std) NPG","48267007","ASLT NPG 2.5NH 250G@75P FM",37]
["48264001","ASLT 2.5AFB 250G@100P FDNY",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"FDNY","GPM",250,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","High-Range","N",20,3,"4826","N/A","N/A",null,null,"4826 2.5 in FDNY 250 100 (Std) BLACK (Std) PG","48264001","ASLT 2.5AFB 250G@100P FDNY",45]
["48264012","ASLT ZT 2.5NH 250G@75P",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"NH","GPM",250,"PSI","N/A",75,"Black","N","ENGLISH","Fixed","High-Range","N",20,3,"4826","N/A","N/A","Y",null,"4826 2.5 in NH 250 75 Black (Std) PG ZT","48264012","ASLT ZT 2.5NH 250G@75P",39]
["48264015","ASLT ZT 2.5NH 250G@100P",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"NH","GPM",250,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","High-Range","N",20,3,"4826","N/A","N/A","Y",null,"4826 2.5 in NH 250 100 (Std) BLACK (Std) PG ZT","48264015","ASLT ZT 2.5NH 250G@100P",46]
["48264017","ASLT 2.5BAF 250G@100P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"BAT","GPM",250,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","High-Range","N",20,3,"4826","N/A","N/A",null,null,"4826 2.5 in BAT 250 100 (Std) BLACK (Std) PG","48264017","ASLT 2.5BAF 250G@100P FM",44]
["48264019","ASLT 1.5NH 250G@75P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",250,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed","High-Range","N",20,3,"4826","N/A","N/A",null,null,"4826 1.5 in NH 250 75 BLACK (Std) PG","48264019","ASLT 1.5NH 250G@75P FM",36]
["48264031","ASLT ZT 2.5NH 250G@50P",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"NH","GPM",250,"PSI","N/A",50,"BLACK","N","ENGLISH","Fixed","High-Range","N",20,3,"4826","N/A","N/A","Y",null,"4826 2.5 in NH 250 50 BLACK (Std) PG ZT","48264031","ASLT ZT 2.5NH 250G@50P",39]
["48264039","ASLT 2.5BAF 300G@75P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"BAT","GPM",300,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed","High-Range","N",20,3,"4826","N/A","N/A",null,null,"4826 2.5 in BAT 300 75 BLACK (Std) PG","48264039","ASLT 2.5BAF 300G@75P FM",37]
["48264042","ASLT 2.5AFY 250G@50P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"PITT6","GPM",250,"PSI","N/A",50,"BLACK","N","ENGLISH","Fixed","High-Range","N",20,3,"4826","N/A","N/A",null,null,"4826 2.5 in PITT6 250 50 BLACK (Std) PG","48264042","ASLT 2.5AFY 250G@50P FM",39]
["48264044","ASLT 2.5NH 250G@50P BFC-E1",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"NH","GPM",250,"PSI","N/A",50,"BLACK","Y","ENGLISH","Fixed","High-Range","N",20,3,"4826","N/A","N/A",null,null,"4826 2.5 in NH 250 50 BLACK (Std) PG ETCH","48264044","ASLT 2.5NH 250G@50P BFC-E1",41]
["48264045","ASLT 2.5NH 250G@50P BFC-T5",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"NH","GPM",250,"PSI","N/A",50,"BLACK","Y","ENGLISH","Fixed","High-Range","N",20,3,"4826","N/A","N/A",null,null,"4826 2.5 in NH 250 50 BLACK (Std) PG ETCH","48264045","ASLT 2.5NH 250G@50P BFC-T5",41]
["48264046","ASLT 2.5NH 250G@50P BFC-E2",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"NH","GPM",250,"PSI","N/A",50,"BLACK","Y","ENGLISH","Fixed","High-Range","N",20,3,"4826","N/A","N/A",null,null,"4826 2.5 in NH 250 50 BLACK (Std) PG ETCH","48264046","ASLT 2.5NH 250G@50P BFC-E2",41]
["48264047","ASLT 2.5AII 250G@50P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"CSA","GPM",250,"PSI","N/A",50,"BLACK","N","ENGLISH","Fixed","High-Range","N",20,3,"4826","N/A","N/A",null,null,"4826 2.5 in CSA 250 50 BLACK (Std) PG","48264047","ASLT 2.5AII 250G@50P FM",37]
["48267008","ASLT NPG 2.5NH 250G@100P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"NH","GPM",250,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","High-Range","Y",20,3,"4826","N/A","N/A",null,null,"4826 2.5 in NH 250 100 (Std) BLACK (Std) NPG","48267008","ASLT NPG 2.5NH 250G@100P FM",44]
["48267013","ASLT NPG 2.5NH 300G@75P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"NH","GPM",300,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed","High-Range","Y",20,3,"4826","N/A","N/A",null,null,"4826 2.5 in NH 300 75 BLACK (Std) NPG","48267013","ASLT NPG 2.5NH 300G@75P FM",37]
["48267030","ASLT NPG 2.5NH 250G@75P W/MTLHDL",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"NH","GPM",250,"PSI","N/A",75,"Black","N","ENGLISH","Fixed","High-Range","Y",20,3,"4826","N/A","N/A",null,null,"4826 2.5 in NH 250 75 Black (Std) NPG","48267030","ASLT NPG 2.5NH 250G@75P W/MTLHDL",37]
["48267039","ASLT NPG 2.5AFY 250G@100P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"PITT6","GPM",250,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","High-Range","Y",20,3,"4826","N/A","N/A",null,null,"4826 2.5 in PITT6 250 100 (Std) BLACK (Std) NPG","48267039","ASLT NPG 2.5AFY 250G@100P FM",47]
["48267043","ASLT NPG 1.5NH 200G@75P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",200,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed","High-Range","Y",20,3,"4826","N/A","N/A",null,null,"4826 1.5 in NH 200 75 BLACK (Std) NPG","48267043","ASLT NPG 1.5NH 200G@75P FM",37]
["48267044","ASLT NPG 2.5AFY 250G@75P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"PITT6","GPM",250,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed","High-Range","Y",20,3,"4826","N/A","N/A",null,null,"4826 2.5 in PITT6 250 75 BLACK (Std) NPG","48267044","ASLT NPG 2.5AFY 250G@75P FM",40]
["48267045","ASLT NPG 2.5ASN 250G@100P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"ASN","GPM",250,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","High-Range","Y",20,3,"4826","N/A","N/A",null,null,"4826 2.5 in ASN 250 100 (Std) BLACK (Std) NPG","48267045","ASLT NPG 2.5ASN 250G@100P FM",45]
["48264003","ASLT 2.5BIM 750L@7b FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"BIM","LPM",750,"BAR","N/A",7,"BLACK","N","ENGLISH","Fixed","High-Range","N","No 2021 Sales","No 2021 Sales","4826","N/A","N/A",null,null,{"$f":"CONCATENATE(AC342,\" \",N342,\" in \",O342,\" \",IF(AD342=\"n/a\",\"\",CONCATENATE(AD342,\" in \",AE342,\" \")),IF(Q342=\"n/a\",\"\",Q342),IF(S342=\"n/a\",\"\",CONCATENATE(IF(X342=\"saber\",\" \",\"\"),S342,\" bore size(s) \")),IF(T342=\"n/a\",\"\",CONCATENATE(IF(X342=\"saber\",\"\",\" \"),T342,IF(T342=100,\" (Std) \",IF(T342=87,\" (CE) \",\" \")))),IF(U342=\"n/a\",\"\",CONCATENATE(U342,IF(U342=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X342,3)=\"tip\",IF(LEFT(X342,1)=\"s\",\"\",IF(Z342=\"n\",IF(T342=\"N/A\",\"PG\",\" PG\"),IF(Z342=\"y\",IF(T342=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z342=\"n\",IF(T342=\"N/A\",\"PG\",\" PG\"),IF(Z342=\"y\",IF(T342=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF342=\"y\",\" ZT\",\"\"),IF(V342=\"N\",\"\",IF(S342=\"n/a\",\" ETCH\",IF(T342=\"N/A\",IF(RIGHT(X342,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X342=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"4826 2.5 in BIM 750 7 BLACK (Std) PG"},{"$f":"A342","v":"48264003"},{"$f":"B342","v":"ASLT 2.5BIM 750L@7b FM"},{"$f":"LEN(AH342)","v":36}]
["48264010","ASLT 2.5NH 950L@7b FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"NH","LPM",950,"BAR","N/A",7,"BLACK","N","ENGLISH","Fixed","High-Range","N","No 2021 Sales","No 2021 Sales","4826","N/A","N/A",null,null,"4826 2.5 in NH 950 7 BLACK (Std) PG","48264010","ASLT 2.5NH 950L@7b FM",35]
["48264011","ASLT 2.5AIK 300G@75P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"AIK","GPM",300,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed","High-Range","N","No 2021 Sales","No 2021 Sales","4826","N/A","N/A",null,null,"4826 2.5 in AIK 300 75 BLACK (Std) PG","48264011","ASLT 2.5AIK 300G@75P FM",37]
["48264014","ASLT 2.5AGZ 250G@75P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"AGZ","GPM",250,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed","High-Range","N","No 2021 Sales","No 2021 Sales","4826","N/A","N/A",null,null,"4826 2.5 in AGZ 250 75 BLACK (Std) PG","48264014","ASLT 2.5AGZ 250G@75P FM",37]
["48264018","ASLT 2.5AKB 250G@100P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"AKB","GPM",250,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","High-Range","N","No 2021 Sales","No 2021 Sales","4826","N/A","N/A",null,null,"4826 2.5 in AKB 250 100 (Std) BLACK (Std) PG","48264018","ASLT 2.5AKB 250G@100P FM",44]
["48264022","ASLT 2.5BIM 350G@100P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"BIM","GPM",350,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","High-Range","N","No 2021 Sales","No 2021 Sales","4826","N/A","N/A",null,null,"4826 2.5 in BIM 350 100 (Std) BLACK (Std) PG","48264022","ASLT 2.5BIM 350G@100P FM",44]
["48264025","ASLT 2.5BSP 750L@5b FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"BSP","LPM",750,"BAR","N/A",5,"BLACK","N","ENGLISH","Fixed","High-Range","N","No 2021 Sales","No 2021 Sales","4826","N/A","N/A",null,null,"4826 2.5 in BSP 750 5 BLACK (Std) PG","48264025","ASLT 2.5BSP 750L@5b FM",36]
["48264027","ASLT 2.5AHB 250G@100P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"AHB","GPM",250,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","High-Range","N","No 2021 Sales","No 2021 Sales","4826","N/A","N/A",null,null,"4826 2.5 in AHB 250 100 (Std) BLACK (Std) PG","48264027","ASLT 2.5AHB 250G@100P FM",44]
["48264028","ASLT 2.5NH 250G@50P YLWBMPR FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"NH","GPM",250,"PSI","N/A",50,"YELLOW","N","ENGLISH","Fixed","High-Range","N","No 2021 Sales","No 2021 Sales","4826","N/A","N/A",null,null,"4826 2.5 in NH 250 50 YELLOW PG","48264028","ASLT 2.5NH 250G@50P YLWBMPR FM",31]
["48264029","ASLT 2.5AJN 250G@75P ORGBMPR FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"AJN","GPM",250,"PSI","N/A",75,"ORANGE","N","ENGLISH","Fixed","High-Range","N","No 2021 Sales","No 2021 Sales","4826","N/A","N/A",null,null,"4826 2.5 in AJN 250 75 ORANGE PG","48264029","ASLT 2.5AJN 250G@75P ORGBMPR FM",32]
["48264032","ASLT 2.5AJZ 250G@50P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"AJZ","GPM",250,"PSI","N/A",50,"BLACK","N","ENGLISH","Fixed","High-Range","N","No 2021 Sales","No 2021 Sales","4826","N/A","N/A",null,null,"4826 2.5 in AJZ 250 50 BLACK (Std) PG","48264032","ASLT 2.5AJZ 250G@50P FM",37]
["48264053","ASLT 2.5NH 250G@75P ORGBMPR FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"NH","GPM",250,"PSI","N/A",75,"ORANGE","N","ENGLISH","Fixed","High-Range","N","No 2021 Sales","No 2021 Sales","4826","N/A","N/A",null,null,{"$f":"CONCATENATE(AC353,\" \",N353,\" in \",O353,\" \",IF(AD353=\"n/a\",\"\",CONCATENATE(AD353,\" in \",AE353,\" \")),IF(Q353=\"n/a\",\"\",Q353),IF(S353=\"n/a\",\"\",CONCATENATE(IF(X353=\"saber\",\" \",\"\"),S353,\" bore size(s) \")),IF(T353=\"n/a\",\"\",CONCATENATE(IF(X353=\"saber\",\"\",\" \"),T353,IF(T353=100,\" (Std) \",IF(T353=87,\" (CE) \",\" \")))),IF(U353=\"n/a\",\"\",CONCATENATE(U353,IF(U353=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X353,3)=\"tip\",IF(LEFT(X353,1)=\"s\",\"\",IF(Z353=\"n\",IF(T353=\"N/A\",\"PG\",\" PG\"),IF(Z353=\"y\",IF(T353=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z353=\"n\",IF(T353=\"N/A\",\"PG\",\" PG\"),IF(Z353=\"y\",IF(T353=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF353=\"y\",\" ZT\",\"\"),IF(V353=\"N\",\"\",IF(S353=\"n/a\",\" ETCH\",IF(T353=\"N/A\",IF(RIGHT(X353,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X353=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"4826 2.5 in NH 250 75 ORANGE PG"},{"$f":"A353","v":"48264053"},{"$f":"B353","v":"ASLT 2.5NH 250G@75P ORGBMPR FM"},{"$f":"LEN(AH353)","v":31}]
["48264054","ASLT 2.5NH 250G@100P YLWBMPR FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"NH","GPM",250,"PSI","N/A",100,"YELLOW","N","ENGLISH","Fixed","High-Range","N","No 2021 Sales","No 2021 Sales","4826","N/A","N/A",null,null,{"$f":"CONCATENATE(AC354,\" \",N354,\" in \",O354,\" \",IF(AD354=\"n/a\",\"\",CONCATENATE(AD354,\" in \",AE354,\" \")),IF(Q354=\"n/a\",\"\",Q354),IF(S354=\"n/a\",\"\",CONCATENATE(IF(X354=\"saber\",\" \",\"\"),S354,\" bore size(s) \")),IF(T354=\"n/a\",\"\",CONCATENATE(IF(X354=\"saber\",\"\",\" \"),T354,IF(T354=100,\" (Std) \",IF(T354=87,\" (CE) \",\" \")))),IF(U354=\"n/a\",\"\",CONCATENATE(U354,IF(U354=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X354,3)=\"tip\",IF(LEFT(X354,1)=\"s\",\"\",IF(Z354=\"n\",IF(T354=\"N/A\",\"PG\",\" PG\"),IF(Z354=\"y\",IF(T354=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z354=\"n\",IF(T354=\"N/A\",\"PG\",\" PG\"),IF(Z354=\"y\",IF(T354=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF354=\"y\",\" ZT\",\"\"),IF(V354=\"N\",\"\",IF(S354=\"n/a\",\" ETCH\",IF(T354=\"N/A\",IF(RIGHT(X354,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X354=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"4826 2.5 in NH 250 100 (Std) YELLOW PG"},{"$f":"A354","v":"48264054"},{"$f":"B354","v":"ASLT 2.5NH 250G@100P YLWBMPR FM"},{"$f":"LEN(AH354)","v":38}]
["48264033","ASLT ZT 2.5AJN 200G@75P",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"AJN","GPM",200,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed","High-Range","N","No 2021 Sales","No 2021 Sales","4826","N/A","N/A","Y",null,"4826 2.5 in AJN 200 75 BLACK (Std) PG ZT","48264033","ASLT ZT 2.5AJN 200G@75P",40]
["48264034","ASLT 2.5BSP 950L@7b FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"BSP","LPM",950,"BAR","N/A",7,"BLACK","N","ENGLISH","Fixed","High-Range","N","No 2021 Sales","No 2021 Sales","4826","N/A","N/A",null,null,"4826 2.5 in BSP 950 7 BLACK (Std) PG","48264034","ASLT 2.5BSP 950L@7b FM",36]
["48264035","ASLT 2.5AII 950L@500K FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"CSA","LPM",950,"kPA","N/A",500,"BLACK","N","ENGLISH","Fixed","High-Range","N","No 2021 Sales","No 2021 Sales","4826","N/A","N/A",null,null,"4826 2.5 in CSA 950 500 BLACK (Std) PG","48264035","ASLT 2.5AII 950L@500K FM",38]
["48264036","ASLT 2.5NH 250G@75P YLWBMPR FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"NH","GPM",250,"PSI","N/A",75,"YELLOW","N","ENGLISH","Fixed","High-Range","N","No 2021 Sales","No 2021 Sales","4826","N/A","N/A",null,null,"4826 2.5 in NH 250 75 YELLOW PG","48264036","ASLT 2.5NH 250G@75P YLWBMPR FM",31]
["48264037","ASLT 2.5NH 210G@50P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"NH","GPM",210,"PSI","N/A",50,"BLACK","N","ENGLISH","Fixed","High-Range","N","No 2021 Sales","No 2021 Sales","4826","N/A","N/A",null,null,"4826 2.5 in NH 210 50 BLACK (Std) PG","48264037","ASLT 2.5NH 210G@50P FM",36]
["48264049","ASLT 2.5BAF 250G@50P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"BAT","GPM",250,"PSI","N/A",50,"BLACK","N","ENGLISH","Fixed","High-Range","N","No 2021 Sales","No 2021 Sales","4826","N/A","N/A",null,null,"4826 2.5 in BAT 250 50 BLACK (Std) PG","48264049","ASLT 2.5BAF 250G@50P FM",37]
["48264050","ASLT 1.5NH 350G@100P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",350,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","High-Range","N","No 2021 Sales","No 2021 Sales","4826","N/A","N/A",null,null,"4826 1.5 in NH 350 100 (Std) BLACK (Std) PG","48264050","ASLT 1.5NH 350G@100P FM",43]
["48264052","ASLT 2.5AII 200G@75P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"CSA","GPM",200,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed","High-Range","N","No 2021 Sales","No 2021 Sales","4826","N/A","N/A",null,null,"4826 2.5 in CSA 200 75 BLACK (Std) PG","48264052","ASLT 2.5AII 200G@75P FM",37]
["48267002","ASLT NPG 2.5NH 300G@100P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"NH","GPM",300,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","High-Range","Y","No 2021 Sales","No 2021 Sales","4826","N/A","N/A",null,null,"4826 2.5 in NH 300 100 (Std) BLACK (Std) NPG","48267002","ASLT NPG 2.5NH 300G@100P FM",44]
["48267012","ASLT NPG 2.5ACY 300G@100P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"ACY","GPM",300,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","High-Range","Y","No 2021 Sales","No 2021 Sales","4826","N/A","N/A",null,null,"4826 2.5 in ACY 300 100 (Std) BLACK (Std) NPG","48267012","ASLT NPG 2.5ACY 300G@100P FM",45]
["48267014","ASLT NPG 2.5AGZ 250G@75P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"AGZ","GPM",250,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed","High-Range","Y","No 2021 Sales","No 2021 Sales","4826","N/A","N/A",null,null,"4826 2.5 in AGZ 250 75 BLACK (Std) NPG","48267014","ASLT NPG 2.5AGZ 250G@75P FM",38]
["48267024","ASLT NPG 2.5AII 950L@350K",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"CSA","LPM",950,"kPa","N/A",350,"BLACK","N","ENGLISH","Fixed","High-Range","Y","No 2021 Sales","No 2021 Sales","4826","N/A","N/A",null,null,"4826 2.5 in CSA 950 350 BLACK (Std) NPG","48267024","ASLT NPG 2.5AII 950L@350K",39]
["48267026","ASLT NPG 2.5NH 200G@75P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"NH","GPM",200,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed","High-Range","Y","No 2021 Sales","No 2021 Sales","4826","N/A","N/A",null,null,"4826 2.5 in NH 200 75 BLACK (Std) NPG","48267026","ASLT NPG 2.5NH 200G@75P FM",37]
["48267028","ASLT NPG 2.5NH 250G@50P YLWBMPR FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"NH","GPM",250,"PSI","N/A",50,"YELLOW","N","ENGLISH","Fixed","High-Range","Y","No 2021 Sales","No 2021 Sales","4826","N/A","N/A",null,null,"4826 2.5 in NH 250 50 YELLOW NPG","48267028","ASLT NPG 2.5NH 250G@50P YLWBMPR FM",32]
["48267037","ASLT NPG 2.5NH 210G@50P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"NH","GPM",210,"PSI","N/A",50,"BLACK","N","ENGLISH","Fixed","High-Range","Y","No 2021 Sales","No 2021 Sales","4826","N/A","N/A",null,null,"4826 2.5 in NH 210 50 BLACK (Std) NPG","48267037","ASLT NPG 2.5NH 210G@50P FM",37]
["48267046","ASLT NPG 1.5NH 300G@100P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",300,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","High-Range","Y","No 2021 Sales","No 2021 Sales","4826","N/A","N/A",null,null,"4826 1.5 in NH 300 100 (Std) BLACK (Std) NPG","48267046","ASLT NPG 1.5NH 300G@100P FM",44]
["48634007","ASLT 1.5NH 150G@100P FM#",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","Mid-Range","N",80,1,"4863","N/A","N/A",null,null,"4863 1.5 in NH 150 100 (Std) BLACK (Std) PG","48634007","ASLT 1.5NH 150G@100P FM#",43]
["48634008","ASLT 1.5NH 150G@75P FM#",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed","Mid-Range","N",80,1,"4863","N/A","N/A",null,null,"4863 1.5 in NH 150 75 BLACK (Std) PG","48634008","ASLT 1.5NH 150G@75P FM#",36]
["48634009","ASLT 1.5NH 175G@75P FM#",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",175,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed","Mid-Range","N",80,1,"4863","N/A","N/A",null,null,"4863 1.5 in NH 175 75 BLACK (Std) PG","48634009","ASLT 1.5NH 175G@75P FM#",36]
["48634013","ASLT 1.5BSP 750L@7b FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"BSP","LPM",750,"BAR","N/A",7,"BLACK","N","ENGLISH","Fixed","Mid-Range","N",80,1,"4863","N/A","N/A",null,null,"4863 1.5 in BSP 750 7 BLACK (Std) PG","48634013","ASLT 1.5BSP 750L@7b FM",36]
["48634026","ASLT 1.5NH 185G@50P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",185,"PSI","N/A",50,"BLACK","N","ENGLISH","Fixed","Mid-Range","N",80,1,"4863","N/A","N/A",null,null,"4863 1.5 in NH 185 50 BLACK (Std) PG","48634026","ASLT 1.5NH 185G@50P FM",36]
["48634029","ASLT 1.5NH 150G@50P FM#",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",50,"BLACK","N","ENGLISH","Fixed","Mid-Range","N",80,1,"4863","N/A","N/A",null,null,"4863 1.5 in NH 150 50 BLACK (Std) PG","48634029","ASLT 1.5NH 150G@50P FM#",36]
["48634038","ASLT 1.5NH 161G@50P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",161,"PSI","N/A",50,"BLACK","N","ENGLISH","Fixed","Mid-Range","N",80,1,"4863","N/A","N/A",null,null,"4863 1.5 in NH 161 50 BLACK (Std) PG","48634038","ASLT 1.5NH 161G@50P FM",36]
["48634001","ASLT 1.5NH 200G@75P FM#",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",200,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed","Mid-Range","N",20,1,"4863","N/A","N/A",null,null,"4863 1.5 in NH 200 75 BLACK (Std) PG","48634001","ASLT 1.5NH 200G@75P FM#",36]
["48634006","ASLT 1.5NH 125G@100P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",125,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","Mid-Range","N",20,1,"4863","N/A","N/A",null,null,"4863 1.5 in NH 125 100 (Std) BLACK (Std) PG","48634006","ASLT 1.5NH 125G@100P FM",43]
["48634019","ASLT 1.5NH 95G@100P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",95,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","Mid-Range","N",20,1,"4863","N/A","N/A",null,null,"4863 1.5 in NH 95 100 (Std) BLACK (Std) PG","48634019","ASLT 1.5NH 95G@100P FM",42]
["48634025","ASLT 1.5NPSH 150G@75P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NPSH","GPM",150,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed","Mid-Range","N",20,1,"4863","N/A","N/A",null,null,"4863 1.5 in NPSH 150 75 BLACK (Std) PG","48634025","ASLT 1.5NPSH 150G@75P FM",38]
["48634054","ASLT 1.5NH 175G@100P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",175,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","Mid-Range","N",20,1,"4863","N/A","N/A",null,null,"4863 1.5 in NH 175 100 (Std) BLACK (Std) PG","48634054","ASLT 1.5NH 175G@100P FM",43]
["48637007","ASLT NPG 1.5NH 150G@100P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","Mid-Range","Y",20,1,"4863","N/A","N/A",null,null,"4863 1.5 in NH 150 100 (Std) BLACK (Std) NPG","48637007","ASLT NPG 1.5NH 150G@100P FM",44]
["48637029","ASLT NPG 1.5NH 150G@50P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",50,"BLACK","N","ENGLISH","Fixed","Mid-Range","Y",20,1,"4863","N/A","N/A",null,null,"4863 1.5 in NH 150 50 BLACK (Std) NPG","48637029","ASLT NPG 1.5NH 150G@50P FM",37]
["48637061","ASLT NPG 1.5ABU 200G@100P FDNY",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"FDNY","GPM",200,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","Mid-Range","Y",20,1,"4863","N/A","N/A",null,null,"4863 1.5 in FDNY 200 100 (Std) BLACK (Std) NPG","48637061","ASLT NPG 1.5ABU 200G@100P FDNY",46]
["48634005","ASLT 1.5NH 125G@75P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",125,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed","Mid-Range","N",20,2,"4863","N/A","N/A",null,null,"4863 1.5 in NH 125 75 BLACK (Std) PG","48634005","ASLT 1.5NH 125G@75P FM",36]
["48634011","ASLT 1.5NPSH 150G@50P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NPSH","GPM",150,"PSI","N/A",50,"BLACK","N","ENGLISH","Fixed","Mid-Range","N",20,2,"4863","N/A","N/A",null,null,"4863 1.5 in NPSH 150 50 BLACK (Std) PG","48634011","ASLT 1.5NPSH 150G@50P FM",38]
["48634028","ASLT 1.5NH 175G@50P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",175,"PSI","N/A",50,"BLACK","N","ENGLISH","Fixed","Mid-Range","N",20,2,"4863","N/A","N/A",null,null,"4863 1.5 in NH 175 50 BLACK (Std) PG","48634028","ASLT 1.5NH 175G@50P FM",36]
["48634032","ASLT 1.5NH 150G@75P YLWBMPR FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",75,"YELLOW","N","ENGLISH","Fixed","Mid-Range","N",20,2,"4863","N/A","N/A",null,null,"4863 1.5 in NH 150 75 YELLOW PG","48634032","ASLT 1.5NH 150G@75P YLWBMPR FM",31]
["48634037","ASLT 1.5NH 150G@75P REDBMPR FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",75,"RED","N","ENGLISH","Fixed","Mid-Range","N",20,2,"4863","N/A","N/A",null,null,"4863 1.5 in NH 150 75 RED PG","48634037","ASLT 1.5NH 150G@75P REDBMPR FM",28]
["48634047","ASLT 1.5NPSH 150G@100P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NPSH","GPM",150,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","Mid-Range","N",20,2,"4863","N/A","N/A",null,null,"4863 1.5 in NPSH 150 100 (Std) BLACK (Std) PG","48634047","ASLT 1.5NPSH 150G@100P FM",45]
["48634050","ASLT 1.5NPSH 550L@500K FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NPSH","LPM",550,"kPa","N/A",500,"BLACK","N","ENGLISH","Fixed","Mid-Range","N",20,2,"4863","N/A","N/A",null,null,"4863 1.5 in NPSH 550 500 BLACK (Std) PG","48634050","ASLT 1.5NPSH 550L@500K FM",39]
["48634056","ASLT 1.5NH 150G@50P ORGBMPR FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",50,"ORANGE","N","ENGLISH","Fixed","Mid-Range","N",20,2,"4863","N/A","N/A",null,null,"4863 1.5 in NH 150 50 ORANGE PG","48634056","ASLT 1.5NH 150G@50P ORGBMPR FM",31]
["48634057","ASLT 1.5NPSH 95G@100P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NPSH","GPM",95,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","Mid-Range","N",20,2,"4863","N/A","N/A",null,null,"4863 1.5 in NPSH 95 100 (Std) BLACK (Std) PG","48634057","ASLT 1.5NPSH 95G@100P FM",44]
["48634061","ASLT 1.5ABU 200G@100P FDNY",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"FDNY","GPM",200,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","Mid-Range","N",20,2,"4863","N/A","N/A",null,null,"4863 1.5 in FDNY 200 100 (Std) BLACK (Std) PG","48634061","ASLT 1.5ABU 200G@100P FDNY",45]
["48634078","ASLT 2.5BIM 475L@7b FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"BIM","LPM",475,"BAR","N/A",7,"BLACK","N","ENGLISH","Fixed","Mid-Range","N",20,2,"4863","N/A","N/A",null,null,"4863 2.5 in BIM 475 7 BLACK (Std) PG","48634078","ASLT 2.5BIM 475L@7b FM",36]
["48634084","ASLT 1.5NPSH 161G@50P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NPSH","GPM",161,"PSI","N/A",50,"BLACK","N","ENGLISH","Fixed","Mid-Range","N",20,2,"4863","N/A","N/A",null,null,"4863 1.5 in NPSH 161 50 BLACK (Std) PG","48634084","ASLT 1.5NPSH 161G@50P FM",38]
["48634095","ASLT 52MM 475L@7b FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2,"STORZ","LPM",475,"BAR","N/A",7,"BLACK","N","ENGLISH","Fixed","Mid-Range","N",20,2,"4863","N/A","N/A",null,null,"4863 2 in STORZ 475 7 BLACK (Std) PG","48634095","ASLT 52MM 475L@7b FM",36]
["48634118","ASLT 1.5ABT 161G@50P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"PCT","GPM",161,"PSI","N/A",50,"BLACK","N","ENGLISH","Fixed","Mid-Range","N",20,2,"4863","N/A","N/A",null,null,"4863 1.5 in PCT 161 50 BLACK (Std) PG","48634118","ASLT 1.5ABT 161G@50P FM",37]
["48634126","ASLT 1.5NH 150@75P MTLTH",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed","Mid-Range","N",20,2,"4863","N/A","N/A",null,null,"4863 1.5 in NH 150 75 BLACK (Std) PG","48634126","ASLT 1.5NH 150@75P MTLTH",36]
["48634136","ASLT 1.5NH 175G@50P FORK FD LOGO",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",175,"PSI","N/A",50,"BLACK","Y","ENGLISH","Fixed","Mid-Range","N",20,2,"4863","N/A","N/A",null,null,"4863 1.5 in NH 175 50 BLACK (Std) PG ETCH","48634136","ASLT 1.5NH 175G@50P FORK FD LOGO",41]
["48634138","ASLT 2.5NH 150G@100P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"NH","GPM",150,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","Mid-Range","N",20,2,"4863","N/A","N/A",null,null,"4863 2.5 in NH 150 100 (Std) BLACK (Std) PG","48634138","ASLT 2.5NH 150G@100P FM",43]
["48637002","ASLT NPG 1.5NH 200G@75P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",200,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed","Mid-Range","Y",20,2,"4863","N/A","N/A",null,null,"4863 1.5 in NH 200 75 BLACK (Std) NPG","48637002","ASLT NPG 1.5NH 200G@75P FM",37]
["48637005","ASLT NPG 1.5NH 125G@75P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",125,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed","Mid-Range","Y",20,2,"4863","N/A","N/A",null,null,"4863 1.5 in NH 125 75 BLACK (Std) NPG","48637005","ASLT NPG 1.5NH 125G@75P FM",37]
["48637008","ASLT NPG 1.5NH 150G@75P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed","Mid-Range","Y",20,2,"4863","N/A","N/A",null,null,"4863 1.5 in NH 150 75 BLACK (Std) NPG","48637008","ASLT NPG 1.5NH 150G@75P FM",37]
["48637098","ASLT NPG 1.5NH 150G@75P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",75,"GREEN","N","ENGLISH","Fixed","Mid-Range","Y",20,2,"4863","N/A","N/A",null,null,{"$f":"CONCATENATE(AC406,\" \",N406,\" in \",O406,\" \",IF(AD406=\"n/a\",\"\",CONCATENATE(AD406,\" in \",AE406,\" \")),IF(Q406=\"n/a\",\"\",Q406),IF(S406=\"n/a\",\"\",CONCATENATE(IF(X406=\"saber\",\" \",\"\"),S406,\" bore size(s) \")),IF(T406=\"n/a\",\"\",CONCATENATE(IF(X406=\"saber\",\"\",\" \"),T406,IF(T406=100,\" (Std) \",IF(T406=87,\" (CE) \",\" \")))),IF(U406=\"n/a\",\"\",CONCATENATE(U406,IF(U406=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X406,3)=\"tip\",IF(LEFT(X406,1)=\"s\",\"\",IF(Z406=\"n\",IF(T406=\"N/A\",\"PG\",\" PG\"),IF(Z406=\"y\",IF(T406=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z406=\"n\",IF(T406=\"N/A\",\"PG\",\" PG\"),IF(Z406=\"y\",IF(T406=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF406=\"y\",\" ZT\",\"\"),IF(V406=\"N\",\"\",IF(S406=\"n/a\",\" ETCH\",IF(T406=\"N/A\",IF(RIGHT(X406,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X406=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"4863 1.5 in NH 150 75 GREEN NPG"},{"$f":"A406","v":"48637098"},{"$f":"B406","v":"ASLT NPG 1.5NH 150G@75P FM"},{"$f":"LEN(AH406)","v":31}]
["48637010","ASLT NPG 1.5NH 200G@100P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",200,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","Mid-Range","Y",20,2,"4863","N/A","N/A",null,null,"4863 1.5 in NH 200 100 (Std) BLACK (Std) NPG","48637010","ASLT NPG 1.5NH 200G@100P FM",44]
["48637026","ASLT NPG 1.5NH 185G@50P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",185,"PSI","N/A",50,"BLACK","N","ENGLISH","Fixed","Mid-Range","Y",20,2,"4863","N/A","N/A",null,null,"4863 1.5 in NH 185 50 BLACK (Std) NPG","48637026","ASLT NPG 1.5NH 185G@50P FM",37]
["48637028","ASLT NPG 1.5NH 175G@50P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",175,"PSI","N/A",50,"BLACK","N","ENGLISH","Fixed","Mid-Range","Y",20,2,"4863","N/A","N/A",null,null,{"$f":"CONCATENATE(AC409,\" \",N409,\" in \",O409,\" \",IF(AD409=\"n/a\",\"\",CONCATENATE(AD409,\" in \",AE409,\" \")),IF(Q409=\"n/a\",\"\",Q409),IF(S409=\"n/a\",\"\",CONCATENATE(IF(X409=\"saber\",\" \",\"\"),S409,\" bore size(s) \")),IF(T409=\"n/a\",\"\",CONCATENATE(IF(X409=\"saber\",\"\",\" \"),T409,IF(T409=100,\" (Std) \",IF(T409=87,\" (CE) \",\" \")))),IF(U409=\"n/a\",\"\",CONCATENATE(U409,IF(U409=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X409,3)=\"tip\",IF(LEFT(X409,1)=\"s\",\"\",IF(Z409=\"n\",IF(T409=\"N/A\",\"PG\",\" PG\"),IF(Z409=\"y\",IF(T409=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z409=\"n\",IF(T409=\"N/A\",\"PG\",\" PG\"),IF(Z409=\"y\",IF(T409=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF409=\"y\",\" ZT\",\"\"),IF(V409=\"N\",\"\",IF(S409=\"n/a\",\" ETCH\",IF(T409=\"N/A\",IF(RIGHT(X409,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X409=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"4863 1.5 in NH 175 50 BLACK (Std) NPG"},{"$f":"A409","v":"48637028"},{"$f":"B409","v":"ASLT NPG 1.5NH 175G@50P FM"},{"$f":"LEN(AH409)","v":37}]
["48637038","ASLT NPG 1.5NH 161G@50P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",161,"PSI","N/A",50,"BLACK","N","ENGLISH","Fixed","Mid-Range","Y",20,2,"4863","N/A","N/A",null,null,"4863 1.5 in NH 161 50 BLACK (Std) NPG","48637038","ASLT NPG 1.5NH 161G@50P FM",37]
["48637090","ASLT NPG 1.5NPSH 360L@700K FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NPSH","LPM",360,"kPa","N/A",700,"BLACK","N","ENGLISH","Fixed","Mid-Range","Y",20,2,"4863","N/A","N/A",null,null,"4863 1.5 in NPSH 360 700 BLACK (Std) NPG","48637090","ASLT NPG 1.5NPSH 360L@700K FM",40]
["48634027","ASLT 1.5NPSH 125G@75P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NPSH","GPM",125,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed","Mid-Range","N",20,3,"4863","N/A","N/A",null,null,"4863 1.5 in NPSH 125 75 BLACK (Std) PG","48634027","ASLT 1.5NPSH 125G@75P FM",38]
["48634034","ASLT 1.5NH 175G@75P BLUEBMPR FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",175,"PSI","N/A",75,"BLUE","N","ENGLISH","Fixed","Mid-Range","N",20,3,"4863","N/A","N/A",null,null,"4863 1.5 in NH 175 75 BLUE PG","48634034","ASLT 1.5NH 175G@75P BLUEBMPR FM",29]
["48634035","ASLT 1.5NH 175G@75P YLWBMPR FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",175,"PSI","N/A",75,"YELLOW","N","ENGLISH","Fixed","Mid-Range","N",20,3,"4863","N/A","N/A",null,null,"4863 1.5 in NH 175 75 YELLOW PG","48634035","ASLT 1.5NH 175G@75P YLWBMPR FM",31]
["48634036","ASLT 1.5NH 175G@75P ORGBMPR FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",175,"PSI","N/A",75,"ORANGE","N","ENGLISH","Fixed","Mid-Range","N",20,3,"4863","N/A","N/A",null,null,"4863 1.5 in NH 175 75 ORANGE PG","48634036","ASLT 1.5NH 175G@75P ORGBMPR FM",31]
["48634039","ASLT 1.5NH 175G@50P YLWBMPR FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",175,"PSI","N/A",50,"YELLOW","N","ENGLISH","Fixed","Mid-Range","N",20,3,"4863","N/A","N/A",null,null,"4863 1.5 in NH 175 50 YELLOW PG","48634039","ASLT 1.5NH 175G@50P YLWBMPR FM",31]
["48634051","ASLT 1.5NH 175G@75P REDBMPR FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",175,"PSI","N/A",75,"RED","N","ENGLISH","Fixed","Mid-Range","N",20,3,"4863","N/A","N/A",null,null,"4863 1.5 in NH 175 75 RED PG","48634051","ASLT 1.5NH 175G@75P REDBMPR FM",28]
["48634053","ASLT 2.5NH 225G@100P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"NH","GPM",225,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","Mid-Range","N",20,3,"4863","N/A","N/A",null,null,"4863 2.5 in NH 225 100 (Std) BLACK (Std) PG","48634053","ASLT 2.5NH 225G@100P FM",43]
["48634067","ASLT 1.5NPSH 570L@350K",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NPSH","LPM",570,"kPA","N/A",350,"BLACK","N","ENGLISH","Fixed","Mid-Range","N",20,3,"4863","N/A","N/A",null,null,"4863 1.5 in NPSH 570 350 BLACK (Std) PG","48634067","ASLT 1.5NPSH 570L@350K",39]
["48634070","ASLT 1.5NPSH 125G@100P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NPSH","GPM",125,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","Mid-Range","N",20,3,"4863","N/A","N/A",null,null,"4863 1.5 in NPSH 125 100 (Std) BLACK (Std) PG","48634070","ASLT 1.5NPSH 125G@100P FM",45]
["48634079","ASLT 2.5NH 200G@75P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"NH","GPM",200,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed","Mid-Range","N",20,3,"4863","N/A","N/A",null,null,"4863 2.5 in NH 200 75 BLACK (Std) PG","48634079","ASLT 2.5NH 200G@75P FM",36]
["48634085","ASLT 1.5NH 150G@100P BLUEBMPR FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",100,"BLUE","N","ENGLISH","Fixed","Mid-Range","N",20,3,"4863","N/A","N/A",null,null,"4863 1.5 in NH 150 100 (Std) BLUE PG","48634085","ASLT 1.5NH 150G@100P BLUEBMPR FM",36]
["48634086","ASLT 1.5NH 150G@100P REDBMPR FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",100,"RED","N","ENGLISH","Fixed","Mid-Range","N",20,3,"4863","N/A","N/A",null,null,"4863 1.5 in NH 150 100 (Std) RED PG","48634086","ASLT 1.5NH 150G@100P REDBMPR FM",35]
["48634089","ASLT 1.5NPSH 200G@75P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NPSH","GPM",200,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed","Mid-Range","N",20,3,"4863","N/A","N/A",null,null,"4863 1.5 in NPSH 200 75 BLACK (Std) PG","48634089","ASLT 1.5NPSH 200G@75P FM",38]
["48634092","ASLT 1.5NPSH 175G@100P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NPSH","GPM",175,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","Mid-Range","N",20,3,"4863","N/A","N/A",null,null,"4863 1.5 in NPSH 175 100 (Std) BLACK (Std) PG","48634092","ASLT 1.5NPSH 175G@100P FM",45]
["48634093","ASLT 1.5NPSH 175G@75P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NPSH","GPM",175,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed","Mid-Range","N",20,3,"4863","N/A","N/A",null,null,"4863 1.5 in NPSH 175 75 BLACK (Std) PG","48634093","ASLT 1.5NPSH 175G@75P FM",38]
["48634098","ASLT 1.5NH 150G@75P GRNBMPR FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",75,"GREEN","N","ENGLISH","Fixed","Mid-Range","N",20,3,"4863","N/A","N/A",null,null,"4863 1.5 in NH 150 75 GREEN PG","48634098","ASLT 1.5NH 150G@75P GRNBMPR FM",30]
["48634104","ASLT 1.5NH 150G@75P BLUEBMPR FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",75,"BLUE","N","ENGLISH","Fixed","Mid-Range","N",20,3,"4863","N/A","N/A",null,null,"4863 1.5 in NH 150 75 BLUE PG","48634104","ASLT 1.5NH 150G@75P BLUEBMPR FM",29]
["48634106","ASLT 1.5NH 150G@50P REDBMPR FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",50,"RED","N","ENGLISH","Fixed","Mid-Range","N",20,3,"4863","N/A","N/A",null,null,"4863 1.5 in NH 150 50 RED PG","48634106","ASLT 1.5NH 150G@50P REDBMPR FM",28]
["48634114","ASLT 1.5NH 150G@75P ORGBMPR FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",75,"ORANGE","N","ENGLISH","Fixed","Mid-Range","N",20,3,"4863","N/A","N/A",null,null,"4863 1.5 in NH 150 75 ORANGE PG","48634114","ASLT 1.5NH 150G@75P ORGBMPR FM",31]
["48634116","ASLT 52MM 750L@7b FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2,"STORZ","LPM",750,"BAR","N/A",7,"BLACK","N","ENGLISH","Fixed","Mid-Range","N",20,3,"4863","N/A","N/A",null,null,"4863 2 in STORZ 750 7 BLACK (Std) PG","48634116","ASLT 52MM 750L@7b FM",36]
["48634117","ASLT 1.5NH 175G@50P ORGBMPR FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",175,"PSI","N/A",50,"ORANGE","N","ENGLISH","Fixed","Mid-Range","N",20,3,"4863","N/A","N/A",null,null,"4863 1.5 in NH 175 50 ORANGE PG","48634117","ASLT 1.5NH 175G@50P ORGBMPR FM",31]
["48634119","ASLT 75MM 750L@7b FM",null,null,null,null,null,null,null,null,"0003","Assault","A",3,"STORZ","LPM",750,"BAR","N/A",7,"BLACK","N","ENGLISH","Fixed","Mid-Range","N",20,3,"4863","N/A","N/A",null,null,"4863 3 in STORZ 750 7 BLACK (Std) PG","48634119","ASLT 75MM 750L@7b FM",36]
["48634156","ASLT 1.5NH 750L@7b FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","LPM",750,"BAR","N/A",7,"BLACK","N","ENGLISH","Fixed","Mid-Range","N",20,3,"4863","N/A","N/A",null,null,{"$f":"CONCATENATE(AC434,\" \",N434,\" in \",O434,\" \",IF(AD434=\"n/a\",\"\",CONCATENATE(AD434,\" in \",AE434,\" \")),IF(Q434=\"n/a\",\"\",Q434),IF(S434=\"n/a\",\"\",CONCATENATE(IF(X434=\"saber\",\" \",\"\"),S434,\" bore size(s) \")),IF(T434=\"n/a\",\"\",CONCATENATE(IF(X434=\"saber\",\"\",\" \"),T434,IF(T434=100,\" (Std) \",IF(T434=87,\" (CE) \",\" \")))),IF(U434=\"n/a\",\"\",CONCATENATE(U434,IF(U434=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X434,3)=\"tip\",IF(LEFT(X434,1)=\"s\",\"\",IF(Z434=\"n\",IF(T434=\"N/A\",\"PG\",\" PG\"),IF(Z434=\"y\",IF(T434=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z434=\"n\",IF(T434=\"N/A\",\"PG\",\" PG\"),IF(Z434=\"y\",IF(T434=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF434=\"y\",\" ZT\",\"\"),IF(V434=\"N\",\"\",IF(S434=\"n/a\",\" ETCH\",IF(T434=\"N/A\",IF(RIGHT(X434,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X434=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"4863 1.5 in NH 750 7 BLACK (Std) PG"},{"$f":"A434","v":"48634156"},{"$f":"B434","v":"ASLT 1.5NH 750L@7b FM"},{"$f":"LEN(AH434)","v":35}]
["48634124","ASLT 1.5NH 175G@50P BLUBMPR FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",175,"PSI","N/A",50,"BLUE","N","ENGLISH","Fixed","Mid-Range","N",20,3,"4863","N/A","N/A",null,null,"4863 1.5 in NH 175 50 BLUE PG","48634124","ASLT 1.5NH 175G@50P BLUBMPR FM",29]
["48634127","ASLT 1.5NH 150G@50P ORGBMPR BFC-E1",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",50,"ORANGE","Y","ENGLISH","Fixed","Mid-Range","N",20,3,"4863","N/A","N/A",null,null,"4863 1.5 in NH 150 50 ORANGE PG ETCH","48634127","ASLT 1.5NH 150G@50P ORGBMPR BFC-E1",36]
["48634128","ASLT 1.5NH 150G@50P GRNBMPR BFC-E1",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",50,"GREEN","Y","ENGLISH","Fixed","Mid-Range","N",20,3,"4863","N/A","N/A",null,null,"4863 1.5 in NH 150 50 GREEN PG ETCH","48634128","ASLT 1.5NH 150G@50P GRNBMPR BFC-E1",35]
["48634129","ASLT 1.5NH 150G@50P BLUBMPR BFC-E1",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",50,"BLUE","Y","ENGLISH","Fixed","Mid-Range","N",20,3,"4863","N/A","N/A",null,null,"4863 1.5 in NH 150 50 BLUE PG ETCH","48634129","ASLT 1.5NH 150G@50P BLUBMPR BFC-E1",34]
["48634130","ASLT 1.5NH 150G@50P BLUBMPR BFC-T5",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",50,"BLUE","Y","ENGLISH","Fixed","Mid-Range","N",20,3,"4863","N/A","N/A",null,null,"4863 1.5 in NH 150 50 BLUE PG ETCH","48634130","ASLT 1.5NH 150G@50P BLUBMPR BFC-T5",34]
["48634131","ASLT 1.5NH 150G@50P BLUBMPR BFC-E2",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",50,"BLUE","Y","ENGLISH","Fixed","Mid-Range","N",20,3,"4863","N/A","N/A",null,null,"4863 1.5 in NH 150 50 BLUE PG ETCH","48634131","ASLT 1.5NH 150G@50P BLUBMPR BFC-E2",34]
["48634132","ASLT 1.5NH 150G@50P GRNBMPR BFC-E2",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",50,"GREEN","Y","ENGLISH","Fixed","Mid-Range","N",20,3,"4863","N/A","N/A",null,null,"4863 1.5 in NH 150 50 GREEN PG ETCH","48634132","ASLT 1.5NH 150G@50P GRNBMPR BFC-E2",35]
["48634133","ASLT 1.5NH 200G@50P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",200,"PSI","N/A",50,"BLACK","N","ENGLISH","Fixed","Mid-Range","N",20,3,"4863","N/A","N/A",null,null,"4863 1.5 in NH 200 50 BLACK (Std) PG","48634133","ASLT 1.5NH 200G@50P FM",36]
["48634135","ASLT 1.5BSP 150G@100P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"BSP","GPM",150,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","Mid-Range","N",20,3,"4863","N/A","N/A",null,null,"4863 1.5 in BSP 150 100 (Std) BLACK (Std) PG","48634135","ASLT 1.5BSP 150G@100P FM",44]
["48634137","ASLT 2.5AII 185G@50P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"CSA","GPM",185,"PSI","N/A",50,"BLACK","N","ENGLISH","Fixed","Mid-Range","N",20,3,"4863","N/A","N/A",null,null,"4863 2.5 in CSA 185 50 BLACK (Std) PG","48634137","ASLT 2.5AII 185G@50P FM",37]
["48634139","ASLT 1.5NH 185G@50P ETCH \"JTFD 1\"",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",185,"PSI","N/A",50,"BLACK","Y","ENGLISH","Fixed","Mid-Range","N",20,3,"4863","N/A","N/A",null,null,"4863 1.5 in NH 185 50 BLACK (Std) PG ETCH","48634139","ASLT 1.5NH 185G@50P ETCH \"JTFD 1\"",41]
["48634140","ASLT 2.5NH 225G@100P ETCH JTFD 1",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"NH","GPM",225,"PSI","N/A",100,"BLACK","Y","ENGLISH","Fixed","Mid-Range","N",20,3,"4863","N/A","N/A",null,null,"4863 2.5 in NH 225 100 (Std) BLACK (Std) PG ETCH","48634140","ASLT 2.5NH 225G@100P ETCH JTFD 1",48]
["48634144","ASLT 2.5NH 125G@100P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",200,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","Mid-Range","N",20,3,"4863","N/A","N/A",null,null,"4863 1.5 in NH 200 100 (Std) BLACK (Std) PG","48634144","ASLT 2.5NH 125G@100P FM",43]
["48634145","ASLT 1.5NH 175G@50P ORGBMPR OCEAN VIEW",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",175,"PSI","N/A",50,"ORANGE","Y","ENGLISH","Fixed","Mid-Range","N",20,3,"4863","N/A","N/A",null,null,"4863 1.5 in NH 175 50 ORANGE PG ETCH","48634145","ASLT 1.5NH 175G@50P ORGBMPR OCEAN VIEW",36]
["48637003","ASLT NPG 2.5NH 150G@50P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"NH","GPM",150,"PSI","N/A",50,"BLACK","N","ENGLISH","Fixed","Mid-Range","Y",20,3,"4863","N/A","N/A",null,null,"4863 2.5 in NH 150 50 BLACK (Std) NPG","48637003","ASLT NPG 2.5NH 150G@50P FM",37]
["48637045","ASLT NPG 1.5NH 150G@50P YLWBMPR FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",50,"YELLOW","N","ENGLISH","Fixed","Mid-Range","Y",20,3,"4863","N/A","N/A",null,null,"4863 1.5 in NH 150 50 YELLOW NPG","48637045","ASLT NPG 1.5NH 150G@50P YLWBMPR FM",32]
["48637047","ASLT NPG 1.5NPSH 150G@100P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NPSH","GPM",150,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","Mid-Range","Y",20,3,"4863","N/A","N/A",null,null,"4863 1.5 in NPSH 150 100 (Std) BLACK (Std) NPG","48637047","ASLT NPG 1.5NPSH 150G@100P FM",46]
["48637084","ASLT NPG 1.5NPSH 161G@50P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NPSH","GPM",161,"PSI","N/A",50,"BLACK","N","ENGLISH","Fixed","Mid-Range","Y",20,3,"4863","N/A","N/A",null,null,"4863 1.5 in NPSH 161 50 BLACK (Std) NPG","48637084","ASLT NPG 1.5NPSH 161G@50P FM",39]
["48637113","ASLT NPG 1.5NPSH 200G@100P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NPSH","GPM",200,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","Mid-Range","Y",20,3,"4863","N/A","N/A",null,null,"4863 1.5 in NPSH 200 100 (Std) BLACK (Std) NPG","48637113","ASLT NPG 1.5NPSH 200G@100P FM",46]
["48634002","ASLT 2.5BIM 750L@7b FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"BIM","LPM",750,"BAR","N/A",7,"BLACK","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 2.5 in BIM 750 7 BLACK (Std) PG","48634002","ASLT 2.5BIM 750L@7b FM",36]
["48634012","ASLT 1.5BSP 475L@7b FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"BSP","LPM",475,"BAR","N/A",7,"BLACK","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in BSP 475 7 BLACK (Std) PG","48634012","ASLT 1.5BSP 475L@7b FM",36]
["48634016","ASLT 1.5NH 161G@50P BLUEBMPR FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",161,"PSI","N/A",50,"BLUE","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NH 161 50 BLUE PG","48634016","ASLT 1.5NH 161G@50P BLUEBMPR FM",29]
["48634017","ASLT 1.5NH 185G@50P GRNBMPR FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",185,"PSI","N/A",50,"GREEN","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NH 185 50 GREEN PG","48634017","ASLT 1.5NH 185G@50P GRNBMPR FM",30]
["48634018","ASLT 1.5BSP 360L@7b FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"BSP","LPM",360,"BAR","N/A",7,"BLACK","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in BSP 360 7 BLACK (Std) PG","48634018","ASLT 1.5BSP 360L@7b FM",36]
["48634125","ASLT 1.5BSP 360L@6b",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"BSP","LPM",360,"BAR","N/A",6,"BLACK","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,{"$f":"CONCATENATE(AC459,\" \",N459,\" in \",O459,\" \",IF(AD459=\"n/a\",\"\",CONCATENATE(AD459,\" in \",AE459,\" \")),IF(Q459=\"n/a\",\"\",Q459),IF(S459=\"n/a\",\"\",CONCATENATE(IF(X459=\"saber\",\" \",\"\"),S459,\" bore size(s) \")),IF(T459=\"n/a\",\"\",CONCATENATE(IF(X459=\"saber\",\"\",\" \"),T459,IF(T459=100,\" (Std) \",IF(T459=87,\" (CE) \",\" \")))),IF(U459=\"n/a\",\"\",CONCATENATE(U459,IF(U459=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X459,3)=\"tip\",IF(LEFT(X459,1)=\"s\",\"\",IF(Z459=\"n\",IF(T459=\"N/A\",\"PG\",\" PG\"),IF(Z459=\"y\",IF(T459=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z459=\"n\",IF(T459=\"N/A\",\"PG\",\" PG\"),IF(Z459=\"y\",IF(T459=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF459=\"y\",\" ZT\",\"\"),IF(V459=\"N\",\"\",IF(S459=\"n/a\",\" ETCH\",IF(T459=\"N/A\",IF(RIGHT(X459,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X459=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"4863 1.5 in BSP 360 6 BLACK (Std) PG"},{"$f":"A459","v":"48634125"},{"$f":"B459","v":"ASLT 1.5BSP 360L@6b"},{"$f":"LEN(AH459)","v":36}]
["48634020","ASLT 2.5BIM 95G@100P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"BIM","GPM",95,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 2.5 in BIM 95 100 (Std) BLACK (Std) PG","48634020","ASLT 2.5BIM 95G@100P FM",43]
["48634021","ASLT 2.5BIM 150G@100P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"BIM","GPM",150,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 2.5 in BIM 150 100 (Std) BLACK (Std) PG","48634021","ASLT 2.5BIM 150G@100P FM",44]
["48634022","ASLT 1.5BSP 550L@5b FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"BSP","LPM",550,"BAR","N/A",5,"BLACK","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in BSP 550 5 BLACK (Std) PG","48634022","ASLT 1.5BSP 550L@5b FM",36]
["48634033","ASLT 1.5NH 150G@50P BLUEBMPR FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",50,"BLUE","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NH 150 50 BLUE PG","48634033","ASLT 1.5NH 150G@50P BLUEBMPR FM",29]
["48634042","ASLT 1.5NPSH 550L@345K FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NPSH","LPM",550,"kPa","N/A",345,"BLACK","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NPSH 550 345 BLACK (Std) PG","48634042","ASLT 1.5NPSH 550L@345K FM",39]
["48634044","ASLT 2.5BIM 475L@4b MTLTH,DETENT",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"BIM","LPM",475,"BAR","N/A",4,"Black","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 2.5 in BIM 475 4 Black (Std) PG","48634044","ASLT 2.5BIM 475L@4b MTLTH,DETENT",36]
["48634045","ASLT 1.5NH 150G@50P YLWBMPR FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",50,"YELLOW","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NH 150 50 YELLOW PG","48634045","ASLT 1.5NH 150G@50P YLWBMPR FM",31]
["48634046","ASLT 1.5NPSH 125G@100P GRNBMPR FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NPSH","GPM",125,"PSI","N/A",100,"GREEN","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NPSH 125 100 (Std) GREEN PG","48634046","ASLT 1.5NPSH 125G@100P GRNBMPR FM",39]
["48634052","ASLT 1.5NH 225G@100P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",225,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NH 225 100 (Std) BLACK (Std) PG","48634052","ASLT 1.5NH 225G@100P FM",43]
["48634058","ASLT 1.5NPSH 550L@500K REDBMPR FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NPSH","LPM",550,"kPa","N/A",500,"RED","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NPSH 550 500 RED PG","48634058","ASLT 1.5NPSH 550L@500K REDBMPR FM",31]
["48634059","ASLT 1.5NPSH 360L@7b FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NPSH","LPM",360,"BAR","N/A",7,"BLACK","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NPSH 360 7 BLACK (Std) PG","48634059","ASLT 1.5NPSH 360L@7b FM",37]
["48634060","ASLT 1.5NH 175G@75P GRNBMPR FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",175,"PSI","N/A",75,"GREEN","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NH 175 75 GREEN PG","48634060","ASLT 1.5NH 175G@75P GRNBMPR FM",30]
["48634065","ASLT ZT 1.5NH 175G@75P BLUEBMPR",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",175,"PSI","N/A",75,"BLUE","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A","Y",null,"4863 1.5 in NH 175 75 BLUE PG ZT","48634065","ASLT ZT 1.5NH 175G@75P BLUEBMPR",32]
["48634066","ASLT 1.5NPSH 185G@50P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NPSH","GPM",185,"PSI","N/A",50,"BLACK","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NPSH 185 50 BLACK (Std) PG","48634066","ASLT 1.5NPSH 185G@50P FM",38]
["48634068","ASLT 1.5NH 150G@100P GRNBMPR FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",100,"GREEN","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NH 150 100 (Std) GREEN PG","48634068","ASLT 1.5NH 150G@100P GRNBMPR FM",37]
["48634069","ASLT 1.5NH 150G@100P ORGBMPR FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",100,"ORANGE","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,{"$f":"CONCATENATE(AC475,\" \",N475,\" in \",O475,\" \",IF(AD475=\"n/a\",\"\",CONCATENATE(AD475,\" in \",AE475,\" \")),IF(Q475=\"n/a\",\"\",Q475),IF(S475=\"n/a\",\"\",CONCATENATE(IF(X475=\"saber\",\" \",\"\"),S475,\" bore size(s) \")),IF(T475=\"n/a\",\"\",CONCATENATE(IF(X475=\"saber\",\"\",\" \"),T475,IF(T475=100,\" (Std) \",IF(T475=87,\" (CE) \",\" \")))),IF(U475=\"n/a\",\"\",CONCATENATE(U475,IF(U475=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X475,3)=\"tip\",IF(LEFT(X475,1)=\"s\",\"\",IF(Z475=\"n\",IF(T475=\"N/A\",\"PG\",\" PG\"),IF(Z475=\"y\",IF(T475=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z475=\"n\",IF(T475=\"N/A\",\"PG\",\" PG\"),IF(Z475=\"y\",IF(T475=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF475=\"y\",\" ZT\",\"\"),IF(V475=\"N\",\"\",IF(S475=\"n/a\",\" ETCH\",IF(T475=\"N/A\",IF(RIGHT(X475,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X475=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"4863 1.5 in NH 150 100 (Std) ORANGE PG"},{"$f":"A475","v":"48634069"},{"$f":"B475","v":"ASLT 1.5NH 150G@100P ORGBMPR FM"},{"$f":"LEN(AH475)","v":38}]
["48634071","ASLT 75MM 200G@75P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",3,"STORZ","GPM",200,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 3 in STORZ 200 75 BLACK (Std) PG","48634071","ASLT 75MM 200G@75P FM",37]
["48634072","ASLT 52MM 360L@7b FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2,"STORZ","LPM",360,"BAR","N/A",7,"BLACK","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 2 in STORZ 360 7 BLACK (Std) PG","48634072","ASLT 52MM 360L@7b FM",36]
["48634073","ASLT 52MM 550L@7b FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2,"STORZ","LPM",550,"BAR","N/A",7,"BLACK","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 2 in STORZ 550 7 BLACK (Std) PG","48634073","ASLT 52MM 550L@7b FM",36]
["48634075","ASLT 1.5ABT 175G@75P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"PCT","GPM",175,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in PCT 175 75 BLACK (Std) PG","48634075","ASLT 1.5ABT 175G@75P FM",37]
["48634076","ASLT 1.5NH 150G@100P YLWBMPR FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",100,"YELLOW","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NH 150 100 (Std) YELLOW PG","48634076","ASLT 1.5NH 150G@100P YLWBMPR FM",38]
["48634077","ASLT 2.5BIM 550L@7b FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"BIM","LPM",550,"BAR","N/A",7,"BLACK","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 2.5 in BIM 550 7 BLACK (Std) PG","48634077","ASLT 2.5BIM 550L@7b FM",36]
["48634080","ASLT 1.5NH 200G@75P BLUEBMPR FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",200,"PSI","N/A",75,"BLUE","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NH 200 75 BLUE PG","48634080","ASLT 1.5NH 200G@75P BLUEBMPR FM",29]
["48634081","ASLT 1.5NH 200G@75P ORGBMPR FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",200,"PSI","N/A",75,"ORANGE","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NH 200 75 ORANGE PG","48634081","ASLT 1.5NH 200G@75P ORGBMPR FM",31]
["48634082","ASLT ZT 1.5NH 200G@100P",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",200,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A","Y",null,"4863 1.5 in NH 200 100 (Std) BLACK (Std) PG ZT","48634082","ASLT ZT 1.5NH 200G@100P",46]
["48634090","ASLT 1.5NPSH 360L@700K FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NPSH","LPM",360,"kPA","N/A",700,"BLACK","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NPSH 360 700 BLACK (Std) PG","48634090","ASLT 1.5NPSH 360L@700K FM",39]
["48634091","ASLT 1.5NPSH 150G@75P ORGBMPR FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NPSH","GPM",150,"PSI","N/A",75,"ORANGE","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NPSH 150 75 ORANGE PG","48634091","ASLT 1.5NPSH 150G@75P ORGBMPR FM",33]
["48634094","ASLT 1.5NH 150G@75P D.F.D.",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NH 150 75 BLACK (Std) PG","48634094","ASLT 1.5NH 150G@75P D.F.D.",36]
["48634096","ASLT 1.5NH 125G@75P GRNBMPR FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",125,"PSI","N/A",75,"GREEN","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NH 125 75 GREEN PG","48634096","ASLT 1.5NH 125G@75P GRNBMPR FM",30]
["48634097","ASLT 2.5BAF 125G@75P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"BAT","GPM",125,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 2.5 in BAT 125 75 BLACK (Std) PG","48634097","ASLT 2.5BAF 125G@75P FM",37]
["48634099","ASLT ZT 1.5NPSH 125G@75P",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NPSH","GPM",125,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A","Y",null,"4863 1.5 in NPSH 125 75 BLACK (Std) PG ZT","48634099","ASLT ZT 1.5NPSH 125G@75P",41]
["48634100","ASLT 38MM 95G@100P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"STORZ","GPM",95,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in STORZ 95 100 (Std) BLACK (Std) PG","48634100","ASLT 38MM 95G@100P FM",45]
["48634102","ASLT 2.5BAF 225G@100P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"BAT","GPM",225,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 2.5 in BAT 225 100 (Std) BLACK (Std) PG","48634102","ASLT 2.5BAF 225G@100P FM",44]
["48634103","ASLT 1.5NH 125G@75P REDBMPR FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",125,"PSI","N/A",75,"RED","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NH 125 75 RED PG","48634103","ASLT 1.5NH 125G@75P REDBMPR FM",28]
["48634105","ASLT 1.5NH 550L@5b FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","LPM",550,"BAR","N/A",5,"BLACK","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NH 550 5 BLACK (Std) PG","48634105","ASLT 1.5NH 550L@5b FM",35]
["48634107","ASLT 1.5NH 150G@50P GRNBMPR FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",50,"GREEN","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NH 150 50 GREEN PG","48634107","ASLT 1.5NH 150G@50P GRNBMPR FM",30]
["48634113","ASLT 1.5NPSH 200G@100P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NPSH","GPM",200,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NPSH 200 100 (Std) BLACK (Std) PG","48634113","ASLT 1.5NPSH 200G@100P FM",45]
["48634115","ASLT 38MM 150G@50PSI",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"STORZ","GPM",150,"PSI","N/A",50,"BLACK","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in STORZ 150 50 BLACK (Std) PG","48634115","ASLT 38MM 150G@50PSI",39]
["48634141","ASLT 2.5NH 95G@100P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"NH","GPM",95,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 2.5 in NH 95 100 (Std) BLACK (Std) PG","48634141","ASLT 2.5NH 95G@100P FM",42]
["48634146","ASLT ZT 1.5NH 150G@75P",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A","Y",null,"4863 1.5 in NH 150 75 BLACK (Std) PG ZT","48634146","ASLT ZT 1.5NH 150G@75P",39]
["48634147","ASLT 2.5BIM 200G@100P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"BIM","GPM",200,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 2.5 in BIM 200 100 (Std) BLACK (Std) PG","48634147","ASLT 2.5BIM 200G@100P FM",44]
["48634149","ASLT 1.5NPSH 475L@500K FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NPSH","LPM",475,"kPA","N/A",500,"BLACK","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NPSH 475 500 BLACK (Std) PG","48634149","ASLT 1.5NPSH 475L@500K FM",39]
["48634150","ASLT 1.5NH 200G@100P REDBMPR FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",200,"PSI","N/A",100,"RED","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NH 200 100 (Std) RED PG","48634150","ASLT 1.5NH 200G@100P REDBMPR FM",35]
["48634151","ASLT 1.5NH 200G@100P BLUEBMPR FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",200,"PSI","N/A",100,"BLUE","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NH 200 100 (Std) BLUE PG","48634151","ASLT 1.5NH 200G@100P BLUEBMPR FM",36]
["48634152","ASLT 1.5NH 200G@100P YLWBMPR FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",200,"PSI","N/A",100,"YELLOW","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NH 200 100 (Std) YELLOW PG","48634152","ASLT 1.5NH 200G@100P YLWBMPR FM",38]
["48634153","ASLT 2.5NH 225G@100P GRNBMPR FM",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"NH","GPM",225,"PSI","N/A",100,"GREEN","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 2.5 in NH 225 100 (Std) GREEN PG","48634153","ASLT 2.5NH 225G@100P GRNBMPR FM",37]
["48634155","ASLT 38MM 750LPM@345KPA",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"STORZ","LPM",750,"kPa","N/A",345,"BLACK","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,{"$f":"CONCATENATE(AC506,\" \",N506,\" in \",O506,\" \",IF(AD506=\"n/a\",\"\",CONCATENATE(AD506,\" in \",AE506,\" \")),IF(Q506=\"n/a\",\"\",Q506),IF(S506=\"n/a\",\"\",CONCATENATE(IF(X506=\"saber\",\" \",\"\"),S506,\" bore size(s) \")),IF(T506=\"n/a\",\"\",CONCATENATE(IF(X506=\"saber\",\"\",\" \"),T506,IF(T506=100,\" (Std) \",IF(T506=87,\" (CE) \",\" \")))),IF(U506=\"n/a\",\"\",CONCATENATE(U506,IF(U506=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X506,3)=\"tip\",IF(LEFT(X506,1)=\"s\",\"\",IF(Z506=\"n\",IF(T506=\"N/A\",\"PG\",\" PG\"),IF(Z506=\"y\",IF(T506=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z506=\"n\",IF(T506=\"N/A\",\"PG\",\" PG\"),IF(Z506=\"y\",IF(T506=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF506=\"y\",\" ZT\",\"\"),IF(V506=\"N\",\"\",IF(S506=\"n/a\",\" ETCH\",IF(T506=\"N/A\",IF(RIGHT(X506,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X506=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"4863 1.5 in STORZ 750 345 BLACK (Std) PG"},{"$f":"A506","v":"48634155"},{"$f":"B506","v":"ASLT 38MM 750LPM@345KPA"},{"$f":"LEN(AH506)","v":40}]
["48634155","ASLT 1.5NH 750L@7b FM\t",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","LPM",750,"BAR","N/A",7,"BLACK","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,{"$f":"CONCATENATE(AC507,\" \",N507,\" in \",O507,\" \",IF(AD507=\"n/a\",\"\",CONCATENATE(AD507,\" in \",AE507,\" \")),IF(Q507=\"n/a\",\"\",Q507),IF(S507=\"n/a\",\"\",CONCATENATE(IF(X507=\"saber\",\" \",\"\"),S507,\" bore size(s) \")),IF(T507=\"n/a\",\"\",CONCATENATE(IF(X507=\"saber\",\"\",\" \"),T507,IF(T507=100,\" (Std) \",IF(T507=87,\" (CE) \",\" \")))),IF(U507=\"n/a\",\"\",CONCATENATE(U507,IF(U507=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X507,3)=\"tip\",IF(LEFT(X507,1)=\"s\",\"\",IF(Z507=\"n\",IF(T507=\"N/A\",\"PG\",\" PG\"),IF(Z507=\"y\",IF(T507=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z507=\"n\",IF(T507=\"N/A\",\"PG\",\" PG\"),IF(Z507=\"y\",IF(T507=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF507=\"y\",\" ZT\",\"\"),IF(V507=\"N\",\"\",IF(S507=\"n/a\",\" ETCH\",IF(T507=\"N/A\",IF(RIGHT(X507,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X507=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"4863 1.5 in NH 750 7 BLACK (Std) PG"},{"$f":"A507","v":"48634155"},{"$f":"B507","v":"ASLT 1.5NH 750L@7b FM\t"},{"$f":"LEN(AH507)","v":35}]
["48637004","ASLT NPG 1.5NH 150G@50P REDBMPR FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",50,"RED","N","ENGLISH","Fixed","Mid-Range","Y","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NH 150 50 RED NPG","48637004","ASLT NPG 1.5NH 150G@50P REDBMPR FM",29]
["48637006","ASLT NPG 1.5NH 125G@100P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",125,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","Mid-Range","Y","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NH 125 100 (Std) BLACK (Std) NPG","48637006","ASLT NPG 1.5NH 125G@100P FM",44]
["48637009","ASLT NPG 1.5NH 175G@75P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",175,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed","Mid-Range","Y","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NH 175 75 BLACK (Std) NPG","48637009","ASLT NPG 1.5NH 175G@75P FM",37]
["48637015","ASLT 1.5NH 185G@50P REDBMPR FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",185,"PSI","N/A",50,"RED","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NH 185 50 RED PG","48637015","ASLT 1.5NH 185G@50P REDBMPR FM",28]
["48637019","ASLT NPG 1.5NH 95G@100P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",95,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","Mid-Range","Y","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NH 95 100 (Std) BLACK (Std) NPG","48637019","ASLT NPG 1.5NH 95G@100P FM",43]
["48637023","ASLT 1.5NH 185G@50P BLUEBMPR FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",185,"PSI","N/A",50,"BLUE","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NH 185 50 BLUE PG","48637023","ASLT 1.5NH 185G@50P BLUEBMPR FM",29]
["48637024","ASLT 1.5NH 185G@50P YLWBMPR FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",185,"PSI","N/A",50,"YELLOW","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NH 185 50 YELLOW PG","48637024","ASLT 1.5NH 185G@50P YLWBMPR FM",31]
["48637025","ASLT 1.5NH 185G@50P ORGBMPR FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",185,"PSI","N/A",50,"ORANGE","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NH 185 50 ORANGE PG","48637025","ASLT 1.5NH 185G@50P ORGBMPR FM",31]
["48637054","ASLT NPG 1.5NH 175G@100P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",175,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","Mid-Range","Y","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NH 175 100 (Std) BLACK (Std) NPG","48637054","ASLT NPG 1.5NH 175G@100P FM",44]
["48634010","ASLT 1.5NH 200G@100P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",200,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","Mid-Range","N",80,1,"4863","N/A","N/A",null,null,"4863 1.5 in NH 200 100 (Std) BLACK (Std) PG","48634010","ASLT 1.5NH 200G@100P FM",43]
["48664001","ASLT TIP 1.5NH 150G@50P#",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",50,"BLACK","N","ENGLISH","Fixed Tip","Mid-Range","N/A",80,1,"4866","N/A","N/A",null,null,"4866 1.5 in NH 150 50 BLACK (Std) ","48664001","ASLT TIP 1.5NH 150G@50P#",34]
["48664002","ASLT TIP 1.5NH 150G@75P#",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed Tip","Mid-Range","N/A",80,1,"4866","N/A","N/A",null,null,"4866 1.5 in NH 150 75 BLACK (Std) ","48664002","ASLT TIP 1.5NH 150G@75P#",34]
["48664003","ASLT TIP 1.5NH 161G@50P#",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",161,"PSI","N/A",50,"BLACK","N","ENGLISH","Fixed Tip","Mid-Range","N/A",80,1,"4866","N/A","N/A",null,null,"4866 1.5 in NH 161 50 BLACK (Std) ","48664003","ASLT TIP 1.5NH 161G@50P#",34]
["48664005","ASLT TIP 1.5NH 185G@50P#",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",185,"PSI","N/A",50,"BLACK","N","ENGLISH","Fixed Tip","Mid-Range","N/A",80,1,"4866","N/A","N/A",null,null,"4866 1.5 in NH 185 50 BLACK (Std) ","48664005","ASLT TIP 1.5NH 185G@50P#",34]
["48664004","ASLT TIP 1.5NH 175G@75P#",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",175,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed Tip","Mid-Range","N/A",20,1,"4866","N/A","N/A",null,null,"4866 1.5 in NH 175 75 BLACK (Std) ","48664004","ASLT TIP 1.5NH 175G@75P#",34]
["48664006","ASLT TIP 1.5NH 200G@75P",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",200,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed Tip","Mid-Range","N/A",20,1,"4866","N/A","N/A",null,null,"4866 1.5 in NH 200 75 BLACK (Std) ","48664006","ASLT TIP 1.5NH 200G@75P",34]
["48664022","ASLT TIP 1.5NPSH 150G@50P",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NPSH","GPM",150,"PSI","N/A",50,"BLACK","N","ENGLISH","Fixed Tip","Mid-Range","N/A",20,1,"4866","N/A","N/A",null,null,"4866 1.5 in NPSH 150 50 BLACK (Std) ","48664022","ASLT TIP 1.5NPSH 150G@50P",36]
["48664031","ASLT TIP 1.5NH 175G@75P REDBMPR",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",175,"PSI","N/A",75,"RED","N","ENGLISH","Fixed Tip","Mid-Range","N/A",20,1,"4866","N/A","N/A",null,null,"4866 1.5 in NH 175 75 RED ","48664031","ASLT TIP 1.5NH 175G@75P REDBMPR",26]
["48664010","ASLT TIP 1.5NH 95G@100P",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",95,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed Tip","Mid-Range","N/A",20,2,"4866","N/A","N/A",null,null,"4866 1.5 in NH 95 100 (Std) BLACK (Std) ","48664010","ASLT TIP 1.5NH 95G@100P",40]
["48664014","ASLT TIP 1.5NH 175G@50P",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",175,"PSI","N/A",50,"BLACK","N","ENGLISH","Fixed Tip","Mid-Range","N/A",20,2,"4866","N/A","N/A",null,null,"4866 1.5 in NH 175 50 BLACK (Std) ","48664014","ASLT TIP 1.5NH 175G@50P",34]
["48664020","ASLT TIP 1.5NH 150G@75P YLWBMPR",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",75,"YELLOW","N","ENGLISH","Fixed Tip","Mid-Range","N/A",20,2,"4866","N/A","N/A",null,null,"4866 1.5 in NH 150 75 YELLOW ","48664020","ASLT TIP 1.5NH 150G@75P YLWBMPR",29]
["48664026","ASLT TIP 1.5NH 150G@100P",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed Tip","Mid-Range","N/A",20,2,"4866","N/A","N/A",null,null,"4866 1.5 in NH 150 100 (Std) BLACK (Std) ","48664026","ASLT TIP 1.5NH 150G@100P",41]
["48664028","ASLT TIP 1.5NH 125G@100P",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",125,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed Tip","Mid-Range","N/A",20,2,"4866","N/A","N/A",null,null,"4866 1.5 in NH 125 100 (Std) BLACK (Std) ","48664028","ASLT TIP 1.5NH 125G@100P",41]
["48664033","ASLT TIP 1.5NH 150G@75P REDBMPR",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",75,"RED","N","ENGLISH","Fixed Tip","Mid-Range","N/A",20,2,"4866","N/A","N/A",null,null,"4866 1.5 in NH 150 75 RED ","48664033","ASLT TIP 1.5NH 150G@75P REDBMPR",26]
["48664034","ASLT TIP 1.5NPSH 550L@500K",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NPSH","LPM",550,"kPA","N/A",500,"BLACK","N","ENGLISH","Fixed Tip","Mid-Range","N/A",20,2,"4866","N/A","N/A",null,null,"4866 1.5 in NPSH 550 500 BLACK (Std) ","48664034","ASLT TIP 1.5NPSH 550L@500K",37]
["48664075","ASLT TIP 1.5NH 200G@100P",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",200,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed Tip","Mid-Range","N/A",20,2,"4866","N/A","N/A",null,null,"4866 1.5 in NH 200 100 (Std) BLACK (Std) ","48664075","ASLT TIP 1.5NH 200G@100P",41]
["48664092","ASLT TIP 1.5NH 150G@100P BDVFD",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",100,"BLACK","Y","ENGLISH","Fixed Tip","Mid-Range","N",20,2,"4866","N/A","N/A",null,null,"4866 1.5 in NH 150 100 (Std) BLACK (Std) PG ETCH","48664092","ASLT TIP 1.5NH 150G@100P BDVFD",48]
["48664012","ASLT TIP 1.5NH 125G@75P",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",125,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed Tip","Mid-Range","N/A",20,3,"4866","N/A","N/A",null,null,"4866 1.5 in NH 125 75 BLACK (Std) ","48664012","ASLT TIP 1.5NH 125G@75P",34]
["48664015","ASLT TIP 1.5NPSH 125G@100P",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NPSH","GPM",125,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed Tip","Mid-Range","N/A",20,3,"4866","N/A","N/A",null,null,"4866 1.5 in NPSH 125 100 (Std) BLACK (Std) ","48664015","ASLT TIP 1.5NPSH 125G@100P",43]
["48664027","ASLT TIP 1.5NH 185G@50P BLUEBMPR",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",185,"PSI","N/A",50,"BLUE","N","ENGLISH","Fixed Tip","Mid-Range","N/A",20,3,"4866","N/A","N/A",null,null,"4866 1.5 in NH 185 50 BLUE ","48664027","ASLT TIP 1.5NH 185G@50P BLUEBMPR",27]
["48664032","ASLT TIP 1.5NH 150G@75P ORGBMPR",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",75,"ORANGE","N","ENGLISH","Fixed Tip","Mid-Range","N/A",20,3,"4866","N/A","N/A",null,null,"4866 1.5 in NH 150 75 ORANGE ","48664032","ASLT TIP 1.5NH 150G@75P ORGBMPR",29]
["48664083","ASLT TIP 1.5NH 150G@50P GRNBMPR",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",50,"GREEN","N","ENGLISH","Fixed Tip","Mid-Range","N/A",20,3,"4866","N/A","N/A",null,null,"4866 1.5 in NH 150 50 GREEN ","48664083","ASLT TIP 1.5NH 150G@50P GRNBMPR",28]
["48664087","ASLT TIP 1.5NH 125G@75P YLWBMPR",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",125,"PSI","N/A",75,"YELLOW","N","ENGLISH","Fixed Tip","Mid-Range","N/A",20,3,"4866","N/A","N/A",null,null,"4866 1.5 in NH 125 75 YELLOW ","48664087","ASLT TIP 1.5NH 125G@75P YLWBMPR",29]
["48664088","ASLT TIP1.5NH 175G@50P YLWBMPR COPLE VFD",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",175,"PSI","N/A",50,"YELLOW","Y","ENGLISH","Fixed Tip","Mid-Range","N",20,3,"4866","N/A","N/A",null,null,{"$f":"CONCATENATE(AC541,\" \",N541,\" in \",O541,\" \",IF(AD541=\"n/a\",\"\",CONCATENATE(AD541,\" in \",AE541,\" \")),IF(Q541=\"n/a\",\"\",Q541),IF(S541=\"n/a\",\"\",CONCATENATE(IF(X541=\"saber\",\" \",\"\"),S541,\" bore size(s) \")),IF(T541=\"n/a\",\"\",CONCATENATE(IF(X541=\"saber\",\"\",\" \"),T541,IF(T541=100,\" (Std) \",IF(T541=87,\" (CE) \",\" \")))),IF(U541=\"n/a\",\"\",CONCATENATE(U541,IF(U541=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X541,3)=\"tip\",IF(LEFT(X541,1)=\"s\",\"\",IF(Z541=\"n\",IF(T541=\"N/A\",\"PG\",\" PG\"),IF(Z541=\"y\",IF(T541=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z541=\"n\",IF(T541=\"N/A\",\"PG\",\" PG\"),IF(Z541=\"y\",IF(T541=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF541=\"y\",\" ZT\",\"\"),IF(V541=\"N\",\"\",IF(S541=\"n/a\",\" ETCH\",IF(T541=\"N/A\",IF(RIGHT(X541,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X541=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"4866 1.5 in NH 175 50 YELLOW PG ETCH"},{"$f":"A541","v":"48664088"},{"$f":"B541","v":"ASLT TIP1.5NH 175G@50P YLWBMPR COPLE VFD"},{"$f":"LEN(AH541)","v":36}]
["48664089","ASLT TIP1.5NH 175G@50P ORGBMPR COPLE VFD",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",175,"PSI","N/A",50,"ORANGE","Y","ENGLISH","Fixed Tip","Mid-Range","N",20,3,"4866","N/A","N/A",null,null,"4866 1.5 in NH 175 50 ORANGE PG ETCH","48664089","ASLT TIP1.5NH 175G@50P ORGBMPR COPLE VFD",36]
["48664090","ASLT TIP 1.5NH 175G@50P COPLE VFD",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",175,"PSI","N/A",50,"BLACK","Y","ENGLISH","Fixed Tip","Mid-Range","N",20,3,"4866","N/A","N/A",null,null,"4866 1.5 in NH 175 50 BLACK (Std) PG ETCH","48664090","ASLT TIP 1.5NH 175G@50P COPLE VFD",41]
["48664008","ASLT TIP 1.5NH 185G@50P ORGBMPR",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",185,"PSI","N/A",50,"ORANGE","N","ENGLISH","Fixed Tip","Mid-Range","N/A",20,4,"4866","N/A","N/A",null,null,"4866 1.5 in NH 185 50 ORANGE ","48664008","ASLT TIP 1.5NH 185G@50P ORGBMPR",29]
["48664007","ASLT TIP 1.5NH 161G@50P YLWBMPR",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",161,"PSI","N/A",50,"YELLOW","N","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NH 161 50 YELLOW ","48664007","ASLT TIP 1.5NH 161G@50P YLWBMPR",29]
["48664009","ASLT TIP 1.5NH 161G@50P GRNBMPR",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",161,"PSI","N/A",50,"GREEN","N","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NH 161 50 GREEN ","48664009","ASLT TIP 1.5NH 161G@50P GRNBMPR",28]
["48664013","ASLT TIP 1.5NPSH 125G@75P",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NPSH","GPM",125,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NPSH 125 75 BLACK (Std) ","48664013","ASLT TIP 1.5NPSH 125G@75P",36]
["48664018","ASLT TIP 1.5NH 175G@50P YLWBMPR",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",175,"PSI","N/A",50,"YELLOW","N","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NH 175 50 YELLOW ","48664018","ASLT TIP 1.5NH 175G@50P YLWBMPR",29]
["48664019","ASLT TIP 1.5NH 175G@75P YLWBMPR",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",175,"PSI","N/A",75,"YELLOW","N","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NH 175 75 YELLOW ","48664019","ASLT TIP 1.5NH 175G@75P YLWBMPR",29]
["48664021","ASLT TIP 1.5NH 185G@50P YLWBMPR",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",185,"PSI","N/A",50,"YELLOW","N","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NH 185 50 YELLOW ","48664021","ASLT TIP 1.5NH 185G@50P YLWBMPR",29]
["48664024","ASLT TIP 1.5NH 175G@75P GRNBMPR",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",175,"PSI","N/A",75,"GREEN","N","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NH 175 75 GREEN ","48664024","ASLT TIP 1.5NH 175G@75P GRNBMPR",28]
["48664025","ASLT TIP 1.5NH 175G@75P ORGBMPR",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",175,"PSI","N/A",75,"ORANGE","N","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NH 175 75 ORANGE ","48664025","ASLT TIP 1.5NH 175G@75P ORGBMPR",29]
["48664029","ASLT TIP 1.5NH 150G@50P METAL TTH",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",50,"BLACK","N","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NH 150 50 BLACK (Std) ","48664029","ASLT TIP 1.5NH 150G@50P METAL TTH",34]
["48664030","ASLT TIP 1.5NH 175G@75P BLUEBMPR",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",175,"PSI","N/A",75,"BLUE","N","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NH 175 75 BLUE ","48664030","ASLT TIP 1.5NH 175G@75P BLUEBMPR",27]
["48664035","ASLT TIP 1.5ABT 175G@75P",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"PCT","GPM",175,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in PCT 175 75 BLACK (Std) ","48664035","ASLT TIP 1.5ABT 175G@75P",35]
["48664095","ASLT TIP 1.5ABX 175G@50P",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"ABX","GPM",175,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,{"$f":"CONCATENATE(AC556,\" \",N556,\" in \",O556,\" \",IF(AD556=\"n/a\",\"\",CONCATENATE(AD556,\" in \",AE556,\" \")),IF(Q556=\"n/a\",\"\",Q556),IF(S556=\"n/a\",\"\",CONCATENATE(IF(X556=\"saber\",\" \",\"\"),S556,\" bore size(s) \")),IF(T556=\"n/a\",\"\",CONCATENATE(IF(X556=\"saber\",\"\",\" \"),T556,IF(T556=100,\" (Std) \",IF(T556=87,\" (CE) \",\" \")))),IF(U556=\"n/a\",\"\",CONCATENATE(U556,IF(U556=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X556,3)=\"tip\",IF(LEFT(X556,1)=\"s\",\"\",IF(Z556=\"n\",IF(T556=\"N/A\",\"PG\",\" PG\"),IF(Z556=\"y\",IF(T556=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z556=\"n\",IF(T556=\"N/A\",\"PG\",\" PG\"),IF(Z556=\"y\",IF(T556=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF556=\"y\",\" ZT\",\"\"),IF(V556=\"N\",\"\",IF(S556=\"n/a\",\" ETCH\",IF(T556=\"N/A\",IF(RIGHT(X556,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X556=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"4866 1.5 in ABX 175 75 BLACK (Std) "},{"$f":"A556","v":"48664095"},{"$f":"B556","v":"ASLT TIP 1.5ABX 175G@50P"},{"$f":"LEN(AH556)","v":35}]
["48664037","ASLT TIP 1.5NH 150G@50P REDBMPR",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",50,"RED","N","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NH 150 50 RED ","48664037","ASLT TIP 1.5NH 150G@50P REDBMPR",26]
["48664038","ASLT TIP 1.5NH 185G@50P REDBMPR",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",185,"PSI","N/A",50,"RED","N","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NH 185 50 RED ","48664038","ASLT TIP 1.5NH 185G@50P REDBMPR",26]
["48664041","ASLT TIP 1.5NH 125G@100P GRNBMPR",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",125,"PSI","N/A",100,"GREEN","N","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NH 125 100 (Std) GREEN ","48664041","ASLT TIP 1.5NH 125G@100P GRNBMPR",35]
["48664042","ASLT TIP 1.5NPSH 200G@75P",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NPSH","GPM",200,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NPSH 200 75 BLACK (Std) ","48664042","ASLT TIP 1.5NPSH 200G@75P",36]
["48664043","ASLT TIP 1.5NPSH 150G@75P",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NPSH","GPM",150,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NPSH 150 75 BLACK (Std) ","48664043","ASLT TIP 1.5NPSH 150G@75P",36]
["48664044","ASLT TIP 1.5NH 150G@75P BLUEBMPR",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",75,"BLUE","N","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NH 150 75 BLUE ","48664044","ASLT TIP 1.5NH 150G@75P BLUEBMPR",27]
["48664045","ASLT TIP 1.5NH 150G@50P YLWBMPR",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",50,"YELLOW","N","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NH 150 50 YELLOW ","48664045","ASLT TIP 1.5NH 150G@50P YLWBMPR",29]
["48664046","ASLT TIP 1.5NH 150G@50P ORGBMPR",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",50,"ORANGE","N","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NH 150 50 ORANGE ","48664046","ASLT TIP 1.5NH 150G@50P ORGBMPR",29]
["48664052","ASLT TIP 1.5NH 150G@100P REDBMPR",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",100,"RED","N","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NH 150 100 (Std) RED ","48664052","ASLT TIP 1.5NH 150G@100P REDBMPR",33]
["48664053","ASLT TIP 1.5NH 150G@100P BLUEBMPR",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",100,"BLUE","N","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NH 150 100 (Std) BLUE ","48664053","ASLT TIP 1.5NH 150G@100P BLUEBMPR",34]
["48664054","ASLT TIP 1.5NH 150G@100P GRNBMPR",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",100,"GREEN","N","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NH 150 100 (Std) GREEN ","48664054","ASLT TIP 1.5NH 150G@100P GRNBMPR",35]
["48664055","ASLT TIP 1.5NPSH 660L@500K",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NPSH","LPM",660,"kPa","N/A",500,"BLACK","N","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NPSH 660 500 BLACK (Std) ","48664055","ASLT TIP 1.5NPSH 660L@500K",37]
["48664094","ASLT TIP 1.5NPSH 660L@5B",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NPSH","LPM",660,"BAR","N/A",5,"BLACK","N","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,{"$f":"CONCATENATE(AC569,\" \",N569,\" in \",O569,\" \",IF(AD569=\"n/a\",\"\",CONCATENATE(AD569,\" in \",AE569,\" \")),IF(Q569=\"n/a\",\"\",Q569),IF(S569=\"n/a\",\"\",CONCATENATE(IF(X569=\"saber\",\" \",\"\"),S569,\" bore size(s) \")),IF(T569=\"n/a\",\"\",CONCATENATE(IF(X569=\"saber\",\"\",\" \"),T569,IF(T569=100,\" (Std) \",IF(T569=87,\" (CE) \",\" \")))),IF(U569=\"n/a\",\"\",CONCATENATE(U569,IF(U569=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X569,3)=\"tip\",IF(LEFT(X569,1)=\"s\",\"\",IF(Z569=\"n\",IF(T569=\"N/A\",\"PG\",\" PG\"),IF(Z569=\"y\",IF(T569=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z569=\"n\",IF(T569=\"N/A\",\"PG\",\" PG\"),IF(Z569=\"y\",IF(T569=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF569=\"y\",\" ZT\",\"\"),IF(V569=\"N\",\"\",IF(S569=\"n/a\",\" ETCH\",IF(T569=\"N/A\",IF(RIGHT(X569,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X569=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"4866 1.5 in NPSH 660 5 BLACK (Std) "},{"$f":"A569","v":"48664094"},{"$f":"B569","v":"ASLT TIP 1.5NPSH 660L@5B"},{"$f":"LEN(AH569)","v":35}]
["48664056","ASLT TIP 1.5NH 161G@50P ORGBMPR",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",161,"PSI","N/A",50,"ORANGE","N","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NH 161 50 ORANGE ","48664056","ASLT TIP 1.5NH 161G@50P ORGBMPR",29]
["48664057","ASLT TIP 1.5NH 125G@100P REDBMPR",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",125,"PSI","N/A",100,"RED","N","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NH 125 100 (Std) RED ","48664057","ASLT TIP 1.5NH 125G@100P REDBMPR",33]
["48664058","ASLT TIP 1.5NH 200G@75P YLWBMPR",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",200,"PSI","N/A",75,"YELLOW","N","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NH 200 75 YELLOW ","48664058","ASLT TIP 1.5NH 200G@75P YLWBMPR",29]
["48664060","ASLT TIP 1.5NH 161G@50P REDBMPR",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",161,"PSI","N/A",50,"RED","N","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NH 161 50 RED ","48664060","ASLT TIP 1.5NH 161G@50P REDBMPR",26]
["48664067","ASLT TIP 1.5NPSH 175G@75P",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NPSH","GPM",175,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NPSH 175 75 BLACK (Std) ","48664067","ASLT TIP 1.5NPSH 175G@75P",36]
["48664068","ASLT TIP 1.5NH 150G@50P BLUEBMPR",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",50,"BLUE","N","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NH 150 50 BLUE ","48664068","ASLT TIP 1.5NH 150G@50P BLUEBMPR",27]
["48664070","ASLT TIP 1.5NPSH 660L@517K",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NPSH","LPM",660,"kPA","N/A",517,"BLACK","N","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NPSH 660 517 BLACK (Std) ","48664070","ASLT TIP 1.5NPSH 660L@517K",37]
["48664077","ASLT TIP 1.5NH 150G@75P GRNBMPR",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",75,"GREEN","N","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NH 150 75 GREEN ","48664077","ASLT TIP 1.5NH 150G@75P GRNBMPR",28]
["48664079","ASLT TIP 1.5NH 175G@100P",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",175,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NH 175 100 (Std) BLACK (Std) ","48664079","ASLT TIP 1.5NH 175G@100P",41]
["48664080","ASLT TIP 1.5NPSH 175G@100P",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NPSH","GPM",175,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NPSH 175 100 (Std) BLACK (Std) ","48664080","ASLT TIP 1.5NPSH 175G@100P",43]
["48664093","ASLT TIP 1.5NPSH 150G@100P",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NPSH","GPM",150,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NPSH 150 100 (Std) BLACK (Std) ","48664093","ASLT TIP 1.5NPSH 150G@100P",43]
["07530001","SHUTOFF 1\"BSPX1.5BSP W/BMP IHR #",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1,"BSP","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","1\"","N",20,1,"0753",1.5,"BSP",null,null,"0753 1 in BSP 1.5 in BSP PG","07530001","SHUTOFF 1\"BSPX1.5BSP W/BMP IHR #",27]
["07530003","SHUTOFF 1\"NHX1.5NH IHR W/BUMPER",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1,"NH","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","1\"","N",20,1,"0753",1.5,"NH",null,null,"0753 1 in NH 1.5 in NH PG","07530003","SHUTOFF 1\"NHX1.5NH IHR W/BUMPER",25]
["07533000","SHUTOFF 1\"BSPX1.5BSP W/BMP IHR L/LATCH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1,"BSP","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","1\"","N",20,1,"0753",1.5,"BSP",null,null,"0753 1 in BSP 1.5 in BSP PG","07533000","SHUTOFF 1\"BSPX1.5BSP W/BMP IHR L/LATCH",27]
["07534004","SHUTOFF HP 1\"BSP X 1.5BSP LPM W/1703",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1,"BSP","LPM","50-230","BAR","N/A",7,"N/A","N","ENGLISH","Breakapart Selectable","1\"","N",20,1,"0753",1.5,"BSP",null,null,"0753 1 in BSP 1.5 in BSP 50-230 7  PG","07534004","SHUTOFF HP 1\"BSP X 1.5BSP LPM W/1703",37]
["07534013","SHUTOFF HP 1\"NHX1.5NH GPM W/1703",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1,"NH","GPM","13-60","PSI","N/A",100,"N/A","N","ENGLISH","Breakapart Selectable","1\"","N",20,3,"0753",1.5,"NH",null,null,"0753 1 in NH 1.5 in NH 13-60 100 (Std)  PG","07534013","SHUTOFF HP 1\"NHX1.5NH GPM W/1703",42]
["07530006","SHUTOFF 1.0NHX1.5NPSH IHR W/BUMPER",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1,"NH","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","1\"","N","No 2021 Sales","No 2021 Sales","0753",1.5,"NPSH",null,null,"0753 1 in NH 1.5 in NPSH PG","07530006","SHUTOFF 1.0NHX1.5NPSH IHR W/BUMPER",27]
["07530007","SHUTOFF 1.0NPSHX1.5\"NH IHR W/BMPR",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1,"NPSH","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","1\"","N","No 2021 Sales","No 2021 Sales","0753",1.5,"NH",null,null,"0753 1 in NPSH 1.5 in NH PG","07530007","SHUTOFF 1.0NPSHX1.5\"NH IHR W/BMPR",27]
["07530009","SHUTOFF 1.0NPSHX1.5NPSH 1HR W/BMPR",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1,"NPSH","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","1\"","N","No 2021 Sales","No 2021 Sales","0753",1.5,"NPSH",null,null,"0753 1 in NPSH 1.5 in NPSH PG","07530009","SHUTOFF 1.0NPSHX1.5NPSH 1HR W/BMPR",29]
["07530010","SHUTOFF 1.0BSPX1.5NH IHR W/BMPR",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1,"BSP","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","1\"","N","No 2021 Sales","No 2021 Sales","0753",1.5,"NH",null,null,"0753 1 in BSP 1.5 in NH PG","07530010","SHUTOFF 1.0BSPX1.5NH IHR W/BMPR",26]
["07532001","SHUTOFF 1.0NHX1.5BSP IHR W/BUMPER",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1,"NH","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","1\"","N","No 2021 Sales","No 2021 Sales","0753",1.5,"BSP",null,null,"0753 1 in NH 1.5 in BSP PG","07532001","SHUTOFF 1.0NHX1.5BSP IHR W/BUMPER",26]
["11250001","SHUTOFF 1.5 NH F X 1.5 NH M CS #",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","1.5\"","Y",20,1,"1125",1.5,"NH",null,null,"1125 1.5 in NH 1.5 in NH NPG","11250001","SHUTOFF 1.5 NH F X 1.5 NH M CS #",28]
["11250002","SHUTOFF 1.5 NPSH F X 1.5 NPSH M CS",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NPSH","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","1.5\"","Y",20,3,"1125",1.5,"NPSH",null,null,"1125 1.5 in NPSH 1.5 in NPSH NPG","11250002","SHUTOFF 1.5 NPSH F X 1.5 NPSH M CS",32]
["11250003","SHUTOFF 1.5 NPSH F X 1.5 NH M CS",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NPSH","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","1.5\"","Y","No 2021 Sales","No 2021 Sales","1125",1.5,"NH",null,null,"1125 1.5 in NPSH 1.5 in NH NPG","11250003","SHUTOFF 1.5 NPSH F X 1.5 NH M CS",30]
["11250011","SHUTOFF 1.5 ABU F X 1.5 ABU M CS FDNY",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"FDNY","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","1.5\"","Y","No 2021 Sales","No 2021 Sales","1125",1.5,"FDNY",null,null,"1125 1.5 in FDNY 1.5 in FDNY NPG","11250011","SHUTOFF 1.5 ABU F X 1.5 ABU M CS FDNY",32]
["11250017","SHUTOFF 1.5NHFX1.5NHM CS METAL HNDL",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","1.5\"","Y","No 2021 Sales","No 2021 Sales","1125",1.5,"NH",null,null,"1125 1.5 in NH 1.5 in NH NPG","11250017","SHUTOFF 1.5NHFX1.5NHM CS METAL HNDL",28]
["14400004","SH/O TIPS 1.5FDNY X 1.5FDNY ABUABU",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"FDNY","N/A","N/A","N/A","15/16\"; 1/2\"","n/a","N/A","N","ENGLISH","Breakapart Stack Tip","1.5\"","N",80,1,"1440",1.5,"FDNY",null,null,"1440 1.5 in FDNY 1.5 in FDNY 15/16\"; 1/2\" bore size(s) PG","14400004","SH/O TIPS 1.5FDNY X 1.5FDNY ABUABU",57]
["14410010","SH/O TIP PG 1.5 ABU X1.5ABU 15/16&1/2",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"FDNY","N/A","N/A","N/A","15/16\"; 1/2\"","n/a","N/A","N","ENGLISH","Breakapart Stack Tip","1.5\"","N",80,1,"1441",1.5,"FDNY",null,null,"1441 1.5 in FDNY 1.5 in FDNY 15/16\"; 1/2\" bore size(s) PG","14410010","SH/O TIP PG 1.5 ABU X1.5ABU 15/16&1/2",57]
["14414001","SH/O TIP 1.5NH X 1.5NH 15/16&1/2",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","15/16\"; 1/2\"","n/a","N/A","N","ENGLISH","Breakapart Stack Tip","1.5\"","N",80,1,"1441",1.5,"NH",null,null,"1441 1.5 in NH 1.5 in NH 15/16\"; 1/2\" bore size(s) PG","14414001","SH/O TIP 1.5NH X 1.5NH 15/16&1/2",53]
["14417002","SH/O NPG TIP 1.5NHX1.5NH 15/16&1/2",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","15/16\"; 1/2\"","n/a","N/A","N","ENGLISH","Breakapart Stack Tip","1.5\"","Y",20,1,"1441",1.5,"NH",null,null,"1441 1.5 in NH 1.5 in NH 15/16\"; 1/2\" bore size(s) NPG","14417002","SH/O NPG TIP 1.5NHX1.5NH 15/16&1/2",54]
["14414002","SH/O TIP 1.5ABU X 1.5ABU 15/16&1/2",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"FDNY","N/A","N/A","N/A","15/16\"; 1/2\"","n/a","N/A","N","ENGLISH","Breakapart Stack Tip","1.5\"","n",20,2,"1441",1.5,"FDNY",null,null,"1441 1.5 in FDNY 1.5 in FDNY 15/16\"; 1/2\" bore size(s) PG","14414002","SH/O TIP 1.5ABU X 1.5ABU 15/16&1/2",57]
["14414004","SH/O TIP 1.5NPSH X 1.5NPSH 15/16&1/2",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NPSH","N/A","N/A","N/A","15/16\"; 1/2\"","n/a","N/A","N","ENGLISH","Breakapart Stack Tip","1.5\"","N",20,2,"1441",1.5,"NPSH",null,null,"1441 1.5 in NPSH 1.5 in NPSH 15/16\"; 1/2\" bore size(s) PG","14414004","SH/O TIP 1.5NPSH X 1.5NPSH 15/16&1/2",57]
["14417001","SH/O NPG MTLHDL TIP 1.5NHXNH 15/16&1/2",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","15/16\"; 1/2\"","n/a","N/A","N","ENGLISH","Breakapart Stack Tip","1.5\"","Y",20,2,"1441",1.5,"NH",null,null,"1441 1.5 in NH 1.5 in NH 15/16\"; 1/2\" bore size(s) NPG","14417001","SH/O NPG MTLHDL TIP 1.5NHXNH 15/16&1/2",54]
["14414007","SH/O TIP 1.5NPSHX1.5NPSH15/16&1/2 MTLHDL",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NPSH","N/A","N/A","N/A","15/16\"; 1/2\"","n/a","N/A","N","ENGLISH","Breakapart Stack Tip","1.5\"","N",20,3,"1441",1.5,"NPSH",null,null,"1441 1.5 in NPSH 1.5 in NPSH 15/16\"; 1/2\" bore size(s) PG","14414007","SH/O TIP 1.5NPSHX1.5NPSH15/16&1/2 MTLHDL",57]
["14414005","SH/O TIP 1.5NH X 1.5NH 15/16&1/2 MTL HDL",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","15/16\"; 1/2\"","n/a","N/A","N","ENGLISH","Breakapart Stack Tip","1.5\"","N","No 2021 Sales","No 2021 Sales","1441",1.5,"NH",null,null,"1441 1.5 in NH 1.5 in NH 15/16\"; 1/2\" bore size(s) PG","14414005","SH/O TIP 1.5NH X 1.5NH 15/16&1/2 MTL HDL",53]
["14414006","SH/O TIP 1.5ABQ X 1.5ABQ 15/16&1/2",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NYCORP","N/A","N/A","N/A","15/16\"; 1/2\"","N/A","N/A","N","ENGLISH","Breakapart Stack Tip","1.5\"","N","No 2021 Sales","No 2021 Sales","1441",1.5,"NYCORP",null,null,"1441 1.5 in NYCORP 1.5 in NYCORP 15/16\"; 1/2\" bore size(s) PG","14414006","SH/O TIP 1.5ABQ X 1.5ABQ 15/16&1/2",61]
["14417003","SH/O NPG TIP 1.5ABU X 1.5ABU 15/16&1/2",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"FDNY","N/A","N/A","N/A","15/16\"; 1/2\"","n/a","N/A","N","ENGLISH","Breakapart Stack Tip","1.5\"","Y","No 2021 Sales","No 2021 Sales","1441",1.5,"FDNY",null,null,"1441 1.5 in FDNY 1.5 in FDNY 15/16\"; 1/2\" bore size(s) NPG","14417003","SH/O NPG TIP 1.5ABU X 1.5ABU 15/16&1/2",58]
["14410001","OBSSH/O TIP PG 1.5 NH X 1.5 NH 15/16&1/2",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","O",1.5,"NH","N/A","N/A","N/A","15/16\"; 1/2\"","N/A","N/A","N","ENGLISH","Breakapart Stack Tip","1.5\"","N",20,4,"1441",1.5,"NH",null,null,{"$f":"CONCATENATE(AC607,\" \",N607,\" in \",O607,\" \",IF(AD607=\"n/a\",\"\",CONCATENATE(AD607,\" in \",AE607,\" \")),IF(Q607=\"n/a\",\"\",Q607),IF(S607=\"n/a\",\"\",CONCATENATE(IF(X607=\"saber\",\" \",\"\"),S607,\" bore size(s) \")),IF(T607=\"n/a\",\"\",CONCATENATE(IF(X607=\"saber\",\"\",\" \"),T607,IF(T607=100,\" (Std) \",IF(T607=87,\" (CE) \",\" \")))),IF(U607=\"n/a\",\"\",CONCATENATE(U607,IF(U607=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X607,3)=\"tip\",IF(LEFT(X607,1)=\"s\",\"\",IF(Z607=\"n\",IF(T607=\"N/A\",\"PG\",\" PG\"),IF(Z607=\"y\",IF(T607=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z607=\"n\",IF(T607=\"N/A\",\"PG\",\" PG\"),IF(Z607=\"y\",IF(T607=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF607=\"y\",\" ZT\",\"\"),IF(V607=\"N\",\"\",IF(S607=\"n/a\",\" ETCH\",IF(T607=\"N/A\",IF(RIGHT(X607,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X607=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"1441 1.5 in NH 1.5 in NH 15/16\"; 1/2\" bore size(s) PG"},{"$f":"A607","v":"14410001"},{"$f":"B607","v":"OBSSH/O TIP PG 1.5 NH X 1.5 NH 15/16&1/2"},{"$f":"LEN(AH607)","v":53}]
["14420003","SH/O TIPS 2.5FDNY X 1.5FDNY    1 1/8&1/2",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"FDNY","N/A","N/A","N/A","1-1/8\"; 1/2\"","n/a","N/A","N","ENGLISH","Breakapart Stack Tip","High-Range","Y",80,1,"1442",1.5,"FDNY",null,null,"1442 2.5 in FDNY 1.5 in FDNY 1-1/8\"; 1/2\" bore size(s) NPG","14420003","SH/O TIPS 2.5FDNY X 1.5FDNY    1 1/8&1/2",58]
["14430022","SH/O TIP PG 2.5 FB X1.5 ABU 1 1/8&1/2",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"FDNY","N/A","N/A","N/A","1-1/8\"; 1/2\"","n/a","N/A","N","ENGLISH","Breakapart Stack Tip","High-Range","N",80,1,"1443",1.5,"FDNY",null,null,"1443 2.5 in FDNY 1.5 in FDNY 1-1/8\"; 1/2\" bore size(s) PG","14430022","SH/O TIP PG 2.5 FB X1.5 ABU 1 1/8&1/2",57]
["14434001","SH/O TIP 2.5NH X 1.5NH 1-1/8&1/2",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","1-1/8\"; 1/2\"","n/a","N/A","N","ENGLISH","Breakapart Stack Tip","High-Range","N",20,1,"1443",1.5,"NH",null,null,"1443 2.5 in NH 1.5 in NH 1-1/8\"; 1/2\" bore size(s) PG","14434001","SH/O TIP 2.5NH X 1.5NH 1-1/8&1/2",53]
["14437004","SH/O NPG 2.5NH X 1.5NH 1-1/8&1/2 MTLHDL",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","1-1/8\"; 1/2\"","N/A","N/A","N","ENGLISH","Breakapart Stack Tip","High-Range","Y",20,2,"1443",1.5,"NH",null,null,"1443 2.5 in NH 1.5 in NH 1-1/8\"; 1/2\" bore size(s) NPG","14437004","SH/O NPG 2.5NH X 1.5NH 1-1/8&1/2 MTLHDL",54]
["14434002","SH/O TIP 2.5AEF X 1.5NH 1-1/8&1/2",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NYCORP","N/A","N/A","N/A","1-1/8\"; 1/2\"","N/A","N/A","N","ENGLISH","Breakapart Stack Tip","High-Range","N",20,3,"1443",1.5,"NH",null,null,"1443 2.5 in NYCORP 1.5 in NH 1-1/8\"; 1/2\" bore size(s) PG","14434002","SH/O TIP 2.5AEF X 1.5NH 1-1/8&1/2",57]
["14434008","SH/O TIP 2.5NH X 1.5NPSH 1-1/8&1/2",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","1-1/8\"; 1/2\"","N/A","N/A","N","ENGLISH","Breakapart Stack Tip","High-Range","N",20,3,"1443",1.5,"NPSH",null,null,"1443 2.5 in NH 1.5 in NPSH 1-1/8\"; 1/2\" bore size(s) PG","14434008","SH/O TIP 2.5NH X 1.5NPSH 1-1/8&1/2",55]
["14437001","SH/O NPG TIP 2.5NH X 1.5NH 1-1/8&1/2",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","1-1/8\"; 1/2\"","n/a","N/A","N","ENGLISH","Breakapart Stack Tip","High-Range","Y",20,3,"1443",1.5,"NH",null,null,"1443 2.5 in NH 1.5 in NH 1-1/8\"; 1/2\" bore size(s) NPG","14437001","SH/O NPG TIP 2.5NH X 1.5NH 1-1/8&1/2",54]
["14437005","SH/O NPG TIP2.5AEFX1.5NPSH1-1/8&1/2MTLHD",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NYCORP","N/A","N/A","N/A","1-1/8\"; 1/2\"","N/A","N/A","N","ENGLISH","Breakapart Stack Tip","High-Range","Y",20,3,"1443",1.5,"NPSH",null,null,"1443 2.5 in NYCORP 1.5 in NPSH 1-1/8\"; 1/2\" bore size(s) NPG","14437005","SH/O NPG TIP2.5AEFX1.5NPSH1-1/8&1/2MTLHD",60]
["14434003","SH/O TIP 2.5AFB X 1.5ABU 1-1/8&1/2",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"FDNY","N/A","N/A","N/A","1-1/8\"; 1/2\"","N/A","N/A","N","ENGLISH","Breakapart Stack Tip","High-Range","N","No 2021 Sales","No 2021 Sales","1443",1.5,"FDNY",null,null,"1443 2.5 in FDNY 1.5 in FDNY 1-1/8\"; 1/2\" bore size(s) PG","14434003","SH/O TIP 2.5AFB X 1.5ABU 1-1/8&1/2",57]
["14434004","SH/O TIP 2.5AEF X 1.5NH 1-1/8&1/2 MTLHDL",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NYCORP","N/A","N/A","N/A","1-1/8\"; 1/2\"","n/a","N/A","N","ENGLISH","Breakapart Stack Tip","High-Range","N","No 2021 Sales","No 2021 Sales","1443",1.5,"NH",null,null,"1443 2.5 in NYCORP 1.5 in NH 1-1/8\"; 1/2\" bore size(s) PG","14434004","SH/O TIP 2.5AEF X 1.5NH 1-1/8&1/2 MTLHDL",57]
["14434005","SH/O TIP 2.5NPSH X 1.5NPSH 1-1/8&1/2",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NPSH","N/A","N/A","N/A","1-1/8\"; 1/2\"","N/A","N/A","N","ENGLISH","Breakapart Stack Tip","High-Range","N","No 2021 Sales","No 2021 Sales","1443",1.5,"NPSH",null,null,"1443 2.5 in NPSH 1.5 in NPSH 1-1/8\"; 1/2\" bore size(s) PG","14434005","SH/O TIP 2.5NPSH X 1.5NPSH 1-1/8&1/2",57]
["14434006","SH/O TIP 2.5AEF X 1.5NPSH 1-1/8&1/2",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NYCORP","N/A","N/A","N/A","1-1/8\"; 1/2\"","N/A","N/A","N","ENGLISH","Breakapart Stack Tip","High-Range","N","No 2021 Sales","No 2021 Sales","1443",1.5,"NPSH",null,null,"1443 2.5 in NYCORP 1.5 in NPSH 1-1/8\"; 1/2\" bore size(s) PG","14434006","SH/O TIP 2.5AEF X 1.5NPSH 1-1/8&1/2",59]
["14434007","SH/O TIP 2.5AEFX1.5NPSH 1-1/8&1/2 MTLHDL",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NYCORP","N/A","N/A","N/A","1-1/8\"; 1/2\"","N/A","N/A","N","ENGLISH","Breakapart Stack Tip","High-Range","N","No 2021 Sales","No 2021 Sales","1443",1.5,"NPSH",null,null,"1443 2.5 in NYCORP 1.5 in NPSH 1-1/8\"; 1/2\" bore size(s) PG","14434007","SH/O TIP 2.5AEFX1.5NPSH 1-1/8&1/2 MTLHDL",59]
["14437002","SH/O NPG TIP 2.5AEF X 1.5NH 1-1/8&1/2",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NYCORP","N/A","N/A","N/A","1-1/8\"; 1/2\"","n/a","N/A","N","ENGLISH","Breakapart Stack Tip","High-Range","Y","No 2021 Sales","No 2021 Sales","1443",1.5,"NH",null,null,"1443 2.5 in NYCORP 1.5 in NH 1-1/8\"; 1/2\" bore size(s) NPG","14437002","SH/O NPG TIP 2.5AEF X 1.5NH 1-1/8&1/2",58]
["14437003","SH/O NPG TIP 2.5AFB X 1.5ABU 1-1/8&1/2",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"FDNY","N/A","N/A","N/A","1-1/8\"; 1/2\"","N/A","N/A","N","ENGLISH","Breakapart Stack Tip","High-Range","Y","No 2021 Sales","No 2021 Sales","1443",1.5,"FDNY",null,null,"1443 2.5 in FDNY 1.5 in FDNY 1-1/8\"; 1/2\" bore size(s) NPG","14437003","SH/O NPG TIP 2.5AFB X 1.5ABU 1-1/8&1/2",58]
["14454003","SH/O TIP 1.5NH X 1.5NH 15/16",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","15/16\"","n/a","N/A","N","ENGLISH","Breakapart Solid Bore Tip","1.5\"","N",80,1,"1445",1.5,"NH",null,null,"1445 1.5 in NH 1.5 in NH 15/16\" bore size(s) PG","14454003","SH/O TIP 1.5NH X 1.5NH 15/16",47]
["14454002","SH/O TIP 1.5NH X 1.5NH 7/8",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","7/8\"","n/a","N/A","N","ENGLISH","Breakapart Solid Bore Tip","1.5\"","N",20,1,"1445",1.5,"NH",null,null,"1445 1.5 in NH 1.5 in NH 7/8\" bore size(s) PG","14454002","SH/O TIP 1.5NH X 1.5NH 7/8",45]
["14454001","SH/O TIP 1.5NH X 1.5NH 1-3/8",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","1-3/8\"","n/a","N/A","N","ENGLISH","Breakapart Solid Bore Tip","1.5\"","N",20,2,"1445",1.5,"NH",null,null,"1445 1.5 in NH 1.5 in NH 1-3/8\" bore size(s) PG","14454001","SH/O TIP 1.5NH X 1.5NH 1-3/8",47]
["14454007","SH/O TIP 1.5NPSH X 1.5NPSH 7/8",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NPSH","N/A","N/A","N/A","7/8\"","n/a","N/A","N","ENGLISH","Breakapart Solid Bore Tip","1.5\"","N",20,2,"1445",1.5,"NPSH",null,null,"1445 1.5 in NPSH 1.5 in NPSH 7/8\" bore size(s) PG","14454007","SH/O TIP 1.5NPSH X 1.5NPSH 7/8",49]
["14454004","SH/O TIP 1.5NPSH X 1.5NPSH 1-3/8",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NPSH","N/A","N/A","N/A","1-3/8\"","n/a","N/A","N","ENGLISH","Breakapart Solid Bore Tip","1.5\"","N",20,3,"1445",1.5,"NPSH",null,null,"1445 1.5 in NPSH 1.5 in NPSH 1-3/8\" bore size(s) PG","14454004","SH/O TIP 1.5NPSH X 1.5NPSH 1-3/8",51]
["14454006","SH/O TIP 1.5NPSH X 1.5NPSH 15/16",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NPSH","N/A","N/A","N/A","15/16\"","n/a","N/A","N","ENGLISH","Breakapart Solid Bore Tip","1.5\"","N",20,3,"1445",1.5,"NPSH",null,null,"1445 1.5 in NPSH 1.5 in NPSH 15/16\" bore size(s) PG","14454006","SH/O TIP 1.5NPSH X 1.5NPSH 15/16",51]
["14454008","SH/O TIP 1.5NH X 1.5NH 1",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","1\"","N/A","N/A","N","ENGLISH","Breakapart Solid Bore Tip","1.5\"","N",20,3,"1445",1.5,"NH",null,null,"1445 1.5 in NH 1.5 in NH 1\" bore size(s) PG","14454008","SH/O TIP 1.5NH X 1.5NH 1",43]
["14457002","SH/O NPG TIP 1.5NH X 1.5NH 7/8",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","7/8\"","N/A","N/A","N","ENGLISH","Breakapart Solid Bore Tip","1.5\"","Y",20,3,"1445",1.5,"NH",null,null,"1445 1.5 in NH 1.5 in NH 7/8\" bore size(s) NPG","14457002","SH/O NPG TIP 1.5NH X 1.5NH 7/8",46]
["14454005","SH/O TIP 1.5NH X 1.5NH 1-1/8",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","1-1/8\"","n/a","N/A","N","ENGLISH","Breakapart Solid Bore Tip","1.5\"","N","No 2021 Sales","No 2021 Sales","1445",1.5,"NH",null,null,"1445 1.5 in NH 1.5 in NH 1-1/8\" bore size(s) PG","14454005","SH/O TIP 1.5NH X 1.5NH 1-1/8",47]
["14457001","SH/O NPG TIP 1.5NH X 1.5NH 1-3/8",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","1-3/8\"","n/a","N/A","N","ENGLISH","Breakapart Solid Bore Tip","1.5\"","Y","No 2021 Sales","No 2021 Sales","1445",1.5,"NH",null,null,"1445 1.5 in NH 1.5 in NH 1-3/8\" bore size(s) NPG","14457001","SH/O NPG TIP 1.5NH X 1.5NH 1-3/8",48,{"$f":"AM632=AH632","v":true},"1445 1.5 in NH 1.5 in NH 1-3/8\" bore size(s) NPG"]
["14464001","SH/O TIP 2.5NH X 1.5NH 1-3/8",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","1-3/8\"","n/a","N/A","N","ENGLISH","Breakapart Solid Bore Tip","1.5\"","N",20,1,"1446",1.5,"NH",null,null,"1446 2.5 in NH 1.5 in NH 1-3/8\" bore size(s) PG","14464001","SH/O TIP 2.5NH X 1.5NH 1-3/8",47]
["14464005","SH/O TIP 2.5NH X 1.5NH 1-1/8",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","1-1/8\"","n/a","N/A","N","ENGLISH","Breakapart Solid Bore Tip","1.5\"","N",20,2,"1446",1.5,"NH",null,null,"1446 2.5 in NH 1.5 in NH 1-1/8\" bore size(s) PG","14464005","SH/O TIP 2.5NH X 1.5NH 1-1/8",47]
["14464007","SH/O TIP 2.5NH X 1.5NPSH 1-1/8",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","1-1/8\"","n/a","N/A","N","ENGLISH","Breakapart Solid Bore Tip","1.5\"","N",20,2,"1446",1.5,"NPSH",null,null,"1446 2.5 in NH 1.5 in NPSH 1-1/8\" bore size(s) PG","14464007","SH/O TIP 2.5NH X 1.5NPSH 1-1/8",49]
["14464008","SH/O TIP 2.5NH X 1.5NH 1-3/16",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","1-3/16\"","n/a","N/A","N","ENGLISH","Breakapart Solid Bore Tip","1.5\"","N",20,2,"1446",1.5,"NH",null,null,"1446 2.5 in NH 1.5 in NH 1-3/16\" bore size(s) PG","14464008","SH/O TIP 2.5NH X 1.5NH 1-3/16",48]
["14464002","SH/O TIP 2.5NH X 1.5NH 15/16",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","15/16\"","n/a","N/A","N","ENGLISH","Breakapart Solid Bore Tip","1.5\"","N",20,3,"1446",1.5,"NH",null,null,"1446 2.5 in NH 1.5 in NH 15/16\" bore size(s) PG","14464002","SH/O TIP 2.5NH X 1.5NH 15/16",47]
["14464003","SH/O TIP 2.5NH X 1.5NH 1-1/4",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","1-1/4\"","n/a","N/A","N","ENGLISH","Breakapart Solid Bore Tip","1.5\"","N",20,3,"1446",1.5,"NH",null,null,"1446 2.5 in NH 1.5 in NH 1-1/4\" bore size(s) PG","14464003","SH/O TIP 2.5NH X 1.5NH 1-1/4",47]
["14464016","SH/O TIP 2.5AII X 1.5NPSH 1-1/8 D",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"CSA","N/A","N/A","N/A","1-1/8\"","N/A","N/A","N","ENGLISH","Breakapart Solid Bore Tip","1.5\"","N",20,3,"1446",1.5,"NPSH",null,null,"1446 2.5 in CSA 1.5 in NPSH 1-1/8\" bore size(s) PG","14464016","SH/O TIP 2.5AII X 1.5NPSH 1-1/8 D",50]
["14464017","SH/O TIP 2.5NH X 1.5NH 1\" D",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","1\"","n/a","N/A","N","ENGLISH","Breakapart Solid Bore Tip","1.5\"","N",20,3,"1446",1.5,"NH",null,null,"1446 2.5 in NH 1.5 in NH 1\" bore size(s) PG","14464017","SH/O TIP 2.5NH X 1.5NH 1\" D",43]
["14464018","SH/O TIP 2.5NH X 1.5NH 7/8\" D",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","7/8\"","N/A","N/A","N","ENGLISH","Breakapart Solid Bore Tip","1.5\"","N",20,3,"1446",1.5,"NH",null,null,"1446 2.5 in NH 1.5 in NH 7/8\" bore size(s) PG","14464018","SH/O TIP 2.5NH X 1.5NH 7/8\" D",45]
["14464004","SH/O TIP 2.5AEF X 1.5NH 1-3/8",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NYCORP","N/A","N/A","N/A","1-3/8\"","n/a","N/A","N","ENGLISH","Breakapart Solid Bore Tip","1.5\"","N","No 2021 Sales","No 2021 Sales","1446",1.5,"NH",null,null,"1446 2.5 in NYCORP 1.5 in NH 1-3/8\" bore size(s) PG","14464004","SH/O TIP 2.5AEF X 1.5NH 1-3/8",51]
["14464006","SH/O TIP 2.5AII X 1.5NPSH 1-3/8",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"CSA","N/A","N/A","N/A","1-3/8\"","n/a","N/A","N","ENGLISH","Breakapart Solid Bore Tip","1.5\"","N","No 2021 Sales","No 2021 Sales","1446",1.5,"NPSH",null,null,"1446 2.5 in CSA 1.5 in NPSH 1-3/8\" bore size(s) PG","14464006","SH/O TIP 2.5AII X 1.5NPSH 1-3/8",50]
["14464009","SH/O TIP 2.5AHB X 1.5NH 1-1/4",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"AHB","N/A","N/A","N/A","1-1/4\"","n/a","N/A","N","ENGLISH","Breakapart Solid Bore Tip","1.5\"","N","No 2021 Sales","No 2021 Sales","1446",1.5,"NH",null,null,"1446 2.5 in AHB 1.5 in NH 1-1/4\" bore size(s) PG","14464009","SH/O TIP 2.5AHB X 1.5NH 1-1/4",48]
["14464010","SH/O TIP 2.5BAF X 1.5NPSH 1-1/8",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"BAT","N/A","N/A","N/A","1-1/8\"","n/a","N/A","N","ENGLISH","Breakapart Solid Bore Tip","1.5\"","N","No 2021 Sales","No 2021 Sales","1446",1.5,"NPSH",null,null,"1446 2.5 in BAT 1.5 in NPSH 1-1/8\" bore size(s) PG","14464010","SH/O TIP 2.5BAF X 1.5NPSH 1-1/8",50]
["14464011","SH/O TIP 2.5AII X 1.5NPSH 1-1/4 D",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"CSA","N/A","N/A","N/A","1-1/4\"","n/a","N/A","N","ENGLISH","Breakapart Solid Bore Tip","1.5\"","N","No 2021 Sales","No 2021 Sales","1446",1.5,"NPSH",null,null,"1446 2.5 in CSA 1.5 in NPSH 1-1/4\" bore size(s) PG","14464011","SH/O TIP 2.5AII X 1.5NPSH 1-1/4 D",50]
["14464012","SH/O TIP 2.5AEF X 1.5NH 1-1/8",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NYCORP","N/A","N/A","N/A","1-1/8\"","n/a","N/A","N","ENGLISH","Breakapart Solid Bore Tip","1.5\"","N","No 2021 Sales","No 2021 Sales","1446",1.5,"NH",null,null,"1446 2.5 in NYCORP 1.5 in NH 1-1/8\" bore size(s) PG","14464012","SH/O TIP 2.5AEF X 1.5NH 1-1/8",51]
["14464013","SH/O TIP 2.5AJZ X 1.5NH 1-3/8",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"AJZ","N/A","N/A","N/A","1-3/8\"","n/a","N/A","N","ENGLISH","Breakapart Solid Bore Tip","1.5\"","N","No 2021 Sales","No 2021 Sales","1446",1.5,"NH",null,null,"1446 2.5 in AJZ 1.5 in NH 1-3/8\" bore size(s) PG","14464013","SH/O TIP 2.5AJZ X 1.5NH 1-3/8",48]
["14464014","SH/O TIP 2.5NPSH X 1.5NPSH 1-1/8",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NPSH","N/A","N/A","N/A","1-1/8\"","N/A","N/A","N","ENGLISH","Breakapart Solid Bore Tip","1.5\"","N","No 2021 Sales","No 2021 Sales","1446",1.5,"NPSH",null,null,"1446 2.5 in NPSH 1.5 in NPSH 1-1/8\" bore size(s) PG","14464014","SH/O TIP 2.5NPSH X 1.5NPSH 1-1/8",51]
["14464019","SH/O TIP 2.5AJE X 1.5NH 1\" D",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"AJE","N/A","N/A","N/A","1\"","N/A","N/A","N","ENGLISH","Breakapart Solid Bore Tip","1.5\"","N","No 2021 Sales","No 2021 Sales","1446",1.5,"NH",null,null,{"$f":"CONCATENATE(AC650,\" \",N650,\" in \",O650,\" \",IF(AD650=\"n/a\",\"\",CONCATENATE(AD650,\" in \",AE650,\" \")),IF(Q650=\"n/a\",\"\",Q650),IF(S650=\"n/a\",\"\",CONCATENATE(IF(X650=\"saber\",\" \",\"\"),S650,\" bore size(s) \")),IF(T650=\"n/a\",\"\",CONCATENATE(IF(X650=\"saber\",\"\",\" \"),T650,IF(T650=100,\" (Std) \",IF(T650=87,\" (CE) \",\" \")))),IF(U650=\"n/a\",\"\",CONCATENATE(U650,IF(U650=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X650,3)=\"tip\",IF(LEFT(X650,1)=\"s\",\"\",IF(Z650=\"n\",IF(T650=\"N/A\",\"PG\",\" PG\"),IF(Z650=\"y\",IF(T650=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z650=\"n\",IF(T650=\"N/A\",\"PG\",\" PG\"),IF(Z650=\"y\",IF(T650=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF650=\"y\",\" ZT\",\"\"),IF(V650=\"N\",\"\",IF(S650=\"n/a\",\" ETCH\",IF(T650=\"N/A\",IF(RIGHT(X650,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X650=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"1446 2.5 in AJE 1.5 in NH 1\" bore size(s) PG"},{"$f":"A650","v":"14464019"},{"$f":"B650","v":"SH/O TIP 2.5AJE X 1.5NH 1\" D"},{"$f":"LEN(AH650)","v":44}]
["14464020","SH/O TIP 2.5AJE X 1.5NH 1-1/8",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"AJE","N/A","N/A","N/A","1-1/8\"","N/A","N/A","N","ENGLISH","Breakapart Solid Bore Tip","1.5\"","N","No 2021 Sales","No 2021 Sales","1446",1.5,"NH",null,null,"1446 2.5 in AJE 1.5 in NH 1-1/8\" bore size(s) PG","14464020","SH/O TIP 2.5AJE X 1.5NH 1-1/8",48]
["14464021","SH/O TIP 2.5ADU X 1.5NH 1-3/8",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"ADU","N/A","N/A","N/A","1-3/8\"","N/A","N/A","N","ENGLISH","Breakapart Solid Bore Tip","1.5\"","N","No 2021 Sales","No 2021 Sales","1446",1.5,"NH",null,null,"1446 2.5 in ADU 1.5 in NH 1-3/8\" bore size(s) PG","14464021","SH/O TIP 2.5ADU X 1.5NH 1-3/8",48]
["14467014","SH/O NPG TIP 2.5NPSH X 1.5NPSH 1-1/8",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NPSH","N/A","N/A","N/A","1-1/8\"","n/a","N/A","N","ENGLISH","Breakapart Solid Bore Tip","1.5\"","Y","No 2021 Sales","No 2021 Sales","1446",1.5,"NPSH",null,null,"1446 2.5 in NPSH 1.5 in NPSH 1-1/8\" bore size(s) NPG","14467014","SH/O NPG TIP 2.5NPSH X 1.5NPSH 1-1/8",52]
["14464015","SH/O TIP 2.5BAF X 1.5NPSH 1-3/8",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"BAT","N/A","N/A","N/A","1-3/8\"","N/A","N/A","N","ENGLISH","Breakapart Solid Bore Tip","1.5\"","N",20,3,"1446",1.5,"NPSH",null,null,"1446 2.5 in BAT 1.5 in NPSH 1-3/8\" bore size(s) PG","14464015","SH/O TIP 2.5BAF X 1.5NPSH 1-3/8",50]
["14470001","BALL SH/O 1.5X1.5NH W/TIP 1/2DSCH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","1/2\"","N/A","N/A","N","ENGLISH","Breakapart Solid Bore Tip","1.5\"","N","No 2021 Sales","No 2021 Sales","1447",1.5,"NH",null,null,"1447 1.5 in NH 1.5 in NH 1/2\" bore size(s) PG","14470001","BALL SH/O 1.5X1.5NH W/TIP 1/2DSCH",45]
["21024001","SHUTOFF 1.0NH X 1.0NH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1,"NH","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","1\"","N",20,3,"2102",1,"NH",null,null,"2102 1 in NH 1 in NH PG","21024001","SHUTOFF 1.0NH X 1.0NH",23]
["21024002","SHUTOFF 1.0NPSH X 1.0NH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1,"NPSH","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","1\"","N","No 2021 Sales","No 2021 Sales","2102",1,"NH",null,null,"2102 1 in NPSH 1 in NH PG","21024002","SHUTOFF 1.0NPSH X 1.0NH",25]
["21024003","SHUTOFF 1.0NPSH X 1.0NPSH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1,"NPSH","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","1\"","N","No 2021 Sales","No 2021 Sales","2102",1,"NPSH",null,null,"2102 1 in NPSH 1 in NPSH PG","21024003","SHUTOFF 1.0NPSH X 1.0NPSH",27]
["21027003","SHUTOFF NPG 1.0NPSH X 1.0NPSH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1,"NPSH","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","1\"","Y","No 2021 Sales","No 2021 Sales","2102",1,"NPSH",null,null,"2102 1 in NPSH 1 in NPSH NPG","21027003","SHUTOFF NPG 1.0NPSH X 1.0NPSH",28]
["21027004","SHUTOFF NPG 1.0NH X 1.0NH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1,"NH","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","1\"","Y","No 2021 Sales","No 2021 Sales","2102",1,"NH",null,null,"2102 1 in NH 1 in NH NPG","21027004","SHUTOFF NPG 1.0NH X 1.0NH",24]
["21264001","SHUTOFF 2.5NH  X 1.5NH#",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N",80,1,"2126",1.5,"NH",null,null,"2126 2.5 in NH 1.5 in NH PG","21264001","SHUTOFF 2.5NH  X 1.5NH#",27]
["21267002","SHUTOFF NPG 2.5NH  X 1.5NH#",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","Y",80,1,"2126",1.5,"NH",null,null,"2126 2.5 in NH 1.5 in NH NPG","21267002","SHUTOFF NPG 2.5NH  X 1.5NH#",28]
["21264007","SHUTOFF 2.5BAF X 1.5NPSH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"BAT","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N",20,1,"2126",1.5,"NPSH",null,null,"2126 2.5 in BAT 1.5 in NPSH PG","21264007","SHUTOFF 2.5BAF X 1.5NPSH",30]
["21264009","SHUTOFF 2.5AEF  X 1.5NH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NYCORP","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N",20,2,"2126",1.5,"NH",null,null,"2126 2.5 in NYCORP 1.5 in NH PG","21264009","SHUTOFF 2.5AEF  X 1.5NH",31]
["21267001","SHUTOFF NPG 2.5BAF X 1.5NPSH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"BAT","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","Y",20,2,"2126",1.5,"NPSH",null,null,"2126 2.5 in BAT 1.5 in NPSH NPG","21267001","SHUTOFF NPG 2.5BAF X 1.5NPSH",31]
["21264014","SHUTOFF 2.5NPSH  X 1.5NPSH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NPSH","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N",20,3,"2126",1.5,"NPSH",null,null,"2126 2.5 in NPSH 1.5 in NPSH PG","21264014","SHUTOFF 2.5NPSH  X 1.5NPSH",31]
["21264041","SHUTOFF 2.5AEF X 1.5ABQ",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NYCORP","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N",20,3,"2126",1.5,"NYCORP",null,null,"2126 2.5 in NYCORP 1.5 in NYCORP PG","21264041","SHUTOFF 2.5AEF X 1.5ABQ",35]
["21264042","SHUTOFF 2.5AGW  X 1.5NH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"AGW","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N",20,3,"2126",1.5,"NH",null,null,"2126 2.5 in AGW 1.5 in NH PG","21264042","SHUTOFF 2.5AGW  X 1.5NH",28]
["21264051","SHUTOFF 2.5ATV  X 1.5NH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","N/A","N/A","N/A","N","ENGLISH","Shutoff","High-Range","N",20,3,"2126",1.5,"NH",null,null,{"$f":"CONCATENATE(AC669,\" \",N669,\" in \",O669,\" \",IF(AD669=\"n/a\",\"\",CONCATENATE(AD669,\" in \",AE669,\" \")),IF(Q669=\"n/a\",\"\",Q669),IF(S669=\"n/a\",\"\",CONCATENATE(IF(X669=\"saber\",\" \",\"\"),S669,\" bore size(s) \")),IF(T669=\"n/a\",\"\",CONCATENATE(IF(X669=\"saber\",\"\",\" \"),T669,IF(T669=100,\" (Std) \",IF(T669=87,\" (CE) \",\" \")))),IF(U669=\"n/a\",\"\",CONCATENATE(U669,IF(U669=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X669,3)=\"tip\",IF(LEFT(X669,1)=\"s\",\"\",IF(Z669=\"n\",IF(T669=\"N/A\",\"PG\",\" PG\"),IF(Z669=\"y\",IF(T669=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z669=\"n\",IF(T669=\"N/A\",\"PG\",\" PG\"),IF(Z669=\"y\",IF(T669=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF669=\"y\",\" ZT\",\"\"),IF(V669=\"N\",\"\",IF(S669=\"n/a\",\" ETCH\",IF(T669=\"N/A\",IF(RIGHT(X669,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X669=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"2126 2.5 in NH 1.5 in NH PG"},{"$f":"A669","v":"21264051"},{"$f":"B669","v":"SHUTOFF 2.5ATV  X 1.5NH"},{"$f":"LEN(AH669)","v":27}]
["21264056","SHUTOFF 2.5AJE  X 1.5NH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"AJE","N/A","N/A","N/A","N/A","N/A","N/A","N","ENGLISH","Shutoff","High-Range","N",20,3,"2126",1.5,"NH",null,null,"2126 2.5 in AJE 1.5 in NH PG","21264056","SHUTOFF 2.5AJE  X 1.5NH",28]
["21264054","SHUTOFF ZT 2.5NH X 1.5NH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N",20,3,"2126",1.5,"NH","Y",null,"2126 2.5 in NH 1.5 in NH PG ZT","21264054","SHUTOFF ZT 2.5NH X 1.5NH",30]
["21267006","SHUTOFF NPG 2.5NH  X 1.5NPSH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","Y",20,3,"2126",1.5,"NPSH",null,null,"2126 2.5 in NH 1.5 in NPSH NPG","21267006","SHUTOFF NPG 2.5NH  X 1.5NPSH",30]
["21267025","SHUTOFF NPG 2.5NH  X 1.5NH BDVFD",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","N/A","N/A","N/A","Y","ENGLISH","Shutoff","High-Range","Y",20,3,"2126",1.5,"NH",null,null,"2126 2.5 in NH 1.5 in NH NPG ETCH","21267025","SHUTOFF NPG 2.5NH  X 1.5NH BDVFD",33]
["21264002","SHUTOFF 2.5JIM X 1.5NH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"JIM","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N",20,4,"2126",1.5,"NH",null,null,"2126 2.5 in JIM 1.5 in NH PG","21264002","SHUTOFF 2.5JIM X 1.5NH",28]
["21264050","SHUTOFF 2.5NH X 1.5NH ENG80INE",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","N/A","N/A","N/A","Y","ENGLISH","Shutoff","High-Range","N",20,4,"2126",1.5,"NH",null,null,{"$f":"CONCATENATE(AC675,\" \",N675,\" in \",O675,\" \",IF(AD675=\"n/a\",\"\",CONCATENATE(AD675,\" in \",AE675,\" \")),IF(Q675=\"n/a\",\"\",Q675),IF(S675=\"n/a\",\"\",CONCATENATE(IF(X675=\"saber\",\" \",\"\"),S675,\" bore size(s) \")),IF(T675=\"n/a\",\"\",CONCATENATE(IF(X675=\"saber\",\"\",\" \"),T675,IF(T675=100,\" (Std) \",IF(T675=87,\" (CE) \",\" \")))),IF(U675=\"n/a\",\"\",CONCATENATE(U675,IF(U675=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X675,3)=\"tip\",IF(LEFT(X675,1)=\"s\",\"\",IF(Z675=\"n\",IF(T675=\"N/A\",\"PG\",\" PG\"),IF(Z675=\"y\",IF(T675=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z675=\"n\",IF(T675=\"N/A\",\"PG\",\" PG\"),IF(Z675=\"y\",IF(T675=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF675=\"y\",\" ZT\",\"\"),IF(V675=\"N\",\"\",IF(S675=\"n/a\",\" ETCH\",IF(T675=\"N/A\",IF(RIGHT(X675,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X675=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"2126 2.5 in NH 1.5 in NH PG ETCH"},{"$f":"A675","v":"21264050"},{"$f":"B675","v":"SHUTOFF 2.5NH X 1.5NH ENG80INE"},{"$f":"LEN(AH675)","v":32}]
["21267014","SHUTOFF NPG 2.5NPSH  X 1.5NPSH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NPSH","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","Y",20,4,"2126",1.5,"NPSH",null,null,"2126 2.5 in NPSH 1.5 in NPSH NPG","21267014","SHUTOFF NPG 2.5NPSH  X 1.5NPSH",32]
["21264003","SHUTOFF 2.5AII X 1.5NPSH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"CSA","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2126",1.5,"NPSH",null,null,"2126 2.5 in CSA 1.5 in NPSH PG","21264003","SHUTOFF 2.5AII X 1.5NPSH",30]
["21264004","SHUTOFF 2.5BIM X 1.5BSP",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"BIM","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2126",1.5,"BSP",null,null,"2126 2.5 in BIM 1.5 in BSP PG","21264004","SHUTOFF 2.5BIM X 1.5BSP",29]
["21264006","SHUTOFF 2.5NH  X 1.5NPSH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2126",1.5,"NPSH",null,null,"2126 2.5 in NH 1.5 in NPSH PG","21264006","SHUTOFF 2.5NH  X 1.5NPSH",29]
["21264013","SHUTOFF 2.5AGZ  X 1.5NH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"AGZ","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2126",1.5,"NH",null,null,"2126 2.5 in AGZ 1.5 in NH PG","21264013","SHUTOFF 2.5AGZ  X 1.5NH",28]
["21264059","SHUTOFF 2.5ADU  X 1.5NH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"ADU","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2126",1.5,"NH",null,null,{"$f":"CONCATENATE(AC681,\" \",N681,\" in \",O681,\" \",IF(AD681=\"n/a\",\"\",CONCATENATE(AD681,\" in \",AE681,\" \")),IF(Q681=\"n/a\",\"\",Q681),IF(S681=\"n/a\",\"\",CONCATENATE(IF(X681=\"saber\",\" \",\"\"),S681,\" bore size(s) \")),IF(T681=\"n/a\",\"\",CONCATENATE(IF(X681=\"saber\",\"\",\" \"),T681,IF(T681=100,\" (Std) \",IF(T681=87,\" (CE) \",\" \")))),IF(U681=\"n/a\",\"\",CONCATENATE(U681,IF(U681=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X681,3)=\"tip\",IF(LEFT(X681,1)=\"s\",\"\",IF(Z681=\"n\",IF(T681=\"N/A\",\"PG\",\" PG\"),IF(Z681=\"y\",IF(T681=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z681=\"n\",IF(T681=\"N/A\",\"PG\",\" PG\"),IF(Z681=\"y\",IF(T681=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF681=\"y\",\" ZT\",\"\"),IF(V681=\"N\",\"\",IF(S681=\"n/a\",\" ETCH\",IF(T681=\"N/A\",IF(RIGHT(X681,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X681=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"2126 2.5 in ADU 1.5 in NH PG"},{"$f":"A681","v":"21264059"},{"$f":"B681","v":"SHUTOFF 2.5ADU  X 1.5NH"},{"$f":"LEN(AH681)","v":28}]
["21264015","SHUTOFF 2.5AFD X 1.5NPSH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"QST","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2126",1.5,"NPSH",null,null,"2126 2.5 in QST 1.5 in NPSH PG","21264015","SHUTOFF 2.5AFD X 1.5NPSH",30]
["21264016","SHUTOFF 2.5AGW  X 1.5ABT",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"AGW","N/A","N/A","N/A","N/A","N/A","N/A","N","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2126",1.5,"PCT",null,null,"2126 2.5 in AGW 1.5 in PCT PG","21264016","SHUTOFF 2.5AGW  X 1.5ABT",29]
["21264017","SHUTOFF 2.5AHB  X 1.5NH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"AHB","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2126",1.5,"NH",null,null,"2126 2.5 in AHB 1.5 in NH PG","21264017","SHUTOFF 2.5AHB  X 1.5NH",28]
["21264018","SHUTOFF 2.5AFY X 1.5NH METAL HDL",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"PITT6","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2126",1.5,"NH",null,null,"2126 2.5 in PITT6 1.5 in NH PG","21264018","SHUTOFF 2.5AFY X 1.5NH METAL HDL",30]
["21264019","SHUTOFF 2.5ADF  X 1.5NH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"ADF","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2126",1.5,"NH",null,null,"2126 2.5 in ADF 1.5 in NH PG","21264019","SHUTOFF 2.5ADF  X 1.5NH",28]
["21264021","SHUTOFF 2.5AFB X 1.5ABU FDNY",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"FDNY","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","Y","No 2021 Sales","No 2021 Sales","2126",1.5,"FDNY",null,null,"2126 2.5 in FDNY 1.5 in FDNY NPG","21264021","SHUTOFF 2.5AFB X 1.5ABU FDNY",32]
["21264028","SHUTOFF 2.5AIP X 1.5NH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"AIP","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2126",1.5,"NH",null,null,"2126 2.5 in AIP 1.5 in NH PG","21264028","SHUTOFF 2.5AIP X 1.5NH",28]
["21264030","SHUTOFF 2.5AEF X 1.5NH METAL HDL",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NYCORP","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2126",1.5,"NH",null,null,"2126 2.5 in NYCORP 1.5 in NH PG","21264030","SHUTOFF 2.5AEF X 1.5NH METAL HDL",31]
["21264031","SHUTOFF 2.5AFY  X 1.5NH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"PITT6","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2126",1.5,"NPSH",null,null,"2126 2.5 in PITT6 1.5 in NPSH PG","21264031","SHUTOFF 2.5AFY  X 1.5NH",32]
["21264032","SHUTOFF 2.5AEF  X 1.5NPSH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NYCORP","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2126",1.5,"NPSH",null,null,"2126 2.5 in NYCORP 1.5 in NPSH PG","21264032","SHUTOFF 2.5AEF  X 1.5NPSH",33]
["21264033","SHUTOFF 2.5AEF X 1.5NPSH METAL HDL",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NYCORP","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2126",1.5,"NPSH",null,null,"2126 2.5 in NYCORP 1.5 in NPSH PG","21264033","SHUTOFF 2.5AEF X 1.5NPSH METAL HDL",33]
["21264034","SHUTOFF 2.5AKB X 1.5NPSH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"AKB","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2126",1.5,"NH",null,null,"2126 2.5 in AKB 1.5 in NH PG","21264034","SHUTOFF 2.5AKB X 1.5NPSH",28]
["21264038","SHUTOFF 2.5AJZ  X 1.5NH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"AJZ","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2126",1.5,"NH",null,null,"2126 2.5 in AJZ 1.5 in NH PG","21264038","SHUTOFF 2.5AJZ  X 1.5NH",28]
["21264039","SHUTOFF 2.5AKB X 1.5NH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"AKB","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2126",1.5,"NH",null,null,"2126 2.5 in AKB 1.5 in NH PG","21264039","SHUTOFF 2.5AKB X 1.5NH",28]
["21264052","SHUTOFF 2.5AKE X 1.5NH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"AKE","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2126",1.5,"NH",null,null,"2126 2.5 in AKE 1.5 in NH PG","21264052","SHUTOFF 2.5AKE X 1.5NH",28]
["21264057","SHUTOFF 65MM X 1.5NPSH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"STORZ","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2126",1.5,"NPSH",null,null,"2126 2.5 in STORZ 1.5 in NPSH PG","21264057","SHUTOFF 65MM X 1.5NPSH",32]
["21267003","SHUTOFF NPG 2.5NH  X 1.5NH MTLHDL",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","Y","No 2021 Sales","No 2021 Sales","2126",1.5,"NH",null,null,"2126 2.5 in NH 1.5 in NH NPG","21267003","SHUTOFF NPG 2.5NH  X 1.5NH MTLHDL",28]
["21267004","SHUTOFF NPG 2.5AFO  X 1.5NH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"AFO","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","Y","No 2021 Sales","No 2021 Sales","2126",1.5,"NH",null,null,"2126 2.5 in AFO 1.5 in NH NPG","21267004","SHUTOFF NPG 2.5AFO  X 1.5NH",29]
["21267009","SHUTOFF NPG 2.5AEF  X 1.5NH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NYCORP","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","Y","No 2021 Sales","No 2021 Sales","2126",1.5,"NH",null,null,"2126 2.5 in NYCORP 1.5 in NH NPG","21267009","SHUTOFF NPG 2.5AEF  X 1.5NH",32]
["21267011","SHUTOFF NPG 2.5AIK X 1.5NH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"AIK","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","Y","No 2021 Sales","No 2021 Sales","2126",1.5,"NH",null,null,"2126 2.5 in AIK 1.5 in NH NPG","21267011","SHUTOFF NPG 2.5AIK X 1.5NH",29]
["21267013","SHUTOFF NPG 2.5AGZ  X 1.5NH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"AGZ","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","Y","No 2021 Sales","No 2021 Sales","2126",1.5,"NH",null,null,"2126 2.5 in AGZ 1.5 in NH NPG","21267013","SHUTOFF NPG 2.5AGZ  X 1.5NH",29]
["21267021","SHUTOFF NPG 2.5AFB X 1.5ABU FDNY",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"FDNY","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","Y","No 2021 Sales","No 2021 Sales","2126",1.5,"FDNY",null,null,"2126 2.5 in FDNY 1.5 in FDNY NPG","21267021","SHUTOFF NPG 2.5AFB X 1.5ABU FDNY",32]
["21267035","SHUTOFF NPG 2.5NH X 1.5NH CHARLOTTE FD",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","Y","No 2021 Sales","No 2021 Sales","2126",1.5,"NH",null,null,"2126 2.5 in NH 1.5 in NH NPG","21267035","SHUTOFF NPG 2.5NH X 1.5NH CHARLOTTE FD",28]
["21274001","SHUTOFF 1.5NH X 1.5NH#",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","1.5\"","N",80,1,"2127",1.5,"NH",null,null,"2127 1.5 in NH 1.5 in NH PG","21274001","SHUTOFF 1.5NH X 1.5NH#",27]
["21274006","SHUTOFF 1.5NPSH X 1.5NPSH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NPSH","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","1.5\"","N",80,1,"2127",1.5,"NPSH",null,null,"2127 1.5 in NPSH 1.5 in NPSH PG","21274006","SHUTOFF 1.5NPSH X 1.5NPSH",31]
["21277001","SHUTOFF NPG 1.5NH X 1.5NH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","1.5\"","Y",80,1,"2127",1.5,"NH",null,null,"2127 1.5 in NH 1.5 in NH NPG","21277001","SHUTOFF NPG 1.5NH X 1.5NH",28]
["21274024","SHUTOFF 2.5BIM X 1.5BSP",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"BIM","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","1.5\"","N",20,2,"2127",1.5,"BSP",null,null,"2127 2.5 in BIM 1.5 in BSP PG","21274024","SHUTOFF 2.5BIM X 1.5BSP",29]
["21274036","SHUTOFF 1.5BSP F X 1.5NH M",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"BSP","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","1.5\"","N",20,2,"2127",1.5,"NH",null,null,"2127 1.5 in BSP 1.5 in NH PG","21274036","SHUTOFF 1.5BSP F X 1.5NH M",28]
["21274053","SHUTOFF 1.5NH X 1.5NH SEQ ETCH F20009",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","N/A","N/A","N/A","Y","ENGLISH","Shutoff","1.5\"","N",20,2,"2127",1.5,"NH",null,null,"2127 1.5 in NH 1.5 in NH PG ETCH","21274053","SHUTOFF 1.5NH X 1.5NH SEQ ETCH F20009",32]
["21277002","SHUTOFF NPG 1.5NH X 1.5NH MTLHDL",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","1.5\"","Y",20,2,"2127",1.5,"NH",null,null,"2127 1.5 in NH 1.5 in NH NPG","21277002","SHUTOFF NPG 1.5NH X 1.5NH MTLHDL",28]
["21277006","SHUTOFF NPG 1.5NPSH X 1.5NPSH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NPSH","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","1.5\"","Y",20,2,"2127",1.5,"NPSH",null,null,"2127 1.5 in NPSH 1.5 in NPSH NPG","21277006","SHUTOFF NPG 1.5NPSH X 1.5NPSH",32]
["21274011","SHUTOFF 1.5NPSH X 1.5NH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NPSH","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","1.5\"","N",20,3,"2127",1.5,"NH",null,null,"2127 1.5 in NPSH 1.5 in NH PG","21274011","SHUTOFF 1.5NPSH X 1.5NH",29]
["21274042","SHUTOFF 1.5ABT X 1.5ABT",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"PCT","N/A","N/A","N/A","N/A","N/A","N/A","N","ENGLISH","Shutoff","1.5\"","N",20,3,"2127",1.5,"PCT",null,null,"2127 1.5 in PCT 1.5 in PCT PG","21274042","SHUTOFF 1.5ABT X 1.5ABT",29]
["21274052","SHUTOFF 1.5NH X 1.5NH OCEAN VIEW FIRE CO",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","N/A","N/A","N/A","Y","ENGLISH","Shutoff","1.5\"","N",20,3,"2127",1.5,"NH",null,null,"2127 1.5 in NH 1.5 in NH PG ETCH","21274052","SHUTOFF 1.5NH X 1.5NH OCEAN VIEW FIRE CO",32]
["21274056","SHUTOFF ZT 1.5NH X 1.5NH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","1.5\"","N",20,3,"2127",1.5,"NH","Y",null,"2127 1.5 in NH 1.5 in NH PG ZT","21274056","SHUTOFF ZT 1.5NH X 1.5NH",30]
["21274002","SHUTOFF 1.5ABU X 1.5ABU FDNY",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"FDNY","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","1.5\"","N",20,4,"2127",1.5,"FDNY",null,null,"2127 1.5 in FDNY 1.5 in FDNY PG","21274002","SHUTOFF 1.5ABU X 1.5ABU FDNY",31]
["21274025","SHUTOFF 1.5ABX X 1.5ABX",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"ABX","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","1.5\"","N",20,4,"2127",1.5,"ABX",null,null,"2127 1.5 in ABX 1.5 in ABX PG","21274025","SHUTOFF 1.5ABX X 1.5ABX",29]
["21274048","SHUTOFF 1.5NH X 1.5NH ENG80INE",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","N/A","N/A","N/A","Y","ENGLISH","Shutoff","1.5\"","N",20,4,"2127",1.5,"NH",null,null,"2127 1.5 in NH 1.5 in NH PG ETCH","21274048","SHUTOFF 1.5NH X 1.5NH ENG80INE",32]
["21274049","SHUTOFF 1.5NH X 1.5NH COPLE VFD",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","N/A","N/A","N/A","Y","ENGLISH","Shutoff","1.5\"","N",20,4,"2127",1.5,"NH",null,null,"2127 1.5 in NH 1.5 in NH PG ETCH","21274049","SHUTOFF 1.5NH X 1.5NH COPLE VFD",32]
["21274051","SHUTOFF 1.5NH X 1.5NH BFC-E1",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","N/A","N/A","N/A","Y","ENGLISH","Shutoff","1.5\"","N",20,4,"2127",1.5,"NH",null,null,"2127 1.5 in NH 1.5 in NH PG ETCH","21274051","SHUTOFF 1.5NH X 1.5NH BFC-E1",32]
["21274005","SHUTOFF 2.5BIM X 1.5NH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"BIM","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","1.5\"","N","No 2021 Sales","No 2021 Sales","2127",1.5,"NH",null,null,"2127 2.5 in BIM 1.5 in NH PG","21274005","SHUTOFF 2.5BIM X 1.5NH",28]
["21274007","SHUTOFF 1.5BSP F X 1.5BSP M",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"BSP","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","1.5\"","N","No 2021 Sales","No 2021 Sales","2127",1.5,"BSP",null,null,"2127 1.5 in BSP 1.5 in BSP PG","21274007","SHUTOFF 1.5BSP F X 1.5BSP M",29]
["21274009","SHUTOFF ZT 52MM X 1.5NH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2,"STORZ","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","1.5\"","N","No 2021 Sales","No 2021 Sales","2127",1.5,"NH","Y",null,"2127 2 in STORZ 1.5 in NH PG ZT","21274009","SHUTOFF ZT 52MM X 1.5NH",31]
["21274014","SHUTOFF 1.5NH X 1.5NH METAL HDL",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","1.5\"","N","No 2021 Sales","No 2021 Sales","2127",1.5,"NH",null,null,"2127 1.5 in NH 1.5 in NH PG","21274014","SHUTOFF 1.5NH X 1.5NH METAL HDL",27]
["21274027","SHUTOFF 52MM X 1.5NH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2,"STORZ","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","1.5\"","N","No 2021 Sales","No 2021 Sales","2127",1.5,"NH",null,null,"2127 2 in STORZ 1.5 in NH PG","21274027","SHUTOFF 52MM X 1.5NH",28]
["21274033","SHUTOFF 1.5ABQ X 1.5ABQ",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NYCORP","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","1.5\"","N","No 2021 Sales","No 2021 Sales","2127",1.5,"NYCORP",null,null,"2127 1.5 in NYCORP 1.5 in NYCORP PG","21274033","SHUTOFF 1.5ABQ X 1.5ABQ",35]
["21274043","SHUTOFF 1.5NPSH X 1.5NPSH  METAL HDL",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NPSH","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","1.5\"","N","No 2021 Sales","No 2021 Sales","2127",1.5,"NPSH",null,null,"2127 1.5 in NPSH 1.5 in NPSH PG","21274043","SHUTOFF 1.5NPSH X 1.5NPSH  METAL HDL",31]
["21277004","SHUTOFF NPG 1.5ABU X 1.5ABU FDNY",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"FDNY","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","1.5\"","Y","No 2021 Sales","No 2021 Sales","2127",1.5,"FDNY",null,null,"2127 1.5 in FDNY 1.5 in FDNY NPG","21277004","SHUTOFF NPG 1.5ABU X 1.5ABU FDNY",32]
["21277011","SHUTOFF NPG 1.5NPSH X 1.5NH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NPSH","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","1.5\"","Y","No 2021 Sales","No 2021 Sales","2127",1.5,"NH",null,null,"2127 1.5 in NPSH 1.5 in NH NPG","21277011","SHUTOFF NPG 1.5NPSH X 1.5NH",30]
["21300100","SHUTOFF TRIDENT 2.5 NH F X 2.5 NH M#",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N",20,1,"2130",2.5,"NH",null,null,"2130 2.5 in NH 2.5 in NH PG","21300100","SHUTOFF TRIDENT 2.5 NH F X 2.5 NH M#",27]
["21300123","SH/OFF TRIDENT 2.5NHX2.5NH SEQ ETCH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","N/A","N/A","N/A","Y","ENGLISH","Shutoff","High-Range","N",20,2,"2130",2.5,"NH",null,null,"2130 2.5 in NH 2.5 in NH PG ETCH","21300123","SH/OFF TRIDENT 2.5NHX2.5NH SEQ ETCH",32]
["21300101","SHUTOFF TRIDENT 2.5AII F X 2.5 AII M",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"CSA","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2130",2.5,"CSA",null,null,"2130 2.5 in CSA 2.5 in CSA PG","21300101","SHUTOFF TRIDENT 2.5AII F X 2.5 AII M",29]
["21300102","SHUTOFF TRIDENT 2.5 AKB F X 2.5 AKB M",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"AKB","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2130",2.5,"AKB",null,null,"2130 2.5 in AKB 2.5 in AKB PG","21300102","SHUTOFF TRIDENT 2.5 AKB F X 2.5 AKB M",29]
["21300103","SHUTOFF TRIDENT 2.5 AFD F X 2.5AFD M",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"QST","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2130",2.5,"QST",null,null,"2130 2.5 in QST 2.5 in QST PG","21300103","SHUTOFF TRIDENT 2.5 AFD F X 2.5AFD M",29]
["21300105","SHUTOFF TRIDENT 2.5 BSP F X 2.5 BSP M PY",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"BSP","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2130",2.5,"BSP",null,null,"2130 2.5 in BSP 2.5 in BSP PG","21300105","SHUTOFF TRIDENT 2.5 BSP F X 2.5 BSP M PY",29]
["21300106","SHUTOFF TRIDENT 2.5NPSH F X 2.5NPSH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NPSH","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2130",2.5,"NPSH",null,null,"2130 2.5 in NPSH 2.5 in NPSH PG","21300106","SHUTOFF TRIDENT 2.5NPSH F X 2.5NPSH",31]
["21300109","SHUTOFF TRIDENT 2.5BAF F X 2.5BAF M",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"BAT","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2130",2.5,"BAT",null,null,"2130 2.5 in BAT 2.5 in BAT PG","21300109","SHUTOFF TRIDENT 2.5BAF F X 2.5BAF M",29]
["21300110","SHUTOFF TRIDENT 2.5ASM F X 2.5ASM M",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"ASM","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2130",2.5,"ASM",null,null,"2130 2.5 in ASM 2.5 in ASM PG","21300110","SHUTOFF TRIDENT 2.5ASM F X 2.5ASM M",29]
["21300111","SHUTOFF TRIDENT 2.5AIK F X 2.5AIK M",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"AIK","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2130",2.5,"AIK",null,null,{"$f":"CONCATENATE(AC740,\" \",N740,\" in \",O740,\" \",IF(AD740=\"n/a\",\"\",CONCATENATE(AD740,\" in \",AE740,\" \")),IF(Q740=\"n/a\",\"\",Q740),IF(S740=\"n/a\",\"\",CONCATENATE(IF(X740=\"saber\",\" \",\"\"),S740,\" bore size(s) \")),IF(T740=\"n/a\",\"\",CONCATENATE(IF(X740=\"saber\",\"\",\" \"),T740,IF(T740=100,\" (Std) \",IF(T740=87,\" (CE) \",\" \")))),IF(U740=\"n/a\",\"\",CONCATENATE(U740,IF(U740=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X740,3)=\"tip\",IF(LEFT(X740,1)=\"s\",\"\",IF(Z740=\"n\",IF(T740=\"N/A\",\"PG\",\" PG\"),IF(Z740=\"y\",IF(T740=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z740=\"n\",IF(T740=\"N/A\",\"PG\",\" PG\"),IF(Z740=\"y\",IF(T740=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF740=\"y\",\" ZT\",\"\"),IF(V740=\"N\",\"\",IF(S740=\"n/a\",\" ETCH\",IF(T740=\"N/A\",IF(RIGHT(X740,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X740=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"2130 2.5 in AIK 2.5 in AIK PG"},{"$f":"A740","v":"21300111"},{"$f":"B740","v":"SHUTOFF TRIDENT 2.5AIK F X 2.5AIK M"},{"$f":"LEN(AH740)","v":29}]
["21300113","SHUTOFF TRIDENT 2.5AGA F X 2.5AGA M",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"AGA","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2130",2.5,"AGA",null,null,"2130 2.5 in AGA 2.5 in AGA PG","21300113","SHUTOFF TRIDENT 2.5AGA F X 2.5AGA M",29]
["21300114","SHUTOFF TRIDENT 2.5 AUS F X 2.5AFD M",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"AUS","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2130",2.5,"QST",null,null,"2130 2.5 in AUS 2.5 in QST PG","21300114","SHUTOFF TRIDENT 2.5 AUS F X 2.5AFD M",29]
["21300116","SHUTOFF TRIDENT 2.5 AFY F X 2.5AFY M",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"PITT6","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2130",2.5,"PITT6",null,null,"2130 2.5 in PITT6 2.5 in PITT6 PG","21300116","SHUTOFF TRIDENT 2.5 AFY F X 2.5AFY M",33]
["21300118","SHUTOFF TRIDENT 2.5ACY X 2.5NH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"ACY","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2130",2.5,"NH",null,null,"2130 2.5 in ACY 2.5 in NH PG","21300118","SHUTOFF TRIDENT 2.5ACY X 2.5NH",28]
["21300119","SHUTOFF TRIDENT 2.5BIM X 2.5BSP M PY",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"BIM","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2130",2.5,"BSP",null,null,"2130 2.5 in BIM 2.5 in BSP PG","21300119","SHUTOFF TRIDENT 2.5BIM X 2.5BSP M PY",29]
["23904001","PLAYPIPE W/SO 2.5NH X 1.5NH#",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N/A",80,1,"2390",1.5,"NH",null,null,"2390 2.5 in NH 1.5 in NH  ","23904001","PLAYPIPE W/SO 2.5NH X 1.5NH#",26]
["23904026","PLAYPIPE W/SO 2.5NH X 1.5NH D.C.F.D.",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","N/A","N/A","N/A","Y","ENGLISH","Shutoff","High-Range","N/A",20,2,"2390",1.5,"NH",null,null,"2390 2.5 in NH 1.5 in NH   ETCH","23904026","PLAYPIPE W/SO 2.5NH X 1.5NH D.C.F.D.",31]
["23904013","PLAYPIPE W/SO 2.5AHB X 1.5NH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"AHB","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N/A",20,3,"2390",1.5,"NH",null,null,"2390 2.5 in AHB 1.5 in NH  ","23904013","PLAYPIPE W/SO 2.5AHB X 1.5NH",27]
["23904016","PLAYPIPE W/SO 2.5BAF X 1.5NPSH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"BAT","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N/A",20,3,"2390",1.5,"NPSH",null,null,"2390 2.5 in BAT 1.5 in NPSH  ","23904016","PLAYPIPE W/SO 2.5BAF X 1.5NPSH",29]
["23904021","PLAYPIPE W/SO 75MM X 1.5BSP",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",3,"STORZ","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N/A",20,3,"2390",1.5,"BSP",null,null,"2390 3 in STORZ 1.5 in BSP  ","23904021","PLAYPIPE W/SO 75MM X 1.5BSP",28]
["23904023","PLAYPIPE W/SO 2.5AJD X 1.5NH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","N/A","N/A","N/A","N","ENGLISH","Shutoff","High-Range","N/A",20,3,"2390",1.5,"NH",null,null,"2390 2.5 in NH 1.5 in NH  ","23904023","PLAYPIPE W/SO 2.5AJD X 1.5NH",26]
["23904006","PLAYPIPE W/SO 2.5AII X 1.5NPSH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"CSA","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N/A","No 2021 Sales","No 2021 Sales","2390",1.5,"NPSH",null,null,"2390 2.5 in CSA 1.5 in NPSH  ","23904006","PLAYPIPE W/SO 2.5AII X 1.5NPSH",29]
["23904007","PLAYPIPE W/SO 2.5AKB X 1.5NPSH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"AKB","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N/A","No 2021 Sales","No 2021 Sales","2390",1.5,"NPSH",null,null,"2390 2.5 in AKB 1.5 in NPSH  ","23904007","PLAYPIPE W/SO 2.5AKB X 1.5NPSH",29]
["23904008","PLAYPIPE W/SO 2.5AGZ X 1.5NH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"AGZ","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N/A","No 2021 Sales","No 2021 Sales","2390",1.5,"NH",null,null,"2390 2.5 in AGZ 1.5 in NH  ","23904008","PLAYPIPE W/SO 2.5AGZ X 1.5NH",27]
["23904009","PLAYPIPE W/SO 2.5JIM X 1.5NH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"JIM","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N/A","No 2021 Sales","No 2021 Sales","2390",1.5,"NH",null,null,"2390 2.5 in JIM 1.5 in NH  ","23904009","PLAYPIPE W/SO 2.5JIM X 1.5NH",27]
["23904011","PLAYPIPE W/SO 2.5AFY X 1.5NH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"PITT6","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N/A","No 2021 Sales","No 2021 Sales","2390",1.5,"NH",null,null,"2390 2.5 in PITT6 1.5 in NH  ","23904011","PLAYPIPE W/SO 2.5AFY X 1.5NH",29]
["23904014","PLAYPIPE W/SO 2.5BSP X 1.5NH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"BSP","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N/A","No 2021 Sales","No 2021 Sales","2390",1.5,"NH",null,null,"2390 2.5 in BSP 1.5 in NH  ","23904014","PLAYPIPE W/SO 2.5BSP X 1.5NH",27]
["23904015","PLAYPIPE W/SO 2.5BSP X 1.5BSP",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"BSP","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N/A","No 2021 Sales","No 2021 Sales","2390",1.5,"BSP",null,null,"2390 2.5 in BSP 1.5 in BSP  ","23904015","PLAYPIPE W/SO 2.5BSP X 1.5BSP",28]
["23904017","PLAYPIPE W/SO 2.5AIJ X 1.5NPSH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"AIJ","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N/A","No 2021 Sales","No 2021 Sales","2390",1.5,"NPSH",null,null,"2390 2.5 in AIJ 1.5 in NPSH  ","23904017","PLAYPIPE W/SO 2.5AIJ X 1.5NPSH",29]
["23904018","PLAYPIPE W/SO 2.5NH X 1.5NPSH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N/A","No 2021 Sales","No 2021 Sales","2390",1.5,"NPSH",null,null,"2390 2.5 in NH 1.5 in NPSH  ","23904018","PLAYPIPE W/SO 2.5NH X 1.5NPSH",28]
["23904022","PLAYPIPE W/SO 2.5AEA X 1.5NH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"AEA","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N/A","No 2021 Sales","No 2021 Sales","2390",1.5,"NH",null,null,"2390 2.5 in AEA 1.5 in NH  ","23904022","PLAYPIPE W/SO 2.5AEA X 1.5NH",27]
["23904024","PLAYPIPE W/SO 2.5BAF X 1.5NH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"BAT","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N/A","No 2021 Sales","No 2021 Sales","2390",1.5,"NH",null,null,"2390 2.5 in BAT 1.5 in NH  ","23904024","PLAYPIPE W/SO 2.5BAF X 1.5NH",27]
["23904027","PLAYPIPE W/SO 2.5AEF X 1.5NH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NYCORP","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N/A","No 2021 Sales","No 2021 Sales","2390",1.5,"NH",null,null,"2390 2.5 in NYCORP 1.5 in NH  ","23904027","PLAYPIPE W/SO 2.5AEF X 1.5NH",30]
["23904025","PLAYPIPE W/SO 2.5AHQ X 1.5NH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"AHQ","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N/A","No 2021 Sales","No 2021 Sales","2390",1.5,"NPSH",null,null,{"$f":"CONCATENATE(AC764,\" \",N764,\" in \",O764,\" \",IF(AD764=\"n/a\",\"\",CONCATENATE(AD764,\" in \",AE764,\" \")),IF(Q764=\"n/a\",\"\",Q764),IF(S764=\"n/a\",\"\",CONCATENATE(IF(X764=\"saber\",\" \",\"\"),S764,\" bore size(s) \")),IF(T764=\"n/a\",\"\",CONCATENATE(IF(X764=\"saber\",\"\",\" \"),T764,IF(T764=100,\" (Std) \",IF(T764=87,\" (CE) \",\" \")))),IF(U764=\"n/a\",\"\",CONCATENATE(U764,IF(U764=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X764,3)=\"tip\",IF(LEFT(X764,1)=\"s\",\"\",IF(Z764=\"n\",IF(T764=\"N/A\",\"PG\",\" PG\"),IF(Z764=\"y\",IF(T764=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z764=\"n\",IF(T764=\"N/A\",\"PG\",\" PG\"),IF(Z764=\"y\",IF(T764=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF764=\"y\",\" ZT\",\"\"),IF(V764=\"N\",\"\",IF(S764=\"n/a\",\" ETCH\",IF(T764=\"N/A\",IF(RIGHT(X764,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X764=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"2390 2.5 in AHQ 1.5 in NPSH  "},{"$f":"A764","v":"23904025"},{"$f":"B764","v":"PLAYPIPE W/SO 2.5AHQ X 1.5NH"},{"$f":"LEN(AH764)","v":29}]
["23904029","PLAYPIPE W/SO 2.5AEH X 1.5NPSH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"AEH","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N/A","No 2021 Sales","No 2021 Sales","2390",1.5,"NPSH",null,null,"2390 2.5 in AEH 1.5 in NPSH  ","23904029","PLAYPIPE W/SO 2.5AEH X 1.5NPSH",29]
["23904031","PLAYPIPE W/SO 2.5AFO X 1.5NH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"AFO","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N/A","No 2021 Sales","No 2021 Sales","2390",1.5,"NPSH",null,null,"2390 2.5 in AFO 1.5 in NPSH  ","23904031","PLAYPIPE W/SO 2.5AFO X 1.5NH",29]
["23904030","PLAYPIPE W/SO 2.5AKA X 1.5NPSH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"AKA","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N/A","No 2021 Sales","No 2021 Sales","2390",1.5,"NPSH",null,null,"2390 2.5 in AKA 1.5 in NPSH  ","23904030","PLAYPIPE W/SO 2.5AKA X 1.5NPSH",29]
["23934001","PP W/STK TIPS 2.5NH X 1.5NH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","1-1/4\"; 1-1/8\"; 1\"","n/a","N/A","N","ENGLISH","Breakapart Stack Tip","High-Range","N/A",80,1,"2393",1.5,"NH",null,null,"2393 2.5 in NH 1.5 in NH 1-1/4\"; 1-1/8\"; 1\" bore size(s)  ","23934001","PP W/STK TIPS 2.5NH X 1.5NH",58]
["23934008","PP W/STK TIPS 2.5NH X 1.5NPSH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","1-1/4\"; 1-1/8\"; 1\"","n/a","N/A","N","ENGLISH","Breakapart Stack Tip","High-Range","N/A",20,2,"2393",1.5,"NPSH",null,null,"2393 2.5 in NH 1.5 in NPSH 1-1/4\"; 1-1/8\"; 1\" bore size(s)  ","23934008","PP W/STK TIPS 2.5NH X 1.5NPSH",60]
["23934011","PP W/STK TIPS 2.5AJD X 1.5NH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","1-1/4\"; 1-1/8\"; 1\"","N/A","N/A","N","ENGLISH","Breakapart Stack Tip","High-Range","N/A",20,2,"2393",1.5,"NH",null,null,"2393 2.5 in NH 1.5 in NH 1-1/4\"; 1-1/8\"; 1\" bore size(s)  ","23934011","PP W/STK TIPS 2.5AJD X 1.5NH",58]
["23904028","PLAYPIPE W/SO 2.5AHU X 1.5NH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"AHU","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N/A",20,3,"2393",1.5,"NH",null,null,"2393 2.5 in AHU 1.5 in NH  ","23904028","PLAYPIPE W/SO 2.5AHU X 1.5NH",27]
["23934010","PP W/STK TIPS 2.5AEA X 1.5NH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"AEA","N/A","N/A","N/A","1-1/4\"; 1-1/8\"; 1\"","n/a","N/A","N","ENGLISH","Breakapart Stack Tip","High-Range","N/A",20,3,"2393",1.5,"NH",null,null,"2393 2.5 in AEA 1.5 in NH 1-1/4\"; 1-1/8\"; 1\" bore size(s)  ","23934010","PP W/STK TIPS 2.5AEA X 1.5NH",59]
["23934002","PP W/STK TIPS 2.5AKB X 1.5NPSH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"AKB","N/A","N/A","N/A","1-1/4\"; 1-1/8\"; 1\"","n/a","N/A","N","ENGLISH","Breakapart Stack Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","2393",1.5,"NPSH",null,null,"2393 2.5 in AKB 1.5 in NPSH 1-1/4\"; 1-1/8\"; 1\" bore size(s)  ","23934002","PP W/STK TIPS 2.5AKB X 1.5NPSH",61]
["23934012","PP W/STK TIPS 2.5AEH X 1.5NPSH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"AEH","N/A","N/A","N/A","1-1/4\"; 1-1/8\"; 1\"","n/a","N/A","N","ENGLISH","Breakapart Stack Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","2393",1.5,"NPSH",null,null,{"$f":"CONCATENATE(AC774,\" \",N774,\" in \",O774,\" \",IF(AD774=\"n/a\",\"\",CONCATENATE(AD774,\" in \",AE774,\" \")),IF(Q774=\"n/a\",\"\",Q774),IF(S774=\"n/a\",\"\",CONCATENATE(IF(X774=\"saber\",\" \",\"\"),S774,\" bore size(s) \")),IF(T774=\"n/a\",\"\",CONCATENATE(IF(X774=\"saber\",\"\",\" \"),T774,IF(T774=100,\" (Std) \",IF(T774=87,\" (CE) \",\" \")))),IF(U774=\"n/a\",\"\",CONCATENATE(U774,IF(U774=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X774,3)=\"tip\",IF(LEFT(X774,1)=\"s\",\"\",IF(Z774=\"n\",IF(T774=\"N/A\",\"PG\",\" PG\"),IF(Z774=\"y\",IF(T774=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z774=\"n\",IF(T774=\"N/A\",\"PG\",\" PG\"),IF(Z774=\"y\",IF(T774=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF774=\"y\",\" ZT\",\"\"),IF(V774=\"N\",\"\",IF(S774=\"n/a\",\" ETCH\",IF(T774=\"N/A\",IF(RIGHT(X774,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X774=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"2393 2.5 in AEH 1.5 in NPSH 1-1/4\"; 1-1/8\"; 1\" bore size(s)  "},{"$f":"A774","v":"23934012"},{"$f":"B774","v":"PP W/STK TIPS 2.5AEH X 1.5NPSH"},{"$f":"LEN(AH774)","v":61}]
["23934014","PP W/STK TIPS 2.5AFD X 1.5NPSH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"QST","N/A","N/A","N/A","1-1/4\"; 1-1/8\"; 1\"","n/a","N/A","N","ENGLISH","Breakapart Stack Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","2393",1.5,"NPSH",null,null,"2393 2.5 in QST 1.5 in NPSH 1-1/4\"; 1-1/8\"; 1\" bore size(s)  ","23934014","PP W/STK TIPS 2.5AFD X 1.5NPSH",61]
["23934004","PP W/STK TIPS 2.5AFY X 1.5NH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"PITT6","N/A","N/A","N/A","1-1/4\"; 1-1/8\"; 1\"","n/a","N/A","N","ENGLISH","Breakapart Stack Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","2393",1.5,"NH",null,null,"2393 2.5 in PITT6 1.5 in NH 1-1/4\"; 1-1/8\"; 1\" bore size(s)  ","23934004","PP W/STK TIPS 2.5AFY X 1.5NH",61]
["23934006","PP W/STK TIPS 2.5AHB X 1.5NH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"AHB","N/A","N/A","N/A","1-1/4\"; 1-1/8\"; 1\"","n/a","N/A","N","ENGLISH","Breakapart Stack Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","2393",1.5,"NH",null,null,"2393 2.5 in AHB 1.5 in NH 1-1/4\"; 1-1/8\"; 1\" bore size(s)  ","23934006","PP W/STK TIPS 2.5AHB X 1.5NH",59]
["23934007","PP W/STK TIPS 2.5BAF X 1.5NPSH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"BAT","N/A","N/A","N/A","1-1/4\"; 1-1/8\"; 1\"","n/a","N/A","N","ENGLISH","Breakapart Stack Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","2393",1.5,"NPSH",null,null,"2393 2.5 in BAT 1.5 in NPSH 1-1/4\"; 1-1/8\"; 1\" bore size(s)  ","23934007","PP W/STK TIPS 2.5BAF X 1.5NPSH",61]
["23934013","PP W/STK TIPS 2.5AKA X 1.5NPSH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"AKA","N/A","N/A","N/A","1-1/4\"; 1-1/8\"; 1\"","n/a","N/A","N","ENGLISH","Breakapart Stack Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","2393",1.5,"NPSH",null,null,"2393 2.5 in AKA 1.5 in NPSH 1-1/4\"; 1-1/8\"; 1\" bore size(s)  ","23934013","PP W/STK TIPS 2.5AKA X 1.5NPSH",61]
["24314001","SBR TIP SO 1.5NH X 1.5NH 15/16D#",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","15/16\"","n/a","N/A","N","ENGLISH","Shutoff","1.5\"","N",80,1,"2431",1.5,"NH",null,null,"2431 1.5 in NH 1.5 in NH 15/16\" bore size(s) PG","24314001","SBR TIP SO 1.5NH X 1.5NH 15/16D#",47]
["24317017","SBR TIP SO NPG 1.5NHX1.5NH 7/8D D.C.F.D.",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","7/8\"","N/A","N/A","Y","ENGLISH","Shutoff","1.5\"","Y",80,1,"2431",1.5,"NH",null,null,"2431 1.5 in NH 1.5 in NH 7/8\" bore size(s) NPG ETCH","24317017","SBR TIP SO NPG 1.5NHX1.5NH 7/8D D.C.F.D.",51]
["24314003","SBR TIP SO 1.5NH X 1.5NH 7/8D",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","7/8\"","n/a","N/A","N","ENGLISH","Shutoff","1.5\"","N",20,1,"2431",1.5,"NH",null,null,"2431 1.5 in NH 1.5 in NH 7/8\" bore size(s) PG","24314003","SBR TIP SO 1.5NH X 1.5NH 7/8D",45]
["24317001","SBR TIP SO NPG 1.5NH X 1.5NH 15/16D",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","15/16\"","n/a","N/A","N","ENGLISH","Shutoff","1.5\"","Y",20,1,"2431",1.5,"NH",null,null,"2431 1.5 in NH 1.5 in NH 15/16\" bore size(s) NPG","24317001","SBR TIP SO NPG 1.5NH X 1.5NH 15/16D",48]
["24317003","SBR TIP SO NPG 1.5NH X 1.5NH 7/8D",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","7/8\"","n/a","N/A","N","ENGLISH","Shutoff","1.5\"","Y",20,1,"2431",1.5,"NH",null,null,"2431 1.5 in NH 1.5 in NH 7/8\" bore size(s) NPG","24317003","SBR TIP SO NPG 1.5NH X 1.5NH 7/8D",46]
["24314002","SBR TIP SO 1.5NH X 1.5NH 1D",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","1\"","n/a","N/A","N","ENGLISH","Shutoff","1.5\"","N",20,2,"2431",1.5,"NH",null,null,"2431 1.5 in NH 1.5 in NH 1\" bore size(s) PG","24314002","SBR TIP SO 1.5NH X 1.5NH 1D",43]
["24314009","SBR TIP SO 1.5NH X 1.5NH 1-1/8D",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","1-1/8\"","n/a","N/A","N","ENGLISH","Shutoff","1.5\"","N",20,2,"2431",1.5,"NH",null,null,"2431 1.5 in NH 1.5 in NH 1-1/8\" bore size(s) PG","24314009","SBR TIP SO 1.5NH X 1.5NH 1-1/8D",47]
["24317002","SBR TIP SO NPG 1.5NH X 1.5NH 1D",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","1\"","n/a","N/A","N","ENGLISH","Shutoff","1.5\"","Y",20,2,"2431",1.5,"NH",null,null,"2431 1.5 in NH 1.5 in NH 1\" bore size(s) NPG","24317002","SBR TIP SO NPG 1.5NH X 1.5NH 1D",44]
["24317010","SBR TIP SO NPG 1.5NH X 1.5NH 15/16 BDVFD",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","15/16\"","N/A","N/A","Y","ENGLISH","Shutoff","1.5\"","Y",20,2,"2431",1.5,"NH",null,null,"2431 1.5 in NH 1.5 in NH 15/16\" bore size(s) NPG ETCH","24317010","SBR TIP SO NPG 1.5NH X 1.5NH 15/16 BDVFD",53]
["24314005","SBR TIP SO 1.5NPSH X 1.5NPSH 1D",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NPSH","N/A","N/A","N/A","1\"","n/a","N/A","N","ENGLISH","Shutoff","1.5\"","N",20,3,"2431",1.5,"NPSH",null,null,"2431 1.5 in NPSH 1.5 in NPSH 1\" bore size(s) PG","24314005","SBR TIP SO 1.5NPSH X 1.5NPSH 1D",47]
["24314013","SBR TIP SO 1.5NPSH X 1.5NPSH 1-1/4D",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NPSH","N/A","N/A","N/A","1-1/4\"","n/a","N/A","N","ENGLISH","Shutoff","1.5\"","N",20,3,"2431",1.5,"NPSH",null,null,"2431 1.5 in NPSH 1.5 in NPSH 1-1/4\" bore size(s) PG","24314013","SBR TIP SO 1.5NPSH X 1.5NPSH 1-1/4D",51]
["24314016","SBR TIP SO 1.5NPSH X 1.5NPSH 7/8D",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NPSH","N/A","N/A","N/A","7/8\"","n/a","N/A","N","ENGLISH","Shutoff","1.5\"","N",20,3,"2431",1.5,"NPSH",null,null,"2431 1.5 in NPSH 1.5 in NPSH 7/8\" bore size(s) PG","24314016","SBR TIP SO 1.5NPSH X 1.5NPSH 7/8D",49]
["24314032","SBR TIP SO 1.5NH X 1.5NH 1-1/4D",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","1-1/4\"","n/a","N/A","N","ENGLISH","Shutoff","1.5\"","N",20,3,"2431",1.5,"NH",null,null,"2431 1.5 in NH 1.5 in NH 1-1/4\" bore size(s) PG","24314032","SBR TIP SO 1.5NH X 1.5NH 1-1/4D",47]
["24314034","SBR TIP SO 1.5NHX1.5NH 15/16D COPLE VFD",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","15/16\"","N/A","N/A","Y","ENGLISH","Shutoff","1.5\"","N/A",20,3,"2431",1.5,"NH",null,null,"2431 1.5 in NH 1.5 in NH 15/16\" bore size(s)   ETCH","24314034","SBR TIP SO 1.5NHX1.5NH 15/16D COPLE VFD",51]
["24317004","SBR TIP SO NPG 1.5NPSH X 1.5NPSH 15/16D",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NPSH","N/A","N/A","N/A","15/16\"","N/A","N/A","N","ENGLISH","Shutoff","1.5\"","Y",20,3,"2431",1.5,"NPSH",null,null,"2431 1.5 in NPSH 1.5 in NPSH 15/16\" bore size(s) NPG","24317004","SBR TIP SO NPG 1.5NPSH X 1.5NPSH 15/16D",52]
["24317009","SBR TIP SO NPG 1.5NH X 1.5NH 1-1/8D",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","1-1/8\"","n/a","N/A","N","ENGLISH","Shutoff","1.5\"","Y",20,3,"2431",1.5,"NH",null,null,"2431 1.5 in NH 1.5 in NH 1-1/8\" bore size(s) NPG","24317009","SBR TIP SO NPG 1.5NH X 1.5NH 1-1/8D",48]
["24314004","SBR TIP SO 1.5NPSH X 1.5NPSH 15/16D",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NPSH","N/A","N/A","N/A","15/16\"","n/a","N/A","N","ENGLISH","Shutoff","1.5\"","N","No 2021 Sales","No 2021 Sales","2431",1.5,"NPSH",null,null,"2431 1.5 in NPSH 1.5 in NPSH 15/16\" bore size(s) PG","24314004","SBR TIP SO 1.5NPSH X 1.5NPSH 15/16D",51]
["24314033","SBR TIP SO 1.5NPSH X 1.5NPSH 1-1/8D",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NPSH","N/A","N/A","N/A","1-1/8\"","n/a","N/A","N","ENGLISH","Shutoff","1.5\"","N","No 2021 Sales","No 2021 Sales","2431",1.5,"NPSH",null,null,"2431 1.5 in NPSH 1.5 in NPSH 1-1/8\" bore size(s) PG","24314033","SBR TIP SO 1.5NPSH X 1.5NPSH 1-1/8D",51]
["24314036","SBR TIP SO 1.5NH X 1.5NH 1-1/16D",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","1-1/16\"","n/a","N/A","N","ENGLISH","Shutoff","1.5\"","N","No 2021 Sales","No 2021 Sales","2431",1.5,"NH",null,null,"2431 1.5 in NH 1.5 in NH 1-1/16\" bore size(s) PG","24314036","SBR TIP SO 1.5NH X 1.5NH 1-1/16D",48]
["24314037","SBR TIP SO 1.5NPSH X 1.5NPSH 1-1/16D",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NPSH","N/A","N/A","N/A","1-1/16\"","n/a","N/A","N","ENGLISH","Shutoff","1.5\"","N","No 2021 Sales","No 2021 Sales","2431",1.5,"NPSH",null,null,"2431 1.5 in NPSH 1.5 in NPSH 1-1/16\" bore size(s) PG","24314037","SBR TIP SO 1.5NPSH X 1.5NPSH 1-1/16D",52]
["24314038","SBR TIP SO 1.5NH X 1.5NH 1-3/16D",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","1-3/16\"","n/a","N/A","N","ENGLISH","Shutoff","1.5\"","N","No 2021 Sales","No 2021 Sales","2431",1.5,"NH",null,null,"2431 1.5 in NH 1.5 in NH 1-3/16\" bore size(s) PG","24314038","SBR TIP SO 1.5NH X 1.5NH 1-3/16D",48]
["24314039","SBR TIP SO 1.5NPSH X 1.5NPSH 1-1/36D",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NPSH","N/A","N/A","N/A","1-3/16\"","n/a","N/A","N","ENGLISH","Shutoff","1.5\"","N","No 2021 Sales","No 2021 Sales","2431",1.5,"NPSH",null,null,"2431 1.5 in NPSH 1.5 in NPSH 1-3/16\" bore size(s) PG","24314039","SBR TIP SO 1.5NPSH X 1.5NPSH 1-1/36D",52]
["24317006","SBRTIP SO NPG 1.5NHX1.5NH 7/8D MTLHDL",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","7/8\"","n/a","N/A","N","ENGLISH","Shutoff","1.5\"","Y","No 2021 Sales","No 2021 Sales","2431",1.5,"NH",null,null,"2431 1.5 in NH 1.5 in NH 7/8\" bore size(s) NPG","24317006","SBRTIP SO NPG 1.5NHX1.5NH 7/8D MTLHDL",46]
["24334002","SBR TIP SO 2.5NHX1.5NH 1-1/8D",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","1-1/8\"","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N",20,1,"2433",1.5,"NH",null,null,"2433 2.5 in NH 1.5 in NH 1-1/8\" bore size(s) PG","24334002","SBR TIP SO 2.5NHX1.5NH 1-1/8D",47]
["24334028","SBR TIP SO 2.5NHX1.5NH 1D",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","1\"","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N",20,1,"2433",1.5,"NH",null,null,{"$f":"CONCATENATE(AC804,\" \",N804,\" in \",O804,\" \",IF(AD804=\"n/a\",\"\",CONCATENATE(AD804,\" in \",AE804,\" \")),IF(Q804=\"n/a\",\"\",Q804),IF(S804=\"n/a\",\"\",CONCATENATE(IF(X804=\"saber\",\" \",\"\"),S804,\" bore size(s) \")),IF(T804=\"n/a\",\"\",CONCATENATE(IF(X804=\"saber\",\"\",\" \"),T804,IF(T804=100,\" (Std) \",IF(T804=87,\" (CE) \",\" \")))),IF(U804=\"n/a\",\"\",CONCATENATE(U804,IF(U804=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X804,3)=\"tip\",IF(LEFT(X804,1)=\"s\",\"\",IF(Z804=\"n\",IF(T804=\"N/A\",\"PG\",\" PG\"),IF(Z804=\"y\",IF(T804=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z804=\"n\",IF(T804=\"N/A\",\"PG\",\" PG\"),IF(Z804=\"y\",IF(T804=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF804=\"y\",\" ZT\",\"\"),IF(V804=\"N\",\"\",IF(S804=\"n/a\",\" ETCH\",IF(T804=\"N/A\",IF(RIGHT(X804,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X804=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"2433 2.5 in NH 1.5 in NH 1\" bore size(s) PG"},{"$f":"A804","v":"24334028"},{"$f":"B804","v":"SBR TIP SO 2.5NHX1.5NH 1D"},{"$f":"LEN(AH804)","v":43}]
["24334001","SBR TIP SO 2.5NHX1.5NH 1-1/4D",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","1-1/4\"","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N",20,2,"2433",1.5,"NH",null,null,"2433 2.5 in NH 1.5 in NH 1-1/4\" bore size(s) PG","24334001","SBR TIP SO 2.5NHX1.5NH 1-1/4D",47]
["24334017","SBR TIP SO 2.5AUC X 1.5NH 1-1/8D",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"AUC","N/A","N/A","N/A","1-1/8\"","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N",20,2,"2433",1.5,"NH",null,null,"2433 2.5 in AUC 1.5 in NH 1-1/8\" bore size(s) PG","24334017","SBR TIP SO 2.5AUC X 1.5NH 1-1/8D",48]
["24337002","SBR TIP SO NPG 2.5NHX1.5NH 1-1/8D",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","1-1/8\"","n/a","N/A","N","ENGLISH","Shutoff","High-Range","Y",20,2,"2433",1.5,"NH",null,null,"2433 2.5 in NH 1.5 in NH 1-1/8\" bore size(s) NPG","24337002","SBR TIP SO NPG 2.5NHX1.5NH 1-1/8D",48]
["24334010","SBR TIP SO 2.5AEF X 1.5NH 1-1/8D",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NYCORP","N/A","N/A","N/A","1-1/8\"","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N",20,3,"2433",1.5,"NH",null,null,"2433 2.5 in NYCORP 1.5 in NH 1-1/8\" bore size(s) PG","24334010","SBR TIP SO 2.5AEF X 1.5NH 1-1/8D",51]
["24334021","SBR TIP SO 2.5BAF X1.5NPSH 1-1/8D",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"BAT","N/A","N/A","N/A","1-1/8\"","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N",20,3,"2433",1.5,"NPSH",null,null,"2433 2.5 in BAT 1.5 in NPSH 1-1/8\" bore size(s) PG","24334021","SBR TIP SO 2.5BAF X1.5NPSH 1-1/8D",50]
["24334022","SBR TIP SO 2.5AHB X 1.5NH 1-1/8D",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","1-1/8\"","N/A","N/A","N","ENGLISH","Shutoff","High-Range","N/A",20,3,"2433",1.5,"NH",null,null,{"$f":"CONCATENATE(AC810,\" \",N810,\" in \",O810,\" \",IF(AD810=\"n/a\",\"\",CONCATENATE(AD810,\" in \",AE810,\" \")),IF(Q810=\"n/a\",\"\",Q810),IF(S810=\"n/a\",\"\",CONCATENATE(IF(X810=\"saber\",\" \",\"\"),S810,\" bore size(s) \")),IF(T810=\"n/a\",\"\",CONCATENATE(IF(X810=\"saber\",\"\",\" \"),T810,IF(T810=100,\" (Std) \",IF(T810=87,\" (CE) \",\" \")))),IF(U810=\"n/a\",\"\",CONCATENATE(U810,IF(U810=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X810,3)=\"tip\",IF(LEFT(X810,1)=\"s\",\"\",IF(Z810=\"n\",IF(T810=\"N/A\",\"PG\",\" PG\"),IF(Z810=\"y\",IF(T810=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z810=\"n\",IF(T810=\"N/A\",\"PG\",\" PG\"),IF(Z810=\"y\",IF(T810=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF810=\"y\",\" ZT\",\"\"),IF(V810=\"N\",\"\",IF(S810=\"n/a\",\" ETCH\",IF(T810=\"N/A\",IF(RIGHT(X810,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X810=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"2433 2.5 in NH 1.5 in NH 1-1/8\" bore size(s)  "},{"$f":"A810","v":"24334022"},{"$f":"B810","v":"SBR TIP SO 2.5AHB X 1.5NH 1-1/8D"},{"$f":"LEN(AH810)","v":46}]
["24337001","SBR TIP SO NPG 2.5NHX1.5NH 1-1/4D",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","1-1/4\"","n/a","N/A","N","ENGLISH","Shutoff","High-Range","Y",20,3,"2433",1.5,"NH",null,null,"2433 2.5 in NH 1.5 in NH 1-1/4\" bore size(s) NPG","24337001","SBR TIP SO NPG 2.5NHX1.5NH 1-1/4D",48]
["24334003","SBR TIP SO 2.5NH X 1.5NH 15/16D",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","15/16\"","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2433",1.5,"NH",null,null,"2433 2.5 in NH 1.5 in NH 15/16\" bore size(s) PG","24334003","SBR TIP SO 2.5NH X 1.5NH 15/16D",47]
["24334007","SBR TIP SO 2.5NHX1.5NPSH 1-1/8D",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","1-1/8\"","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2433",1.5,"NPSH",null,null,"2433 2.5 in NH 1.5 in NPSH 1-1/8\" bore size(s) PG","24334007","SBR TIP SO 2.5NHX1.5NPSH 1-1/8D",49]
["24334008","SBR TIP SO 2.5AFYX1.5NH 1-1/8D",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"PITT6","N/A","N/A","N/A","1-1/8\"","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2433",1.5,"NH",null,null,"2433 2.5 in PITT6 1.5 in NH 1-1/8\" bore size(s) PG","24334008","SBR TIP SO 2.5AFYX1.5NH 1-1/8D",50]
["24334013","SBR TIP SO 2.5AHC X 1.5NH 1-1/8D",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"AHC","N/A","N/A","N/A","1-1/8\"","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2433",1.5,"NH",null,null,"2433 2.5 in AHC 1.5 in NH 1-1/8\" bore size(s) PG","24334013","SBR TIP SO 2.5AHC X 1.5NH 1-1/8D",48]
["24334016","SBR TIP SO 2.5NHX1.5NH 7/8D",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","7/8\"","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2433",1.5,"NH",null,null,"2433 2.5 in NH 1.5 in NH 7/8\" bore size(s) PG","24334016","SBR TIP SO 2.5NHX1.5NH 7/8D",45]
["24334027","SBR TIP SO 2.5AKBX1.5NPSH 1-1/8D",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"AKB","N/A","N/A","N/A","1-1/8\"","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2433",1.5,"NPSH",null,null,"2433 2.5 in AKB 1.5 in NPSH 1-1/8\" bore size(s) PG","24334027","SBR TIP SO 2.5AKBX1.5NPSH 1-1/8D",50]
["24337003","SBR TIP SO NPG 2.5BAF X1.5NPSH 1-1/8D",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"BAT","N/A","N/A","N/A","1-1/8\"","n/a","N/A","N","ENGLISH","Shutoff","High-Range","Y","No 2021 Sales","No 2021 Sales","2433",1.5,"NPSH",null,null,"2433 2.5 in BAT 1.5 in NPSH 1-1/8\" bore size(s) NPG","24337003","SBR TIP SO NPG 2.5BAF X1.5NPSH 1-1/8D",51]
["24337007","SBR TIP SO NPG 2.5NHX1.5NPSH 1-1/8D",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","1-1/8\"","n/a","N/A","N","ENGLISH","Shutoff","High-Range","Y","No 2021 Sales","No 2021 Sales","2433",1.5,"NPSH",null,null,"2433 2.5 in NH 1.5 in NPSH 1-1/8\" bore size(s) NPG","24337007","SBR TIP SO NPG 2.5NHX1.5NPSH 1-1/8D",50]
["24334023","SBR TIP SO 2.5NHX1.5NH 1-1/16D",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","1-1/16\"","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2433",1.5,"NH",null,null,"2433 2.5 in NH 1.5 in NH 1-1/16\" bore size(s) PG","24334023","SBR TIP SO 2.5NHX1.5NH 1-1/16D",48]
["24334024","SBR TIP SO 2.5NHX1.5NPSH 1-1/16D",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","1-1/16\"","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2433",1.5,"NPSH",null,null,"2433 2.5 in NH 1.5 in NPSH 1-1/16\" bore size(s) PG","24334024","SBR TIP SO 2.5NHX1.5NPSH 1-1/16D",50]
["24334025","SBR TIP SO 2.5NHX1.5NH 1-3/16D",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","1-3/16\"","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2433",1.5,"NH",null,null,"2433 2.5 in NH 1.5 in NH 1-3/16\" bore size(s) PG","24334025","SBR TIP SO 2.5NHX1.5NH 1-3/16D",48]
["24334026","SBR TIP SO 2.5NHX1.5NPSH 1-3/16D",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","1-3/16\"","n/a","N/A","N","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2433",1.5,"NPSH",null,null,"2433 2.5 in NH 1.5 in NPSH 1-3/16\" bore size(s) PG","24334026","SBR TIP SO 2.5NHX1.5NPSH 1-3/16D",50]
["04164001","TIP 1.5NH X 1.5NH 1-1/4D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","1-1/4\"","n/a","N/A","N","ENGLISH","SB Tip","1.5\"","N/A",20,2,"0416",1.5,"NH",null,null,"0416 1.5 in NH 1.5 in NH 1-1/4\" bore size(s) ","04164001","TIP 1.5NH X 1.5NH 1-1/4D",45]
["04164013","TIP 1.5BSP X 1.5BSP 1-1/4D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"BSP","N/A","N/A","N/A","1-1/4\"","n/a","N/A","N","ENGLISH","SB Tip","1.5\"","N/A",20,2,"0416",1.5,"BSP",null,null,{"$f":"CONCATENATE(AC825,\" \",N825,\" in \",O825,\" \",IF(AD825=\"n/a\",\"\",CONCATENATE(AD825,\" in \",AE825,\" \")),IF(Q825=\"n/a\",\"\",Q825),IF(S825=\"n/a\",\"\",CONCATENATE(IF(X825=\"saber\",\" \",\"\"),S825,\" bore size(s) \")),IF(T825=\"n/a\",\"\",CONCATENATE(IF(X825=\"saber\",\"\",\" \"),T825,IF(T825=100,\" (Std) \",IF(T825=87,\" (CE) \",\" \")))),IF(U825=\"n/a\",\"\",CONCATENATE(U825,IF(U825=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X825,3)=\"tip\",IF(LEFT(X825,1)=\"s\",\"\",IF(Z825=\"n\",IF(T825=\"N/A\",\"PG\",\" PG\"),IF(Z825=\"y\",IF(T825=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z825=\"n\",IF(T825=\"N/A\",\"PG\",\" PG\"),IF(Z825=\"y\",IF(T825=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF825=\"y\",\" ZT\",\"\"),IF(V825=\"N\",\"\",IF(S825=\"n/a\",\" ETCH\",IF(T825=\"N/A\",IF(RIGHT(X825,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X825=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"0416 1.5 in BSP 1.5 in BSP 1-1/4\" bore size(s) "},{"$f":"A825","v":"04164013"},{"$f":"B825","v":"TIP 1.5BSP X 1.5BSP 1-1/4D"},{"$f":"LEN(AH825)","v":47}]
["04164002","TIP 1.5NH X 1.5NH 1-1/8D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","1-1/8\"","n/a","N/A","N","ENGLISH","SB Tip","1.5\"","N/A",20,3,"0416",1.5,"NH",null,null,"0416 1.5 in NH 1.5 in NH 1-1/8\" bore size(s) ","04164002","TIP 1.5NH X 1.5NH 1-1/8D",45]
["04164004","TIP 1.5NH X 1.5NH 7/8D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","7/8\"","n/a","N/A","N","ENGLISH","SB Tip","1.5\"","N/A",20,3,"0416",1.5,"NH",null,null,"0416 1.5 in NH 1.5 in NH 7/8\" bore size(s) ","04164004","TIP 1.5NH X 1.5NH 7/8D",43]
["04164007","TIP 1.5ABE X 1.5ABE 1-1/4D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"ABE","N/A","N/A","N/A","1-1/4\"","n/a","N/A","N","ENGLISH","SB Tip","1.5\"","N/A",20,3,"0416",1.5,"ABE",null,null,"0416 1.5 in ABE 1.5 in ABE 1-1/4\" bore size(s) ","04164007","TIP 1.5ABE X 1.5ABE 1-1/4D",47]
["04160036","TIP 1.5 ABE X 1.5 ABE 1 1/4 DSCH PY",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"ABE","N/A","N/A","N/A","1-1/4\"","n/a","N/A","N","ENGLISH","SB Tip","1.5\"","N/A","No 2021 Sales","No 2021 Sales","0416",1.5,"ABE",null,null,"0416 1.5 in ABE 1.5 in ABE 1-1/4\" bore size(s) ","04160036","TIP 1.5 ABE X 1.5 ABE 1 1/4 DSCH PY",47]
["04160413","TIP 1.5BSP X 1.5BSP 1-1/4D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"BSP","N/A","N/A","N/A","1-1/4\"","n/a","N/A","N","ENGLISH","SB Tip","1.5\"","N/A","No 2021 Sales","No 2021 Sales","0416",1.5,"BSP",null,null,"0416 1.5 in BSP 1.5 in BSP 1-1/4\" bore size(s) ","04160413","TIP 1.5BSP X 1.5BSP 1-1/4D",47]
["04164003","TIP 1.5NH X 1.5NH 3/4D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","3/4\"","n/a","N/A","N","ENGLISH","SB Tip","1.5\"","N/A","No 2021 Sales","No 2021 Sales","0416",1.5,"NH",null,null,"0416 1.5 in NH 1.5 in NH 3/4\" bore size(s) ","04164003","TIP 1.5NH X 1.5NH 3/4D",43]
["04164005","TIP 1.5NSPH X 1.5NPSH 7/8D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NPSH","N/A","N/A","N/A","7/8\"","n/a","N/A","N","ENGLISH","SB Tip","1.5\"","N/A","No 2021 Sales","No 2021 Sales","0416",1.5,"NPSH",null,null,"0416 1.5 in NPSH 1.5 in NPSH 7/8\" bore size(s) ","04164005","TIP 1.5NSPH X 1.5NPSH 7/8D",47]
["04164006","TIP 1.5NH X 1.5NH 1D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","1\"","n/a","N/A","N","ENGLISH","SB Tip","1.5\"","N/A","No 2021 Sales","No 2021 Sales","0416",1.5,"NH",null,null,"0416 1.5 in NH 1.5 in NH 1\" bore size(s) ","04164006","TIP 1.5NH X 1.5NH 1D",41]
["04164008","TIP 1.5NPSH X 1.5NPSH 1-1/8D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NPSH","N/A","N/A","N/A","1-1/8\"","n/a","N/A","N","ENGLISH","SB Tip","1.5\"","N/A","No 2021 Sales","No 2021 Sales","0416",1.5,"NPSH",null,null,"0416 1.5 in NPSH 1.5 in NPSH 1-1/8\" bore size(s) ","04164008","TIP 1.5NPSH X 1.5NPSH 1-1/8D",49]
["04164009","TIP 1.5NH X 1.5ABE 1-1/4D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","1-1/4\"","n/a","N/A","N","ENGLISH","SB Tip","1.5\"","N/A","No 2021 Sales","No 2021 Sales","0416",1.5,"ABE",null,null,"0416 1.5 in NH 1.5 in ABE 1-1/4\" bore size(s) ","04164009","TIP 1.5NH X 1.5ABE 1-1/4D",46]
["04164010","TIP 1.5NPSH X 1.5NPSH 1D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NPSH","N/A","N/A","N/A","1\"","n/a","N/A","N","ENGLISH","SB Tip","1.5\"","N/A","No 2021 Sales","No 2021 Sales","0416",1.5,"NPSH",null,null,"0416 1.5 in NPSH 1.5 in NPSH 1\" bore size(s) ","04164010","TIP 1.5NPSH X 1.5NPSH 1D",45]
["04164011","TIP 1.5ABE X 1.5NH 1-1/4D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"ABE","N/A","N/A","N/A","1-1/4\"","n/a","N/A","N","ENGLISH","SB Tip","1.5\"","N/A","No 2021 Sales","No 2021 Sales","0416",1.5,"NH",null,null,"0416 1.5 in ABE 1.5 in NH 1-1/4\" bore size(s) ","04164011","TIP 1.5ABE X 1.5NH 1-1/4D",46]
["04164012","TIP 1.5BSP X 1.5BSP 1D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"BSP","N/A","N/A","N/A","1\"","n/a","N/A","N","ENGLISH","SB Tip","1.5\"","N/A","No 2021 Sales","No 2021 Sales","0416",1.5,"BSP",null,null,"0416 1.5 in BSP 1.5 in BSP 1\" bore size(s) ","04164012","TIP 1.5BSP X 1.5BSP 1D",43]
["04394005","TIP DUAL STK 1.5NH 15/16&1/2D#",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","15/16\"; 1/2\"","N/A","N/A","N","ENGLISH","Stack Tip","1.5\"","N/A",20,1,"0439",1,"NH",null,null,"0439 1.5 in NH 1 in NH 15/16\"; 1/2\" bore size(s) ","04394005","TIP DUAL STK 1.5NH 15/16&1/2D#",49]
["04394002","TIP DUAL STK 1.5NH 1-1/8&1/2D#",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","1-1/8\"; 1/2\"","N/A","N/A","N","ENGLISH","Stack Tip","1.5\"","N/A",20,2,"0439",1,"NH",null,null,"0439 1.5 in NH 1 in NH 1-1/8\"; 1/2\" bore size(s) ","04394002","TIP DUAL STK 1.5NH 1-1/8&1/2D#",49]
["04394006","TIP DUAL STK 1.5NH 1-1/16&15/16D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","1-1/16\"; 15/16\"","N/A","N/A","N","ENGLISH","Stack Tip","1.5\"","N/A",20,2,"0439",1,"NH",null,null,"0439 1.5 in NH 1 in NH 1-1/16\"; 15/16\" bore size(s) ","04394006","TIP DUAL STK 1.5NH 1-1/16&15/16D",52]
["04394001","TIP DUAL STK 1.5ABU FDNY 1/2&15/16D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"FDNY","N/A","N/A","N/A","15/16\"; 1/2\"","N/A","N/A","N","ENGLISH","Stack Tip","1.5\"","N/A","No 2021 Sales","No 2021 Sales","0439",1,"NH",null,null,"0439 1.5 in FDNY 1 in NH 15/16\"; 1/2\" bore size(s) ","04394001","TIP DUAL STK 1.5ABU FDNY 1/2&15/16D",51]
["04394003","TIP DUAL STK 1.5ABU FDNY 1-1/8&1/2D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"FDNY","N/A","N/A","N/A","1-1/8\"; 1/2\"","N/A","N/A","N","ENGLISH","Stack Tip","1.5\"","N/A","No 2021 Sales","No 2021 Sales","0439",1,"NH",null,null,"0439 1.5 in FDNY 1 in NH 1-1/8\"; 1/2\" bore size(s) ","04394003","TIP DUAL STK 1.5ABU FDNY 1-1/8&1/2D",51]
["04394004","TIP DUAL STK 1.5NPSH 1-1/8&1/2D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NPSH","N/A","N/A","N/A","1-1/8\"; 1/2\"","N/A","N/A","N","ENGLISH","Stack Tip","1.5\"","N/A","No 2021 Sales","No 2021 Sales","0439",1,"NH",null,null,"0439 1.5 in NPSH 1 in NH 1-1/8\"; 1/2\" bore size(s) ","04394004","TIP DUAL STK 1.5NPSH 1-1/8&1/2D",51]
["04394008","TIP DUAL STK 1.5NPSH 15/16&1/2D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NPSH","N/A","N/A","N/A","15/16\"; 1/2\"","N/A","N/A","N","ENGLISH","Stack Tip","1.5\"","N/A","No 2021 Sales","No 2021 Sales","0439",1,"NH",null,null,"0439 1.5 in NPSH 1 in NH 15/16\"; 1/2\" bore size(s) ","04394008","TIP DUAL STK 1.5NPSH 15/16&1/2D",51]
["04394010","TIP DUAL STK 1.5ABQ 15/16 &1/2D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NYCORP","N/A","N/A","N/A","15/16\"; 1/2\"","N/A","N/A","N","ENGLISH","Stack Tip","1.5\"","N/A","No 2021 Sales","No 2021 Sales","0439",1,"NH",null,null,"0439 1.5 in NYCORP 1 in NH 15/16\"; 1/2\" bore size(s) ","04394010","TIP DUAL STK 1.5ABQ 15/16 &1/2D",53]
["04890501","PLAIN DELUGE TIP 2.5NH 1 3/8D POLISH",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"NH","N/A","N/A","N/A","1-3/8\"","N/A","N/A","N","ENGLISH","SB Tip","High-Range","N/A",20,1,"0489","N/A","N/A",null,null,"0489 2.5 in NH 1-3/8\" bore size(s) ","04890501","PLAIN DELUGE TIP 2.5NH 1 3/8D POLISH",35]
["04890500","PLAIN DELUGE TIP 2.5NH 1 1/2D POLISH#",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"NH","N/A","N/A","N/A","1-1/2\"","N/A","N/A","N","ENGLISH","SB Tip","High-Range","N/A",20,2,"0489","N/A","N/A",null,null,"0489 2.5 in NH 1-1/2\" bore size(s) ","04890500","PLAIN DELUGE TIP 2.5NH 1 1/2D POLISH#",35]
["04890506","PLAIN DELUGE TIP 2.5NH 1 1/8D POLISH",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"NH","N/A","N/A","N/A","1-1/8\"","N/A","N/A","N","ENGLISH","SB Tip","High-Range","N/A",20,2,"0489","N/A","N/A",null,null,"0489 2.5 in NH 1-1/8\" bore size(s) ","04890506","PLAIN DELUGE TIP 2.5NH 1 1/8D POLISH",35]
["04890502","PLAIN DELUGE TIP 2.5NH 1 1/4DSCH POLISH",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"NH","N/A","N/A","N/A","1-1/4\"","N/A","N/A","N","ENGLISH","SB Tip","High-Range","N/A",20,3,"0489","N/A","N/A",null,null,"0489 2.5 in NH 1-1/4\" bore size(s) ","04890502","PLAIN DELUGE TIP 2.5NH 1 1/4DSCH POLISH",35]
["04890530","PLAIN DELUGE TIP 2.5AFD 1 3/8D POLISH",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"QST","N/A","N/A","N/A","1-3/8\"","N/A","N/A","N","ENGLISH","SB Tip","High-Range","N/A",20,3,"0489","N/A","N/A",null,null,"0489 2.5 in QST 1-3/8\" bore size(s) ","04890530","PLAIN DELUGE TIP 2.5AFD 1 3/8D POLISH",36]
["04890598","PLAIN DELUGE TIP 2.5BAF 1 3/8D POLISH",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"BAT","N/A","N/A","N/A","1-3/8\"","N/A","N/A","N","ENGLISH","SB Tip","High-Range","N/A",20,3,"0489","N/A","N/A",null,null,"0489 2.5 in BAT 1-3/8\" bore size(s) ","04890598","PLAIN DELUGE TIP 2.5BAF 1 3/8D POLISH",36]
["04890528","PLAIN DELUGE TIP 2.5AEF 2\"DSCH POLISH",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"NYCORP","N/A","N/A","N/A","2\"","N/A","N/A","N","ENGLISH","SB Tip","High-Range","N/A",20,4,"0489","N/A","N/A",null,null,"0489 2.5 in NYCORP 2\" bore size(s) ","04890528","PLAIN DELUGE TIP 2.5AEF 2\"DSCH POLISH",35]
["04890540","PLAIN DELUGE TIP 2.5AKB 1 1/2DSCH POLISH",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"AKB","N/A","N/A","N/A","1-1/2\"","N/A","N/A","N","ENGLISH","SB Tip","High-Range","N/A",20,4,"0489","N/A","N/A",null,null,"0489 2.5 in AKB 1-1/2\" bore size(s) ","04890540","PLAIN DELUGE TIP 2.5AKB 1 1/2DSCH POLISH",36]
["04890634","PLAIN DELUGE TIP 2.5 NH 15/16DSCH POLISH",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"NH","N/A","N/A","N/A","15/16\"","N/A","N/A","N","ENGLISH","SB Tip","High-Range","N/A",20,4,"0489","N/A","N/A",null,null,"0489 2.5 in NH 15/16\" bore size(s) ","04890634","PLAIN DELUGE TIP 2.5 NH 15/16DSCH POLISH",35]
["04890641","PLAIN DELUGE 5IP 2.5AEA1 3/8D POLISH",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"AEA","N/A","N/A","N/A","1-3/8\"","N/A","N/A","N","ENGLISH","SB Tip","High-Range","N/A",20,4,"0489","N/A","N/A",null,null,"0489 2.5 in AEA 1-3/8\" bore size(s) ","04890641","PLAIN DELUGE 5IP 2.5AEA1 3/8D POLISH",36]
["04890134","PLAIN DELUGE TIP 2.5NH W/1 1/2DSCH CF/NC",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"NH","N/A","N/A","N/A","1-1/2\"","N/A","N/A","N","ENGLISH","SB Tip","High-Range","N/A",20,4,"0489","N/A","N/A",null,null,{"$f":"CONCATENATE(AC857,\" \",N857,\" in \",O857,\" \",IF(AD857=\"n/a\",\"\",CONCATENATE(AD857,\" in \",AE857,\" \")),IF(Q857=\"n/a\",\"\",Q857),IF(S857=\"n/a\",\"\",CONCATENATE(IF(X857=\"saber\",\" \",\"\"),S857,\" bore size(s) \")),IF(T857=\"n/a\",\"\",CONCATENATE(IF(X857=\"saber\",\"\",\" \"),T857,IF(T857=100,\" (Std) \",IF(T857=87,\" (CE) \",\" \")))),IF(U857=\"n/a\",\"\",CONCATENATE(U857,IF(U857=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X857,3)=\"tip\",IF(LEFT(X857,1)=\"s\",\"\",IF(Z857=\"n\",IF(T857=\"N/A\",\"PG\",\" PG\"),IF(Z857=\"y\",IF(T857=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z857=\"n\",IF(T857=\"N/A\",\"PG\",\" PG\"),IF(Z857=\"y\",IF(T857=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF857=\"y\",\" ZT\",\"\"),IF(V857=\"N\",\"\",IF(S857=\"n/a\",\" ETCH\",IF(T857=\"N/A\",IF(RIGHT(X857,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X857=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"0489 2.5 in NH 1-1/2\" bore size(s) "},{"$f":"A857","v":"04890134"},{"$f":"B857","v":"PLAIN DELUGE TIP 2.5NH W/1 1/2DSCH CF/NC"},{"$f":"LEN(AH857)","v":35}]
["04890507","PLAIN DELUGE TIP 2.5AII 1 1/2DSCH POLISH",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"CSA","N/A","N/A","N/A","1-1/2\"","N/A","N/A","N","ENGLISH","SB Tip","High-Range","N/A",20,4,"0489","N/A","N/A",null,null,"0489 2.5 in CSA 1-1/2\" bore size(s) ","04890507","PLAIN DELUGE TIP 2.5AII 1 1/2DSCH POLISH",36]
["04890512","PLAIN DELUGE TIP 2.5AFB 1 1/4DFDNYPOLISH",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"FDNY","N/A","N/A","N/A","1-1/4\"","N/A","N/A","N","ENGLISH","SB Tip","High-Range","N/A",20,4,"0489","N/A","N/A",null,null,"0489 2.5 in FDNY 1-1/4\" bore size(s) ","04890512","PLAIN DELUGE TIP 2.5AFB 1 1/4DFDNYPOLISH",37]
["04890513","PLAIN DELUGE TIP 2.5AFB 1 1/2DFDNYPOLISH",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"FDNY","N/A","N/A","N/A","1-1/2\"","N/A","N/A","N","ENGLISH","SB Tip","High-Range","N/A",20,4,"0489","N/A","N/A",null,null,"0489 2.5 in FDNY 1-1/2\" bore size(s) ","04890513","PLAIN DELUGE TIP 2.5AFB 1 1/2DFDNYPOLISH",37]
["04890516","PLAIN DELUGE TIP 2.5BAF 1 1/2DSCH POLISH",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"BAT","N/A","N/A","N/A","1-1/2\"","N/A","N/A","N","ENGLISH","SB Tip","High-Range","N/A",20,4,"0489","N/A","N/A",null,null,"0489 2.5 in BAT 1-1/2\" bore size(s) ","04890516","PLAIN DELUGE TIP 2.5BAF 1 1/2DSCH POLISH",36]
["04890520","PLAIN DELUGE TIP 2.5AII 1 1/4DSCH POLISH",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"CSA","N/A","N/A","N/A","1-1/4\"","N/A","N/A","N","ENGLISH","SB Tip","High-Range","N/A",20,4,"0489","N/A","N/A",null,null,"0489 2.5 in CSA 1-1/4\" bore size(s) ","04890520","PLAIN DELUGE TIP 2.5AII 1 1/4DSCH POLISH",36]
["04890521","PLAIN DELUGE TIP 2.5AFD 1 1/2DSCH POLISH",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"QST","N/A","N/A","N/A","1-1/2\"","N/A","N/A","N","ENGLISH","SB Tip","High-Range","N/A",20,4,"0489","N/A","N/A",null,null,"0489 2.5 in QST 1-1/2\" bore size(s) ","04890521","PLAIN DELUGE TIP 2.5AFD 1 1/2DSCH POLISH",36]
["04890529","PLAIN DELUGE TIP 2.5NH 1 D POLISH",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"NH","N/A","N/A","N/A","1\"","N/A","N/A","N","ENGLISH","SB Tip","High-Range","N/A",20,4,"0489","N/A","N/A",null,null,"0489 2.5 in NH 1\" bore size(s) ","04890529","PLAIN DELUGE TIP 2.5NH 1 D POLISH",31]
["04890539","PLAIN DELUGE TIP 2.5BSP 1 3/8D POLISH",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"BSP","N/A","N/A","N/A","1-3/8\"","N/A","N/A","N","ENGLISH","SB Tip","High-Range","N/A",20,4,"0489","N/A","N/A",null,null,"0489 2.5 in BSP 1-3/8\" bore size(s) ","04890539","PLAIN DELUGE TIP 2.5BSP 1 3/8D POLISH",36]
["04890595","PLAIN DELUGE TIP 2.5AFD 1 1/4D POLISH",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"QST","N/A","N/A","N/A","1-1/4\"","N/A","N/A","N","ENGLISH","SB Tip","High-Range","N/A",20,4,"0489","N/A","N/A",null,null,"0489 2.5 in QST 1-1/4\" bore size(s) ","04890595","PLAIN DELUGE TIP 2.5AFD 1 1/4D POLISH",36]
["04890599","PLAIN DELUGE TIP 2.5 AEF 1 1/8D POLISH",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"AEF","N/A","N/A","N/A","1-1/8\"","N/A","N/A","N","ENGLISH","SB Tip","High-Range","N/A",20,4,"0489","N/A","N/A",null,null,"0489 2.5 in AEF 1-1/8\" bore size(s) ","04890599","PLAIN DELUGE TIP 2.5 AEF 1 1/8D POLISH",36]
["04890606","PLAIN DELUGE TIP 2.5 AKB 1 3/8D POLISH",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"AKB","N/A","N/A","N/A","1-3/8\"","N/A","N/A","N","ENGLISH","SB Tip","High-Range","N/A",20,4,"0489","N/A","N/A",null,null,"0489 2.5 in AKB 1-3/8\" bore size(s) ","04890606","PLAIN DELUGE TIP 2.5 AKB 1 3/8D POLISH",36]
["04890622","PLAIN DELUGE 5IP 2.5AII 1 3/8D POLISH",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"CSA","N/A","N/A","N/A","1-3/8\"","N/A","N/A","N","ENGLISH","SB Tip","High-Range","N/A",20,4,"0489","N/A","N/A",null,null,"0489 2.5 in CSA 1-3/8\" bore size(s) ","04890622","PLAIN DELUGE 5IP 2.5AII 1 3/8D POLISH",36]
["04890623","PLAIN DELUGE TIP 2.5NH 7/8D POLISH",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"NH","N/A","N/A","N/A","7/8\"","N/A","N/A","N","ENGLISH","SB Tip","High-Range","N/A",20,4,"0489","N/A","N/A",null,null,"0489 2.5 in NH 7/8\" bore size(s) ","04890623","PLAIN DELUGE TIP 2.5NH 7/8D POLISH",33]
["04890631","PLAIN DELUGE TIP 2.5BAF 7/8DSCH POLISH",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"BAT","N/A","N/A","N/A","7/8\"","N/A","N/A","N","ENGLISH","SB Tip","High-Range","N/A",20,4,"0489","N/A","N/A",null,null,"0489 2.5 in BAT 7/8\" bore size(s) ","04890631","PLAIN DELUGE TIP 2.5BAF 7/8DSCH POLISH",34]
["04890632","PLAIN DELUGE TIP 2.5 AFD 7/8D POLISH",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"QST","N/A","N/A","N/A","7/8\"","N/A","N/A","N","ENGLISH","SB Tip","High-Range","N/A",20,4,"0489","N/A","N/A",null,null,"0489 2.5 in QST 7/8\" bore size(s) ","04890632","PLAIN DELUGE TIP 2.5 AFD 7/8D POLISH",34]
["04890633","PLAIN DELUGE TIP 2.5BAF 15/16DSCH POLISH",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"BAT","N/A","N/A","N/A","15/16\"","N/A","N/A","N","ENGLISH","SB Tip","High-Range","N/A",20,4,"0489","N/A","N/A",null,null,"0489 2.5 in BAT 15/16\" bore size(s) ","04890633","PLAIN DELUGE TIP 2.5BAF 15/16DSCH POLISH",36]
["04890639","PLAIN DELUGE TIP 2.5AKB 1 1/4D POLISH",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"AKB","N/A","N/A","N/A","1-1/4\"","N/A","N/A","N","ENGLISH","SB Tip","High-Range","N/A",20,4,"0489","N/A","N/A",null,null,"0489 2.5 in AKB 1-1/4\" bore size(s) ","04890639","PLAIN DELUGE TIP 2.5AKB 1 1/4D POLISH",36]
["04890545","OBS PLAIN DELUGE TIP 2.5AFD 2\"DSCH POL",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","O",2.5,"QST","N/A","N/A","N/A","2\"","N/A","N/A","N","ENGLISH","SB Tip","High-Range","N/A",20,4,"0489","N/A","N/A",null,null,"0489 2.5 in QST 2\" bore size(s) ","04890545","OBS PLAIN DELUGE TIP 2.5AFD 2\"DSCH POL",32]
["14174004","TIP PLAIN 1.5NH 7/8D#",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","7/8\"","n/a","N/A","N","ENGLISH","SB Tip","1.5\"","N/A",20,2,"1417","N/A","N/A",null,null,"1417 1.5 in NH 7/8\" bore size(s) ","14174004","TIP PLAIN 1.5NH 7/8D#",33]
["14174005","TIP PLAIN 1.5NPSH 7/8D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NPSH","N/A","N/A","N/A","7/8\"","n/a","N/A","N","ENGLISH","SB Tip","1.5\"","N/A",20,2,"1417","N/A","N/A",null,null,"1417 1.5 in NPSH 7/8\" bore size(s) ","14174005","TIP PLAIN 1.5NPSH 7/8D",35]
["14174006","TIP PLAIN 1.5NH 15/16D#",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","15/16\"","n/a","N/A","N","ENGLISH","SB Tip","1.5\"","N/A",20,2,"1417","N/A","N/A",null,null,"1417 1.5 in NH 15/16\" bore size(s) ","14174006","TIP PLAIN 1.5NH 15/16D#",35]
["14174009","TIP PLAIN 1.5NH 1-1/8D#",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","1-1/8\"","n/a","N/A","N","ENGLISH","SB Tip","1.5\"","N/A",20,2,"1417","N/A","N/A",null,null,"1417 1.5 in NH 1-1/8\" bore size(s) ","14174009","TIP PLAIN 1.5NH 1-1/8D#",35]
["14174001","TIP PLAIN 1.5NH 3/8D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","3/8\"","n/a","N/A","N","ENGLISH","SB Tip","1.5\"","N/A",20,3,"1417","N/A","N/A",null,null,"1417 1.5 in NH 3/8\" bore size(s) ","14174001","TIP PLAIN 1.5NH 3/8D",33]
["14174002","TIP PLAIN 1.5NH 1/2D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","1/2\"","n/a","N/A","N","ENGLISH","SB Tip","1.5\"","N/A",20,3,"1417","N/A","N/A",null,null,"1417 1.5 in NH 1/2\" bore size(s) ","14174002","TIP PLAIN 1.5NH 1/2D",33]
["14174003","TIP PLAIN 1.5NH 3/4D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","3/4\"","n/a","N/A","N","ENGLISH","SB Tip","1.5\"","N/A",20,3,"1417","N/A","N/A",null,null,"1417 1.5 in NH 3/4\" bore size(s) ","14174003","TIP PLAIN 1.5NH 3/4D",33]
["14174008","TIP PLAIN 1.5NH 1D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","1\"","n/a","N/A","N","ENGLISH","SB Tip","1.5\"","N/A",20,3,"1417","N/A","N/A",null,null,"1417 1.5 in NH 1\" bore size(s) ","14174008","TIP PLAIN 1.5NH 1D",31]
["14174010","TIP PLAIN 1.5NPSH 1-1/8D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NPSH","N/A","N/A","N/A","1-1/8\"","n/a","N/A","N","ENGLISH","SB Tip","1.5\"","N/A",20,3,"1417","N/A","N/A",null,null,"1417 1.5 in NPSH 1-1/8\" bore size(s) ","14174010","TIP PLAIN 1.5NPSH 1-1/8D",37]
["14174019","TIP PLAIN 1.5NPSH 3/8D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NPSH","N/A","N/A","N/A","3/8\"","n/a","N/A","N","ENGLISH","SB Tip","1.5\"","N/A",20,3,"1417","N/A","N/A",null,null,"1417 1.5 in NPSH 3/8\" bore size(s) ","14174019","TIP PLAIN 1.5NPSH 3/8D",35]
["14174007","TIP PLAIN 1.5NPSH 15/16D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NPSH","N/A","N/A","N/A","15/16\"","n/a","N/A","N","ENGLISH","SB Tip","1.5\"","N/A",20,4,"1417","N/A","N/A",null,null,"1417 1.5 in NPSH 15/16\" bore size(s) ","14174007","TIP PLAIN 1.5NPSH 15/16D",37]
["14174018","TIP PLAIN 1.5NPSH 1D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NPSH","N/A","N/A","N/A","1\"","n/a","N/A","N","ENGLISH","SB Tip","1.5\"","N/A",20,4,"1417","N/A","N/A",null,null,"1417 1.5 in NPSH 1\" bore size(s) ","14174018","TIP PLAIN 1.5NPSH 1D",33]
["14174012","TIP PLAIN 1.5NPSH 1/2D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NPSH","N/A","N/A","N/A","1/2\"","n/a","N/A","N","ENGLISH","SB Tip","1.5\"","N/A","No 2021 Sales","No 2021 Sales","1417","N/A","N/A",null,null,"1417 1.5 in NPSH 1/2\" bore size(s) ","14174012","TIP PLAIN 1.5NPSH 1/2D",35]
["14174020","TIP PLAIN 1.5BSP 3/4D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"BSP","N/A","N/A","N/A","3/4\"","n/a","N/A","N","ENGLISH","SB Tip","1.5\"","N/A","No 2021 Sales","No 2021 Sales","1417","N/A","N/A",null,null,{"$f":"CONCATENATE(AC889,\" \",N889,\" in \",O889,\" \",IF(AD889=\"n/a\",\"\",CONCATENATE(AD889,\" in \",AE889,\" \")),IF(Q889=\"n/a\",\"\",Q889),IF(S889=\"n/a\",\"\",CONCATENATE(IF(X889=\"saber\",\" \",\"\"),S889,\" bore size(s) \")),IF(T889=\"n/a\",\"\",CONCATENATE(IF(X889=\"saber\",\"\",\" \"),T889,IF(T889=100,\" (Std) \",IF(T889=87,\" (CE) \",\" \")))),IF(U889=\"n/a\",\"\",CONCATENATE(U889,IF(U889=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X889,3)=\"tip\",IF(LEFT(X889,1)=\"s\",\"\",IF(Z889=\"n\",IF(T889=\"N/A\",\"PG\",\" PG\"),IF(Z889=\"y\",IF(T889=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z889=\"n\",IF(T889=\"N/A\",\"PG\",\" PG\"),IF(Z889=\"y\",IF(T889=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF889=\"y\",\" ZT\",\"\"),IF(V889=\"N\",\"\",IF(S889=\"n/a\",\" ETCH\",IF(T889=\"N/A\",IF(RIGHT(X889,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X889=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"1417 1.5 in BSP 3/4\" bore size(s) "},{"$f":"A889","v":"14174020"},{"$f":"B889","v":"TIP PLAIN 1.5BSP 3/4D"},{"$f":"LEN(AH889)","v":34}]
["14204001","TIP TRIPLE STK 1.5NH 1,1-1/8,1-1/4#",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","1-1/4\"; 1-1/8\"; 1\"","n/a","N/A","N","ENGLISH","Stack Tip","1.5\"","N/A",20,1,"1420",1.5,"NH",null,null,"1420 1.5 in NH 1.5 in NH 1-1/4\"; 1-1/8\"; 1\" bore size(s) ","14204001","TIP TRIPLE STK 1.5NH 1,1-1/8,1-1/4#",57]
["14204009","TIP TRIPLE STK 1.5NH 1,1-1/8,1-1/4 BDVFD",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","1-1/4\"; 1-1/8\"; 1\"","N/A","N/A","Y","ENGLISH","Stack Tip","1.5\"","N/A",20,3,"1420",1.5,"NH",null,null,"1420 1.5 in NH 1.5 in NH 1-1/4\"; 1-1/8\"; 1\" bore size(s) ETCH","14204009","TIP TRIPLE STK 1.5NH 1,1-1/8,1-1/4 BDVFD",61]
["14204010","TIP TRI STK 1.5NH 1,1-1/8,1-1/4 D.C.F.D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","1-1/4\"; 1-1/8\"; 1\"","N/A","N/A","Y","ENGLISH","Stack Tip","1.5\"","N/A",20,3,"1420",1.5,"NH",null,null,"1420 1.5 in NH 1.5 in NH 1-1/4\"; 1-1/8\"; 1\" bore size(s) ETCH","14204010","TIP TRI STK 1.5NH 1,1-1/8,1-1/4 D.C.F.D",61]
["14204002","TIP TRIPLE STK 1.5NPSH 1,1-1/8,1-1/4",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NPSH","N/A","N/A","N/A","1-1/4\"; 1-1/8\"; 1\"","n/a","N/A","N","ENGLISH","Stack Tip","1.5\"","N/A",20,4,"1420",1.5,"NH",null,null,"1420 1.5 in NPSH 1.5 in NH 1-1/4\"; 1-1/8\"; 1\" bore size(s) ","14204002","TIP TRIPLE STK 1.5NPSH 1,1-1/8,1-1/4",59]
["14994001","TIP 1.5NH 7/8D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","7/8\"","n/a","N/A","N","ENGLISH","SB Tip","1.5\"","N/A",20,1,"1499","N/A","N/A",null,null,{"$f":"CONCATENATE(AC894,\" \",N894,\" in \",O894,\" \",IF(AD894=\"n/a\",\"\",CONCATENATE(AD894,\" in \",AE894,\" \")),IF(Q894=\"n/a\",\"\",Q894),IF(S894=\"n/a\",\"\",CONCATENATE(IF(X894=\"saber\",\" \",\"\"),S894,\" bore size(s) \")),IF(T894=\"n/a\",\"\",CONCATENATE(IF(X894=\"saber\",\"\",\" \"),T894,IF(T894=100,\" (Std) \",IF(T894=87,\" (CE) \",\" \")))),IF(U894=\"n/a\",\"\",CONCATENATE(U894,IF(U894=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X894,3)=\"tip\",IF(LEFT(X894,1)=\"s\",\"\",IF(Z894=\"n\",IF(T894=\"N/A\",\"PG\",\" PG\"),IF(Z894=\"y\",IF(T894=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z894=\"n\",IF(T894=\"N/A\",\"PG\",\" PG\"),IF(Z894=\"y\",IF(T894=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF894=\"y\",\" ZT\",\"\"),IF(V894=\"N\",\"\",IF(S894=\"n/a\",\" ETCH\",IF(T894=\"N/A\",IF(RIGHT(X894,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X894=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"1499 1.5 in NH 7/8\" bore size(s) "},{"$f":"A894","v":"14994001"},{"$f":"B894","v":"TIP 1.5NH 7/8D"},{"$f":"LEN(AH894)","v":33}]
["14994003","TIP 1.5NH 15/16D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","15/16\"","n/a","N/A","N","ENGLISH","SB Tip","1.5\"","N/A",20,1,"1499","N/A","N/A",null,null,"1499 1.5 in NH 15/16\" bore size(s) ","14994003","TIP 1.5NH 15/16D",35]
["14994009","TIP 1.5NH 1-1/8D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","1-1/8\"","n/a","N/A","N","ENGLISH","SB Tip","1.5\"","N/A",20,1,"1499","N/A","N/A",null,null,"1499 1.5 in NH 1-1/8\" bore size(s) ","14994009","TIP 1.5NH 1-1/8D",35]
["14994004","TIP 1.5NPSH 15/16D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NPSH","N/A","N/A","N/A","15/16\"","n/a","N/A","N","ENGLISH","SB Tip","1.5\"","N/A",20,2,"1499","N/A","N/A",null,null,"1499 1.5 in NPSH 15/16\" bore size(s) ","14994004","TIP 1.5NPSH 15/16D",37]
["14994005","TIP 1.5NH 1D#",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","1\"","n/a","N/A","N","ENGLISH","SB Tip","1.5\"","N/A",20,2,"1499","N/A","N/A",null,null,"1499 1.5 in NH 1\" bore size(s) ","14994005","TIP 1.5NH 1D#",31]
["14994010","TIP 1.5NPSH 1-1/8D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NPSH","N/A","N/A","N/A","1-1/8\"","n/a","N/A","N","ENGLISH","SB Tip","1.5\"","N/A",20,2,"1499","N/A","N/A",null,null,"1499 1.5 in NPSH 1-1/8\" bore size(s) ","14994010","TIP 1.5NPSH 1-1/8D",37]
["14994011","TIP 1.5NH 1-3/16D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","1-3/16\"","n/a","N/A","N","ENGLISH","SB Tip","1.5\"","N/A",20,2,"1499","N/A","N/A",null,null,"1499 1.5 in NH 1-3/16\" bore size(s) ","14994011","TIP 1.5NH 1-3/16D",36]
["14994013","TIP 1.5NH 1-1/4D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","1-1/4\"","n/a","N/A","N","ENGLISH","SB Tip","1.5\"","N/A",20,2,"1499","N/A","N/A",null,null,"1499 1.5 in NH 1-1/4\" bore size(s) ","14994013","TIP 1.5NH 1-1/4D",35]
["14994015","TIP 1.5NH 1-3/8D#",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","1-3/8\"","n/a","N/A","N","ENGLISH","SB Tip","1.5\"","N/A",20,2,"1499","N/A","N/A",null,null,"1499 1.5 in NH 1-3/8\" bore size(s) ","14994015","TIP 1.5NH 1-3/8D#",35]
["14994045","TIP 1.5BSP 1-3/8D (35MM)",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"BSP","N/A","N/A","N/A","1-3/8\"","n/a","N/A","N","ENGLISH","SB Tip","1.5\"","N/A",20,2,"1499","N/A","N/A",null,null,{"$f":"CONCATENATE(AC903,\" \",N903,\" in \",O903,\" \",IF(AD903=\"n/a\",\"\",CONCATENATE(AD903,\" in \",AE903,\" \")),IF(Q903=\"n/a\",\"\",Q903),IF(S903=\"n/a\",\"\",CONCATENATE(IF(X903=\"saber\",\" \",\"\"),S903,\" bore size(s) \")),IF(T903=\"n/a\",\"\",CONCATENATE(IF(X903=\"saber\",\"\",\" \"),T903,IF(T903=100,\" (Std) \",IF(T903=87,\" (CE) \",\" \")))),IF(U903=\"n/a\",\"\",CONCATENATE(U903,IF(U903=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X903,3)=\"tip\",IF(LEFT(X903,1)=\"s\",\"\",IF(Z903=\"n\",IF(T903=\"N/A\",\"PG\",\" PG\"),IF(Z903=\"y\",IF(T903=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z903=\"n\",IF(T903=\"N/A\",\"PG\",\" PG\"),IF(Z903=\"y\",IF(T903=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF903=\"y\",\" ZT\",\"\"),IF(V903=\"N\",\"\",IF(S903=\"n/a\",\" ETCH\",IF(T903=\"N/A\",IF(RIGHT(X903,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X903=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"1499 1.5 in BSP 1-3/8\" bore size(s) "},{"$f":"A903","v":"14994045"},{"$f":"B903","v":"TIP 1.5BSP 1-3/8D (35MM)"},{"$f":"LEN(AH903)","v":36}]
["14994006","TIP 1.5NPSH 1D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NPSH","N/A","N/A","N/A","1\"","n/a","N/A","N","ENGLISH","SB Tip","1.5\"","N/A",20,3,"1499","N/A","N/A",null,null,"1499 1.5 in NPSH 1\" bore size(s) ","14994006","TIP 1.5NPSH 1D",33]
["14994014","TIP 1.5NPSH 1-1/4D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NPSH","N/A","N/A","N/A","1-1/4\"","n/a","N/A","N","ENGLISH","SB Tip","1.5\"","N/A",20,3,"1499","N/A","N/A",null,null,"1499 1.5 in NPSH 1-1/4\" bore size(s) ","14994014","TIP 1.5NPSH 1-1/4D",37]
["14994026","TIP 1.5BSP 7/8D (22MM)",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"BSP","N/A","N/A","N/A","7/8\"","n/a","N/A","N","ENGLISH","SB Tip","1.5\"","N/A",20,3,"1499","N/A","N/A",null,null,"1499 1.5 in BSP 7/8\" bore size(s) ","14994026","TIP 1.5BSP 7/8D (22MM)",34]
["14994029","TIP 1.5ABT 7/8D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"PCT","N/A","N/A","N/A","7/8\"","N/A","N/A","N","ENGLISH","SB Tip","1.5\"","N/A",20,3,"1499","N/A","N/A",null,null,"1499 1.5 in PCT 7/8\" bore size(s) ","14994029","TIP 1.5ABT 7/8D",34]
["14994049","TIP 1.5NH 7/8D SPC ETCH GPM/PSI",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","7/8\"","N/A","N/A","Y","ENGLISH","SB Tip","1.5\"","N/A",20,3,"1499","N/A","N/A",null,null,"1499 1.5 in NH 7/8\" bore size(s) ETCH","14994049","TIP 1.5NH 7/8D SPC ETCH GPM/PSI",37]
["14994051","TIP 1.5NH 7/8D OCEAN VIEW FIRE CO",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","7/8\"","N/A","N/A","Y","ENGLISH","SB Tip","1.5\"","N/A",20,3,"1499","N/A","N/A",null,null,"1499 1.5 in NH 7/8\" bore size(s) ETCH","14994051","TIP 1.5NH 7/8D OCEAN VIEW FIRE CO",37]
["14994002","TIP 1.5NPSH 7/8D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NPSH","N/A","N/A","N/A","7/8\"","n/a","N/A","N","ENGLISH","SB Tip","1.5\"","N/A",20,4,"1499","N/A","N/A",null,null,"1499 1.5 in NPSH 7/8\" bore size(s) ","14994002","TIP 1.5NPSH 7/8D",35]
["14994007","TIP 1.5NH 1-1/16D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","1-1/16\"","n/a","N/A","N","ENGLISH","SB Tip","1.5\"","N/A",20,4,"1499","N/A","N/A",null,null,"1499 1.5 in NH 1-1/16\" bore size(s) ","14994007","TIP 1.5NH 1-1/16D",36]
["14994008","TIP 1.5NPSH 1-1/16D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NPSH","N/A","N/A","N/A","1-1/16\"","N/A","N/A","N","ENGLISH","SB Tip","1.5\"","N/A",20,4,"1499","N/A","N/A",null,null,"1499 1.5 in NPSH 1-1/16\" bore size(s) ","14994008","TIP 1.5NPSH 1-1/16D",38]
["14994012","TIP 1.5NPSH 1-3/16D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NPSH","N/A","N/A","N/A","1-3/16\"","n/a","N/A","N","ENGLISH","SB Tip","1.5\"","N/A",20,4,"1499","N/A","N/A",null,null,"1499 1.5 in NPSH 1-3/16\" bore size(s) ","14994012","TIP 1.5NPSH 1-3/16D",38]
["14994038","TIP 1.5 ABX 15/16D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"ABX","N/A","N/A","N/A","15/16\"","N/A","N/A","N","ENGLISH","SB Tip","1.5\"","N/A",20,4,"1499","N/A","N/A",null,null,"1499 1.5 in ABX 15/16\" bore size(s) ","14994038","TIP 1.5 ABX 15/16D",36]
["14994039","TIP 1.5ABQ 1D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NYCORP","N/A","N/A","N/A","1\"","N/A","N/A","N","ENGLISH","SB Tip","1.5\"","N/A",20,4,"1499","N/A","N/A",null,null,"1499 1.5 in NYCORP 1\" bore size(s) ","14994039","TIP 1.5ABQ 1D",35]
["14994016","TIP 1.5NPSH 1-3/8D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NPSH","N/A","N/A","N/A","1-3/8\"","N/A","N/A","N","ENGLISH","SB Tip","1.5\"","N/A","No 2021 Sales","No 2021 Sales","1499","N/A","N/A",null,null,"1499 1.5 in NPSH 1-3/8\" bore size(s) ","14994016","TIP 1.5NPSH 1-3/8D",37]
["14994021","TIP 1.5ABU 1-1/16D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"FDNY","N/A","N/A","N/A","1-1/16\"","N/A","N/A","N","ENGLISH","SB Tip","1.5\"","N/A","No 2021 Sales","No 2021 Sales","1499","N/A","N/A",null,null,"1499 1.5 in FDNY 1-1/16\" bore size(s) ","14994021","TIP 1.5ABU 1-1/16D",38]
["14994022","TIP 1.5ABT 1-1/8D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"PCT","N/A","N/A","N/A","1-1/8\"","N/A","N/A","N","ENGLISH","SB Tip","1.5\"","N/A","No 2021 Sales","No 2021 Sales","1499","N/A","N/A",null,null,"1499 1.5 in PCT 1-1/8\" bore size(s) ","14994022","TIP 1.5ABT 1-1/8D",36]
["14990023","OBS TIP 1.5 NH   7/8 D   W/SCREW",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","O",1.5,"NH","N/A","N/A","N/A","7/8\"","N/A","N/A","N","ENGLISH","SB Tip","1.5\"","N/A",20,4,"1499","N/A","N/A",null,null,"1499 1.5 in NH 7/8\" bore size(s) ","14990023","OBS TIP 1.5 NH   7/8 D   W/SCREW",33]
["24204001","TIP STK 2.5NH X 1.5NH 1-3/8D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"NH","N/A","N/A","N/A","1-3/8\"; 1-1/4\"; 1\"","N/A","N/A","N","ENGLISH","Stack Tip","High-Range","N/A",20,1,"2420",1.5,"NH",null,null,"2420 2.5 in NH 1.5 in NH 1-3/8\"; 1-1/4\"; 1\" bore size(s) ","24204001","TIP STK 2.5NH X 1.5NH 1-3/8D",57]
["24204018","TIP STK 2.5AEF X 1.5NH 1-3/8D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"AEH","N/A","N/A","N/A","1-3/8\"; 1-1/4\"; 1\"","N/A","N/A","N","ENGLISH","Stack Tip","High-Range","N/A",20,1,"2420",1.5,"NH",null,null,{"$f":"CONCATENATE(AC921,\" \",N921,\" in \",O921,\" \",IF(AD921=\"n/a\",\"\",CONCATENATE(AD921,\" in \",AE921,\" \")),IF(Q921=\"n/a\",\"\",Q921),IF(S921=\"n/a\",\"\",CONCATENATE(IF(X921=\"saber\",\" \",\"\"),S921,\" bore size(s) \")),IF(T921=\"n/a\",\"\",CONCATENATE(IF(X921=\"saber\",\"\",\" \"),T921,IF(T921=100,\" (Std) \",IF(T921=87,\" (CE) \",\" \")))),IF(U921=\"n/a\",\"\",CONCATENATE(U921,IF(U921=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X921,3)=\"tip\",IF(LEFT(X921,1)=\"s\",\"\",IF(Z921=\"n\",IF(T921=\"N/A\",\"PG\",\" PG\"),IF(Z921=\"y\",IF(T921=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z921=\"n\",IF(T921=\"N/A\",\"PG\",\" PG\"),IF(Z921=\"y\",IF(T921=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF921=\"y\",\" ZT\",\"\"),IF(V921=\"N\",\"\",IF(S921=\"n/a\",\" ETCH\",IF(T921=\"N/A\",IF(RIGHT(X921,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X921=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"2420 2.5 in AEH 1.5 in NH 1-3/8\"; 1-1/4\"; 1\" bore size(s) "},{"$f":"A921","v":"24204018"},{"$f":"B921","v":"TIP STK 2.5AEF X 1.5NH 1-3/8D"},{"$f":"LEN(AH921)","v":58}]
["24204002","TIP STK 2.5NH X 1.5NH 1-1/4D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"NH","N/A","N/A","N/A","1-1/4\"; 1-1/8\"; 1\"","N/A","N/A","N","ENGLISH","Stack Tip","High-Range","N/A",20,2,"2420",1.5,"NH",null,null,"2420 2.5 in NH 1.5 in NH 1-1/4\"; 1-1/8\"; 1\" bore size(s) ","24204002","TIP STK 2.5NH X 1.5NH 1-1/4D",57]
["24204006","TIP STK 2.5AKB X 1.5NPSH 1-1/2D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"AKB","N/A","N/A","N/A","1-1/2\"; 1-1/4\"; 1\"","N/A","N/A","N","ENGLISH","Stack Tip","High-Range","N/A",20,3,"2420",1.5,"NPSH",null,null,"2420 2.5 in AKB 1.5 in NPSH 1-1/2\"; 1-1/4\"; 1\" bore size(s) ","24204006","TIP STK 2.5AKB X 1.5NPSH 1-1/2D",60]
["24204008","TIP STK 2.5BAF X 1.5NH 1-1/4D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"BAT","N/A","N/A","N/A","1-1/4\"; 1-1/8\"; 1\"","N/A","N/A","N","ENGLISH","Stack Tip","High-Range","N/A",20,3,"2420",1.5,"NH",null,null,"2420 2.5 in BAT 1.5 in NH 1-1/4\"; 1-1/8\"; 1\" bore size(s) ","24204008","TIP STK 2.5BAF X 1.5NH 1-1/4D",58]
["24204009","TIP STK 2.5NH X 1.5NH 1-1/2D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"NH","N/A","N/A","N/A","1-1/2\"; 1-1/4\"; 1\"","N/A","N/A","N","ENGLISH","Stack Tip","High-Range","N/A",20,3,"2420",1.5,"NH",null,null,"2420 2.5 in NH 1.5 in NH 1-1/2\"; 1-1/4\"; 1\" bore size(s) ","24204009","TIP STK 2.5NH X 1.5NH 1-1/2D",57]
["24204015","TIP STK 2.5BAF X 1.5NPSH 1-3/8D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"BAT","N/A","N/A","N/A","1-3/8\"; 1-1/4\"; 1\"","N/A","N/A","N","ENGLISH","Stack Tip","High-Range","N/A",20,3,"2420",1.5,"NPSH",null,null,"2420 2.5 in BAT 1.5 in NPSH 1-3/8\"; 1-1/4\"; 1\" bore size(s) ","24204015","TIP STK 2.5BAF X 1.5NPSH 1-3/8D",60]
["24204017","TIP STK 2.5AII X 1.5NPSH 1-1/2D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"CSA","N/A","N/A","N/A","1-1/2\"; 1-1/4\"; 1\"","N/A","N/A","N","ENGLISH","Stack Tip","High-Range","N",20,3,"2420",1.5,"NPSH",null,null,"2420 2.5 in CSA 1.5 in NPSH 1-1/2\"; 1-1/4\"; 1\" bore size(s) ","24204017","TIP STK 2.5AII X 1.5NPSH 1-1/2D",60]
["24204012","TIP STK 2.5AFB X 1.5ABU 1-1/2D L/DOM",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"FDNY","N/A","N/A","N/A","1-1/2\"; 1-1/4\"; 1\"","N/A","N/A","N","ENGLISH","Stack Tip","High-Range","N/A",20,4,"2420",1.5,"FDNY",null,null,"2420 2.5 in FDNY 1.5 in FDNY 1-1/2\"; 1-1/4\"; 1\" bore size(s) ","24204012","TIP STK 2.5AFB X 1.5ABU 1-1/2D L/DOM",61]
["24204016","TIP STK 2.5BAF X 1.5NPSH 1-1/4D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"BAT","N/A","N/A","N/A","1-1/4\"; 1-1/8\"; 1\"","N/A","N/A","N","ENGLISH","Stack Tip","High-Range","N/A",20,4,"2420",1.5,"NPSH",null,null,"2420 2.5 in BAT 1.5 in NPSH 1-1/4\"; 1-1/8\"; 1\" bore size(s) ","24204016","TIP STK 2.5BAF X 1.5NPSH 1-1/4D",60]
["24204005","TIP STK 2.5AIK X 1.5NH 1-1/4D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"AIK","N/A","N/A","N/A","1-1/4\"; 1-1/8\"; 1\"","N/A","N/A","N","ENGLISH","Stack Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","2420",1.5,"NH",null,null,"2420 2.5 in AIK 1.5 in NH 1-1/4\"; 1-1/8\"; 1\" bore size(s) ","24204005","TIP STK 2.5AIK X 1.5NH 1-1/4D",58]
["24204010","TIP STK 2.5AKB X 1.5NPSH 1-1/4D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"AKB","N/A","N/A","N/A","1-1/4\"; 1-1/8\"; 1\"","N/A","N/A","N","ENGLISH","Stack Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","2420",1.5,"NPSH",null,null,"2420 2.5 in AKB 1.5 in NPSH 1-1/4\"; 1-1/8\"; 1\" bore size(s) ","24204010","TIP STK 2.5AKB X 1.5NPSH 1-1/4D",60]
["24204011","TIP STK 2.5AKB X 1.5NH 1-1/4D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"AKB","N/A","N/A","N/A","1-1/4\"; 1-1/8\"; 1\"","N/A","N/A","N","ENGLISH","Stack Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","2420",1.5,"NH",null,null,{"$f":"CONCATENATE(AC932,\" \",N932,\" in \",O932,\" \",IF(AD932=\"n/a\",\"\",CONCATENATE(AD932,\" in \",AE932,\" \")),IF(Q932=\"n/a\",\"\",Q932),IF(S932=\"n/a\",\"\",CONCATENATE(IF(X932=\"saber\",\" \",\"\"),S932,\" bore size(s) \")),IF(T932=\"n/a\",\"\",CONCATENATE(IF(X932=\"saber\",\"\",\" \"),T932,IF(T932=100,\" (Std) \",IF(T932=87,\" (CE) \",\" \")))),IF(U932=\"n/a\",\"\",CONCATENATE(U932,IF(U932=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X932,3)=\"tip\",IF(LEFT(X932,1)=\"s\",\"\",IF(Z932=\"n\",IF(T932=\"N/A\",\"PG\",\" PG\"),IF(Z932=\"y\",IF(T932=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z932=\"n\",IF(T932=\"N/A\",\"PG\",\" PG\"),IF(Z932=\"y\",IF(T932=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF932=\"y\",\" ZT\",\"\"),IF(V932=\"N\",\"\",IF(S932=\"n/a\",\" ETCH\",IF(T932=\"N/A\",IF(RIGHT(X932,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X932=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"2420 2.5 in AKB 1.5 in NH 1-1/4\"; 1-1/8\"; 1\" bore size(s) "},{"$f":"A932","v":"24204011"},{"$f":"B932","v":"TIP STK 2.5AKB X 1.5NH 1-1/4D"},{"$f":"LEN(AH932)","v":58}]
["24204013","TIP STK 2.5BAF X 1.5NPSH 1-1/2D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"BAT","N/A","N/A","N/A","1-1/2\"; 1-1/4\"; 1\"","N/A","N/A","N","ENGLISH","Stack Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","2420",1.5,"NPSH",null,null,"2420 2.5 in BAT 1.5 in NPSH 1-1/2\"; 1-1/4\"; 1\" bore size(s) ","24204013","TIP STK 2.5BAF X 1.5NPSH 1-1/2D",60]
["24204019","TIP STK 2.5AFD X 1.5NH 1-3/8D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"QST","N/A","N/A","N/A","1-3/8\"; 1-1/4\"; 1\"","N/A","N/A","N","ENGLISH","Stack Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","2420",1.5,"NPSH",null,null,"2420 2.5 in QST 1.5 in NPSH 1-3/8\"; 1-1/4\"; 1\" bore size(s) ","24204019","TIP STK 2.5AFD X 1.5NH 1-3/8D",60]
["24204020","TIP STK 2.5NPSH X 1.5NPSH 1-1/4D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"NPSH","N/A","N/A","N/A","1-1/4\"; 1-1/8\"; 1\"","N/A","N/A","N","ENGLISH","Stack Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","2420",1.5,"NPSH",null,null,{"$f":"CONCATENATE(AC935,\" \",N935,\" in \",O935,\" \",IF(AD935=\"n/a\",\"\",CONCATENATE(AD935,\" in \",AE935,\" \")),IF(Q935=\"n/a\",\"\",Q935),IF(S935=\"n/a\",\"\",CONCATENATE(IF(X935=\"saber\",\" \",\"\"),S935,\" bore size(s) \")),IF(T935=\"n/a\",\"\",CONCATENATE(IF(X935=\"saber\",\"\",\" \"),T935,IF(T935=100,\" (Std) \",IF(T935=87,\" (CE) \",\" \")))),IF(U935=\"n/a\",\"\",CONCATENATE(U935,IF(U935=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X935,3)=\"tip\",IF(LEFT(X935,1)=\"s\",\"\",IF(Z935=\"n\",IF(T935=\"N/A\",\"PG\",\" PG\"),IF(Z935=\"y\",IF(T935=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z935=\"n\",IF(T935=\"N/A\",\"PG\",\" PG\"),IF(Z935=\"y\",IF(T935=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF935=\"y\",\" ZT\",\"\"),IF(V935=\"N\",\"\",IF(S935=\"n/a\",\" ETCH\",IF(T935=\"N/A\",IF(RIGHT(X935,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X935=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"2420 2.5 in NPSH 1.5 in NPSH 1-1/4\"; 1-1/8\"; 1\" bore size(s) "},{"$f":"A935","v":"24204020"},{"$f":"B935","v":"TIP STK 2.5NPSH X 1.5NPSH 1-1/4D"},{"$f":"LEN(AH935)","v":61}]
["30152004","NOZ IND/MAR 1.5 NH      95G @100P RDGN",null,null,null,null,null,null,null,null,"0006","Industrial Nozzles","A",1.5,"NH","GPM",100,"PSI","N/A",100,"BLACK","N","ENGLISH","Gov/Ind Fixed","1.5\"","Y",20,2,"3015","N/A","N/A",null,null,"3015 1.5 in NH 100 100 (Std) BLACK (Std) NPG","30152004","NOZ IND/MAR 1.5 NH      95G @100P RDGN",44]
["30152001","NOZ IND/MAR 1.5 NPSH 95G @100P RDGN",null,null,null,null,null,null,null,null,"0006","Industrial Nozzles","A",1.5,"NPSH","GPM",95,"PSI","N/A",100,"BLACK","N","ENGLISH","Gov/Ind Fixed","1.5\"","Y",20,3,"3015","N/A","N/A",null,null,"3015 1.5 in NPSH 95 100 (Std) BLACK (Std) NPG","30152001","NOZ IND/MAR 1.5 NPSH 95G @100P RDGN",45]
["30152006","NOZ IND/MAR 2.5 BIM 95G@100P RDGN",null,null,null,null,null,null,null,null,"0006","Industrial Nozzles","A",2.5,"BIM","GPM",95,"PSI","N/A",100,"BLACK","N","ENGLISH","Gov/Ind Fixed","1.5\"","Y","No 2021 Sales","No 2021 Sales","3015","N/A","N/A",null,null,"3015 2.5 in BIM 95 100 (Std) BLACK (Std) NPG","30152006","NOZ IND/MAR 2.5 BIM 95G@100P RDGN",44]
["30152007","NOZ IND/MAR 1.5 BSP 360LPM@7bar CS RDGN",null,null,null,null,null,null,null,null,"0006","Industrial Nozzles","A",1.5,"BSP","LPM",360,"BAR","N/A",7,"BLACK","N","ENGLISH","Gov/Ind Fixed","1.5\"","Y","No 2021 Sales","No 2021 Sales","3015","N/A","N/A",null,null,"3015 1.5 in BSP 360 7 BLACK (Std) NPG","30152007","NOZ IND/MAR 1.5 BSP 360LPM@7bar CS RDGN",37]
["30162001","NOZ IND/MAR 1.5 NH      125G @100P RDGN",null,null,null,null,null,null,null,null,"0006","Industrial Nozzles","A",1.5,"NH","GPM",125,"PSI","N/A",100,"BLACK","N","ENGLISH","Gov/Ind Fixed","1.5\"","Y","No 2021 Sales","No 2021 Sales","3016","N/A","N/A",null,null,"3016 1.5 in NH 125 100 (Std) BLACK (Std) NPG","30162001","NOZ IND/MAR 1.5 NH      125G @100P RDGN",44]
["30162002","NOZ IND/MAR 1.5 NPSH 125G @100P RDGN",null,null,null,null,null,null,null,null,"0006","Industrial Nozzles","A",1.5,"NPSH","GPM",125,"PSI","N/A",100,"BLACK","N","ENGLISH","Gov/Ind Fixed","1.5\"","Y","No 2021 Sales","No 2021 Sales","3016","N/A","N/A",null,null,"3016 1.5 in NPSH 125 100 (Std) BLACK (Std) NPG","30162002","NOZ IND/MAR 1.5 NPSH 125G @100P RDGN",46]
["37160004","TBJT IND 1.5 NH 60-125 GPM FM#",null,null,null,null,null,null,null,null,"0006","Industrial Nozzles","A",1.5,"NH","GPM","60-125","PSI","N/A",100,"BLACK","N","ENGLISH","GOV/IND Selectable","1.5\"","Y",20,1,"3716","N/A","N/A",null,null,"3716 1.5 in NH 60-125 100 (Std) BLACK (Std) NPG","37160004","TBJT IND 1.5 NH 60-125 GPM FM#",47]
["37160006","TBJT IND 1.5 BSP 230-475LPM FC FM",null,null,null,null,null,null,null,null,"0006","Industrial Nozzles","A",1.5,"BSP","LPM","230-475","BAR","N/A",7,"BLACK","N","ENGLISH","GOV/IND Selectable","1.5\"","N",20,1,"3716","N/A","N/A",null,null,"3716 1.5 in BSP 230-475 7 BLACK (Std) PG","37160006","TBJT IND 1.5 BSP 230-475LPM FC FM",40]
["37160005","TBJT IND 1.5 NPSH 60-125 GPM FM@",null,null,null,null,null,null,null,null,"0006","Industrial Nozzles","A",1.5,"NPSH","GPM","60-125","PSI","N/A",100,"BLACK","N","ENGLISH","GOV/IND Selectable","1.5\"","Y","No 2021 Sales","No 2021 Sales","3716","N/A","N/A",null,null,"3716 1.5 in NPSH 60-125 100 (Std) BLACK (Std) NPG","37160005","TBJT IND 1.5 NPSH 60-125 GPM FM@",49]
["37160008","TBJT IND 2.5 BIM 230-475LPM FC FM",null,null,null,null,null,null,null,null,"0006","Industrial Nozzles","A",2.5,"BIM","LPM","230-475","BAR","N/A",7,"BLACK","N","ENGLISH","GOV/IND Selectable","1.5\"","Y","No 2021 Sales","No 2021 Sales","3716","N/A","N/A",null,null,"3716 2.5 in BIM 230-475 7 BLACK (Std) NPG","37160008","TBJT IND 2.5 BIM 230-475LPM FC FM",41]
["37160011","TBJT IND 1.5 BSP 60-125 GPM FM",null,null,null,null,null,null,null,null,"0006","Industrial Nozzles","A",1.5,"BSP","GPM","60-125","PSI","N/A",100,"BLACK","N","ENGLISH","GOV/IND Selectable","1.5\"","Y","No 2021 Sales","No 2021 Sales","3716","N/A","N/A",null,null,"3716 1.5 in BSP 60-125 100 (Std) BLACK (Std) NPG","37160011","TBJT IND 1.5 BSP 60-125 GPM FM",48]
["37160012","TBJT IND 1.5 NH 230-475LPM FM",null,null,null,null,null,null,null,null,"0006","Industrial Nozzles","A",1.5,"NH","LPM","230-475","BAR","N/A",7,"BLACK","N","ENGLISH","GOV/IND Selectable","1.5\"","Y","No 2021 Sales","No 2021 Sales","3716","N/A","N/A",null,null,"3716 1.5 in NH 230-475 7 BLACK (Std) NPG","37160012","TBJT IND 1.5 NH 230-475LPM FM",40]
["37210001","NOZ IND 1.5 NH 60-125 GPM FC W/PG # FM",null,null,null,null,null,null,null,null,"0006","Industrial Nozzles","A",1.5,"NH","GPM","60-125","PSI","N/A",100,"BLACK","N","ENGLISH","GOV/IND Selectable","1.5\"","N",80,1,"3721","N/A","N/A",null,null,"3721 1.5 in NH 60-125 100 (Std) BLACK (Std) PG","37210001","NOZ IND 1.5 NH 60-125 GPM FC W/PG # FM",46]
["37210004","NOZ IND 1.5 BSP 230-475 L PG FC FM",null,null,null,null,null,null,null,null,"0006","Industrial Nozzles","A",1.5,"BSP","LPM","230-475","BAR","N/A",7,"BLACK","N","ENGLISH","GOV/IND Selectable","1.5\"","N",20,1,"3721","N/A","N/A",null,null,"3721 1.5 in BSP 230-475 7 BLACK (Std) PG","37210004","NOZ IND 1.5 BSP 230-475 L PG FC FM",40]
["37210002","NOZ IND 1.5 NPSH 60-125 G P/G  FC FM",null,null,null,null,null,null,null,null,"0006","Industrial Nozzles","A",1.5,"NPSH","GPM","60-125","PSI","N/A",100,"BLACK","N","ENGLISH","GOV/IND Selectable","1.5\"","N",20,2,"3721","N/A","N/A",null,null,"3721 1.5 in NPSH 60-125 100 (Std) BLACK (Std) PG","37210002","NOZ IND 1.5 NPSH 60-125 G P/G  FC FM",48]
["37210006","NOZ IND 2.5 BIM 230-475L PG FC FM",null,null,null,null,null,null,null,null,"0006","Industrial Nozzles","A",2.5,"BIM","LPM","230-475","BAR","N/A",7,"BLACK","N","ENGLISH","GOV/IND Selectable","1.5\"","N",20,2,"3721","N/A","N/A",null,null,"3721 2.5 in BIM 230-475 7 BLACK (Std) PG","37210006","NOZ IND 2.5 BIM 230-475L PG FC FM",40]
["37210017","NOZ IND 1.5 NH 230-475LPM P/G FC FM",null,null,null,null,null,null,null,null,"0006","Industrial Nozzles","A",1.5,"NH","LPM","230-475","PSI","N/A",100,"BLACK","N","ENGLISH","GOV/IND Selectable","1.5\"","N",20,2,"3721","N/A","N/A",null,null,"3721 1.5 in NH 230-475 100 (Std) BLACK (Std) PG","37210017","NOZ IND 1.5 NH 230-475LPM P/G FC FM",47]
["37210007","NOZ IND 2.5 NH 60-125 GPM PG FC W/PG FM",null,null,null,null,null,null,null,null,"0006","Industrial Nozzles","A",2.5,"NH","GPM","60-125","PSI","N/A",100,"BLACK","N","ENGLISH","GOV/IND Selectable","1.5\"","N","No 2021 Sales","No 2021 Sales","3721","N/A","N/A",null,null,"3721 2.5 in NH 60-125 100 (Std) BLACK (Std) PG","37210007","NOZ IND 2.5 NH 60-125 GPM PG FC W/PG FM",46]
["37210008","NOZ IND 1.5BSP LPM SPC STP PG GERM FC FM",null,null,null,null,null,null,null,null,"0006","Industrial Nozzles","A",1.5,"BSP","LPM","230-475","BAR","N/A",7,"BLACK","N","GERMAN","GOV/IND Selectable","1.5\"","N","No 2021 Sales","No 2021 Sales","3721","N/A","N/A",null,null,"3721 1.5 in BSP 230-475 7 BLACK (Std) PG","37210008","NOZ IND 1.5BSP LPM SPC STP PG GERM FC FM",40]
["37210009","NOZ IND 1.5 NPSH 230-475LPM P/G FC FM",null,null,null,null,null,null,null,null,"0006","Industrial Nozzles","A",1.5,"NPSH","LPM","230-475","BAR","N/A",7,"BLACK","N","ENGLISH","GOV/IND Selectable","1.5\"","N","No 2021 Sales","No 2021 Sales","3721","N/A","N/A",null,null,"3721 1.5 in NPSH 230-475 7 BLACK (Std) PG","37210009","NOZ IND 1.5 NPSH 230-475LPM P/G FC FM",41]
["37210013","NOZ IND JIM 65mm 230-475L PG FC FM",null,null,null,null,null,null,null,null,"0006","Industrial Nozzles","A",2.5,"JIM","LPM","230-475","BAR","N/A",7,"BLACK","N","ENGLISH","GOV/IND Selectable","1.5\"","N","No 2021 Sales","No 2021 Sales","3721","N/A","N/A",null,null,"3721 2.5 in JIM 230-475 7 BLACK (Std) PG","37210013","NOZ IND JIM 65mm 230-475L PG FC FM",40]
["37210014","NOZ IND 2.5 BIM 230-475L REDPG FC FM",null,null,null,null,null,null,null,null,"0006","Industrial Nozzles","A",2.5,"BIM","LPM","230-475","BAR","N/A",7,"BLACK","N","ENGLISH","GOV/IND Selectable","1.5\"","N","No 2021 Sales","No 2021 Sales","3721","N/A","N/A",null,null,"3721 2.5 in BIM 230-475 7 BLACK (Std) PG","37210014","NOZ IND 2.5 BIM 230-475L REDPG FC FM",40]
["37210015","NOZ IND 2.5 BIM 265-390-500L PG FC FM",null,null,null,null,null,null,null,null,"0006","Industrial Nozzles","A",2.5,"BIM","LPM","265-500","BAR","N/A",7,"BLACK","N","ENGLISH","GOV/IND Selectable","1.5\"","N","No 2021 Sales","No 2021 Sales","3721","N/A","N/A",null,null,"3721 2.5 in BIM 265-500 7 BLACK (Std) PG","37210015","NOZ IND 2.5 BIM 265-390-500L PG FC FM",40]
["37210016","NOZ IND 52MM 230-475L PG FC FM",null,null,null,null,null,null,null,null,"0006","Industrial Nozzles","A",2,"STORZ","LPM","230-475","BAR","N/A",7,"BLACK","N","ENGLISH","GOV/IND Selectable","1.5\"","N","No 2021 Sales","No 2021 Sales","3721","N/A","N/A",null,null,"3721 2 in STORZ 230-475 7 BLACK (Std) PG","37210016","NOZ IND 52MM 230-475L PG FC FM",40]
["37210018","NOZ IND 1.5 NH 75-117GPM @ 50PSI FC W/PG",null,null,null,null,null,null,null,null,"0006","Industrial Nozzles","A",1.5,"NH","GPM","75-117","PSI","N/A",100,"BLACK","N","ENGLISH","GOV/IND Selectable","1.5\"","N","No 2021 Sales","No 2021 Sales","3721","N/A","N/A",null,null,"3721 1.5 in NH 75-117 100 (Std) BLACK (Std) PG","37210018","NOZ IND 1.5 NH 75-117GPM @ 50PSI FC W/PG",46]
["37250500","NOZ IND TBJT 2.5 NH 120-250 GPM CS",null,null,null,null,null,null,null,null,"0006","Industrial Nozzles","A",2.5,"NH","GPM","120-250","PSI","N/A",100,"BLACK","N","ENGLISH","GOV/IND Selectable","High-Range","Y","No 2021 Sales","No 2021 Sales","3725","N/A","N/A",null,null,"3725 2.5 in NH 120-250 100 (Std) BLACK (Std) NPG","37250500","NOZ IND TBJT 2.5 NH 120-250 GPM CS",48]
["37250501","NOZ IND TBJT 2.5 BIM 450-950 LPM CS",null,null,null,null,null,null,null,null,"0006","Industrial Nozzles","A",2.5,"BIM","LPM","450-950","BAR","N/A",7,"BLACK","N","ENGLISH","GOV/IND Selectable","High-Range","Y","No 2021 Sales","No 2021 Sales","3725","N/A","N/A",null,null,{"$f":"CONCATENATE(AC962,\" \",N962,\" in \",O962,\" \",IF(AD962=\"n/a\",\"\",CONCATENATE(AD962,\" in \",AE962,\" \")),IF(Q962=\"n/a\",\"\",Q962),IF(S962=\"n/a\",\"\",CONCATENATE(IF(X962=\"saber\",\" \",\"\"),S962,\" bore size(s) \")),IF(T962=\"n/a\",\"\",CONCATENATE(IF(X962=\"saber\",\"\",\" \"),T962,IF(T962=100,\" (Std) \",IF(T962=87,\" (CE) \",\" \")))),IF(U962=\"n/a\",\"\",CONCATENATE(U962,IF(U962=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X962,3)=\"tip\",IF(LEFT(X962,1)=\"s\",\"\",IF(Z962=\"n\",IF(T962=\"N/A\",\"PG\",\" PG\"),IF(Z962=\"y\",IF(T962=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z962=\"n\",IF(T962=\"N/A\",\"PG\",\" PG\"),IF(Z962=\"y\",IF(T962=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF962=\"y\",\" ZT\",\"\"),IF(V962=\"N\",\"\",IF(S962=\"n/a\",\" ETCH\",IF(T962=\"N/A\",IF(RIGHT(X962,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X962=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"3725 2.5 in BIM 450-950 7 BLACK (Std) NPG"},{"$f":"A962","v":"37250501"},{"$f":"B962","v":"NOZ IND TBJT 2.5 BIM 450-950 LPM CS"},{"$f":"LEN(AH962)","v":41}]
["37250502","NOZ IND TBJT 2.5 BSP 450-950 LPM CS",null,null,null,null,null,null,null,null,"0006","Industrial Nozzles","A",2.5,"BSP","LPM","450-95","BAR","N/A",7,"BLACK","N","ENGLISH","GOV/IND Selectable","High-Range","Y","No 2021 Sales","No 2021 Sales","3725","N/A","N/A",null,null,"3725 2.5 in BSP 450-95 7 BLACK (Std) NPG","37250502","NOZ IND TBJT 2.5 BSP 450-950 LPM CS",40]
["20320001","COAST GUARD NOZZLE 1.5 NH QQC390* 4210#",null,null,null,null,null,null,null,null,"0007","Navy Coast Guard","A",1.5,"NH","GPM",55,"PSI","N/A",100,"N/A","N","ENGLISH","Specialty","1.5\"","Y",80,1,"2032","N/A","N/A",null,null,"2032 1.5 in NH 55 100 (Std)  NPG","20320001","COAST GUARD NOZZLE 1.5 NH QQC390* 4210#",32]
["20320002","COAST GUARD NOZZLE 1.5 NPSH QQ-C-390* 4",null,null,null,null,null,null,null,null,"0007","Navy Coast Guard","A",1.5,"NPSH","GPM",55,"PSI","N/A",100,"N/A","N","ENGLISH","Specialty","1.5\"","Y",20,2,"2032","N/A","N/A",null,null,"2032 1.5 in NPSH 55 100 (Std)  NPG","20320002","COAST GUARD NOZZLE 1.5 NPSH QQ-C-390* 4",34]
["20320006","COAST GUARD NOZZLE 2.5 BIM TYPE CS",null,null,null,null,null,null,null,null,"0007","Navy Coast Guard","O",2.5,"BIM","GPM",55,"PSI","N/A",100,"N/A","N","ENGLISH","Specialty","1.5\"","Y","No 2021 Sales","No 2021 Sales","2032","N/A","N/A",null,null,"2032 2.5 in BIM 55 100 (Std)  NPG","20320006","COAST GUARD NOZZLE 2.5 BIM TYPE CS",33]
["20460001","COAST GUARD NOZZLE 2.5 NH QQC-390#",null,null,null,null,null,null,null,null,"0007","Navy Coast Guard","A",2.5,"NH","GPM",106,"PSI","N/A",100,"N/A","N","ENGLISH","Specialty","High-Range","N/A",80,1,"2046","N/A","N/A",null,null,"2046 2.5 in NH 106 100 (Std)  ","20460001","COAST GUARD NOZZLE 2.5 NH QQC-390#",30]
["20460002","COAST GUARD NOZZLE 2.5 BSP QQC-390",null,null,null,null,null,null,null,null,"0007","Navy Coast Guard","A",2.5,"BSP","GPM",106,"PSI","N/A",100,"N/A","N","ENGLISH","Specialty","High-Range","Y","No 2021 Sales","No 2021 Sales","2046","N/A","N/A",null,null,"2046 2.5 in BSP 106 100 (Std)  NPG","20460002","COAST GUARD NOZZLE 2.5 BSP QQC-390",34]
["20460003","COAST GUARD NOZZLE 2.5 NPSH BALL TYPE CS",null,null,null,null,null,null,null,null,"0007","Navy Coast Guard","A",2.5,"NPSH","GPM",106,"PSI","N/A",100,"N/A","N","ENGLISH","Specialty","High-Range","Y","No 2021 Sales","No 2021 Sales","2046","N/A","N/A",null,null,"2046 2.5 in NPSH 106 100 (Std)  NPG","20460003","COAST GUARD NOZZLE 2.5 NPSH BALL TYPE CS",35]
["20460004","COAST GUARD NOZZLE 2.5 AFA QQC-390",null,null,null,null,null,null,null,null,"0007","Navy Coast Guard","A",2.5,"AFA","GPM",106,"PSI","N/A",100,"N/A","N","ENGLISH","Specialty","High-Range","Y","No 2021 Sales","No 2021 Sales","2046","N/A","N/A",null,null,"2046 2.5 in AFA 106 100 (Std)  NPG","20460004","COAST GUARD NOZZLE 2.5 AFA QQC-390",34]
["20460005","COAST GUARD NOZZLE 2.5 AFB FDNY QQC-390",null,null,null,null,null,null,null,null,"0007","Navy Coast Guard","A",2.5,"FDNY","GPM",106,"PSI","N/A",100,"N/A","N","ENGLISH","Specialty","High-Range","Y","No 2021 Sales","No 2021 Sales","2046","N/A","N/A",null,null,"2046 2.5 in FDNY 106 100 (Std)  NPG","20460005","COAST GUARD NOZZLE 2.5 AFB FDNY QQC-390",35]
["20460006","COAST GUARD NOZZLE 2.5 BIM QQC-390",null,null,null,null,null,null,null,null,"0007","Navy Coast Guard","A",2.5,"BIM","GPM",106,"PSI","N/A",100,"N/A","N","ENGLISH","Specialty","High-Range","Y","No 2021 Sales","No 2021 Sales","2046","N/A","N/A",null,null,"2046 2.5 in BIM 106 100 (Std)  NPG","20460006","COAST GUARD NOZZLE 2.5 BIM QQC-390",34]
["20690002","NAVY NOZZLE 1.5 NPSH ASTM B-62*4210",null,null,null,null,null,null,null,null,"0007","Navy Coast Guard","A",1.5,"NPSH","GPM",52,"PSI","N/A",100,"N/A","N","ENGLISH","Specialty","1.5\"","Y",20,1,"2069","N/A","N/A",null,null,"2069 1.5 in NPSH 52 100 (Std)  NPG","20690002","NAVY NOZZLE 1.5 NPSH ASTM B-62*4210",34]
["20690001","NAVY NOZZLE 1.5 NH ASTM B-62",null,null,null,null,null,null,null,null,"0007","Navy Coast Guard","A",1.5,"NH","GPM",52,"PSI","N/A",100,"N/A","N","ENGLISH","Specialty","1.5\"","N/A",20,3,"2069","N/A","N/A",null,null,"2069 1.5 in NH 52 100 (Std)  ","20690001","NAVY NOZZLE 1.5 NH ASTM B-62",29]
["20690003","NAVY NOZZLE 1.5 ABU ASTM B-62",null,null,null,null,null,null,null,null,"0007","Navy Coast Guard","A",1.5,"FDNY","GPM",52,"PSI","N/A",100,"N/A","N","ENGLISH","Specialty","1.5\"","Y","No 2021 Sales","No 2021 Sales","2069","N/A","N/A",null,null,"2069 1.5 in FDNY 52 100 (Std)  NPG","20690003","NAVY NOZZLE 1.5 ABU ASTM B-62",34]
["20690004","NAVY NOZZLE 1.5 BSP ASTM B-62",null,null,null,null,null,null,null,null,"0007","Navy Coast Guard","A",1.5,"BSP","GPM",52,"PSI","N/A",100,"N/A","N","ENGLISH","Specialty","1.5\"","Y","No 2021 Sales","No 2021 Sales","2069","N/A","N/A",null,null,"2069 1.5 in BSP 52 100 (Std)  NPG","20690004","NAVY NOZZLE 1.5 BSP ASTM B-62",33]
["20740001","NAVY NOZZLE 2.5 NH ASTM B-62* NSN: 4210-",null,null,null,null,null,null,null,null,"0007","Navy Coast Guard","A",2.5,"NH","GPM",132,"PSI","N/A",100,"N/A","N","ENGLISH","Specialty","High-Range","Y",80,1,"2074","N/A","N/A",null,null,"2074 2.5 in NH 132 100 (Std)  NPG","20740001","NAVY NOZZLE 2.5 NH ASTM B-62* NSN: 4210-",33]
["20740003","NAVY NOZZLE 2.5 AFB ASTMB62 FDNY",null,null,null,null,null,null,null,null,"0007","Navy Coast Guard","A",2.5,"FDNY","GPM",132,"PSI","N/A",100,"N/A","N","ENGLISH","Specialty","High-Range","Y","No 2021 Sales","No 2021 Sales","2074","N/A","N/A",null,null,"2074 2.5 in FDNY 132 100 (Std)  NPG","20740003","NAVY NOZZLE 2.5 AFB ASTMB62 FDNY",35]
["30192012","NOZ IND/MAR 1.5 NH  95G @100P CS",null,null,null,null,null,null,null,null,"0007","Navy Coast Guard","A",1.5,"NH","GPM",95,"PSI","N/A",100,"BLACK","N","ENGLISH","Gov/Ind Fixed","1.5\"","N",80,1,"3019","N/A","N/A",null,null,"3019 1.5 in NH 95 100 (Std) BLACK (Std) PG","30192012","NOZ IND/MAR 1.5 NH  95G @100P CS",42]
["30192009","NOZ IND/MAR 1.5 BSP     95G @100P",null,null,null,null,null,null,null,null,"0007","Navy Coast Guard","A",1.5,"BSP","GPM",95,"PSI","N/A",100,"BLACK","N","ENGLISH","Gov/Ind Fixed","1.5\"","N",20,1,"3019","N/A","N/A",null,null,"3019 1.5 in BSP 95 100 (Std) BLACK (Std) PG","30192009","NOZ IND/MAR 1.5 BSP     95G @100P",43]
["30192001","NOZ IND/MAR 1.5 NPSH 95G @100P RDGN",null,null,null,null,null,null,null,null,"0007","Navy Coast Guard","A",1.5,"NPSH","GPM",95,"PSI","N/A",100,"BLACK","N","ENGLISH","Gov/Ind Fixed","1.5\"","N",20,2,"3019","N/A","N/A",null,null,"3019 1.5 in NPSH 95 100 (Std) BLACK (Std) PG","30192001","NOZ IND/MAR 1.5 NPSH 95G @100P RDGN",44]
["30192004","NOZ IND/MAR 1.5 BSP   360L @7B RDGN",null,null,null,null,null,null,null,null,"0007","Navy Coast Guard","A",1.5,"BSP","LPM",360,"BAR","N/A",7,"BLACK","N","ENGLISH","Gov/Ind Fixed","1.5\"","N",20,2,"3019","N/A","N/A",null,null,"3019 1.5 in BSP 360 7 BLACK (Std) PG","30192004","NOZ IND/MAR 1.5 BSP   360L @7B RDGN",36]
["30192002","NOZ IND/MAR 2.5 BIM       95G @100P RDGN",null,null,null,null,null,null,null,null,"0007","Navy Coast Guard","A",2.5,"BIM","GPM",95,"PSI","N/A",100,"BLACK","N","ENGLISH","Gov/Ind Fixed","1.5\"","N","No 2021 Sales","No 2021 Sales","3019","N/A","N/A",null,null,"3019 2.5 in BIM 95 100 (Std) BLACK (Std) PG","30192002","NOZ IND/MAR 2.5 BIM       95G @100P RDGN",43]
["30192003","NOZ IND/MAR 1.5 52MM 360L @7B GERM",null,null,null,null,null,null,null,null,"0007","Navy Coast Guard","A",2,"STORZ","LPM",360,"BAR","N/A",7,"BLACK","N","GERMAN","Gov/Ind Fixed","1.5\"","N","No 2021 Sales","No 2021 Sales","3019","N/A","N/A",null,null,"3019 2 in STORZ 360 7 BLACK (Std) PG","30192003","NOZ IND/MAR 1.5 52MM 360L @7B GERM",36]
["30192007","NOZ IND/MAR 1.5 NPSH 360L @7B",null,null,null,null,null,null,null,null,"0007","Navy Coast Guard","A",1.5,"NPSH","LPM",360,"BAR","N/A",7,"BLACK","N","ENGLISH","Gov/Ind Fixed","1.5\"","N","No 2021 Sales","No 2021 Sales","3019","N/A","N/A",null,null,"3019 1.5 in NPSH 360 7 BLACK (Std) PG","30192007","NOZ IND/MAR 1.5 NPSH 360L @7B",37]
["30192010","NOZ IND/MAR 1.5 BSP   360L @7B GERM",null,null,null,null,null,null,null,null,"0007","Navy Coast Guard","A",1.5,"BSP","LPM",360,"BAR","N/A",7,"BLACK","N","GERMAN","Gov/Ind Fixed","1.5\"","N","No 2021 Sales","No 2021 Sales","3019","N/A","N/A",null,null,"3019 1.5 in BSP 360 7 BLACK (Std) PG","30192010","NOZ IND/MAR 1.5 BSP   360L @7B GERM",36]
["30192013","NOZ IND/MAR 1.5 NPSH 227L @7b",null,null,null,null,null,null,null,null,"0007","Navy Coast Guard","A",1.5,"NPSH","LPM",227,"BAR","N/A",7,"BLACK","N","ENGLISH","Gov/Ind Fixed","1.5\"","N","No 2021 Sales","No 2021 Sales","3019","N/A","N/A",null,null,"3019 1.5 in NPSH 227 7 BLACK (Std) PG","30192013","NOZ IND/MAR 1.5 NPSH 227L @7b",37]
["30192014","NOZ IND/MAR 1.5NPSH 170L@700kPa CS",null,null,null,null,null,null,null,null,"0007","Navy Coast Guard","A",1.5,"NPSH","LPM",170,"kPa","N/A",700,"BLACK","N","ENGLISH","Gov/Ind Fixed","1.5\"","N","No 2021 Sales","No 2021 Sales","3019","N/A","N/A",null,null,"3019 1.5 in NPSH 170 700 BLACK (Std) PG","30192014","NOZ IND/MAR 1.5NPSH 170L@700kPa CS",39]
["30192016","NOZ IND/MAR 1.5BSP 360L@7b SPAN WHTHDLPG",null,null,null,null,null,null,null,null,"0007","Navy Coast Guard","A",1.5,"BSP","LPM",360,"BAR","N/A",7,"BLACK","N","SPANISH","Gov/Ind Fixed","1.5\"","N","No 2021 Sales","No 2021 Sales","3019","N/A","N/A",null,null,"3019 1.5 in BSP 360 7 BLACK (Std) PG","30192016","NOZ IND/MAR 1.5BSP 360L@7b SPAN WHTHDLPG",36]
["30192017","NOZ IND/MAR 1.5 BSP 227L@7b",null,null,null,null,null,null,null,null,"0007","Navy Coast Guard","A",1.5,"BSP","LPM",227,"BAR","N/A",7,"BLACK","N","ENGLISH","Gov/Ind Fixed","1.5\"","N","No 2021 Sales","No 2021 Sales","3019","N/A","N/A",null,null,"3019 1.5 in BSP 227 7 BLACK (Std) PG","30192017","NOZ IND/MAR 1.5 BSP 227L@7b",36]
["30192018","NOZ IND/MAR 1.5NH 45GPM@100PSI CS",null,null,null,null,null,null,null,null,"0007","Navy Coast Guard","A",1.5,"NH","GPM",45,"PSI","N/A",100,"BLACK","N","ENGLISH","Gov/Ind Fixed","1.5\"","N","No 2021 Sales","No 2021 Sales","3019","N/A","N/A",null,null,"3019 1.5 in NH 45 100 (Std) BLACK (Std) PG","30192018","NOZ IND/MAR 1.5NH 45GPM@100PSI CS",42]
["30192019","NOZ IND/MAR 1.5 52MM 360L@7b",null,null,null,null,null,null,null,null,"0007","Navy Coast Guard","A",2,"STORZ","LPM",360,"BAR","N/A",7,"BLACK","N","ENGLISH","Gov/Ind Fixed","1.5\"","N","No 2021 Sales","No 2021 Sales","3019","N/A","N/A",null,null,"3019 2 in STORZ 360 7 BLACK (Std) PG","30192019","NOZ IND/MAR 1.5 52MM 360L@7b",36]
["30192020","NOZ IND/MAR 1.5 52MM 95G@100P",null,null,null,null,null,null,null,null,"0007","Navy Coast Guard","A",2,"STORZ","GPM",95,"PSI","N/A",100,"BLACK","N","ENGLISH","Gov/Ind Fixed","1.5\"","N","No 2021 Sales","No 2021 Sales","3019","N/A","N/A",null,null,"3019 2 in STORZ 95 100 (Std) BLACK (Std) PG","30192020","NOZ IND/MAR 1.5 52MM 95G@100P",43]
["30200002","NOZ NAVY                  1.5 NPSH 95 G",null,null,null,null,null,null,null,null,"0007","Navy Coast Guard","A",1.5,"NPSH","GPM",95,"PSI","N/A",100,"BLACK","N","ENGLISH","Gov/Ind Fixed","1.5\"","N",80,1,"3020","N/A","N/A",null,null,"3020 1.5 in NPSH 95 100 (Std) BLACK (Std) PG","30200002","NOZ NAVY                  1.5 NPSH 95 G",44]
["30200003","NOZ COAST GUARD 1.5 NH      95G  #",null,null,null,null,null,null,null,null,"0007","Navy Coast Guard","A",1.5,"NH","GPM",95,"PSI","N/A",100,"BLACK","N","ENGLISH","Gov/Ind Fixed","1.5\"","N",80,1,"3020","N/A","N/A",null,null,"3020 1.5 in NH 95 100 (Std) BLACK (Std) PG","30200003","NOZ COAST GUARD 1.5 NH      95G  #",42]
["30200006","NOZ NAVY                  2.5 BIM    95G",null,null,null,null,null,null,null,null,"0007","Navy Coast Guard","A",2.5,"BIM","GPM",95,"PSI","N/A",100,"BLACK","N","ENGLISH","Gov/Ind Fixed","1.5\"","N",80,1,"3020","N/A","N/A",null,null,"3020 2.5 in BIM 95 100 (Std) BLACK (Std) PG","30200006","NOZ NAVY                  2.5 BIM    95G",43]
["30200007","NOZ COAST GUARD 1.5 BSP   95G",null,null,null,null,null,null,null,null,"0007","Navy Coast Guard","A",1.5,"BSP","GPM",95,"PSI","N/A",100,"BLACK","N","ENGLISH","Gov/Ind Fixed","1.5\"","N",20,2,"3020","N/A","N/A",null,null,"3020 1.5 in BSP 95 100 (Std) BLACK (Std) PG","30200007","NOZ COAST GUARD 1.5 BSP   95G",43]
["30200009","NOZ NAVY                  1.5 52MM 95G",null,null,null,null,null,null,null,null,"0007","Navy Coast Guard","A",2,"STORZ","GPM",95,"PSI","N/A",100,"BLACK","N","ENGLISH","Gov/Ind Fixed","1.5\"","N","No 2021 Sales","No 2021 Sales","3020","N/A","N/A",null,null,"3020 2 in STORZ 95 100 (Std) BLACK (Std) PG","30200009","NOZ NAVY                  1.5 52MM 95G",43]
["30200010","NOZ COAST GUARD 1.5 ABU 95G FDNY",null,null,null,null,null,null,null,null,"0007","Navy Coast Guard","A",1.5,"FDNY","GPM",95,"PSI","N/A",100,"BLACK","N","ENGLISH","Gov/Ind Fixed","1.5\"","N","No 2021 Sales","No 2021 Sales","3020","N/A","N/A",null,null,"3020 1.5 in FDNY 95 100 (Std) BLACK (Std) PG","30200010","NOZ COAST GUARD 1.5 ABU 95G FDNY",44]
["30200012","NOZ COAST GUARD TYPE 38MM 95GPM",null,null,null,null,null,null,null,null,"0007","Navy Coast Guard","A",1.5,"STORZ","GPM",95,"PSI","N/A",100,"BLACK","N","ENGLISH","Gov/Ind Fixed","1.5\"","N","No 2021 Sales","No 2021 Sales","3020","N/A","N/A",null,null,"3020 1.5 in STORZ 95 100 (Std) BLACK (Std) PG","30200012","NOZ COAST GUARD TYPE 38MM 95GPM",45]
["30200013","NOZ COAST GUARD TYPE 38MM 360L@7b",null,null,null,null,null,null,null,null,"0007","Navy Coast Guard","A",1.5,"STORZ","LPM",360,"BAR","N/A",7,"BLACK","N","ENGLISH","Gov/Ind Fixed","1.5\"","N","No 2021 Sales","No 2021 Sales","3020","N/A","N/A",null,null,"3020 1.5 in STORZ 360 7 BLACK (Std) PG","30200013","NOZ COAST GUARD TYPE 38MM 360L@7b",38]
["30212001","NOZ IND/MAR 1.5 NH      125G@100P",null,null,null,null,null,null,null,null,"0007","Navy Coast Guard","A",1.5,"NH","GPM",125,"PSI","N/A",100,"BLACK","N","ENGLISH","Gov/Ind Fixed","1.5\"","N",20,1,"3021","N/A","N/A",null,null,"3021 1.5 in NH 125 100 (Std) BLACK (Std) PG","30212001","NOZ IND/MAR 1.5 NH      125G@100P",43]
["30212008","NOZ IND/MAR 1.5 BSP     475L@7b",null,null,null,null,null,null,null,null,"0007","Navy Coast Guard","A",1.5,"BSP","LPM",475,"BAR","N/A",7,"BLACK","N","ENGLISH","Gov/Ind Fixed","1.5\"","N",20,1,"3021","N/A","N/A",null,null,"3021 1.5 in BSP 475 7 BLACK (Std) PG","30212008","NOZ IND/MAR 1.5 BSP     475L@7b",36]
["30212003","NOZ IND/MAR  2.5 BIM      475L@7b",null,null,null,null,null,null,null,null,"0007","Navy Coast Guard","A",2.5,"BIM","LPM",475,"BAR","N/A",7,"BLACK","N","ENGLISH","Gov/Ind Fixed","1.5\"","N",20,2,"3021","N/A","N/A",null,null,"3021 2.5 in BIM 475 7 BLACK (Std) PG","30212003","NOZ IND/MAR  2.5 BIM      475L@7b",36]
["30212002","NOZ IND/MAR 1.5 NPSH 125G@100P",null,null,null,null,null,null,null,null,"0007","Navy Coast Guard","A",1.5,"NPSH","GPM",125,"PSI","N/A",100,"BLACK","N","ENGLISH","Gov/Ind Fixed","1.5\"","N",20,3,"3021","N/A","N/A",null,null,"3021 1.5 in NPSH 125 100 (Std) BLACK (Std) PG","30212002","NOZ IND/MAR 1.5 NPSH 125G@100P",45]
["30212007","NOZ IND/MAR 1.5 BSP     125G@100P",null,null,null,null,null,null,null,null,"0007","Navy Coast Guard","A",1.5,"BSP","GPM",125,"PSI","N/A",100,"BLACK","N","ENGLISH","Gov/Ind Fixed","1.5\"","N",20,3,"3021","N/A","N/A",null,null,"3021 1.5 in BSP 125 100 (Std) BLACK (Std) PG","30212007","NOZ IND/MAR 1.5 BSP     125G@100P",44]
["30212009","NOZ IND/MAR 1.5 NH        475L@7b",null,null,null,null,null,null,null,null,"0007","Navy Coast Guard","A",1.5,"NH","LPM",475,"BAR","N/A",7,"BLACK","N","ENGLISH","Gov/Ind Fixed","1.5\"","N","No 2021 Sales","No 2021 Sales","3021","N/A","N/A",null,null,"3021 1.5 in NH 475 7 BLACK (Std) PG","30212009","NOZ IND/MAR 1.5 NH        475L@7b",35]
["30220001","NOZ COAST GUARD 1.5 NH      95G  #",null,null,null,null,null,null,null,null,"0007","Navy Coast Guard","A",1.5,"NH","GPM",95,"PSI","N/A",100,"BLACK","N","ENGLISH","Gov/Ind Fixed","1.5\"","Y",80,1,"3022","N/A","N/A",null,null,"3022 1.5 in NH 95 100 (Std) BLACK (Std) NPG","30220001","NOZ COAST GUARD 1.5 NH      95G  #",43]
["30220002","NOZ COAST GUARD 1.5 NPSH 95G",null,null,null,null,null,null,null,null,"0007","Navy Coast Guard","A",1.5,"NPSH","GPM",95,"PSI","N/A",100,"BLACK","N","ENGLISH","Gov/Ind Fixed","1.5\"","Y",20,3,"3022","N/A","N/A",null,null,"3022 1.5 in NPSH 95 100 (Std) BLACK (Std) NPG","30220002","NOZ COAST GUARD 1.5 NPSH 95G",45]
["30220004","NOZ COAST GUARD  2.5 BIM     95G",null,null,null,null,null,null,null,null,"0007","Navy Coast Guard","A",2.5,"BIM","LPM",95,"PSI","N/A",100,"BLACK","N","ENGLISH","Gov/Ind Fixed","1.5\"","Y","No 2021 Sales","No 2021 Sales","3022","N/A","N/A",null,null,"3022 2.5 in BIM 95 100 (Std) BLACK (Std) NPG","30220004","NOZ COAST GUARD  2.5 BIM     95G",44]
["30230002","NOZ NAVY 1.5 NPSH 125G",null,null,null,null,null,null,null,null,"0007","Navy Coast Guard","A",1.5,"NPSH","GPM",125,"PSI","N/A",100,"BLACK","N","ENGLISH","Gov/Ind Fixed","1.5\"","N",80,1,"3023","N/A","N/A",null,null,"3023 1.5 in NPSH 125 100 (Std) BLACK (Std) PG","30230002","NOZ NAVY 1.5 NPSH 125G",45]
["30230003","NOZ NAVY 1.5 NH 125G",null,null,null,null,null,null,null,null,"0007","Navy Coast Guard","A",1.5,"NH","GPM",125,"PSI","N/A",100,"BLACK","N","ENGLISH","Gov/Ind Fixed","1.5\"","N",80,1,"3023","N/A","N/A",null,null,"3023 1.5 in NH 125 100 (Std) BLACK (Std) PG","30230003","NOZ NAVY 1.5 NH 125G",43]
["30230004","NOZ NAVY 1.5 BSP 125G",null,null,null,null,null,null,null,null,"0007","Navy Coast Guard","A",1.5,"BSP","GPM",125,"PSI","N/A",100,"BLACK","N","ENGLISH","Gov/Ind Fixed","1.5\"","N","No 2021 Sales","No 2021 Sales","3023","N/A","N/A",null,null,"3023 1.5 in BSP 125 100 (Std) BLACK (Std) PG","30230004","NOZ NAVY 1.5 BSP 125G",44]
["30230005","NOZ NAVY 2.5 BIM 475L@7b",null,null,null,null,null,null,null,null,"0007","Navy Coast Guard","A",2.5,"BIM","LPM",475,"BAR","N/A",7,"BLACK","N","ENGLISH","Gov/Ind Fixed","1.5\"","N","No 2021 Sales","No 2021 Sales","3023","N/A","N/A",null,null,"3023 2.5 in BIM 475 7 BLACK (Std) PG","30230005","NOZ NAVY 2.5 BIM 475L@7b",36]
["30250008","NOZ IND TYPE 1 2.5\"BIM     250GPM  RDGN",null,null,null,null,null,null,null,null,"0007","Navy Coast Guard","A",2.5,"BIM","LPM",250,"PSI","N/A",100,"BLACK","N","ENGLISH","Gov/Ind Fixed","High-Range","N",80,1,"3025","N/A","N/A",null,null,"3025 2.5 in BIM 250 100 (Std) BLACK (Std) PG","30250008","NOZ IND TYPE 1 2.5\"BIM     250GPM  RDGN",44]
["30250001","NOZ IND 2.5\"NH 250 GPM TYPE I REDESIGN",null,null,null,null,null,null,null,null,"0007","Navy Coast Guard","A",2.5,"NH","GPM",250,"PSI","N/A",100,"BLACK","N","ENGLISH","Gov/Ind Fixed","High-Range","N",20,2,"3025","N/A","N/A",null,null,"3025 2.5 in NH 250 100 (Std) BLACK (Std) PG","30250001","NOZ IND 2.5\"NH 250 GPM TYPE I REDESIGN",43]
["30250011","NOZ IND TYPE 1 2.5\" BSP 250GPM  RDGN",null,null,null,null,null,null,null,null,"0007","Navy Coast Guard","A",2.5,"BSP","GPM",250,"PSI","N/A",100,"BLACK","N","ENGLISH","Gov/Ind Fixed","High-Range","Y","No 2021 Sales","No 2021 Sales","3025","N/A","N/A",null,null,"3025 2.5 in BSP 250 100 (Std) BLACK (Std) NPG","30250011","NOZ IND TYPE 1 2.5\" BSP 250GPM  RDGN",45]
["30250012","NOZ IND TYPE 1 2.5\"AFD 250GPM RDSGN",null,null,null,null,null,null,null,null,"0007","Navy Coast Guard","A",2.5,"QST","GPM",250,"PSI","N/A",100,"BLACK","N","ENGLISH","Gov/Ind Fixed","High-Range","Y","No 2021 Sales","No 2021 Sales","3025","N/A","N/A",null,null,"3025 2.5 in QST 250 100 (Std) BLACK (Std) NPG","30250012","NOZ IND TYPE 1 2.5\"AFD 250GPM RDSGN",45]
["30270001","NOZ  2.5\"NH  250 GPM  NAVY-1904",null,null,null,null,null,null,null,null,"0007","Navy Coast Guard","A",2.5,"NH","GPM",250,"PSI","N/A",100,"BLACK","N","ENGLISH","Gov/Ind Fixed","High-Range","N","No 2021 Sales","No 2021 Sales","3027","N/A","N/A",null,null,"3027 2.5 in NH 250 100 (Std) BLACK (Std) PG","30270001","NOZ  2.5\"NH  250 GPM  NAVY-1904",43]
["15120002","OBS NOZ SBJT 1.0 NH 1/2D  60G W/PG",null,null,null,null,null,null,null,null,"0048","SABER JET NOZZLE","A",1,"NH","GPM",60,"PSI","1/2\"",100,"BLACK","N","ENGLISH","Saber","1\"","N","No 2021 Sales","No 2021 Sales","1512","N/A","N/A",null,null,"1512 1 in NH 60 1/2\" bore size(s) 100 (Std) BLACK (Std) PG","15120002","OBS NOZ SBJT 1.0 NH 1/2D  60G W/PG",58]
["15204002","SBJT 1.5NH 5/8 TIP 95G/360L",null,null,null,null,null,null,null,null,"0048","SABER JET NOZZLE","A",1.5,"NH","GPM",95,"PSI","5/8\"",100,"BLACK","N","ENGLISH","Saber","1.5\"","N",20,1,"1520","N/A","N/A",null,null,"1520 1.5 in NH 95 5/8\" bore size(s) 100 (Std) BLACK (Std) PG","15204002","SBJT 1.5NH 5/8 TIP 95G/360L",60]
["15204004","SBJT 1.5NPSH 5/8 TIP 95G/360L",null,null,null,null,null,null,null,null,"0048","SABER JET NOZZLE","A",1.5,"NPSH","GPM",95,"PSI","5/8\"",100,"BLACK","N","ENGLISH","Saber","1.5\"","N",20,2,"1520","N/A","N/A",null,null,"1520 1.5 in NPSH 95 5/8\" bore size(s) 100 (Std) BLACK (Std) PG","15204004","SBJT 1.5NPSH 5/8 TIP 95G/360L",62]
["15204009","SBJT 2.5BIM 5/8 TIP 95G/360L",null,null,null,null,null,null,null,null,"0048","SABER JET NOZZLE","A",2.5,"BIM","GPM",95,"PSI","5/8\"",100,"BLACK","N","ENGLISH","Saber","1.5\"","N",20,2,"1520","N/A","N/A",null,null,"1520 2.5 in BIM 95 5/8\" bore size(s) 100 (Std) BLACK (Std) PG","15204009","SBJT 2.5BIM 5/8 TIP 95G/360L",61]
["15204001","SBJT 1.5NH 1/2 TIP 95G/360L",null,null,null,null,null,null,null,null,"0048","SABER JET NOZZLE","A",1.5,"NH","GPM",95,"PSI","1/2\"",100,"BLACK","N","ENGLISH","Saber","1.5\"","N","No 2021 Sales","No 2021 Sales","1520","N/A","N/A",null,null,"1520 1.5 in NH 95 1/2\" bore size(s) 100 (Std) BLACK (Std) PG","15204001","SBJT 1.5NH 1/2 TIP 95G/360L",60]
["15204003","SBJT 1.5NPSH 1/2 TIP 95G/360L",null,null,null,null,null,null,null,null,"0048","SABER JET NOZZLE","A",1.5,"NPSH","GPM",95,"PSI","1/2\"",100,"BLACK","N","ENGLISH","Saber","1.5\"","N","No 2021 Sales","No 2021 Sales","1520","N/A","N/A",null,null,"1520 1.5 in NPSH 95 1/2\" bore size(s) 100 (Std) BLACK (Std) PG","15204003","SBJT 1.5NPSH 1/2 TIP 95G/360L",62]
["15204005","SBJT 1.5BSP 1/2 TIP 95G/360L",null,null,null,null,null,null,null,null,"0048","SABER JET NOZZLE","A",1.5,"BSP","GPM",95,"PSI","1/2\"",100,"BLACK","N","ENGLISH","Saber","1.5\"","N","No 2021 Sales","No 2021 Sales","1520","N/A","N/A",null,null,{"$f":"CONCATENATE(AC1026,\" \",N1026,\" in \",O1026,\" \",IF(AD1026=\"n/a\",\"\",CONCATENATE(AD1026,\" in \",AE1026,\" \")),IF(Q1026=\"n/a\",\"\",Q1026),IF(S1026=\"n/a\",\"\",CONCATENATE(IF(X1026=\"saber\",\" \",\"\"),S1026,\" bore size(s) \")),IF(T1026=\"n/a\",\"\",CONCATENATE(IF(X1026=\"saber\",\"\",\" \"),T1026,IF(T1026=100,\" (Std) \",IF(T1026=87,\" (CE) \",\" \")))),IF(U1026=\"n/a\",\"\",CONCATENATE(U1026,IF(U1026=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X1026,3)=\"tip\",IF(LEFT(X1026,1)=\"s\",\"\",IF(Z1026=\"n\",IF(T1026=\"N/A\",\"PG\",\" PG\"),IF(Z1026=\"y\",IF(T1026=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z1026=\"n\",IF(T1026=\"N/A\",\"PG\",\" PG\"),IF(Z1026=\"y\",IF(T1026=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF1026=\"y\",\" ZT\",\"\"),IF(V1026=\"N\",\"\",IF(S1026=\"n/a\",\" ETCH\",IF(T1026=\"N/A\",IF(RIGHT(X1026,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X1026=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"1520 1.5 in BSP 95 1/2\" bore size(s) 100 (Std) BLACK (Std) PG"},{"$f":"A1026","v":"15204005"},{"$f":"B1026","v":"SBJT 1.5BSP 1/2 TIP 95G/360L"},{"$f":"LEN(AH1026)","v":61}]
["15204006","SBJT 1.5BSP M 1/2 TIP 95G/360L",null,null,null,null,null,null,null,null,"0048","SABER JET NOZZLE","A",1.5,"BSP","GPM",95,"PSI","1/2\"",100,"BLACK","N","ENGLISH","Saber","1.5\"","N","No 2021 Sales","No 2021 Sales","1520","N/A","N/A",null,null,"1520 1.5 in BSP 95 1/2\" bore size(s) 100 (Std) BLACK (Std) PG","15204006","SBJT 1.5BSP M 1/2 TIP 95G/360L",61]
["15204007","SBJT 1.5BSP 5/8 TIP 95G/360L",null,null,null,null,null,null,null,null,"0048","SABER JET NOZZLE","A",1.5,"BSP","GPM",95,"PSI","5/8\"",100,"BLACK","N","ENGLISH","Saber","1.5\"","N","No 2021 Sales","No 2021 Sales","1520","N/A","N/A",null,null,"1520 1.5 in BSP 95 5/8\" bore size(s) 100 (Std) BLACK (Std) PG","15204007","SBJT 1.5BSP 5/8 TIP 95G/360L",61]
["15204008","SBJT 52MM 1/2 TIP 95G/360L",null,null,null,null,null,null,null,null,"0048","SABER JET NOZZLE","A",2,"STORZ","GPM",95,"PSI","1/2\"",100,"BLACK","N","ENGLISH","Saber","1.5\"","N","No 2021 Sales","No 2021 Sales","1520","N/A","N/A",null,null,"1520 2 in STORZ 95 1/2\" bore size(s) 100 (Std) BLACK (Std) PG","15204008","SBJT 52MM 1/2 TIP 95G/360L",61]
["15204017","SBJT 38MM 1/2 TIP 95G/360L",null,null,null,null,null,null,null,null,"0048","SABER JET NOZZLE","A",1.5,"STORZ","GPM",95,"PSI","1/2\"",100,"BLACK","N","ENGLISH","Saber","1.5\"","N","No 2021 Sales","No 2021 Sales","1520","N/A","N/A",null,null,"1520 1.5 in STORZ 95 1/2\" bore size(s) 100 (Std) BLACK (Std) PG","15204017","SBJT 38MM 1/2 TIP 95G/360L",63]
["15204018","SBJT ZT 1.5NPSH 5/8 TIP 95G/360L",null,null,null,null,null,null,null,null,"0048","SABER JET NOZZLE","A",1.5,"NPSH","GPM",95,"PSI","5/8\"",100,"BLACK","N","ENGLISH","Saber","1.5\"","N","No 2021 Sales","No 2021 Sales","1520","N/A","N/A","Y",null,"1520 1.5 in NPSH 95 5/8\" bore size(s) 100 (Std) BLACK (Std) PG ZT","15204018","SBJT ZT 1.5NPSH 5/8 TIP 95G/360L",65]
["15234019","SBJT 65MM JIM 1D",null,null,null,null,null,null,null,null,"0048","SABER JET NOZZLE","A",2.5,"JIM","GPM",135,"PSI","1\"",100,"BLACK","N","ENGLISH","Saber","Mid-Range","N",80,1,"1523","N/A","N/A",null,null,"1523 2.5 in JIM 135 1\" bore size(s) 100 (Std) BLACK (Std) PG","15234019","SBJT 65MM JIM 1D",60]
["15234005","SBJT 1.5NH 15/16D",null,null,null,null,null,null,null,null,"0048","SABER JET NOZZLE","A",1.5,"NH","GPM",135,"PSI","15/16\"",100,"BLACK","N","ENGLISH","Saber","Mid-Range","N",20,1,"1523","N/A","N/A",null,null,"1523 1.5 in NH 135 15/16\" bore size(s) 100 (Std) BLACK (Std) PG","15234005","SBJT 1.5NH 15/16D",63]
["15234008","SBJT 1.5NPSH 15/16D",null,null,null,null,null,null,null,null,"0048","SABER JET NOZZLE","A",1.5,"NPSH","GPM",135,"PSI","15/16\"",100,"BLACK","N","ENGLISH","Saber","Mid-Range","N",20,1,"1523","N/A","N/A",null,null,"1523 1.5 in NPSH 135 15/16\" bore size(s) 100 (Std) BLACK (Std) PG","15234008","SBJT 1.5NPSH 15/16D",65]
["15234010","SBJT 65MM JIM 3/4D",null,null,null,null,null,null,null,null,"0048","SABER JET NOZZLE","A",2.5,"JIM","GPM",135,"PSI","3/4\"",100,"BLACK","N","ENGLISH","Saber","Mid-Range","N",20,1,"1523","N/A","N/A",null,null,"1523 2.5 in JIM 135 3/4\" bore size(s) 100 (Std) BLACK (Std) PG","15234010","SBJT 65MM JIM 3/4D",62]
["15234002","SBJT 1.5NH 1D",null,null,null,null,null,null,null,null,"0048","SABER JET NOZZLE","A",1.5,"NH","GPM",135,"PSI","1\"",100,"BLACK","N","ENGLISH","Saber","Mid-Range","N",20,2,"1523","N/A","N/A",null,null,"1523 1.5 in NH 135 1\" bore size(s) 100 (Std) BLACK (Std) PG","15234002","SBJT 1.5NH 1D",59]
["15234003","SBJT 1.5NH 3/4D",null,null,null,null,null,null,null,null,"0048","SABER JET NOZZLE","A",1.5,"NH","GPM",135,"PSI","3/4\"",100,"BLACK","N","ENGLISH","Saber","Mid-Range","N",20,2,"1523","N/A","N/A",null,null,"1523 1.5 in NH 135 3/4\" bore size(s) 100 (Std) BLACK (Std) PG","15234003","SBJT 1.5NH 3/4D",61]
["15234004","SBJT 1.5NH 7/8D",null,null,null,null,null,null,null,null,"0048","SABER JET NOZZLE","A",1.5,"NH","GPM",135,"PSI","7/8\"",100,"BLACK","N","ENGLISH","Saber","Mid-Range","N",20,2,"1523","N/A","N/A",null,null,"1523 1.5 in NH 135 7/8\" bore size(s) 100 (Std) BLACK (Std) PG","15234004","SBJT 1.5NH 7/8D",61]
["15234007","SBJT 1.5NPSH 7/8D",null,null,null,null,null,null,null,null,"0048","SABER JET NOZZLE","A",1.5,"NPSH","GPM",135,"PSI","7/8\"",100,"BLACK","N","ENGLISH","Saber","Mid-Range","N",20,2,"1523","N/A","N/A",null,null,"1523 1.5 in NPSH 135 7/8\" bore size(s) 100 (Std) BLACK (Std) PG","15234007","SBJT 1.5NPSH 7/8D",63]
["15234020","SBJT 1.5BSP 1D",null,null,null,null,null,null,null,null,"0048","SABER JET NOZZLE","A",1.5,"BSP","GPM",135,"PSI","1\"",100,"BLACK","N","ENGLISH","Saber","Mid-Range","N",20,2,"1523","N/A","N/A",null,null,"1523 1.5 in BSP 135 1\" bore size(s) 100 (Std) BLACK (Std) PG","15234020","SBJT 1.5BSP 1D",60]
["15234026","SBJT 1.5BSP 15/16D",null,null,null,null,null,null,null,null,"0048","SABER JET NOZZLE","A",1.5,"BSP","GPM",135,"PSI","15/16\"",100,"BLACK","N","ENGLISH","Saber","Mid-Range","N",20,2,"1523","N/A","N/A",null,null,"1523 1.5 in BSP 135 15/16\" bore size(s) 100 (Std) BLACK (Std) PG","15234026","SBJT 1.5BSP 15/16D",64]
["15234027","SBJT 38MM 15/16D",null,null,null,null,null,null,null,null,"0048","SABER JET NOZZLE","A",1.5,"STORZ","GPM",135,"PSI","15/16\"",100,"BLACK","N","ENGLISH","Saber","Mid-Range","N",20,2,"1523","N/A","N/A",null,null,"1523 1.5 in STORZ 135 15/16\" bore size(s) 100 (Std) BLACK (Std) PG","15234027","SBJT 38MM 15/16D",66]
["15234021","SBJT 1.5NPSH 3/4D",null,null,null,null,null,null,null,null,"0048","SABER JET NOZZLE","A",1.5,"NPSH","GPM",135,"PSI","3/4\"",100,"BLACK","N","ENGLISH","Saber","Mid-Range","N",20,3,"1523","N/A","N/A",null,null,"1523 1.5 in NPSH 135 3/4\" bore size(s) 100 (Std) BLACK (Std) PG","15234021","SBJT 1.5NPSH 3/4D",63]
["15234001","SBJT 1.5BSP 3/4D",null,null,null,null,null,null,null,null,"0048","SABER JET NOZZLE","A",1.5,"BSP","GPM",135,"PSI","3/4\"",100,"BLACK","N","ENGLISH","Saber","Mid-Range","N","No 2021 Sales","No 2021 Sales","1523","N/A","N/A",null,null,"1523 1.5 in BSP 135 3/4\" bore size(s) 100 (Std) BLACK (Std) PG","15234001","SBJT 1.5BSP 3/4D",62]
["15234006","SBJT 1.5NPSH 1D",null,null,null,null,null,null,null,null,"0048","SABER JET NOZZLE","A",1.5,"NPSH","GPM",135,"PSI","1\"",100,"BLACK","N","ENGLISH","Saber","Mid-Range","N","No 2021 Sales","No 2021 Sales","1523","N/A","N/A",null,null,"1523 1.5 in NPSH 135 1\" bore size(s) 100 (Std) BLACK (Std) PG","15234006","SBJT 1.5NPSH 1D",61]
["15234009","SBJT 2.5BIM 7/8D",null,null,null,null,null,null,null,null,"0048","SABER JET NOZZLE","A",2.5,"BIM","GPM",135,"PSI","7/8\"",100,"BLACK","N","ENGLISH","Saber","Mid-Range","N","No 2021 Sales","No 2021 Sales","1523","N/A","N/A",null,null,"1523 2.5 in BIM 135 7/8\" bore size(s) 100 (Std) BLACK (Std) PG","15234009","SBJT 2.5BIM 7/8D",62]
["15234022","SBJT ZT 65MM JIM 1D",null,null,null,null,null,null,null,null,"0048","SABER JET NOZZLE","A",2.5,"JIM","GPM",135,"PSI","1\"",100,"BLACK","N","ENGLISH","Saber","Mid-Range","N","No 2021 Sales","No 2021 Sales","1523","N/A","N/A","Y",null,"1523 2.5 in JIM 135 1\" bore size(s) 100 (Std) BLACK (Std) PG ZT","15234022","SBJT ZT 65MM JIM 1D",63]
["15234023","SBJT 2.5NH 1D",null,null,null,null,null,null,null,null,"0048","SABER JET NOZZLE","A",2.5,"NH","GPM",135,"PSI","1\"",100,"BLACK","N","ENGLISH","Saber","Mid-Range","N","No 2021 Sales","No 2021 Sales","1523","N/A","N/A",null,null,"1523 2.5 in NH 135 1\" bore size(s) 100 (Std) BLACK (Std) PG","15234023","SBJT 2.5NH 1D",59]
["15234025","SBJT 2.5BIM 1D",null,null,null,null,null,null,null,null,"0048","SABER JET NOZZLE","A",2.5,"BIM","GPM",135,"PSI","1\"",100,"BLACK","N","ENGLISH","Saber","Mid-Range","N","No 2021 Sales","No 2021 Sales","1523","N/A","N/A",null,null,"1523 2.5 in BIM 135 1\" bore size(s) 100 (Std) BLACK (Std) PG","15234025","SBJT 2.5BIM 1D",60]
["15234028","SBJT ZT 1.5NH 15/16D",null,null,null,null,null,null,null,null,"0048","SABER JET NOZZLE","A",2.5,"NH","GPM",135,"PSI","15/16\"",100,"BLACK","N","ENGLISH","Saber","Mid-Range","N","No 2021 Sales","No 2021 Sales","1523","N/A","N/A","Y",null,"1523 2.5 in NH 135 15/16\" bore size(s) 100 (Std) BLACK (Std) PG ZT","15234028","SBJT ZT 1.5NH 15/16D",66]
["15234029","SBJT 2.5BIM 3/4D",null,null,null,null,null,null,null,null,"0048","SABER JET NOZZLE","A",2.5,"BIM","GPM",135,"PSI","3/4\"",100,"BLACK","N","ENGLISH","Saber","Mid-Range","N","No 2021 Sales","No 2021 Sales","1523","N/A","N/A",null,null,"1523 2.5 in BIM 135 3/4\" bore size(s) 100 (Std) BLACK (Std) PG","15234029","SBJT 2.5BIM 3/4D",62]
["15237005","OBS SBJT NPG 1.5NH 15/16D",null,null,null,null,null,null,null,null,"0048","SABER JET NOZZLE","O",1.5,"NH","GPM",135,"PSI","15/16\"",100,"BLACK","N","ENGLISH","Saber","Mid-Range","Y",20,3,"1523","N/A","N/A",null,null,"1523 1.5 in NH 135 15/16\" bore size(s) 100 (Std) BLACK (Std) NPG","15237005","OBS SBJT NPG 1.5NH 15/16D",64]
["15284008","SBJT 2.5NH 1-1/8D",null,null,null,null,null,null,null,null,"0048","SABER JET NOZZLE","A",2.5,"NH","GPM",135,"PSI","1-1/8\"",100,"BLACK","N","ENGLISH","Saber","High-Range","N",20,1,"1528","N/A","N/A",null,null,"1528 2.5 in NH 135 1-1/8\" bore size(s) 100 (Std) BLACK (Std) PG","15284008","SBJT 2.5NH 1-1/8D",63]
["15284002","SBJT 1.5NH 1-1/8D",null,null,null,null,null,null,null,null,"0048","SABER JET NOZZLE","A",1.5,"NH","GPM",135,"PSI","1-1/8\"",100,"BLACK","N","ENGLISH","Saber","High-Range","N",20,2,"1528","N/A","N/A",null,null,"1528 1.5 in NH 135 1-1/8\" bore size(s) 100 (Std) BLACK (Std) PG","15284002","SBJT 1.5NH 1-1/8D",63]
["15284003","SBJT 1.5NPSH 1-1/8D",null,null,null,null,null,null,null,null,"0048","SABER JET NOZZLE","A",1.5,"NPSH","GPM",135,"PSI","1-1/8\"",100,"BLACK","N","ENGLISH","Saber","High-Range","N",20,2,"1528","N/A","N/A",null,null,"1528 1.5 in NPSH 135 1-1/8\" bore size(s) 100 (Std) BLACK (Std) PG","15284003","SBJT 1.5NPSH 1-1/8D",65]
["15284004","SBJT 2.5BAF 1-1/8D",null,null,null,null,null,null,null,null,"0048","SABER JET NOZZLE","A",2.5,"BAT","GPM",135,"PSI","1-1/8\"",100,"BLACK","N","ENGLISH","Saber","High-Range","N",20,2,"1528","N/A","N/A",null,null,"1528 2.5 in BAT 135 1-1/8\" bore size(s) 100 (Std) BLACK (Std) PG","15284004","SBJT 2.5BAF 1-1/8D",64]
["15284005","SBJT 2.5BIM 1-1/8D",null,null,null,null,null,null,null,null,"0048","SABER JET NOZZLE","A",2.5,"BIM","GPM",135,"PSI","1-1/8\"",100,"BLACK","N","ENGLISH","Saber","High-Range","N",20,2,"1528","N/A","N/A",null,null,"1528 2.5 in BIM 135 1-1/8\" bore size(s) 100 (Std) BLACK (Std) PG","15284005","SBJT 2.5BIM 1-1/8D",64]
["15284016","SBJT 75MM 1-1/8D",null,null,null,null,null,null,null,null,"0048","SABER JET NOZZLE","A",3,"STORZ","GPM",135,"PSI","1-1/8\"",100,"BLACK","N","ENGLISH","Saber","High-Range","N",20,2,"1528","N/A","N/A",null,null,"1528 3 in STORZ 135 1-1/8\" bore size(s) 100 (Std) BLACK (Std) PG","15284016","SBJT 75MM 1-1/8D",64]
["15284015","SBJT 2.5AEA 1-1/8D",null,null,null,null,null,null,null,null,"0048","SABER JET NOZZLE","A",2.5,"AEA","GPM",135,"PSI","1-1/8\"",100,"BLACK","N","ENGLISH","Saber","High-Range","N",20,3,"1528","N/A","N/A",null,null,"1528 2.5 in AEA 135 1-1/8\" bore size(s) 100 (Std) BLACK (Std) PG","15284015","SBJT 2.5AEA 1-1/8D",64]
["15284014","SBJT 2.5NPSH 1-1/8D",null,null,null,null,null,null,null,null,"0048","SABER JET NOZZLE","A",2.5,"NPSH","GPM",135,"PSI","1-1/8\"",100,"BLACK","N","ENGLISH","Saber","High-Range","N",20,4,"1528","N/A","N/A",null,null,"1528 2.5 in NPSH 135 1-1/8\" bore size(s) 100 (Std) BLACK (Std) PG","15284014","SBJT 2.5NPSH 1-1/8D",65]
["15284001","SBJT 1.5BSP 1-1/8D",null,null,null,null,null,null,null,null,"0048","SABER JET NOZZLE","A",1.5,"BSP","GPM",135,"PSI","1-1/8\"",100,"BLACK","N","ENGLISH","Saber","High-Range","N","No 2021 Sales","No 2021 Sales","1528","N/A","N/A",null,null,"1528 1.5 in BSP 135 1-1/8\" bore size(s) 100 (Std) BLACK (Std) PG","15284001","SBJT 1.5BSP 1-1/8D",64]
["15284006","SBJT 2.5BSP 1-1/8D",null,null,null,null,null,null,null,null,"0048","SABER JET NOZZLE","A",2.5,"BSP","GPM",135,"PSI","1-1/8\"",100,"BLACK","N","ENGLISH","Saber","High-Range","N","No 2021 Sales","No 2021 Sales","1528","N/A","N/A",null,null,"1528 2.5 in BSP 135 1-1/8\" bore size(s) 100 (Std) BLACK (Std) PG","15284006","SBJT 2.5BSP 1-1/8D",64]
["15284007","SBJT 2.5JIM 1-1/8D",null,null,null,null,null,null,null,null,"0048","SABER JET NOZZLE","A",2.5,"JIM","GPM",135,"PSI","1-1/8\"",100,"BLACK","N","ENGLISH","Saber","High-Range","N","No 2021 Sales","No 2021 Sales","1528","N/A","N/A",null,null,"1528 2.5 in JIM 135 1-1/8\" bore size(s) 100 (Std) BLACK (Std) PG","15284007","SBJT 2.5JIM 1-1/8D",64]
["15284012","SBJT ZT 1.5NH 1-1/8D",null,null,null,null,null,null,null,null,"0048","SABER JET NOZZLE","A",1.5,"NH","GPM",135,"PSI","1-1/8\"",100,"BLACK","N","ENGLISH","Saber","High-Range","N","No 2021 Sales","No 2021 Sales","1528","N/A","N/A","Y",null,"1528 1.5 in NH 135 1-1/8\" bore size(s) 100 (Std) BLACK (Std) PG ZT","15284012","SBJT ZT 1.5NH 1-1/8D",66]
["15284013","SBJT 52MM 1-1/8D",null,null,null,null,null,null,null,null,"0048","SABER JET NOZZLE","A",2,"STORZ","GPM",135,"PSI","1-1/8\"",100,"BLACK","N","ENGLISH","Saber","High-Range","N","No 2021 Sales","No 2021 Sales","1528","N/A","N/A",null,null,"1528 2 in STORZ 135 1-1/8\" bore size(s) 100 (Std) BLACK (Std) PG","15284013","SBJT 52MM 1-1/8D",64]
["15284017","SBJT 2.5AEA 1-1/8D SPC AMA",null,null,null,null,null,null,null,null,"0048","SABER JET NOZZLE","A",2.5,"AEA","GPM",135,"PSI","1-1/8\"",100,"BLACK","N","ENGLISH","Saber","High-Range","N","No 2021 Sales","No 2021 Sales","1528","N/A","N/A",null,null,"1528 2.5 in AEA 135 1-1/8\" bore size(s) 100 (Std) BLACK (Std) PG","15284017","SBJT 2.5AEA 1-1/8D SPC AMA",64]
["16024005","PROVENGER 1.0\"NH 5-40G@75P",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",1,"NH","GPM","5-40","PSI","N/A",75,"BLACK","N","ENGLISH","Selectable","1\"","N",80,1,"1602","N/A","N/A",null,null,"1602 1 in NH 5-40 75 BLACK (Std) PG","16024005","PROVENGER 1.0\"NH 5-40G@75P",35]
["16024006","PROVENGER 1.0\"NH 5-40G@100P#",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",1,"NH","GPM","5-40","PSI","N/A",100,"BLACK","N","ENGLISH","Selectable","1\"","N",80,1,"1602","N/A","N/A",null,null,"1602 1 in NH 5-40 100 (Std) BLACK (Std) PG","16024006","PROVENGER 1.0\"NH 5-40G@100P#",42]
["16024003","PROVENGER 1.0\"BSP 19-150LPM@7b",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",1,"BSP","LPM","19-50","BAR","N/A",7,"BLACK","N","ENGLISH","Selectable","1\"","N",20,1,"1602","N/A","N/A",null,null,"1602 1 in BSP 19-50 7 BLACK (Std) PG","16024003","PROVENGER 1.0\"BSP 19-150LPM@7b",36]
["16025001","PROVENGER 1\"NH 45-200L@6b CCCF",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",1,"NH","LPM","45-200","BAR","N/A",7,"BLACK","CCCF","CHINESE","Selectable","1\"","N",20,1,"1602","N/A","N/A",null,null,"1602 1 in NH 45-200 7 BLACK (Std) PG ETCH","16025001","PROVENGER 1\"NH 45-200L@6b CCCF",41]
["16024002","PROVENGER 1.0\"BSP 19-150LPM@6b EN",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",1,"BSP","LPM","19-150","BAR","N/A",6,"BLACK","N","ENGLISH","Selectable","1\"","N",20,2,"1602","N/A","N/A",null,null,"1602 1 in BSP 19-150 6 BLACK (Std) PG","16024002","PROVENGER 1.0\"BSP 19-150LPM@6b EN",37]
["16024007","PROVENGER 1.0\"NPSH 5-40G@100P",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",1,"NPSH","GPM","5-40","PSI","N/A",100,"BLACK","N","ENGLISH","Selectable","1\"","N",20,2,"1602","N/A","N/A",null,null,"1602 1 in NPSH 5-40 100 (Std) BLACK (Std) PG","16024007","PROVENGER 1.0\"NPSH 5-40G@100P",44]
["16024004","PROVENGER 1.0\"BSP 45-200LPM@6b EN",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",1,"BSP","LPM","45-200","BAR","N/A",6,"BLACK","N","ENGLISH","Selectable","1\"","N",20,3,"1602","N/A","N/A",null,null,"1602 1 in BSP 45-200 6 BLACK (Std) PG","16024004","PROVENGER 1.0\"BSP 45-200LPM@6b EN",37]
["16024009","PROVENGER 1.0\"NH 12-53G@87P",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",1,"NH","GPM","12-53","PSI","N/A",87,"BLACK","N","ENGLISH","Selectable","1\"","N",20,3,"1602","N/A","N/A",null,null,"1602 1 in NH 12-53 87 (CE) BLACK (Std) PG","16024009","PROVENGER 1.0\"NH 12-53G@87P",41]
["16024010","PROVENGER 1.0\"NPSH 5-40G@75P",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",1,"NPSH","GPM","5-40","PSI","N/A",75,"BLACK","N","ENGLISH","Selectable","1\"","N",20,3,"1602","N/A","N/A",null,null,{"$f":"CONCATENATE(AC1075,\" \",N1075,\" in \",O1075,\" \",IF(AD1075=\"n/a\",\"\",CONCATENATE(AD1075,\" in \",AE1075,\" \")),IF(Q1075=\"n/a\",\"\",Q1075),IF(S1075=\"n/a\",\"\",CONCATENATE(IF(X1075=\"saber\",\" \",\"\"),S1075,\" bore size(s) \")),IF(T1075=\"n/a\",\"\",CONCATENATE(IF(X1075=\"saber\",\"\",\" \"),T1075,IF(T1075=100,\" (Std) \",IF(T1075=87,\" (CE) \",\" \")))),IF(U1075=\"n/a\",\"\",CONCATENATE(U1075,IF(U1075=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X1075,3)=\"tip\",IF(LEFT(X1075,1)=\"s\",\"\",IF(Z1075=\"n\",IF(T1075=\"N/A\",\"PG\",\" PG\"),IF(Z1075=\"y\",IF(T1075=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z1075=\"n\",IF(T1075=\"N/A\",\"PG\",\" PG\"),IF(Z1075=\"y\",IF(T1075=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF1075=\"y\",\" ZT\",\"\"),IF(V1075=\"N\",\"\",IF(S1075=\"n/a\",\" ETCH\",IF(T1075=\"N/A\",IF(RIGHT(X1075,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X1075=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"1602 1 in NPSH 5-40 75 BLACK (Std) PG"},{"$f":"A1075","v":"16024010"},{"$f":"B1075","v":"PROVENGER 1.0\"NPSH 5-40G@75P"},{"$f":"LEN(AH1075)","v":37}]
["16024011","PROVENGER 1.0\"NH 45-200LPM@6b",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",1,"NH","LPM","45-200","BAR","N/A",6,"BLACK","N","ENGLISH","Selectable","1\"","N",20,3,"1602","N/A","N/A",null,null,"1602 1 in NH 45-200 6 BLACK (Std) PG","16024011","PROVENGER 1.0\"NH 45-200LPM@6b",36]
["16027005","OBS PROVENGER NPG 1.0\"NH 5-40G@75P",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","O",1,"NH","GPM","5-40","PSI","N/A",75,"BLACK","N","ENGLISH","Selectable","1\"","Y",20,3,"1602","N/A","N/A",null,null,"1602 1 in NH 5-40 75 BLACK (Std) NPG","16027005","OBS PROVENGER NPG 1.0\"NH 5-40G@75P",36]
["16164003","PROVENGER 1.5BSP 115-550L@7b FM",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",1.5,"BSP","LPM","115-550","BAR","N/A",7,"BLACK","N","ENGLISH","Selectable","1.5\"","N",80,1,"1616","N/A","N/A",null,null,"1616 1.5 in BSP 115-550 7 BLACK (Std) PG","16164003","PROVENGER 1.5BSP 115-550L@7b FM",40]
["16164004","PROVENGER 1.5NH 30-150G@75P FM#",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",1.5,"NH","GPM","30-150","PSI","N/A",75,"BLACK","N","ENGLISH","Selectable","1.5\"","N",80,1,"1616","N/A","N/A",null,null,"1616 1.5 in NH 30-150 75 BLACK (Std) PG","16164004","PROVENGER 1.5NH 30-150G@75P FM#",39]
["16164006","PROVENGER 1.5NH 30-150G@100P FM#",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",1.5,"NH","GPM","30-150","PSI","N/A",100,"BLACK","N","ENGLISH","Selectable","1.5\"","N",80,1,"1616","N/A","N/A",null,null,"1616 1.5 in NH 30-150 100 (Std) BLACK (Std) PG","16164006","PROVENGER 1.5NH 30-150G@100P FM#",46]
["16164009","PROVENGER 1.5NPSH 30-150G@100P FM",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",1.5,"NPSH","GPM","30-150","PSI","N/A",100,"BLACK","N","ENGLISH","Selectable","1.5\"","N",80,1,"1616","N/A","N/A",null,null,"1616 1.5 in NPSH 30-150 100 (Std) BLACK (Std) PG","16164009","PROVENGER 1.5NPSH 30-150G@100P FM",48]
["16164012","PROVENGER 2.5NH 30-150G@100P FM",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",2.5,"NH","GPM","30-150","PSI","N/A",100,"BLACK","N","ENGLISH","Selectable","1.5\"","N",80,1,"1616","N/A","N/A",null,null,"1616 2.5 in NH 30-150 100 (Std) BLACK (Std) PG","16164012","PROVENGER 2.5NH 30-150G@100P FM",46]
["16164029","PROVENGER 1.5BSP 115-550L@6b EN",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",1.5,"BSP","LPM","115-550","BAR","N/A",6,"BLACK","N","ENGLISH","Selectable","1.5\"","N",80,1,"1616","N/A","N/A",null,null,"1616 1.5 in BSP 115-550 6 BLACK (Std) PG","16164029","PROVENGER 1.5BSP 115-550L@6b EN",40]
["16164019","PROVENGER 38MM 30-150G@100P FM",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",1.5,"STORZ","GPM","30-150","PSI","N/A",100,"BLACK","N","ENGLISH","Selectable","1.5\"","N",20,1,"1616","N/A","N/A",null,null,"1616 1.5 in STORZ 30-150 100 (Std) BLACK (Std) PG","16164019","PROVENGER 38MM 30-150G@100P FM",49]
["16164033","PROVENGER 52MM 115-550L@7b",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",2,"STORZ","LPM","115-550","BAR","N/A",7,"BLACK","N","ENGLISH","Selectable","1.5\"","N",20,1,"1616","N/A","N/A",null,null,"1616 2 in STORZ 115-550 7 BLACK (Std) PG","16164033","PROVENGER 52MM 115-550L@7b",40]
["16165003","PROVENGER 1.5 NH PG 115-550L@5b CCCF",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",1.5,"NH","LPM","115-550","BAR","N/A",5,"BLACK","CCCF","CHINESE","Selectable","1.5\"","N",20,1,"1616","N/A","N/A",null,null,"1616 1.5 in NH 115-550 5 BLACK (Std) PG ETCH","16165003","PROVENGER 1.5 NH PG 115-550L@5b CCCF",44]
["16164007","PROVENGER 1.5NH 115-550L@7b FM",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",1.5,"NH","LPM","115-550","BAR","N/A",7,"BLACK","N","ENGLISH","Selectable","1.5\"","N",20,2,"1616","N/A","N/A",null,null,"1616 1.5 in NH 115-550 7 BLACK (Std) PG","16164007","PROVENGER 1.5NH 115-550L@7b FM",39]
["16164008","PROVENGER 1.5NPSH 30-150G@75P FM",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",1.5,"NPSH","GPM","30-150","PSI","N/A",75,"BLACK","N","ENGLISH","Selectable","1.5\"","N",20,2,"1616","N/A","N/A",null,null,"1616 1.5 in NPSH 30-150 75 BLACK (Std) PG","16164008","PROVENGER 1.5NPSH 30-150G@75P FM",41]
["16164010","PROVENGER 2.5BIM 30-150G@100P FM",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",2.5,"BIM","GPM","30-150","PSI","N/A",100,"BLACK","N","ENGLISH","Selectable","1.5\"","N",20,2,"1616","N/A","N/A",null,null,"1616 2.5 in BIM 30-150 100 (Std) BLACK (Std) PG","16164010","PROVENGER 2.5BIM 30-150G@100P FM",47]
["16164011","PROVENGER 2.5BIM 115-550L@7b FM",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",2.5,"BIM","LPM","115-550","BAR","N/A",7,"BLACK","N","ENGLISH","Selectable","1.5\"","N",20,2,"1616","N/A","N/A",null,null,"1616 2.5 in BIM 115-550 7 BLACK (Std) PG","16164011","PROVENGER 2.5BIM 115-550L@7b FM",40]
["16164013","PROVENGER 2.5NH 285-750L@7b FM",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",2.5,"NH","LPM","285-750","BAR","N/A",7,"BLACK","N","ENGLISH","Selectable","1.5\"","N",20,2,"1616","N/A","N/A",null,null,{"$f":"CONCATENATE(AC1091,\" \",N1091,\" in \",O1091,\" \",IF(AD1091=\"n/a\",\"\",CONCATENATE(AD1091,\" in \",AE1091,\" \")),IF(Q1091=\"n/a\",\"\",Q1091),IF(S1091=\"n/a\",\"\",CONCATENATE(IF(X1091=\"saber\",\" \",\"\"),S1091,\" bore size(s) \")),IF(T1091=\"n/a\",\"\",CONCATENATE(IF(X1091=\"saber\",\"\",\" \"),T1091,IF(T1091=100,\" (Std) \",IF(T1091=87,\" (CE) \",\" \")))),IF(U1091=\"n/a\",\"\",CONCATENATE(U1091,IF(U1091=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X1091,3)=\"tip\",IF(LEFT(X1091,1)=\"s\",\"\",IF(Z1091=\"n\",IF(T1091=\"N/A\",\"PG\",\" PG\"),IF(Z1091=\"y\",IF(T1091=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z1091=\"n\",IF(T1091=\"N/A\",\"PG\",\" PG\"),IF(Z1091=\"y\",IF(T1091=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF1091=\"y\",\" ZT\",\"\"),IF(V1091=\"N\",\"\",IF(S1091=\"n/a\",\" ETCH\",IF(T1091=\"N/A\",IF(RIGHT(X1091,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X1091=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"1616 2.5 in NH 285-750 7 BLACK (Std) PG"},{"$f":"A1091","v":"16164013"},{"$f":"B1091","v":"PROVENGER 2.5NH 285-750L@7b FM"},{"$f":"LEN(AH1091)","v":39}]
["16164018","PROVENGER 2.5BIM 115-550L@6b EN",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",2.5,"BIM","LPM","115-550","BAR","N/A",6,"BLACK","N","ENGLISH","Selectable","1.5\"","N",20,2,"1616","N/A","N/A",null,null,"1616 2.5 in BIM 115-550 6 BLACK (Std) PG","16164018","PROVENGER 2.5BIM 115-550L@6b EN",40]
["16164034","PROVENGER 75MM STORZ 115-550L@7b FM",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",3,"STORZ","LPM","115-550","BAR","N/A",7,"BLACK","N","ENGLISH","Selectable","1.5\"","N",20,2,"1616","N/A","N/A",null,null,"1616 3 in STORZ 115-550 7 BLACK (Std) PG","16164034","PROVENGER 75MM STORZ 115-550L@7b FM",40]
["16164028","PROVENGER 2.5BAF 30-150G@100P FM",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",2.5,"BAT","GPM","30-150","PSI","N/A",100,"BLACK","N","ENGLISH","Selectable","1.5\"","N",20,3,"1616","N/A","N/A",null,null,"1616 2.5 in BAT 30-150 100 (Std) BLACK (Std) PG","16164028","PROVENGER 2.5BAF 30-150G@100P FM",47]
["16164031","PROVENGER 2.5AFD 30-150G@100P FM",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",2.5,"QST","GPM","30-150","PSI","N/A",100,"BLACK","N","ENGLISH","Selectable","1.5\"","N",20,3,"1616","N/A","N/A",null,null,"1616 2.5 in QST 30-150 100 (Std) BLACK (Std) PG","16164031","PROVENGER 2.5AFD 30-150G@100P FM",47]
["16164032","PROVENGER 1.5BSP 115-550L@5b",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",1.5,"BSP","LPM","115-550","BAR","N/A",5,"BLACK","N","ENGLISH","Selectable","1.5\"","N",20,3,"1616","N/A","N/A",null,null,"1616 1.5 in BSP 115-550 5 BLACK (Std) PG","16164032","PROVENGER 1.5BSP 115-550L@5b",40]
["16165004","PROVENGER JIM 65MM 115-550L@5b DINGLEE",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",2.5,"JIM","LPM","115-550","BAR","N/A",5,"BLACK","CCCF","CHINESE","Selectable","1.5\"","N",20,3,"1616","N/A","N/A",null,null,"1616 2.5 in JIM 115-550 5 BLACK (Std) PG ETCH","16165004","PROVENGER JIM 65MM 115-550L@5b DINGLEE",45]
["16165005","PROVENGER JIM 65MM 285-750L@5b DINGLEE",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",2.5,"JIM","LPM","285-750","BAR","N/A",5,"BLACK","CCCF","CHINESE","Selectable","1.5\"","N",20,3,"1616","N/A","N/A",null,null,"1616 2.5 in JIM 285-750 5 BLACK (Std) PG ETCH","16165005","PROVENGER JIM 65MM 285-750L@5b DINGLEE",45]
["16165006","PROVENGER 1.5NH 115-550L@7b DINGLEE",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",1.5,"NH","LPM","115-550","BAR","N/A",7,"BLACK","CCCF","CHINESE","Selectable","1.5\"","N",20,4,"1616","N/A","N/A",null,null,"1616 1.5 in NH 115-550 7 BLACK (Std) PG ETCH","16165006","PROVENGER 1.5NH 115-550L@7b DINGLEE",44]
["16165007","PROVENGER 2.5NH 285-750L@7b DINGLEE",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",2.5,"NH","LPM","285-750","BAR","N/A",7,"BLACK","CCCF","CHINESE","Selectable","1.5\"","N",20,4,"1616","N/A","N/A",null,null,"1616 2.5 in NH 285-750 7 BLACK (Std) PG ETCH","16165007","PROVENGER 2.5NH 285-750L@7b DINGLEE",44]
["16165008","PROVENGER 1.5NH 115-550L@5b DINGLEE",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",1.5,"NH","LPM","115-550","BAR","N/A",5,"BLACK","CCCF","CHINESE","Selectable","1.5\"","N",20,4,"1616","N/A","N/A",null,null,"1616 1.5 in NH 115-550 5 BLACK (Std) PG ETCH","16165008","PROVENGER 1.5NH 115-550L@5b DINGLEE",44]
["16164014","PROVENGER 2.5NH 30-150G@75P FM",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",2.5,"NH","GPM","30-150","PSI","N/A",75,"BLACK","N","ENGLISH","Selectable","1.5\"","N","No 2021 Sales","No 2021 Sales","1616","N/A","N/A",null,null,"1616 2.5 in NH 30-150 75 BLACK (Std) PG","16164014","PROVENGER 2.5NH 30-150G@75P FM",39]
["16164016","PROVENGER 1.5BIM 115-550L@6b FM/EN",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",1.5,"BIM","LPM","115-550","BAR","N/A",6,"BLACK","N","ENGLISH","Selectable","1.5\"","N","No 2021 Sales","No 2021 Sales","1616","N/A","N/A",null,null,"1616 1.5 in BIM 115-550 6 BLACK (Std) PG","16164016","PROVENGER 1.5BIM 115-550L@6b FM/EN",40]
["16164016","PROVENGER 1.5BSP 115-550L@5b",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",1.5,"BSP","LPM","115-550","BAR","N/A",5,"BLACK","N","ENGLISH","Selectable","1.5\"","N","No 2021 Sales","No 2021 Sales","1616","N/A","N/A",null,null,"1616 1.5 in BSP 115-550 5 BLACK (Std) PG","16164016","PROVENGER 1.5BSP 115-550L@5b",40]
["16164017","PROVENGER 2.5BIM 285-750L@7b FM",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",2.5,"BIM","LPM","285-750","BAR","N/A",7,"BLACK","N","ENGLISH","Selectable","1.5\"","N","No 2021 Sales","No 2021 Sales","1616","N/A","N/A",null,null,"1616 2.5 in BIM 285-750 7 BLACK (Std) PG","16164017","PROVENGER 2.5BIM 285-750L@7b FM",40]
["16164020","PROVENGER 2.5NH 115-550L@7b FM",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",2.5,"NH","LPM","115-550","BAR","N/A",7,"BLACK","N","ENGLISH","Selectable","1.5\"","N","No 2021 Sales","No 2021 Sales","1616","N/A","N/A",null,null,"1616 2.5 in NH 115-550 7 BLACK (Std) PG","16164020","PROVENGER 2.5NH 115-550L@7b FM",39]
["16164021","PROVENGER 52MM 30-150G@100P FM",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",2,"STORZ","GPM","30-150","PSI","N/A",100,"BLACK","N","ENGLISH","Selectable","1.5\"","N","No 2021 Sales","No 2021 Sales","1616","N/A","N/A",null,null,"1616 2 in STORZ 30-150 100 (Std) BLACK (Std) PG","16164021","PROVENGER 52MM 30-150G@100P FM",47]
["16164022","PROVENGER 1.5NH 30-150G@100P MTLTTH",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",1.5,"NH","GPM","30-150","PSI","N/A",100,"BLACK","N","ENGLISH","Selectable","1.5\"","N","No 2021 Sales","No 2021 Sales","1616","N/A","N/A",null,null,"1616 1.5 in NH 30-150 100 (Std) BLACK (Std) PG","16164022","PROVENGER 1.5NH 30-150G@100P MTLTTH",46]
["16164024","PROVENGER 38MM 115-550L@6b EN",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",1.5,"STORZ","LPM","115-550","BAR","N/A",6,"BLACK","N","ENGLISH","Selectable","1.5\"","N","No 2021 Sales","No 2021 Sales","1616","N/A","N/A",null,null,"1616 1.5 in STORZ 115-550 6 BLACK (Std) PG","16164024","PROVENGER 38MM 115-550L@6b EN",42]
["16164025","PROVENGER ZT 2.5BIM 115-550L@7b",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",2.5,"BIM","LPM","115-550","BAR","N/A",7,"BLACK","N","ENGLISH","Selectable","1.5\"","N","No 2021 Sales","No 2021 Sales","1616","N/A","N/A","Y",null,"1616 2.5 in BIM 115-550 7 BLACK (Std) PG ZT","16164025","PROVENGER ZT 2.5BIM 115-550L@7b",43]
["16164026","PROVENGER 65MM 30-150G@100P FM",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",2.5,"STORZ","GPM","30-150","PSI","N/A",100,"BLACK","N","ENGLISH","Selectable","1.5\"","N","No 2021 Sales","No 2021 Sales","1616","N/A","N/A",null,null,"1616 2.5 in STORZ 30-150 100 (Std) BLACK (Std) PG","16164026","PROVENGER 65MM 30-150G@100P FM",49]
["16164027","PROVENGER 2.5NH 30-150G@100P DARLEY",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","O",2.5,"NH","GPM","30-150","PSI","N/A",100,"BLACK","Y","ENGLISH","Selectable","1.5\"","N","No 2021 Sales","No 2021 Sales","1616","N/A","N/A",null,null,"1616 2.5 in NH 30-150 100 (Std) BLACK (Std) PG ETCH","16164027","PROVENGER 2.5NH 30-150G@100P DARLEY",51]
["16164030","PROVENGER 52MM 30-150G@100P FM",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","O",2,"STORZ","GPM","30-150","PSI","N/A",100,"BLACK","N","ENGLISH","Selectable","1.5\"","N","No 2021 Sales","No 2021 Sales","1616","N/A","N/A",null,null,"1616 2 in STORZ 30-150 100 (Std) BLACK (Std) PG","16164030","PROVENGER 52MM 30-150G@100P FM",47]
["16164035","PROVENGER 1.5ABX 30-150G@100P FM",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",1.5,"ABX","GPM","30-150","PSI","N/A",100,"BLACK","N","ENGLISH","Selectable","1.5\"","N","No 2021 Sales","No 2021 Sales","1616","N/A","N/A",null,null,"1616 1.5 in ABX 30-150 100 (Std) BLACK (Std) PG","16164035","PROVENGER 1.5ABX 30-150G@100P FM",47]
["16167009","OBS PROVENGER NPG 1.5NPSH 30-150G@100P",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","O",1.5,"NPSH","GPM","30-150","PSI","N/A",100,"BLACK","N","ENGLISH","Selectable","1.5\"","Y",20,3,"1616","N/A","N/A",null,null,"1616 1.5 in NPSH 30-150 100 (Std) BLACK (Std) NPG","16167009","OBS PROVENGER NPG 1.5NPSH 30-150G@100P",49]
["41164004","PROVENGER 1.5NH FIXED 150G@100P FM",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",1.5,"NH","GPM",150,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","1.5\"","N",80,1,"4116","N/A","N/A",null,null,"4116 1.5 in NH 150 100 (Std) BLACK (Std) PG","41164004","PROVENGER 1.5NH FIXED 150G@100P FM",43]
["41164002","PROVENGER 1.5NH FIXED 95G@100P FM",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",1.5,"NH","GPM",95,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","1.5\"","N",20,1,"4116","N/A","N/A",null,null,"4116 1.5 in NH 95 100 (Std) BLACK (Std) PG","41164002","PROVENGER 1.5NH FIXED 95G@100P FM",42]
["41164003","PROVENGER 1.5NH FIXED 150G@75P FM",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",1.5,"NH","GPM",150,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed","1.5\"","N",20,1,"4116","N/A","N/A",null,null,"4116 1.5 in NH 150 75 BLACK (Std) PG","41164003","PROVENGER 1.5NH FIXED 150G@75P FM",36]
["41164008","PROVENGER 2.5BIM FIXED 125G@100P FM",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",2.5,"BIM","GPM",125,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","1.5\"","N",20,1,"4116","N/A","N/A",null,null,"4116 2.5 in BIM 125 100 (Std) BLACK (Std) PG","41164008","PROVENGER 2.5BIM FIXED 125G@100P FM",44]
["41164009","PROVENGER 2.5BIM FIXED 550L@7b FM",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",2.5,"BIM","LPM",550,"BAR","N/A",7,"BLACK","N","ENGLISH","Fixed","1.5\"","N",20,1,"4116","N/A","N/A",null,null,"4116 2.5 in BIM 550 7 BLACK (Std) PG","41164009","PROVENGER 2.5BIM FIXED 550L@7b FM",36]
["41164014","PROVENGER 2.5BIM FIXED 95G@100P FM",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",2.5,"BIM","GPM",95,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","1.5\"","N",20,1,"4116","N/A","N/A",null,null,"4116 2.5 in BIM 95 100 (Std) BLACK (Std) PG","41164014","PROVENGER 2.5BIM FIXED 95G@100P FM",43]
["41164012","PROVENGER 2.5NH FIXED 150G@100P FM",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",2.5,"NH","GPM",150,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","1.5\"","N",20,2,"4116","N/A","N/A",null,null,"4116 2.5 in NH 150 100 (Std) BLACK (Std) PG","41164012","PROVENGER 2.5NH FIXED 150G@100P FM",43]
["41164013","PROVENGER 2.5BIM FIXED 150G@100P FM",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",2.5,"BIM","GPM",150,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","1.5\"","N",20,2,"4116","N/A","N/A",null,null,"4116 2.5 in BIM 150 100 (Std) BLACK (Std) PG","41164013","PROVENGER 2.5BIM FIXED 150G@100P FM",44]
["41164016","PROVENGER 1.5NH FIXED 125G@100P FM",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",1.5,"NH","GPM",125,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","1.5\"","N",20,2,"4116","N/A","N/A",null,null,"4116 1.5 in NH 125 100 (Std) BLACK (Std) PG","41164016","PROVENGER 1.5NH FIXED 125G@100P FM",43]
["41164019","PROVENGER 1.5NH FIXED 125G@75P FM",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",1.5,"NH","GPM",125,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed","1.5\"","N",20,2,"4116","N/A","N/A",null,null,"4116 1.5 in NH 125 75 BLACK (Std) PG","41164019","PROVENGER 1.5NH FIXED 125G@75P FM",36]
["41164024","PROVENGER 2.5NH FIXED 150G@75P FM",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",2.5,"NH","GPM",150,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed","1.5\"","N",20,2,"4116","N/A","N/A",null,null,"4116 2.5 in NH 150 75 BLACK (Std) PG","41164024","PROVENGER 2.5NH FIXED 150G@75P FM",36]
["41164001","PROVENGER 1.5NH FIXED 95G@75P FM",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",1.5,"NH","GPM",95,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed","1.5\"","N",20,3,"4116","N/A","N/A",null,null,"4116 1.5 in NH 95 75 BLACK (Std) PG","41164001","PROVENGER 1.5NH FIXED 95G@75P FM",35]
["41164006","PROVENGER 1.5NPSH FIXED 150G@75P FM",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",1.5,"NPSH","GPM",150,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed","1.5\"","N",20,3,"4116","N/A","N/A",null,null,"4116 1.5 in NPSH 150 75 BLACK (Std) PG","41164006","PROVENGER 1.5NPSH FIXED 150G@75P FM",38]
["41164011","PROVENGER 1.5NPSH FIXED 150G@100P FM",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",1.5,"NPSH","GPM",150,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","1.5\"","N",20,3,"4116","N/A","N/A",null,null,"4116 1.5 in NPSH 150 100 (Std) BLACK (Std) PG","41164011","PROVENGER 1.5NPSH FIXED 150G@100P FM",45]
["41164018","PROVENGER 2.5NH FIXED 125G@100P FM",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",2.5,"NH","GPM",125,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","1.5\"","N",20,3,"4116","N/A","N/A",null,null,"4116 2.5 in NH 125 100 (Std) BLACK (Std) PG","41164018","PROVENGER 2.5NH FIXED 125G@100P FM",43]
["41164021","PROVENGER 1.5NH FIXED 60G@75P FM",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",1.5,"NH","GPM",60,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed","1.5\"","N",20,3,"4116","N/A","N/A",null,null,"4116 1.5 in NH 60 75 BLACK (Std) PG","41164021","PROVENGER 1.5NH FIXED 60G@75P FM",35]
["41164027","PROVENGER 1.5NH FIXED 550L@6b FM",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",1.5,"NH","LPM",550,"BAR","N/A",6,"BLACK","N","ENGLISH","Fixed","1.5\"","N",20,3,"4116","N/A","N/A",null,null,"4116 1.5 in NH 550 6 BLACK (Std) PG","41164027","PROVENGER 1.5NH FIXED 550L@6b FM",35]
["41164010","PROVENGER 1.5BSP FIXED 550L@7b FM",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",1.5,"BSP","LPM",550,"BAR","N/A",7,"BLACK","N","ENGLISH","Fixed","1.5\"","N","No 2021 Sales","No 2021 Sales","4116","N/A","N/A",null,null,"4116 1.5 in BSP 550 7 BLACK (Std) PG","41164010","PROVENGER 1.5BSP FIXED 550L@7b FM",36]
["41164015","PROVENGER 1.5BSP FIXED 550L@6b FM",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",1.5,"BSP","LPM",550,"BAR","N/A",6,"BLACK","N","ENGLISH","Fixed","1.5\"","N","No 2021 Sales","No 2021 Sales","4116","N/A","N/A",null,null,"4116 1.5 in BSP 550 6 BLACK (Std) PG","41164015","PROVENGER 1.5BSP FIXED 550L@6b FM",36]
["41164017","PROVENGER 1.5NPSH FIXED 125G@100P FM",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",1.5,"NPSH","GPM",125,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","1.5\"","N","No 2021 Sales","No 2021 Sales","4116","N/A","N/A",null,null,"4116 1.5 in NPSH 125 100 (Std) BLACK (Std) PG","41164017","PROVENGER 1.5NPSH FIXED 125G@100P FM",45]
["41164020","PROVENGER 2.5NH FIXED 125G@75P FM",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",2.5,"NH","GPM",125,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed","1.5\"","N","No 2021 Sales","No 2021 Sales","4116","N/A","N/A",null,null,"4116 2.5 in NH 125 75 BLACK (Std) PG","41164020","PROVENGER 2.5NH FIXED 125G@75P FM",36]
["41164023","PROVENGER 1.5NPSH FIXED 500L@700k FM",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",1.5,"NPSH","LPM",500,"kPA","N/A",700,"BLACK","N","ENGLISH","Fixed","1.5\"","N","No 2021 Sales","No 2021 Sales","4116","N/A","N/A",null,null,"4116 1.5 in NPSH 500 700 BLACK (Std) PG","41164023","PROVENGER 1.5NPSH FIXED 500L@700k FM",39]
["41164025","PROVENGER 2.5BIM FIXED 230L@6b FM",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",1.5,"BSP","LPM",230,"BAR","N/A",6,"BLACK","N","ENGLISH","Fixed","1.5\"","N","No 2021 Sales","No 2021 Sales","4116","N/A","N/A",null,null,{"$f":"CONCATENATE(AC1138,\" \",N1138,\" in \",O1138,\" \",IF(AD1138=\"n/a\",\"\",CONCATENATE(AD1138,\" in \",AE1138,\" \")),IF(Q1138=\"n/a\",\"\",Q1138),IF(S1138=\"n/a\",\"\",CONCATENATE(IF(X1138=\"saber\",\" \",\"\"),S1138,\" bore size(s) \")),IF(T1138=\"n/a\",\"\",CONCATENATE(IF(X1138=\"saber\",\"\",\" \"),T1138,IF(T1138=100,\" (Std) \",IF(T1138=87,\" (CE) \",\" \")))),IF(U1138=\"n/a\",\"\",CONCATENATE(U1138,IF(U1138=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X1138,3)=\"tip\",IF(LEFT(X1138,1)=\"s\",\"\",IF(Z1138=\"n\",IF(T1138=\"N/A\",\"PG\",\" PG\"),IF(Z1138=\"y\",IF(T1138=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z1138=\"n\",IF(T1138=\"N/A\",\"PG\",\" PG\"),IF(Z1138=\"y\",IF(T1138=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF1138=\"y\",\" ZT\",\"\"),IF(V1138=\"N\",\"\",IF(S1138=\"n/a\",\" ETCH\",IF(T1138=\"N/A\",IF(RIGHT(X1138,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X1138=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"4116 1.5 in BSP 230 6 BLACK (Std) PG"},{"$f":"A1138","v":"41164025"},{"$f":"B1138","v":"PROVENGER 2.5BIM FIXED 230L@6b FM"},{"$f":"LEN(AH1138)","v":36}]
["41164025","PROVENGER 2.5BIM FIXED 230L@6b FM",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",2.5,"BIM","LPM",230,"BAR","N/A",6,"BLACK","N","ENGLISH","Fixed","1.5\"","N","No 2021 Sales","No 2021 Sales","4116","N/A","N/A",null,null,"4116 2.5 in BIM 230 6 BLACK (Std) PG","41164025","PROVENGER 2.5BIM FIXED 230L@6b FM",36]
["41167004","OBS PROVNGR NPG 1.5NH FIXED 150G@100P FM",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","O",1.5,"NH","GPM",150,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","1.5\"","Y",20,2,"4116","N/A","N/A",null,null,"4116 1.5 in NH 150 100 (Std) BLACK (Std) NPG","41167004","OBS PROVNGR NPG 1.5NH FIXED 150G@100P FM",44]
["41164005","OBS PROVENGER 1.5NH FIXED 175G@75P",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","O",1.5,"NH","GPM",175,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed","1.5\"","N",20,3,"4116","N/A","N/A",null,null,"4116 1.5 in NH 175 75 BLACK (Std) PG","41164005","OBS PROVENGER 1.5NH FIXED 175G@75P",36]
["18204001","ULTRAJET 1.5NH 3/4 TIP",null,null,null,null,null,null,null,null,"0097","Ultrajet Nozzle","A",1.5,"NH","GPM",118,"PSI","3/4\"",50,"Black","N","ENGLISH","Saber","Mid-Range","N",80,1,"1820","N/A","N/A",null,null,"1820 1.5 in NH 118 3/4\" bore size(s) 50 Black (Std) PG","18204001","ULTRAJET 1.5NH 3/4 TIP",54]
["18204003","ULTRAJET 1.5NH 15/16 TIP#",null,null,null,null,null,null,null,null,"0097","Ultrajet Nozzle","A",1.5,"NH","GPM",185,"PSI","15/16\"",50,"Black","N","ENGLISH","Saber","Mid-Range","N",80,1,"1820","N/A","N/A",null,null,"1820 1.5 in NH 185 15/16\" bore size(s) 50 Black (Std) PG","18204003","ULTRAJET 1.5NH 15/16 TIP#",56]
["18204004","ULTRAJET 1.5NH 1 TIP",null,null,null,null,null,null,null,null,"0097","Ultrajet Nozzle","A",1.5,"NH","GPM",210,"PSI","1\"",50,"Black","N","ENGLISH","Saber","Mid-Range","N",80,1,"1820","N/A","N/A",null,null,"1820 1.5 in NH 210 1\" bore size(s) 50 Black (Std) PG","18204004","ULTRAJET 1.5NH 1 TIP",52]
["18204006","ULTRAJET 1.5NPSH 7/8 TIP",null,null,null,null,null,null,null,null,"0097","Ultrajet Nozzle","A",1.5,"NPSH","GPM",161,"PSI","7/8\"",50,"Black","N","ENGLISH","Saber","Mid-Range","N",80,1,"1820","N/A","N/A",null,null,"1820 1.5 in NPSH 161 7/8\" bore size(s) 50 Black (Std) PG","18204006","ULTRAJET 1.5NPSH 7/8 TIP",56]
["18204009","ULTRAJET 2.5NH 1 TIP",null,null,null,null,null,null,null,null,"0097","Ultrajet Nozzle","A",2.5,"NH","GPM",210,"PSI","1\"",50,"Black","N","ENGLISH","Saber","Mid-Range","N",80,1,"1820","N/A","N/A",null,null,"1820 2.5 in NH 210 1\" bore size(s) 50 Black (Std) PG","18204009","ULTRAJET 2.5NH 1 TIP",52]
["18204002","ULTRAJET 1.5NH 7/8 TIP",null,null,null,null,null,null,null,null,"0097","Ultrajet Nozzle","A",1.5,"NH","GPM",161,"PSI","7/8\"",50,"Black","N","ENGLISH","Saber","Mid-Range","N",20,1,"1820","N/A","N/A",null,null,"1820 1.5 in NH 161 7/8\" bore size(s) 50 Black (Std) PG","18204002","ULTRAJET 1.5NH 7/8 TIP",54]
["18204007","ULTRAJET 1.5NPSH 15/16 TIP",null,null,null,null,null,null,null,null,"0097","Ultrajet Nozzle","A",1.5,"NPSH","GPM",185,"PSI","15/16\"",50,"Black","N","ENGLISH","Saber","Mid-Range","N",20,1,"1820","N/A","N/A",null,null,"1820 1.5 in NPSH 185 15/16\" bore size(s) 50 Black (Std) PG","18204007","ULTRAJET 1.5NPSH 15/16 TIP",58]
["18204014","ULTRAJET 2.5BIM 7/8 TIP",null,null,null,null,null,null,null,null,"0097","Ultrajet Nozzle","A",2.5,"BIM","GPM",161,"PSI","7/8\"",50,"BLACK","N","ENGLISH","Saber","Mid-Range","N",20,1,"1820","N/A","N/A",null,null,"1820 2.5 in BIM 161 7/8\" bore size(s) 50 BLACK (Std) PG","18204014","ULTRAJET 2.5BIM 7/8 TIP",55]
["18204005","ULTRAJET 1.5NPSH 3/4 TIP",null,null,null,null,null,null,null,null,"0097","Ultrajet Nozzle","A",1.5,"NPSH","GPM",118,"PSI","3/4\"",50,"Black","N","ENGLISH","Saber","Mid-Range","N",20,2,"1820","N/A","N/A",null,null,"1820 1.5 in NPSH 118 3/4\" bore size(s) 50 Black (Std) PG","18204005","ULTRAJET 1.5NPSH 3/4 TIP",56]
["18204008","ULTRAJET 2.5NH 15/16 TIP",null,null,null,null,null,null,null,null,"0097","Ultrajet Nozzle","A",2.5,"NH","GPM",185,"PSI","15/16\"",50,"BLACK","N","ENGLISH","Saber","Mid-Range","N",20,2,"1820","N/A","N/A",null,null,"1820 2.5 in NH 185 15/16\" bore size(s) 50 BLACK (Std) PG","18204008","ULTRAJET 2.5NH 15/16 TIP",56]
["18204021","ULTRAJET 1.5NPSH 1 TIP",null,null,null,null,null,null,null,null,"0097","Ultrajet Nozzle","A",1.5,"NPSH","GPM",210,"PSI","1\"",50,"Black","N","ENGLISH","Saber","Mid-Range","N",20,2,"1820","N/A","N/A",null,null,"1820 1.5 in NPSH 210 1\" bore size(s) 50 Black (Std) PG","18204021","ULTRAJET 1.5NPSH 1 TIP",54]
["18204028","ULTRAJET 2.5BAF  1 TIP",null,null,null,null,null,null,null,null,"0097","Ultrajet Nozzle","A",2.5,"BAT","GPM",210,"PSI","1\"",50,"BLACK","N","ENGLISH","Saber","Mid-Range","N",20,2,"1820","N/A","N/A",null,null,"1820 2.5 in BAT 210 1\" bore size(s) 50 BLACK (Std) PG","18204028","ULTRAJET 2.5BAF  1 TIP",53]
["18204029","ULTRAJET 2.5AII 7/8 TIP",null,null,null,null,null,null,null,null,"0097","Ultrajet Nozzle","A",2.5,"CSA","GPM",161,"PSI","7/8\"",50,"BLACK","N","ENGLISH","Saber","Mid-Range","N",20,2,"1820","N/A","N/A",null,null,"1820 2.5 in CSA 161 7/8\" bore size(s) 50 BLACK (Std) PG","18204029","ULTRAJET 2.5AII 7/8 TIP",55]
["18200004","OBS ULTRAJET 2.5 BIM 3/4 TIP W/PG CE",null,null,null,null,null,null,null,null,"0097","Ultrajet Nozzle","A",2.5,"BIM","GPM",118,"PSI","3/4\"",50,"BLACK","N","ENGLISH","Saber","Mid-Range","N","No 2021 Sales","No 2021 Sales","1820","N/A","N/A",null,null,"1820 2.5 in BIM 118 3/4\" bore size(s) 50 BLACK (Std) PG","18200004","OBS ULTRAJET 2.5 BIM 3/4 TIP W/PG CE",55]
["18204010","ULTRAJET 2.5BIM 3/4 TIP EN",null,null,null,null,null,null,null,null,"0097","Ultrajet Nozzle","A",2.5,"BIM","GPM",118,"PSI","3/4\"",50,"BLACK","N","ENGLISH","Saber","Mid-Range","N","No 2021 Sales","No 2021 Sales","1820","N/A","N/A",null,null,{"$f":"CONCATENATE(AC1156,\" \",N1156,\" in \",O1156,\" \",IF(AD1156=\"n/a\",\"\",CONCATENATE(AD1156,\" in \",AE1156,\" \")),IF(Q1156=\"n/a\",\"\",Q1156),IF(S1156=\"n/a\",\"\",CONCATENATE(IF(X1156=\"saber\",\" \",\"\"),S1156,\" bore size(s) \")),IF(T1156=\"n/a\",\"\",CONCATENATE(IF(X1156=\"saber\",\"\",\" \"),T1156,IF(T1156=100,\" (Std) \",IF(T1156=87,\" (CE) \",\" \")))),IF(U1156=\"n/a\",\"\",CONCATENATE(U1156,IF(U1156=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X1156,3)=\"tip\",IF(LEFT(X1156,1)=\"s\",\"\",IF(Z1156=\"n\",IF(T1156=\"N/A\",\"PG\",\" PG\"),IF(Z1156=\"y\",IF(T1156=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z1156=\"n\",IF(T1156=\"N/A\",\"PG\",\" PG\"),IF(Z1156=\"y\",IF(T1156=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF1156=\"y\",\" ZT\",\"\"),IF(V1156=\"N\",\"\",IF(S1156=\"n/a\",\" ETCH\",IF(T1156=\"N/A\",IF(RIGHT(X1156,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X1156=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"1820 2.5 in BIM 118 3/4\" bore size(s) 50 BLACK (Std) PG"},{"$f":"A1156","v":"18204010"},{"$f":"B1156","v":"ULTRAJET 2.5BIM 3/4 TIP EN"},{"$f":"LEN(AH1156)","v":55}]
["18204030","ULTRAJET 2.5BIM 15/16 TIP",null,null,null,null,null,null,null,null,"0097","Ultrajet Nozzle","A",2.5,"BIM","GPM",118,"PSI","15/16\"",50,"BLACK","N","ENGLISH","Saber","Mid-Range","N","No 2021 Sales","No 2021 Sales","1820","N/A","N/A",null,null,{"$f":"CONCATENATE(AC1157,\" \",N1157,\" in \",O1157,\" \",IF(AD1157=\"n/a\",\"\",CONCATENATE(AD1157,\" in \",AE1157,\" \")),IF(Q1157=\"n/a\",\"\",Q1157),IF(S1157=\"n/a\",\"\",CONCATENATE(IF(X1157=\"saber\",\" \",\"\"),S1157,\" bore size(s) \")),IF(T1157=\"n/a\",\"\",CONCATENATE(IF(X1157=\"saber\",\"\",\" \"),T1157,IF(T1157=100,\" (Std) \",IF(T1157=87,\" (CE) \",\" \")))),IF(U1157=\"n/a\",\"\",CONCATENATE(U1157,IF(U1157=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X1157,3)=\"tip\",IF(LEFT(X1157,1)=\"s\",\"\",IF(Z1157=\"n\",IF(T1157=\"N/A\",\"PG\",\" PG\"),IF(Z1157=\"y\",IF(T1157=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z1157=\"n\",IF(T1157=\"N/A\",\"PG\",\" PG\"),IF(Z1157=\"y\",IF(T1157=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF1157=\"y\",\" ZT\",\"\"),IF(V1157=\"N\",\"\",IF(S1157=\"n/a\",\" ETCH\",IF(T1157=\"N/A\",IF(RIGHT(X1157,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X1157=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"1820 2.5 in BIM 118 15/16\" bore size(s) 50 BLACK (Std) PG"},{"$f":"A1157","v":"18204030"},{"$f":"B1157","v":"ULTRAJET 2.5BIM 15/16 TIP"},{"$f":"LEN(AH1157)","v":57}]
["18204011","ULTRAJET 38MM STZ 7/8 TIP",null,null,null,null,null,null,null,null,"0097","Ultrajet Nozzle","A",1.5,"STORZ","GPM",161,"PSI","7/8\"",50,"BLACK","N","ENGLISH","Saber","Mid-Range","N","No 2021 Sales","No 2021 Sales","1820","N/A","N/A",null,null,"1820 1.5 in STORZ 161 7/8\" bore size(s) 50 BLACK (Std) PG","18204011","ULTRAJET 38MM STZ 7/8 TIP",57]
["18204012","ULTRAJET 65MM JIM 1 TIP",null,null,null,null,null,null,null,null,"0097","Ultrajet Nozzle","A",2.5,"JIM","GPM",210,"PSI","1\"",50,"BLACK","N","ENGLISH","Saber","Mid-Range","N","No 2021 Sales","No 2021 Sales","1820","N/A","N/A",null,null,"1820 2.5 in JIM 210 1\" bore size(s) 50 BLACK (Std) PG","18204012","ULTRAJET 65MM JIM 1 TIP",53]
["18204013","ULTRAJET 1.5BIM 3/4 TIP EN",null,null,null,null,null,null,null,null,"0097","Ultrajet Nozzle","A",1.5,"BIM","GPM",118,"PSI","3/4\"",50,"BLACK","N","ENGLISH","Saber","Mid-Range","N","No 2021 Sales","No 2021 Sales","1820","N/A","N/A",null,null,"1820 1.5 in BIM 118 3/4\" bore size(s) 50 BLACK (Std) PG","18204013","ULTRAJET 1.5BIM 3/4 TIP EN",55]
["18204015","ULTRAJET ZT 1.5NH 3/4 TIP",null,null,null,null,null,null,null,null,"0097","Ultrajet Nozzle","A",1.5,"NH","GPM",118,"PSI","3/4\"",50,"BLACK","N","ENGLISH","Saber","Mid-Range","N","No 2021 Sales","No 2021 Sales","1820","N/A","N/A","Y",null,{"$f":"CONCATENATE(AC1161,\" \",N1161,\" in \",O1161,\" \",IF(AD1161=\"n/a\",\"\",CONCATENATE(AD1161,\" in \",AE1161,\" \")),IF(Q1161=\"n/a\",\"\",Q1161),IF(S1161=\"n/a\",\"\",CONCATENATE(IF(X1161=\"saber\",\" \",\"\"),S1161,\" bore size(s) \")),IF(T1161=\"n/a\",\"\",CONCATENATE(IF(X1161=\"saber\",\"\",\" \"),T1161,IF(T1161=100,\" (Std) \",IF(T1161=87,\" (CE) \",\" \")))),IF(U1161=\"n/a\",\"\",CONCATENATE(U1161,IF(U1161=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X1161,3)=\"tip\",IF(LEFT(X1161,1)=\"s\",\"\",IF(Z1161=\"n\",IF(T1161=\"N/A\",\"PG\",\" PG\"),IF(Z1161=\"y\",IF(T1161=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z1161=\"n\",IF(T1161=\"N/A\",\"PG\",\" PG\"),IF(Z1161=\"y\",IF(T1161=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF1161=\"y\",\" ZT\",\"\"),IF(V1161=\"N\",\"\",IF(S1161=\"n/a\",\" ETCH\",IF(T1161=\"N/A\",IF(RIGHT(X1161,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X1161=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"1820 1.5 in NH 118 3/4\" bore size(s) 50 BLACK (Std) PG ZT"},{"$f":"A1161","v":"18204015"},{"$f":"B1161","v":"ULTRAJET ZT 1.5NH 3/4 TIP"},{"$f":"LEN(AH1161)","v":57}]
["18204031","ULTRAJET ZT 1.5NH 7/8 TIP",null,null,null,null,null,null,null,null,"0097","Ultrajet Nozzle","A",1.5,"NH","GPM",118,"PSI","7/8\"",50,"BLACK","N","ENGLISH","Saber","Mid-Range","N","No 2021 Sales","No 2021 Sales","1820","N/A","N/A","Y",null,"1820 1.5 in NH 118 7/8\" bore size(s) 50 BLACK (Std) PG ZT","18204031","ULTRAJET ZT 1.5NH 7/8 TIP",57]
["18204016","ULTRAJET ZT 2.5NH 1 TIP",null,null,null,null,null,null,null,null,"0097","Ultrajet Nozzle","A",2.5,"NH","GPM",210,"PSI","1\"",50,"BLACK","N","ENGLISH","Saber","Mid-Range","N","No 2021 Sales","No 2021 Sales","1820","N/A","N/A","Y",null,"1820 2.5 in NH 210 1\" bore size(s) 50 BLACK (Std) PG ZT","18204016","ULTRAJET ZT 2.5NH 1 TIP",55]
["18204017","ULTRAJET 2.5AFD 3/4 TIP",null,null,null,null,null,null,null,null,"0097","Ultrajet Nozzle","A",2.5,"QST","GPM",118,"PSI","3/4\"",50,"BLACK","N","ENGLISH","Saber","Mid-Range","N","No 2021 Sales","No 2021 Sales","1820","N/A","N/A",null,null,"1820 2.5 in QST 118 3/4\" bore size(s) 50 BLACK (Std) PG","18204017","ULTRAJET 2.5AFD 3/4 TIP",55]
["18204018","ULTRAJET 2.5AII 15/16 TIP",null,null,null,null,null,null,null,null,"0097","Ultrajet Nozzle","A",2.5,"CSA","GPM",185,"PSI","15/16\"",50,"Black","N","ENGLISH","Saber","Mid-Range","N","No 2021 Sales","No 2021 Sales","1820","N/A","N/A",null,null,"1820 2.5 in CSA 185 15/16\" bore size(s) 50 Black (Std) PG","18204018","ULTRAJET 2.5AII 15/16 TIP",57]
["18204020","ULTRAJET 2.5AKB 1 TIP",null,null,null,null,null,null,null,null,"0097","Ultrajet Nozzle","A",2.5,"AKB","GPM",210,"PSI","1\"",50,"Black","N","ENGLISH","Saber","Mid-Range","N","No 2021 Sales","No 2021 Sales","1820","N/A","N/A",null,null,"1820 2.5 in AKB 210 1\" bore size(s) 50 Black (Std) PG","18204020","ULTRAJET 2.5AKB 1 TIP",53]
["18204022","ULTRAJET 38MM 3/4 TIP EN",null,null,null,null,null,null,null,null,"0097","Ultrajet Nozzle","A",1.5,"STORZ","GPM",118,"PSI","3/4\"",50,"BLACK","N","ENGLISH","Saber","Mid-Range","N","No 2021 Sales","No 2021 Sales","1820","N/A","N/A",null,null,"1820 1.5 in STORZ 118 3/4\" bore size(s) 50 BLACK (Std) PG","18204022","ULTRAJET 38MM 3/4 TIP EN",57]
["18204023","ULTRAJET 2.5AII 3/4 TIP",null,null,null,null,null,null,null,null,"0097","Ultrajet Nozzle","A",2.5,"CSA","GPM",118,"PSI","3/4\"",50,"BLACK","N","ENGLISH","Saber","Mid-Range","N","No 2021 Sales","No 2021 Sales","1820","N/A","N/A",null,null,"1820 2.5 in CSA 118 3/4\" bore size(s) 50 BLACK (Std) PG","18204023","ULTRAJET 2.5AII 3/4 TIP",55]
["18204024","ULTRAJET 1.5BSP 1 TIP",null,null,null,null,null,null,null,null,"0097","Ultrajet Nozzle","A",1.5,"BSP","GPM",210,"PSI","1\"",50,"BLACK","N","ENGLISH","Saber","Mid-Range","N","No 2021 Sales","No 2021 Sales","1820","N/A","N/A",null,null,"1820 1.5 in BSP 210 1\" bore size(s) 50 BLACK (Std) PG","18204024","ULTRAJET 1.5BSP 1 TIP",53]
["18204025","ULTRAJET 38MM STZ 1\" TIP",null,null,null,null,null,null,null,null,"0097","Ultrajet Nozzle","A",1.5,"STORZ","GPM",210,"PSI","1\"",50,"BLACK","N","ENGLISH","Saber","Mid-Range","N","No 2021 Sales","No 2021 Sales","1820","N/A","N/A",null,null,"1820 1.5 in STORZ 210 1\" bore size(s) 50 BLACK (Std) PG","18204025","ULTRAJET 38MM STZ 1\" TIP",55]
["18204026","ULTRAJET 2.5AKB 7/8 TIP",null,null,null,null,null,null,null,null,"0097","Ultrajet Nozzle","A",2.5,"AKB","GPM",161,"PSI","7/8\"",50,"Black","N","ENGLISH","Saber","Mid-Range","N","No 2021 Sales","No 2021 Sales","1820","N/A","N/A",null,null,"1820 2.5 in AKB 161 7/8\" bore size(s) 50 Black (Std) PG","18204026","ULTRAJET 2.5AKB 7/8 TIP",55]
["18204027","ULTRAJET 52MM STZ 1\" TIP",null,null,null,null,null,null,null,null,"0097","Ultrajet Nozzle","A",2,"STORZ","GPM",210,"PSI","1\"",50,"BLACK","N","ENGLISH","Saber","Mid-Range","N","No 2021 Sales","No 2021 Sales","1820","N/A","N/A",null,null,"1820 2 in STORZ 210 1\" bore size(s) 50 BLACK (Std) PG","18204027","ULTRAJET 52MM STZ 1\" TIP",53]
["18204032","ULTRAJET 2.5NH 7/8 TIP",null,null,null,null,null,null,null,null,"0097","Ultrajet Nozzle","A",2.5,"NH","GPM",161,"PSI","7/8\"",50,"BLACK","N","ENGLISH","Saber","Mid-Range","N","No 2021 Sales","No 2021 Sales","1820","N/A","N/A",null,null,"1820 2.5 in NH 161 7/8\" bore size(s) 50 BLACK (Std) PG","18204032","ULTRAJET 2.5NH 7/8 TIP",54]
["18205001","ULTRAJET 2.5 65MM JIM 7/8 TIP W/PG CCCF",null,null,null,null,null,null,null,null,"0097","Ultrajet Nozzle","A",2.5,"JIM","GPM",161,"PSI","7/8\"",50,"BLACK","CCCF","ENGLISH","Saber","Mid-Range","N","No 2021 Sales","No 2021 Sales","1820","N/A","N/A",null,null,"1820 2.5 in JIM 161 7/8\" bore size(s) 50 BLACK (Std) PG ETCH","18205001","ULTRAJET 2.5 65MM JIM 7/8 TIP W/PG CCCF",60]
["18205002","ULTRAJET 2.5 65MM JIM 3/4 TIP W/PG CCCF",null,null,null,null,null,null,null,null,"0097","Ultrajet Nozzle","A",2.5,"JIM","GPM",118,"PSI","3/4\"",50,"BLACK","CCCF","ENGLISH","Saber","Mid-Range","N","No 2021 Sales","No 2021 Sales","1820","N/A","N/A",null,null,"1820 2.5 in JIM 118 3/4\" bore size(s) 50 BLACK (Std) PG ETCH","18205002","ULTRAJET 2.5 65MM JIM 3/4 TIP W/PG CCCF",60]
["18207005","OBS ULTRAJET NPG 1.5NPSH 3/4 TIP",null,null,null,null,null,null,null,null,"0097","Ultrajet Nozzle","O",1.5,"NPSH","GPM",118,"PSI","3/4\"",50,"BLACK","N","ENGLISH","Saber","Mid-Range","Y",20,2,"1820","N/A","N/A",null,null,"1820 1.5 in NPSH 118 3/4\" bore size(s) 50 BLACK (Std) NPG","18207005","OBS ULTRAJET NPG 1.5NPSH 3/4 TIP",57]
["18200026","OBS ULTRAJET 1.5 NPSH 3/4 TIP W/PG",null,null,null,null,null,null,null,null,"0097","Ultrajet Nozzle","O",1.5,"NPSH","GPM",118,"PSI","3/4\"",50,"BLACK","N","ENGLISH","Saber","Mid-Range","N",20,3,"1820","N/A","N/A",null,null,"1820 1.5 in NPSH 118 3/4\" bore size(s) 50 BLACK (Std) PG","18200026","OBS ULTRAJET 1.5 NPSH 3/4 TIP W/PG",56]
["18207028","OBS ULTRAJET NPG 2.5BAF 1 TIP",null,null,null,null,null,null,null,null,"0097","Ultrajet Nozzle","O",2.5,"BAT","GPM",210,"PSI","1\"",50,"BLACK","N","ENGLISH","Saber","Mid-Range","Y",20,3,"1820","N/A","N/A",null,null,"1820 2.5 in BAT 210 1\" bore size(s) 50 BLACK (Std) NPG","18207028","OBS ULTRAJET NPG 2.5BAF 1 TIP",54]
[]
[]
["17024011","TBJT 1.0 NH 13-60G@100P UNIONVILLE E-210",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1,"NH","GPM","13-60","PSI","n/a",100,"BLACK","Y","ENGLISH","Selectable","1\"","N","No 2021 Sales","No 2021 Sales","1702","N/A","N/A",null,null,{"$f":"CONCATENATE(AC1181,\" \",N1181,\" in \",O1181,\" \",IF(AD1181=\"n/a\",\"\",CONCATENATE(AD1181,\" in \",AE1181,\" \")),IF(Q1181=\"n/a\",\"\",Q1181),IF(S1181=\"n/a\",\"\",CONCATENATE(IF(X1181=\"saber\",\" \",\"\"),S1181,\" bore size(s) \")),IF(T1181=\"n/a\",\"\",CONCATENATE(IF(X1181=\"saber\",\"\",\" \"),T1181,IF(T1181=100,\" (Std) \",IF(T1181=87,\" (CE) \",\" \")))),IF(U1181=\"n/a\",\"\",CONCATENATE(U1181,IF(U1181=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X1181,3)=\"tip\",IF(LEFT(X1181,1)=\"s\",\"\",IF(Z1181=\"n\",IF(T1181=\"N/A\",\"PG\",\" PG\"),IF(Z1181=\"y\",IF(T1181=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z1181=\"n\",IF(T1181=\"N/A\",\"PG\",\" PG\"),IF(Z1181=\"y\",IF(T1181=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF1181=\"y\",\" ZT\",\"\"),IF(V1181=\"N\",\"\",IF(S1181=\"n/a\",\" ETCH\",IF(T1181=\"N/A\",IF(RIGHT(X1181,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X1181=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"1702 1 in NH 13-60 100 (Std) BLACK (Std) PG ETCH"},{"$f":"A1181","v":"17024011"},{"$f":"B1181","v":"TBJT 1.0 NH 13-60G@100P UNIONVILLE E-210"},{"$f":"LEN(AH1181)","v":48}]
["17024012","TBJT 1.0 NH 13-60G@100P ORGBMPR BCFD",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1,"NH","GPM","13-60","PSI","n/a",100,"ORANGE","Y","ENGLISH","Selectable","1\"","N","No 2021 Sales","No 2021 Sales","1702","N/A","N/A",null,null,"1702 1 in NH 13-60 100 (Std) ORANGE PG ETCH","17024012","TBJT 1.0 NH 13-60G@100P ORGBMPR BCFD",43]
["17024013","TBJT 1.0 NH 13-60G@100P YLWBMPR BCFD",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1,"NH","GPM","13-60","PSI","n/a",100,"YELLOW","Y","ENGLISH","Selectable","1\"","N","No 2021 Sales","No 2021 Sales","1702","N/A","N/A",null,null,"1702 1 in NH 13-60 100 (Std) YELLOW PG ETCH","17024013","TBJT 1.0 NH 13-60G@100P YLWBMPR BCFD",43]
["17144008","TBJT TIP 1.5NH 30-125G@100P SUMMERFIELD",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","30-125","PSI","n/a",100,"BLACK","Y","ENGLISH","Selectable Tip","1.5\"","N/A","No 2021 Sales","No 2021 Sales","1714","N/A","N/A",null,null,"1714 1.5 in NH 30-125 100 (Std) BLACK (Std) ETCH","17144008","TBJT TIP 1.5NH 30-125G@100P SUMMERFIELD",48]
["17204033","TBJT 1.5NH 30-125G@75P ORGBMPR MVFD",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","30-125","PSI","N/A",75,"ORANGE","Y","ENGLISH","Selectable","1.5\"","N","No 2021 Sales","No 2021 Sales","1720","N/A","N/A",null,null,"1720 1.5 in NH 30-125 75 ORANGE PG ETCH","17204033","TBJT 1.5NH 30-125G@75P ORGBMPR MVFD",39]
["17204034","TBJT 1.5NH 30-125G@75P MVFD",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","30-125","PSI","N/A",75,"BLACK","Y","ENGLISH","Selectable","1.5\"","N","No 2021 Sales","No 2021 Sales","1720","N/A","N/A",null,null,"1720 1.5 in NH 30-125 75 BLACK (Std) PG ETCH","17204034","TBJT 1.5NH 30-125G@75P MVFD",44]
["17207033","TBJT NPG 1.5NH 30-125G@75P ORGBMPR MVFD",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","30-125","PSI","n/a",75,"ORANGE","Y","ENGLISH","Selectable","1.5\"","Y","No 2021 Sales","No 2021 Sales","1720","N/A","N/A",null,null,"1720 1.5 in NH 30-125 75 ORANGE NPG ETCH","17207033","TBJT NPG 1.5NH 30-125G@75P ORGBMPR MVFD",40]
["17207034","TBJT NPG 1.5NH 30-125G@75P ETCH MVFD",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","30-125","PSI","n/a",75,"BLACK","Y","ENGLISH","Selectable","1.5\"","Y","No 2021 Sales","No 2021 Sales","1720","N/A","N/A",null,null,"1720 1.5 in NH 30-125 75 BLACK (Std) NPG ETCH","17207034","TBJT NPG 1.5NH 30-125G@75P ETCH MVFD",45]
["17234007","TBJT 1.5NH 95-200G@100P FINLEYFIRE.COM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","95-200","PSI","n/a",100,"BLACK","Y","ENGLISH","Selectable","Mid-Range","N","No 2021 Sales","No 2021 Sales","1723","N/A","N/A",null,null,"1723 1.5 in NH 95-200 100 (Std) BLACK (Std) PG ETCH","17234007","TBJT 1.5NH 95-200G@100P FINLEYFIRE.COM",51]
["17334000","TBJT NOZ S/A  65MM JIM 125-250G@75P CCCF",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"JIM","GPM","125-250","PSI","N/A",75,"BLACK","CCCF","ENGLISH","Selectable","High-Range","N","No 2021 Sales","No 2021 Sales","1733","N/A","N/A",null,null,"1733 2.5 in JIM 125-250 75 BLACK (Std) PG ETCH","17334000","TBJT NOZ S/A  65MM JIM 125-250G@75P CCCF",46]
["17334001","TBJT S/A  65MM JIM 475-950 LPM@7b CCCF",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"JIM","LPM","475-950","BAR","N/A",7,"BLACK","CCCF","ENGLISH","Selectable","High-Range","N","No 2021 Sales","No 2021 Sales","1733","N/A","N/A",null,null,"1733 2.5 in JIM 475-950 7 BLACK (Std) PG ETCH","17334001","TBJT S/A  65MM JIM 475-950 LPM@7b CCCF",45]
["17334008","TBJT 75MM 125-250G@100P FM BOMBEROS LOGO",null,null,null,null,null,null,null,null,"0001","Turbojet","A",3,"STORZ","GPM","125-250","PSI","N/A",100,"BLACK","Y","ENGLISH","Selectable","High-Range","N","No 2021 Sales","No 2021 Sales","1733","N/A","N/A",null,null,"1733 3 in STORZ 125-250 100 (Std) BLACK (Std) PG ETCH","17334008","TBJT 75MM 125-250G@100P FM BOMBEROS LOGO",53]
["17334026","TBJT 2.5NH 125-250G@100P MVFD",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"NH","GPM","125-250","PSI","N/A",100,"BLACK","Y","ENGLISH","Selectable","High-Range","N","No 2021 Sales","No 2021 Sales","1733","N/A","N/A",null,null,"1733 2.5 in NH 125-250 100 (Std) BLACK (Std) PG ETCH","17334026","TBJT 2.5NH 125-250G@100P MVFD",52]
["17335000","TBJT PG 65MM JIM 125-250G@75P CCCF",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"JIM","GPM","125-250","PSI","N/A",75,"BLACK","CCCF","ENGLISH","Selectable","High-Range","N","No 2021 Sales","No 2021 Sales","1733","N/A","N/A",null,null,"1733 2.5 in JIM 125-250 75 BLACK (Std) PG ETCH","17335000","TBJT PG 65MM JIM 125-250G@75P CCCF",46]
["17335001","TBJT 65MM JIM 475-950L@7b W/770  CCCF",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"JIM","LPM","475-950","BAR","N/A",7,"BLACK","CCCF","ENGLISH","Selectable","High-Range","N","No 2021 Sales","No 2021 Sales","1733","N/A","N/A",null,null,"1733 2.5 in JIM 475-950 7 BLACK (Std) PG ETCH","17335001","TBJT 65MM JIM 475-950L@7b W/770  CCCF",45]
["17337011","TBJT NPG 2.5NH 125-250G@75P UNIONVILLE",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"NH","GPM","125-250","PSI","n/a",75,"BLACK","Y","ENGLISH","Selectable","High-Range","Y","No 2021 Sales","No 2021 Sales","1733","N/A","N/A",null,null,"1733 2.5 in NH 125-250 75 BLACK (Std) NPG ETCH","17337011","TBJT NPG 2.5NH 125-250G@75P UNIONVILLE",46]
["17337012","TBJT NPG 2.5NH 125-250G@100P ETCH MVFD",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"NH","GPM","125-250","PSI","n/a",100,"BLACK","Y","ENGLISH","Selectable","High-Range","Y","No 2021 Sales","No 2021 Sales","1733","N/A","N/A",null,null,"1733 2.5 in NH 125-250 100 (Std) BLACK (Std) NPG ETCH","17337012","TBJT NPG 2.5NH 125-250G@100P ETCH MVFD",53]
["17444009","TBJTTIP 1.5NH 125-250G@100P SACO FD LOGO",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","125-250","PSI","N/A",100,"BLACK","Y","ENGLISH","Selectable Tip","High-Range","N/A",20,3,"1744","N/A","N/A",null,null,"1744 1.5 in NH 125-250 100 (Std) BLACK (Std) ETCH","17444009","TBJTTIP 1.5NH 125-250G@100P SACO FD LOGO",49]
["17634012","TBJT 52MM 30-200G@100P FM BOMBEROS LOGO",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2,"STORZ","GPM","30-200","PSI","N/A",100,"BLACK","Y","ENGLISH","Selectable","Mid-Range","N","No 2021 Sales","No 2021 Sales","1763","N/A","N/A",null,null,"1763 2 in STORZ 30-200 100 (Std) BLACK (Std) PG ETCH","17634012","TBJT 52MM 30-200G@100P FM BOMBEROS LOGO",52]
["17634025","TBJT 1.5NH 30-200G@75P REDBMPR SHERBORN",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","30-200","PSI","n/a",75,"RED","Y","ENGLISH","Selectable","Mid-Range","N","No 2021 Sales","No 2021 Sales","1763","N/A","N/A",null,null,"1763 1.5 in NH 30-200 75 RED PG ETCH","17634025","TBJT 1.5NH 30-200G@75P REDBMPR SHERBORN",36]
["17664006","TBJT TIP 1.5NH 30-200G@75P UNIONVILLE",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","30-200","PSI","n/a",75,"BLACK","Y","ENGLISH","Selectable Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","1766","N/A","N/A",null,null,"1766 1.5 in NH 30-200 75 BLACK (Std) ETCH","17664006","TBJT TIP 1.5NH 30-200G@75P UNIONVILLE",41]
["27310001","TBJT TIP PLAYPIPE 65MMX1.5BSP 292",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"STORZ","LPM","115-750","BAR","N/A",7,"BLACK","Y","ENGLISH","Breakapart Stack Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","2731",1.5,"BSP",null,null,"2731 2.5 in STORZ 1.5 in BSP 115-750 7 BLACK (Std)  ETCH","27310001","TBJT TIP PLAYPIPE 65MMX1.5BSP 292",56]
["27310002","TBJT TIP PLAYPIPE 65MMX1.5BSP 292",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"STORZ","LPM","115-750","BAR","N/A",7,"BLACK","Y","ENGLISH","Breakapart Stack Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","2731",1.5,"BSP",null,null,"2731 2.5 in STORZ 1.5 in BSP 115-750 7 BLACK (Std)  ETCH","27310002","TBJT TIP PLAYPIPE 65MMX1.5BSP 292",56]
["27310003","TBJT TIP PPE 65MMX1.5BSP 292 SS BALL",null,null,null,null,null,null,null,null,"0001","Turbojet","A",2.5,"STORZ","LPM","115-750","BAR","N/A",7,"BLACK","Y","ENGLISH","Breakapart Stack Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","2731",1.5,"BSP",null,null,"2731 2.5 in STORZ 1.5 in BSP 115-750 7 BLACK (Std)  ETCH","27310003","TBJT TIP PPE 65MMX1.5BSP 292 SS BALL",56]
["48027006","ASLT NPG 1\"NH 40G@100P CHARLOTTE FD",null,null,null,null,null,null,null,null,"0003","Assault","A",1,"NH","GPM",40,"PSI","N/A",100,"BLACK","Y","ENGLISH","Fixed","1\"","Y",20,2,"4802","N/A","N/A",null,null,"4802 1 in NH 40 100 (Std) BLACK (Std) NPG ETCH","48027006","ASLT NPG 1\"NH 40G@100P CHARLOTTE FD",46]
["48024018","ASLT 1.0 NH 25G@100P GROVETOWN",null,null,null,null,null,null,null,null,"0003","Assault","A",1,"NH","GPM",25,"PSI","N/A",100,"BLACK","Y","ENGLISH","Fixed","1\"","N","No 2021 Sales","No 2021 Sales","4802","N/A","N/A",null,null,"4802 1 in NH 25 100 (Std) BLACK (Std) PG ETCH","48024018","ASLT 1.0 NH 25G@100P GROVETOWN",45]
["48244039","ASLT TIP 1.5NH 265G@50P SEQ ETCH/SPCFLOW",null,null,null,null,null,null,null,null,"0003","Assault","O",1.5,"NH","GPM",265,"PSI","N/A",50,"BLACK","Y","ENGLISH","Fixed Tip","High-Range","N/A",20,2,"4824","N/A","N/A",null,null,"4824 1.5 in NH 265 50 BLACK (Std)  ETCH","48244039","ASLT TIP 1.5NH 265G@50P SEQ ETCH/SPCFLOW",39]
["48244006","ASLT TIP 1.5NH 250G@75P WFD SEQ",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",250,"PSI","N/A",75,"BLACK","Y","ENGLISH","Fixed Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","4824","N/A","N/A",null,null,"4824 1.5 in NH 250 75 BLACK (Std)  ETCH","48244006","ASLT TIP 1.5NH 250G@75P WFD SEQ",39]
["48244007","ASLT TIP 1.5NH 300G@75P NCFD L-204",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",300,"PSI","N/A",75,"BLACK","Y","ENGLISH","Fixed Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","4824","N/A","N/A",null,null,"4824 1.5 in NH 300 75 BLACK (Std)  ETCH","48244007","ASLT TIP 1.5NH 300G@75P NCFD L-204",39]
["48244010","ASLT TIP 1.5NH 250G@50P LCFR ENGINE 10",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",250,"PSI","N/A",50,"BLACK","Y","ENGLISH","Fixed Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","4824","N/A","N/A",null,null,"4824 1.5 in NH 250 50 BLACK (Std)  ETCH","48244010","ASLT TIP 1.5NH 250G@50P LCFR ENGINE 10",39]
["48244011","ASLT TIP 1.5NH 250G@50P LCFR TRAINING",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",250,"PSI","N/A",50,"BLACK","Y","ENGLISH","Fixed Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","4824","N/A","N/A",null,null,"4824 1.5 in NH 250 50 BLACK (Std)  ETCH","48244011","ASLT TIP 1.5NH 250G@50P LCFR TRAINING",39]
["48244012","ASLT TIP 1.5NH 250G@75P YLWBMPR BCFD",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",250,"PSI","N/A",75,"YELLOW","Y","ENGLISH","Fixed Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","4824","N/A","N/A",null,null,"4824 1.5 in NH 250 75 YELLOW  ETCH","48244012","ASLT TIP 1.5NH 250G@75P YLWBMPR BCFD",34]
["48244014","ASLT TIP 1.5NH 250G@50P  RES-ENG 208",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",250,"PSI","N/A",50,"BLACK","Y","ENGLISH","Fixed Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","4824","N/A","N/A",null,null,"4824 1.5 in NH 250 50 BLACK (Std)  ETCH","48244014","ASLT TIP 1.5NH 250G@50P  RES-ENG 208",39]
["48244024","ASLT TIP 1.5NH 250G@50P  ENO FD",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",250,"PSI","N/A",50,"BLACK","Y","ENGLISH","Fixed Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","4824","N/A","N/A",null,null,"4824 1.5 in NH 250 50 BLACK (Std)  ETCH","48244024","ASLT TIP 1.5NH 250G@50P  ENO FD",39]
["48244026","ASLT TIP 1.5NH 250G@50P LCFR ENGINE 20",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",250,"PSI","N/A",50,"BLACK","Y","ENGLISH","Fixed Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","4824","N/A","N/A",null,null,"4824 1.5 in NH 250 50 BLACK (Std)  ETCH","48244026","ASLT TIP 1.5NH 250G@50P LCFR ENGINE 20",39]
["48244027","ASLT TIP 1.5NH 250G@50P LCFR ENGINE 50",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",250,"PSI","N/A",50,"BLACK","Y","ENGLISH","Fixed Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","4824","N/A","N/A",null,null,"4824 1.5 in NH 250 50 BLACK (Std)  ETCH","48244027","ASLT TIP 1.5NH 250G@50P LCFR ENGINE 50",39]
["48244028","ASLT TIP 1.5NH 250G@50P GASTONIA FD",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",250,"PSI","N/A",50,"BLACK","Y","ENGLISH","Fixed Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","4824","N/A","N/A",null,null,"4824 1.5 in NH 250 50 BLACK (Std)  ETCH","48244028","ASLT TIP 1.5NH 250G@50P GASTONIA FD",39]
["48244029","ASLT TIP 1.5NH 250G@50P MTLTTH ETCH SAC",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",250,"PSI","N/A",50,"BLACK","Y","ENGLISH","Fixed Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","4824","N/A","N/A",null,null,"4824 1.5 in NH 250 50 BLACK (Std)  ETCH","48244029","ASLT TIP 1.5NH 250G@50P MTLTTH ETCH SAC",39]
["48244033","ASLT TIP 1.5NH 250G@50P 1589",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",250,"PSI","N/A",50,"BLACK","Y","ENGLISH","Fixed Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","4824","N/A","N/A",null,null,"4824 1.5 in NH 250 50 BLACK (Std)  ETCH","48244033","ASLT TIP 1.5NH 250G@50P 1589",39]
["48244036","ASLT TIP 1.5NH 250G@50P N1596",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",250,"PSI","N/A",50,"BLACK","Y","ENGLISH","Fixed Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","4824","N/A","N/A",null,null,"4824 1.5 in NH 250 50 BLACK (Std)  ETCH","48244036","ASLT TIP 1.5NH 250G@50P N1596",39]
["48264016","ASLT 2.5NH 350G@100P YLWBMPR BCFD",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"NH","GPM",350,"PSI","N/A",100,"YELLOW","Y","ENGLISH","Fixed","High-Range","N","No 2021 Sales","No 2021 Sales","4826","N/A","N/A",null,null,"4826 2.5 in NH 350 100 (Std) YELLOW PG ETCH","48264016","ASLT 2.5NH 350G@100P YLWBMPR BCFD",43]
["48264023","ASLT 2.5NH 250G@75P SHERBORN",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"NH","GPM",250,"PSI","N/A",75,"BLACK","Y","ENGLISH","Fixed","High-Range","N","No 2021 Sales","No 2021 Sales","4826","N/A","N/A",null,null,"4826 2.5 in NH 250 75 BLACK (Std) PG ETCH","48264023","ASLT 2.5NH 250G@75P SHERBORN",41]
["48264030","ASLT 2.5NH 250G@50P D.F.D.",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"NH","GPM",250,"PSI","N/A",50,"BLACK","Y","ENGLISH","Fixed","High-Range","N","No 2021 Sales","No 2021 Sales","4826","N/A","N/A",null,null,"4826 2.5 in NH 250 50 BLACK (Std) PG ETCH","48264030","ASLT 2.5NH 250G@50P D.F.D.",41]
["48267001","ASLT NPG 2.5NH 250G@50P ORGBMPR OAK",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"NH","GPM",250,"PSI","N/A",50,"ORANGE","Y","ENGLISH","Fixed","High-Range","Y","No 2021 Sales","No 2021 Sales","4826","N/A","N/A",null,null,"4826 2.5 in NH 250 50 ORANGE NPG ETCH","48267001","ASLT NPG 2.5NH 250G@50P ORGBMPR OAK",37]
["48267016","ASLT NPG 2.5NH 250@75 ORGBMPR CHARLOTTE",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"NH","GPM",250,"PSI","N/A",75,"ORANGE","Y","ENGLISH","Fixed","High-Range","Y","No 2021 Sales","No 2021 Sales","4826","N/A","N/A",null,null,"4826 2.5 in NH 250 75 ORANGE NPG ETCH","48267016","ASLT NPG 2.5NH 250@75 ORGBMPR CHARLOTTE",37]
["48267023","ASLT NPG 2.5AFY 300G@100P STA 236",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"PITT6","GPM",300,"PSI","N/A",100,"BLACK","Y","ENGLISH","Fixed","High-Range","Y","No 2021 Sales","No 2021 Sales","4826","N/A","N/A",null,null,"4826 2.5 in PITT6 300 100 (Std) BLACK (Std) NPG ETCH","48267023","ASLT NPG 2.5AFY 300G@100P STA 236",52]
["48267029","ASLT NPG 2.5NH 350G@100P YLWBMPR BCFD",null,null,null,null,null,null,null,null,"0003","Assault","A",2.5,"NH","GPM",350,"PSI","N/A",100,"YELLOW","Y","ENGLISH","Fixed","High-Range","Y","No 2021 Sales","No 2021 Sales","4826","N/A","N/A",null,null,"4826 2.5 in NH 350 100 (Std) YELLOW NPG ETCH","48267029","ASLT NPG 2.5NH 350G@100P YLWBMPR BCFD",44]
["48634120","ASLT 1.5NH 175G@50P SEQ ETCH FG15-21-001",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",175,"PSI","N/A",50,"BLACK","Y","ENGLISH","Fixed","Mid-Range","N",20,2,"4863","N/A","N/A",null,null,"4863 1.5 in NH 175 50 BLACK (Std) PG ETCH","48634120","ASLT 1.5NH 175G@50P SEQ ETCH FG15-21-001",41]
["48634023","ASLT 1.5NH 150G@75P YLWBMPR BFC 1",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",75,"YELLOW","Y","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NH 150 75 YELLOW PG ETCH","48634023","ASLT 1.5NH 150G@75P YLWBMPR BFC 1",36]
["48634024","ASLT 1.5NH 150G@75P REDBMPR BFC 1",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",75,"RED","Y","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NH 150 75 RED PG ETCH","48634024","ASLT 1.5NH 150G@75P REDBMPR BFC 1",33]
["48634030","ASLT 1.5NH 175G@75P NYA FD",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",175,"PSI","N/A",75,"BLACK","Y","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NH 175 75 BLACK (Std) PG ETCH","48634030","ASLT 1.5NH 175G@75P NYA FD",41]
["48634031","ASLT 1.5NH 161G@50P CLEVELAND",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",161,"PSI","N/A",50,"BLACK","Y","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NH 161 50 BLACK (Std) PG ETCH","48634031","ASLT 1.5NH 161G@50P CLEVELAND",41]
["48634040","ASLT 1.5NH 150G@100P GASTONIA FD",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",100,"BLACK","Y","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NH 150 100 (Std) BLACK (Std) PG ETCH","48634040","ASLT 1.5NH 150G@100P GASTONIA FD",48]
["48634041","ASLT 1.5NH 200G@75P NCFD L-204",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",200,"PSI","N/A",75,"BLACK","Y","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NH 200 75 BLACK (Std) PG ETCH","48634041","ASLT 1.5NH 200G@75P NCFD L-204",41]
["48634043","ASLT 1.5NH 150G@75P FINLEYFIRE.COM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",75,"BLACK","Y","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NH 150 75 BLACK (Std) PG ETCH","48634043","ASLT 1.5NH 150G@75P FINLEYFIRE.COM",41]
["48634055","ASLT 1.5NH 175G@75P HARVARD",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",175,"PSI","N/A",75,"BLACK","Y","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NH 175 75 BLACK (Std) PG ETCH","48634055","ASLT 1.5NH 175G@75P HARVARD",41]
["48634062","ASLT 1.5NH 161G@50P  RES-ENG 208",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",161,"PSI","N/A",50,"BLACK","Y","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NH 161 50 BLACK (Std) PG ETCH","48634062","ASLT 1.5NH 161G@50P  RES-ENG 208",41]
["48634063","ASLT 1.5NH 175G@75P TEMPLETON",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",175,"PSI","N/A",75,"BLACK","Y","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NH 175 75 BLACK (Std) PG ETCH","48634063","ASLT 1.5NH 175G@75P TEMPLETON",41]
["48634064","ASLT 1.5NH 175G@75P SHERBORN",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",175,"PSI","N/A",75,"BLACK","Y","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NH 175 75 BLACK (Std) PG ETCH","48634064","ASLT 1.5NH 175G@75P SHERBORN",41]
["48634083","ASLT 1.5NH 125G@100P ENO FD",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",125,"PSI","N/A",100,"BLACK","Y","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NH 125 100 (Std) BLACK (Std) PG ETCH","48634083","ASLT 1.5NH 125G@100P ENO FD",48]
["48634101","ASLT 1.5NH 200G@75P REDBMPR 01535",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",200,"PSI","N/A",75,"RED","Y","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NH 200 75 RED PG ETCH","48634101","ASLT 1.5NH 200G@75P REDBMPR 01535",33]
["48634108","ASLT 1.5NH 150G@50P BLUBMPR RFD STATION6",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",50,"BLUE","Y","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NH 150 50 BLUE PG ETCH","48634108","ASLT 1.5NH 150G@50P BLUBMPR RFD STATION6",34]
["48634109","ASLT 1.5NH 150G@50P REDBMPR RFD STATION6",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",50,"RED","Y","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NH 150 50 RED PG ETCH","48634109","ASLT 1.5NH 150G@50P REDBMPR RFD STATION6",33]
["48634110","ASLT 1.5NH 150G@50P ORGBMPR RFD STATION6",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",50,"ORANGE","Y","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NH 150 50 ORANGE PG ETCH","48634110","ASLT 1.5NH 150G@50P ORGBMPR RFD STATION6",36]
["48634111","ASLT 1.5NH 150G@50P GRNBMPR RFD STATION6",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",50,"GREEN","Y","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,{"$f":"CONCATENATE(AC1245,\" \",N1245,\" in \",O1245,\" \",IF(AD1245=\"n/a\",\"\",CONCATENATE(AD1245,\" in \",AE1245,\" \")),IF(Q1245=\"n/a\",\"\",Q1245),IF(S1245=\"n/a\",\"\",CONCATENATE(IF(X1245=\"saber\",\" \",\"\"),S1245,\" bore size(s) \")),IF(T1245=\"n/a\",\"\",CONCATENATE(IF(X1245=\"saber\",\"\",\" \"),T1245,IF(T1245=100,\" (Std) \",IF(T1245=87,\" (CE) \",\" \")))),IF(U1245=\"n/a\",\"\",CONCATENATE(U1245,IF(U1245=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X1245,3)=\"tip\",IF(LEFT(X1245,1)=\"s\",\"\",IF(Z1245=\"n\",IF(T1245=\"N/A\",\"PG\",\" PG\"),IF(Z1245=\"y\",IF(T1245=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z1245=\"n\",IF(T1245=\"N/A\",\"PG\",\" PG\"),IF(Z1245=\"y\",IF(T1245=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF1245=\"y\",\" ZT\",\"\"),IF(V1245=\"N\",\"\",IF(S1245=\"n/a\",\" ETCH\",IF(T1245=\"N/A\",IF(RIGHT(X1245,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X1245=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"4863 1.5 in NH 150 50 GREEN PG ETCH"},{"$f":"A1245","v":"48634111"},{"$f":"B1245","v":"ASLT 1.5NH 150G@50P GRNBMPR RFD STATION6"},{"$f":"LEN(AH1245)","v":35}]
["48637001","ASLT NPG 1.5NH 150G@75P ORGBMPR OAK",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",75,"ORANGE","Y","ENGLISH","Fixed","Mid-Range","Y","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NH 150 75 ORANGE NPG ETCH","48637001","ASLT NPG 1.5NH 150G@75P ORGBMPR OAK",37]
["48637014","ASLT NPG 1.5NH 161G@50P CLEVELAND VFD",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",161,"PSI","N/A",50,"BLACK","Y","ENGLISH","Fixed","Mid-Range","Y","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NH 161 50 BLACK (Std) NPG ETCH","48637014","ASLT NPG 1.5NH 161G@50P CLEVELAND VFD",42]
["48637040","ASLT NPG 1.5NH 150G@100P GASTONIA FD",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",100,"BLACK","Y","ENGLISH","Fixed","Mid-Range","Y","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NH 150 100 (Std) BLACK (Std) NPG ETCH","48637040","ASLT NPG 1.5NH 150G@100P GASTONIA FD",49]
["48637063","ASLT NPG 1.5NH 150@50 ORGBMPR CHARLOTTE",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",50,"ORANGE","Y","ENGLISH","Fixed","Mid-Range","Y","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NH 150 50 ORANGE NPG ETCH","48637063","ASLT NPG 1.5NH 150@50 ORGBMPR CHARLOTTE",37]
["48637064","ASLT NPG 1.5NH 150@50 REDBMPR CHARLOTTE",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",50,"RED","Y","ENGLISH","Fixed","Mid-Range","Y","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NH 150 50 RED NPG ETCH","48637064","ASLT NPG 1.5NH 150@50 REDBMPR CHARLOTTE",34]
["48637065","ASLT NPG 1.5NH 150@75 ORGBMPR CHARLOTTE",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",75,"ORANGE","Y","ENGLISH","Fixed","Mid-Range","Y","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NH 150 75 ORANGE NPG ETCH","48637065","ASLT NPG 1.5NH 150@75 ORGBMPR CHARLOTTE",37]
["48664011","ASLT TIP 1.5NH 185G@50P REDBMPR DURHAM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",185,"PSI","N/A",50,"RED","Y","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NH 185 50 RED  ETCH","48664011","ASLT TIP 1.5NH 185G@50P REDBMPR DURHAM",31]
["48664016","ASLT TIP 1.5NH 185G@50P ORGBMPR WFD SEQ",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",185,"PSI","N/A",50,"ORANGE","Y","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NH 185 50 ORANGE  ETCH","48664016","ASLT TIP 1.5NH 185G@50P ORGBMPR WFD SEQ",34]
["48664017","ASLT TIP 1.5NH 150G@50P YLWBMPR WFD SEQ",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",50,"YELLOW","Y","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NH 150 50 YELLOW  ETCH","48664017","ASLT TIP 1.5NH 150G@50P YLWBMPR WFD SEQ",34]
["48664023","ASLT TIP 1.5NH 150G@75P FINLEYFIRE.COM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",75,"BLACK","Y","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NH 150 75 BLACK (Std)  ETCH","48664023","ASLT TIP 1.5NH 150G@75P FINLEYFIRE.COM",39]
["48664036","ASLT TIP 1.5NH 175G@75P YLWBMPR BCFD",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",175,"PSI","N/A",75,"YELLOW","Y","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NH 175 75 YELLOW  ETCH","48664036","ASLT TIP 1.5NH 175G@75P YLWBMPR BCFD",34]
["48664039","ASLT TIP 1.5NH 161G@50P RES-ENG 208",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",161,"PSI","N/A",50,"BLACK","Y","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NH 161 50 BLACK (Std)  ETCH","48664039","ASLT TIP 1.5NH 161G@50P RES-ENG 208",39]
["48664040","ASLT TIP 1.5NH 95G@100P RES-ENG 208",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",95,"PSI","N/A",100,"BLACK","Y","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NH 95 100 (Std) BLACK (Std)  ETCH","48664040","ASLT TIP 1.5NH 95G@100P RES-ENG 208",45]
["48664047","ASLT TIP 1.5NH 161G@50P LCFR ENGINE 10",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",161,"PSI","N/A",50,"BLACK","Y","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NH 161 50 BLACK (Std)  ETCH","48664047","ASLT TIP 1.5NH 161G@50P LCFR ENGINE 10",39]
["48664049","ASLT TIP 1.5NH 150G@50P RICHMOND FD",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",50,"BLACK","Y","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NH 150 50 BLACK (Std)  ETCH","48664049","ASLT TIP 1.5NH 150G@50P RICHMOND FD",39]
["48664050","ASLT TIP 1.5NH 175G@50P GRNBMPR RBFR",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",175,"PSI","N/A",50,"GREEN","Y","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NH 175 50 GREEN  ETCH","48664050","ASLT TIP 1.5NH 175G@50P GRNBMPR RBFR",33]
["48664051","ASLT TIP 1.5NH 175G@50P REDBMPR RBFR",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",175,"PSI","N/A",50,"RED","Y","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NH 175 50 RED  ETCH","48664051","ASLT TIP 1.5NH 175G@50P REDBMPR RBFR",31]
["48664059","ASLT TIP 1.5NH 161G@50P ENO FD",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",161,"PSI","N/A",50,"BLACK","Y","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NH 161 50 BLACK (Std)  ETCH","48664059","ASLT TIP 1.5NH 161G@50P ENO FD",39]
["48664061","ASLT TIP 1.5NH 161G@50P WINGATE",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",161,"PSI","N/A",50,"BLACK","Y","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NH 161 50 BLACK (Std)  ETCH","48664061","ASLT TIP 1.5NH 161G@50P WINGATE",39]
["48664062","ASLT TIP 1.5NH 161G@50P YLWBMPR WINGATE",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",161,"PSI","N/A",50,"YELLOW","Y","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NH 161 50 YELLOW  ETCH","48664062","ASLT TIP 1.5NH 161G@50P YLWBMPR WINGATE",34]
["48664063","ASLT TIP 1.5NH 161G@50P GRNBMPR WINGATE",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",161,"PSI","N/A",50,"GREEN","Y","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NH 161 50 GREEN  ETCH","48664063","ASLT TIP 1.5NH 161G@50P GRNBMPR WINGATE",33]
["48664064","ASLT TIP 1.5NH 161G@50P REDBMPR WINGATE",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",161,"PSI","N/A",50,"RED","Y","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NH 161 50 RED  ETCH","48664064","ASLT TIP 1.5NH 161G@50P REDBMPR WINGATE",31]
["48664065","ASLT TIP 1.5NH 161G@50P LCFR ENGINE 20",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",161,"PSI","N/A",50,"BLACK","Y","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NH 161 50 BLACK (Std)  ETCH","48664065","ASLT TIP 1.5NH 161G@50P LCFR ENGINE 20",39]
["48664066","ASLT TIP 1.5NH 161G@50P LCFR ENGINE 50",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",161,"PSI","N/A",50,"BLACK","Y","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NH 161 50 BLACK (Std)  ETCH","48664066","ASLT TIP 1.5NH 161G@50P LCFR ENGINE 50",39]
["48664069","ASLT TIP 1.5NH 175G@50P YLWBMPR FCFRD",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",175,"PSI","N/A",50,"YELLOW","Y","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NH 175 50 YELLOW  ETCH","48664069","ASLT TIP 1.5NH 175G@50P YLWBMPR FCFRD",34]
["48664071","ASLT TIP 1.5NH 150G@50P REDBMPR WFD SEQ",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",50,"RED","Y","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NH 150 50 RED  ETCH","48664071","ASLT TIP 1.5NH 150G@50P REDBMPR WFD SEQ",31]
["48664072","ASLT TIP 1.5NH 185G@50P ORGBMPR WFD 001S",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",185,"PSI","N/A",50,"ORANGE","Y","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NH 185 50 ORANGE  ETCH","48664072","ASLT TIP 1.5NH 185G@50P ORGBMPR WFD 001S",34]
["48664073","ASLT TIP 1.5NH 175G@50P BLUEBMPR 1585",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",175,"PSI","N/A",50,"BLUE","Y","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NH 175 50 BLUE  ETCH","48664073","ASLT TIP 1.5NH 175G@50P BLUEBMPR 1585",32]
["48664074","ASLT TIP 1.5NH 175G@50P ORGBMPR 1586",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",175,"PSI","N/A",50,"ORANGE","Y","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NH 175 50 ORANGE  ETCH","48664074","ASLT TIP 1.5NH 175G@50P ORGBMPR 1586",34]
["48664076","ASLT TIP 1.5NH 161G@50P WFD, E-31",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",161,"PSI","N/A",50,"BLACK","Y","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NH 161 50 BLACK (Std)  ETCH","48664076","ASLT TIP 1.5NH 161G@50P WFD, E-31",39]
["48664078","ASLTTIP 1.5NH 161@50 GRNBMPR SUMMERFIELD",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",161,"PSI","N/A",50,"GREEN","Y","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NH 161 50 GREEN  ETCH","48664078","ASLTTIP 1.5NH 161@50 GRNBMPR SUMMERFIELD",33]
["48664081","ASLT TIP 1.5NH 175G@50P N1592",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",175,"PSI","N/A",50,"BLACK","Y","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NH 175 50 BLACK (Std)  ETCH","48664081","ASLT TIP 1.5NH 175G@50P N1592",39]
["48664082","ASLT TIP 1.5NH 175G@50P N1593",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",175,"PSI","N/A",50,"BLACK","Y","ENGLISH","Fixed Tip","Mid-Range","N/A","No 2021 Sales","No 2021 Sales","4866","N/A","N/A",null,null,"4866 1.5 in NH 175 50 BLACK (Std)  ETCH","48664082","ASLT TIP 1.5NH 175G@50P N1593",39]
["14414003","SH/O TIP 1.5NH X 1.5NH 15/16&1/2 FINLEY",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","15/16\"; 1/2\"","N/A","N/A","Y","ENGLISH","Breakapart Stack Tip","1.5\"","n","No 2021 Sales","No 2021 Sales","1441",1.5,"NH",null,null,"1441 1.5 in NH 1.5 in NH 15/16\"; 1/2\" bore size(s) PGETCH","14414003","SH/O TIP 1.5NH X 1.5NH 15/16&1/2 FINLEY",57]
["14454009","SH/O TIP 1.5NH X 1.5NH 15/16 SEQ ETCH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","15/16\"","N/A","N/A","Y","ENGLISH","Breakapart Solid Bore Tip","1.5\"","N",20,2,"1445",1.5,"NH",null,null,"1445 1.5 in NH 1.5 in NH 15/16\" bore size(s) PGETCH","14454009","SH/O TIP 1.5NH X 1.5NH 15/16 SEQ ETCH",51]
["14465000","NOZ SH/O PG  2.5JIMX1.5NH  7/8  CCCF",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"JIM","N/A","N/A","N/A","7/8\"","n/a","N/A","CCCF","ENGLISH","Breakapart Solid Bore Tip","1.5\"","N","No 2021 Sales","No 2021 Sales","1446",1.5,"NH",null,null,"1446 2.5 in JIM 1.5 in NH 7/8\" bore size(s) PGETCH","14465000","NOZ SH/O PG  2.5JIMX1.5NH  7/8  CCCF",50]
["21264043","SHUTOFF 2.5NH X 1.5NH FLFR SQ49",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","High-Range","N",20,3,"2126",1.5,"NH",null,null,"2126 2.5 in NH 1.5 in NH PG ETCH","21264043","SHUTOFF 2.5NH X 1.5NH FLFR SQ49",32]
["21264044","SHUTOFF 2.5NH X 1.5NH FLFR E49",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","High-Range","N",20,3,"2126",1.5,"NH",null,null,"2126 2.5 in NH 1.5 in NH PG ETCH","21264044","SHUTOFF 2.5NH X 1.5NH FLFR E49",32]
["21264045","SHUTOFF 2.5NH X 1.5NH FLFR E2",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","High-Range","N",20,3,"2126",1.5,"NH",null,null,"2126 2.5 in NH 1.5 in NH PG ETCH","21264045","SHUTOFF 2.5NH X 1.5NH FLFR E2",32]
["21264046","SHUTOFF 2.5NH X 1.5NH FLFR E46",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","High-Range","N",20,3,"2126",1.5,"NH",null,null,"2126 2.5 in NH 1.5 in NH PG ETCH","21264046","SHUTOFF 2.5NH X 1.5NH FLFR E46",32]
["21264047","SHUTOFF 2.5NH X 1.5NH FLFR SQ53",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","High-Range","N",20,3,"2126",1.5,"NH",null,null,"2126 2.5 in NH 1.5 in NH PG ETCH","21264047","SHUTOFF 2.5NH X 1.5NH FLFR SQ53",32]
["21264048","SHUTOFF 2.5NH X 1.5NH CREEDMOOR FD",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","High-Range","N",20,3,"2126",1.5,"NH",null,null,"2126 2.5 in NH 1.5 in NH PG ETCH","21264048","SHUTOFF 2.5NH X 1.5NH CREEDMOOR FD",32]
["21264049","SHUTOFF 2.5AJS X 1.5NH SEQ ETCH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"AJS","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","High-Range","N",20,3,"2126",1.5,"NH",null,null,"2126 2.5 in AJS 1.5 in NH PG ETCH","21264049","SHUTOFF 2.5AJS X 1.5NH SEQ ETCH",33]
["21267005","SHUTOFF NPG 2.5NH X 1.5NH ENG80INE",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","High-Range","Y",20,3,"2126",1.5,"NH",null,null,"2126 2.5 in NH 1.5 in NH NPG ETCH","21267005","SHUTOFF NPG 2.5NH X 1.5NH ENG80INE",33]
["21264005","SHUTOFF 2.5NH  X 1.5NH DURHAM",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2126",1.5,"NH",null,null,"2126 2.5 in NH 1.5 in NH PG ETCH","21264005","SHUTOFF 2.5NH  X 1.5NH DURHAM",32]
["21264008","SHUTOFF 2.5NH  X 1.5NH GASTONIA FD",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2126",1.5,"NH",null,null,"2126 2.5 in NH 1.5 in NH PG ETCH","21264008","SHUTOFF 2.5NH  X 1.5NH GASTONIA FD",32]
["21264010","SHUTOFF 2.5NH  X 1.5NH NCFD L-204",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2126",1.5,"NH",null,null,"2126 2.5 in NH 1.5 in NH PG ETCH","21264010","SHUTOFF 2.5NH  X 1.5NH NCFD L-204",32]
["21264011","SHUTOFF 2.5NH  X 1.5NH SPEC ETCH 2.5\" NH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2126",1.5,"NH",null,null,"2126 2.5 in NH 1.5 in NH PG ETCH","21264011","SHUTOFF 2.5NH  X 1.5NH SPEC ETCH 2.5\" NH",32]
["21264012","SHUTOFF 2.5AEF X 1.5NH ETCH 2.5\" NY CORP",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NYCORP","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2126",1.5,"NH",null,null,"2126 2.5 in NYCORP 1.5 in NH PG ETCH","21264012","SHUTOFF 2.5AEF X 1.5NH ETCH 2.5\" NY CORP",36]
["21264020","SHUTOFF 2.5NH  X 1.5NH RES-ENG 208",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2126",1.5,"NH",null,null,"2126 2.5 in NH 1.5 in NH PG ETCH","21264020","SHUTOFF 2.5NH  X 1.5NH RES-ENG 208",32]
["21264022","SHUTOFF 2.5NH  X 1.5NH SHERBORN",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2126",1.5,"NH",null,null,"2126 2.5 in NH 1.5 in NH PG ETCH","21264022","SHUTOFF 2.5NH  X 1.5NH SHERBORN",32]
["21264023","SHUTOFF 2.5NH X 1.5NH FLFD E13",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2126",1.5,"NH",null,null,"2126 2.5 in NH 1.5 in NH PG ETCH","21264023","SHUTOFF 2.5NH X 1.5NH FLFD E13",32]
["21264024","SHUTOFF 2.5NH X 1.5NH FLFD E8",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2126",1.5,"NH",null,null,"2126 2.5 in NH 1.5 in NH PG ETCH","21264024","SHUTOFF 2.5NH X 1.5NH FLFD E8",32]
["21264025","SHUTOFF 2.5NH X 1.5NH FLFD SPARE",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2126",1.5,"NH",null,null,"2126 2.5 in NH 1.5 in NH PG ETCH","21264025","SHUTOFF 2.5NH X 1.5NH FLFD SPARE",32]
["21264026","SHUTOFF 2.5NH X 1.5NH RICHMOND FD",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2126",1.5,"NH",null,null,"2126 2.5 in NH 1.5 in NH PG ETCH","21264026","SHUTOFF 2.5NH X 1.5NH RICHMOND FD",32]
["21264027","SHUTOFF 2.5NH X 1.5NH FLFD",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2126",1.5,"NH",null,null,"2126 2.5 in NH 1.5 in NH PG ETCH","21264027","SHUTOFF 2.5NH X 1.5NH FLFD",32]
["21264029","SHUTOFF 2.5NH X 1.5NH ENO FD",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2126",1.5,"NH",null,null,"2126 2.5 in NH 1.5 in NH PG ETCH","21264029","SHUTOFF 2.5NH X 1.5NH ENO FD",32]
["21264035","SHUTOFF 2.5NH X 1.5NH CHARLOTTE FD",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2126",1.5,"NH",null,null,"2126 2.5 in NH 1.5 in NH PG ETCH","21264035","SHUTOFF 2.5NH X 1.5NH CHARLOTTE FD",32]
["21264036","SHUTOFF 2.5NH  X 1.5NH D.F.D.",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2126",1.5,"NH",null,null,"2126 2.5 in NH 1.5 in NH PG ETCH","21264036","SHUTOFF 2.5NH  X 1.5NH D.F.D.",32]
["21264037","SHUTOFF 2.5NH  X 1.5NH FCFD TA",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2126",1.5,"NH",null,null,"2126 2.5 in NH 1.5 in NH PG ETCH","21264037","SHUTOFF 2.5NH  X 1.5NH FCFD TA",32]
["21264040","SHUTOFF 2.5NH X 1.5NH LFC4",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2126",1.5,"NH",null,null,"2126 2.5 in NH 1.5 in NH PG ETCH","21264040","SHUTOFF 2.5NH X 1.5NH LFC4",32]
["21267008","SHUTOFF NPG 2.5NH  X 1.5NH GASTONIA FD",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","High-Range","Y","No 2021 Sales","No 2021 Sales","2126",1.5,"NH",null,null,"2126 2.5 in NH 1.5 in NH NPG ETCH","21267008","SHUTOFF NPG 2.5NH  X 1.5NH GASTONIA FD",33]
["21267012","SHUTOFF NPG 2.5NH  X 1.5NH SUMMERFIELD",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","High-Range","Y","No 2021 Sales","No 2021 Sales","2126",1.5,"NH",null,null,"2126 2.5 in NH 1.5 in NH NPG ETCH","21267012","SHUTOFF NPG 2.5NH  X 1.5NH SUMMERFIELD",33]
["21274037","SHUTOFF 1.5NH X 1.5NH FLFR SQ29",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","N",20,3,"2127",1.5,"NH",null,null,{"$f":"CONCATENATE(AC1309,\" \",N1309,\" in \",O1309,\" \",IF(AD1309=\"n/a\",\"\",CONCATENATE(AD1309,\" in \",AE1309,\" \")),IF(Q1309=\"n/a\",\"\",Q1309),IF(S1309=\"n/a\",\"\",CONCATENATE(IF(X1309=\"saber\",\" \",\"\"),S1309,\" bore size(s) \")),IF(T1309=\"n/a\",\"\",CONCATENATE(IF(X1309=\"saber\",\"\",\" \"),T1309,IF(T1309=100,\" (Std) \",IF(T1309=87,\" (CE) \",\" \")))),IF(U1309=\"n/a\",\"\",CONCATENATE(U1309,IF(U1309=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X1309,3)=\"tip\",IF(LEFT(X1309,1)=\"s\",\"\",IF(Z1309=\"n\",IF(T1309=\"N/A\",\"PG\",\" PG\"),IF(Z1309=\"y\",IF(T1309=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z1309=\"n\",IF(T1309=\"N/A\",\"PG\",\" PG\"),IF(Z1309=\"y\",IF(T1309=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF1309=\"y\",\" ZT\",\"\"),IF(V1309=\"N\",\"\",IF(S1309=\"n/a\",\" ETCH\",IF(T1309=\"N/A\",IF(RIGHT(X1309,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X1309=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"2127 1.5 in NH 1.5 in NH PG ETCH"},{"$f":"A1309","v":"21274037"},{"$f":"B1309","v":"SHUTOFF 1.5NH X 1.5NH FLFR SQ29"},{"$f":"LEN(AH1309)","v":32}]
["21274038","SHUTOFF 1.5NH X 1.5NH FLFR E49",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","N",20,3,"2127",1.5,"NH",null,null,"2127 1.5 in NH 1.5 in NH PG ETCH","21274038","SHUTOFF 1.5NH X 1.5NH FLFR E49",32]
["21274039","SHUTOFF 1.5NH X 1.5NH FLFR E2",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","N",20,3,"2127",1.5,"NH",null,null,"2127 1.5 in NH 1.5 in NH PG ETCH","21274039","SHUTOFF 1.5NH X 1.5NH FLFR E2",32]
["21274040","SHUTOFF 1.5NH X 1.5NH FLFR E46",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","N",20,3,"2127",1.5,"NH",null,null,"2127 1.5 in NH 1.5 in NH PG ETCH","21274040","SHUTOFF 1.5NH X 1.5NH FLFR E46",32]
["21274041","SHUTOFF 1.5NH X 1.5NH FLFR SQ53",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","N",20,3,"2127",1.5,"NH",null,null,"2127 1.5 in NH 1.5 in NH PG ETCH","21274041","SHUTOFF 1.5NH X 1.5NH FLFR SQ53",32]
["21274044","SHUTOFF 1.5NH X 1.5NH CONTRA COSTA FIRE",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","N",20,3,"2127",1.5,"NH",null,null,"2127 1.5 in NH 1.5 in NH PG ETCH","21274044","SHUTOFF 1.5NH X 1.5NH CONTRA COSTA FIRE",32]
["21277007","SHUTOFF NPG 1.5NH X 1.5NH ENG80INE",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","Y",20,3,"2127",1.5,"NH",null,null,"2127 1.5 in NH 1.5 in NH NPG ETCH","21277007","SHUTOFF NPG 1.5NH X 1.5NH ENG80INE",33]
["21277008","SHUTOFF NPG 1.5NH X 1.5NH CREEDMOOR FD",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","Y",20,3,"2127",1.5,"NH",null,null,"2127 1.5 in NH 1.5 in NH NPG ETCH","21277008","SHUTOFF NPG 1.5NH X 1.5NH CREEDMOOR FD",33]
["21274003","SHUTOFF 1.5NH X 1.5NH DURHAM",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","N","No 2021 Sales","No 2021 Sales","2127",1.5,"NH",null,null,"2127 1.5 in NH 1.5 in NH PG ETCH","21274003","SHUTOFF 1.5NH X 1.5NH DURHAM",32]
["21274004","SHUTOFF 1.5NH X 1.5NH CLEVELAND",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","N","No 2021 Sales","No 2021 Sales","2127",1.5,"NH",null,null,"2127 1.5 in NH 1.5 in NH PG ETCH","21274004","SHUTOFF 1.5NH X 1.5NH CLEVELAND",32]
["21274008","SHUTOFF 1.5NH X 1.5NH FINLEYFIRE.COM",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","N","No 2021 Sales","No 2021 Sales","2127",1.5,"NH",null,null,"2127 1.5 in NH 1.5 in NH PG ETCH","21274008","SHUTOFF 1.5NH X 1.5NH FINLEYFIRE.COM",32]
["21274010","SHUTOFF 1.5NH X 1.5NH SEQ ETCH TFD",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","N","No 2021 Sales","No 2021 Sales","2127",1.5,"NH",null,null,"2127 1.5 in NH 1.5 in NH PG ETCH","21274010","SHUTOFF 1.5NH X 1.5NH SEQ ETCH TFD",32]
["21274012","SHUTOFF 1.5NH X 1.5NH SEQ ETCH TFD",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","N","No 2021 Sales","No 2021 Sales","2127",1.5,"NH",null,null,"2127 1.5 in NH 1.5 in NH PG ETCH","21274012","SHUTOFF 1.5NH X 1.5NH SEQ ETCH TFD",32]
["21274013","SHUTOFF 1.5NH X 1.5NH RES-ENG 208",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","N","No 2021 Sales","No 2021 Sales","2127",1.5,"NH",null,null,"2127 1.5 in NH 1.5 in NH PG ETCH","21274013","SHUTOFF 1.5NH X 1.5NH RES-ENG 208",32]
["21274015","SHUTOFF 1.5NH X 1.5NH FLFD E13",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","N","No 2021 Sales","No 2021 Sales","2127",1.5,"NH",null,null,"2127 1.5 in NH 1.5 in NH PG ETCH","21274015","SHUTOFF 1.5NH X 1.5NH FLFD E13",32]
["21274016","SHUTOFF 1.5NH X 1.5NH FLFD E8",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","N","No 2021 Sales","No 2021 Sales","2127",1.5,"NH",null,null,"2127 1.5 in NH 1.5 in NH PG ETCH","21274016","SHUTOFF 1.5NH X 1.5NH FLFD E8",32]
["21274017","SHUTOFF 1.5NH X 1.5NH FLFD SPARE",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","N","No 2021 Sales","No 2021 Sales","2127",1.5,"NH",null,null,"2127 1.5 in NH 1.5 in NH PG ETCH","21274017","SHUTOFF 1.5NH X 1.5NH FLFD SPARE",32]
["21274018","SHUTOFF 1.5NH X 1.5NH UNIONVILLE",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","N","No 2021 Sales","No 2021 Sales","2127",1.5,"NH",null,null,"2127 1.5 in NH 1.5 in NH PG ETCH","21274018","SHUTOFF 1.5NH X 1.5NH UNIONVILLE",32]
["21274019","SHUTOFF 1.5NH X 1.5NH RICHMOND FD",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","N","No 2021 Sales","No 2021 Sales","2127",1.5,"NH",null,null,"2127 1.5 in NH 1.5 in NH PG ETCH","21274019","SHUTOFF 1.5NH X 1.5NH RICHMOND FD",32]
["21274020","SHUTOFF 1.5NH X 1.5NH FLFD",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","N","No 2021 Sales","No 2021 Sales","2127",1.5,"NH",null,null,"2127 1.5 in NH 1.5 in NH PG ETCH","21274020","SHUTOFF 1.5NH X 1.5NH FLFD",32]
["21274021","SHUTOFF 1.5NH X 1.5NH LITTLETON",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","N","No 2021 Sales","No 2021 Sales","2127",1.5,"NH",null,null,"2127 1.5 in NH 1.5 in NH PG ETCH","21274021","SHUTOFF 1.5NH X 1.5NH LITTLETON",32]
["21274022","SHUTOFF 1.5NPSH X 1.5NPSH KITTERY FIRE",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NPSH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","N","No 2021 Sales","No 2021 Sales","2127",1.5,"NPSH",null,null,"2127 1.5 in NPSH 1.5 in NPSH PG ETCH","21274022","SHUTOFF 1.5NPSH X 1.5NPSH KITTERY FIRE",36]
["21274023","SHUTOFF 1.5NH X 1.5NH SEQ ETCH TFD",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","N","No 2021 Sales","No 2021 Sales","2127",1.5,"NH",null,null,"2127 1.5 in NH 1.5 in NH PG ETCH","21274023","SHUTOFF 1.5NH X 1.5NH SEQ ETCH TFD",32]
["21274026","SHUTOFF 1.5NH X 1.5NH SEQ ETCH TFD",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","N","No 2021 Sales","No 2021 Sales","2127",1.5,"NH",null,null,"2127 1.5 in NH 1.5 in NH PG ETCH","21274026","SHUTOFF 1.5NH X 1.5NH SEQ ETCH TFD",32]
["21274028","SHUTOFF 1.5NH X 1.5NH SEQ ETCH TFD",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","N","No 2021 Sales","No 2021 Sales","2127",1.5,"NH",null,null,"2127 1.5 in NH 1.5 in NH PG ETCH","21274028","SHUTOFF 1.5NH X 1.5NH SEQ ETCH TFD",32]
["21274029","SHUTOFF 1.5NH X 1.5NH D.F.D.",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","N","No 2021 Sales","No 2021 Sales","2127",1.5,"NH",null,null,"2127 1.5 in NH 1.5 in NH PG ETCH","21274029","SHUTOFF 1.5NH X 1.5NH D.F.D.",32]
["21274030","SHUTOFF 1.5NH X 1.5NH WFD, E-31",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","N","No 2021 Sales","No 2021 Sales","2127",1.5,"NH",null,null,"2127 1.5 in NH 1.5 in NH PG ETCH","21274030","SHUTOFF 1.5NH X 1.5NH WFD, E-31",32]
["21274031","SHUTOFF 1.5NH X 1.5NH FLFR",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","N","No 2021 Sales","No 2021 Sales","2127",1.5,"NH",null,null,"2127 1.5 in NH 1.5 in NH PG ETCH","21274031","SHUTOFF 1.5NH X 1.5NH FLFR",32]
["21274032","SHUTOFF 1.5NH X 1.5NH SEQ ETCH F18960",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","N","No 2021 Sales","No 2021 Sales","2127",1.5,"NH",null,null,"2127 1.5 in NH 1.5 in NH PG ETCH","21274032","SHUTOFF 1.5NH X 1.5NH SEQ ETCH F18960",32]
["21274034","SHUTOFF 1.5NH X 1.5NH LFC4",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","N","No 2021 Sales","No 2021 Sales","2127",1.5,"NH",null,null,"2127 1.5 in NH 1.5 in NH PG ETCH","21274034","SHUTOFF 1.5NH X 1.5NH LFC4",32]
["21274035","SHUTOFF 1.5NH X 1.5NH GROVETOWN",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","N","No 2021 Sales","No 2021 Sales","2127",1.5,"NH",null,null,"2127 1.5 in NH 1.5 in NH PG ETCH","21274035","SHUTOFF 1.5NH X 1.5NH GROVETOWN",32]
["21274045","SHUTOFF 1.5NHX1.5NH SEQ ETCH SB15-20-001",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","N","No 2021 Sales","No 2021 Sales","2127",1.5,"NH",null,null,"2127 1.5 in NH 1.5 in NH PG ETCH","21274045","SHUTOFF 1.5NHX1.5NH SEQ ETCH SB15-20-001",32]
["21277003","SHUTOFF NPG 1.5NH X 1.5NH CONTRA COSTA",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","Y","No 2021 Sales","No 2021 Sales","2127",1.5,"NH",null,null,"2127 1.5 in NH 1.5 in NH NPG ETCH","21277003","SHUTOFF NPG 1.5NH X 1.5NH CONTRA COSTA",33]
["21277010","SHUTOFF NPG 1.5NH X1.5NH MTLHDL SPC LOGO",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","Y","No 2021 Sales","No 2021 Sales","2127",1.5,"NH",null,null,"2127 1.5 in NH 1.5 in NH NPG ETCH","21277010","SHUTOFF NPG 1.5NH X1.5NH MTLHDL SPC LOGO",33]
["21277012","SHUTOFF NPG 1.5NH X 1.5NH SUMMERFIELD",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","Y","No 2021 Sales","No 2021 Sales","2127",1.5,"NH",null,null,"2127 1.5 in NH 1.5 in NH NPG ETCH","21277012","SHUTOFF NPG 1.5NH X 1.5NH SUMMERFIELD",33]
["21277018","SHUTOFF NPG 1.5NH X 1.5NH UNIONVILLE",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","Y","No 2021 Sales","No 2021 Sales","2127",1.5,"NH",null,null,"2127 1.5 in NH 1.5 in NH NPG ETCH","21277018","SHUTOFF NPG 1.5NH X 1.5NH UNIONVILLE",33]
["21300122","SH/OFF TRIDENT 2.5NHX2.5NH SEQ ETCH TFD",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","High-Range","N",20,2,"2130",2.5,"NH",null,null,"2130 2.5 in NH 2.5 in NH PG ETCH","21300122","SH/OFF TRIDENT 2.5NHX2.5NH SEQ ETCH TFD",32]
["21300112","SHUTOFF TRIDENT 2.5NHFX2.5NHM SPC ETCH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2130",2.5,"NH",null,null,"2130 2.5 in NH 2.5 in NH PG ETCH","21300112","SHUTOFF TRIDENT 2.5NHFX2.5NHM SPC ETCH",32]
["21300115","S/OFF TRIDENT 2.5NHFX2.5NHM ETCH MPFD",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2130",2.5,"NH",null,null,"2130 2.5 in NH 2.5 in NH PG ETCH","21300115","S/OFF TRIDENT 2.5NHFX2.5NHM ETCH MPFD",32]
["21300117","SH/OFF TRIDENT 2.5NHX2.5NH SEQ ETCH TFD",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2130",2.5,"NH",null,null,"2130 2.5 in NH 2.5 in NH PG ETCH","21300117","SH/OFF TRIDENT 2.5NHX2.5NH SEQ ETCH TFD",32]
["21300120","SH/OFF TRIDENT 2.5NHX2.5NH SEQ ETCH TFD",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2130",2.5,"NH",null,null,"2130 2.5 in NH 2.5 in NH PG ETCH","21300120","SH/OFF TRIDENT 2.5NHX2.5NH SEQ ETCH TFD",32]
["21300121","SHUTOFF TRIDENT 2.5NH X 2.5NH TFD",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2130",2.5,"NH",null,null,"2130 2.5 in NH 2.5 in NH PG ETCH","21300121","SHUTOFF TRIDENT 2.5NH X 2.5NH TFD",32]
["23904020","PLAYPIPE W/SO 2.5NH X 1.5NH SACO FD LOGO",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","High-Range","N/A",20,3,"2390",1.5,"NH",null,null,"2390 2.5 in NH 1.5 in NH   ETCH","23904020","PLAYPIPE W/SO 2.5NH X 1.5NH SACO FD LOGO",31]
["23904005","PLAYPIPE W/SO 2.5NH X 1.5NH WFD SEQ",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","High-Range","N/A","No 2021 Sales","No 2021 Sales","2390",1.5,"NH",null,null,"2390 2.5 in NH 1.5 in NH   ETCH","23904005","PLAYPIPE W/SO 2.5NH X 1.5NH WFD SEQ",31]
["23904010","PLAYPIPE W/SO 2.5NH X 1.5NH RES-ENG 208",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","High-Range","N/A","No 2021 Sales","No 2021 Sales","2390",1.5,"NH",null,null,"2390 2.5 in NH 1.5 in NH   ETCH","23904010","PLAYPIPE W/SO 2.5NH X 1.5NH RES-ENG 208",31]
["23904012","PLAYPIPE W/SO 2.5NH X 1.5NH UNIONVILLE",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","High-Range","N/A","No 2021 Sales","No 2021 Sales","2390",1.5,"NH",null,null,"2390 2.5 in NH 1.5 in NH   ETCH","23904012","PLAYPIPE W/SO 2.5NH X 1.5NH UNIONVILLE",31]
["23904019","PLAYPIPE W/SO 2.5NHX1.5NH WFD 001-20-2.5",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","Y","ENGLISH","Shutoff","High-Range","N/A","No 2021 Sales","No 2021 Sales","2390",1.5,"NH",null,null,"2390 2.5 in NH 1.5 in NH   ETCH","23904019","PLAYPIPE W/SO 2.5NHX1.5NH WFD 001-20-2.5",31]
["23934009","PP W/STK TIPS 2.5NH X 1.5NH SACO FD LOGO",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","1-1/4\"; 1-1/8\"; 1\"","n/a","N/A","Y","ENGLISH","Breakapart Stack Tip","High-Range","N/A",20,3,"2393",1.5,"NH",null,null,"2393 2.5 in NH 1.5 in NH 1-1/4\"; 1-1/8\"; 1\" bore size(s)  ETCH","23934009","PP W/STK TIPS 2.5NH X 1.5NH SACO FD LOGO",62]
["23934003","PP W/STK TIPS 2.5NH X 1.5NH RES-ENG 208",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","1-1/4\"; 1-1/8\"; 1\"","n/a","N/A","Y","ENGLISH","Breakapart Stack Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","2393",1.5,"NH",null,null,"2393 2.5 in NH 1.5 in NH 1-1/4\"; 1-1/8\"; 1\" bore size(s)  ETCH","23934003","PP W/STK TIPS 2.5NH X 1.5NH RES-ENG 208",62]
["23934005","PP W/STK TIPS 2.5NH X 1.5NH UNIONVILLE",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","1-1/4\"; 1-1/8\"; 1\"","n/a","N/A","Y","ENGLISH","Breakapart Stack Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","2393",1.5,"NH",null,null,"2393 2.5 in NH 1.5 in NH 1-1/4\"; 1-1/8\"; 1\" bore size(s)  ETCH","23934005","PP W/STK TIPS 2.5NH X 1.5NH UNIONVILLE",62]
["24314010","SBR TIP SO 1.5NH X 1.5NH 15/16D DURHAM",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","15/16\"","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","N","No 2021 Sales","No 2021 Sales","2431",1.5,"NH",null,null,"2431 1.5 in NH 1.5 in NH 15/16\" bore size(s) PG ETCH","24314010","SBR TIP SO 1.5NH X 1.5NH 15/16D DURHAM",52]
["24314011","SBR TIP SO 1.5NH X 1.5NH 15/16D WFD SEQ",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","15/16\"","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","N","No 2021 Sales","No 2021 Sales","2431",1.5,"NH",null,null,"2431 1.5 in NH 1.5 in NH 15/16\" bore size(s) PG ETCH","24314011","SBR TIP SO 1.5NH X 1.5NH 15/16D WFD SEQ",52]
["24314012","SBR TIP SO 1.5NH X 1.5NH 15/16D WFD SEQ",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","15/16\"","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","N","No 2021 Sales","No 2021 Sales","2431",1.5,"NH",null,null,"2431 1.5 in NH 1.5 in NH 15/16\" bore size(s) PG ETCH","24314012","SBR TIP SO 1.5NH X 1.5NH 15/16D WFD SEQ",52]
["24314014","SBR TIP SO 1.5NH X 1.5NH 1-1/8D FINLEY",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","1-1/8\"","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","N","No 2021 Sales","No 2021 Sales","2431",1.5,"NH",null,null,"2431 1.5 in NH 1.5 in NH 1-1/8\" bore size(s) PG ETCH","24314014","SBR TIP SO 1.5NH X 1.5NH 1-1/8D FINLEY",52]
["24314015","SBR TIP SO 1.5NH X 1.5NH 7/8D LCFR ENG10",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","7/8\"","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","N","No 2021 Sales","No 2021 Sales","2431",1.5,"NH",null,null,"2431 1.5 in NH 1.5 in NH 7/8\" bore size(s) PG ETCH","24314015","SBR TIP SO 1.5NH X 1.5NH 7/8D LCFR ENG10",50]
["24314017","SBR TIP SO 1.5NH X 1.5NH 1-1/8D BCFD",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","1-1/8\"","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","N","No 2021 Sales","No 2021 Sales","2431",1.5,"NH",null,null,"2431 1.5 in NH 1.5 in NH 1-1/8\" bore size(s) PG ETCH","24314017","SBR TIP SO 1.5NH X 1.5NH 1-1/8D BCFD",52]
["24314018","SBRTIP SO 1.5NHX1.5NH 1D MTLHDL RBFR",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","1\"","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","N","No 2021 Sales","No 2021 Sales","2431",1.5,"NH",null,null,"2431 1.5 in NH 1.5 in NH 1\" bore size(s) PG ETCH","24314018","SBRTIP SO 1.5NHX1.5NH 1D MTLHDL RBFR",48]
["24314019","SBR TIP SO 1.5NH X 1.5NH 15/16D ENO FD",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","15/16\"","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","N","No 2021 Sales","No 2021 Sales","2431",1.5,"NH",null,null,"2431 1.5 in NH 1.5 in NH 15/16\" bore size(s) PG ETCH","24314019","SBR TIP SO 1.5NH X 1.5NH 15/16D ENO FD",52]
["24314020","SBR TIP SO 1.5NH X 1.5NH 7/8D LCFR ENG20",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","7/8\"","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","N","No 2021 Sales","No 2021 Sales","2431",1.5,"NH",null,null,"2431 1.5 in NH 1.5 in NH 7/8\" bore size(s) PG ETCH","24314020","SBR TIP SO 1.5NH X 1.5NH 7/8D LCFR ENG20",50]
["24314021","SBR TIP SO 1.5NH X 1.5NH 7/8D LCFR ENG50",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","7/8\"","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","N","No 2021 Sales","No 2021 Sales","2431",1.5,"NH",null,null,"2431 1.5 in NH 1.5 in NH 7/8\" bore size(s) PG ETCH","24314021","SBR TIP SO 1.5NH X 1.5NH 7/8D LCFR ENG50",50]
["24314022","SBR TIP SO 1.5NH X 1.5NH 15/16D SAC",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","15/16\"","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","N","No 2021 Sales","No 2021 Sales","2431",1.5,"NH",null,null,"2431 1.5 in NH 1.5 in NH 15/16\" bore size(s) PG ETCH","24314022","SBR TIP SO 1.5NH X 1.5NH 15/16D SAC",52]
["24314023","SBRTIP SO1.5NHX1.5NH 15/16D MTLHDL FCFRD",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","15/16\"","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","N","No 2021 Sales","No 2021 Sales","2431",1.5,"NH",null,null,"2431 1.5 in NH 1.5 in NH 15/16\" bore size(s) PG ETCH","24314023","SBRTIP SO1.5NHX1.5NH 15/16D MTLHDL FCFRD",52]
["24314024","SBR TIP SO 1.5NH X 1.5NH 15/16D FCFD TA",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","15/16\"","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","N","No 2021 Sales","No 2021 Sales","2431",1.5,"NH",null,null,"2431 1.5 in NH 1.5 in NH 15/16\" bore size(s) PG ETCH","24314024","SBR TIP SO 1.5NH X 1.5NH 15/16D FCFD TA",52]
["24314025","SBR TIP SO 1.5NH X 1.5NH 15/16D WFD SEQ",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","15/16\"","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","N","No 2021 Sales","No 2021 Sales","2431",1.5,"NH",null,null,"2431 1.5 in NH 1.5 in NH 15/16\" bore size(s) PG ETCH","24314025","SBR TIP SO 1.5NH X 1.5NH 15/16D WFD SEQ",52]
["24314026","SBR TIP SO 1.5NH X 1.5NH 15/16D WFD 001S",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","15/16\"","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","N","No 2021 Sales","No 2021 Sales","2431",1.5,"NH",null,null,{"$f":"CONCATENATE(AC1373,\" \",N1373,\" in \",O1373,\" \",IF(AD1373=\"n/a\",\"\",CONCATENATE(AD1373,\" in \",AE1373,\" \")),IF(Q1373=\"n/a\",\"\",Q1373),IF(S1373=\"n/a\",\"\",CONCATENATE(IF(X1373=\"saber\",\" \",\"\"),S1373,\" bore size(s) \")),IF(T1373=\"n/a\",\"\",CONCATENATE(IF(X1373=\"saber\",\"\",\" \"),T1373,IF(T1373=100,\" (Std) \",IF(T1373=87,\" (CE) \",\" \")))),IF(U1373=\"n/a\",\"\",CONCATENATE(U1373,IF(U1373=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X1373,3)=\"tip\",IF(LEFT(X1373,1)=\"s\",\"\",IF(Z1373=\"n\",IF(T1373=\"N/A\",\"PG\",\" PG\"),IF(Z1373=\"y\",IF(T1373=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z1373=\"n\",IF(T1373=\"N/A\",\"PG\",\" PG\"),IF(Z1373=\"y\",IF(T1373=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF1373=\"y\",\" ZT\",\"\"),IF(V1373=\"N\",\"\",IF(S1373=\"n/a\",\" ETCH\",IF(T1373=\"N/A\",IF(RIGHT(X1373,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X1373=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"2431 1.5 in NH 1.5 in NH 15/16\" bore size(s) PG ETCH"},{"$f":"A1373","v":"24314026"},{"$f":"B1373","v":"SBR TIP SO 1.5NH X 1.5NH 15/16D WFD 001S"},{"$f":"LEN(AH1373)","v":52}]
["24314027","SBR TIP SO 1.5NHX1.5NH 15/16D 1585-1588",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","15/16\"","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","N","No 2021 Sales","No 2021 Sales","2431",1.5,"NH",null,null,"2431 1.5 in NH 1.5 in NH 15/16\" bore size(s) PG ETCH","24314027","SBR TIP SO 1.5NHX1.5NH 15/16D 1585-1588",52]
["24314028","SBR TIP SO 1.5NH X 1.5NH 15/16D N1592",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","15/16\"","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","N","No 2021 Sales","No 2021 Sales","2431",1.5,"NH",null,null,"2431 1.5 in NH 1.5 in NH 15/16\" bore size(s) PG ETCH","24314028","SBR TIP SO 1.5NH X 1.5NH 15/16D N1592",52]
["24314029","SBR TIP SO 1.5NH X 1.5NH 15/16D N1593",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","15/16\"","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","N","No 2021 Sales","No 2021 Sales","2431",1.5,"NH",null,null,"2431 1.5 in NH 1.5 in NH 15/16\" bore size(s) PG ETCH","24314029","SBR TIP SO 1.5NH X 1.5NH 15/16D N1593",52]
["24314030","SBR TIP SO 1.5NH X 1.5NH 15/16D N1594",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","15/16\"","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","N","No 2021 Sales","No 2021 Sales","2431",1.5,"NH",null,null,"2431 1.5 in NH 1.5 in NH 15/16\" bore size(s) PG ETCH","24314030","SBR TIP SO 1.5NH X 1.5NH 15/16D N1594",52]
["24314031","SBR TIP SO 1.5NH X 1.5NH 15/16D N1595",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","15/16\"","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","N","No 2021 Sales","No 2021 Sales","2431",1.5,"NH",null,null,"2431 1.5 in NH 1.5 in NH 15/16\" bore size(s) PG ETCH","24314031","SBR TIP SO 1.5NH X 1.5NH 15/16D N1595",52]
["24317007","SBR TIP SO NPG 1.5NH X 1.5NH 1D CONTRA",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","1\"","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","Y","No 2021 Sales","No 2021 Sales","2431",1.5,"NH",null,null,"2431 1.5 in NH 1.5 in NH 1\" bore size(s) NPG ETCH","24317007","SBR TIP SO NPG 1.5NH X 1.5NH 1D CONTRA",49]
["24317008","SBR TIP SO NPG 1.5NH X1.5NH 7/8D WINGATE",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","7/8\"","n/a","N/A","Y","ENGLISH","Shutoff","1.5\"","Y","No 2021 Sales","No 2021 Sales","2431",1.5,"NH",null,null,"2431 1.5 in NH 1.5 in NH 7/8\" bore size(s) NPG ETCH","24317008","SBR TIP SO NPG 1.5NH X1.5NH 7/8D WINGATE",51]
["24337004","SBR TIP SO NPG 2.5NHX1.5NH 1-1/8D ETCH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","1-1/8\"","n/a","N/A","Y","ENGLISH","Shutoff","High-Range","Y",20,2,"2433",1.5,"NH",null,null,"2433 2.5 in NH 1.5 in NH 1-1/8\" bore size(s) NPG ETCH","24337004","SBR TIP SO NPG 2.5NHX1.5NH 1-1/8D ETCH",53]
["24334004","SBR TIP SO 2.5NHX1.5NH 1-1/8D LCFR ENG10",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","1-1/8\"","n/a","N/A","Y","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2433",1.5,"NH",null,null,"2433 2.5 in NH 1.5 in NH 1-1/8\" bore size(s) PG ETCH","24334004","SBR TIP SO 2.5NHX1.5NH 1-1/8D LCFR ENG10",52]
["24334005","SBR TIP SO 2.5NHX1.5NH 1-1/8D LCFR TRAIN",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","1-1/8\"","n/a","N/A","Y","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2433",1.5,"NH",null,null,"2433 2.5 in NH 1.5 in NH 1-1/8\" bore size(s) PG ETCH","24334005","SBR TIP SO 2.5NHX1.5NH 1-1/8D LCFR TRAIN",52]
["24334006","SBR TIP SO ZT 2.5NHX1.5NH 1-1/4D BCFD",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","1-1/4\"","n/a","N/A","Y","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2433",1.5,"NH","Y",null,"2433 2.5 in NH 1.5 in NH 1-1/4\" bore size(s) PG ZT ETCH","24334006","SBR TIP SO ZT 2.5NHX1.5NH 1-1/4D BCFD",55]
["24334009","SBR TIP SO 2.5NHX1.5NH 1-1/4D RBFR",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","1-1/4\"","n/a","N/A","Y","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2433",1.5,"NH",null,null,"2433 2.5 in NH 1.5 in NH 1-1/4\" bore size(s) PG ETCH","24334009","SBR TIP SO 2.5NHX1.5NH 1-1/4D RBFR",52]
["24334011","SBR TIP SO 2.5NHX1.5NH 1-1/8D LCFR ENG20",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","1-1/8\"","n/a","N/A","Y","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2433",1.5,"NH",null,null,"2433 2.5 in NH 1.5 in NH 1-1/8\" bore size(s) PG ETCH","24334011","SBR TIP SO 2.5NHX1.5NH 1-1/8D LCFR ENG20",52]
["24334012","SBR TIP SO 2.5NHX1.5NH 1-1/8D LCFR ENG50",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","1-1/8\"","n/a","N/A","Y","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2433",1.5,"NH",null,null,"2433 2.5 in NH 1.5 in NH 1-1/8\" bore size(s) PG ETCH","24334012","SBR TIP SO 2.5NHX1.5NH 1-1/8D LCFR ENG50",52]
["24334014","SBR TIP SO 2.5NH X 1.5NH 15/16D 1589",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","15/16\"","n/a","N/A","Y","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2433",1.5,"NH",null,null,"2433 2.5 in NH 1.5 in NH 15/16\" bore size(s) PG ETCH","24334014","SBR TIP SO 2.5NH X 1.5NH 15/16D 1589",52]
["24334015","SBR TIP SO 2.5NHX1.5NH 1-1/4D 1590-1591",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","1-1/4\"","n/a","N/A","Y","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2433",1.5,"NH",null,null,"2433 2.5 in NH 1.5 in NH 1-1/4\" bore size(s) PG ETCH","24334015","SBR TIP SO 2.5NHX1.5NH 1-1/4D 1590-1591",52]
["24334018","SBR TIP SO 2.5NH X 1.5NH 15/16D N1596",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","15/16\"","n/a","N/A","Y","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2433",1.5,"NH",null,null,"2433 2.5 in NH 1.5 in NH 15/16\" bore size(s) PG ETCH","24334018","SBR TIP SO 2.5NH X 1.5NH 15/16D N1596",52]
["24334019","SBR TIP SO 2.5NH X 1.5NH 15/16D N1597",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","15/16\"","n/a","N/A","Y","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2433",1.5,"NH",null,null,"2433 2.5 in NH 1.5 in NH 15/16\" bore size(s) PG ETCH","24334019","SBR TIP SO 2.5NH X 1.5NH 15/16D N1597",52]
["24334020","SBR TIP SO 2.5NH X 1.5NH 15/16D N1598",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",2.5,"NH","N/A","N/A","N/A","15/16\"","n/a","N/A","Y","ENGLISH","Shutoff","High-Range","N","No 2021 Sales","No 2021 Sales","2433",1.5,"NH",null,null,"2433 2.5 in NH 1.5 in NH 15/16\" bore size(s) PG ETCH","24334020","SBR TIP SO 2.5NH X 1.5NH 15/16D N1598",52]
["04394007","TIP DUAL STK 1.5NH 15/16&1/2D FINLEYFIRE",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","15/16\"; 1/2\"","N/A","N/A","Y","ENGLISH","Stack Tip","1.5\"","N/A","No 2021 Sales","No 2021 Sales","0439",1,"NH",null,null,"0439 1.5 in NH 1 in NH 15/16\"; 1/2\" bore size(s) ETCH","04394007","TIP DUAL STK 1.5NH 15/16&1/2D FINLEYFIRE",53]
["04394009","TIP DUAL STK 1.5NH 1-1/8&1/2D UNIONVILLE",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","1-1/8\"; 1/2\"","N/A","N/A","Y","ENGLISH","Stack Tip","1.5\"","N/A","No 2021 Sales","No 2021 Sales","0439",1,"NH",null,null,"0439 1.5 in NH 1 in NH 1-1/8\"; 1/2\" bore size(s) ETCH","04394009","TIP DUAL STK 1.5NH 1-1/8&1/2D UNIONVILLE",53]
["14174011","TIP PLAIN 1.5NH 1D FINLEYFIRE.COM",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","1\"","n/a","N/A","Y","ENGLISH","SB Tip","1.5\"","N/A","No 2021 Sales","No 2021 Sales","1417","N/A","N/A",null,null,"1417 1.5 in NH 1\" bore size(s) ETCH","14174011","TIP PLAIN 1.5NH 1D FINLEYFIRE.COM",35]
["14174013","TIP PLAIN 1.5NH 7/8D RICHMOND FD",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","7/8\"","n/a","N/A","Y","ENGLISH","SB Tip","1.5\"","N/A","No 2021 Sales","No 2021 Sales","1417","N/A","N/A",null,null,"1417 1.5 in NH 7/8\" bore size(s) ETCH","14174013","TIP PLAIN 1.5NH 7/8D RICHMOND FD",37]
["14174014","TIP PLAIN 1.5NH 1-1/8D ETCH N1594",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","1-1/8\"","n/a","N/A","Y","ENGLISH","SB Tip","1.5\"","N/A","No 2021 Sales","No 2021 Sales","1417","N/A","N/A",null,null,"1417 1.5 in NH 1-1/8\" bore size(s) ETCH","14174014","TIP PLAIN 1.5NH 1-1/8D ETCH N1594",39]
["14174015","TIP PLAIN 1.5NH 1-1/8D ETCH N1595",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","1-1/8\"","n/a","N/A","Y","ENGLISH","SB Tip","1.5\"","N/A","No 2021 Sales","No 2021 Sales","1417","N/A","N/A",null,null,"1417 1.5 in NH 1-1/8\" bore size(s) ETCH","14174015","TIP PLAIN 1.5NH 1-1/8D ETCH N1595",39]
["14174016","TIP PLAIN 1.5NH 1-1/8D ETCH N1597",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","1-1/8\"","n/a","N/A","Y","ENGLISH","SB Tip","1.5\"","N/A","No 2021 Sales","No 2021 Sales","1417","N/A","N/A",null,null,"1417 1.5 in NH 1-1/8\" bore size(s) ETCH","14174016","TIP PLAIN 1.5NH 1-1/8D ETCH N1597",39]
["14174017","TIP PLAIN 1.5NH 1-1/8D ETCH N1598",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","1-1/8\"","n/a","N/A","Y","ENGLISH","SB Tip","1.5\"","N/A","No 2021 Sales","No 2021 Sales","1417","N/A","N/A",null,null,"1417 1.5 in NH 1-1/8\" bore size(s) ETCH","14174017","TIP PLAIN 1.5NH 1-1/8D ETCH N1598",39]
["14204003","TIP TRIPLE STK 1.5BSP 1,1-1/8,1-1/4",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"BSP","N/A","N/A","N/A","1-1/4\"; 1-1/8\"; 1\"","n/a","N/A","Y","ENGLISH","Stack Tip","1.5\"","N/A","No 2021 Sales","No 2021 Sales","1420",1.5,"NH",null,null,"1420 1.5 in BSP 1.5 in NH 1-1/4\"; 1-1/8\"; 1\" bore size(s) ETCH","14204003","TIP TRIPLE STK 1.5BSP 1,1-1/8,1-1/4",62]
["14204004","TIP TRI STK 1.5NH 1,1-1/8,1-1/4 DURHAM",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","1-1/4\"; 1-1/8\"; 1\"","n/a","N/A","Y","ENGLISH","Stack Tip","1.5\"","N/A","No 2021 Sales","No 2021 Sales","1420",1.5,"NH",null,null,"1420 1.5 in NH 1.5 in NH 1-1/4\"; 1-1/8\"; 1\" bore size(s) ETCH","14204004","TIP TRI STK 1.5NH 1,1-1/8,1-1/4 DURHAM",61]
["14204006","TIP TRISTK 1.5NH 1,1-1/8,1-1/4UNIONVILLE",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","1-1/4\"; 1-1/8\"; 1\"","n/a","N/A","Y","ENGLISH","Stack Tip","1.5\"","N/A","No 2021 Sales","No 2021 Sales","1420",1.5,"NH",null,null,"1420 1.5 in NH 1.5 in NH 1-1/4\"; 1-1/8\"; 1\" bore size(s) ETCH","14204006","TIP TRISTK 1.5NH 1,1-1/8,1-1/4UNIONVILLE",61]
["14204007","TIP TRI STK 1.5NH 1,1-1/8,1-1/4 SACO FD",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","1-1/4\"; 1-1/8\"; 1\"","n/a","N/A","Y","ENGLISH","Stack Tip","1.5\"","N/A","No 2021 Sales","No 2021 Sales","1420",1.5,"NH",null,null,"1420 1.5 in NH 1.5 in NH 1-1/4\"; 1-1/8\"; 1\" bore size(s) ETCH","14204007","TIP TRI STK 1.5NH 1,1-1/8,1-1/4 SACO FD",61]
["14994030","TIP 1.5NH 15/16D SPEC ETCH GPM/PSI",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","15/16\"","n/a","N/A","Y","ENGLISH","SB Tip","1.5\"","N/A",20,3,"1499","N/A","N/A",null,null,"1499 1.5 in NH 15/16\" bore size(s) ETCH","14994030","TIP 1.5NH 15/16D SPEC ETCH GPM/PSI",39]
["14994042","TIP 1.5NH 1-3/16D CREEDMOOR FD",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","1-3/16\"","N/A","N/A","Y","ENGLISH","SB Tip","1.5\"","N/A",20,3,"1499","N/A","N/A",null,null,"1499 1.5 in NH 1-3/16\" bore size(s) ETCH","14994042","TIP 1.5NH 1-3/16D CREEDMOOR FD",40]
["14994023","TIP 1.5NH 1-3/16D SPEC ETCH GPM/PSI",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","1-3/16\"","N/A","N/A","Y","ENGLISH","SB Tip","1.5\"","N/A",20,4,"1499","N/A","N/A",null,null,"1499 1.5 in NH 1-3/16\" bore size(s) ETCH","14994023","TIP 1.5NH 1-3/16D SPEC ETCH GPM/PSI",40]
["14994040","TIP 1.5NH 15/16D  ETCH ENG80INE",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","15/16\"","N/A","N/A","Y","ENGLISH","SB Tip","1.5\"","N/A",20,4,"1499","N/A","N/A",null,null,"1499 1.5 in NH 15/16\" bore size(s) ETCH","14994040","TIP 1.5NH 15/16D  ETCH ENG80INE",39]
["14994041","TIP 1.5NH 1-3/16D ETCH ENG80INE",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","1-3/16\"","N/A","N/A","Y","ENGLISH","SB Tip","1.5\"","N/A",20,4,"1499","N/A","N/A",null,null,"1499 1.5 in NH 1-3/16\" bore size(s) ETCH","14994041","TIP 1.5NH 1-3/16D ETCH ENG80INE",40]
["14994043","TIP 1.5NH 15/16D CREEDMOOR FD",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","15/16\"","N/A","N/A","Y","ENGLISH","SB Tip","1.5\"","N/A",20,4,"1499","N/A","N/A",null,null,"1499 1.5 in NH 15/16\" bore size(s) ETCH","14994043","TIP 1.5NH 15/16D CREEDMOOR FD",39]
["14994017","TIP 1.5NH 15/16D DURHAM",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","15/16\"","N/A","N/A","Y","ENGLISH","SB Tip","1.5\"","N/A","No 2021 Sales","No 2021 Sales","1499","N/A","N/A",null,null,"1499 1.5 in NH 15/16\" bore size(s) ETCH","14994017","TIP 1.5NH 15/16D DURHAM",39]
["14994018","TIP 1.5NH 1-3/16D DURHAM",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","1-3/16\"","N/A","N/A","Y","ENGLISH","SB Tip","1.5\"","N/A","No 2021 Sales","No 2021 Sales","1499","N/A","N/A",null,null,"1499 1.5 in NH 1-3/16\" bore size(s) ETCH","14994018","TIP 1.5NH 1-3/16D DURHAM",40]
["14994019","TIP 1.5NH 1-1/8D DURHAM",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","1-1/8\"","N/A","N/A","Y","ENGLISH","SB Tip","1.5\"","N/A","No 2021 Sales","No 2021 Sales","1499","N/A","N/A",null,null,"1499 1.5 in NH 1-1/8\" bore size(s) ETCH","14994019","TIP 1.5NH 1-1/8D DURHAM",39]
["14994020","TIP 1.5NH 7/8D CLEVELAND",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","7/8\"","N/A","N/A","Y","ENGLISH","SB Tip","1.5\"","N/A","No 2021 Sales","No 2021 Sales","1499","N/A","N/A",null,null,"1499 1.5 in NH 7/8\" bore size(s) ETCH","14994020","TIP 1.5NH 7/8D CLEVELAND",37]
["14994024","TIP 1.5NH 1-1/8D RICHMOND FD",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","1-1/8\"","N/A","N/A","Y","ENGLISH","SB Tip","1.5\"","N/A","No 2021 Sales","No 2021 Sales","1499","N/A","N/A",null,null,"1499 1.5 in NH 1-1/8\" bore size(s) ETCH","14994024","TIP 1.5NH 1-1/8D RICHMOND FD",39]
["14994025","TIP 1.5NPSH 1D KITTERY FIRE DEPT",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NPSH","N/A","N/A","N/A","1\"","N/A","N/A","Y","ENGLISH","SB Tip","1.5\"","N/A","No 2021 Sales","No 2021 Sales","1499","N/A","N/A",null,null,"1499 1.5 in NPSH 1\" bore size(s) ETCH","14994025","TIP 1.5NPSH 1D KITTERY FIRE DEPT",37]
["14994027","TIP 1.5NPSH 7/8D KITTERY FIRE DEPT",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NPSH","N/A","N/A","N/A","7/8\"","N/A","N/A","Y","ENGLISH","SB Tip","1.5\"","N/A","No 2021 Sales","No 2021 Sales","1499","N/A","N/A",null,null,"1499 1.5 in NPSH 7/8\" bore size(s) ETCH","14994027","TIP 1.5NPSH 7/8D KITTERY FIRE DEPT",39]
["14994028","TIP 1.5NH 1-1/8D ENO FD",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","1-1/8\"","N/A","N/A","Y","ENGLISH","SB Tip","1.5\"","N/A","No 2021 Sales","No 2021 Sales","1499","N/A","N/A",null,null,"1499 1.5 in NH 1-1/8\" bore size(s) ETCH","14994028","TIP 1.5NH 1-1/8D ENO FD",39]
["14994031","TIP 1.5NH 1-1/16D D.F.D.",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","1-1/16\"","N/A","N/A","Y","ENGLISH","SB Tip","1.5\"","N/A","No 2021 Sales","No 2021 Sales","1499","N/A","N/A",null,null,"1499 1.5 in NH 1-1/16\" bore size(s) ETCH","14994031","TIP 1.5NH 1-1/16D D.F.D.",40]
["14994032","TIP 1.5NH 15/16D D.F.D.",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","15/16\"","n/a","N/A","Y","ENGLISH","SB Tip","1.5\"","N/A","No 2021 Sales","No 2021 Sales","1499","N/A","N/A",null,null,"1499 1.5 in NH 15/16\" bore size(s) ETCH","14994032","TIP 1.5NH 15/16D D.F.D.",39]
["14994033","TIP 1.5NH 7/8D WFD, E-31",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","7/8\"","N/A","N/A","Y","ENGLISH","SB Tip","1.5\"","N/A","No 2021 Sales","No 2021 Sales","1499","N/A","N/A",null,null,"1499 1.5 in NH 7/8\" bore size(s) ETCH","14994033","TIP 1.5NH 7/8D WFD, E-31",37]
["14994034","TIP 1.5NH 7/8D SUMMERFIELD FD",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","7/8\"","N/A","N/A","Y","ENGLISH","SB Tip","1.5\"","N/A","No 2021 Sales","No 2021 Sales","1499","N/A","N/A",null,null,"1499 1.5 in NH 7/8\" bore size(s) ETCH","14994034","TIP 1.5NH 7/8D SUMMERFIELD FD",37]
["14994035","TIP 1.5NH 1-1/8D SUMMERFIELD FD",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","1-1/8\"","N/A","N/A","Y","ENGLISH","SB Tip","1.5\"","N/A","No 2021 Sales","No 2021 Sales","1499","N/A","N/A",null,null,"1499 1.5 in NH 1-1/8\" bore size(s) ETCH","14994035","TIP 1.5NH 1-1/8D SUMMERFIELD FD",39]
["14994036","TIP 1.5NH 1-3/16D CHARLOTTE FD",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","1-3/16\"","n/a","N/A","Y","ENGLISH","SB Tip","1.5\"","N/A","No 2021 Sales","No 2021 Sales","1499","N/A","N/A",null,null,"1499 1.5 in NH 1-3/16\" bore size(s) ETCH","14994036","TIP 1.5NH 1-3/16D CHARLOTTE FD",40]
["14994037","TIP 1.5NH 15/16D ETCH SPC LOGO",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","15/16\"","N/A","N/A","Y","ENGLISH","SB Tip","1.5\"","N/A","No 2021 Sales","No 2021 Sales","1499","N/A","N/A",null,null,"1499 1.5 in NH 15/16\" bore size(s) ETCH","14994037","TIP 1.5NH 15/16D ETCH SPC LOGO",39]
["14994044","TIP 1.5NH 15/16D SEQ ETCH SB15-20-001",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","15/16\"","N/A","N/A","Y","ENGLISH","SB Tip","1.5\"","N/A","No 2021 Sales","No 2021 Sales","1499","N/A","N/A",null,null,"1499 1.5 in NH 15/16\" bore size(s) ETCH","14994044","TIP 1.5NH 15/16D SEQ ETCH SB15-20-001",39]
["24204007","TIP STK 2.5NH X 1.5NH 1-3/8D UNIONVILLE",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"NH","N/A","N/A","N/A","1-3/8\"; 1-1/4\"; 1\"","N/A","N/A","Y","ENGLISH","Stack Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","2420",1.5,"NH",null,null,"2420 2.5 in NH 1.5 in NH 1-3/8\"; 1-1/4\"; 1\" bore size(s) ETCH","24204007","TIP STK 2.5NH X 1.5NH 1-3/8D UNIONVILLE",61]
["24204014","TIP STK 2.5NHX1.5NH 1-3/8D BOILING SPRGS",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"NH","N/A","N/A","N/A","1-3/8\"; 1-1/4\"; 1\"","N/A","N/A","Y","ENGLISH","Stack Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","2420",1.5,"NH",null,null,"2420 2.5 in NH 1.5 in NH 1-3/8\"; 1-1/4\"; 1\" bore size(s) ETCH","24204014","TIP STK 2.5NHX1.5NH 1-3/8D BOILING SPRGS",61]
["30205000","NOZ IND 1.5 NH CCCF",null,null,null,null,null,null,null,null,"0007","Navy Coast Guard","A",1.5,"NH","LPM",360,"BAR","N/A",5,"BLACK","CCCF","ENGLISH","Gov/Ind Fixed","1.5\"","N","No 2021 Sales","No 2021 Sales","3020","N/A","N/A",null,null,"3020 1.5 in NH 360 5 BLACK (Std) PG ETCH","30205000","NOZ IND 1.5 NH CCCF",40]
["15234024","SBJT 1.5NH 15/16D LENOLA",null,null,null,null,null,null,null,null,"0048","SABER JET NOZZLE","A",1.5,"NH","GPM",135,"PSI","15/16\"",100,"BLACK","Y","ENGLISH","Saber","Mid-Range","N","No 2021 Sales","No 2021 Sales","1523","N/A","N/A",null,null,"1523 1.5 in NH 135 15/16\" bore size(s) 100 (Std) BLACK (Std) PG ETCH","15234024","SBJT 1.5NH 15/16D LENOLA",68]
["16025000","PROVENGER 1\"BSP 45-200L@6b CCCF",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",1,"BSP","LPM","45-200","BAR","N/A",6,"BLACK","CCCF","ENGLISH","Selectable","1\"","N","No 2021 Sales","No 2021 Sales","1602","N/A","N/A",null,null,"1602 1 in BSP 45-200 6 BLACK (Std) PG ETCH","16025000","PROVENGER 1\"BSP 45-200L@6b CCCF",42]
["16164005","PROVENGER 1.5NH 30-150G@100P DRLY PVT",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",1.5,"NH","GPM","30-150","PSI","N/A",100,"BLACK","Y","ENGLISH","Selectable","1.5\"","N",80,1,"1616","N/A","N/A",null,null,"1616 1.5 in NH 30-150 100 (Std) BLACK (Std) PG ETCH","16164005","PROVENGER 1.5NH 30-150G@100P DRLY PVT",51]
["16165001","PROVENGER JIM 65MM PG 115-550L@5b CCCF",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",2.5,"JIM","LPM","115-550","BAR","N/A",5,"BLACK","CCCF","ENGLISH","Selectable","1.5\"","N",80,1,"1616","N/A","N/A",null,null,"1616 2.5 in JIM 115-550 5 BLACK (Std) PG ETCH","16165001","PROVENGER JIM 65MM PG 115-550L@5b CCCF",45]
["16164023","PROVENGER 1.5NPSH 30-150G@87P EN",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",1.5,"NPSH","GPM","30-150","PSI","N/A",87,"BLACK","Y","ENGLISH","Selectable","1.5\"","N","No 2021 Sales","No 2021 Sales","1616","N/A","N/A",null,null,"1616 1.5 in NPSH 30-150 87 (CE) BLACK (Std) PG ETCH","16164023","PROVENGER 1.5NPSH 30-150G@87P EN",51]
["16165000","PROV JIM 65MM 115-550L@7b W/638  CCCF",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",2.5,"JIM","LPM","115-550","BAR","N/A",7,"BLACK","CCCF","ENGLISH","Selectable","1.5\"","N","No 2021 Sales","No 2021 Sales","1616","N/A","N/A",null,null,"1616 2.5 in JIM 115-550 7 BLACK (Std) PG ETCH","16165000","PROV JIM 65MM 115-550L@7b W/638  CCCF",45]
["16165002","PROVENGER JIM 65MM PG 285-750L@5b CCCF",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",2.5,"JIM","LPM","285-750","BAR","N/A",5,"BLACK","CCCF","ENGLISH","Selectable","1.5\"","N","No 2021 Sales","No 2021 Sales","1616","N/A","N/A",null,null,"1616 2.5 in JIM 285-750 5 BLACK (Std) PG ETCH","16165002","PROVENGER JIM 65MM PG 285-750L@5b CCCF",45]
["17024001W","TBJT 1.0 NH 13-60G@100P FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1,"NH","GPM","13-60","PSI","n/a",100,"BLACK","N","ENGLISH","Selectable","1\"","N",20,2,"1702","N/A","N/A",null,null,{"$f":"CONCATENATE(AC1437,\" \",N1437,\" in \",O1437,\" \",IF(AD1437=\"n/a\",\"\",CONCATENATE(AD1437,\" in \",AE1437,\" \")),IF(Q1437=\"n/a\",\"\",Q1437),IF(S1437=\"n/a\",\"\",CONCATENATE(IF(X1437=\"saber\",\" \",\"\"),S1437,\" bore size(s) \")),IF(T1437=\"n/a\",\"\",CONCATENATE(IF(X1437=\"saber\",\"\",\" \"),T1437,IF(T1437=100,\" (Std) \",IF(T1437=87,\" (CE) \",\" \")))),IF(U1437=\"n/a\",\"\",CONCATENATE(U1437,IF(U1437=\"black\",\" (Std)\",\"\"))),IF(RIGHT(X1437,3)=\"tip\",IF(LEFT(X1437,1)=\"s\",\"\",IF(Z1437=\"n\",IF(T1437=\"N/A\",\"PG\",\" PG\"),IF(Z1437=\"y\",IF(T1437=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(Z1437=\"n\",IF(T1437=\"N/A\",\"PG\",\" PG\"),IF(Z1437=\"y\",IF(T1437=\"N/A\",\"NPG\",\" NPG\"),\" \"))),IF(AF1437=\"y\",\" ZT\",\"\"),IF(V1437=\"N\",\"\",IF(S1437=\"n/a\",\" ETCH\",IF(T1437=\"N/A\",IF(RIGHT(X1437,3)=\"Tip\",\"ETCH\",\" ETCH\"),IF(X1437=\"SABER\",\" ETCH\",\"ETCH\")))))","v":"1702 1 in NH 13-60 100 (Std) BLACK (Std) PG"},{"$f":"A1437","v":"17024001W"},{"$f":"B1437","v":"TBJT 1.0 NH 13-60G@100P FM"},{"$f":"LEN(AH1437)","v":43}]
["17204001W","TBJT 1.5NH 30-125G@100P FM",null,null,null,null,null,null,null,null,"0001","Turbojet","A",1.5,"NH","GPM","30-125","PSI","N/A",100,"BLACK","N","ENGLISH","Selectable","1.5\"","N","No 2021 Sales","No 2021 Sales","1720","N/A","N/A",null,null,"1720 1.5 in NH 30-125 100 (Std) BLACK (Std) PG","17204001W","TBJT 1.5NH 30-125G@100P FM",46]
["48080001","NOZ 1\"NH UHP HAND LINE 20GPM@1400PSI",null,null,null,null,null,null,null,null,"0003","Assault","A",1,"NH","GPM",20,"PSI","N/A",1400,"BLACK","N","ENGLISH","Fixed","1\"","N",20,3,"4808","N/A","N/A",null,null,"4808 1 in NH 20 1400 BLACK (Std) PG","48080001","NOZ 1\"NH UHP HAND LINE 20GPM@1400PSI",35]
["48080005","NOZ 1\"NH UHP HAND LINE 15GPM@1500PSI",null,null,null,null,null,null,null,null,"0003","Assault","A",1,"NH","GPM",15,"PSI","N/A",1500,"BLACK","N","ENGLISH","Fixed","1\"","N",20,3,"4808","N/A","N/A",null,null,"4808 1 in NH 15 1500 BLACK (Std) PG","48080005","NOZ 1\"NH UHP HAND LINE 15GPM@1500PSI",35]
["48080011","NOZ 1\"NH UHP HAND LINE 30GPM@1500PSI",null,null,null,null,null,null,null,null,"0003","Assault","A",1,"NH","GPM",30,"PSI","N/A",1500,"BLACK","N","ENGLISH","Fixed","1\"","N",20,3,"4808","N/A","N/A",null,null,"4808 1 in NH 30 1500 BLACK (Std) PG","48080011","NOZ 1\"NH UHP HAND LINE 30GPM@1500PSI",35]
["48080021","NOZ 1\"NH UHP HANDLINE 15G@1100P",null,null,null,null,null,null,null,null,"0003","Assault","A",1,"NH","GPM",15,"PSI","N/A",1100,"BLACK","N","ENGLISH","Fixed","1\"","N",20,3,"4808","N/A","N/A",null,null,"4808 1 in NH 15 1100 BLACK (Std) PG","48080021","NOZ 1\"NH UHP HANDLINE 15G@1100P",35]
["48080025","NOZ 1\"NPSH UHP HAND LINE 15GPM@1500PSI",null,null,null,null,null,null,null,null,"0003","Assault","A",1,"NPSH","GPM",15,"PSI","N/A",1500,"BLACK","N","ENGLISH","Fixed","1\"","N",20,3,"4808","N/A","N/A",null,null,"4808 1 in NPSH 15 1500 BLACK (Std) PG","48080025","NOZ 1\"NPSH UHP HAND LINE 15GPM@1500PSI",37]
["48080002","NOZ 1\"UHP HND LN 20GPM@1200PSI SPC",null,null,null,null,null,null,null,null,"0003","Assault","A",1,"SAE-8","GPM",20,"PSI","N/A",1200,"BLACK","N","ENGLISH","Fixed","1\"","N","No 2021 Sales","No 2021 Sales","4808","N/A","N/A",null,null,"4808 1 in SAE-8 20 1200 BLACK (Std) PG","48080002","NOZ 1\"UHP HND LN 20GPM@1200PSI SPC",38]
["48080003","NOZ 1\"UHP HD LN 15GPM@1200PSI SPC",null,null,null,null,null,null,null,null,"0003","Assault","A",1,"SAE-8","GPM",15,"PSI","N/A",1200,"BLACK","N","ENGLISH","Fixed","1\"","N","No 2021 Sales","No 2021 Sales","4808","N/A","N/A",null,null,"4808 1 in SAE-8 15 1200 BLACK (Std) PG","48080003","NOZ 1\"UHP HD LN 15GPM@1200PSI SPC",38]
["48080004","NOZ 1\"NH UHP HANDLINE 16.5-17.5G@1100P",null,null,null,null,null,null,null,null,"0003","Assault","A",1,"NH","GPM",17,"PSI","N/A",1100,"BLACK","N","ENGLISH","Fixed","1\"","N","No 2021 Sales","No 2021 Sales","4808","N/A","N/A",null,null,"4808 1 in NH 17 1100 BLACK (Std) PG","48080004","NOZ 1\"NH UHP HANDLINE 16.5-17.5G@1100P",35]
["48080006","NOZ 1\"UHP HND LN 20G@1400P SPC",null,null,null,null,null,null,null,null,"0003","Assault","O",1,"SAE-8","GPM",20,"PSI","n/a",1400,"BLACK","N","ENGLISH","Fixed","1\"","N","No 2021 Sales","No 2021 Sales","4808","N/A","N/A",null,null,"4808 1 in SAE-8 20 1400 BLACK (Std) PG","48080006","NOZ 1\"UHP HND LN 20G@1400P SPC",38]
["48080007","NOZ 1\"UHP HD LN 15GPM@1400PSI SPC",null,null,null,null,null,null,null,null,"0003","Assault","A",1,"SAE-8","GPM",15,"PSI","n/a",1400,"BLACK","N","ENGLISH","Fixed","1\"","N","No 2021 Sales","No 2021 Sales","4808","N/A","N/A",null,null,"4808 1 in SAE-8 15 1400 BLACK (Std) PG","48080007","NOZ 1\"UHP HD LN 15GPM@1400PSI SPC",38]
["48080010","NOZ 1\"NPT UHP HANDLINE 16.5-17.5G@1100P",null,null,null,null,null,null,null,null,"0003","Assault","A",1,"NPT","GPM",17,"PSI","N/A",1100,"BLACK","N","ENGLISH","Fixed","1\"","N","No 2021 Sales","No 2021 Sales","4808","N/A","N/A",null,null,"4808 1 in NPT 17 1100 BLACK (Std) PG","48080010","NOZ 1\"NPT UHP HANDLINE 16.5-17.5G@1100P",36]
["48080012","NOZ 1\"NH UHP HAND LINE 30GPM@600PSI",null,null,null,null,null,null,null,null,"0003","Assault","A",1,"NH","GPM",30,"PSI","N/A",600,"BLACK","N","ENGLISH","Fixed","1\"","N","No 2021 Sales","No 2021 Sales","4808","N/A","N/A",null,null,"4808 1 in NH 30 600 BLACK (Std) PG","48080012","NOZ 1\"NH UHP HAND LINE 30GPM@600PSI",34]
["48080013","NOZ 1\"NPSH  UHP HAND LINE 30G@600P",null,null,null,null,null,null,null,null,"0003","Assault","A",1,"NPSH","GPM",30,"PSI","N/A",600,"BLACK","N","ENGLISH","Fixed","1\"","N","No 2021 Sales","No 2021 Sales","4808","N/A","N/A",null,null,"4808 1 in NPSH 30 600 BLACK (Std) PG","48080013","NOZ 1\"NPSH  UHP HAND LINE 30G@600P",36]
["48080014","NOZ 1.5NH UHP HAND LINE 15G@1400P",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",15,"PSI","n/a",1400,"BLACK","N","ENGLISH","Fixed","1\"","N","No 2021 Sales","No 2021 Sales","4808","N/A","N/A",null,null,"4808 1.5 in NH 15 1400 BLACK (Std) PG","48080014","NOZ 1.5NH UHP HAND LINE 15G@1400P",37]
["48080015","NOZ 1\"NPT UHP HANDLINE 20G@1100P",null,null,null,null,null,null,null,null,"0003","Assault","A",1,"NPT","GPM",20,"PSI","N/A",1100,"BLACK","N","ENGLISH","Fixed","1\"","N","No 2021 Sales","No 2021 Sales","4808","N/A","N/A",null,null,"4808 1 in NPT 20 1100 BLACK (Std) PG","48080015","NOZ 1\"NPT UHP HANDLINE 20G@1100P",36]
["48080016","NOZ 1\"NH UHP HAND LINE 20GPM@1500PSI",null,null,null,null,null,null,null,null,"0003","Assault","A",1,"NH","GPM",20,"PSI","n/a",1500,"BLACK","N","ENGLISH","Fixed","1\"","N","No 2021 Sales","No 2021 Sales","4808","N/A","N/A",null,null,"4808 1 in NH 20 1500 BLACK (Std) PG","48080016","NOZ 1\"NH UHP HAND LINE 20GPM@1500PSI",35]
["48080017","NOZ 1\"BSP UHP HAND LINE 20GPM@1400PSI",null,null,null,null,null,null,null,null,"0003","Assault","A",1,"BSP","GPM",20,"PSI","n/a",1400,"BLACK","N","ENGLISH","Fixed","1\"","N","No 2021 Sales","No 2021 Sales","4808","N/A","N/A",null,null,"4808 1 in BSP 20 1400 BLACK (Std) PG","48080017","NOZ 1\"BSP UHP HAND LINE 20GPM@1400PSI",36]
["48080018","NOZ 1\"NH UHP HAND LINE 15G@1400P",null,null,null,null,null,null,null,null,"0003","Assault","A",1,"NH","GPM",15,"PSI","n/a",1400,"BLACK","N","ENGLISH","Fixed","1\"","N","No 2021 Sales","No 2021 Sales","4808","N/A","N/A",null,null,"4808 1 in NH 15 1400 BLACK (Std) PG","48080018","NOZ 1\"NH UHP HAND LINE 15G@1400P",35]
["48080019","NOZ 1\"NPT UHP HANDLINE 10G@1250P",null,null,null,null,null,null,null,null,"0003","Assault","A",1,"NPT","GPM",10,"PSI","N/A",1250,"BLACK","N","ENGLISH","Fixed","1\"","N","No 2021 Sales","No 2021 Sales","4808","N/A","N/A",null,null,"4808 1 in NPT 10 1250 BLACK (Std) PG","48080019","NOZ 1\"NPT UHP HANDLINE 10G@1250P",36]
["48080020","NOZ 1\"NPT UHP HANDLINE 15G@1100P",null,null,null,null,null,null,null,null,"0003","Assault","A",1,"NPT","GPM",15,"PSI","N/A",1100,"BLACK","N","ENGLISH","Fixed","1\"","N","No 2021 Sales","No 2021 Sales","4808","N/A","N/A",null,null,"4808 1 in NPT 15 1100 BLACK (Std) PG","48080020","NOZ 1\"NPT UHP HANDLINE 15G@1100P",36]
["48080022","NOZ 1\"NPT UHP HAND LINE 30GPM@1500PSI",null,null,null,null,null,null,null,null,"0003","Assault","A",1,"NPT","GPM",30,"PSI","N/A",1500,"BLACK","N","ENGLISH","Fixed","1\"","N","No 2021 Sales","No 2021 Sales","4808","N/A","N/A",null,null,"4808 1 in NPT 30 1500 BLACK (Std) PG","48080022","NOZ 1\"NPT UHP HAND LINE 30GPM@1500PSI",36]
["48080023","NOZ 1\"NPSH UHP HAND LINE 30GPM@1500PSI",null,null,null,null,null,null,null,null,"0003","Assault","A",1,"NPSH","GPM",30,"PSI","N/A",1500,"BLACK","N","ENGLISH","Fixed","1\"","N","No 2021 Sales","No 2021 Sales","4808","N/A","N/A",null,null,"4808 1 in NPSH 30 1500 BLACK (Std) PG","48080023","NOZ 1\"NPSH UHP HAND LINE 30GPM@1500PSI",37]
["48080024","NOZ 1\"NH UHP HND LN 20GPM@1200PSI",null,null,null,null,null,null,null,null,"0003","Assault","A",1,"NH","GPM",20,"PSI","N/A",1200,"BLACK","N","ENGLISH","Fixed","1\"","N","No 2021 Sales","No 2021 Sales","4808","N/A","N/A",null,null,"4808 1 in NH 20 1200 BLACK (Std) PG","48080024","NOZ 1\"NH UHP HND LN 20GPM@1200PSI",35]
["48634007W","ASLT 1.5NH 150G@100P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",100,"BLACK","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NH 150 100 (Std) BLACK (Std) PG","48634007W","ASLT 1.5NH 150G@100P FM",43]
["48634008W","ASLT 1.5NH 150G@75P FM",null,null,null,null,null,null,null,null,"0003","Assault","A",1.5,"NH","GPM",150,"PSI","N/A",75,"BLACK","N","ENGLISH","Fixed","Mid-Range","N","No 2021 Sales","No 2021 Sales","4863","N/A","N/A",null,null,"4863 1.5 in NH 150 75 BLACK (Std) PG","48634008W","ASLT 1.5NH 150G@75P FM",36]
["21274001W","SHUTOFF 1.5NH X 1.5NH",null,null,null,null,null,null,null,null,"0004","Ball Shutoff & Playpipe","A",1.5,"NH","N/A","N/A","N/A","N/A","n/a","N/A","N","ENGLISH","Shutoff","1.5\"","N",20,3,"2127",1.5,"NH",null,null,"2127 1.5 in NH 1.5 in NH PG","21274001W","SHUTOFF 1.5NH X 1.5NH",27]
["04890503","PLAIN DELUGE TIP 2.5NH 1 3/4D POL ALUM",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"NH","N/A","N/A","N/A","1-3/4\"","N/A","N/A","N","ENGLISH","SB Tip","High-Range","N/A",20,2,"0489","N/A","N/A",null,null,"0489 2.5 in NH 1-3/4\" bore size(s) ","04890503","PLAIN DELUGE TIP 2.5NH 1 3/4D POL ALUM",35]
["04890504","PLAIN DELUGE TIP 2.5NH 2DSCH POLISH",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"NH","N/A","N/A","N/A","2\"","N/A","N/A","N","ENGLISH","SB Tip","High-Range","N/A",20,2,"0489","N/A","N/A",null,null,"0489 2.5 in NH 2\" bore size(s) ","04890504","PLAIN DELUGE TIP 2.5NH 2DSCH POLISH",31]
["04890132","PLAIN DELUGE TIP 2.5\"NH, 1 3/4D CF/NC",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"NH","N/A","N/A","N/A","1-3/4\"","N/A","N/A","N","ENGLISH","SB Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","0489","N/A","N/A",null,null,"0489 2.5 in NH 1-3/4\" bore size(s) ","04890132","PLAIN DELUGE TIP 2.5\"NH, 1 3/4D CF/NC",35]
["04890133","PLAIN DELUGE TIP 2.5\"NH W/2 DSCH CF/NC",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"NH","N/A","N/A","N/A","2\"","N/A","N/A","N","ENGLISH","SB Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","0489","N/A","N/A",null,null,"0489 2.5 in NH 2\" bore size(s) ","04890133","PLAIN DELUGE TIP 2.5\"NH W/2 DSCH CF/NC",31]
["04890505","PLAIN DELUGE TIP 2.5NH 2 1/4D POLISH",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"NH","N/A","N/A","N/A","2-1/4\"","N/A","N/A","N","ENGLISH","SB Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","0489","N/A","N/A",null,null,"0489 2.5 in NH 2-1/4\" bore size(s) ","04890505","PLAIN DELUGE TIP 2.5NH 2 1/4D POLISH",35]
["04890509","PLAIN DELUGE TIP 2.5AII 2 1/4D POLISH",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"CSA","N/A","N/A","N/A","2-1/4\"","n/a","N/A","N","ENGLISH","SB Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","0489","N/A","N/A",null,null,"0489 2.5 in CSA 2-1/4\" bore size(s) ","04890509","PLAIN DELUGE TIP 2.5AII 2 1/4D POLISH",36]
["04890511","PLAIN DELUGE TIP 2.5AFB 1 3/4DFDNYPOLISH",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"FDNY","N/A","N/A","N/A","1-3/4\"","n/a","N/A","N","ENGLISH","SB Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","0489","N/A","N/A",null,null,"0489 2.5 in FDNY 1-3/4\" bore size(s) ","04890511","PLAIN DELUGE TIP 2.5AFB 1 3/4DFDNYPOLISH",37]
["04890527","PLAIN DELUGE TIP 2.5AEF 1 3/4DSCH POLISH",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"NYCORP","N/A","N/A","N/A","1-3/4\"","n/a","N/A","N","ENGLISH","SB Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","0489","N/A","N/A",null,null,"0489 2.5 in NYCORP 1-3/4\" bore size(s) ","04890527","PLAIN DELUGE TIP 2.5AEF 1 3/4DSCH POLISH",39]
["04890534","PLAIN DELUGE TIP 2.5BSP 2\"DSCH POLISH",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"BSP","N/A","N/A","N/A","2\"","n/a","N/A","N","ENGLISH","SB Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","0489","N/A","N/A",null,null,"0489 2.5 in BSP 2\" bore size(s) ","04890534","PLAIN DELUGE TIP 2.5BSP 2\"DSCH POLISH",32]
["04890544","PLAIN DELUGE TIP 2.5AII 2\"DSCH POLISH",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"CSA","N/A","N/A","N/A","2\"","N/A","N/A","N","ENGLISH","SB Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","0489","N/A","N/A",null,null,"0489 2.5 in CSA 2\" bore size(s) ","04890544","PLAIN DELUGE TIP 2.5AII 2\"DSCH POLISH",32]
["04890593","PLAIN DELUGE TIP 2.5ASM 2\"DSCH POLISH",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"ASM","N/A","N/A","N/A","2\"","n/a","N/A","N","ENGLISH","SB Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","0489","N/A","N/A",null,null,"0489 2.5 in ASM 2\" bore size(s) ","04890593","PLAIN DELUGE TIP 2.5ASM 2\"DSCH POLISH",32]
["04890602","PLAIN DELUGE TIP 2.5AIK 1/3/4DSCH POLISH",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"AIK","N/A","N/A","N/A","1-3/4\"","n/a","N/A","N","ENGLISH","SB Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","0489","N/A","N/A",null,null,"0489 2.5 in AIK 1-3/4\" bore size(s) ","04890602","PLAIN DELUGE TIP 2.5AIK 1/3/4DSCH POLISH",36]
["04890605","PLAIN DELUGE TIP 2.5AFY 2\"DSCH POLISH",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"PITT6","N/A","N/A","N/A","2\"","n/a","N/A","N","ENGLISH","SB Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","0489","N/A","N/A",null,null,"0489 2.5 in PITT6 2\" bore size(s) ","04890605","PLAIN DELUGE TIP 2.5AFY 2\"DSCH POLISH",34]
["04890607","PLAIN DELUGE TIP 2.5AFD 1 3/4DSCH POLISH",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"QST","N/A","N/A","N/A","1-3/4\"","n/a","N/A","N","ENGLISH","SB Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","0489","N/A","N/A",null,null,"0489 2.5 in QST 1-3/4\" bore size(s) ","04890607","PLAIN DELUGE TIP 2.5AFD 1 3/4DSCH POLISH",36]
["04890611","PLAIN DELUGE TIP 2.5AHC 2DSCH POLISH",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"AHC","N/A","N/A","N/A","2\"","n/a","N/A","N","ENGLISH","SB Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","0489","N/A","N/A",null,null,"0489 2.5 in AHC 2\" bore size(s) ","04890611","PLAIN DELUGE TIP 2.5AHC 2DSCH POLISH",32]
["14994001W","TIP 1.5NH 7/8D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","7/8\"","N/A","N/A","N","ENGLISH","SB Tip","1.5\"","N/A",20,4,"1499","N/A","N/A",null,null,"1499 1.5 in NH 7/8\" bore size(s) ","14994001W","TIP 1.5NH 7/8D",33]
["14994003W","TIP 1.5NH 15/16D",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",1.5,"NH","N/A","N/A","N/A","15/16\"","N/A","N/A","N","ENGLISH","SB Tip","1.5\"","N/A",20,4,"1499","N/A","N/A",null,null,"1499 1.5 in NH 15/16\" bore size(s) ","14994003W","TIP 1.5NH 15/16D",35]
["16164006W","PROVENGER 1.5NH 30-150G@100P FM",null,null,null,null,null,null,null,null,"0087","Avenger Nozzle","A",1.5,"NH","GPM","30-150","PSI","N/A",100,"BLACK","N","ENGLISH","Selectable","1.5\"","N",20,3,"1616","N/A","N/A",null,null,"1616 1.5 in NH 30-150 100 (Std) BLACK (Std) PG","16164006W","PROVENGER 1.5NH 30-150G@100P FM",46]
["04890619","PLAIN DELUGE TIP 2.5NH 2DSCH POLISH SAC",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"NH","N/A","N/A","N/A","2\"","N/A","N/A","Y","ENGLISH","SB Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","0489","N/A","N/A",null,null,"0489 2.5 in NH 2\" bore size(s) ETCH","04890619","PLAIN DELUGE TIP 2.5NH 2DSCH POLISH SAC",35]
["04890621","PLAIN DELUGE TIP 2.5NH 1 3/4D POL AL SAC",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"NH","N/A","N/A","N/A","1-3/4\"","N/A","N/A","Y","ENGLISH","SB Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","0489","N/A","N/A",null,null,"0489 2.5 in NH 1-3/4\" bore size(s) ETCH","04890621","PLAIN DELUGE TIP 2.5NH 1 3/4D POL AL SAC",39]
["04890626","PLAIN DELUGE TIP 2.5 NH1 3/4D POL TK 36",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"NH","N/A","N/A","N/A","1-3/4\"","N/A","N/A","Y","ENGLISH","SB Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","0489","N/A","N/A",null,null,"0489 2.5 in NH 1-3/4\" bore size(s) ETCH","04890626","PLAIN DELUGE TIP 2.5 NH1 3/4D POL TK 36",39]
["04890627","PLAIN DELUGE TIP2.5NH 2D POL ETCH TK 36",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"NH","N/A","N/A","N/A","2\"","N/A","N/A","Y","ENGLISH","SB Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","0489","N/A","N/A",null,null,"0489 2.5 in NH 2\" bore size(s) ETCH","04890627","PLAIN DELUGE TIP2.5NH 2D POL ETCH TK 36",35]
["04890628","PLAIN DELUGE TIP 2.5 NH1 3/4D MFA-SPFLD",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"NH","N/A","N/A","N/A","1-3/4\"","N/A","N/A","Y","ENGLISH","SB Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","0489","N/A","N/A",null,null,"0489 2.5 in NH 1-3/4\" bore size(s) ETCH","04890628","PLAIN DELUGE TIP 2.5 NH1 3/4D MFA-SPFLD",39]
["04890629","PLAIN DELUGE TIP2.5NH 2D MFA-SPFLD",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"NH","N/A","N/A","N/A","2\"","N/A","N/A","Y","ENGLISH","SB Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","0489","N/A","N/A",null,null,"0489 2.5 in NH 2\" bore size(s) ETCH","04890629","PLAIN DELUGE TIP2.5NH 2D MFA-SPFLD",35]
["04890637","PLAIN DELUGE TIP 2.5NH 1.75D DCFD",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"NH","N/A","N/A","N/A","1-3/4\"","N/A","N/A","Y","ENGLISH","SB Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","0489","N/A","N/A",null,null,"0489 2.5 in NH 1-3/4\" bore size(s) ETCH","04890637","PLAIN DELUGE TIP 2.5NH 1.75D DCFD",39]
["04890638","PLAIN DELUGE TIP 2.5NH 2\"D DCFD",null,null,null,null,null,null,null,null,"0005","Nozzle Tip","A",2.5,"NH","N/A","N/A","N/A","2\"","N/A","N/A","Y","ENGLISH","SB Tip","High-Range","N/A","No 2021 Sales","No 2021 Sales","0489","N/A","N/A",null,null,"0489 2.5 in NH 2\" bore size(s) ETCH","04890638","PLAIN DELUGE TIP 2.5NH 2\"D DCFD",35]

{"sheet":"6-27-22 Adds","index":8,"n_rows":1391,"n_cols":15,"rows_kept":1391,"cut":false,"hidden":true,"merged":[]}
["Style",null,"Item","Desc","On DataSource?",null,null,null,null,null,null,null,null,null,"asdfa"]
["1702",null,"17034006","TBJT TIP 1.0 W/1.5BSP 50-230L@6b ENGLISH",{"$f":"_xlfn.XLOOKUP(C2,DataSource!A:A,DataSource!AH:AH)","v":"1703 1.5 in BSP 50-230 6 BLACK (Std)"},"Add"]
["1703",null,"17144009","TBJT TIP 1.5NH 115-475L@7b",{"$f":"_xlfn.XLOOKUP(C3,DataSource!A:A,DataSource!AH:AH)","v":"1714 1.5 in NH 115-475 7 BLACK (Std)"},"Add"]
["1704",null,"17204044","TBJT 52MM 30-125G@75P",{"$f":"_xlfn.XLOOKUP(C4,DataSource!A:A,DataSource!AH:AH)","v":"1720 2 in STORZ 30-125 75 BLACK (Std) PG"},"Add"]
["1711",null,"17334040","TBJT 2.5AJE 125-250G@100P FM",{"$f":"_xlfn.XLOOKUP(C5,DataSource!A:A,DataSource!AH:AH)","v":"1733 2.5 in AJE 125-250 100 (Std) BLACK (Std) PG"},"Add"]
["1714",null,"17334041","TBJT 2.5AJN 125-250G@100P FM",{"$f":"_xlfn.XLOOKUP(C6,DataSource!A:A,DataSource!AH:AH)","v":"1733 2.5 in AJN 125-250 100 (Std) BLACK (Std) PG"},"Add"]
["1717",null,"17334043","TBJT 2.5AHY 125-250G@75P",{"$f":"_xlfn.XLOOKUP(C7,DataSource!A:A,DataSource!AH:AH)","v":"1733 2.5 in AHY 125-250 75 BLACK (Std) PG"},"Add"]
["1720",null,"17334044","TBJT 2.5NH 125-250G@75P REDBMPR",{"$f":"_xlfn.XLOOKUP(C8,DataSource!A:A,DataSource!AH:AH)","v":"1733 2.5 in NH 125-250 75 RED PG"},"Add"]
["1723",null,"17334045","TBJT 2.5NH 125-250G@75P YLWBMPR",{"$f":"_xlfn.XLOOKUP(C9,DataSource!A:A,DataSource!AH:AH)","v":"1733 2.5 in NH 125-250 75 YELLOW PG"},"Add"]
["1727",null,"17337019","TBJT NPG 2.5AEF 125-250G@100P FM",{"$f":"_xlfn.XLOOKUP(C10,DataSource!A:A,DataSource!AH:AH)","v":"1733 2.5 in AEF 125-250 100 (Std) BLACK (Std) NPG"},"Add"]
["1733",null,"17334039","TBJT 65MM 125-250G@75P",{"$f":"_xlfn.XLOOKUP(C11,DataSource!A:A,DataSource!AH:AH)","v":"1733 2.5 in STORZ 125-250 75 BLACK (Std) PG"},"Add"]
["1737",null,"17334042","TBJT ZT 65MM 475-950L@7b",{"$f":"_xlfn.XLOOKUP(C12,DataSource!A:A,DataSource!AH:AH)","v":"1733 2.5 in STORZ 475-950 7 BLACK (Std) PG ZT"},"Add"]
["1744",null,"48244043","ASLT TIP 1.5NPSH 1140L@5B",{"$f":"_xlfn.XLOOKUP(C13,DataSource!A:A,DataSource!AH:AH)","v":"4824 1.5 in NPSH 1140 5 BLACK (Std) "},"Add"]
["1763",null,"48264051","ASLT 2.5AHB 250G@50P FM",{"$f":"_xlfn.XLOOKUP(C14,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in AHB 250 50 BLACK (Std) PG"},"Add"]
["1766",null,"48634125","ASLT 1.5BSP 360L@6b",{"$f":"_xlfn.XLOOKUP(C15,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in BSP 360 6 BLACK (Std) PG"},"Add"]
["1772",null,"48634156","ASLT 1.5NH 750L@7b FM",{"$f":"_xlfn.XLOOKUP(C16,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 750 7 BLACK (Std) PG"},"Add"]
["4802",null,"48664094","ASLT TIP 1.5NPSH 660L@5B",{"$f":"_xlfn.XLOOKUP(C17,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NPSH 660 5 BLACK (Std) "},"Add"]
["4808",null,"48664095","ASLT TIP 1.5ABX 175G@50P",{"$f":"_xlfn.XLOOKUP(C18,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in ABX 175 75 BLACK (Std) "},"Add"]
["4820",null,"14464019","SH/O TIP 2.5AJE X 1.5NH 1\" D",{"$f":"_xlfn.XLOOKUP(C19,DataSource!A:A,DataSource!AH:AH)","v":"1446 2.5 in AJE 1.5 in NH 1\" bore size(s) PG"},"Add"]
["4824",null,"14464020","SH/O TIP 2.5AJE X 1.5NH 1-1/8",{"$f":"_xlfn.XLOOKUP(C20,DataSource!A:A,DataSource!AH:AH)","v":"1446 2.5 in AJE 1.5 in NH 1-1/8\" bore size(s) PG"},"Add"]
["4826",null,"14464021","SH/O TIP 2.5ADU X 1.5NH 1-3/8",{"$f":"_xlfn.XLOOKUP(C21,DataSource!A:A,DataSource!AH:AH)","v":"1446 2.5 in ADU 1.5 in NH 1-3/8\" bore size(s) PG"},"Add"]
["4863",null,"21264056","SHUTOFF 2.5AJE  X 1.5NH",{"$f":"_xlfn.XLOOKUP(C22,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in AJE 1.5 in NH PG"},"Add"]
["4866",null,"23904025","PLAYPIPE W/SO 2.5AHQ X 1.5NH",{"$f":"_xlfn.XLOOKUP(C23,DataSource!A:A,DataSource!AH:AH)","v":"2390 2.5 in AHQ 1.5 in NPSH  "},"Add"]
["0753",null,"23904029","PLAYPIPE W/SO 2.5AEH X 1.5NPSH",{"$f":"_xlfn.XLOOKUP(C24,DataSource!A:A,DataSource!AH:AH)","v":"2390 2.5 in AEH 1.5 in NPSH  "},"Add"]
["1125",null,"23904031","PLAYPIPE W/SO 2.5AFO X 1.5NH",{"$f":"_xlfn.XLOOKUP(C25,DataSource!A:A,DataSource!AH:AH)","v":"2390 2.5 in AFO 1.5 in NPSH  "},"Add"]
["1440",null,"23934012","PP W/STK TIPS 2.5AEH X 1.5NPSH",{"$f":"_xlfn.XLOOKUP(C26,DataSource!A:A,DataSource!AH:AH)","v":"2393 2.5 in AEH 1.5 in NPSH 1-1/4\"; 1-1/8\"; 1\" bore size(s)  "},"Add"]
["1441",null,"23934014","PP W/STK TIPS 2.5AFD X 1.5NPSH",{"$f":"_xlfn.XLOOKUP(C27,DataSource!A:A,DataSource!AH:AH)","v":"2393 2.5 in QST 1.5 in NPSH 1-1/4\"; 1-1/8\"; 1\" bore size(s)  "},"Add"]
["1442",null,"24334028","SBR TIP SO 2.5NHX1.5NH 1D",{"$f":"_xlfn.XLOOKUP(C28,DataSource!A:A,DataSource!AH:AH)","v":"2433 2.5 in NH 1.5 in NH 1\" bore size(s) PG"},"Add"]
["1443",null,"04164013","TIP 1.5BSP X 1.5BSP 1-1/4D",{"$f":"_xlfn.XLOOKUP(C29,DataSource!A:A,DataSource!AH:AH)","v":"0416 1.5 in BSP 1.5 in BSP 1-1/4\" bore size(s) "},"Add"]
["1445",null,"04890134","PLAIN DELUGE TIP 2.5NH W/1 1/2DSCH CF/NC",{"$f":"_xlfn.XLOOKUP(C30,DataSource!A:A,DataSource!AH:AH)","v":"0489 2.5 in NH 1-1/2\" bore size(s) "},"Add"]
["1446",null,"04890507","PLAIN DELUGE TIP 2.5AII 1 1/2DSCH POLISH",{"$f":"_xlfn.XLOOKUP(C31,DataSource!A:A,DataSource!AH:AH)","v":"0489 2.5 in CSA 1-1/2\" bore size(s) "},"Add"]
["1447",null,"04890512","PLAIN DELUGE TIP 2.5AFB 1 1/4DFDNYPOLISH",{"$f":"_xlfn.XLOOKUP(C32,DataSource!A:A,DataSource!AH:AH)","v":"0489 2.5 in FDNY 1-1/4\" bore size(s) "},"Add"]
["2102",null,"04890513","PLAIN DELUGE TIP 2.5AFB 1 1/2DFDNYPOLISH",{"$f":"_xlfn.XLOOKUP(C33,DataSource!A:A,DataSource!AH:AH)","v":"0489 2.5 in FDNY 1-1/2\" bore size(s) "},"Add"]
["2126",null,"04890516","PLAIN DELUGE TIP 2.5BAF 1 1/2DSCH POLISH",{"$f":"_xlfn.XLOOKUP(C34,DataSource!A:A,DataSource!AH:AH)","v":"0489 2.5 in BAT 1-1/2\" bore size(s) "},"Add"]
["2127",null,"04890520","PLAIN DELUGE TIP 2.5AII 1 1/4DSCH POLISH",{"$f":"_xlfn.XLOOKUP(C35,DataSource!A:A,DataSource!AH:AH)","v":"0489 2.5 in CSA 1-1/4\" bore size(s) "},"Add"]
["2130",null,"04890529","PLAIN DELUGE TIP 2.5NH 1 D POLISH",{"$f":"_xlfn.XLOOKUP(C36,DataSource!A:A,DataSource!AH:AH)","v":"0489 2.5 in NH 1\" bore size(s) "},"Add"]
["2390",null,"04890539","PLAIN DELUGE TIP 2.5BSP 1 3/8D POLISH",{"$f":"_xlfn.XLOOKUP(C37,DataSource!A:A,DataSource!AH:AH)","v":"0489 2.5 in BSP 1-3/8\" bore size(s) "},"Add"]
["2393",null,"04890595","PLAIN DELUGE TIP 2.5AFD 1 1/4D POLISH",{"$f":"_xlfn.XLOOKUP(C38,DataSource!A:A,DataSource!AH:AH)","v":"0489 2.5 in QST 1-1/4\" bore size(s) "},"Add"]
["2431",null,"04890599","PLAIN DELUGE TIP 2.5 AEF 1 1/8D POLISH",{"$f":"_xlfn.XLOOKUP(C39,DataSource!A:A,DataSource!AH:AH)","v":"0489 2.5 in AEF 1-1/8\" bore size(s) "},"Add"]
["2433",null,"04890622","PLAIN DELUGE 5IP 2.5AII 1 3/8D POLISH",{"$f":"_xlfn.XLOOKUP(C40,DataSource!A:A,DataSource!AH:AH)","v":"0489 2.5 in CSA 1-3/8\" bore size(s) "},"Add"]
["0416",null,"04890623","PLAIN DELUGE TIP 2.5NH 7/8D POLISH",{"$f":"_xlfn.XLOOKUP(C41,DataSource!A:A,DataSource!AH:AH)","v":"0489 2.5 in NH 7/8\" bore size(s) "},"Add"]
["0439",null,"04890631","PLAIN DELUGE TIP 2.5BAF 7/8DSCH POLISH",{"$f":"_xlfn.XLOOKUP(C42,DataSource!A:A,DataSource!AH:AH)","v":"0489 2.5 in BAT 7/8\" bore size(s) "},"Add"]
["0489",null,"04890632","PLAIN DELUGE TIP 2.5 AFD 7/8D POLISH",{"$f":"_xlfn.XLOOKUP(C43,DataSource!A:A,DataSource!AH:AH)","v":"0489 2.5 in QST 7/8\" bore size(s) "},"Add"]
["1417",null,"04890633","PLAIN DELUGE TIP 2.5BAF 15/16DSCH POLISH",{"$f":"_xlfn.XLOOKUP(C44,DataSource!A:A,DataSource!AH:AH)","v":"0489 2.5 in BAT 15/16\" bore size(s) "},"Add"]
["1420",null,"04890639","PLAIN DELUGE TIP 2.5AKB 1 1/4D POLISH",{"$f":"_xlfn.XLOOKUP(C45,DataSource!A:A,DataSource!AH:AH)","v":"0489 2.5 in AKB 1-1/4\" bore size(s) "},"Add"]
["1499",null,"04890521","PLAIN DELUGE TIP 2.5AFD 1 1/2DSCH POLISH",{"$f":"_xlfn.XLOOKUP(C46,DataSource!A:A,DataSource!AH:AH)","v":"0489 2.5 in QST 1-1/2\" bore size(s) "},"Add"]
["2420",null,"04890606","PLAIN DELUGE TIP 2.5 AKB 1 3/8D POLISH",{"$f":"_xlfn.XLOOKUP(C47,DataSource!A:A,DataSource!AH:AH)","v":"0489 2.5 in AKB 1-3/8\" bore size(s) "},"Add"]
["3015",null,"14994045","TIP 1.5BSP 1-3/8D (35MM)",{"$f":"_xlfn.XLOOKUP(C48,DataSource!A:A,DataSource!AH:AH)","v":"1499 1.5 in BSP 1-3/8\" bore size(s) "},"Add"]
["3016",null,"24204011","TIP STK 2.5AKB X 1.5NH 1-1/4D",{"$f":"_xlfn.XLOOKUP(C49,DataSource!A:A,DataSource!AH:AH)","v":"2420 2.5 in AKB 1.5 in NH 1-1/4\"; 1-1/8\"; 1\" bore size(s) "},"Add"]
["3716",null,"24204018","TIP STK 2.5AEF X 1.5NH 1-3/8D",{"$f":"_xlfn.XLOOKUP(C50,DataSource!A:A,DataSource!AH:AH)","v":"2420 2.5 in AEH 1.5 in NH 1-3/8\"; 1-1/4\"; 1\" bore size(s) "},"Add"]
["3721",null,"16024011","PROVENGER 1.0\"NH 45-200LPM@6b",{"$f":"_xlfn.XLOOKUP(C51,DataSource!A:A,DataSource!AH:AH)","v":"1602 1 in NH 45-200 6 BLACK (Std) PG"},"Add"]
["3725",null,"41164026","PROVENGER 1.5BSP FIXED 230L@6b EN",{"$f":"_xlfn.XLOOKUP(C52,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Add"]
["2032",null,"18204030","ULTRAJET 2.5BIM 15/16 TIP",{"$f":"_xlfn.XLOOKUP(C53,DataSource!A:A,DataSource!AH:AH)","v":"1820 2.5 in BIM 118 15/16\" bore size(s) 50 BLACK (Std) PG"},"Add"]
["2046",null,"18204031","ULTRAJET ZT 1.5NH 7/8 TIP",{"$f":"_xlfn.XLOOKUP(C54,DataSource!A:A,DataSource!AH:AH)","v":"1820 1.5 in NH 118 7/8\" bore size(s) 50 BLACK (Std) PG ZT"},"Add"]
["2069",null,"21267033","SHUTOFF NPG 2.5AEF X 1.5NPSH  MTLHDL",{"$f":"_xlfn.XLOOKUP(C55,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Handle Metal"]
["2074",null,"17335003","TBJT 2.5NH 125-250G@100P DINGLEE",{"$f":"_xlfn.XLOOKUP(C56,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Intercompany"]
["3019",null,"17335002","TBJT 65MM JIM 125-250G@75P DINGLEE",{"$f":"_xlfn.XLOOKUP(C57,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Intercompany"]
["3020",null,"15235001","SBJT 2.5NH 1D DINGLEE",{"$f":"_xlfn.XLOOKUP(C58,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Intercompany"]
["3021",null,"15235002","SBJT 65MM JIM 1D DINGLEE",{"$f":"_xlfn.XLOOKUP(C59,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Intercompany"]
["3022",null,"15235003","SBJT 65MM JIM 3/4D DINGLEE",{"$f":"_xlfn.XLOOKUP(C60,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Intercompany"]
["3023",null,"21264801","SHUTOFF MB 2.5AFB X 1.5ABU FDNY",{"$f":"_xlfn.XLOOKUP(C61,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Metal Ball"]
["3025",null,"21274801","SHUTOFF MB 1.5ABU X 1.5ABU FDNY",{"$f":"_xlfn.XLOOKUP(C62,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Metal Ball"]
["3027",null,"48080008","SWVL ASSY 1\"NPT UHP HANDLINE",{"$f":"_xlfn.XLOOKUP(C63,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Part"]
["1512",null,"17024022","TBJT 1.0 NH 13-60G@100P DURHAM CITY FIRE",{"$f":"_xlfn.XLOOKUP(C64,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
["1520",null,"17204043","TBJT 1.5NH 30-125G@100P DURHAM CITY FIRE",{"$f":"_xlfn.XLOOKUP(C65,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
["1523",null,"17634042","TBJT 1.5NPSH 30-200G@75P SACO FD LOGO",{"$f":"_xlfn.XLOOKUP(C66,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
["1528",null,"48264043","ASLT 2.5NH 250G@50P REDBMPR DICKEY136",{"$f":"_xlfn.XLOOKUP(C67,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
["1602",null,"48264055","ASLT 2.5NH 250G@50P NVFD",{"$f":"_xlfn.XLOOKUP(C68,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
["1616",null,"48267003","ASLT NPG 2.5NH 250G@50P WCFD",{"$f":"_xlfn.XLOOKUP(C69,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
["4116",null,"48634074","ASLT 1.5NH 95G@75P SPC*SEE NOTES*",{"$f":"_xlfn.XLOOKUP(C70,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
["1820",null,"48634123","ASLT 1.5NH 150G@100P ORGBMPR ETCH NDHS",{"$f":"_xlfn.XLOOKUP(C71,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
[null,null,"48634148","ASLT 1.5NH 175G@75P FAYETTE FD 11-21",{"$f":"_xlfn.XLOOKUP(C72,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
["2731",null,"48634154","ASLT 1.5NH 95G@100P DURHAM CITY FIRE",{"$f":"_xlfn.XLOOKUP(C73,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
[null,null,"48634157","ASLT 1.5NH 185G@50P NVFD",{"$f":"_xlfn.XLOOKUP(C74,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
[null,null,"48634158","ASLT 1.5NH 185G@50P STRATFORD FD ENG 1",{"$f":"_xlfn.XLOOKUP(C75,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
[null,null,"48634159","ASLT 1.5NH 185G@50P STRATFORD FD ENG 2",{"$f":"_xlfn.XLOOKUP(C76,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
[null,null,"48634160","ASLT 1.5NH 185G@50P STRATFORD FD ENG 3",{"$f":"_xlfn.XLOOKUP(C77,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
[null,null,"48634161","ASLT 1.5NH 185G@50P STRATFORD FD ENG 4",{"$f":"_xlfn.XLOOKUP(C78,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
[null,null,"48634162","ASLT 1.5NH 185G@50P STRATFORD FD ENG 6",{"$f":"_xlfn.XLOOKUP(C79,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
[null,null,"48634163","ASLT 1.5NH 185G@50P STRATFORD FD ENG 7",{"$f":"_xlfn.XLOOKUP(C80,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
[null,null,"48634164","ASLT 1.5NH 185G@50P STRATFORD FD ENG 8",{"$f":"_xlfn.XLOOKUP(C81,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
[null,null,"48634165","ASLT 1.5NH 185G@50P STRATFORD FD",{"$f":"_xlfn.XLOOKUP(C82,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
[null,null,"48637108","ASLT NPG 1.5NH 150G@50P FTA LOGO",{"$f":"_xlfn.XLOOKUP(C83,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
[null,null,"48637109","ASLT NPG 1.5NH 161G@50P FTA LOGO",{"$f":"_xlfn.XLOOKUP(C84,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
[null,null,"48637110","ASLT NPG 1.5NH 175G@50P FTA LOGO",{"$f":"_xlfn.XLOOKUP(C85,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
[null,null,"48637114","ASLT 1.5NH 185G@50P BLUEBMPR WCFD",{"$f":"_xlfn.XLOOKUP(C86,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
[null,null,"48637115","ASLT 1.5NH 185G@50P YLWBMPR WCFD",{"$f":"_xlfn.XLOOKUP(C87,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
[null,null,"48637116","ASLT 1.5NH 185G@50P ORGBMPR WCFD",{"$f":"_xlfn.XLOOKUP(C88,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
[null,null,"48637117","ASLT NPG 1.5NH 185G@50P WCFD",{"$f":"_xlfn.XLOOKUP(C89,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
[null,null,"48664084","ASLT TIP 1.5NH 150G@50P FTA LOGO",{"$f":"_xlfn.XLOOKUP(C90,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
[null,null,"48664085","ASLT TIP 1.5NH 161G@50P FTA LOGO",{"$f":"_xlfn.XLOOKUP(C91,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
[null,null,"48664086","ASLT TIP 1.5NH 175G@50P FTA LOGO",{"$f":"_xlfn.XLOOKUP(C92,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
[null,null,"48664091","ASLT TIP 1.5NH 161G@50P REDBMR DICKEY136",{"$f":"_xlfn.XLOOKUP(C93,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
[null,null,"48664096","ASLT TIP 1.5NH 185G@50P DURHAM CITY FIRE",{"$f":"_xlfn.XLOOKUP(C94,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
[null,null,"48664097","ASLT TIP1.5NH 185@50 REDBMPR DURHAM CITY",{"$f":"_xlfn.XLOOKUP(C95,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
[null,null,"48664098","ASLT TIP1.5NH 185@50 YLWBMPR DURHAM CITY",{"$f":"_xlfn.XLOOKUP(C96,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
[null,null,"21264055","SHUTOFF 2.5NH X 1.5NH STACK ROAD VFD",{"$f":"_xlfn.XLOOKUP(C97,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
[null,null,"21264058","SHUTOFF 2.5NH X 1.5NH DURHAM CITY FIRE",{"$f":"_xlfn.XLOOKUP(C98,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
[null,null,"21267010","SHUTOFF NPG 2.5NH X 1.5NH FTA LOGO",{"$f":"_xlfn.XLOOKUP(C99,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
[null,null,"21267036","SHUTOFF NPG 2.5NH X 1.5NH WCFD",{"$f":"_xlfn.XLOOKUP(C100,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
[null,null,"21274047","SHUTOFF 1.5NH X 1.5NH ETCH NDHS",{"$f":"_xlfn.XLOOKUP(C101,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
[null,null,"21274050","SHUTOFF 1.5NH X 1.5NH DICKEY 136",{"$f":"_xlfn.XLOOKUP(C102,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
[null,null,"21274057","SHUTOFF 1.5NH X 1.5NH DURHAM CITY FIRE",{"$f":"_xlfn.XLOOKUP(C103,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
[null,null,"21277013","SHUTOFF NPG 1.5NH X 1.5NH FTA LOGO",{"$f":"_xlfn.XLOOKUP(C104,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
[null,null,"21277019","SHUTOFF NPG 1.5NH X 1.5NH WCFD",{"$f":"_xlfn.XLOOKUP(C105,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
[null,null,"23904032","PLAYPIPE W/SO 2.5NHX1.5NPSH SACO FD LOGO",{"$f":"_xlfn.XLOOKUP(C106,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
[null,null,"24314040","SBR TIP SO1.5NHX1.5NH 15/16D DURHAM CITY",{"$f":"_xlfn.XLOOKUP(C107,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
[null,null,"24317014","SBRTIPSO NPG 1.5NHX1.5NH 15/16D FTA LOGO",{"$f":"_xlfn.XLOOKUP(C108,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
[null,null,"24317015","SBR TIP SO NPG 1.5NHX1.5NH 7/8D FTA LOGO",{"$f":"_xlfn.XLOOKUP(C109,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
[null,null,"24337006","SBR TIP SO NPG 2.5NHX1.5NH 1-1/4D CONTRA",{"$f":"_xlfn.XLOOKUP(C110,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
[null,null,"24314041","SBR TIP SO 1.5NH X 1.5NH 7/8D D.C.F.D.",{"$f":"_xlfn.XLOOKUP(C111,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
[null,null,"24314035","SBR TIP SO 1.5NH X 1.5NH 7/8D DICKEY 136",{"$f":"_xlfn.XLOOKUP(C112,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
[null,null,"04890636","PLAIN DELUGE TIP 2.5NH 1.5D DCFD",{"$f":"_xlfn.XLOOKUP(C113,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
[null,null,"04890643","PLN DLGE TIP 2.5NH 1-3/8D POL DURHAM",{"$f":"_xlfn.XLOOKUP(C114,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
[null,null,"14174021","TIP PLAIN 1.5NH 15/16D WCFD",{"$f":"_xlfn.XLOOKUP(C115,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
[null,null,"14174022","TIP PLAIN 1.5NH 1-1/8D WCFD",{"$f":"_xlfn.XLOOKUP(C116,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
[null,null,"14204008","TIP TRIPLE STK 1.5NH 1,1-1/8,1-1/4\"NDHS\"",{"$f":"_xlfn.XLOOKUP(C117,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
[null,null,"14994046","TIP 1.5NH 7/8D FTA LOGO",{"$f":"_xlfn.XLOOKUP(C118,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
[null,null,"14994047","TIP 1.5NH 15/16D FTA LOGO",{"$f":"_xlfn.XLOOKUP(C119,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
[null,null,"14994048","TIP 1.5NH 1-3/16D FTA LOGO",{"$f":"_xlfn.XLOOKUP(C120,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
[null,null,"14994050","TIP 1.5NH 1-1/16D SEQ ETCH SB15-20-001",{"$f":"_xlfn.XLOOKUP(C121,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
[null,null,"14994052","TIP 1.5NH 1-1/8D STACK ROAD VFD",{"$f":"_xlfn.XLOOKUP(C122,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
[null,null,"14994053","TIP 1.5NH 15/16D DURHAM CITY FIRE",{"$f":"_xlfn.XLOOKUP(C123,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
[null,null,"14994054","TIP 1.5NH 1-3/16D DURHAM CITY FIRE",{"$f":"_xlfn.XLOOKUP(C124,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
[null,null,"14994055","TIP 1.5NH 1-1/8D DURHAM CITY FIRE",{"$f":"_xlfn.XLOOKUP(C125,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
[null,null,"14994056","TIP 1.5NH 15/16D ENO FD",{"$f":"_xlfn.XLOOKUP(C126,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
[null,null,"14994057","TIP 1.5NH 1-3/16D ENO FD",{"$f":"_xlfn.XLOOKUP(C127,DataSource!A:A,DataSource!AH:AH)","v":{"$error":"#N/A"}},"Special Etch"]
[null,null,"48664035","ASLT TIP 1.5ABT 175G@75P",{"$f":"_xlfn.XLOOKUP(C128,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in PCT 175 75 BLACK (Std) "}]
[null,null,"48664070","ASLT TIP 1.5NPSH 660L@517K",{"$f":"_xlfn.XLOOKUP(C129,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NPSH 660 517 BLACK (Std) "}]
[null,null,"48664055","ASLT TIP 1.5NPSH 660L@500K",{"$f":"_xlfn.XLOOKUP(C130,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NPSH 660 500 BLACK (Std) "}]
[null,null,"48664034","ASLT TIP 1.5NPSH 550L@500K",{"$f":"_xlfn.XLOOKUP(C131,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NPSH 550 500 BLACK (Std) "}]
[null,null,"48664042","ASLT TIP 1.5NPSH 200G@75P",{"$f":"_xlfn.XLOOKUP(C132,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NPSH 200 75 BLACK (Std) "}]
[null,null,"48664067","ASLT TIP 1.5NPSH 175G@75P",{"$f":"_xlfn.XLOOKUP(C133,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NPSH 175 75 BLACK (Std) "}]
[null,null,"48664080","ASLT TIP 1.5NPSH 175G@100P",{"$f":"_xlfn.XLOOKUP(C134,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NPSH 175 100 (Std) BLACK (Std) "}]
[null,null,"48664043","ASLT TIP 1.5NPSH 150G@75P",{"$f":"_xlfn.XLOOKUP(C135,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NPSH 150 75 BLACK (Std) "}]
[null,null,"48664022","ASLT TIP 1.5NPSH 150G@50P",{"$f":"_xlfn.XLOOKUP(C136,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NPSH 150 50 BLACK (Std) "}]
[null,null,"48664093","ASLT TIP 1.5NPSH 150G@100P",{"$f":"_xlfn.XLOOKUP(C137,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NPSH 150 100 (Std) BLACK (Std) "}]
[null,null,"48664013","ASLT TIP 1.5NPSH 125G@75P",{"$f":"_xlfn.XLOOKUP(C138,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NPSH 125 75 BLACK (Std) "}]
[null,null,"48664015","ASLT TIP 1.5NPSH 125G@100P",{"$f":"_xlfn.XLOOKUP(C139,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NPSH 125 100 (Std) BLACK (Std) "}]
[null,null,"48664040","ASLT TIP 1.5NH 95G@100P RES-ENG 208",{"$f":"_xlfn.XLOOKUP(C140,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 95 100 (Std) BLACK (Std)  ETCH"}]
[null,null,"48664010","ASLT TIP 1.5NH 95G@100P",{"$f":"_xlfn.XLOOKUP(C141,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 95 100 (Std) BLACK (Std) "}]
[null,null,"48664058","ASLT TIP 1.5NH 200G@75P YLWBMPR",{"$f":"_xlfn.XLOOKUP(C142,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 200 75 YELLOW "}]
[null,null,"48664006","ASLT TIP 1.5NH 200G@75P",{"$f":"_xlfn.XLOOKUP(C143,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 200 75 BLACK (Std) "}]
[null,null,"48664075","ASLT TIP 1.5NH 200G@100P",{"$f":"_xlfn.XLOOKUP(C144,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 200 100 (Std) BLACK (Std) "}]
[null,null,"48664021","ASLT TIP 1.5NH 185G@50P YLWBMPR",{"$f":"_xlfn.XLOOKUP(C145,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 185 50 YELLOW "}]
[null,null,"48664011","ASLT TIP 1.5NH 185G@50P REDBMPR DURHAM",{"$f":"_xlfn.XLOOKUP(C146,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 185 50 RED  ETCH"}]
[null,null,"48664038","ASLT TIP 1.5NH 185G@50P REDBMPR",{"$f":"_xlfn.XLOOKUP(C147,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 185 50 RED "}]
[null,null,"48664016","ASLT TIP 1.5NH 185G@50P ORGBMPR WFD SEQ",{"$f":"_xlfn.XLOOKUP(C148,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 185 50 ORANGE  ETCH"}]
[null,null,"48664072","ASLT TIP 1.5NH 185G@50P ORGBMPR WFD 001S",{"$f":"_xlfn.XLOOKUP(C149,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 185 50 ORANGE  ETCH"}]
[null,null,"48664008","ASLT TIP 1.5NH 185G@50P ORGBMPR",{"$f":"_xlfn.XLOOKUP(C150,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 185 50 ORANGE "}]
[null,null,"48664027","ASLT TIP 1.5NH 185G@50P BLUEBMPR",{"$f":"_xlfn.XLOOKUP(C151,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 185 50 BLUE "}]
[null,null,"48664005","ASLT TIP 1.5NH 185G@50P#",{"$f":"_xlfn.XLOOKUP(C152,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 185 50 BLACK (Std) "}]
[null,null,"48664036","ASLT TIP 1.5NH 175G@75P YLWBMPR BCFD",{"$f":"_xlfn.XLOOKUP(C153,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 175 75 YELLOW  ETCH"}]
[null,null,"48664019","ASLT TIP 1.5NH 175G@75P YLWBMPR",{"$f":"_xlfn.XLOOKUP(C154,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 175 75 YELLOW "}]
[null,null,"48664031","ASLT TIP 1.5NH 175G@75P REDBMPR",{"$f":"_xlfn.XLOOKUP(C155,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 175 75 RED "}]
[null,null,"48664025","ASLT TIP 1.5NH 175G@75P ORGBMPR",{"$f":"_xlfn.XLOOKUP(C156,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 175 75 ORANGE "}]
[null,null,"48664024","ASLT TIP 1.5NH 175G@75P GRNBMPR",{"$f":"_xlfn.XLOOKUP(C157,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 175 75 GREEN "}]
[null,null,"48664030","ASLT TIP 1.5NH 175G@75P BLUEBMPR",{"$f":"_xlfn.XLOOKUP(C158,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 175 75 BLUE "}]
[null,null,"48664004","ASLT TIP 1.5NH 175G@75P#",{"$f":"_xlfn.XLOOKUP(C159,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 175 75 BLACK (Std) "}]
[null,null,"48664088","ASLT TIP1.5NH 175G@50P YLWBMPR COPLE VFD",{"$f":"_xlfn.XLOOKUP(C160,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 175 50 YELLOW PG ETCH"}]
[null,null,"48664069","ASLT TIP 1.5NH 175G@50P YLWBMPR FCFRD",{"$f":"_xlfn.XLOOKUP(C161,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 175 50 YELLOW  ETCH"}]
[null,null,"48664018","ASLT TIP 1.5NH 175G@50P YLWBMPR",{"$f":"_xlfn.XLOOKUP(C162,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 175 50 YELLOW "}]
[null,null,"48664051","ASLT TIP 1.5NH 175G@50P REDBMPR RBFR",{"$f":"_xlfn.XLOOKUP(C163,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 175 50 RED  ETCH"}]
[null,null,"48664089","ASLT TIP1.5NH 175G@50P ORGBMPR COPLE VFD",{"$f":"_xlfn.XLOOKUP(C164,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 175 50 ORANGE PG ETCH"}]
[null,null,"48664074","ASLT TIP 1.5NH 175G@50P ORGBMPR 1586",{"$f":"_xlfn.XLOOKUP(C165,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 175 50 ORANGE  ETCH"}]
[null,null,"48664050","ASLT TIP 1.5NH 175G@50P GRNBMPR RBFR",{"$f":"_xlfn.XLOOKUP(C166,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 175 50 GREEN  ETCH"}]
[null,null,"48664073","ASLT TIP 1.5NH 175G@50P BLUEBMPR 1585",{"$f":"_xlfn.XLOOKUP(C167,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 175 50 BLUE  ETCH"}]
[null,null,"48664090","ASLT TIP 1.5NH 175G@50P COPLE VFD",{"$f":"_xlfn.XLOOKUP(C168,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 175 50 BLACK (Std) PG ETCH"}]
[null,null,"48664081","ASLT TIP 1.5NH 175G@50P N1592",{"$f":"_xlfn.XLOOKUP(C169,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 175 50 BLACK (Std)  ETCH"}]
[null,null,"48664082","ASLT TIP 1.5NH 175G@50P N1593",{"$f":"_xlfn.XLOOKUP(C170,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 175 50 BLACK (Std)  ETCH"}]
[null,null,"48664014","ASLT TIP 1.5NH 175G@50P",{"$f":"_xlfn.XLOOKUP(C171,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 175 50 BLACK (Std) "}]
[null,null,"48664079","ASLT TIP 1.5NH 175G@100P",{"$f":"_xlfn.XLOOKUP(C172,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 175 100 (Std) BLACK (Std) "}]
[null,null,"48664062","ASLT TIP 1.5NH 161G@50P YLWBMPR WINGATE",{"$f":"_xlfn.XLOOKUP(C173,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 161 50 YELLOW  ETCH"}]
[null,null,"48664007","ASLT TIP 1.5NH 161G@50P YLWBMPR",{"$f":"_xlfn.XLOOKUP(C174,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 161 50 YELLOW "}]
[null,null,"48664064","ASLT TIP 1.5NH 161G@50P REDBMPR WINGATE",{"$f":"_xlfn.XLOOKUP(C175,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 161 50 RED  ETCH"}]
[null,null,"48664060","ASLT TIP 1.5NH 161G@50P REDBMPR",{"$f":"_xlfn.XLOOKUP(C176,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 161 50 RED "}]
[null,null,"48664056","ASLT TIP 1.5NH 161G@50P ORGBMPR",{"$f":"_xlfn.XLOOKUP(C177,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 161 50 ORANGE "}]
[null,null,"48664063","ASLT TIP 1.5NH 161G@50P GRNBMPR WINGATE",{"$f":"_xlfn.XLOOKUP(C178,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 161 50 GREEN  ETCH"}]
[null,null,"48664078","ASLTTIP 1.5NH 161@50 GRNBMPR SUMMERFIELD",{"$f":"_xlfn.XLOOKUP(C179,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 161 50 GREEN  ETCH"}]
[null,null,"48664009","ASLT TIP 1.5NH 161G@50P GRNBMPR",{"$f":"_xlfn.XLOOKUP(C180,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 161 50 GREEN "}]
[null,null,"48664039","ASLT TIP 1.5NH 161G@50P RES-ENG 208",{"$f":"_xlfn.XLOOKUP(C181,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 161 50 BLACK (Std)  ETCH"}]
[null,null,"48664047","ASLT TIP 1.5NH 161G@50P LCFR ENGINE 10",{"$f":"_xlfn.XLOOKUP(C182,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 161 50 BLACK (Std)  ETCH"}]
[null,null,"48664059","ASLT TIP 1.5NH 161G@50P ENO FD",{"$f":"_xlfn.XLOOKUP(C183,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 161 50 BLACK (Std)  ETCH"}]
[null,null,"48664061","ASLT TIP 1.5NH 161G@50P WINGATE",{"$f":"_xlfn.XLOOKUP(C184,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 161 50 BLACK (Std)  ETCH"}]
[null,null,"48664065","ASLT TIP 1.5NH 161G@50P LCFR ENGINE 20",{"$f":"_xlfn.XLOOKUP(C185,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 161 50 BLACK (Std)  ETCH"}]
[null,null,"48664066","ASLT TIP 1.5NH 161G@50P LCFR ENGINE 50",{"$f":"_xlfn.XLOOKUP(C186,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 161 50 BLACK (Std)  ETCH"}]
[null,null,"48664076","ASLT TIP 1.5NH 161G@50P WFD, E-31",{"$f":"_xlfn.XLOOKUP(C187,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 161 50 BLACK (Std)  ETCH"}]
[null,null,"48664003","ASLT TIP 1.5NH 161G@50P#",{"$f":"_xlfn.XLOOKUP(C188,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 161 50 BLACK (Std) "}]
[null,null,"48664020","ASLT TIP 1.5NH 150G@75P YLWBMPR",{"$f":"_xlfn.XLOOKUP(C189,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 150 75 YELLOW "}]
[null,null,"48664033","ASLT TIP 1.5NH 150G@75P REDBMPR",{"$f":"_xlfn.XLOOKUP(C190,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 150 75 RED "}]
[null,null,"48664032","ASLT TIP 1.5NH 150G@75P ORGBMPR",{"$f":"_xlfn.XLOOKUP(C191,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 150 75 ORANGE "}]
[null,null,"48664077","ASLT TIP 1.5NH 150G@75P GRNBMPR",{"$f":"_xlfn.XLOOKUP(C192,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 150 75 GREEN "}]
[null,null,"48664044","ASLT TIP 1.5NH 150G@75P BLUEBMPR",{"$f":"_xlfn.XLOOKUP(C193,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 150 75 BLUE "}]
[null,null,"48664023","ASLT TIP 1.5NH 150G@75P FINLEYFIRE.COM",{"$f":"_xlfn.XLOOKUP(C194,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 150 75 BLACK (Std)  ETCH"}]
[null,null,"48664002","ASLT TIP 1.5NH 150G@75P#",{"$f":"_xlfn.XLOOKUP(C195,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 150 75 BLACK (Std) "}]
[null,null,"48664017","ASLT TIP 1.5NH 150G@50P YLWBMPR WFD SEQ",{"$f":"_xlfn.XLOOKUP(C196,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 150 50 YELLOW  ETCH"}]
[null,null,"48664045","ASLT TIP 1.5NH 150G@50P YLWBMPR",{"$f":"_xlfn.XLOOKUP(C197,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 150 50 YELLOW "}]
[null,null,"48664071","ASLT TIP 1.5NH 150G@50P REDBMPR WFD SEQ",{"$f":"_xlfn.XLOOKUP(C198,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 150 50 RED  ETCH"}]
[null,null,"48664037","ASLT TIP 1.5NH 150G@50P REDBMPR",{"$f":"_xlfn.XLOOKUP(C199,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 150 50 RED "}]
[null,null,"48664046","ASLT TIP 1.5NH 150G@50P ORGBMPR",{"$f":"_xlfn.XLOOKUP(C200,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 150 50 ORANGE "}]
[null,null,"48664083","ASLT TIP 1.5NH 150G@50P GRNBMPR",{"$f":"_xlfn.XLOOKUP(C201,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 150 50 GREEN "}]
[null,null,"48664068","ASLT TIP 1.5NH 150G@50P BLUEBMPR",{"$f":"_xlfn.XLOOKUP(C202,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 150 50 BLUE "}]
[null,null,"48664049","ASLT TIP 1.5NH 150G@50P RICHMOND FD",{"$f":"_xlfn.XLOOKUP(C203,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 150 50 BLACK (Std)  ETCH"}]
[null,null,"48664001","ASLT TIP 1.5NH 150G@50P#",{"$f":"_xlfn.XLOOKUP(C204,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 150 50 BLACK (Std) "}]
[null,null,"48664029","ASLT TIP 1.5NH 150G@50P METAL TTH",{"$f":"_xlfn.XLOOKUP(C205,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 150 50 BLACK (Std) "}]
[null,null,"48664052","ASLT TIP 1.5NH 150G@100P REDBMPR",{"$f":"_xlfn.XLOOKUP(C206,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 150 100 (Std) RED "}]
[null,null,"48664054","ASLT TIP 1.5NH 150G@100P GRNBMPR",{"$f":"_xlfn.XLOOKUP(C207,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 150 100 (Std) GREEN "}]
[null,null,"48664053","ASLT TIP 1.5NH 150G@100P BLUEBMPR",{"$f":"_xlfn.XLOOKUP(C208,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 150 100 (Std) BLUE "}]
[null,null,"48664092","ASLT TIP 1.5NH 150G@100P BDVFD",{"$f":"_xlfn.XLOOKUP(C209,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 150 100 (Std) BLACK (Std) PG ETCH"}]
[null,null,"48664026","ASLT TIP 1.5NH 150G@100P",{"$f":"_xlfn.XLOOKUP(C210,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 150 100 (Std) BLACK (Std) "}]
[null,null,"48664087","ASLT TIP 1.5NH 125G@75P YLWBMPR",{"$f":"_xlfn.XLOOKUP(C211,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 125 75 YELLOW "}]
[null,null,"48664012","ASLT TIP 1.5NH 125G@75P",{"$f":"_xlfn.XLOOKUP(C212,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 125 75 BLACK (Std) "}]
[null,null,"48664057","ASLT TIP 1.5NH 125G@100P REDBMPR",{"$f":"_xlfn.XLOOKUP(C213,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 125 100 (Std) RED "}]
[null,null,"48664041","ASLT TIP 1.5NH 125G@100P GRNBMPR",{"$f":"_xlfn.XLOOKUP(C214,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 125 100 (Std) GREEN "}]
[null,null,"48664028","ASLT TIP 1.5NH 125G@100P",{"$f":"_xlfn.XLOOKUP(C215,DataSource!A:A,DataSource!AH:AH)","v":"4866 1.5 in NH 125 100 (Std) BLACK (Std) "}]
[null,null,"48634119","ASLT 75MM 750L@7b FM",{"$f":"_xlfn.XLOOKUP(C216,DataSource!A:A,DataSource!AH:AH)","v":"4863 3 in STORZ 750 7 BLACK (Std) PG"}]
[null,null,"48634071","ASLT 75MM 200G@75P FM",{"$f":"_xlfn.XLOOKUP(C217,DataSource!A:A,DataSource!AH:AH)","v":"4863 3 in STORZ 200 75 BLACK (Std) PG"}]
[null,null,"48634141","ASLT 2.5NH 95G@100P FM",{"$f":"_xlfn.XLOOKUP(C218,DataSource!A:A,DataSource!AH:AH)","v":"4863 2.5 in NH 95 100 (Std) BLACK (Std) PG"}]
[null,null,"48634153","ASLT 2.5NH 225G@100P GRNBMPR FM",{"$f":"_xlfn.XLOOKUP(C219,DataSource!A:A,DataSource!AH:AH)","v":"4863 2.5 in NH 225 100 (Std) GREEN PG"}]
[null,null,"48634140","ASLT 2.5NH 225G@100P ETCH JTFD 1",{"$f":"_xlfn.XLOOKUP(C220,DataSource!A:A,DataSource!AH:AH)","v":"4863 2.5 in NH 225 100 (Std) BLACK (Std) PG ETCH"}]
[null,null,"48634053","ASLT 2.5NH 225G@100P FM",{"$f":"_xlfn.XLOOKUP(C221,DataSource!A:A,DataSource!AH:AH)","v":"4863 2.5 in NH 225 100 (Std) BLACK (Std) PG"}]
[null,null,"48634079","ASLT 2.5NH 200G@75P FM",{"$f":"_xlfn.XLOOKUP(C222,DataSource!A:A,DataSource!AH:AH)","v":"4863 2.5 in NH 200 75 BLACK (Std) PG"}]
[null,null,"48637003","ASLT NPG 2.5NH 150G@50P FM",{"$f":"_xlfn.XLOOKUP(C223,DataSource!A:A,DataSource!AH:AH)","v":"4863 2.5 in NH 150 50 BLACK (Std) NPG"}]
[null,null,"48634138","ASLT 2.5NH 150G@100P FM",{"$f":"_xlfn.XLOOKUP(C224,DataSource!A:A,DataSource!AH:AH)","v":"4863 2.5 in NH 150 100 (Std) BLACK (Std) PG"}]
[null,null,"48634137","ASLT 2.5AII 185G@50P FM",{"$f":"_xlfn.XLOOKUP(C225,DataSource!A:A,DataSource!AH:AH)","v":"4863 2.5 in CSA 185 50 BLACK (Std) PG"}]
[null,null,"48634020","ASLT 2.5BIM 95G@100P FM",{"$f":"_xlfn.XLOOKUP(C226,DataSource!A:A,DataSource!AH:AH)","v":"4863 2.5 in BIM 95 100 (Std) BLACK (Std) PG"}]
[null,null,"48634002","ASLT 2.5BIM 750L@7b FM",{"$f":"_xlfn.XLOOKUP(C227,DataSource!A:A,DataSource!AH:AH)","v":"4863 2.5 in BIM 750 7 BLACK (Std) PG"}]
[null,null,"48634077","ASLT 2.5BIM 550L@7b FM",{"$f":"_xlfn.XLOOKUP(C228,DataSource!A:A,DataSource!AH:AH)","v":"4863 2.5 in BIM 550 7 BLACK (Std) PG"}]
[null,null,"48634078","ASLT 2.5BIM 475L@7b FM",{"$f":"_xlfn.XLOOKUP(C229,DataSource!A:A,DataSource!AH:AH)","v":"4863 2.5 in BIM 475 7 BLACK (Std) PG"}]
[null,null,"48634044","ASLT 2.5BIM 475L@4b MTLTH,DETENT",{"$f":"_xlfn.XLOOKUP(C230,DataSource!A:A,DataSource!AH:AH)","v":"4863 2.5 in BIM 475 4 Black (Std) PG"}]
[null,null,"48634147","ASLT 2.5BIM 200G@100P FM",{"$f":"_xlfn.XLOOKUP(C231,DataSource!A:A,DataSource!AH:AH)","v":"4863 2.5 in BIM 200 100 (Std) BLACK (Std) PG"}]
[null,null,"48634021","ASLT 2.5BIM 150G@100P FM",{"$f":"_xlfn.XLOOKUP(C232,DataSource!A:A,DataSource!AH:AH)","v":"4863 2.5 in BIM 150 100 (Std) BLACK (Std) PG"}]
[null,null,"48634102","ASLT 2.5BAF 225G@100P FM",{"$f":"_xlfn.XLOOKUP(C233,DataSource!A:A,DataSource!AH:AH)","v":"4863 2.5 in BAT 225 100 (Std) BLACK (Std) PG"}]
[null,null,"48634097","ASLT 2.5BAF 125G@75P FM",{"$f":"_xlfn.XLOOKUP(C234,DataSource!A:A,DataSource!AH:AH)","v":"4863 2.5 in BAT 125 75 BLACK (Std) PG"}]
[null,null,"48634116","ASLT 52MM 750L@7b FM",{"$f":"_xlfn.XLOOKUP(C235,DataSource!A:A,DataSource!AH:AH)","v":"4863 2 in STORZ 750 7 BLACK (Std) PG"}]
[null,null,"48634073","ASLT 52MM 550L@7b FM",{"$f":"_xlfn.XLOOKUP(C236,DataSource!A:A,DataSource!AH:AH)","v":"4863 2 in STORZ 550 7 BLACK (Std) PG"}]
[null,null,"48634095","ASLT 52MM 475L@7b FM",{"$f":"_xlfn.XLOOKUP(C237,DataSource!A:A,DataSource!AH:AH)","v":"4863 2 in STORZ 475 7 BLACK (Std) PG"}]
[null,null,"48634072","ASLT 52MM 360L@7b FM",{"$f":"_xlfn.XLOOKUP(C238,DataSource!A:A,DataSource!AH:AH)","v":"4863 2 in STORZ 360 7 BLACK (Std) PG"}]
[null,null,"48634100","ASLT 38MM 95G@100P FM",{"$f":"_xlfn.XLOOKUP(C239,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in STORZ 95 100 (Std) BLACK (Std) PG"}]
[null,null,"48634155","ASLT 38MM 750LPM@345KPA",{"$f":"_xlfn.XLOOKUP(C240,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in STORZ 750 345 BLACK (Std) PG"}]
[null,null,"48634115","ASLT 38MM 150G@50P",{"$f":"_xlfn.XLOOKUP(C241,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in STORZ 150 50 BLACK (Std) PG"}]
[null,null,"48634075","ASLT 1.5ABT 175G@75P FM",{"$f":"_xlfn.XLOOKUP(C242,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in PCT 175 75 BLACK (Std) PG"}]
[null,null,"48634118","ASLT 1.5ABT 161G@50P FM",{"$f":"_xlfn.XLOOKUP(C243,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in PCT 161 50 BLACK (Std) PG"}]
[null,null,"48634057","ASLT 1.5NPSH 95G@100P FM",{"$f":"_xlfn.XLOOKUP(C244,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NPSH 95 100 (Std) BLACK (Std) PG"}]
[null,null,"48634067","ASLT 1.5NPSH 570L@350K",{"$f":"_xlfn.XLOOKUP(C245,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NPSH 570 350 BLACK (Std) PG"}]
[null,null,"48634058","ASLT 1.5NPSH 550L@500K REDBMPR FM",{"$f":"_xlfn.XLOOKUP(C246,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NPSH 550 500 RED PG"}]
[null,null,"48634050","ASLT 1.5NPSH 550L@500K FM",{"$f":"_xlfn.XLOOKUP(C247,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NPSH 550 500 BLACK (Std) PG"}]
[null,null,"48634042","ASLT 1.5NPSH 550L@345K FM",{"$f":"_xlfn.XLOOKUP(C248,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NPSH 550 345 BLACK (Std) PG"}]
[null,null,"48634149","ASLT 1.5NPSH 475L@500K FM",{"$f":"_xlfn.XLOOKUP(C249,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NPSH 475 500 BLACK (Std) PG"}]
[null,null,"48634090","ASLT 1.5NPSH 360L@700K FM",{"$f":"_xlfn.XLOOKUP(C250,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NPSH 360 700 BLACK (Std) PG"}]
[null,null,"48637090","ASLT NPG 1.5NPSH 360L@700K FM",{"$f":"_xlfn.XLOOKUP(C251,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NPSH 360 700 BLACK (Std) NPG"}]
[null,null,"48634059","ASLT 1.5NPSH 360L@7b FM",{"$f":"_xlfn.XLOOKUP(C252,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NPSH 360 7 BLACK (Std) PG"}]
[null,null,"48634089","ASLT 1.5NPSH 200G@75P FM",{"$f":"_xlfn.XLOOKUP(C253,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NPSH 200 75 BLACK (Std) PG"}]
[null,null,"48634113","ASLT 1.5NPSH 200G@100P FM",{"$f":"_xlfn.XLOOKUP(C254,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NPSH 200 100 (Std) BLACK (Std) PG"}]
[null,null,"48637113","ASLT NPG 1.5NPSH 200G@100P FM",{"$f":"_xlfn.XLOOKUP(C255,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NPSH 200 100 (Std) BLACK (Std) NPG"}]
[null,null,"48634066","ASLT 1.5NPSH 185G@50P FM",{"$f":"_xlfn.XLOOKUP(C256,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NPSH 185 50 BLACK (Std) PG"}]
[null,null,"48634093","ASLT 1.5NPSH 175G@75P FM",{"$f":"_xlfn.XLOOKUP(C257,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NPSH 175 75 BLACK (Std) PG"}]
[null,null,"48634092","ASLT 1.5NPSH 175G@100P FM",{"$f":"_xlfn.XLOOKUP(C258,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NPSH 175 100 (Std) BLACK (Std) PG"}]
[null,null,"48634084","ASLT 1.5NPSH 161G@50P FM",{"$f":"_xlfn.XLOOKUP(C259,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NPSH 161 50 BLACK (Std) PG"}]
[null,null,"48637084","ASLT NPG 1.5NPSH 161G@50P FM",{"$f":"_xlfn.XLOOKUP(C260,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NPSH 161 50 BLACK (Std) NPG"}]
[null,null,"48634091","ASLT 1.5NPSH 150G@75P ORGBMPR FM",{"$f":"_xlfn.XLOOKUP(C261,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NPSH 150 75 ORANGE PG"}]
[null,null,"48634025","ASLT 1.5NPSH 150G@75P FM",{"$f":"_xlfn.XLOOKUP(C262,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NPSH 150 75 BLACK (Std) PG"}]
[null,null,"48634011","ASLT 1.5NPSH 150G@50P FM",{"$f":"_xlfn.XLOOKUP(C263,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NPSH 150 50 BLACK (Std) PG"}]
[null,null,"48634047","ASLT 1.5NPSH 150G@100P FM",{"$f":"_xlfn.XLOOKUP(C264,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NPSH 150 100 (Std) BLACK (Std) PG"}]
[null,null,"48637047","ASLT NPG 1.5NPSH 150G@100P FM",{"$f":"_xlfn.XLOOKUP(C265,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NPSH 150 100 (Std) BLACK (Std) NPG"}]
[null,null,"48634099","ASLT ZT 1.5NPSH 125G@75P",{"$f":"_xlfn.XLOOKUP(C266,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NPSH 125 75 BLACK (Std) PG ZT"}]
[null,null,"48634027","ASLT 1.5NPSH 125G@75P FM",{"$f":"_xlfn.XLOOKUP(C267,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NPSH 125 75 BLACK (Std) PG"}]
[null,null,"48634046","ASLT 1.5NPSH 125G@100P GRNBMPR FM",{"$f":"_xlfn.XLOOKUP(C268,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NPSH 125 100 (Std) GREEN PG"}]
[null,null,"48634070","ASLT 1.5NPSH 125G@100P FM",{"$f":"_xlfn.XLOOKUP(C269,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NPSH 125 100 (Std) BLACK (Std) PG"}]
[null,null,"48634019","ASLT 1.5NH 95G@100P FM",{"$f":"_xlfn.XLOOKUP(C270,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 95 100 (Std) BLACK (Std) PG"}]
[null,null,"48637019","ASLT NPG 1.5NH 95G@100P FM",{"$f":"_xlfn.XLOOKUP(C271,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 95 100 (Std) BLACK (Std) NPG"}]
[null,null,"48634105","ASLT 1.5NH 550L@5b FM",{"$f":"_xlfn.XLOOKUP(C272,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 550 5 BLACK (Std) PG"}]
[null,null,"48634052","ASLT 1.5NH 225G@100P FM",{"$f":"_xlfn.XLOOKUP(C273,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 225 100 (Std) BLACK (Std) PG"}]
[null,null,"48634101","ASLT 1.5NH 200G@75P REDBMPR 01535",{"$f":"_xlfn.XLOOKUP(C274,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 200 75 RED PG ETCH"}]
[null,null,"48634081","ASLT 1.5NH 200G@75P ORGBMPR FM",{"$f":"_xlfn.XLOOKUP(C275,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 200 75 ORANGE PG"}]
[null,null,"48634080","ASLT 1.5NH 200G@75P BLUEBMPR FM",{"$f":"_xlfn.XLOOKUP(C276,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 200 75 BLUE PG"}]
[null,null,"48634041","ASLT 1.5NH 200G@75P NCFD L-204",{"$f":"_xlfn.XLOOKUP(C277,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 200 75 BLACK (Std) PG ETCH"}]
[null,null,"48634001","ASLT 1.5NH 200G@75P FM#",{"$f":"_xlfn.XLOOKUP(C278,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 200 75 BLACK (Std) PG"}]
[null,null,"48637002","ASLT NPG 1.5NH 200G@75P FM",{"$f":"_xlfn.XLOOKUP(C279,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 200 75 BLACK (Std) NPG"}]
[null,null,"48634133","ASLT 1.5NH 200G@50P FM",{"$f":"_xlfn.XLOOKUP(C280,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 200 50 BLACK (Std) PG"}]
[null,null,"48634152","ASLT 1.5NH 200G@100P YLWBMPR FM",{"$f":"_xlfn.XLOOKUP(C281,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 200 100 (Std) YELLOW PG"}]
[null,null,"48634150","ASLT 1.5NH 200G@100P REDBMPR FM",{"$f":"_xlfn.XLOOKUP(C282,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 200 100 (Std) RED PG"}]
[null,null,"48634151","ASLT 1.5NH 200G@100P BLUEBMPR FM",{"$f":"_xlfn.XLOOKUP(C283,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 200 100 (Std) BLUE PG"}]
[null,null,"48634082","ASLT ZT 1.5NH 200G@100P",{"$f":"_xlfn.XLOOKUP(C284,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 200 100 (Std) BLACK (Std) PG ZT"}]
[null,null,"48634010","ASLT 1.5NH 200G@100P FM",{"$f":"_xlfn.XLOOKUP(C285,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 200 100 (Std) BLACK (Std) PG"}]
[null,null,"48634144","ASLT 2.5NH 125G@100P FM",{"$f":"_xlfn.XLOOKUP(C286,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 200 100 (Std) BLACK (Std) PG"}]
[null,null,"48637010","ASLT NPG 1.5NH 200G@100P FM",{"$f":"_xlfn.XLOOKUP(C287,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 200 100 (Std) BLACK (Std) NPG"}]
[null,null,"48637024","ASLT 1.5NH 185G@50P YLWBMPR FM",{"$f":"_xlfn.XLOOKUP(C288,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 185 50 YELLOW PG"}]
[null,null,"48637015","ASLT 1.5NH 185G@50P REDBMPR FM",{"$f":"_xlfn.XLOOKUP(C289,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 185 50 RED PG"}]
[null,null,"48637025","ASLT 1.5NH 185G@50P ORGBMPR FM",{"$f":"_xlfn.XLOOKUP(C290,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 185 50 ORANGE PG"}]
[null,null,"48634017","ASLT 1.5NH 185G@50P GRNBMPR FM",{"$f":"_xlfn.XLOOKUP(C291,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 185 50 GREEN PG"}]
[null,null,"48637023","ASLT 1.5NH 185G@50P BLUEBMPR FM",{"$f":"_xlfn.XLOOKUP(C292,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 185 50 BLUE PG"}]
[null,null,"48634139","ASLT 1.5NH 185G@50P ETCH JTFD 1",{"$f":"_xlfn.XLOOKUP(C293,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 185 50 BLACK (Std) PG ETCH"}]
[null,null,"48634026","ASLT 1.5NH 185G@50P FM",{"$f":"_xlfn.XLOOKUP(C294,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 185 50 BLACK (Std) PG"}]
[null,null,"48637026","ASLT NPG 1.5NH 185G@50P FM",{"$f":"_xlfn.XLOOKUP(C295,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 185 50 BLACK (Std) NPG"}]
[null,null,"48634035","ASLT 1.5NH 175G@75P YLWBMPR FM",{"$f":"_xlfn.XLOOKUP(C296,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 175 75 YELLOW PG"}]
[null,null,"48634051","ASLT 1.5NH 175G@75P REDBMPR FM",{"$f":"_xlfn.XLOOKUP(C297,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 175 75 RED PG"}]
[null,null,"48634036","ASLT 1.5NH 175G@75P ORGBMPR FM",{"$f":"_xlfn.XLOOKUP(C298,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 175 75 ORANGE PG"}]
[null,null,"48634060","ASLT 1.5NH 175G@75P GRNBMPR FM",{"$f":"_xlfn.XLOOKUP(C299,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 175 75 GREEN PG"}]
[null,null,"48634065","ASLT ZT 1.5NH 175G@75P BLUEBMPR",{"$f":"_xlfn.XLOOKUP(C300,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 175 75 BLUE PG ZT"}]
[null,null,"48634034","ASLT 1.5NH 175G@75P BLUEBMPR FM",{"$f":"_xlfn.XLOOKUP(C301,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 175 75 BLUE PG"}]
[null,null,"48634030","ASLT 1.5NH 175G@75P NYA FD",{"$f":"_xlfn.XLOOKUP(C302,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 175 75 BLACK (Std) PG ETCH"}]
[null,null,"48634055","ASLT 1.5NH 175G@75P HARVARD",{"$f":"_xlfn.XLOOKUP(C303,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 175 75 BLACK (Std) PG ETCH"}]
[null,null,"48634063","ASLT 1.5NH 175G@75P TEMPLETON",{"$f":"_xlfn.XLOOKUP(C304,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 175 75 BLACK (Std) PG ETCH"}]
[null,null,"48634064","ASLT 1.5NH 175G@75P SHERBORN",{"$f":"_xlfn.XLOOKUP(C305,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 175 75 BLACK (Std) PG ETCH"}]
[null,null,"48634009","ASLT 1.5NH 175G@75P FM#",{"$f":"_xlfn.XLOOKUP(C306,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 175 75 BLACK (Std) PG"}]
[null,null,"48637009","ASLT NPG 1.5NH 175G@75P FM",{"$f":"_xlfn.XLOOKUP(C307,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 175 75 BLACK (Std) NPG"}]
[null,null,"48634039","ASLT 1.5NH 175G@50P YLWBMPR FM",{"$f":"_xlfn.XLOOKUP(C308,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 175 50 YELLOW PG"}]
[null,null,"48634145","ASLT 1.5NH 175G@50P ORGBMPR OCEAN VIEW",{"$f":"_xlfn.XLOOKUP(C309,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 175 50 ORANGE PG ETCH"}]
[null,null,"48634117","ASLT 1.5NH 175G@50P ORGBMPR FM",{"$f":"_xlfn.XLOOKUP(C310,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 175 50 ORANGE PG"}]
[null,null,"48634124","ASLT 1.5NH 175G@50P BLUBMPR FM",{"$f":"_xlfn.XLOOKUP(C311,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 175 50 BLUE PG"}]
[null,null,"48634120","ASLT 1.5NH 175G@50P SEQ ETCH FG15-21-001",{"$f":"_xlfn.XLOOKUP(C312,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 175 50 BLACK (Std) PG ETCH"}]
[null,null,"48634136","ASLT 1.5NH 175G@50P FORK FD LOGO",{"$f":"_xlfn.XLOOKUP(C313,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 175 50 BLACK (Std) PG ETCH"}]
[null,null,"48634028","ASLT 1.5NH 175G@50P FM",{"$f":"_xlfn.XLOOKUP(C314,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 175 50 BLACK (Std) PG"}]
[null,null,"48637028","ASLT NPG 1.5NH 175G@50P FM",{"$f":"_xlfn.XLOOKUP(C315,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 175 50 BLACK (Std) NPG"}]
[null,null,"48634054","ASLT 1.5NH 175G@100P FM",{"$f":"_xlfn.XLOOKUP(C316,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 175 100 (Std) BLACK (Std) PG"}]
[null,null,"48637054","ASLT NPG 1.5NH 175G@100P FM",{"$f":"_xlfn.XLOOKUP(C317,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 175 100 (Std) BLACK (Std) NPG"}]
[null,null,"48634016","ASLT 1.5NH 161G@50P BLUEBMPR FM",{"$f":"_xlfn.XLOOKUP(C318,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 161 50 BLUE PG"}]
[null,null,"48634031","ASLT 1.5NH 161G@50P CLEVELAND",{"$f":"_xlfn.XLOOKUP(C319,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 161 50 BLACK (Std) PG ETCH"}]
[null,null,"48634062","ASLT 1.5NH 161G@50P  RES-ENG 208",{"$f":"_xlfn.XLOOKUP(C320,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 161 50 BLACK (Std) PG ETCH"}]
[null,null,"48634038","ASLT 1.5NH 161G@50P FM",{"$f":"_xlfn.XLOOKUP(C321,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 161 50 BLACK (Std) PG"}]
[null,null,"48637014","ASLT NPG 1.5NH 161G@50P CLEVELAND VFD",{"$f":"_xlfn.XLOOKUP(C322,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 161 50 BLACK (Std) NPG ETCH"}]
[null,null,"48637038","ASLT NPG 1.5NH 161G@50P FM",{"$f":"_xlfn.XLOOKUP(C323,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 161 50 BLACK (Std) NPG"}]
[null,null,"48634023","ASLT 1.5NH 150G@75P YLWBMPR BFC 1",{"$f":"_xlfn.XLOOKUP(C324,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 150 75 YELLOW PG ETCH"}]
[null,null,"48634032","ASLT 1.5NH 150G@75P YLWBMPR FM",{"$f":"_xlfn.XLOOKUP(C325,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 150 75 YELLOW PG"}]
[null,null,"48634024","ASLT 1.5NH 150G@75P REDBMPR BFC 1",{"$f":"_xlfn.XLOOKUP(C326,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 150 75 RED PG ETCH"}]
[null,null,"48634037","ASLT 1.5NH 150G@75P REDBMPR FM",{"$f":"_xlfn.XLOOKUP(C327,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 150 75 RED PG"}]
[null,null,"48634114","ASLT 1.5NH 150G@75P ORGBMPR FM",{"$f":"_xlfn.XLOOKUP(C328,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 150 75 ORANGE PG"}]
[null,null,"48637001","ASLT NPG 1.5NH 150G@75P ORGBMPR OAK",{"$f":"_xlfn.XLOOKUP(C329,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 150 75 ORANGE NPG ETCH"}]
[null,null,"48637065","ASLT NPG 1.5NH 150@75 ORGBMPR CHARLOTTE",{"$f":"_xlfn.XLOOKUP(C330,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 150 75 ORANGE NPG ETCH"}]
[null,null,"48634098","ASLT 1.5NH 150G@75P GRNBMPR FM",{"$f":"_xlfn.XLOOKUP(C331,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 150 75 GREEN PG"}]
[null,null,"48637098","ASLT NPG 1.5NH 150G@75P GRN BMPR FM",{"$f":"_xlfn.XLOOKUP(C332,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 150 75 GREEN NPG"}]
[null,null,"48634104","ASLT 1.5NH 150G@75P BLUEBMPR FM",{"$f":"_xlfn.XLOOKUP(C333,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 150 75 BLUE PG"}]
[null,null,"48634146","ASLT ZT 1.5NH 150G@75P",{"$f":"_xlfn.XLOOKUP(C334,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 150 75 BLACK (Std) PG ZT"}]
[null,null,"48634043","ASLT 1.5NH 150G@75P FINLEYFIRE.COM",{"$f":"_xlfn.XLOOKUP(C335,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 150 75 BLACK (Std) PG ETCH"}]
[null,null,"48634008","ASLT 1.5NH 150G@75P FM#",{"$f":"_xlfn.XLOOKUP(C336,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 150 75 BLACK (Std) PG"}]
[null,null,"48634094","ASLT 1.5NH 150G@75P D.F.D.",{"$f":"_xlfn.XLOOKUP(C337,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 150 75 BLACK (Std) PG"}]
[null,null,"48634126","ASLT 1.5NH 150@75P MTLTH YLWBMPR",{"$f":"_xlfn.XLOOKUP(C338,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 150 75 BLACK (Std) PG"}]
[null,null,"48637008","ASLT NPG 1.5NH 150G@75P FM",{"$f":"_xlfn.XLOOKUP(C339,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 150 75 BLACK (Std) NPG"}]
[null,null,"48634045","ASLT 1.5NH 150G@50P YLWBMPR FM",{"$f":"_xlfn.XLOOKUP(C340,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 150 50 YELLOW PG"}]
[null,null,"48637045","ASLT NPG 1.5NH 150G@50P YLWBMPR FM",{"$f":"_xlfn.XLOOKUP(C341,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 150 50 YELLOW NPG"}]
[null,null,"48634109","ASLT 1.5NH 150G@50P REDBMPR RFD STATION6",{"$f":"_xlfn.XLOOKUP(C342,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 150 50 RED PG ETCH"}]
[null,null,"48634106","ASLT 1.5NH 150G@50P REDBMPR FM",{"$f":"_xlfn.XLOOKUP(C343,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 150 50 RED PG"}]
[null,null,"48637064","ASLT NPG 1.5NH 150@50 REDBMPR CHARLOTTE",{"$f":"_xlfn.XLOOKUP(C344,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 150 50 RED NPG ETCH"}]
[null,null,"48637004","ASLT NPG 1.5NH 150G@50P REDBMPR FM",{"$f":"_xlfn.XLOOKUP(C345,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 150 50 RED NPG"}]
[null,null,"48634110","ASLT 1.5NH 150G@50P ORGBMPR RFD STATION6",{"$f":"_xlfn.XLOOKUP(C346,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 150 50 ORANGE PG ETCH"}]
[null,null,"48634127","ASLT 1.5NH 150G@50P ORGBMPR BFC-E1",{"$f":"_xlfn.XLOOKUP(C347,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 150 50 ORANGE PG ETCH"}]
[null,null,"48634056","ASLT 1.5NH 150G@50P ORGBMPR FM",{"$f":"_xlfn.XLOOKUP(C348,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 150 50 ORANGE PG"}]
[null,null,"48637063","ASLT NPG 1.5NH 150@50 ORGBMPR CHARLOTTE",{"$f":"_xlfn.XLOOKUP(C349,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 150 50 ORANGE NPG ETCH"}]
[null,null,"48634111","ASLT 1.5NH 150G@50P GRNBMPR RFD STATION6",{"$f":"_xlfn.XLOOKUP(C350,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 150 50 GREEN PG ETCH"}]
[null,null,"48634128","ASLT 1.5NH 150G@50P GRNBMPR BFC-E1",{"$f":"_xlfn.XLOOKUP(C351,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 150 50 GREEN PG ETCH"}]
[null,null,"48634132","ASLT 1.5NH 150G@50P GRNBMPR BFC-E2",{"$f":"_xlfn.XLOOKUP(C352,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 150 50 GREEN PG ETCH"}]
[null,null,"48634107","ASLT 1.5NH 150G@50P GRNBMPR FM",{"$f":"_xlfn.XLOOKUP(C353,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 150 50 GREEN PG"}]
[null,null,"48634108","ASLT 1.5NH 150G@50P BLUBMPR RFD STATION6",{"$f":"_xlfn.XLOOKUP(C354,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 150 50 BLUE PG ETCH"}]
[null,null,"48634129","ASLT 1.5NH 150G@50P BLUBMPR BFC-E1",{"$f":"_xlfn.XLOOKUP(C355,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 150 50 BLUE PG ETCH"}]
[null,null,"48634130","ASLT 1.5NH 150G@50P BLUBMPR BFC-T5",{"$f":"_xlfn.XLOOKUP(C356,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 150 50 BLUE PG ETCH"}]
[null,null,"48634131","ASLT 1.5NH 150G@50P BLUBMPR BFC-E2",{"$f":"_xlfn.XLOOKUP(C357,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 150 50 BLUE PG ETCH"}]
[null,null,"48634033","ASLT 1.5NH 150G@50P BLUEBMPR FM",{"$f":"_xlfn.XLOOKUP(C358,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 150 50 BLUE PG"}]
[null,null,"48634029","ASLT 1.5NH 150G@50P FM#",{"$f":"_xlfn.XLOOKUP(C359,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 150 50 BLACK (Std) PG"}]
[null,null,"48637029","ASLT NPG 1.5NH 150G@50P FM",{"$f":"_xlfn.XLOOKUP(C360,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 150 50 BLACK (Std) NPG"}]
[null,null,"48634076","ASLT 1.5NH 150G@100P YLWBMPR FM",{"$f":"_xlfn.XLOOKUP(C361,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 150 100 (Std) YELLOW PG"}]
[null,null,"48634086","ASLT 1.5NH 150G@100P REDBMPR FM",{"$f":"_xlfn.XLOOKUP(C362,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 150 100 (Std) RED PG"}]
[null,null,"48634069","ASLT 1.5NH 150G@100P ORGBMPR FM",{"$f":"_xlfn.XLOOKUP(C363,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 150 100 (Std) ORANGE PG"}]
[null,null,"48634068","ASLT 1.5NH 150G@100P GRNBMPR FM",{"$f":"_xlfn.XLOOKUP(C364,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 150 100 (Std) GREEN PG"}]
[null,null,"48634085","ASLT 1.5NH 150G@100P BLUEBMPR FM",{"$f":"_xlfn.XLOOKUP(C365,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 150 100 (Std) BLUE PG"}]
[null,null,"48634040","ASLT 1.5NH 150G@100P GASTONIA FD",{"$f":"_xlfn.XLOOKUP(C366,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 150 100 (Std) BLACK (Std) PG ETCH"}]
[null,null,"48634007","ASLT 1.5NH 150G@100P FM#",{"$f":"_xlfn.XLOOKUP(C367,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 150 100 (Std) BLACK (Std) PG"}]
[null,null,"48637040","ASLT NPG 1.5NH 150G@100P GASTONIA FD",{"$f":"_xlfn.XLOOKUP(C368,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 150 100 (Std) BLACK (Std) NPG ETCH"}]
[null,null,"48637007","ASLT NPG 1.5NH 150G@100P FM",{"$f":"_xlfn.XLOOKUP(C369,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 150 100 (Std) BLACK (Std) NPG"}]
[null,null,"48634103","ASLT 1.5NH 125G@75P REDBMPR FM",{"$f":"_xlfn.XLOOKUP(C370,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 125 75 RED PG"}]
[null,null,"48634096","ASLT 1.5NH 125G@75P GRNBMPR FM",{"$f":"_xlfn.XLOOKUP(C371,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 125 75 GREEN PG"}]
[null,null,"48634005","ASLT 1.5NH 125G@75P FM",{"$f":"_xlfn.XLOOKUP(C372,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 125 75 BLACK (Std) PG"}]
[null,null,"48637005","ASLT NPG 1.5NH 125G@75P FM",{"$f":"_xlfn.XLOOKUP(C373,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 125 75 BLACK (Std) NPG"}]
[null,null,"48634083","ASLT 1.5NH 125G@100P ENO FD",{"$f":"_xlfn.XLOOKUP(C374,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 125 100 (Std) BLACK (Std) PG ETCH"}]
[null,null,"48634006","ASLT 1.5NH 125G@100P FM",{"$f":"_xlfn.XLOOKUP(C375,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 125 100 (Std) BLACK (Std) PG"}]
[null,null,"48637006","ASLT NPG 1.5NH 125G@100P FM",{"$f":"_xlfn.XLOOKUP(C376,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in NH 125 100 (Std) BLACK (Std) NPG"}]
[null,null,"48634061","ASLT 1.5ABU 200G@100P FDNY",{"$f":"_xlfn.XLOOKUP(C377,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in FDNY 200 100 (Std) BLACK (Std) PG"}]
[null,null,"48637061","ASLT NPG 1.5ABU 200G@100P FDNY",{"$f":"_xlfn.XLOOKUP(C378,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in FDNY 200 100 (Std) BLACK (Std) NPG"}]
[null,null,"48634013","ASLT 1.5BSP 750L@7b FM",{"$f":"_xlfn.XLOOKUP(C379,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in BSP 750 7 BLACK (Std) PG"}]
[null,null,"48634022","ASLT 1.5BSP 550L@5b FM",{"$f":"_xlfn.XLOOKUP(C380,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in BSP 550 5 BLACK (Std) PG"}]
[null,null,"48634012","ASLT 1.5BSP 475L@7b FM",{"$f":"_xlfn.XLOOKUP(C381,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in BSP 475 7 BLACK (Std) PG"}]
[null,null,"48634018","ASLT 1.5BSP 360L@7b FM",{"$f":"_xlfn.XLOOKUP(C382,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in BSP 360 7 BLACK (Std) PG"}]
[null,null,"48634135","ASLT 1.5BSP 150G@100P FM",{"$f":"_xlfn.XLOOKUP(C383,DataSource!A:A,DataSource!AH:AH)","v":"4863 1.5 in BSP 150 100 (Std) BLACK (Std) PG"}]
[null,null,"48267023","ASLT NPG 2.5AFY 300G@100P STA 236",{"$f":"_xlfn.XLOOKUP(C384,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in PITT6 300 100 (Std) BLACK (Std) NPG ETCH"}]
[null,null,"48267044","ASLT NPG 2.5AFY 250G@75P FM",{"$f":"_xlfn.XLOOKUP(C385,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in PITT6 250 75 BLACK (Std) NPG"}]
[null,null,"48264042","ASLT 2.5AFY 250G@50P FM",{"$f":"_xlfn.XLOOKUP(C386,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in PITT6 250 50 BLACK (Std) PG"}]
[null,null,"48267039","ASLT NPG 2.5AFY 250G@100P FM",{"$f":"_xlfn.XLOOKUP(C387,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in PITT6 250 100 (Std) BLACK (Std) NPG"}]
[null,null,"48264010","ASLT 2.5NH 950L@7b FM",{"$f":"_xlfn.XLOOKUP(C388,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in NH 950 7 BLACK (Std) PG"}]
[null,null,"48264016","ASLT 2.5NH 350G@100P YLWBMPR BCFD",{"$f":"_xlfn.XLOOKUP(C389,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in NH 350 100 (Std) YELLOW PG ETCH"}]
[null,null,"48267029","ASLT NPG 2.5NH 350G@100P YLWBMPR BCFD",{"$f":"_xlfn.XLOOKUP(C390,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in NH 350 100 (Std) YELLOW NPG ETCH"}]
[null,null,"48264009","ASLT 2.5NH 350G@100P FM",{"$f":"_xlfn.XLOOKUP(C391,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in NH 350 100 (Std) BLACK (Std) PG"}]
[null,null,"48264013","ASLT 2.5NH 300G@75P FM",{"$f":"_xlfn.XLOOKUP(C392,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in NH 300 75 BLACK (Std) PG"}]
[null,null,"48267013","ASLT NPG 2.5NH 300G@75P FM",{"$f":"_xlfn.XLOOKUP(C393,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in NH 300 75 BLACK (Std) NPG"}]
[null,null,"48264021","ASLT 2.5NH 300G@100P FM",{"$f":"_xlfn.XLOOKUP(C394,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in NH 300 100 (Std) BLACK (Std) PG"}]
[null,null,"48267002","ASLT NPG 2.5NH 300G@100P FM",{"$f":"_xlfn.XLOOKUP(C395,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in NH 300 100 (Std) BLACK (Std) NPG"}]
[null,null,"48264036","ASLT 2.5NH 250G@75P YLWBMPR FM",{"$f":"_xlfn.XLOOKUP(C396,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in NH 250 75 YELLOW PG"}]
[null,null,"48264053","ASLT 2.5NH 250G@75P ORGBMPR FM",{"$f":"_xlfn.XLOOKUP(C397,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in NH 250 75 ORANGE PG"}]
[null,null,"48267016","ASLT NPG 2.5NH 250@75 ORGBMPR CHARLOTTE",{"$f":"_xlfn.XLOOKUP(C398,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in NH 250 75 ORANGE NPG ETCH"}]
[null,null,"48264012","ASLT ZT 2.5NH 250G@75P",{"$f":"_xlfn.XLOOKUP(C399,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in NH 250 75 Black (Std) PG ZT"}]
[null,null,"48264023","ASLT 2.5NH 250G@75P SHERBORN",{"$f":"_xlfn.XLOOKUP(C400,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in NH 250 75 BLACK (Std) PG ETCH"}]
[null,null,"48264007","ASLT 2.5NH 250G@75P FM",{"$f":"_xlfn.XLOOKUP(C401,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in NH 250 75 BLACK (Std) PG"}]
[null,null,"48267007","ASLT NPG 2.5NH 250G@75P FM",{"$f":"_xlfn.XLOOKUP(C402,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in NH 250 75 BLACK (Std) NPG"}]
[null,null,"48267030","ASLT NPG 2.5NH 250G@75P W/MTLHDL",{"$f":"_xlfn.XLOOKUP(C403,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in NH 250 75 Black (Std) NPG"}]
[null,null,"48264028","ASLT 2.5NH 250G@50P YLWBMPR FM",{"$f":"_xlfn.XLOOKUP(C404,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in NH 250 50 YELLOW PG"}]
[null,null,"48267028","ASLT NPG 2.5NH 250G@50P YLWBMPR FM",{"$f":"_xlfn.XLOOKUP(C405,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in NH 250 50 YELLOW NPG"}]
[null,null,"48267001","ASLT NPG 2.5NH 250G@50P ORGBMPR OAK",{"$f":"_xlfn.XLOOKUP(C406,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in NH 250 50 ORANGE NPG ETCH"}]
[null,null,"48264031","ASLT ZT 2.5NH 250G@50P",{"$f":"_xlfn.XLOOKUP(C407,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in NH 250 50 BLACK (Std) PG ZT"}]
[null,null,"48264030","ASLT 2.5NH 250G@50P D.F.D.",{"$f":"_xlfn.XLOOKUP(C408,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in NH 250 50 BLACK (Std) PG ETCH"}]
[null,null,"48264044","ASLT 2.5NH 250G@50P BFC-E1",{"$f":"_xlfn.XLOOKUP(C409,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in NH 250 50 BLACK (Std) PG ETCH"}]
[null,null,"48264045","ASLT 2.5NH 250G@50P BFC-T5",{"$f":"_xlfn.XLOOKUP(C410,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in NH 250 50 BLACK (Std) PG ETCH"}]
[null,null,"48264046","ASLT 2.5NH 250G@50P BFC-E2",{"$f":"_xlfn.XLOOKUP(C411,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in NH 250 50 BLACK (Std) PG ETCH"}]
[null,null,"48264006","ASLT 2.5NH 250G@50P FM",{"$f":"_xlfn.XLOOKUP(C412,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in NH 250 50 BLACK (Std) PG"}]
[null,null,"48267006","ASLT NPG 2.5NH 250G@50P FM",{"$f":"_xlfn.XLOOKUP(C413,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in NH 250 50 BLACK (Std) NPG"}]
[null,null,"48264054","ASLT 2.5NH 250G@100P YLWBMPR FM",{"$f":"_xlfn.XLOOKUP(C414,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in NH 250 100 (Std) YELLOW PG"}]
[null,null,"48264015","ASLT ZT 2.5NH 250G@100P",{"$f":"_xlfn.XLOOKUP(C415,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in NH 250 100 (Std) BLACK (Std) PG ZT"}]
[null,null,"48264008","ASLT 2.5NH 250G@100P FM",{"$f":"_xlfn.XLOOKUP(C416,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in NH 250 100 (Std) BLACK (Std) PG"}]
[null,null,"48267008","ASLT NPG 2.5NH 250G@100P FM",{"$f":"_xlfn.XLOOKUP(C417,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in NH 250 100 (Std) BLACK (Std) NPG"}]
[null,null,"48264037","ASLT 2.5NH 210G@50P FM",{"$f":"_xlfn.XLOOKUP(C418,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in NH 210 50 BLACK (Std) PG"}]
[null,null,"48267037","ASLT NPG 2.5NH 210G@50P FM",{"$f":"_xlfn.XLOOKUP(C419,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in NH 210 50 BLACK (Std) NPG"}]
[null,null,"48264026","ASLT 2.5NH 200G@75P FM",{"$f":"_xlfn.XLOOKUP(C420,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in NH 200 75 BLACK (Std) PG"}]
[null,null,"48267026","ASLT NPG 2.5NH 200G@75P FM",{"$f":"_xlfn.XLOOKUP(C421,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in NH 200 75 BLACK (Std) NPG"}]
[null,null,"48264005","ASLT 2.5NH 200G@100P FM",{"$f":"_xlfn.XLOOKUP(C422,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in NH 200 100 (Std) BLACK (Std) PG"}]
[null,null,"48264001","ASLT 2.5AFB 250G@100P FDNY",{"$f":"_xlfn.XLOOKUP(C423,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in FDNY 250 100 (Std) BLACK (Std) PG"}]
[null,null,"48264020","ASLT 2.5AII 950L@700K FM",{"$f":"_xlfn.XLOOKUP(C424,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in CSA 950 700 BLACK (Std) PG"}]
[null,null,"48264035","ASLT 2.5AII 950L@500K FM",{"$f":"_xlfn.XLOOKUP(C425,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in CSA 950 500 BLACK (Std) PG"}]
[null,null,"48264024","ASLT 2.5AII 950L@350K",{"$f":"_xlfn.XLOOKUP(C426,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in CSA 950 350 BLACK (Std) PG"}]
[null,null,"48267024","ASLT NPG 2.5AII 950L@350K",{"$f":"_xlfn.XLOOKUP(C427,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in CSA 950 350 BLACK (Std) NPG"}]
[null,null,"48264047","ASLT 2.5AII 250G@50P FM",{"$f":"_xlfn.XLOOKUP(C428,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in CSA 250 50 BLACK (Std) PG"}]
[null,null,"48264052","ASLT 2.5AII 200G@75P FM",{"$f":"_xlfn.XLOOKUP(C429,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in CSA 200 75 BLACK (Std) PG"}]
[null,null,"48264034","ASLT 2.5BSP 950L@7b FM",{"$f":"_xlfn.XLOOKUP(C430,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in BSP 950 7 BLACK (Std) PG"}]
[null,null,"48264025","ASLT 2.5BSP 750L@5b FM",{"$f":"_xlfn.XLOOKUP(C431,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in BSP 750 5 BLACK (Std) PG"}]
[null,null,"48264048","ASLT 2.5BSP 1140L@7b FM",{"$f":"_xlfn.XLOOKUP(C432,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in BSP 1140 7 BLACK (Std) PG"}]
[null,null,"48264004","ASLT 2.5BIM 950L@7b FM",{"$f":"_xlfn.XLOOKUP(C433,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in BIM 950 7 BLACK (Std) PG"}]
[null,null,"48264003","ASLT 2.5BIM 750L@7b FM",{"$f":"_xlfn.XLOOKUP(C434,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in BIM 750 7 BLACK (Std) PG"}]
[null,null,"48264022","ASLT 2.5BIM 350G@100P FM",{"$f":"_xlfn.XLOOKUP(C435,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in BIM 350 100 (Std) BLACK (Std) PG"}]
[null,null,"48264002","ASLT 2.5BIM 250G@75P FM",{"$f":"_xlfn.XLOOKUP(C436,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in BIM 250 75 BLACK (Std) PG"}]
[null,null,"48264039","ASLT 2.5BAF 300G@75P FM",{"$f":"_xlfn.XLOOKUP(C437,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in BAT 300 75 BLACK (Std) PG"}]
[null,null,"48264049","ASLT 2.5BAF 250G@50P FM",{"$f":"_xlfn.XLOOKUP(C438,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in BAT 250 50 BLACK (Std) PG"}]
[null,null,"48264017","ASLT 2.5BAF 250G@100P FM",{"$f":"_xlfn.XLOOKUP(C439,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in BAT 250 100 (Std) BLACK (Std) PG"}]
[null,null,"48264038","ASLT 2.5BAF 200G@75P FM",{"$f":"_xlfn.XLOOKUP(C440,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in BAT 200 75 BLACK (Std) PG"}]
[null,null,"48267045","ASLT NPG 2.5ASN 250G@100P FM",{"$f":"_xlfn.XLOOKUP(C441,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in ASN 250 100 (Std) BLACK (Std) NPG"}]
[null,null,"48264018","ASLT 2.5AKB 250G@100P FM",{"$f":"_xlfn.XLOOKUP(C442,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in AKB 250 100 (Std) BLACK (Std) PG"}]
[null,null,"48264032","ASLT 2.5AJZ 250G@50P FM",{"$f":"_xlfn.XLOOKUP(C443,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in AJZ 250 50 BLACK (Std) PG"}]
[null,null,"48264029","ASLT 2.5AJN 250G@75P ORGBMPR FM",{"$f":"_xlfn.XLOOKUP(C444,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in AJN 250 75 ORANGE PG"}]
[null,null,"48264033","ASLT ZT 2.5AJN 200G@75P",{"$f":"_xlfn.XLOOKUP(C445,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in AJN 200 75 BLACK (Std) PG ZT"}]
[null,null,"48264011","ASLT 2.5AIK 300G@75P FM",{"$f":"_xlfn.XLOOKUP(C446,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in AIK 300 75 BLACK (Std) PG"}]
[null,null,"48264027","ASLT 2.5AHB 250G@100P FM",{"$f":"_xlfn.XLOOKUP(C447,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in AHB 250 100 (Std) BLACK (Std) PG"}]
[null,null,"48264014","ASLT 2.5AGZ 250G@75P FM",{"$f":"_xlfn.XLOOKUP(C448,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in AGZ 250 75 BLACK (Std) PG"}]
[null,null,"48267014","ASLT NPG 2.5AGZ 250G@75P FM",{"$f":"_xlfn.XLOOKUP(C449,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in AGZ 250 75 BLACK (Std) NPG"}]
[null,null,"48267012","ASLT NPG 2.5ACY 300G@100P FM",{"$f":"_xlfn.XLOOKUP(C450,DataSource!A:A,DataSource!AH:AH)","v":"4826 2.5 in ACY 300 100 (Std) BLACK (Std) NPG"}]
[null,null,"48264050","ASLT 1.5NH 350G@100P FM",{"$f":"_xlfn.XLOOKUP(C451,DataSource!A:A,DataSource!AH:AH)","v":"4826 1.5 in NH 350 100 (Std) BLACK (Std) PG"}]
[null,null,"48267046","ASLT NPG 1.5NH 300G@100P FM",{"$f":"_xlfn.XLOOKUP(C452,DataSource!A:A,DataSource!AH:AH)","v":"4826 1.5 in NH 300 100 (Std) BLACK (Std) NPG"}]
[null,null,"48264019","ASLT 1.5NH 250G@75P FM",{"$f":"_xlfn.XLOOKUP(C453,DataSource!A:A,DataSource!AH:AH)","v":"4826 1.5 in NH 250 75 BLACK (Std) PG"}]
[null,null,"48267043","ASLT NPG 1.5NH 200G@75P FM",{"$f":"_xlfn.XLOOKUP(C454,DataSource!A:A,DataSource!AH:AH)","v":"4826 1.5 in NH 200 75 BLACK (Std) NPG"}]
[null,null,"48264040","ASLT ZT 1.5NH 200G@100P",{"$f":"_xlfn.XLOOKUP(C455,DataSource!A:A,DataSource!AH:AH)","v":"4826 1.5 in NH 200 100 (Std) Black (Std) PG ZT"}]
[null,null,"48264041","ASLT 1.5NH 200G@100P FM",{"$f":"_xlfn.XLOOKUP(C456,DataSource!A:A,DataSource!AH:AH)","v":"4826 1.5 in NH 200 100 (Std) BLACK (Std) PG"}]
[null,null,"48244037","ASLT TIP 1.5ABT 250G@50P",{"$f":"_xlfn.XLOOKUP(C457,DataSource!A:A,DataSource!AH:AH)","v":"4824 1.5 in PCT 250 50 BLACK (Std) "}]
[null,null,"48244038","ASLT TIP 1.5ABT 210G@50P",{"$f":"_xlfn.XLOOKUP(C458,DataSource!A:A,DataSource!AH:AH)","v":"4824 1.5 in PCT 210 50 BLACK (Std) "}]
[null,null,"48244040","ASLT TIP 1.5NPSH 750L@7b",{"$f":"_xlfn.XLOOKUP(C459,DataSource!A:A,DataSource!AH:AH)","v":"4824 1.5 in NPSH 750 7 BLACK (Std) "}]
[null,null,"48244018","ASLT TIP 1.5NPSH 300G@75P",{"$f":"_xlfn.XLOOKUP(C460,DataSource!A:A,DataSource!AH:AH)","v":"4824 1.5 in NPSH 300 75 BLACK (Std) "}]
[null,null,"48244041","ASLT TIP 1.5NPSH 300G@100P",{"$f":"_xlfn.XLOOKUP(C461,DataSource!A:A,DataSource!AH:AH)","v":"4824 1.5 in NPSH 300 100 (Std) BLACK (Std) "}]
[null,null,"48244016","ASLT TIP 1.5NPSH 250G@50P",{"$f":"_xlfn.XLOOKUP(C462,DataSource!A:A,DataSource!AH:AH)","v":"4824 1.5 in NPSH 250 50 BLACK (Std) "}]
[null,null,"48244020","ASLT TIP 1.5NPSH 250G@100P",{"$f":"_xlfn.XLOOKUP(C463,DataSource!A:A,DataSource!AH:AH)","v":"4824 1.5 in NPSH 250 100 (Std) BLACK (Std) "}]
[null,null,"48244031","ASLT TIP 1.5NPSH 1140L@517K",{"$f":"_xlfn.XLOOKUP(C464,DataSource!A:A,DataSource!AH:AH)","v":"4824 1.5 in NPSH 1140 517 BLACK (Std) "}]
[null,null,"48244022","ASLT TIP 1.5NH 950L@7b",{"$f":"_xlfn.XLOOKUP(C465,DataSource!A:A,DataSource!AH:AH)","v":"4824 1.5 in NH 950 7 BLACK (Std) "}]
[null,null,"48244002","ASLT TIP 1.5NH 350G@100P",{"$f":"_xlfn.XLOOKUP(C466,DataSource!A:A,DataSource!AH:AH)","v":"4824 1.5 in NH 350 100 (Std) BLACK (Std) "}]
[null,null,"48244007","ASLT TIP 1.5NH 300G@75P NCFD L-204",{"$f":"_xlfn.XLOOKUP(C467,DataSource!A:A,DataSource!AH:AH)","v":"4824 1.5 in NH 300 75 BLACK (Std)  ETCH"}]
[null,null,"48244003","ASLT TIP 1.5NH 300G@75P",{"$f":"_xlfn.XLOOKUP(C468,DataSource!A:A,DataSource!AH:AH)","v":"4824 1.5 in NH 300 75 BLACK (Std) "}]
[null,null,"48244013","ASLT TIP 1.5NH 300G@100P",{"$f":"_xlfn.XLOOKUP(C469,DataSource!A:A,DataSource!AH:AH)","v":"4824 1.5 in NH 300 100 (Std) BLACK (Std) "}]
[null,null,"48244012","ASLT TIP 1.5NH 250G@75P YLWBMPR BCFD",{"$f":"_xlfn.XLOOKUP(C470,DataSource!A:A,DataSource!AH:AH)","v":"4824 1.5 in NH 250 75 YELLOW  ETCH"}]
[null,null,"48244009","ASLT TIP 1.5NH 250G@75P RED BMPR",{"$f":"_xlfn.XLOOKUP(C471,DataSource!A:A,DataSource!AH:AH)","v":"4824 1.5 in NH 250 75 RED "}]
[null,null,"48244008","ASLT TIP 1.5NH 250G@75P",{"$f":"_xlfn.XLOOKUP(C472,DataSource!A:A,DataSource!AH:AH)","v":"4824 1.5 in NH 250 75 BLACK (Std) "}]
[null,null,"48244034","ASLT TIP 1.5NH 250G@50P YLWBMPR",{"$f":"_xlfn.XLOOKUP(C473,DataSource!A:A,DataSource!AH:AH)","v":"4824 1.5 in NH 250 50 YELLOW "}]
[null,null,"48244025","ASLT TIP 1.5NH 250G@50P REDBMPR",{"$f":"_xlfn.XLOOKUP(C474,DataSource!A:A,DataSource!AH:AH)","v":"4824 1.5 in NH 250 50 RED "}]
[null,null,"48244021","ASLT TIP 1.5NH 250G@50P ORGBMPR RBFR",{"$f":"_xlfn.XLOOKUP(C475,DataSource!A:A,DataSource!AH:AH)","v":"4824 1.5 in NH 250 50 ORANGE "}]
[null,null,"48244010","ASLT TIP 1.5NH 250G@50P LCFR ENGINE 10",{"$f":"_xlfn.XLOOKUP(C476,DataSource!A:A,DataSource!AH:AH)","v":"4824 1.5 in NH 250 50 BLACK (Std)  ETCH"}]
[null,null,"48244011","ASLT TIP 1.5NH 250G@50P LCFR TRAINING",{"$f":"_xlfn.XLOOKUP(C477,DataSource!A:A,DataSource!AH:AH)","v":"4824 1.5 in NH 250 50 BLACK (Std)  ETCH"}]
[null,null,"48244014","ASLT TIP 1.5NH 250G@50P  RES-ENG 208",{"$f":"_xlfn.XLOOKUP(C478,DataSource!A:A,DataSource!AH:AH)","v":"4824 1.5 in NH 250 50 BLACK (Std)  ETCH"}]
[null,null,"48244024","ASLT TIP 1.5NH 250G@50P  ENO FD",{"$f":"_xlfn.XLOOKUP(C479,DataSource!A:A,DataSource!AH:AH)","v":"4824 1.5 in NH 250 50 BLACK (Std)  ETCH"}]
[null,null,"48244026","ASLT TIP 1.5NH 250G@50P LCFR ENGINE 20",{"$f":"_xlfn.XLOOKUP(C480,DataSource!A:A,DataSource!AH:AH)","v":"4824 1.5 in NH 250 50 BLACK (Std)  ETCH"}]
[null,null,"48244027","ASLT TIP 1.5NH 250G@50P LCFR ENGINE 50",{"$f":"_xlfn.XLOOKUP(C481,DataSource!A:A,DataSource!AH:AH)","v":"4824 1.5 in NH 250 50 BLACK (Std)  ETCH"}]
[null,null,"48244028","ASLT TIP 1.5NH 250G@50P GASTONIA FD",{"$f":"_xlfn.XLOOKUP(C482,DataSource!A:A,DataSource!AH:AH)","v":"4824 1.5 in NH 250 50 BLACK (Std)  ETCH"}]
[null,null,"48244029","ASLT TIP 1.5NH 250G@50P MTLTTH ETCH SAC",{"$f":"_xlfn.XLOOKUP(C483,DataSource!A:A,DataSource!AH:AH)","v":"4824 1.5 in NH 250 50 BLACK (Std)  ETCH"}]
[null,null,"48244033","ASLT TIP 1.5NH 250G@50P 1589",{"$f":"_xlfn.XLOOKUP(C484,DataSource!A:A,DataSource!AH:AH)","v":"4824 1.5 in NH 250 50 BLACK (Std)  ETCH"}]
[null,null,"48244036","ASLT TIP 1.5NH 250G@50P N1596",{"$f":"_xlfn.XLOOKUP(C485,DataSource!A:A,DataSource!AH:AH)","v":"4824 1.5 in NH 250 50 BLACK (Std)  ETCH"}]
[null,null,"48244001","ASLT TIP 1.5NH 250G@50P#",{"$f":"_xlfn.XLOOKUP(C486,DataSource!A:A,DataSource!AH:AH)","v":"4824 1.5 in NH 250 50 BLACK (Std) "}]
[null,null,"48244017","ASLT TIP 1.5NH 250G@100P",{"$f":"_xlfn.XLOOKUP(C487,DataSource!A:A,DataSource!AH:AH)","v":"4824 1.5 in NH 250 100 (Std) BLACK (Std) "}]
[null,null,"48244032","ASLT TIP 1.5NH 210G@50P YLWBMPR",{"$f":"_xlfn.XLOOKUP(C488,DataSource!A:A,DataSource!AH:AH)","v":"4824 1.5 in NH 210 50 YELLOW "}]
[null,null,"48244042","ASLT TIP 1.5NH 210G@50P",{"$f":"_xlfn.XLOOKUP(C489,DataSource!A:A,DataSource!AH:AH)","v":"4824 1.5 in NH 210 50 BLACK (Std) "}]
[null,null,"48244015","ASLT TIP 1.5NH 200G@75P",{"$f":"_xlfn.XLOOKUP(C490,DataSource!A:A,DataSource!AH:AH)","v":"4824 1.5 in NH 200 75 BLACK (Std) "}]
[null,null,"48244035","ASLT TIP 1.5NH 200G@100P",{"$f":"_xlfn.XLOOKUP(C491,DataSource!A:A,DataSource!AH:AH)","v":"4824 1.5 in NH 200 100 (Std) BLACK (Std) "}]
[null,null,"48244030","ASLT TIP 1.5NH 1325L@7b",{"$f":"_xlfn.XLOOKUP(C492,DataSource!A:A,DataSource!AH:AH)","v":"4824 1.5 in NH 1325 7 BLACK (Std) "}]
[null,null,"48244004","ASLT TIP 1.5ABU 250G@100P FDNY",{"$f":"_xlfn.XLOOKUP(C493,DataSource!A:A,DataSource!AH:AH)","v":"4824 1.5 in FDNY 250 100 (Std) BLACK (Std) "}]
[null,null,"48244023","ASLT TIP 1.5BSP 950L@7b",{"$f":"_xlfn.XLOOKUP(C494,DataSource!A:A,DataSource!AH:AH)","v":"4824 1.5 in BSP 950 7 BLACK (Std) "}]
[null,null,"48244019","ASLT TIP 1.5BSP 1325L@7b",{"$f":"_xlfn.XLOOKUP(C495,DataSource!A:A,DataSource!AH:AH)","v":"4824 1.5 in BSP 1325 7 BLACK (Std) "}]
[null,null,"48080014","NOZ 1.5NH UHP HAND LINE 15G@1400P",{"$f":"_xlfn.XLOOKUP(C496,DataSource!A:A,DataSource!AH:AH)","v":"4808 1.5 in NH 15 1400 BLACK (Std) PG"}]
[null,null,"48080002","NOZ 1\"UHP HND LN 20GPM@1200PSI SPC",{"$f":"_xlfn.XLOOKUP(C497,DataSource!A:A,DataSource!AH:AH)","v":"4808 1 in SAE-8 20 1200 BLACK (Std) PG"}]
[null,null,"48080022","NOZ 1\"NPT UHP HAND LINE 30GPM@1500PSI",{"$f":"_xlfn.XLOOKUP(C498,DataSource!A:A,DataSource!AH:AH)","v":"4808 1 in NPT 30 1500 BLACK (Std) PG"}]
[null,null,"48080015","NOZ 1\"NPT UHP HANDLINE 20G@1100P",{"$f":"_xlfn.XLOOKUP(C499,DataSource!A:A,DataSource!AH:AH)","v":"4808 1 in NPT 20 1100 BLACK (Std) PG"}]
[null,null,"48080010","NOZ 1\"NPT UHP HANDLINE 16.5-17.5G@1100P",{"$f":"_xlfn.XLOOKUP(C500,DataSource!A:A,DataSource!AH:AH)","v":"4808 1 in NPT 17 1100 BLACK (Std) PG"}]
[null,null,"48080027","NOZ 1\"NPT UHP HANDLINE 15G@1400P",{"$f":"_xlfn.XLOOKUP(C501,DataSource!A:A,DataSource!AH:AH)","v":"4808 1 in NPT 15 1400 BLACK (Std) PG"}]
[null,null,"48080020","NOZ 1\"NPT UHP HANDLINE 15G@1100P",{"$f":"_xlfn.XLOOKUP(C502,DataSource!A:A,DataSource!AH:AH)","v":"4808 1 in NPT 15 1100 BLACK (Std) PG"}]
[null,null,"48080019","NOZ 1\"NPT UHP HANDLINE 10G@1250P",{"$f":"_xlfn.XLOOKUP(C503,DataSource!A:A,DataSource!AH:AH)","v":"4808 1 in NPT 10 1250 BLACK (Std) PG"}]
[null,null,"48080013","NOZ 1\"NPSH  UHP HAND LINE 30G@600P",{"$f":"_xlfn.XLOOKUP(C504,DataSource!A:A,DataSource!AH:AH)","v":"4808 1 in NPSH 30 600 BLACK (Std) PG"}]
[null,null,"48080023","NOZ 1\"NPSH UHP HAND LINE 30GPM@1500PSI",{"$f":"_xlfn.XLOOKUP(C505,DataSource!A:A,DataSource!AH:AH)","v":"4808 1 in NPSH 30 1500 BLACK (Std) PG"}]
[null,null,"48080025","NOZ 1\"NPSH UHP HAND LINE 15GPM@1500PSI",{"$f":"_xlfn.XLOOKUP(C506,DataSource!A:A,DataSource!AH:AH)","v":"4808 1 in NPSH 15 1500 BLACK (Std) PG"}]
[null,null,"48080012","NOZ 1\"NH UHP HAND LINE 30GPM@600PSI",{"$f":"_xlfn.XLOOKUP(C507,DataSource!A:A,DataSource!AH:AH)","v":"4808 1 in NH 30 600 BLACK (Std) PG"}]
[null,null,"48080011","NOZ 1\"NH UHP HAND LINE 30GPM@1500PSI",{"$f":"_xlfn.XLOOKUP(C508,DataSource!A:A,DataSource!AH:AH)","v":"4808 1 in NH 30 1500 BLACK (Std) PG"}]
[null,null,"48080016","NOZ 1\"NH UHP HAND LINE 20GPM@1500PSI",{"$f":"_xlfn.XLOOKUP(C509,DataSource!A:A,DataSource!AH:AH)","v":"4808 1 in NH 20 1500 BLACK (Std) PG"}]
[null,null,"48080001","NOZ 1\"NH UHP HAND LINE 20GPM@1400PSI",{"$f":"_xlfn.XLOOKUP(C510,DataSource!A:A,DataSource!AH:AH)","v":"4808 1 in NH 20 1400 BLACK (Std) PG"}]
[null,null,"48080024","NOZ 1\"NH UHP HND LN 20GPM@1200PSI",{"$f":"_xlfn.XLOOKUP(C511,DataSource!A:A,DataSource!AH:AH)","v":"4808 1 in NH 20 1200 BLACK (Std) PG"}]
[null,null,"48080004","NOZ 1\"NH UHP HANDLINE 16.5-17.5G@1100P",{"$f":"_xlfn.XLOOKUP(C512,DataSource!A:A,DataSource!AH:AH)","v":"4808 1 in NH 17 1100 BLACK (Std) PG"}]
[null,null,"48080005","NOZ 1\"NH UHP HAND LINE 15GPM@1500PSI",{"$f":"_xlfn.XLOOKUP(C513,DataSource!A:A,DataSource!AH:AH)","v":"4808 1 in NH 15 1500 BLACK (Std) PG"}]
[null,null,"48080018","NOZ 1\"NH UHP HAND LINE 15G@1400P",{"$f":"_xlfn.XLOOKUP(C514,DataSource!A:A,DataSource!AH:AH)","v":"4808 1 in NH 15 1400 BLACK (Std) PG"}]
[null,null,"48080026","NOZ 1\"NH UHP HD LN 15GPM@1200PSI",{"$f":"_xlfn.XLOOKUP(C515,DataSource!A:A,DataSource!AH:AH)","v":"4808 1 in NH 15 1200 BLACK (Std) PG"}]
[null,null,"48080021","NOZ 1\"NH UHP HANDLINE 15G@1100P",{"$f":"_xlfn.XLOOKUP(C516,DataSource!A:A,DataSource!AH:AH)","v":"4808 1 in NH 15 1100 BLACK (Std) PG"}]
[null,null,"48080017","NOZ 1\"BSP UHP HAND LINE 20GPM@1400PSI",{"$f":"_xlfn.XLOOKUP(C517,DataSource!A:A,DataSource!AH:AH)","v":"4808 1 in BSP 20 1400 BLACK (Std) PG"}]
[null,null,"48024701","ASLT 1.0 BSPX25MMSTZ 150L@6b EN",{"$f":"_xlfn.XLOOKUP(C518,DataSource!A:A,DataSource!AH:AH)","v":"4802 1 in STORZ 150 6 BLACK (Std) PG"}]
[null,null,"48024015","ASLT 1.0 NPSH 40G@100P FM",{"$f":"_xlfn.XLOOKUP(C519,DataSource!A:A,DataSource!AH:AH)","v":"4802 1 in NPSH 40 100 (Std) BLACK (Std) PG"}]
[null,null,"48024013","ASLT 1.0 NPSH 25G@100P FM",{"$f":"_xlfn.XLOOKUP(C520,DataSource!A:A,DataSource!AH:AH)","v":"4802 1 in NPSH 25 100 (Std) BLACK (Std) PG"}]
[null,null,"48027013","ASLT NPG 1.0 NPSH 25G@100P FM",{"$f":"_xlfn.XLOOKUP(C521,DataSource!A:A,DataSource!AH:AH)","v":"4802 1 in NPSH 25 100 (Std) BLACK (Std) NPG"}]
[null,null,"48024016","ASLT 1.0 NH 50L@7b FM",{"$f":"_xlfn.XLOOKUP(C522,DataSource!A:A,DataSource!AH:AH)","v":"4802 1 in NH 50 7 BLACK (Std) PG"}]
[null,null,"48024011","ASLT 1.0 NH 40G@100P REDBMPR FM",{"$f":"_xlfn.XLOOKUP(C523,DataSource!A:A,DataSource!AH:AH)","v":"4802 1 in NH 40 100 (Std) RED PG"}]
[null,null,"48024012","ASLT 1.0 NH 40G@100P ORGBMPR FM",{"$f":"_xlfn.XLOOKUP(C524,DataSource!A:A,DataSource!AH:AH)","v":"4802 1 in NH 40 100 (Std) ORANGE PG"}]
[null,null,"48024001","ASLT 1.0 NH 40G@100P FM",{"$f":"_xlfn.XLOOKUP(C525,DataSource!A:A,DataSource!AH:AH)","v":"4802 1 in NH 40 100 (Std) BLACK (Std) PG"}]
[null,null,"48027006","ASLT NPG 1\"NH 40G@100P CHARLOTTE FD",{"$f":"_xlfn.XLOOKUP(C526,DataSource!A:A,DataSource!AH:AH)","v":"4802 1 in NH 40 100 (Std) BLACK (Std) NPG ETCH"}]
[null,null,"48027018","ASLT NPG 1\"NH 40G@100P D.C.F.D",{"$f":"_xlfn.XLOOKUP(C527,DataSource!A:A,DataSource!AH:AH)","v":"4802 1 in NH 40 100 (Std) BLACK (Std) NPG ETCH"}]
[null,null,"48027001","ASLT NPG 1.0 NH 40G@100P FM",{"$f":"_xlfn.XLOOKUP(C528,DataSource!A:A,DataSource!AH:AH)","v":"4802 1 in NH 40 100 (Std) BLACK (Std) NPG"}]
[null,null,"48024014","ASLT 1.0 NH 25G@100P YLWBMPR FM",{"$f":"_xlfn.XLOOKUP(C529,DataSource!A:A,DataSource!AH:AH)","v":"4802 1 in NH 25 100 (Std) YELLOW PG"}]
[null,null,"48024018","ASLT 1.0 NH 25G@100P GROVETOWN",{"$f":"_xlfn.XLOOKUP(C530,DataSource!A:A,DataSource!AH:AH)","v":"4802 1 in NH 25 100 (Std) BLACK (Std) PG ETCH"}]
[null,null,"48024002","ASLT 1.0 NH 25G@100P FM",{"$f":"_xlfn.XLOOKUP(C531,DataSource!A:A,DataSource!AH:AH)","v":"4802 1 in NH 25 100 (Std) BLACK (Std) PG"}]
[null,null,"48024021","ASLT 1.0 NH 13G@100P RED BUMPER FM",{"$f":"_xlfn.XLOOKUP(C532,DataSource!A:A,DataSource!AH:AH)","v":"4802 1 in NH 13 100 (Std) RED PG"}]
[null,null,"48024004","ASLT 1.0 NH 13G@100P FM",{"$f":"_xlfn.XLOOKUP(C533,DataSource!A:A,DataSource!AH:AH)","v":"4802 1 in NH 13 100 (Std) BLACK (Std) PG"}]
[null,null,"48024003","ASLT 1.0 NH 100L@7b FM",{"$f":"_xlfn.XLOOKUP(C534,DataSource!A:A,DataSource!AH:AH)","v":"4802 1 in NH 100 7 BLACK (Std) PG"}]
[null,null,"48024020","ASLT 1.0BSP 50L@7b FM",{"$f":"_xlfn.XLOOKUP(C535,DataSource!A:A,DataSource!AH:AH)","v":"4802 1 in BSP 50 7 BLACK (Std) PG"}]
[null,null,"48024010","ASLT 1.0 BSP 150L@7b FM",{"$f":"_xlfn.XLOOKUP(C536,DataSource!A:A,DataSource!AH:AH)","v":"4802 1 in BSP 150 7 BLACK (Std) PG"}]
[null,null,"48024005","ASLT 1.0 BSP 100L@7b DETENT",{"$f":"_xlfn.XLOOKUP(C537,DataSource!A:A,DataSource!AH:AH)","v":"4802 1 in BSP 100 7 BLACK (Std) PG"}]
[null,null,"48024019","ASLT 1.0 BSP 100L@7b",{"$f":"_xlfn.XLOOKUP(C538,DataSource!A:A,DataSource!AH:AH)","v":"4802 1 in BSP 100 7 BLACK (Std) PG"}]
[null,null,"48024707","ASLT 1.0 BSP 100L@6b EN",{"$f":"_xlfn.XLOOKUP(C539,DataSource!A:A,DataSource!AH:AH)","v":"4802 1 in BSP 100 6 BLACK (Std) PG"}]
[null,null,"41164024","PROVENGER 2.5NH FIXED 150G@75P FM",{"$f":"_xlfn.XLOOKUP(C540,DataSource!A:A,DataSource!AH:AH)","v":"4116 2.5 in NH 150 75 BLACK (Std) PG"}]
[null,null,"41164012","PROVENGER 2.5NH FIXED 150G@100P FM",{"$f":"_xlfn.XLOOKUP(C541,DataSource!A:A,DataSource!AH:AH)","v":"4116 2.5 in NH 150 100 (Std) BLACK (Std) PG"}]
[null,null,"41164020","PROVENGER 2.5NH FIXED 125G@75P FM",{"$f":"_xlfn.XLOOKUP(C542,DataSource!A:A,DataSource!AH:AH)","v":"4116 2.5 in NH 125 75 BLACK (Std) PG"}]
[null,null,"41164018","PROVENGER 2.5NH FIXED 125G@100P FM",{"$f":"_xlfn.XLOOKUP(C543,DataSource!A:A,DataSource!AH:AH)","v":"4116 2.5 in NH 125 100 (Std) BLACK (Std) PG"}]
[null,null,"41164014","PROVENGER 2.5BIM FIXED 95G@100P FM",{"$f":"_xlfn.XLOOKUP(C544,DataSource!A:A,DataSource!AH:AH)","v":"4116 2.5 in BIM 95 100 (Std) BLACK (Std) PG"}]
[null,null,"41164009","PROVENGER 2.5BIM FIXED 550L@7b FM",{"$f":"_xlfn.XLOOKUP(C545,DataSource!A:A,DataSource!AH:AH)","v":"4116 2.5 in BIM 550 7 BLACK (Std) PG"}]
[null,null,"41164025","PROVENGER 2.5BIM FIXED 230L@6b FM",{"$f":"_xlfn.XLOOKUP(C546,DataSource!A:A,DataSource!AH:AH)","v":"4116 1.5 in BSP 230 6 BLACK (Std) PG"}]
[null,null,"41164013","PROVENGER 2.5BIM FIXED 150G@100P FM",{"$f":"_xlfn.XLOOKUP(C547,DataSource!A:A,DataSource!AH:AH)","v":"4116 2.5 in BIM 150 100 (Std) BLACK (Std) PG"}]
[null,null,"41164008","PROVENGER 2.5BIM FIXED 125G@100P FM",{"$f":"_xlfn.XLOOKUP(C548,DataSource!A:A,DataSource!AH:AH)","v":"4116 2.5 in BIM 125 100 (Std) BLACK (Std) PG"}]
[null,null,"41164023","PROVENGER 1.5NPSH FIXED 500L@700k FM",{"$f":"_xlfn.XLOOKUP(C549,DataSource!A:A,DataSource!AH:AH)","v":"4116 1.5 in NPSH 500 700 BLACK (Std) PG"}]
[null,null,"41164006","PROVENGER 1.5NPSH FIXED 150G@75P FM",{"$f":"_xlfn.XLOOKUP(C550,DataSource!A:A,DataSource!AH:AH)","v":"4116 1.5 in NPSH 150 75 BLACK (Std) PG"}]
[null,null,"41164011","PROVENGER 1.5NPSH FIXED 150G@100P FM",{"$f":"_xlfn.XLOOKUP(C551,DataSource!A:A,DataSource!AH:AH)","v":"4116 1.5 in NPSH 150 100 (Std) BLACK (Std) PG"}]
[null,null,"41164017","PROVENGER 1.5NPSH FIXED 125G@100P FM",{"$f":"_xlfn.XLOOKUP(C552,DataSource!A:A,DataSource!AH:AH)","v":"4116 1.5 in NPSH 125 100 (Std) BLACK (Std) PG"}]
[null,null,"41164001","PROVENGER 1.5NH FIXED 95G@75P FM",{"$f":"_xlfn.XLOOKUP(C553,DataSource!A:A,DataSource!AH:AH)","v":"4116 1.5 in NH 95 75 BLACK (Std) PG"}]
[null,null,"41164002","PROVENGER 1.5NH FIXED 95G@100P FM",{"$f":"_xlfn.XLOOKUP(C554,DataSource!A:A,DataSource!AH:AH)","v":"4116 1.5 in NH 95 100 (Std) BLACK (Std) PG"}]
[null,null,"41164021","PROVENGER 1.5NH FIXED 60G@75P FM",{"$f":"_xlfn.XLOOKUP(C555,DataSource!A:A,DataSource!AH:AH)","v":"4116 1.5 in NH 60 75 BLACK (Std) PG"}]
[null,null,"41164027","PROVENGER 1.5NH FIXED 550L@6b FM",{"$f":"_xlfn.XLOOKUP(C556,DataSource!A:A,DataSource!AH:AH)","v":"4116 1.5 in NH 550 6 BLACK (Std) PG"}]
[null,null,"41164003","PROVENGER 1.5NH FIXED 150G@75P FM",{"$f":"_xlfn.XLOOKUP(C557,DataSource!A:A,DataSource!AH:AH)","v":"4116 1.5 in NH 150 75 BLACK (Std) PG"}]
[null,null,"41164004","PROVENGER 1.5NH FIXED 150G@100P FM",{"$f":"_xlfn.XLOOKUP(C558,DataSource!A:A,DataSource!AH:AH)","v":"4116 1.5 in NH 150 100 (Std) BLACK (Std) PG"}]
[null,null,"41164019","PROVENGER 1.5NH FIXED 125G@75P FM",{"$f":"_xlfn.XLOOKUP(C559,DataSource!A:A,DataSource!AH:AH)","v":"4116 1.5 in NH 125 75 BLACK (Std) PG"}]
[null,null,"41164016","PROVENGER 1.5NH FIXED 125G@100P FM",{"$f":"_xlfn.XLOOKUP(C560,DataSource!A:A,DataSource!AH:AH)","v":"4116 1.5 in NH 125 100 (Std) BLACK (Std) PG"}]
[null,null,"41164010","PROVENGER 1.5BSP FIXED 550L@7b FM",{"$f":"_xlfn.XLOOKUP(C561,DataSource!A:A,DataSource!AH:AH)","v":"4116 1.5 in BSP 550 7 BLACK (Std) PG"}]
[null,null,"41164015","PROVENGER 1.5BSP FIXED 550L@6b FM",{"$f":"_xlfn.XLOOKUP(C562,DataSource!A:A,DataSource!AH:AH)","v":"4116 1.5 in BSP 550 6 BLACK (Std) PG"}]
[null,null,"24334008","SBR TIP SO 2.5AFYX1.5NH 1-1/8D",{"$f":"_xlfn.XLOOKUP(C563,DataSource!A:A,DataSource!AH:AH)","v":"2433 2.5 in PITT6 1.5 in NH 1-1/8\" bore size(s) PG"}]
[null,null,"24334010","SBR TIP SO 2.5AEF X 1.5NH 1-1/8D",{"$f":"_xlfn.XLOOKUP(C564,DataSource!A:A,DataSource!AH:AH)","v":"2433 2.5 in NYCORP 1.5 in NH 1-1/8\" bore size(s) PG"}]
[null,null,"24334026","SBR TIP SO 2.5NHX1.5NPSH 1-3/16D",{"$f":"_xlfn.XLOOKUP(C565,DataSource!A:A,DataSource!AH:AH)","v":"2433 2.5 in NH 1.5 in NPSH 1-3/16\" bore size(s) PG"}]
[null,null,"24334007","SBR TIP SO 2.5NHX1.5NPSH 1-1/8D",{"$f":"_xlfn.XLOOKUP(C566,DataSource!A:A,DataSource!AH:AH)","v":"2433 2.5 in NH 1.5 in NPSH 1-1/8\" bore size(s) PG"}]
[null,null,"24337007","SBR TIP SO NPG 2.5NHX1.5NPSH 1-1/8D",{"$f":"_xlfn.XLOOKUP(C567,DataSource!A:A,DataSource!AH:AH)","v":"2433 2.5 in NH 1.5 in NPSH 1-1/8\" bore size(s) NPG"}]
[null,null,"24334024","SBR TIP SO 2.5NHX1.5NPSH 1-1/16D",{"$f":"_xlfn.XLOOKUP(C568,DataSource!A:A,DataSource!AH:AH)","v":"2433 2.5 in NH 1.5 in NPSH 1-1/16\" bore size(s) PG"}]
[null,null,"24334016","SBR TIP SO 2.5NHX1.5NH 7/8D",{"$f":"_xlfn.XLOOKUP(C569,DataSource!A:A,DataSource!AH:AH)","v":"2433 2.5 in NH 1.5 in NH 7/8\" bore size(s) PG"}]
[null,null,"24334014","SBR TIP SO 2.5NH X 1.5NH 15/16D 1589",{"$f":"_xlfn.XLOOKUP(C570,DataSource!A:A,DataSource!AH:AH)","v":"2433 2.5 in NH 1.5 in NH 15/16\" bore size(s) PG ETCH"}]
[null,null,"24334018","SBR TIP SO 2.5NH X 1.5NH 15/16D N1596",{"$f":"_xlfn.XLOOKUP(C571,DataSource!A:A,DataSource!AH:AH)","v":"2433 2.5 in NH 1.5 in NH 15/16\" bore size(s) PG ETCH"}]
[null,null,"24334019","SBR TIP SO 2.5NH X 1.5NH 15/16D N1597",{"$f":"_xlfn.XLOOKUP(C572,DataSource!A:A,DataSource!AH:AH)","v":"2433 2.5 in NH 1.5 in NH 15/16\" bore size(s) PG ETCH"}]
[null,null,"24334020","SBR TIP SO 2.5NH X 1.5NH 15/16D N1598",{"$f":"_xlfn.XLOOKUP(C573,DataSource!A:A,DataSource!AH:AH)","v":"2433 2.5 in NH 1.5 in NH 15/16\" bore size(s) PG ETCH"}]
[null,null,"24334003","SBR TIP SO 2.5NH X 1.5NH 15/16D",{"$f":"_xlfn.XLOOKUP(C574,DataSource!A:A,DataSource!AH:AH)","v":"2433 2.5 in NH 1.5 in NH 15/16\" bore size(s) PG"}]
[null,null,"24334025","SBR TIP SO 2.5NHX1.5NH 1-3/16D",{"$f":"_xlfn.XLOOKUP(C575,DataSource!A:A,DataSource!AH:AH)","v":"2433 2.5 in NH 1.5 in NH 1-3/16\" bore size(s) PG"}]
[null,null,"24334004","SBR TIP SO 2.5NHX1.5NH 1-1/8D LCFR ENG10",{"$f":"_xlfn.XLOOKUP(C576,DataSource!A:A,DataSource!AH:AH)","v":"2433 2.5 in NH 1.5 in NH 1-1/8\" bore size(s) PG ETCH"}]
[null,null,"24334005","SBR TIP SO 2.5NHX1.5NH 1-1/8D LCFR TRAIN",{"$f":"_xlfn.XLOOKUP(C577,DataSource!A:A,DataSource!AH:AH)","v":"2433 2.5 in NH 1.5 in NH 1-1/8\" bore size(s) PG ETCH"}]
[null,null,"24334011","SBR TIP SO 2.5NHX1.5NH 1-1/8D LCFR ENG20",{"$f":"_xlfn.XLOOKUP(C578,DataSource!A:A,DataSource!AH:AH)","v":"2433 2.5 in NH 1.5 in NH 1-1/8\" bore size(s) PG ETCH"}]
[null,null,"24334012","SBR TIP SO 2.5NHX1.5NH 1-1/8D LCFR ENG50",{"$f":"_xlfn.XLOOKUP(C579,DataSource!A:A,DataSource!AH:AH)","v":"2433 2.5 in NH 1.5 in NH 1-1/8\" bore size(s) PG ETCH"}]
[null,null,"24334002","SBR TIP SO 2.5NHX1.5NH 1-1/8D",{"$f":"_xlfn.XLOOKUP(C580,DataSource!A:A,DataSource!AH:AH)","v":"2433 2.5 in NH 1.5 in NH 1-1/8\" bore size(s) PG"}]
[null,null,"24337004","SBR TIP SO NPG 2.5NHX1.5NH 1-1/8D ETCH",{"$f":"_xlfn.XLOOKUP(C581,DataSource!A:A,DataSource!AH:AH)","v":"2433 2.5 in NH 1.5 in NH 1-1/8\" bore size(s) NPG ETCH"}]
[null,null,"24337002","SBR TIP SO NPG 2.5NHX1.5NH 1-1/8D",{"$f":"_xlfn.XLOOKUP(C582,DataSource!A:A,DataSource!AH:AH)","v":"2433 2.5 in NH 1.5 in NH 1-1/8\" bore size(s) NPG"}]
[null,null,"24334022","SBR TIP SO 2.5AHB X 1.5NH 1-1/8D",{"$f":"_xlfn.XLOOKUP(C583,DataSource!A:A,DataSource!AH:AH)","v":"2433 2.5 in NH 1.5 in NH 1-1/8\" bore size(s)  "}]
[null,null,"24334006","SBR TIP SO ZT 2.5NHX1.5NH 1-1/4D BCFD",{"$f":"_xlfn.XLOOKUP(C584,DataSource!A:A,DataSource!AH:AH)","v":"2433 2.5 in NH 1.5 in NH 1-1/4\" bore size(s) PG ZT ETCH"}]
[null,null,"24334009","SBR TIP SO 2.5NHX1.5NH 1-1/4D RBFR",{"$f":"_xlfn.XLOOKUP(C585,DataSource!A:A,DataSource!AH:AH)","v":"2433 2.5 in NH 1.5 in NH 1-1/4\" bore size(s) PG ETCH"}]
[null,null,"24334015","SBR TIP SO 2.5NHX1.5NH 1-1/4D 1590-1591",{"$f":"_xlfn.XLOOKUP(C586,DataSource!A:A,DataSource!AH:AH)","v":"2433 2.5 in NH 1.5 in NH 1-1/4\" bore size(s) PG ETCH"}]
[null,null,"24334001","SBR TIP SO 2.5NHX1.5NH 1-1/4D",{"$f":"_xlfn.XLOOKUP(C587,DataSource!A:A,DataSource!AH:AH)","v":"2433 2.5 in NH 1.5 in NH 1-1/4\" bore size(s) PG"}]
[null,null,"24337001","SBR TIP SO NPG 2.5NHX1.5NH 1-1/4D",{"$f":"_xlfn.XLOOKUP(C588,DataSource!A:A,DataSource!AH:AH)","v":"2433 2.5 in NH 1.5 in NH 1-1/4\" bore size(s) NPG"}]
[null,null,"24334023","SBR TIP SO 2.5NHX1.5NH 1-1/16D",{"$f":"_xlfn.XLOOKUP(C589,DataSource!A:A,DataSource!AH:AH)","v":"2433 2.5 in NH 1.5 in NH 1-1/16\" bore size(s) PG"}]
[null,null,"24334021","SBR TIP SO 2.5BAF X1.5NPSH 1-1/8D",{"$f":"_xlfn.XLOOKUP(C590,DataSource!A:A,DataSource!AH:AH)","v":"2433 2.5 in BAT 1.5 in NPSH 1-1/8\" bore size(s) PG"}]
[null,null,"24337003","SBR TIP SO NPG 2.5BAF X1.5NPSH 1-1/8D",{"$f":"_xlfn.XLOOKUP(C591,DataSource!A:A,DataSource!AH:AH)","v":"2433 2.5 in BAT 1.5 in NPSH 1-1/8\" bore size(s) NPG"}]
[null,null,"24334017","SBR TIP SO 2.5AUC X 1.5NH 1-1/8D",{"$f":"_xlfn.XLOOKUP(C592,DataSource!A:A,DataSource!AH:AH)","v":"2433 2.5 in AUC 1.5 in NH 1-1/8\" bore size(s) PG"}]
[null,null,"24334027","SBR TIP SO 2.5AKBX1.5NPSH 1-1/8D",{"$f":"_xlfn.XLOOKUP(C593,DataSource!A:A,DataSource!AH:AH)","v":"2433 2.5 in AKB 1.5 in NPSH 1-1/8\" bore size(s) PG"}]
[null,null,"24334013","SBR TIP SO 2.5AHC X 1.5NH 1-1/8D",{"$f":"_xlfn.XLOOKUP(C594,DataSource!A:A,DataSource!AH:AH)","v":"2433 2.5 in AHC 1.5 in NH 1-1/8\" bore size(s) PG"}]
[null,null,"24314016","SBR TIP SO 1.5NPSH X 1.5NPSH 7/8D",{"$f":"_xlfn.XLOOKUP(C595,DataSource!A:A,DataSource!AH:AH)","v":"2431 1.5 in NPSH 1.5 in NPSH 7/8\" bore size(s) PG"}]
[null,null,"24314004","SBR TIP SO 1.5NPSH X 1.5NPSH 15/16D",{"$f":"_xlfn.XLOOKUP(C596,DataSource!A:A,DataSource!AH:AH)","v":"2431 1.5 in NPSH 1.5 in NPSH 15/16\" bore size(s) PG"}]
[null,null,"24317004","SBR TIP SO NPG 1.5NPSH X 1.5NPSH 15/16D",{"$f":"_xlfn.XLOOKUP(C597,DataSource!A:A,DataSource!AH:AH)","v":"2431 1.5 in NPSH 1.5 in NPSH 15/16\" bore size(s) NPG"}]
[null,null,"24314039","SBR TIP SO 1.5NPSH X 1.5NPSH 1-1/36D",{"$f":"_xlfn.XLOOKUP(C598,DataSource!A:A,DataSource!AH:AH)","v":"2431 1.5 in NPSH 1.5 in NPSH 1-3/16\" bore size(s) PG"}]
[null,null,"24314033","SBR TIP SO 1.5NPSH X 1.5NPSH 1-1/8D",{"$f":"_xlfn.XLOOKUP(C599,DataSource!A:A,DataSource!AH:AH)","v":"2431 1.5 in NPSH 1.5 in NPSH 1-1/8\" bore size(s) PG"}]
[null,null,"24314013","SBR TIP SO 1.5NPSH X 1.5NPSH 1-1/4D",{"$f":"_xlfn.XLOOKUP(C600,DataSource!A:A,DataSource!AH:AH)","v":"2431 1.5 in NPSH 1.5 in NPSH 1-1/4\" bore size(s) PG"}]
[null,null,"24314037","SBR TIP SO 1.5NPSH X 1.5NPSH 1-1/16D",{"$f":"_xlfn.XLOOKUP(C601,DataSource!A:A,DataSource!AH:AH)","v":"2431 1.5 in NPSH 1.5 in NPSH 1-1/16\" bore size(s) PG"}]
[null,null,"24314005","SBR TIP SO 1.5NPSH X 1.5NPSH 1D",{"$f":"_xlfn.XLOOKUP(C602,DataSource!A:A,DataSource!AH:AH)","v":"2431 1.5 in NPSH 1.5 in NPSH 1\" bore size(s) PG"}]
[null,null,"24314015","SBR TIP SO 1.5NH X 1.5NH 7/8D LCFR ENG10",{"$f":"_xlfn.XLOOKUP(C603,DataSource!A:A,DataSource!AH:AH)","v":"2431 1.5 in NH 1.5 in NH 7/8\" bore size(s) PG ETCH"}]
[null,null,"24314020","SBR TIP SO 1.5NH X 1.5NH 7/8D LCFR ENG20",{"$f":"_xlfn.XLOOKUP(C604,DataSource!A:A,DataSource!AH:AH)","v":"2431 1.5 in NH 1.5 in NH 7/8\" bore size(s) PG ETCH"}]
[null,null,"24314021","SBR TIP SO 1.5NH X 1.5NH 7/8D LCFR ENG50",{"$f":"_xlfn.XLOOKUP(C605,DataSource!A:A,DataSource!AH:AH)","v":"2431 1.5 in NH 1.5 in NH 7/8\" bore size(s) PG ETCH"}]
[null,null,"24314003","SBR TIP SO 1.5NH X 1.5NH 7/8D",{"$f":"_xlfn.XLOOKUP(C606,DataSource!A:A,DataSource!AH:AH)","v":"2431 1.5 in NH 1.5 in NH 7/8\" bore size(s) PG"}]
[null,null,"24317008","SBR TIP SO NPG 1.5NH X1.5NH 7/8D WINGATE",{"$f":"_xlfn.XLOOKUP(C607,DataSource!A:A,DataSource!AH:AH)","v":"2431 1.5 in NH 1.5 in NH 7/8\" bore size(s) NPG ETCH"}]
[null,null,"24317017","SBR TIP SO NPG 1.5NHX1.5NH 7/8D D.C.F.D.",{"$f":"_xlfn.XLOOKUP(C608,DataSource!A:A,DataSource!AH:AH)","v":"2431 1.5 in NH 1.5 in NH 7/8\" bore size(s) NPG ETCH"}]
[null,null,"24317003","SBR TIP SO NPG 1.5NH X 1.5NH 7/8D",{"$f":"_xlfn.XLOOKUP(C609,DataSource!A:A,DataSource!AH:AH)","v":"2431 1.5 in NH 1.5 in NH 7/8\" bore size(s) NPG"}]
[null,null,"24317006","SBRTIP SO NPG 1.5NHX1.5NH 7/8D MTLHDL",{"$f":"_xlfn.XLOOKUP(C610,DataSource!A:A,DataSource!AH:AH)","v":"2431 1.5 in NH 1.5 in NH 7/8\" bore size(s) NPG"}]
[null,null,"24314010","SBR TIP SO1.5NHX1.5NH 15/16D DURHAM FIRE",{"$f":"_xlfn.XLOOKUP(C611,DataSource!A:A,DataSource!AH:AH)","v":"2431 1.5 in NH 1.5 in NH 15/16\" bore size(s) PG ETCH"}]
[null,null,"24314011","SBR TIP SO 1.5NH X 1.5NH 15/16D WFD SEQ",{"$f":"_xlfn.XLOOKUP(C612,DataSource!A:A,DataSource!AH:AH)","v":"2431 1.5 in NH 1.5 in NH 15/16\" bore size(s) PG ETCH"}]
[null,null,"24314012","SBR TIP SO 1.5NH X 1.5NH 15/16D WFD SEQ",{"$f":"_xlfn.XLOOKUP(C613,DataSource!A:A,DataSource!AH:AH)","v":"2431 1.5 in NH 1.5 in NH 15/16\" bore size(s) PG ETCH"}]
[null,null,"24314019","SBR TIP SO 1.5NH X 1.5NH 15/16D ENO FD",{"$f":"_xlfn.XLOOKUP(C614,DataSource!A:A,DataSource!AH:AH)","v":"2431 1.5 in NH 1.5 in NH 15/16\" bore size(s) PG ETCH"}]
[null,null,"24314022","SBR TIP SO 1.5NH X 1.5NH 15/16D SAC",{"$f":"_xlfn.XLOOKUP(C615,DataSource!A:A,DataSource!AH:AH)","v":"2431 1.5 in NH 1.5 in NH 15/16\" bore size(s) PG ETCH"}]
[null,null,"24314023","SBRTIP SO1.5NHX1.5NH 15/16D MTLHDL FCFRD",{"$f":"_xlfn.XLOOKUP(C616,DataSource!A:A,DataSource!AH:AH)","v":"2431 1.5 in NH 1.5 in NH 15/16\" bore size(s) PG ETCH"}]
[null,null,"24314024","SBR TIP SO 1.5NH X 1.5NH 15/16D FCFD TA",{"$f":"_xlfn.XLOOKUP(C617,DataSource!A:A,DataSource!AH:AH)","v":"2431 1.5 in NH 1.5 in NH 15/16\" bore size(s) PG ETCH"}]
[null,null,"24314025","SBR TIP SO 1.5NH X 1.5NH 15/16D WFD SEQ",{"$f":"_xlfn.XLOOKUP(C618,DataSource!A:A,DataSource!AH:AH)","v":"2431 1.5 in NH 1.5 in NH 15/16\" bore size(s) PG ETCH"}]
[null,null,"24314026","SBR TIP SO 1.5NH X 1.5NH 15/16D WFD 001S",{"$f":"_xlfn.XLOOKUP(C619,DataSource!A:A,DataSource!AH:AH)","v":"2431 1.5 in NH 1.5 in NH 15/16\" bore size(s) PG ETCH"}]
[null,null,"24314027","SBR TIP SO 1.5NHX1.5NH 15/16D 1585-1588",{"$f":"_xlfn.XLOOKUP(C620,DataSource!A:A,DataSource!AH:AH)","v":"2431 1.5 in NH 1.5 in NH 15/16\" bore size(s) PG ETCH"}]
[null,null,"24314028","SBR TIP SO 1.5NH X 1.5NH 15/16D N1592",{"$f":"_xlfn.XLOOKUP(C621,DataSource!A:A,DataSource!AH:AH)","v":"2431 1.5 in NH 1.5 in NH 15/16\" bore size(s) PG ETCH"}]
[null,null,"24314029","SBR TIP SO 1.5NH X 1.5NH 15/16D N1593",{"$f":"_xlfn.XLOOKUP(C622,DataSource!A:A,DataSource!AH:AH)","v":"2431 1.5 in NH 1.5 in NH 15/16\" bore size(s) PG ETCH"}]
[null,null,"24314030","SBR TIP SO 1.5NH X 1.5NH 15/16D N1594",{"$f":"_xlfn.XLOOKUP(C623,DataSource!A:A,DataSource!AH:AH)","v":"2431 1.5 in NH 1.5 in NH 15/16\" bore size(s) PG ETCH"}]
[null,null,"24314031","SBR TIP SO 1.5NH X 1.5NH 15/16D N1595",{"$f":"_xlfn.XLOOKUP(C624,DataSource!A:A,DataSource!AH:AH)","v":"2431 1.5 in NH 1.5 in NH 15/16\" bore size(s) PG ETCH"}]
[null,null,"24314001","SBR TIP SO 1.5NH X 1.5NH 15/16D#",{"$f":"_xlfn.XLOOKUP(C625,DataSource!A:A,DataSource!AH:AH)","v":"2431 1.5 in NH 1.5 in NH 15/16\" bore size(s) PG"}]
[null,null,"24317010","SBR TIP SO NPG 1.5NH X 1.5NH 15/16 BDVFD",{"$f":"_xlfn.XLOOKUP(C626,DataSource!A:A,DataSource!AH:AH)","v":"2431 1.5 in NH 1.5 in NH 15/16\" bore size(s) NPG ETCH"}]
[null,null,"24317001","SBR TIP SO NPG 1.5NH X 1.5NH 15/16D",{"$f":"_xlfn.XLOOKUP(C627,DataSource!A:A,DataSource!AH:AH)","v":"2431 1.5 in NH 1.5 in NH 15/16\" bore size(s) NPG"}]
[null,null,"24314034","SBR TIP SO 1.5NHX1.5NH 15/16D COPLE VFD",{"$f":"_xlfn.XLOOKUP(C628,DataSource!A:A,DataSource!AH:AH)","v":"2431 1.5 in NH 1.5 in NH 15/16\" bore size(s)   ETCH"}]
[null,null,"24314038","SBR TIP SO 1.5NH X 1.5NH 1-3/16D",{"$f":"_xlfn.XLOOKUP(C629,DataSource!A:A,DataSource!AH:AH)","v":"2431 1.5 in NH 1.5 in NH 1-3/16\" bore size(s) PG"}]
[null,null,"24314014","SBR TIP SO 1.5NH X 1.5NH 1-1/8D FINLEY",{"$f":"_xlfn.XLOOKUP(C630,DataSource!A:A,DataSource!AH:AH)","v":"2431 1.5 in NH 1.5 in NH 1-1/8\" bore size(s) PG ETCH"}]
[null,null,"24314017","SBR TIP SO 1.5NH X 1.5NH 1-1/8D BCFD",{"$f":"_xlfn.XLOOKUP(C631,DataSource!A:A,DataSource!AH:AH)","v":"2431 1.5 in NH 1.5 in NH 1-1/8\" bore size(s) PG ETCH"}]
[null,null,"24314009","SBR TIP SO 1.5NH X 1.5NH 1-1/8D",{"$f":"_xlfn.XLOOKUP(C632,DataSource!A:A,DataSource!AH:AH)","v":"2431 1.5 in NH 1.5 in NH 1-1/8\" bore size(s) PG"}]
[null,null,"24317009","SBR TIP SO NPG 1.5NH X 1.5NH 1-1/8D",{"$f":"_xlfn.XLOOKUP(C633,DataSource!A:A,DataSource!AH:AH)","v":"2431 1.5 in NH 1.5 in NH 1-1/8\" bore size(s) NPG"}]
[null,null,"24314032","SBR TIP SO 1.5NH X 1.5NH 1-1/4D",{"$f":"_xlfn.XLOOKUP(C634,DataSource!A:A,DataSource!AH:AH)","v":"2431 1.5 in NH 1.5 in NH 1-1/4\" bore size(s) PG"}]
[null,null,"24314036","SBR TIP SO 1.5NH X 1.5NH 1-1/16D",{"$f":"_xlfn.XLOOKUP(C635,DataSource!A:A,DataSource!AH:AH)","v":"2431 1.5 in NH 1.5 in NH 1-1/16\" bore size(s) PG"}]
[null,null,"24314018","SBRTIP SO 1.5NHX1.5NH 1D MTLHDL RBFR",{"$f":"_xlfn.XLOOKUP(C636,DataSource!A:A,DataSource!AH:AH)","v":"2431 1.5 in NH 1.5 in NH 1\" bore size(s) PG ETCH"}]
[null,null,"24314002","SBR TIP SO 1.5NH X 1.5NH 1D",{"$f":"_xlfn.XLOOKUP(C637,DataSource!A:A,DataSource!AH:AH)","v":"2431 1.5 in NH 1.5 in NH 1\" bore size(s) PG"}]
[null,null,"24317007","SBR TIP SO NPG 1.5NH X 1.5NH 1D CONTRA",{"$f":"_xlfn.XLOOKUP(C638,DataSource!A:A,DataSource!AH:AH)","v":"2431 1.5 in NH 1.5 in NH 1\" bore size(s) NPG ETCH"}]
[null,null,"24317002","SBR TIP SO NPG 1.5NH X 1.5NH 1D",{"$f":"_xlfn.XLOOKUP(C639,DataSource!A:A,DataSource!AH:AH)","v":"2431 1.5 in NH 1.5 in NH 1\" bore size(s) NPG"}]
[null,null,"24204019","TIP STK 2.5AFD X 1.5NH 1-3/8D",{"$f":"_xlfn.XLOOKUP(C640,DataSource!A:A,DataSource!AH:AH)","v":"2420 2.5 in QST 1.5 in NPSH 1-3/8\"; 1-1/4\"; 1\" bore size(s) "}]
[null,null,"24204020","TIP STK 2.5NPSH X 1.5NPSH 1-1/4D",{"$f":"_xlfn.XLOOKUP(C641,DataSource!A:A,DataSource!AH:AH)","v":"2420 2.5 in NPSH 1.5 in NPSH 1-1/4\"; 1-1/8\"; 1\" bore size(s) "}]
[null,null,"24204007","TIP STK 2.5NH X 1.5NH 1-3/8D UNIONVILLE",{"$f":"_xlfn.XLOOKUP(C642,DataSource!A:A,DataSource!AH:AH)","v":"2420 2.5 in NH 1.5 in NH 1-3/8\"; 1-1/4\"; 1\" bore size(s) ETCH"}]
[null,null,"24204014","TIP STK 2.5NHX1.5NH 1-3/8D BOILING SPRGS",{"$f":"_xlfn.XLOOKUP(C643,DataSource!A:A,DataSource!AH:AH)","v":"2420 2.5 in NH 1.5 in NH 1-3/8\"; 1-1/4\"; 1\" bore size(s) ETCH"}]
[null,null,"24204001","TIP STK 2.5NH X 1.5NH 1-3/8D",{"$f":"_xlfn.XLOOKUP(C644,DataSource!A:A,DataSource!AH:AH)","v":"2420 2.5 in NH 1.5 in NH 1-3/8\"; 1-1/4\"; 1\" bore size(s) "}]
[null,null,"24204002","TIP STK 2.5NH X 1.5NH 1-1/4D",{"$f":"_xlfn.XLOOKUP(C645,DataSource!A:A,DataSource!AH:AH)","v":"2420 2.5 in NH 1.5 in NH 1-1/4\"; 1-1/8\"; 1\" bore size(s) "}]
[null,null,"24204009","TIP STK 2.5NH X 1.5NH 1-1/2D",{"$f":"_xlfn.XLOOKUP(C646,DataSource!A:A,DataSource!AH:AH)","v":"2420 2.5 in NH 1.5 in NH 1-1/2\"; 1-1/4\"; 1\" bore size(s) "}]
[null,null,"24204012","TIP STK 2.5AFB X 1.5ABU 1-1/2D L/DOM",{"$f":"_xlfn.XLOOKUP(C647,DataSource!A:A,DataSource!AH:AH)","v":"2420 2.5 in FDNY 1.5 in FDNY 1-1/2\"; 1-1/4\"; 1\" bore size(s) "}]
[null,null,"24204017","TIP STK 2.5AII X 1.5NPSH 1-1/2D",{"$f":"_xlfn.XLOOKUP(C648,DataSource!A:A,DataSource!AH:AH)","v":"2420 2.5 in CSA 1.5 in NPSH 1-1/2\"; 1-1/4\"; 1\" bore size(s) "}]
[null,null,"24204015","TIP STK 2.5BAF X 1.5NPSH 1-3/8D",{"$f":"_xlfn.XLOOKUP(C649,DataSource!A:A,DataSource!AH:AH)","v":"2420 2.5 in BAT 1.5 in NPSH 1-3/8\"; 1-1/4\"; 1\" bore size(s) "}]
[null,null,"24204016","TIP STK 2.5BAF X 1.5NPSH 1-1/4D",{"$f":"_xlfn.XLOOKUP(C650,DataSource!A:A,DataSource!AH:AH)","v":"2420 2.5 in BAT 1.5 in NPSH 1-1/4\"; 1-1/8\"; 1\" bore size(s) "}]
[null,null,"24204013","TIP STK 2.5BAF X 1.5NPSH 1-1/2D",{"$f":"_xlfn.XLOOKUP(C651,DataSource!A:A,DataSource!AH:AH)","v":"2420 2.5 in BAT 1.5 in NPSH 1-1/2\"; 1-1/4\"; 1\" bore size(s) "}]
[null,null,"24204008","TIP STK 2.5BAF X 1.5NH 1-1/4D",{"$f":"_xlfn.XLOOKUP(C652,DataSource!A:A,DataSource!AH:AH)","v":"2420 2.5 in BAT 1.5 in NH 1-1/4\"; 1-1/8\"; 1\" bore size(s) "}]
[null,null,"24204010","TIP STK 2.5AKB X 1.5NPSH 1-1/4D",{"$f":"_xlfn.XLOOKUP(C653,DataSource!A:A,DataSource!AH:AH)","v":"2420 2.5 in AKB 1.5 in NPSH 1-1/4\"; 1-1/8\"; 1\" bore size(s) "}]
[null,null,"24204006","TIP STK 2.5AKB X 1.5NPSH 1-1/2D",{"$f":"_xlfn.XLOOKUP(C654,DataSource!A:A,DataSource!AH:AH)","v":"2420 2.5 in AKB 1.5 in NPSH 1-1/2\"; 1-1/4\"; 1\" bore size(s) "}]
[null,null,"24204005","TIP STK 2.5AIK X 1.5NH 1-1/4D",{"$f":"_xlfn.XLOOKUP(C655,DataSource!A:A,DataSource!AH:AH)","v":"2420 2.5 in AIK 1.5 in NH 1-1/4\"; 1-1/8\"; 1\" bore size(s) "}]
[null,null,"23934004","PP W/STK TIPS 2.5AFY X 1.5NH",{"$f":"_xlfn.XLOOKUP(C656,DataSource!A:A,DataSource!AH:AH)","v":"2393 2.5 in PITT6 1.5 in NH 1-1/4\"; 1-1/8\"; 1\" bore size(s)  "}]
[null,null,"23934008","PP W/STK TIPS 2.5NH X 1.5NPSH",{"$f":"_xlfn.XLOOKUP(C657,DataSource!A:A,DataSource!AH:AH)","v":"2393 2.5 in NH 1.5 in NPSH 1-1/4\"; 1-1/8\"; 1\" bore size(s)  "}]
[null,null,"23934003","PP W/STK TIPS 2.5NH X 1.5NH RES-ENG 208",{"$f":"_xlfn.XLOOKUP(C658,DataSource!A:A,DataSource!AH:AH)","v":"2393 2.5 in NH 1.5 in NH 1-1/4\"; 1-1/8\"; 1\" bore size(s)  ETCH"}]
[null,null,"23934005","PP W/STK TIPS 2.5NH X 1.5NH UNIONVILLE",{"$f":"_xlfn.XLOOKUP(C659,DataSource!A:A,DataSource!AH:AH)","v":"2393 2.5 in NH 1.5 in NH 1-1/4\"; 1-1/8\"; 1\" bore size(s)  ETCH"}]
[null,null,"23934009","PP W/STK TIPS 2.5NH X 1.5NH SACO FD LOGO",{"$f":"_xlfn.XLOOKUP(C660,DataSource!A:A,DataSource!AH:AH)","v":"2393 2.5 in NH 1.5 in NH 1-1/4\"; 1-1/8\"; 1\" bore size(s)  ETCH"}]
[null,null,"23934001","PP W/STK TIPS 2.5NH X 1.5NH",{"$f":"_xlfn.XLOOKUP(C661,DataSource!A:A,DataSource!AH:AH)","v":"2393 2.5 in NH 1.5 in NH 1-1/4\"; 1-1/8\"; 1\" bore size(s)  "}]
[null,null,"23934011","PP W/STK TIPS 2.5AJD X 1.5NH",{"$f":"_xlfn.XLOOKUP(C662,DataSource!A:A,DataSource!AH:AH)","v":"2393 2.5 in NH 1.5 in NH 1-1/4\"; 1-1/8\"; 1\" bore size(s)  "}]
[null,null,"23934007","PP W/STK TIPS 2.5BAF X 1.5NPSH",{"$f":"_xlfn.XLOOKUP(C663,DataSource!A:A,DataSource!AH:AH)","v":"2393 2.5 in BAT 1.5 in NPSH 1-1/4\"; 1-1/8\"; 1\" bore size(s)  "}]
[null,null,"23934002","PP W/STK TIPS 2.5AKB X 1.5NPSH",{"$f":"_xlfn.XLOOKUP(C664,DataSource!A:A,DataSource!AH:AH)","v":"2393 2.5 in AKB 1.5 in NPSH 1-1/4\"; 1-1/8\"; 1\" bore size(s)  "}]
[null,null,"23934013","PP W/STK TIPS 2.5AKA X 1.5NPSH",{"$f":"_xlfn.XLOOKUP(C665,DataSource!A:A,DataSource!AH:AH)","v":"2393 2.5 in AKA 1.5 in NPSH 1-1/4\"; 1-1/8\"; 1\" bore size(s)  "}]
[null,null,"23904028","PLAYPIPE W/SO 2.5AHU X 1.5NH",{"$f":"_xlfn.XLOOKUP(C666,DataSource!A:A,DataSource!AH:AH)","v":"2393 2.5 in AHU 1.5 in NH  "}]
[null,null,"23934006","PP W/STK TIPS 2.5AHB X 1.5NH",{"$f":"_xlfn.XLOOKUP(C667,DataSource!A:A,DataSource!AH:AH)","v":"2393 2.5 in AHB 1.5 in NH 1-1/4\"; 1-1/8\"; 1\" bore size(s)  "}]
[null,null,"23934010","PP W/STK TIPS 2.5AEA X 1.5NH",{"$f":"_xlfn.XLOOKUP(C668,DataSource!A:A,DataSource!AH:AH)","v":"2393 2.5 in AEA 1.5 in NH 1-1/4\"; 1-1/8\"; 1\" bore size(s)  "}]
[null,null,"23904021","PLAYPIPE W/SO 75MM X 1.5BSP",{"$f":"_xlfn.XLOOKUP(C669,DataSource!A:A,DataSource!AH:AH)","v":"2390 3 in STORZ 1.5 in BSP  "}]
[null,null,"23904011","PLAYPIPE W/SO 2.5AFY X 1.5NH",{"$f":"_xlfn.XLOOKUP(C670,DataSource!A:A,DataSource!AH:AH)","v":"2390 2.5 in PITT6 1.5 in NH  "}]
[null,null,"23904027","PLAYPIPE W/SO 2.5AEF X 1.5NH",{"$f":"_xlfn.XLOOKUP(C671,DataSource!A:A,DataSource!AH:AH)","v":"2390 2.5 in NYCORP 1.5 in NH  "}]
[null,null,"23904018","PLAYPIPE W/SO 2.5NH X 1.5NPSH",{"$f":"_xlfn.XLOOKUP(C672,DataSource!A:A,DataSource!AH:AH)","v":"2390 2.5 in NH 1.5 in NPSH  "}]
[null,null,"23904005","PLAYPIPE W/SO 2.5NH X 1.5NH WFD SEQ",{"$f":"_xlfn.XLOOKUP(C673,DataSource!A:A,DataSource!AH:AH)","v":"2390 2.5 in NH 1.5 in NH   ETCH"}]
[null,null,"23904010","PLAYPIPE W/SO 2.5NH X 1.5NH RES-ENG 208",{"$f":"_xlfn.XLOOKUP(C674,DataSource!A:A,DataSource!AH:AH)","v":"2390 2.5 in NH 1.5 in NH   ETCH"}]
[null,null,"23904012","PLAYPIPE W/SO 2.5NH X 1.5NH UNIONVILLE",{"$f":"_xlfn.XLOOKUP(C675,DataSource!A:A,DataSource!AH:AH)","v":"2390 2.5 in NH 1.5 in NH   ETCH"}]
[null,null,"23904019","PLAYPIPE W/SO 2.5NHX1.5NH WFD 001-20-2.5",{"$f":"_xlfn.XLOOKUP(C676,DataSource!A:A,DataSource!AH:AH)","v":"2390 2.5 in NH 1.5 in NH   ETCH"}]
[null,null,"23904020","PLAYPIPE W/SO 2.5NH X 1.5NH SACO FD LOGO",{"$f":"_xlfn.XLOOKUP(C677,DataSource!A:A,DataSource!AH:AH)","v":"2390 2.5 in NH 1.5 in NH   ETCH"}]
[null,null,"23904026","PLAYPIPE W/SO 2.5NH X 1.5NH D.C.F.D.",{"$f":"_xlfn.XLOOKUP(C678,DataSource!A:A,DataSource!AH:AH)","v":"2390 2.5 in NH 1.5 in NH   ETCH"}]
[null,null,"23904001","PLAYPIPE W/SO 2.5NH X 1.5NH#",{"$f":"_xlfn.XLOOKUP(C679,DataSource!A:A,DataSource!AH:AH)","v":"2390 2.5 in NH 1.5 in NH  "}]
[null,null,"23904023","PLAYPIPE W/SO 2.5AJD X 1.5NH",{"$f":"_xlfn.XLOOKUP(C680,DataSource!A:A,DataSource!AH:AH)","v":"2390 2.5 in NH 1.5 in NH  "}]
[null,null,"23904009","PLAYPIPE W/SO 2.5JIM X 1.5NH",{"$f":"_xlfn.XLOOKUP(C681,DataSource!A:A,DataSource!AH:AH)","v":"2390 2.5 in JIM 1.5 in NH  "}]
[null,null,"23904006","PLAYPIPE W/SO 2.5AII X 1.5NPSH",{"$f":"_xlfn.XLOOKUP(C682,DataSource!A:A,DataSource!AH:AH)","v":"2390 2.5 in CSA 1.5 in NPSH  "}]
[null,null,"23904014","PLAYPIPE W/SO 2.5BSP X 1.5NH",{"$f":"_xlfn.XLOOKUP(C683,DataSource!A:A,DataSource!AH:AH)","v":"2390 2.5 in BSP 1.5 in NH  "}]
[null,null,"23904015","PLAYPIPE W/SO 2.5BSP X 1.5BSP",{"$f":"_xlfn.XLOOKUP(C684,DataSource!A:A,DataSource!AH:AH)","v":"2390 2.5 in BSP 1.5 in BSP  "}]
[null,null,"23904016","PLAYPIPE W/SO 2.5BAF X 1.5NPSH",{"$f":"_xlfn.XLOOKUP(C685,DataSource!A:A,DataSource!AH:AH)","v":"2390 2.5 in BAT 1.5 in NPSH  "}]
[null,null,"23904024","PLAYPIPE W/SO 2.5BAF X 1.5NH",{"$f":"_xlfn.XLOOKUP(C686,DataSource!A:A,DataSource!AH:AH)","v":"2390 2.5 in BAT 1.5 in NH  "}]
[null,null,"23904007","PLAYPIPE W/SO 2.5AKB X 1.5NPSH",{"$f":"_xlfn.XLOOKUP(C687,DataSource!A:A,DataSource!AH:AH)","v":"2390 2.5 in AKB 1.5 in NPSH  "}]
[null,null,"23904030","PLAYPIPE W/SO 2.5AKA X 1.5NPSH",{"$f":"_xlfn.XLOOKUP(C688,DataSource!A:A,DataSource!AH:AH)","v":"2390 2.5 in AKA 1.5 in NPSH  "}]
[null,null,"23904017","PLAYPIPE W/SO 2.5AIJ X 1.5NPSH",{"$f":"_xlfn.XLOOKUP(C689,DataSource!A:A,DataSource!AH:AH)","v":"2390 2.5 in AIJ 1.5 in NPSH  "}]
[null,null,"23904013","PLAYPIPE W/SO 2.5AHB X 1.5NH",{"$f":"_xlfn.XLOOKUP(C690,DataSource!A:A,DataSource!AH:AH)","v":"2390 2.5 in AHB 1.5 in NH  "}]
[null,null,"23904008","PLAYPIPE W/SO 2.5AGZ X 1.5NH",{"$f":"_xlfn.XLOOKUP(C691,DataSource!A:A,DataSource!AH:AH)","v":"2390 2.5 in AGZ 1.5 in NH  "}]
[null,null,"23904022","PLAYPIPE W/SO 2.5AEA X 1.5NH",{"$f":"_xlfn.XLOOKUP(C692,DataSource!A:A,DataSource!AH:AH)","v":"2390 2.5 in AEA 1.5 in NH  "}]
[null,null,"21300103","SHUTOFF TRIDENT 2.5 AFD F X 2.5AFD M",{"$f":"_xlfn.XLOOKUP(C693,DataSource!A:A,DataSource!AH:AH)","v":"2130 2.5 in QST 2.5 in QST PG"}]
[null,null,"21300116","SHUTOFF TRIDENT 2.5 AFY F X 2.5AFY M",{"$f":"_xlfn.XLOOKUP(C694,DataSource!A:A,DataSource!AH:AH)","v":"2130 2.5 in PITT6 2.5 in PITT6 PG"}]
[null,null,"21300106","SHUTOFF TRIDENT 2.5NPSH F X 2.5NPSH",{"$f":"_xlfn.XLOOKUP(C695,DataSource!A:A,DataSource!AH:AH)","v":"2130 2.5 in NPSH 2.5 in NPSH PG"}]
[null,null,"21300115","S/OFF TRIDENT 2.5NHFX2.5NHM ETCH MPFD",{"$f":"_xlfn.XLOOKUP(C696,DataSource!A:A,DataSource!AH:AH)","v":"2130 2.5 in NH 2.5 in NH PG ETCH"}]
[null,null,"21300117","SH/OFF TRIDENT 2.5NHX2.5NH SEQ ETCH TFD",{"$f":"_xlfn.XLOOKUP(C697,DataSource!A:A,DataSource!AH:AH)","v":"2130 2.5 in NH 2.5 in NH PG ETCH"}]
[null,null,"21300120","SH/OFF TRIDENT 2.5NHX2.5NH SEQ ETCH TFD",{"$f":"_xlfn.XLOOKUP(C698,DataSource!A:A,DataSource!AH:AH)","v":"2130 2.5 in NH 2.5 in NH PG ETCH"}]
[null,null,"21300121","SHUTOFF TRIDENT 2.5NH X 2.5NH TFD",{"$f":"_xlfn.XLOOKUP(C699,DataSource!A:A,DataSource!AH:AH)","v":"2130 2.5 in NH 2.5 in NH PG ETCH"}]
[null,null,"21300122","SH/OFF TRIDENT 2.5NHX2.5NH SEQ ETCH TFD",{"$f":"_xlfn.XLOOKUP(C700,DataSource!A:A,DataSource!AH:AH)","v":"2130 2.5 in NH 2.5 in NH PG ETCH"}]
[null,null,"21300123","SH/OFF TRIDENT 2.5NHX2.5NH SEQ ETCH",{"$f":"_xlfn.XLOOKUP(C701,DataSource!A:A,DataSource!AH:AH)","v":"2130 2.5 in NH 2.5 in NH PG ETCH"}]
[null,null,"21300100","SHUTOFF TRIDENT 2.5 NH F X 2.5 NH M#",{"$f":"_xlfn.XLOOKUP(C702,DataSource!A:A,DataSource!AH:AH)","v":"2130 2.5 in NH 2.5 in NH PG"}]
[null,null,"21300119","SHUTOFF TRIDENT 2.5BIM X 2.5BSP M PY",{"$f":"_xlfn.XLOOKUP(C703,DataSource!A:A,DataSource!AH:AH)","v":"2130 2.5 in BIM 2.5 in BSP PG"}]
[null,null,"21300109","SHUTOFF TRIDENT 2.5BAF F X 2.5BAF M",{"$f":"_xlfn.XLOOKUP(C704,DataSource!A:A,DataSource!AH:AH)","v":"2130 2.5 in BAT 2.5 in BAT PG"}]
[null,null,"21300114","SHUTOFF TRIDENT 2.5 AUS F X 2.5AFD M",{"$f":"_xlfn.XLOOKUP(C705,DataSource!A:A,DataSource!AH:AH)","v":"2130 2.5 in AUS 2.5 in QST PG"}]
[null,null,"21300111","SHUTOFF TRIDENT 2.5AIK F X 2.5AIK M",{"$f":"_xlfn.XLOOKUP(C706,DataSource!A:A,DataSource!AH:AH)","v":"2130 2.5 in AIK 2.5 in AIK PG"}]
[null,null,"21300113","SHUTOFF TRIDENT 2.5AGA F X 2.5AGA M",{"$f":"_xlfn.XLOOKUP(C707,DataSource!A:A,DataSource!AH:AH)","v":"2130 2.5 in AGA 2.5 in AGA PG"}]
[null,null,"21300118","SHUTOFF TRIDENT 2.5ACY X 2.5NH",{"$f":"_xlfn.XLOOKUP(C708,DataSource!A:A,DataSource!AH:AH)","v":"2130 2.5 in ACY 2.5 in NH PG"}]
[null,null,"21274005","SHUTOFF 2.5BIM X 1.5NH",{"$f":"_xlfn.XLOOKUP(C709,DataSource!A:A,DataSource!AH:AH)","v":"2127 2.5 in BIM 1.5 in NH PG"}]
[null,null,"21274024","SHUTOFF 2.5BIM X 1.5BSP",{"$f":"_xlfn.XLOOKUP(C710,DataSource!A:A,DataSource!AH:AH)","v":"2127 2.5 in BIM 1.5 in BSP PG"}]
[null,null,"21274009","SHUTOFF ZT 52MM X 1.5NH",{"$f":"_xlfn.XLOOKUP(C711,DataSource!A:A,DataSource!AH:AH)","v":"2127 2 in STORZ 1.5 in NH PG ZT"}]
[null,null,"21274027","SHUTOFF 52MM X 1.5NH",{"$f":"_xlfn.XLOOKUP(C712,DataSource!A:A,DataSource!AH:AH)","v":"2127 2 in STORZ 1.5 in NH PG"}]
[null,null,"21274042","SHUTOFF 1.5ABT X 1.5ABT",{"$f":"_xlfn.XLOOKUP(C713,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in PCT 1.5 in PCT PG"}]
[null,null,"21274033","SHUTOFF 1.5ABQ X 1.5ABQ",{"$f":"_xlfn.XLOOKUP(C714,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in NYCORP 1.5 in NYCORP PG"}]
[null,null,"21274022","SHUTOFF 1.5NPSH X 1.5NPSH KITTERY FIRE",{"$f":"_xlfn.XLOOKUP(C715,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in NPSH 1.5 in NPSH PG ETCH"}]
[null,null,"21274006","SHUTOFF 1.5NPSH X 1.5NPSH",{"$f":"_xlfn.XLOOKUP(C716,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in NPSH 1.5 in NPSH PG"}]
[null,null,"21274043","SHUTOFF 1.5NPSH X 1.5NPSH  METAL HDL",{"$f":"_xlfn.XLOOKUP(C717,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in NPSH 1.5 in NPSH PG"}]
[null,null,"21277006","SHUTOFF NPG 1.5NPSH X 1.5NPSH",{"$f":"_xlfn.XLOOKUP(C718,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in NPSH 1.5 in NPSH NPG"}]
[null,null,"21274011","SHUTOFF 1.5NPSH X 1.5NH",{"$f":"_xlfn.XLOOKUP(C719,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in NPSH 1.5 in NH PG"}]
[null,null,"21277011","SHUTOFF NPG 1.5NPSH X 1.5NH",{"$f":"_xlfn.XLOOKUP(C720,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in NPSH 1.5 in NH NPG"}]
[null,null,"21274056","SHUTOFF ZT 1.5NH X 1.5NH",{"$f":"_xlfn.XLOOKUP(C721,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in NH 1.5 in NH PG ZT"}]
[null,null,"21274003","SHUTOFF 1.5NH X 1.5NH DURHAM FIRE RES",{"$f":"_xlfn.XLOOKUP(C722,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in NH 1.5 in NH PG ETCH"}]
[null,null,"21274004","SHUTOFF 1.5NH X 1.5NH CLEVELAND",{"$f":"_xlfn.XLOOKUP(C723,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in NH 1.5 in NH PG ETCH"}]
[null,null,"21274008","SHUTOFF 1.5NH X 1.5NH FINLEYFIRE.COM",{"$f":"_xlfn.XLOOKUP(C724,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in NH 1.5 in NH PG ETCH"}]
[null,null,"21274010","SHUTOFF 1.5NH X 1.5NH SEQ ETCH TFD",{"$f":"_xlfn.XLOOKUP(C725,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in NH 1.5 in NH PG ETCH"}]
[null,null,"21274012","SHUTOFF 1.5NH X 1.5NH SEQ ETCH TFD",{"$f":"_xlfn.XLOOKUP(C726,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in NH 1.5 in NH PG ETCH"}]
[null,null,"21274013","SHUTOFF 1.5NH X 1.5NH RES-ENG 208",{"$f":"_xlfn.XLOOKUP(C727,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in NH 1.5 in NH PG ETCH"}]
[null,null,"21274015","SHUTOFF 1.5NH X 1.5NH FLFD E13",{"$f":"_xlfn.XLOOKUP(C728,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in NH 1.5 in NH PG ETCH"}]
[null,null,"21274016","SHUTOFF 1.5NH X 1.5NH FLFD E8",{"$f":"_xlfn.XLOOKUP(C729,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in NH 1.5 in NH PG ETCH"}]
[null,null,"21274017","SHUTOFF 1.5NH X 1.5NH FLFD SPARE",{"$f":"_xlfn.XLOOKUP(C730,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in NH 1.5 in NH PG ETCH"}]
[null,null,"21274018","SHUTOFF 1.5NH X 1.5NH UNIONVILLE",{"$f":"_xlfn.XLOOKUP(C731,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in NH 1.5 in NH PG ETCH"}]
[null,null,"21274019","SHUTOFF 1.5NH X 1.5NH RICHMOND FD",{"$f":"_xlfn.XLOOKUP(C732,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in NH 1.5 in NH PG ETCH"}]
[null,null,"21274020","SHUTOFF 1.5NH X 1.5NH FLFD",{"$f":"_xlfn.XLOOKUP(C733,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in NH 1.5 in NH PG ETCH"}]
[null,null,"21274021","SHUTOFF 1.5NH X 1.5NH LITTLETON",{"$f":"_xlfn.XLOOKUP(C734,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in NH 1.5 in NH PG ETCH"}]
[null,null,"21274023","SHUTOFF 1.5NH X 1.5NH SEQ ETCH TFD",{"$f":"_xlfn.XLOOKUP(C735,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in NH 1.5 in NH PG ETCH"}]
[null,null,"21274026","SHUTOFF 1.5NH X 1.5NH SEQ ETCH TFD",{"$f":"_xlfn.XLOOKUP(C736,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in NH 1.5 in NH PG ETCH"}]
[null,null,"21274028","SHUTOFF 1.5NH X 1.5NH SEQ ETCH TFD",{"$f":"_xlfn.XLOOKUP(C737,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in NH 1.5 in NH PG ETCH"}]
[null,null,"21274029","SHUTOFF 1.5NH X 1.5NH D.F.D.",{"$f":"_xlfn.XLOOKUP(C738,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in NH 1.5 in NH PG ETCH"}]
[null,null,"21274030","SHUTOFF 1.5NH X 1.5NH WFD, E-31",{"$f":"_xlfn.XLOOKUP(C739,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in NH 1.5 in NH PG ETCH"}]
[null,null,"21274031","SHUTOFF 1.5NH X 1.5NH FLFR",{"$f":"_xlfn.XLOOKUP(C740,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in NH 1.5 in NH PG ETCH"}]
[null,null,"21274032","SHUTOFF 1.5NH X 1.5NH SEQ ETCH F18960",{"$f":"_xlfn.XLOOKUP(C741,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in NH 1.5 in NH PG ETCH"}]
[null,null,"21274034","SHUTOFF 1.5NH X 1.5NH LFC4",{"$f":"_xlfn.XLOOKUP(C742,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in NH 1.5 in NH PG ETCH"}]
[null,null,"21274035","SHUTOFF 1.5NH X 1.5NH GROVETOWN",{"$f":"_xlfn.XLOOKUP(C743,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in NH 1.5 in NH PG ETCH"}]
[null,null,"21274037","SHUTOFF 1.5NH X 1.5NH FLFR SQ29",{"$f":"_xlfn.XLOOKUP(C744,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in NH 1.5 in NH PG ETCH"}]
[null,null,"21274038","SHUTOFF 1.5NH X 1.5NH FLFR E49",{"$f":"_xlfn.XLOOKUP(C745,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in NH 1.5 in NH PG ETCH"}]
[null,null,"21274039","SHUTOFF 1.5NH X 1.5NH FLFR E2",{"$f":"_xlfn.XLOOKUP(C746,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in NH 1.5 in NH PG ETCH"}]
[null,null,"21274040","SHUTOFF 1.5NH X 1.5NH FLFR E46",{"$f":"_xlfn.XLOOKUP(C747,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in NH 1.5 in NH PG ETCH"}]
[null,null,"21274041","SHUTOFF 1.5NH X 1.5NH FLFR SQ53",{"$f":"_xlfn.XLOOKUP(C748,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in NH 1.5 in NH PG ETCH"}]
[null,null,"21274044","SHUTOFF 1.5NH X 1.5NH CONTRA COSTA FIRE",{"$f":"_xlfn.XLOOKUP(C749,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in NH 1.5 in NH PG ETCH"}]
[null,null,"21274045","SHUTOFF 1.5NHX1.5NH SEQ ETCH SB15-20-001",{"$f":"_xlfn.XLOOKUP(C750,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in NH 1.5 in NH PG ETCH"}]
[null,null,"21274048","SHUTOFF 1.5NH X 1.5NH ENG80INE",{"$f":"_xlfn.XLOOKUP(C751,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in NH 1.5 in NH PG ETCH"}]
[null,null,"21274049","SHUTOFF 1.5NH X 1.5NH COPLE VFD",{"$f":"_xlfn.XLOOKUP(C752,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in NH 1.5 in NH PG ETCH"}]
[null,null,"21274051","SHUTOFF 1.5NH X 1.5NH BFC-E1",{"$f":"_xlfn.XLOOKUP(C753,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in NH 1.5 in NH PG ETCH"}]
[null,null,"21274052","SHUTOFF 1.5NH X 1.5NH OCEAN VIEW FIRE CO",{"$f":"_xlfn.XLOOKUP(C754,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in NH 1.5 in NH PG ETCH"}]
[null,null,"21274053","SHUTOFF 1.5NH X 1.5NH SEQ ETCH F20009",{"$f":"_xlfn.XLOOKUP(C755,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in NH 1.5 in NH PG ETCH"}]
[null,null,"21274001","SHUTOFF 1.5NH X 1.5NH#",{"$f":"_xlfn.XLOOKUP(C756,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in NH 1.5 in NH PG"}]
[null,null,"21274014","SHUTOFF 1.5NH X 1.5NH METAL HDL",{"$f":"_xlfn.XLOOKUP(C757,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in NH 1.5 in NH PG"}]
[null,null,"21277003","SHUTOFF NPG 1.5NH X 1.5NH CONTRA COSTA",{"$f":"_xlfn.XLOOKUP(C758,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in NH 1.5 in NH NPG ETCH"}]
[null,null,"21277007","SHUTOFF NPG 1.5NH X 1.5NH ENG80INE",{"$f":"_xlfn.XLOOKUP(C759,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in NH 1.5 in NH NPG ETCH"}]
[null,null,"21277008","SHUTOFF NPG 1.5NH X 1.5NH CREEDMOOR FD",{"$f":"_xlfn.XLOOKUP(C760,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in NH 1.5 in NH NPG ETCH"}]
[null,null,"21277010","SHUTOFF NPG 1.5NH X1.5NH MTLHDL SPC LOGO",{"$f":"_xlfn.XLOOKUP(C761,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in NH 1.5 in NH NPG ETCH"}]
[null,null,"21277012","SHUTOFF NPG 1.5NH X 1.5NH SUMMERFIELD",{"$f":"_xlfn.XLOOKUP(C762,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in NH 1.5 in NH NPG ETCH"}]
[null,null,"21277018","SHUTOFF NPG 1.5NH X 1.5NH UNIONVILLE",{"$f":"_xlfn.XLOOKUP(C763,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in NH 1.5 in NH NPG ETCH"}]
[null,null,"21277001","SHUTOFF NPG 1.5NH X 1.5NH",{"$f":"_xlfn.XLOOKUP(C764,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in NH 1.5 in NH NPG"}]
[null,null,"21277002","SHUTOFF NPG 1.5NH X 1.5NH MTLHDL",{"$f":"_xlfn.XLOOKUP(C765,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in NH 1.5 in NH NPG"}]
[null,null,"21274002","SHUTOFF 1.5ABU X 1.5ABU FDNY",{"$f":"_xlfn.XLOOKUP(C766,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in FDNY 1.5 in FDNY PG"}]
[null,null,"21277004","SHUTOFF NPG 1.5ABU X 1.5ABU FDNY",{"$f":"_xlfn.XLOOKUP(C767,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in FDNY 1.5 in FDNY NPG"}]
[null,null,"21274036","SHUTOFF 1.5BSP F X 1.5NH M",{"$f":"_xlfn.XLOOKUP(C768,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in BSP 1.5 in NH PG"}]
[null,null,"21274007","SHUTOFF 1.5BSP F X 1.5BSP M",{"$f":"_xlfn.XLOOKUP(C769,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in BSP 1.5 in BSP PG"}]
[null,null,"21274025","SHUTOFF 1.5ABX X 1.5ABX",{"$f":"_xlfn.XLOOKUP(C770,DataSource!A:A,DataSource!AH:AH)","v":"2127 1.5 in ABX 1.5 in ABX PG"}]
[null,null,"21264057","SHUTOFF 65MM X 1.5NPSH",{"$f":"_xlfn.XLOOKUP(C771,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in STORZ 1.5 in NPSH PG"}]
[null,null,"21264015","SHUTOFF 2.5AFD X 1.5NPSH",{"$f":"_xlfn.XLOOKUP(C772,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in QST 1.5 in NPSH PG"}]
[null,null,"21264031","SHUTOFF 2.5AFY  X 1.5NH",{"$f":"_xlfn.XLOOKUP(C773,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in PITT6 1.5 in NPSH PG"}]
[null,null,"21264018","SHUTOFF 2.5AFY X 1.5NH METAL HDL",{"$f":"_xlfn.XLOOKUP(C774,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in PITT6 1.5 in NH PG"}]
[null,null,"21264041","SHUTOFF 2.5AEF X 1.5ABQ",{"$f":"_xlfn.XLOOKUP(C775,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in NYCORP 1.5 in NYCORP PG"}]
[null,null,"21264032","SHUTOFF 2.5AEF  X 1.5NPSH",{"$f":"_xlfn.XLOOKUP(C776,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in NYCORP 1.5 in NPSH PG"}]
[null,null,"21264033","SHUTOFF 2.5AEF X 1.5NPSH METAL HDL",{"$f":"_xlfn.XLOOKUP(C777,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in NYCORP 1.5 in NPSH PG"}]
[null,null,"21264012","SHUTOFF 2.5AEF X 1.5NH ETCH 2.5\" NY CORP",{"$f":"_xlfn.XLOOKUP(C778,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in NYCORP 1.5 in NH PG ETCH"}]
[null,null,"21264009","SHUTOFF 2.5AEF  X 1.5NH",{"$f":"_xlfn.XLOOKUP(C779,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in NYCORP 1.5 in NH PG"}]
[null,null,"21264030","SHUTOFF 2.5AEF X 1.5NH METAL HDL",{"$f":"_xlfn.XLOOKUP(C780,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in NYCORP 1.5 in NH PG"}]
[null,null,"21267009","SHUTOFF NPG 2.5AEF  X 1.5NH",{"$f":"_xlfn.XLOOKUP(C781,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in NYCORP 1.5 in NH NPG"}]
[null,null,"21264014","SHUTOFF 2.5NPSH  X 1.5NPSH",{"$f":"_xlfn.XLOOKUP(C782,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in NPSH 1.5 in NPSH PG"}]
[null,null,"21267014","SHUTOFF NPG 2.5NPSH  X 1.5NPSH",{"$f":"_xlfn.XLOOKUP(C783,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in NPSH 1.5 in NPSH NPG"}]
[null,null,"21264006","SHUTOFF 2.5NH  X 1.5NPSH",{"$f":"_xlfn.XLOOKUP(C784,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in NH 1.5 in NPSH PG"}]
[null,null,"21267006","SHUTOFF NPG 2.5NH  X 1.5NPSH",{"$f":"_xlfn.XLOOKUP(C785,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in NH 1.5 in NPSH NPG"}]
[null,null,"21264054","SHUTOFF ZT 2.5NH X 1.5NH",{"$f":"_xlfn.XLOOKUP(C786,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in NH 1.5 in NH PG ZT"}]
[null,null,"21264005","SHUTOFF 2.5NH  X 1.5NH DURHAM FIRE RES",{"$f":"_xlfn.XLOOKUP(C787,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in NH 1.5 in NH PG ETCH"}]
[null,null,"21264008","SHUTOFF 2.5NH  X 1.5NH GASTONIA FD",{"$f":"_xlfn.XLOOKUP(C788,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in NH 1.5 in NH PG ETCH"}]
[null,null,"21264010","SHUTOFF 2.5NH  X 1.5NH NCFD L-204",{"$f":"_xlfn.XLOOKUP(C789,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in NH 1.5 in NH PG ETCH"}]
[null,null,"21264011","SHUTOFF 2.5NH  X 1.5NH SPEC ETCH 2.5\" NH",{"$f":"_xlfn.XLOOKUP(C790,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in NH 1.5 in NH PG ETCH"}]
[null,null,"21264020","SHUTOFF 2.5NH  X 1.5NH RES-ENG 208",{"$f":"_xlfn.XLOOKUP(C791,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in NH 1.5 in NH PG ETCH"}]
[null,null,"21264022","SHUTOFF 2.5NH  X 1.5NH SHERBORN",{"$f":"_xlfn.XLOOKUP(C792,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in NH 1.5 in NH PG ETCH"}]
[null,null,"21264023","SHUTOFF 2.5NH X 1.5NH FLFD E13",{"$f":"_xlfn.XLOOKUP(C793,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in NH 1.5 in NH PG ETCH"}]
[null,null,"21264024","SHUTOFF 2.5NH X 1.5NH FLFD E8",{"$f":"_xlfn.XLOOKUP(C794,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in NH 1.5 in NH PG ETCH"}]
[null,null,"21264025","SHUTOFF 2.5NH X 1.5NH FLFD SPARE",{"$f":"_xlfn.XLOOKUP(C795,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in NH 1.5 in NH PG ETCH"}]
[null,null,"21264026","SHUTOFF 2.5NH X 1.5NH RICHMOND FD",{"$f":"_xlfn.XLOOKUP(C796,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in NH 1.5 in NH PG ETCH"}]
[null,null,"21264027","SHUTOFF 2.5NH X 1.5NH FLFD",{"$f":"_xlfn.XLOOKUP(C797,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in NH 1.5 in NH PG ETCH"}]
[null,null,"21264029","SHUTOFF 2.5NH X 1.5NH ENO FD",{"$f":"_xlfn.XLOOKUP(C798,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in NH 1.5 in NH PG ETCH"}]
[null,null,"21264035","SHUTOFF 2.5NH X 1.5NH CHARLOTTE FD",{"$f":"_xlfn.XLOOKUP(C799,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in NH 1.5 in NH PG ETCH"}]
[null,null,"21264036","SHUTOFF 2.5NH  X 1.5NH D.F.D.",{"$f":"_xlfn.XLOOKUP(C800,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in NH 1.5 in NH PG ETCH"}]
[null,null,"21264037","SHUTOFF 2.5NH  X 1.5NH FCFD TA",{"$f":"_xlfn.XLOOKUP(C801,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in NH 1.5 in NH PG ETCH"}]
[null,null,"21264040","SHUTOFF 2.5NH X 1.5NH LFC4",{"$f":"_xlfn.XLOOKUP(C802,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in NH 1.5 in NH PG ETCH"}]
[null,null,"21264043","SHUTOFF 2.5NH X 1.5NH FLFR SQ49",{"$f":"_xlfn.XLOOKUP(C803,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in NH 1.5 in NH PG ETCH"}]
[null,null,"21264044","SHUTOFF 2.5NH X 1.5NH FLFR E49",{"$f":"_xlfn.XLOOKUP(C804,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in NH 1.5 in NH PG ETCH"}]
[null,null,"21264045","SHUTOFF 2.5NH X 1.5NH FLFR E2",{"$f":"_xlfn.XLOOKUP(C805,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in NH 1.5 in NH PG ETCH"}]
[null,null,"21264046","SHUTOFF 2.5NH X 1.5NH FLFR E46",{"$f":"_xlfn.XLOOKUP(C806,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in NH 1.5 in NH PG ETCH"}]
[null,null,"21264047","SHUTOFF 2.5NH X 1.5NH FLFR SQ53",{"$f":"_xlfn.XLOOKUP(C807,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in NH 1.5 in NH PG ETCH"}]
[null,null,"21264048","SHUTOFF 2.5NH X 1.5NH CREEDMOOR FD",{"$f":"_xlfn.XLOOKUP(C808,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in NH 1.5 in NH PG ETCH"}]
[null,null,"21264050","SHUTOFF 2.5NH X 1.5NH ENG80INE",{"$f":"_xlfn.XLOOKUP(C809,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in NH 1.5 in NH PG ETCH"}]
[null,null,"21264001","SHUTOFF 2.5NH  X 1.5NH#",{"$f":"_xlfn.XLOOKUP(C810,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in NH 1.5 in NH PG"}]
[null,null,"21264051","SHUTOFF 2.5ATV  X 1.5NH",{"$f":"_xlfn.XLOOKUP(C811,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in NH 1.5 in NH PG"}]
[null,null,"21267005","SHUTOFF NPG 2.5NH X 1.5NH ENG80INE",{"$f":"_xlfn.XLOOKUP(C812,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in NH 1.5 in NH NPG ETCH"}]
[null,null,"21267008","SHUTOFF NPG 2.5NH  X 1.5NH GASTONIA FD",{"$f":"_xlfn.XLOOKUP(C813,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in NH 1.5 in NH NPG ETCH"}]
[null,null,"21267012","SHUTOFF NPG 2.5NH  X 1.5NH SUMMERFIELD",{"$f":"_xlfn.XLOOKUP(C814,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in NH 1.5 in NH NPG ETCH"}]
[null,null,"21267025","SHUTOFF NPG 2.5NH  X 1.5NH BDVFD",{"$f":"_xlfn.XLOOKUP(C815,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in NH 1.5 in NH NPG ETCH"}]
[null,null,"21267002","SHUTOFF NPG 2.5NH  X 1.5NH#",{"$f":"_xlfn.XLOOKUP(C816,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in NH 1.5 in NH NPG"}]
[null,null,"21267003","SHUTOFF NPG 2.5NH  X 1.5NH MTLHDL",{"$f":"_xlfn.XLOOKUP(C817,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in NH 1.5 in NH NPG"}]
[null,null,"21267035","SHUTOFF NPG 2.5NH X 1.5NH CHARLOTTE FD",{"$f":"_xlfn.XLOOKUP(C818,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in NH 1.5 in NH NPG"}]
[null,null,"21264002","SHUTOFF 2.5JIM X 1.5NH",{"$f":"_xlfn.XLOOKUP(C819,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in JIM 1.5 in NH PG"}]
[null,null,"21264021","SHUTOFF 2.5AFB X 1.5ABU FDNY",{"$f":"_xlfn.XLOOKUP(C820,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in FDNY 1.5 in FDNY NPG"}]
[null,null,"21267021","SHUTOFF NPG 2.5AFB X 1.5ABU FDNY",{"$f":"_xlfn.XLOOKUP(C821,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in FDNY 1.5 in FDNY NPG"}]
[null,null,"21264003","SHUTOFF 2.5AII X 1.5NPSH",{"$f":"_xlfn.XLOOKUP(C822,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in CSA 1.5 in NPSH PG"}]
[null,null,"21264004","SHUTOFF 2.5BIM X 1.5BSP",{"$f":"_xlfn.XLOOKUP(C823,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in BIM 1.5 in BSP PG"}]
[null,null,"21264007","SHUTOFF 2.5BAF X 1.5NPSH",{"$f":"_xlfn.XLOOKUP(C824,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in BAT 1.5 in NPSH PG"}]
[null,null,"21267001","SHUTOFF NPG 2.5BAF X 1.5NPSH",{"$f":"_xlfn.XLOOKUP(C825,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in BAT 1.5 in NPSH NPG"}]
[null,null,"21264052","SHUTOFF 2.5AKE X 1.5NH",{"$f":"_xlfn.XLOOKUP(C826,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in AKE 1.5 in NH PG"}]
[null,null,"21264034","SHUTOFF 2.5AKB X 1.5NPSH",{"$f":"_xlfn.XLOOKUP(C827,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in AKB 1.5 in NH PG"}]
[null,null,"21264039","SHUTOFF 2.5AKB X 1.5NH",{"$f":"_xlfn.XLOOKUP(C828,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in AKB 1.5 in NH PG"}]
[null,null,"21264038","SHUTOFF 2.5AJZ  X 1.5NH",{"$f":"_xlfn.XLOOKUP(C829,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in AJZ 1.5 in NH PG"}]
[null,null,"21264049","SHUTOFF 2.5AJS X 1.5NH SEQ ETCH",{"$f":"_xlfn.XLOOKUP(C830,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in AJS 1.5 in NH PG ETCH"}]
[null,null,"21264028","SHUTOFF 2.5AIP X 1.5NH",{"$f":"_xlfn.XLOOKUP(C831,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in AIP 1.5 in NH PG"}]
[null,null,"21267011","SHUTOFF NPG 2.5AIK X 1.5NH",{"$f":"_xlfn.XLOOKUP(C832,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in AIK 1.5 in NH NPG"}]
[null,null,"21264017","SHUTOFF 2.5AHB  X 1.5NH",{"$f":"_xlfn.XLOOKUP(C833,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in AHB 1.5 in NH PG"}]
[null,null,"21264013","SHUTOFF 2.5AGZ  X 1.5NH",{"$f":"_xlfn.XLOOKUP(C834,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in AGZ 1.5 in NH PG"}]
[null,null,"21267013","SHUTOFF NPG 2.5AGZ  X 1.5NH",{"$f":"_xlfn.XLOOKUP(C835,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in AGZ 1.5 in NH NPG"}]
[null,null,"21264016","SHUTOFF 2.5AGW  X 1.5ABT",{"$f":"_xlfn.XLOOKUP(C836,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in AGW 1.5 in PCT PG"}]
[null,null,"21264042","SHUTOFF 2.5AGW  X 1.5NH",{"$f":"_xlfn.XLOOKUP(C837,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in AGW 1.5 in NH PG"}]
[null,null,"21267004","SHUTOFF NPG 2.5AFO  X 1.5NH",{"$f":"_xlfn.XLOOKUP(C838,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in AFO 1.5 in NH NPG"}]
[null,null,"21264059","SHUTOFF 2.5ADU  X 1.5NH",{"$f":"_xlfn.XLOOKUP(C839,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in ADU 1.5 in NH PG"}]
[null,null,"21264019","SHUTOFF 2.5ADF  X 1.5NH",{"$f":"_xlfn.XLOOKUP(C840,DataSource!A:A,DataSource!AH:AH)","v":"2126 2.5 in ADF 1.5 in NH PG"}]
[null,null,"21024003","SHUTOFF 1.0NPSH X 1.0NPSH",{"$f":"_xlfn.XLOOKUP(C841,DataSource!A:A,DataSource!AH:AH)","v":"2102 1 in NPSH 1 in NPSH PG"}]
[null,null,"21027003","SHUTOFF NPG 1.0NPSH X 1.0NPSH",{"$f":"_xlfn.XLOOKUP(C842,DataSource!A:A,DataSource!AH:AH)","v":"2102 1 in NPSH 1 in NPSH NPG"}]
[null,null,"21024002","SHUTOFF 1.0NPSH X 1.0NH",{"$f":"_xlfn.XLOOKUP(C843,DataSource!A:A,DataSource!AH:AH)","v":"2102 1 in NPSH 1 in NH PG"}]
[null,null,"21024001","SHUTOFF 1.0NH X 1.0NH",{"$f":"_xlfn.XLOOKUP(C844,DataSource!A:A,DataSource!AH:AH)","v":"2102 1 in NH 1 in NH PG"}]
[null,null,"21027004","SHUTOFF NPG 1.0NH X 1.0NH",{"$f":"_xlfn.XLOOKUP(C845,DataSource!A:A,DataSource!AH:AH)","v":"2102 1 in NH 1 in NH NPG"}]
[null,null,"18204017","ULTRAJET 2.5AFD 3/4 TIP",{"$f":"_xlfn.XLOOKUP(C846,DataSource!A:A,DataSource!AH:AH)","v":"1820 2.5 in QST 118 3/4\" bore size(s) 50 BLACK (Std) PG"}]
[null,null,"18204016","ULTRAJET ZT 2.5NH 1 TIP",{"$f":"_xlfn.XLOOKUP(C847,DataSource!A:A,DataSource!AH:AH)","v":"1820 2.5 in NH 210 1\" bore size(s) 50 BLACK (Std) PG ZT"}]
[null,null,"18204009","ULTRAJET 2.5NH 1 TIP",{"$f":"_xlfn.XLOOKUP(C848,DataSource!A:A,DataSource!AH:AH)","v":"1820 2.5 in NH 210 1\" bore size(s) 50 Black (Std) PG"}]
[null,null,"18204008","ULTRAJET 2.5NH 15/16 TIP",{"$f":"_xlfn.XLOOKUP(C849,DataSource!A:A,DataSource!AH:AH)","v":"1820 2.5 in NH 185 15/16\" bore size(s) 50 BLACK (Std) PG"}]
[null,null,"18204032","ULTRAJET 2.5NH 7/8 TIP",{"$f":"_xlfn.XLOOKUP(C850,DataSource!A:A,DataSource!AH:AH)","v":"1820 2.5 in NH 161 7/8\" bore size(s) 50 BLACK (Std) PG"}]
[null,null,"18204012","ULTRAJET 65MM JIM 1 TIP",{"$f":"_xlfn.XLOOKUP(C851,DataSource!A:A,DataSource!AH:AH)","v":"1820 2.5 in JIM 210 1\" bore size(s) 50 BLACK (Std) PG"}]
[null,null,"18204018","ULTRAJET 2.5AII 15/16 TIP",{"$f":"_xlfn.XLOOKUP(C852,DataSource!A:A,DataSource!AH:AH)","v":"1820 2.5 in CSA 185 15/16\" bore size(s) 50 Black (Std) PG"}]
[null,null,"18204029","ULTRAJET 2.5AII 7/8 TIP",{"$f":"_xlfn.XLOOKUP(C853,DataSource!A:A,DataSource!AH:AH)","v":"1820 2.5 in CSA 161 7/8\" bore size(s) 50 BLACK (Std) PG"}]
[null,null,"18204023","ULTRAJET 2.5AII 3/4 TIP",{"$f":"_xlfn.XLOOKUP(C854,DataSource!A:A,DataSource!AH:AH)","v":"1820 2.5 in CSA 118 3/4\" bore size(s) 50 BLACK (Std) PG"}]
[null,null,"18204014","ULTRAJET 2.5BIM 7/8 TIP",{"$f":"_xlfn.XLOOKUP(C855,DataSource!A:A,DataSource!AH:AH)","v":"1820 2.5 in BIM 161 7/8\" bore size(s) 50 BLACK (Std) PG"}]
[null,null,"18204010","ULTRAJET 2.5BIM 3/4 TIP EN",{"$f":"_xlfn.XLOOKUP(C856,DataSource!A:A,DataSource!AH:AH)","v":"1820 2.5 in BIM 118 3/4\" bore size(s) 50 BLACK (Std) PG"}]
[null,null,"18204028","ULTRAJET 2.5BAF  1 TIP",{"$f":"_xlfn.XLOOKUP(C857,DataSource!A:A,DataSource!AH:AH)","v":"1820 2.5 in BAT 210 1\" bore size(s) 50 BLACK (Std) PG"}]
[null,null,"18204020","ULTRAJET 2.5AKB 1 TIP",{"$f":"_xlfn.XLOOKUP(C858,DataSource!A:A,DataSource!AH:AH)","v":"1820 2.5 in AKB 210 1\" bore size(s) 50 Black (Std) PG"}]
[null,null,"18204026","ULTRAJET 2.5AKB 7/8 TIP",{"$f":"_xlfn.XLOOKUP(C859,DataSource!A:A,DataSource!AH:AH)","v":"1820 2.5 in AKB 161 7/8\" bore size(s) 50 Black (Std) PG"}]
[null,null,"18204027","ULTRAJET 52MM STZ 1\" TIP",{"$f":"_xlfn.XLOOKUP(C860,DataSource!A:A,DataSource!AH:AH)","v":"1820 2 in STORZ 210 1\" bore size(s) 50 BLACK (Std) PG"}]
[null,null,"18204025","ULTRAJET 38MM STZ 1\" TIP",{"$f":"_xlfn.XLOOKUP(C861,DataSource!A:A,DataSource!AH:AH)","v":"1820 1.5 in STORZ 210 1\" bore size(s) 50 BLACK (Std) PG"}]
[null,null,"18204011","ULTRAJET 38MM STZ 7/8 TIP",{"$f":"_xlfn.XLOOKUP(C862,DataSource!A:A,DataSource!AH:AH)","v":"1820 1.5 in STORZ 161 7/8\" bore size(s) 50 BLACK (Std) PG"}]
[null,null,"18204022","ULTRAJET 38MM 3/4 TIP EN",{"$f":"_xlfn.XLOOKUP(C863,DataSource!A:A,DataSource!AH:AH)","v":"1820 1.5 in STORZ 118 3/4\" bore size(s) 50 BLACK (Std) PG"}]
[null,null,"18204021","ULTRAJET 1.5NPSH 1 TIP",{"$f":"_xlfn.XLOOKUP(C864,DataSource!A:A,DataSource!AH:AH)","v":"1820 1.5 in NPSH 210 1\" bore size(s) 50 Black (Std) PG"}]
[null,null,"18204007","ULTRAJET 1.5NPSH 15/16 TIP",{"$f":"_xlfn.XLOOKUP(C865,DataSource!A:A,DataSource!AH:AH)","v":"1820 1.5 in NPSH 185 15/16\" bore size(s) 50 Black (Std) PG"}]
[null,null,"18204006","ULTRAJET 1.5NPSH 7/8 TIP",{"$f":"_xlfn.XLOOKUP(C866,DataSource!A:A,DataSource!AH:AH)","v":"1820 1.5 in NPSH 161 7/8\" bore size(s) 50 Black (Std) PG"}]
[null,null,"18204005","ULTRAJET 1.5NPSH 3/4 TIP",{"$f":"_xlfn.XLOOKUP(C867,DataSource!A:A,DataSource!AH:AH)","v":"1820 1.5 in NPSH 118 3/4\" bore size(s) 50 Black (Std) PG"}]
[null,null,"18204004","ULTRAJET 1.5NH 1 TIP",{"$f":"_xlfn.XLOOKUP(C868,DataSource!A:A,DataSource!AH:AH)","v":"1820 1.5 in NH 210 1\" bore size(s) 50 Black (Std) PG"}]
[null,null,"18204003","ULTRAJET 1.5NH 15/16 TIP#",{"$f":"_xlfn.XLOOKUP(C869,DataSource!A:A,DataSource!AH:AH)","v":"1820 1.5 in NH 185 15/16\" bore size(s) 50 Black (Std) PG"}]
[null,null,"18204002","ULTRAJET 1.5NH 7/8 TIP",{"$f":"_xlfn.XLOOKUP(C870,DataSource!A:A,DataSource!AH:AH)","v":"1820 1.5 in NH 161 7/8\" bore size(s) 50 Black (Std) PG"}]
[null,null,"18204015","ULTRAJET ZT 1.5NH 3/4 TIP",{"$f":"_xlfn.XLOOKUP(C871,DataSource!A:A,DataSource!AH:AH)","v":"1820 1.5 in NH 118 3/4\" bore size(s) 50 BLACK (Std) PG ZT"}]
[null,null,"18204001","ULTRAJET 1.5NH 3/4 TIP",{"$f":"_xlfn.XLOOKUP(C872,DataSource!A:A,DataSource!AH:AH)","v":"1820 1.5 in NH 118 3/4\" bore size(s) 50 Black (Std) PG"}]
[null,null,"18204024","ULTRAJET 1.5BSP 1 TIP",{"$f":"_xlfn.XLOOKUP(C873,DataSource!A:A,DataSource!AH:AH)","v":"1820 1.5 in BSP 210 1\" bore size(s) 50 BLACK (Std) PG"}]
[null,null,"18204013","ULTRAJET 1.5BIM 3/4 TIP EN",{"$f":"_xlfn.XLOOKUP(C874,DataSource!A:A,DataSource!AH:AH)","v":"1820 1.5 in BIM 118 3/4\" bore size(s) 50 BLACK (Std) PG"}]
[null,null,"17724006","TBJT 1\"NH 13-60G@100P 180 DEG FOG",{"$f":"_xlfn.XLOOKUP(C875,DataSource!A:A,DataSource!AH:AH)","v":"1772 1 in NH 13-60 100 (Std) BLACK (Std) PG"}]
[null,null,"17664005","TBJT TIP 1.5NPSH 30-200G@75P",{"$f":"_xlfn.XLOOKUP(C876,DataSource!A:A,DataSource!AH:AH)","v":"1766 1.5 in NPSH 30-200 75 BLACK (Std)"}]
[null,null,"17664007","TBJT TIP 1.5NPSH 30-200G@100P",{"$f":"_xlfn.XLOOKUP(C877,DataSource!A:A,DataSource!AH:AH)","v":"1766 1.5 in NPSH 30-200 100 (Std) BLACK (Std)"}]
[null,null,"17664014","TBJT TIP 1.5NH 30-200G@75P ORGBMPR",{"$f":"_xlfn.XLOOKUP(C878,DataSource!A:A,DataSource!AH:AH)","v":"1766 1.5 in NH 30-200 75 ORANGE"}]
[null,null,"17664006","TBJT TIP 1.5NH 30-200G@75P UNIONVILLE",{"$f":"_xlfn.XLOOKUP(C879,DataSource!A:A,DataSource!AH:AH)","v":"1766 1.5 in NH 30-200 75 BLACK (Std) ETCH"}]
[null,null,"17664002","TBJT TIP 1.5NH 30-200G@75P",{"$f":"_xlfn.XLOOKUP(C880,DataSource!A:A,DataSource!AH:AH)","v":"1766 1.5 in NH 30-200 75 BLACK (Std)"}]
[null,null,"17664010","TBJT TIP 1.5NH 30-200G@100P YEL BMPR",{"$f":"_xlfn.XLOOKUP(C881,DataSource!A:A,DataSource!AH:AH)","v":"1766 1.5 in NH 30-200 100 (Std) YELLOW"}]
[null,null,"17664009","TBJT TIP 1.5NH 30-200G@100P RED BMPR",{"$f":"_xlfn.XLOOKUP(C882,DataSource!A:A,DataSource!AH:AH)","v":"1766 1.5 in NH 30-200 100 (Std) RED"}]
[null,null,"17664013","TBJT TIP 1.5NH 30-200G@100P ORG  BMPR",{"$f":"_xlfn.XLOOKUP(C883,DataSource!A:A,DataSource!AH:AH)","v":"1766 1.5 in NH 30-200 100 (Std) ORANGE"}]
[null,null,"17664011","TBJT TIP 1.5NH 30-200G@100P GRN BMPR",{"$f":"_xlfn.XLOOKUP(C884,DataSource!A:A,DataSource!AH:AH)","v":"1766 1.5 in NH 30-200 100 (Std) GREEN"}]
[null,null,"17664012","TBJT TIP 1.5NH 30-200G@100P BLU BMPR",{"$f":"_xlfn.XLOOKUP(C885,DataSource!A:A,DataSource!AH:AH)","v":"1766 1.5 in NH 30-200 100 (Std) BLUE"}]
[null,null,"17664001","TBJT TIP 1.5NH 30-200G@100P",{"$f":"_xlfn.XLOOKUP(C886,DataSource!A:A,DataSource!AH:AH)","v":"1766 1.5 in NH 30-200 100 (Std) BLACK (Std)"}]
[null,null,"17664008","TBJT TIP 1.5NH 30-200G@100P MTLTTH",{"$f":"_xlfn.XLOOKUP(C887,DataSource!A:A,DataSource!AH:AH)","v":"1766 1.5 in NH 30-200 100 (Std) BLACK (Std)"}]
[null,null,"17664003","TBJT TIP 1.5BSP 115-750L@7b",{"$f":"_xlfn.XLOOKUP(C888,DataSource!A:A,DataSource!AH:AH)","v":"1766 1.5 in BSP 115-750 7 BLACK (Std)"}]
[null,null,"17634029","TBJT 75MM 30-200G@100P FM",{"$f":"_xlfn.XLOOKUP(C889,DataSource!A:A,DataSource!AH:AH)","v":"1763 3 in STORZ 30-200 100 (Std) BLACK (Std) PG"}]
[null,null,"17634013","TBJT 75MM 115-750L@7b FM",{"$f":"_xlfn.XLOOKUP(C890,DataSource!A:A,DataSource!AH:AH)","v":"1763 3 in STORZ 115-750 7 BLACK (Std) PG"}]
[null,null,"17634038","TBJT 2.5NH 30-200G@75P",{"$f":"_xlfn.XLOOKUP(C891,DataSource!A:A,DataSource!AH:AH)","v":"1763 2.5 in NH 30-200 75 BLACK (Std) PG"}]
[null,null,"17634016","TBJT 2.5NH 30-200G@100P FM",{"$f":"_xlfn.XLOOKUP(C892,DataSource!A:A,DataSource!AH:AH)","v":"1763 2.5 in NH 30-200 100 (Std) BLACK (Std) PG"}]
[null,null,"17634026","TBJT ZT 2.5BIM 115-750L@7b",{"$f":"_xlfn.XLOOKUP(C893,DataSource!A:A,DataSource!AH:AH)","v":"1763 2.5 in BIM 115-750 7 BLACK (Std) PG ZT"}]
[null,null,"17634002","TBJT 2.5BIM 115-750L@7b FM",{"$f":"_xlfn.XLOOKUP(C894,DataSource!A:A,DataSource!AH:AH)","v":"1763 2.5 in BIM 115-750 7 BLACK (Std) PG"}]
[null,null,"17634005","TBJT 52MM 30-200G@100P FM",{"$f":"_xlfn.XLOOKUP(C895,DataSource!A:A,DataSource!AH:AH)","v":"1763 2 in STORZ 30-200 100 (Std) BLACK (Std) PG"}]
[null,null,"17634004","TBJT 52MM 115-750L@7b FM",{"$f":"_xlfn.XLOOKUP(C896,DataSource!A:A,DataSource!AH:AH)","v":"1763 2 in STORZ 115-750 7 BLACK (Std) PG"}]
[null,null,"17634036","TBJT 38MM 30-200G@75P",{"$f":"_xlfn.XLOOKUP(C897,DataSource!A:A,DataSource!AH:AH)","v":"1763 1.5 in STORZ 30-200 75 BLACK (Std) PG"}]
[null,null,"17634015","TBJT 1.5NPSH 30-200G@75P",{"$f":"_xlfn.XLOOKUP(C898,DataSource!A:A,DataSource!AH:AH)","v":"1763 1.5 in NPSH 30-200 75 BLACK (Std) PG"}]
[null,null,"17637015","TBJT NPG 1.5NPSH 30-200G@75P",{"$f":"_xlfn.XLOOKUP(C899,DataSource!A:A,DataSource!AH:AH)","v":"1763 1.5 in NPSH 30-200 75 BLACK (Std) NPG"}]
[null,null,"17634034","TBJT ZT 1.5NPSH 30-200G@100P",{"$f":"_xlfn.XLOOKUP(C900,DataSource!A:A,DataSource!AH:AH)","v":"1763 1.5 in NPSH 30-200 100 (Std) BLACK (Std) PG ZT"}]
[null,null,"17634020","TBJT 1.5NPSH 30-200G@100P FM",{"$f":"_xlfn.XLOOKUP(C901,DataSource!A:A,DataSource!AH:AH)","v":"1763 1.5 in NPSH 30-200 100 (Std) BLACK (Std) PG"}]
[null,null,"17637020","TBJT NPG 1.5NPSH 30-200G@100P FM",{"$f":"_xlfn.XLOOKUP(C902,DataSource!A:A,DataSource!AH:AH)","v":"1763 1.5 in NPSH 30-200 100 (Std) BLACK (Std) NPG"}]
[null,null,"17634023","TBJT 1.5 NPSH 115-750L@7b FM",{"$f":"_xlfn.XLOOKUP(C903,DataSource!A:A,DataSource!AH:AH)","v":"1763 1.5 in NPSH 115-750 7 BLACK (Std) PG"}]
[null,null,"17634019","TBJT ZT 1.5NPSH 115-750L@5b",{"$f":"_xlfn.XLOOKUP(C904,DataSource!A:A,DataSource!AH:AH)","v":"1763 1.5 in NPSH 115-750 5 BLACK (Std) PG ZT"}]
[null,null,"17634018","TBJT 1.5NPSH 115-750L@5b/500K",{"$f":"_xlfn.XLOOKUP(C905,DataSource!A:A,DataSource!AH:AH)","v":"1763 1.5 in NPSH 115-750 5 BLACK (Std) PG"}]
[null,null,"17634025","TBJT 1.5NH 30-200G@75P REDBMPR SHERBORN",{"$f":"_xlfn.XLOOKUP(C906,DataSource!A:A,DataSource!AH:AH)","v":"1763 1.5 in NH 30-200 75 RED PG ETCH"}]
[null,null,"17634021","TBJT 1.5NH 30-200G@75P REDBMPR",{"$f":"_xlfn.XLOOKUP(C907,DataSource!A:A,DataSource!AH:AH)","v":"1763 1.5 in NH 30-200 75 RED PG"}]
[null,null,"17634040","TBJT 1.5NH 30-200G@75P ORGBMPR",{"$f":"_xlfn.XLOOKUP(C908,DataSource!A:A,DataSource!AH:AH)","v":"1763 1.5 in NH 30-200 75 ORANGE PG"}]
[null,null,"17634041","TBJT 1.5NH 30-200G@75P GRNBMPR",{"$f":"_xlfn.XLOOKUP(C909,DataSource!A:A,DataSource!AH:AH)","v":"1763 1.5 in NH 30-200 75 GREEN PG"}]
[null,null,"17634039","TBJT 1.5NH 30-200G@75P BLUEBMPR",{"$f":"_xlfn.XLOOKUP(C910,DataSource!A:A,DataSource!AH:AH)","v":"1763 1.5 in NH 30-200 75 BLUE PG"}]
[null,null,"17634027","TBJT ZT 1.5NH 30-200G@75P",{"$f":"_xlfn.XLOOKUP(C911,DataSource!A:A,DataSource!AH:AH)","v":"1763 1.5 in NH 30-200 75 BLACK (Std) PG ZT"}]
[null,null,"17634003","TBJT 1.5NH 30-200G@75P#",{"$f":"_xlfn.XLOOKUP(C912,DataSource!A:A,DataSource!AH:AH)","v":"1763 1.5 in NH 30-200 75 BLACK (Std) PG"}]
[null,null,"17637003","TBJT NPG 1.5NH 30-200G@75P",{"$f":"_xlfn.XLOOKUP(C913,DataSource!A:A,DataSource!AH:AH)","v":"1763 1.5 in NH 30-200 75 BLACK (Std) NPG"}]
[null,null,"17634022","TBJT 1.5NH 30-200G@100P YLWBMPR FM",{"$f":"_xlfn.XLOOKUP(C914,DataSource!A:A,DataSource!AH:AH)","v":"1763 1.5 in NH 30-200 100 (Std) YELLOW PG"}]
[null,null,"17637022","TBJT NPG 1.5NH 30-200G@100P YLWBMPR FM",{"$f":"_xlfn.XLOOKUP(C915,DataSource!A:A,DataSource!AH:AH)","v":"1763 1.5 in NH 30-200 100 (Std) YELLOW NPG"}]
[null,null,"17634011","TBJT 1.5NH 30-200G@100P REDBMPR FM",{"$f":"_xlfn.XLOOKUP(C916,DataSource!A:A,DataSource!AH:AH)","v":"1763 1.5 in NH 30-200 100 (Std) RED PG"}]
[null,null,"17637011","TBJT NPG 1.5NH 30-200G@100P REDBMPR FM",{"$f":"_xlfn.XLOOKUP(C917,DataSource!A:A,DataSource!AH:AH)","v":"1763 1.5 in NH 30-200 100 (Std) RED NPG"}]
[null,null,"17634032","TBJT 1.5NH 30-200G@100P ORGBMPR FM",{"$f":"_xlfn.XLOOKUP(C918,DataSource!A:A,DataSource!AH:AH)","v":"1763 1.5 in NH 30-200 100 (Std) ORANGE PG"}]
[null,null,"17634030","TBJT 1.5NH 30-200G@100P GRNBMPR FM",{"$f":"_xlfn.XLOOKUP(C919,DataSource!A:A,DataSource!AH:AH)","v":"1763 1.5 in NH 30-200 100 (Std) GREEN PG"}]
[null,null,"17637030","TBJT NPG 1.5NH 30-200G@100P GRNBMPR FM",{"$f":"_xlfn.XLOOKUP(C920,DataSource!A:A,DataSource!AH:AH)","v":"1763 1.5 in NH 30-200 100 (Std) GREEN NPG"}]
[null,null,"17634031","TBJT 1.5NH 30-200G@100P BLUEBMPR FM",{"$f":"_xlfn.XLOOKUP(C921,DataSource!A:A,DataSource!AH:AH)","v":"1763 1.5 in NH 30-200 100 (Std) BLUE PG"}]
[null,null,"17637031","TBJT NPG 1.5NH 30-200G@100P BLUEBMPR FM",{"$f":"_xlfn.XLOOKUP(C922,DataSource!A:A,DataSource!AH:AH)","v":"1763 1.5 in NH 30-200 100 (Std) BLUE NPG"}]
[null,null,"17634024","TBJT ZT 1.5NH 30-200G@100P",{"$f":"_xlfn.XLOOKUP(C923,DataSource!A:A,DataSource!AH:AH)","v":"1763 1.5 in NH 30-200 100 (Std) BLACK (Std) PG ZT"}]
[null,null,"17634001","TBJT 1.5NH 30-200G@100P FM#",{"$f":"_xlfn.XLOOKUP(C924,DataSource!A:A,DataSource!AH:AH)","v":"1763 1.5 in NH 30-200 100 (Std) BLACK (Std) PG"}]
[null,null,"17637001","TBJT NPG 1.5NH 30-200G@100P FM",{"$f":"_xlfn.XLOOKUP(C925,DataSource!A:A,DataSource!AH:AH)","v":"1763 1.5 in NH 30-200 100 (Std) BLACK (Std) NPG"}]
[null,null,"17634028","TBJT 1.5NH 115-750L@7b FM",{"$f":"_xlfn.XLOOKUP(C926,DataSource!A:A,DataSource!AH:AH)","v":"1763 1.5 in NH 115-750 7 BLACK (Std) PG"}]
[null,null,"17634014","TBJT 1.5 BSP 115-750L@7b FM",{"$f":"_xlfn.XLOOKUP(C927,DataSource!A:A,DataSource!AH:AH)","v":"1763 1.5 in BSP 115-750 7 BLACK (Std) PG"}]
[null,null,"17634033","TBJT 1.5ABP 30-200G@100P FM",{"$f":"_xlfn.XLOOKUP(C928,DataSource!A:A,DataSource!AH:AH)","v":"1763 1.5 in ABP 30-200 100 (Std) BLACK (Std) PG"}]
[null,null,"17444004","TBJT TIP 1.5NPSH 475-950L@5b",{"$f":"_xlfn.XLOOKUP(C929,DataSource!A:A,DataSource!AH:AH)","v":"1744 1.5 in NPSH 475-900 5 BLACK (Std)"}]
[null,null,"17444008","TBJT TIP 1.5NPSH 125-250G@75P",{"$f":"_xlfn.XLOOKUP(C930,DataSource!A:A,DataSource!AH:AH)","v":"1744 1.5 in NPSH 125-250 75 BLACK (Std)"}]
[null,null,"17444007","TBJT TIP 1.5NPSH 125-250G@100P",{"$f":"_xlfn.XLOOKUP(C931,DataSource!A:A,DataSource!AH:AH)","v":"1744 1.5 in NPSH 125-250 100 (Std) BLACK (Std)"}]
[null,null,"17444005","TBJT TIP 1.5NH 475-950L@7b",{"$f":"_xlfn.XLOOKUP(C932,DataSource!A:A,DataSource!AH:AH)","v":"1744 1.5 in NH 475-950 7 BLACK (Std)"}]
[null,null,"17444006","TBJT TIP 1.5NH 125-250G@75P",{"$f":"_xlfn.XLOOKUP(C933,DataSource!A:A,DataSource!AH:AH)","v":"1744 1.5 in NH 125-250 75 BLACK (Std)"}]
[null,null,"17444010","TBJT TIP 1.5NH 125-250G@100P YEL BMPR",{"$f":"_xlfn.XLOOKUP(C934,DataSource!A:A,DataSource!AH:AH)","v":"1744 1.5 in NH 125-250 100 (Std) YELLOW"}]
[null,null,"17444002","TBJT TIP 1.5NH 125-250G@100P REDBMPR",{"$f":"_xlfn.XLOOKUP(C935,DataSource!A:A,DataSource!AH:AH)","v":"1744 1.5 in NH 125-250 100 (Std) RED"}]
[null,null,"17444009","TBJTTIP 1.5NH 125-250G@100P SACO FD LOGO",{"$f":"_xlfn.XLOOKUP(C936,DataSource!A:A,DataSource!AH:AH)","v":"1744 1.5 in NH 125-250 100 (Std) BLACK (Std) ETCH"}]
[null,null,"17444001","TBJT TIP 1.5NH 125-250G@100P#",{"$f":"_xlfn.XLOOKUP(C937,DataSource!A:A,DataSource!AH:AH)","v":"1744 1.5 in NH 125-250 100 (Std) BLACK (Std)"}]
[null,null,"17444003","TBJT TIP 1.5BSP 475-950L@7b",{"$f":"_xlfn.XLOOKUP(C938,DataSource!A:A,DataSource!AH:AH)","v":"1744 1.5 in BSP 475-950 7 BLACK (Std)"}]
[null,null,"17374004","TBJT TIP 1.5NPSH 95-200G@100P",{"$f":"_xlfn.XLOOKUP(C939,DataSource!A:A,DataSource!AH:AH)","v":"1737 1.5 in NPSH 95-200 100 (Std) BLACK (Std)"}]
[null,null,"17374003","TBJT TIP 1.5NPSH 360-750L@5b/500K",{"$f":"_xlfn.XLOOKUP(C940,DataSource!A:A,DataSource!AH:AH)","v":"1737 1.5 in NPSH 360-750 5 BLACK (Std)"}]
[null,null,"17374005","TBJT TIP 1.5NH 95-200G@75P REDBMPR",{"$f":"_xlfn.XLOOKUP(C941,DataSource!A:A,DataSource!AH:AH)","v":"1737 1.5 in NH 95-200 75 RED"}]
[null,null,"17374006","TBJT TIP 1.5NH 95-200G@75P ORG BMPR",{"$f":"_xlfn.XLOOKUP(C942,DataSource!A:A,DataSource!AH:AH)","v":"1737 1.5 in NH 95-200 75 ORANGE"}]
[null,null,"17374001","TBJT TIP 1.5NH 95-200G@75P",{"$f":"_xlfn.XLOOKUP(C943,DataSource!A:A,DataSource!AH:AH)","v":"1737 1.5 in NH 95-200 75 BLACK (Std)"}]
[null,null,"17374032","TBJT TIP 1.5NH 95-200G@100P REDBMPR",{"$f":"_xlfn.XLOOKUP(C944,DataSource!A:A,DataSource!AH:AH)","v":"1737 1.5 in NH 95-200 100 (Std) RED"}]
[null,null,"17374002","TBJT TIP 1.5NH 95-200G@100P",{"$f":"_xlfn.XLOOKUP(C945,DataSource!A:A,DataSource!AH:AH)","v":"1737 1.5 in NH 95-200 100 (Std) BLACK (Std)"}]
[null,null,"17334005","TBJT 75MM 475-950L@7b FM",{"$f":"_xlfn.XLOOKUP(C946,DataSource!A:A,DataSource!AH:AH)","v":"1733 3 in STORZ 475-950 7 BLACK (Std) PG"}]
[null,null,"17334004","TBJT 75MM 125-250G@100P FM",{"$f":"_xlfn.XLOOKUP(C947,DataSource!A:A,DataSource!AH:AH)","v":"1733 3 in STORZ 125-250 100 (Std) BLACK (Std) PG"}]
[null,null,"17337008","TBJT NPG 65MM 475-950L@7b FM",{"$f":"_xlfn.XLOOKUP(C948,DataSource!A:A,DataSource!AH:AH)","v":"1733 2.5 in STORZ 475-950 7 BLACK (Std) NPG"}]
[null,null,"17337002","TBJT NPG 65MM 125-250G@100P FM",{"$f":"_xlfn.XLOOKUP(C949,DataSource!A:A,DataSource!AH:AH)","v":"1733 2.5 in STORZ 125-250 100 (Std) BLACK (Std) NPG"}]
[null,null,"17334032","TBJT 2.5AFD 125-250G@100P FM",{"$f":"_xlfn.XLOOKUP(C950,DataSource!A:A,DataSource!AH:AH)","v":"1733 2.5 in QST 125-250 100 (Std) BLACK (Std) PG"}]
[null,null,"17334019","TBJT 2.5AEF 125-250G@100P FM",{"$f":"_xlfn.XLOOKUP(C951,DataSource!A:A,DataSource!AH:AH)","v":"1733 2.5 in NYCORP 125-250 100 (Std) BLACK (Std) PG"}]
[null,null,"17334013","TBJT 2.5NH 125-250G@75P ORGBMPR",{"$f":"_xlfn.XLOOKUP(C952,DataSource!A:A,DataSource!AH:AH)","v":"1733 2.5 in NH 125-250 75 ORANGE PG"}]
[null,null,"17334020","TBJT ZT 2.5NH 125-250G@75P",{"$f":"_xlfn.XLOOKUP(C953,DataSource!A:A,DataSource!AH:AH)","v":"1733 2.5 in NH 125-250 75 BLACK (Std) PG ZT"}]
[null,null,"17334035","TBJT 2.5NH 125-250G@75P MT.PLEASANT",{"$f":"_xlfn.XLOOKUP(C954,DataSource!A:A,DataSource!AH:AH)","v":"1733 2.5 in NH 125-250 75 BLACK (Std) PG ETCH"}]
[null,null,"17334036","TBJT 2.5NH 125-250G@75P RED BANKS",{"$f":"_xlfn.XLOOKUP(C955,DataSource!A:A,DataSource!AH:AH)","v":"1733 2.5 in NH 125-250 75 BLACK (Std) PG ETCH"}]
[null,null,"17334037","TBJT 2.5NH 125-250G@75P VICTORIA",{"$f":"_xlfn.XLOOKUP(C956,DataSource!A:A,DataSource!AH:AH)","v":"1733 2.5 in NH 125-250 75 BLACK (Std) PG ETCH"}]
[null,null,"17334038","TBJT 2.5NH 125-250G@75P WATSON",{"$f":"_xlfn.XLOOKUP(C957,DataSource!A:A,DataSource!AH:AH)","v":"1733 2.5 in NH 125-250 75 BLACK (Std) PG ETCH"}]
[null,null,"17337011","TBJT NPG 2.5NH 125-250G@75P UNIONVILLE",{"$f":"_xlfn.XLOOKUP(C958,DataSource!A:A,DataSource!AH:AH)","v":"1733 2.5 in NH 125-250 75 BLACK (Std) NPG ETCH"}]
[null,null,"17337007","TBJT NPG 2.5NH 125-250G@75P",{"$f":"_xlfn.XLOOKUP(C959,DataSource!A:A,DataSource!AH:AH)","v":"1733 2.5 in NH 125-250 75 BLACK (Std) NPG"}]
[null,null,"17334017","TBJT 2.5NH 125-250G@100P ORGBMPR FM",{"$f":"_xlfn.XLOOKUP(C960,DataSource!A:A,DataSource!AH:AH)","v":"1733 2.5 in NH 125-250 100 (Std) ORANGE PG"}]
[null,null,"17334011","TBJT ZT 2.5NH 125-250G@100P",{"$f":"_xlfn.XLOOKUP(C961,DataSource!A:A,DataSource!AH:AH)","v":"1733 2.5 in NH 125-250 100 (Std) BLACK (Std) PG ZT"}]
[null,null,"17334026","TBJT 2.5NH 125-250G@100P MVFD",{"$f":"_xlfn.XLOOKUP(C962,DataSource!A:A,DataSource!AH:AH)","v":"1733 2.5 in NH 125-250 100 (Std) BLACK (Std) PG ETCH"}]
[null,null,"17334028","TBJT 2.5NH125-250G@100P SEQ ETCH APPLING",{"$f":"_xlfn.XLOOKUP(C963,DataSource!A:A,DataSource!AH:AH)","v":"1733 2.5 in NH 125-250 100 (Std) BLACK (Std) PG ETCH"}]
[null,null,"17334029","TBJT 2.5NH125-250G@100P SEQ ETCH STA 1-8",{"$f":"_xlfn.XLOOKUP(C964,DataSource!A:A,DataSource!AH:AH)","v":"1733 2.5 in NH 125-250 100 (Std) BLACK (Std) PG ETCH"}]
[null,null,"17334002","TBJT 2.5NH 125-250G@100P FM#",{"$f":"_xlfn.XLOOKUP(C965,DataSource!A:A,DataSource!AH:AH)","v":"1733 2.5 in NH 125-250 100 (Std) BLACK (Std) PG"}]
[null,null,"17334007","TBJT 2.5NH 125-250G@75P",{"$f":"_xlfn.XLOOKUP(C966,DataSource!A:A,DataSource!AH:AH)","v":"1733 2.5 in NH 125-250 100 (Std) BLACK (Std) PG"}]
[null,null,"17337012","TBJT NPG 2.5NH 125-250G@100P ETCH MVFD",{"$f":"_xlfn.XLOOKUP(C967,DataSource!A:A,DataSource!AH:AH)","v":"1733 2.5 in NH 125-250 100 (Std) BLACK (Std) NPG ETCH"}]
[null,null,"17337001","TBJT NPG 2.5NH 125-250G@100P FM",{"$f":"_xlfn.XLOOKUP(C968,DataSource!A:A,DataSource!AH:AH)","v":"1733 2.5 in NH 125-250 100 (Std) BLACK (Std) NPG"}]
[null,null,"17335000","TBJT PG 65MM JIM 125-250G@75P CCCF",{"$f":"_xlfn.XLOOKUP(C969,DataSource!A:A,DataSource!AH:AH)","v":"1733 2.5 in JIM 125-250 75 BLACK (Std) PG ETCH"}]
[null,null,"17334003","TBJT 65MM JIM 125-250G@100P FM",{"$f":"_xlfn.XLOOKUP(C970,DataSource!A:A,DataSource!AH:AH)","v":"1733 2.5 in JIM 125-250 100 (Std) BLACK (Std) PG"}]
[null,null,"17334016","TBJT 2.5AII 475-900L@7b/700K FM",{"$f":"_xlfn.XLOOKUP(C971,DataSource!A:A,DataSource!AH:AH)","v":"1733 2.5 in CSA 475-900 700 BLACK (Std) PG"}]
[null,null,"17334010","TBJT 2.5AII 125-250G@100P FM",{"$f":"_xlfn.XLOOKUP(C972,DataSource!A:A,DataSource!AH:AH)","v":"1733 2.5 in CSA 125-250 100 (Std) BLACK (Std) PG"}]
[null,null,"17334022","TBJT ZT 2.5BSP 475-950L@7b",{"$f":"_xlfn.XLOOKUP(C973,DataSource!A:A,DataSource!AH:AH)","v":"1733 2.5 in BSP 475-950 7 BLACK (Std) PG ZT"}]
[null,null,"17334021","TBJT 2.5BSP 475-950L@7b FM",{"$f":"_xlfn.XLOOKUP(C974,DataSource!A:A,DataSource!AH:AH)","v":"1733 2.5 in BSP 475-950 7 BLACK (Std) PG"}]
[null,null,"17334014","TBJT ZT 2.5BIM 475-950L@7b",{"$f":"_xlfn.XLOOKUP(C975,DataSource!A:A,DataSource!AH:AH)","v":"1733 2.5 in BIM 475-950 7 BLACK (Std) PG ZT"}]
[null,null,"17334006","TBJT 2.5BIM 475-950L@7b FM",{"$f":"_xlfn.XLOOKUP(C976,DataSource!A:A,DataSource!AH:AH)","v":"1733 2.5 in BIM 475-950 7 BLACK (Std) PG"}]
[null,null,"17334030","TBJT 2.5BAF 475-900L@7b/700K FM",{"$f":"_xlfn.XLOOKUP(C977,DataSource!A:A,DataSource!AH:AH)","v":"1733 2.5 in BAT 475-900 7 BLACK (Std) PG"}]
[null,null,"17334023","TBJT 2.5BAF 125-250G@75P",{"$f":"_xlfn.XLOOKUP(C978,DataSource!A:A,DataSource!AH:AH)","v":"1733 2.5 in BAT 125-250 75 BLACK (Std) PG"}]
[null,null,"17334027","TBJT ZT 2.5BAF 125-250G@100P",{"$f":"_xlfn.XLOOKUP(C979,DataSource!A:A,DataSource!AH:AH)","v":"1733 2.5 in BAT 125-250 100 (Std) BLACK (Std) PG ZT"}]
[null,null,"17334009","TBJT 2.5BAF 125-250G@100P FM",{"$f":"_xlfn.XLOOKUP(C980,DataSource!A:A,DataSource!AH:AH)","v":"1733 2.5 in BAT 125-250 100 (Std) BLACK (Std) PG"}]
[null,null,"17337009","TBJT NPG 2.5BAF 125-250G@100P FM",{"$f":"_xlfn.XLOOKUP(C981,DataSource!A:A,DataSource!AH:AH)","v":"1733 2.5 in BAT 125-250 100 (Std) BLACK (Std) NPG"}]
[null,null,"17334015","TBJT 2.5AKB 125-250G@100P FM",{"$f":"_xlfn.XLOOKUP(C982,DataSource!A:A,DataSource!AH:AH)","v":"1733 2.5 in AKB 125-250 100 (Std) BLACK (Std) PG"}]
[null,null,"17334031","TBJT 2.5AKA 125-250G@100P FM",{"$f":"_xlfn.XLOOKUP(C983,DataSource!A:A,DataSource!AH:AH)","v":"1733 2.5 in AKA 125-250 100 (Std) BLACK (Std) PG"}]
[null,null,"17334033","TBJT 2.5AHQ 125-250G@100P FM",{"$f":"_xlfn.XLOOKUP(C984,DataSource!A:A,DataSource!AH:AH)","v":"1733 2.5 in AHQ 125-250 100 (Std) BLACK (Std) PG"}]
[null,null,"17334018","TBJT 2.5AHB 125-250G@75P",{"$f":"_xlfn.XLOOKUP(C985,DataSource!A:A,DataSource!AH:AH)","v":"1733 2.5 in AHB 125-250 75 BLACK (Std) PG"}]
[null,null,"17334024","TBJT 2.5AGZ 125-250G@100P FM",{"$f":"_xlfn.XLOOKUP(C986,DataSource!A:A,DataSource!AH:AH)","v":"1733 2.5 in AGZ 125-250 100 (Std) BLACK (Std) PG"}]
[null,null,"17334034","TBJT 2.5AGA 125-250G@100P FM",{"$f":"_xlfn.XLOOKUP(C987,DataSource!A:A,DataSource!AH:AH)","v":"1733 2.5 in AGA 125-250 100 (Std) BLACK (Std) PG"}]
[null,null,"17337003","TBJT NPG 2.5AGA 125-250G@100P FM",{"$f":"_xlfn.XLOOKUP(C988,DataSource!A:A,DataSource!AH:AH)","v":"1733 2.5 in AGA 125-250 100 (Std) BLACK (Std) NPG"}]
[null,null,"17337014","TBJT NPG 2.5AEA 125-250G@100P FM",{"$f":"_xlfn.XLOOKUP(C989,DataSource!A:A,DataSource!AH:AH)","v":"1733 2.5 in AEA 125-250 100 (Std) BLACK (Std) PG"}]
[null,null,"17234011","TBJT 75MM 360-750L@7b",{"$f":"_xlfn.XLOOKUP(C990,DataSource!A:A,DataSource!AH:AH)","v":"1723 3 in STORZ 360-750 7 BLACK (Std) PG"}]
[null,null,"17234018","TBJT 52MM 95-200G@100P",{"$f":"_xlfn.XLOOKUP(C991,DataSource!A:A,DataSource!AH:AH)","v":"1723 2.5 in STORZ 95-200 100 (Std) BLACK (Std) PG"}]
[null,null,"17234024","TBJT 2.5NH 95-200G@75P",{"$f":"_xlfn.XLOOKUP(C992,DataSource!A:A,DataSource!AH:AH)","v":"1723 2.5 in NH 95-200 75 BLACK (Std) PG"}]
[null,null,"17234025","TBJT 2.5NH 95-200G@100P",{"$f":"_xlfn.XLOOKUP(C993,DataSource!A:A,DataSource!AH:AH)","v":"1723 2.5 in NH 95-200 75 BLACK (Std) PG"}]
[null,null,"17234010","TBJT 2.5BIM 360-750L@7b",{"$f":"_xlfn.XLOOKUP(C994,DataSource!A:A,DataSource!AH:AH)","v":"1723 2.5 in BIM 360-750 7 BLACK (Std) PG"}]
[null,null,"17234022","TBJT 2.5AJD 95-200G@100P",{"$f":"_xlfn.XLOOKUP(C995,DataSource!A:A,DataSource!AH:AH)","v":"1723 2.5 in AJD 95-200 100 (Std) BLACK (Std) PG"}]
[null,null,"17234008","TBJT 1.5NPSH 95-200G@75P",{"$f":"_xlfn.XLOOKUP(C996,DataSource!A:A,DataSource!AH:AH)","v":"1723 1.5 in NPSH 95-200 75 BLACK (Std) PG"}]
[null,null,"17234023","TBJT ZT 1.5NPSH 95-200G@100P",{"$f":"_xlfn.XLOOKUP(C997,DataSource!A:A,DataSource!AH:AH)","v":"1723 1.5 in NPSH 95-200 100 (Std) BLACK (Std) PG ZT"}]
[null,null,"17234003","TBJT 1.5NPSH 95-200G@100P",{"$f":"_xlfn.XLOOKUP(C998,DataSource!A:A,DataSource!AH:AH)","v":"1723 1.5 in NPSH 95-200 100 (Std) BLACK (Std) PG"}]
[null,null,"17237003","TBJT NPG 1.5NPSH 95-200G@100P",{"$f":"_xlfn.XLOOKUP(C999,DataSource!A:A,DataSource!AH:AH)","v":"1723 1.5 in NPSH 95-200 100 (Std) BLACK (Std) NPG"}]
[null,null,"17234013","TBJT 1.5NPSH 360-750L@700K",{"$f":"_xlfn.XLOOKUP(C1000,DataSource!A:A,DataSource!AH:AH)","v":"1723 1.5 in NPSH 360-750 700 BLACK (Std) PG"}]
[null,null,"17234006","TBJT 1.5NH 95-200G@75P YLWBMPR",{"$f":"_xlfn.XLOOKUP(C1001,DataSource!A:A,DataSource!AH:AH)","v":"1723 1.5 in NH 95-200 75 YELLOW PG"}]
[null,null,"17234017","TBJT 1.5NH 95-200G@75P REDBMPR",{"$f":"_xlfn.XLOOKUP(C1002,DataSource!A:A,DataSource!AH:AH)","v":"1723 1.5 in NH 95-200 75 RED PG"}]
[null,null,"17234026","TBJT 1.5NH 95-200G@75P MT. PLEASANT",{"$f":"_xlfn.XLOOKUP(C1003,DataSource!A:A,DataSource!AH:AH)","v":"1723 1.5 in NH 95-200 75 BLACK (Std) PG ETCH"}]
[null,null,"17234027","TBJT 1.5NH 95-200G@75P RED BANKS",{"$f":"_xlfn.XLOOKUP(C1004,DataSource!A:A,DataSource!AH:AH)","v":"1723 1.5 in NH 95-200 75 BLACK (Std) PG ETCH"}]
[null,null,"17234028","TBJT 1.5NH 95-200G@75P VICTORIA",{"$f":"_xlfn.XLOOKUP(C1005,DataSource!A:A,DataSource!AH:AH)","v":"1723 1.5 in NH 95-200 75 BLACK (Std) PG ETCH"}]
[null,null,"17234029","TBJT 1.5NH 95-200G@75P WATSON",{"$f":"_xlfn.XLOOKUP(C1006,DataSource!A:A,DataSource!AH:AH)","v":"1723 1.5 in NH 95-200 75 BLACK (Std) PG ETCH"}]
[null,null,"17234002","TBJT 1.5NH 95-200G@75P",{"$f":"_xlfn.XLOOKUP(C1007,DataSource!A:A,DataSource!AH:AH)","v":"1723 1.5 in NH 95-200 75 BLACK (Std) PG"}]
[null,null,"17237001","TBJT NPG 1.5NH 95-200G@75P",{"$f":"_xlfn.XLOOKUP(C1008,DataSource!A:A,DataSource!AH:AH)","v":"1723 1.5 in NH 95-200 75 BLACK (Std) NPG"}]
[null,null,"17234015","TBJT 1.5NH 95-200G@100P YLWBMPR",{"$f":"_xlfn.XLOOKUP(C1009,DataSource!A:A,DataSource!AH:AH)","v":"1723 1.5 in NH 95-200 100 (Std) YELLOW PG"}]
[null,null,"17234005","TBJT 1.5NH 95-200G@100P REDBMPR",{"$f":"_xlfn.XLOOKUP(C1010,DataSource!A:A,DataSource!AH:AH)","v":"1723 1.5 in NH 95-200 100 (Std) RED PG"}]
[null,null,"17237004","TBJT NPG 1.5NH 95-200G@100P REDBMPR",{"$f":"_xlfn.XLOOKUP(C1011,DataSource!A:A,DataSource!AH:AH)","v":"1723 1.5 in NH 95-200 100 (Std) RED NPG"}]
[null,null,"17234012","TBJT 1.5NH 95-200G@100P ORGBMPR",{"$f":"_xlfn.XLOOKUP(C1012,DataSource!A:A,DataSource!AH:AH)","v":"1723 1.5 in NH 95-200 100 (Std) ORANGE PG"}]
[null,null,"17234020","TBJT 1.5NH 95-200G@100P GRNBMPR",{"$f":"_xlfn.XLOOKUP(C1013,DataSource!A:A,DataSource!AH:AH)","v":"1723 1.5 in NH 95-200 100 (Std) GREEN PG"}]
[null,null,"17234021","TBJT ZT 1.5NH 95-200G@100P",{"$f":"_xlfn.XLOOKUP(C1014,DataSource!A:A,DataSource!AH:AH)","v":"1723 1.5 in NH 95-200 100 (Std) BLACK (Std) PG ZT"}]
[null,null,"17234007","TBJT 1.5NH 95-200G@100P FINLEYFIRE.COM",{"$f":"_xlfn.XLOOKUP(C1015,DataSource!A:A,DataSource!AH:AH)","v":"1723 1.5 in NH 95-200 100 (Std) BLACK (Std) PG ETCH"}]
[null,null,"17234001","TBJT 1.5NH 95-200G@100P#",{"$f":"_xlfn.XLOOKUP(C1016,DataSource!A:A,DataSource!AH:AH)","v":"1723 1.5 in NH 95-200 100 (Std) BLACK (Std) PG"}]
[null,null,"17237002","TBJT NPG 1.5NH 95-200G@100P#",{"$f":"_xlfn.XLOOKUP(C1017,DataSource!A:A,DataSource!AH:AH)","v":"1723 1.5 in NH 95-200 100 (Std) BLACK (Std) NPG"}]
[null,null,"17234014","TBJT ZT 1.5BSP 360-750L@7b",{"$f":"_xlfn.XLOOKUP(C1018,DataSource!A:A,DataSource!AH:AH)","v":"1723 1.5 in BSP 360-750 7 BLACK (Std) PG ZT"}]
[null,null,"17234009","TBJT 1.5BSP 360-750L@7b",{"$f":"_xlfn.XLOOKUP(C1019,DataSource!A:A,DataSource!AH:AH)","v":"1723 1.5 in BSP 360-750 7 BLACK (Std) PG"}]
[null,null,"17234016","TBJT 1.5ABX 95-200G@100P",{"$f":"_xlfn.XLOOKUP(C1020,DataSource!A:A,DataSource!AH:AH)","v":"1723 1.5 in ABX 95-200 100 (Std) BLACK (Std) PG"}]
[null,null,"17204014","TBJT 75MM 115-475L@7b FM",{"$f":"_xlfn.XLOOKUP(C1021,DataSource!A:A,DataSource!AH:AH)","v":"1720 3 in STORZ 115-475 7 BLACK (Std) PG"}]
[null,null,"17204013","TBJT 65MM 115-475L@7b FM",{"$f":"_xlfn.XLOOKUP(C1022,DataSource!A:A,DataSource!AH:AH)","v":"1720 2.5 in STORZ 115-475 7 BLACK (Std) PG"}]
[null,null,"17204024","TBJT ZT 2.5NH 30-125G@100P",{"$f":"_xlfn.XLOOKUP(C1023,DataSource!A:A,DataSource!AH:AH)","v":"1720 2.5 in NH 30-125 100 (Std) BLACK (Std) PG ZT"}]
[null,null,"17204040","TBJT 2.5BIM 30-125G@100P FM#",{"$f":"_xlfn.XLOOKUP(C1024,DataSource!A:A,DataSource!AH:AH)","v":"1720 2.5 in BIM 30-125 100 (Std) BLACK (Std) PG"}]
[null,null,"17204039","TBJT 2.5BIM 115-475L@7b SPECIAL",{"$f":"_xlfn.XLOOKUP(C1025,DataSource!A:A,DataSource!AH:AH)","v":"1720 2.5 in BIM 115-475 7 BLACK (Std) PG ETCH"}]
[null,null,"17204003","TBJT 2.5BIM 115-475L@7b FM#",{"$f":"_xlfn.XLOOKUP(C1026,DataSource!A:A,DataSource!AH:AH)","v":"1720 2.5 in BIM 115-475 7 BLACK (Std) PG"}]
[null,null,"17204045","TBJT 2.5BIM 115-475L@5b",{"$f":"_xlfn.XLOOKUP(C1027,DataSource!A:A,DataSource!AH:AH)","v":"1720 2.5 in BIM 115-475 5 BLACK (Std) PG"}]
[null,null,"17204036","TBJT ZT 2.5BIM 100-450L@6b",{"$f":"_xlfn.XLOOKUP(C1028,DataSource!A:A,DataSource!AH:AH)","v":"1720 2.5 in BIM 100-450 6 BLACK (Std) PG ZT"}]
[null,null,"17204037","TBJT  2.5BIM 100-450L@6b",{"$f":"_xlfn.XLOOKUP(C1029,DataSource!A:A,DataSource!AH:AH)","v":"1720 2.5 in BIM 100-450 6 BLACK (Std) PG"}]
[null,null,"17204702","TBJT 2.5BIM 100-450L@6b EN",{"$f":"_xlfn.XLOOKUP(C1030,DataSource!A:A,DataSource!AH:AH)","v":"1720 2.5 in BIM 100-450 6 BLACK (Std) PG"}]
[null,null,"17204027","TBJT 52MM 30-125G@100P FM",{"$f":"_xlfn.XLOOKUP(C1031,DataSource!A:A,DataSource!AH:AH)","v":"1720 2 in STORZ 30-125 100 (Std) BLACK (Std) PG"}]
[null,null,"17204012","TBJT 52MM 115-475L@7b FM",{"$f":"_xlfn.XLOOKUP(C1032,DataSource!A:A,DataSource!AH:AH)","v":"1720 2 in STORZ 115-475 7 BLACK (Std) PG"}]
[null,null,"17204020","TBJT 52MM 115-475L@7b GERMAN FM",{"$f":"_xlfn.XLOOKUP(C1033,DataSource!A:A,DataSource!AH:AH)","v":"1720 2 in STORZ 115-475 7 BLACK (Std) PG"}]
[null,null,"17204032","TBJT 38MM 30-125G@100P FM",{"$f":"_xlfn.XLOOKUP(C1034,DataSource!A:A,DataSource!AH:AH)","v":"1720 1.5 in STORZ 30-125 100 (Std) BLACK (Std) PG"}]
[null,null,"17204026","TBJT 38MM 115-475L@7b FM",{"$f":"_xlfn.XLOOKUP(C1035,DataSource!A:A,DataSource!AH:AH)","v":"1720 1.5 in STORZ 115-475 7 BLACK (Std) PG"}]
[null,null,"17204023","TBJT 1.5NPSH 30-125G@75P",{"$f":"_xlfn.XLOOKUP(C1036,DataSource!A:A,DataSource!AH:AH)","v":"1720 1.5 in NPSH 30-125 75 BLACK (Std) PG"}]
[null,null,"17204041","TBJT ZT 1.5NPSH 30-125G@100P",{"$f":"_xlfn.XLOOKUP(C1037,DataSource!A:A,DataSource!AH:AH)","v":"1720 1.5 in NPSH 30-125 100 (Std) BLACK (Std) PG ZT"}]
[null,null,"17204002","TBJT 1.5NPSH 30-125G@100P FM",{"$f":"_xlfn.XLOOKUP(C1038,DataSource!A:A,DataSource!AH:AH)","v":"1720 1.5 in NPSH 30-125 100 (Std) BLACK (Std) PG"}]
[null,null,"17207002","TBJT NPG 1.5NPSH 30-125G@100P FM",{"$f":"_xlfn.XLOOKUP(C1039,DataSource!A:A,DataSource!AH:AH)","v":"1720 1.5 in NPSH 30-125 100 (Std) BLACK (Std) NPG"}]
[null,null,"17204005","TBJT 1.5NPSH 115-475L@7b FM",{"$f":"_xlfn.XLOOKUP(C1040,DataSource!A:A,DataSource!AH:AH)","v":"1720 1.5 in NPSH 115-475 7 BLACK (Std) PG"}]
[null,null,"17204019","TBJT 1.5NPSH 115-475L@5b",{"$f":"_xlfn.XLOOKUP(C1041,DataSource!A:A,DataSource!AH:AH)","v":"1720 1.5 in NPSH 115-475 5 BLACK (Std) PG"}]
[null,null,"17204046","TBJT 1.5NH 30-125G@75P YLWBMPR",{"$f":"_xlfn.XLOOKUP(C1042,DataSource!A:A,DataSource!AH:AH)","v":"1720 1.5 in NH 30-125 75 YELLOW PG"}]
[null,null,"17204047","TBJT 1.5NH 30-125G@75P REDBMPR",{"$f":"_xlfn.XLOOKUP(C1043,DataSource!A:A,DataSource!AH:AH)","v":"1720 1.5 in NH 30-125 75 RED PG"}]
[null,null,"17204033","TBJT 1.5NH 30-125G@75P ORGBMPR MVFD",{"$f":"_xlfn.XLOOKUP(C1044,DataSource!A:A,DataSource!AH:AH)","v":"1720 1.5 in NH 30-125 75 ORANGE PG ETCH"}]
[null,null,"17204048","TBJT 1.5NH 30-125G@75P ORGBMPR",{"$f":"_xlfn.XLOOKUP(C1045,DataSource!A:A,DataSource!AH:AH)","v":"1720 1.5 in NH 30-125 75 ORANGE PG"}]
[null,null,"17207033","TBJT NPG 1.5NH 30-125G@75P ORGBMPR MVFD",{"$f":"_xlfn.XLOOKUP(C1046,DataSource!A:A,DataSource!AH:AH)","v":"1720 1.5 in NH 30-125 75 ORANGE NPG ETCH"}]
[null,null,"17204031","TBJT ZT 1.5NH 30-125G@ 75P",{"$f":"_xlfn.XLOOKUP(C1047,DataSource!A:A,DataSource!AH:AH)","v":"1720 1.5 in NH 30-125 75 BLACK (Std) PG ZT"}]
[null,null,"17204034","TBJT 1.5NH 30-125G@75P MVFD",{"$f":"_xlfn.XLOOKUP(C1048,DataSource!A:A,DataSource!AH:AH)","v":"1720 1.5 in NH 30-125 75 BLACK (Std) PG ETCH"}]
[null,null,"17204011","TBJT 1.5NH 30-125G@75P",{"$f":"_xlfn.XLOOKUP(C1049,DataSource!A:A,DataSource!AH:AH)","v":"1720 1.5 in NH 30-125 75 BLACK (Std) PG"}]
[null,null,"17207034","TBJT NPG 1.5NH 30-125G@75P ETCH MVFD",{"$f":"_xlfn.XLOOKUP(C1050,DataSource!A:A,DataSource!AH:AH)","v":"1720 1.5 in NH 30-125 75 BLACK (Std) NPG ETCH"}]
[null,null,"17207011","TBJT NPG 1.5NH 30-125G@75P",{"$f":"_xlfn.XLOOKUP(C1051,DataSource!A:A,DataSource!AH:AH)","v":"1720 1.5 in NH 30-125 75 BLACK (Std) NPG"}]
[null,null,"17204042","TBJT 1.5NH 30-125G@100P YLWBMPR FM",{"$f":"_xlfn.XLOOKUP(C1052,DataSource!A:A,DataSource!AH:AH)","v":"1720 1.5 in NH 30-125 100 (Std) YELLOW PG"}]
[null,null,"17204018","TBJT ZT 1.5NH 30-125G@100P",{"$f":"_xlfn.XLOOKUP(C1053,DataSource!A:A,DataSource!AH:AH)","v":"1720 1.5 in NH 30-125 100 (Std) BLACK (Std) PG ZT"}]
[null,null,"17204038","TBJT 1.5NH 30-125G@100P DE STATE FS LOGO",{"$f":"_xlfn.XLOOKUP(C1054,DataSource!A:A,DataSource!AH:AH)","v":"1720 1.5 in NH 30-125 100 (Std) BLACK (Std) PG ETCH"}]
[null,null,"17204001","TBJT 1.5NH 30-125G@100P FM",{"$f":"_xlfn.XLOOKUP(C1055,DataSource!A:A,DataSource!AH:AH)","v":"1720 1.5 in NH 30-125 100 (Std) BLACK (Std) PG"}]
[null,null,"17207001","TBJT NPG 1.5NH 30-125G@100P FM",{"$f":"_xlfn.XLOOKUP(C1056,DataSource!A:A,DataSource!AH:AH)","v":"1720 1.5 in NH 30-125 100 (Std) BLACK (Std) NPG"}]
[null,null,"17204049","TBJT 1.5NH 115-475L@5b",{"$f":"_xlfn.XLOOKUP(C1057,DataSource!A:A,DataSource!AH:AH)","v":"1720 1.5 in NH 115-475 5 BLACK (Std) PG"}]
[null,null,"17204022","TBJT ZT 1.5 ADPT EXT 115-475L@7b",{"$f":"_xlfn.XLOOKUP(C1058,DataSource!A:A,DataSource!AH:AH)","v":"1720 1.5 in N/A 115-475 7 BLACK (Std) PG ZT"}]
[null,null,"17204004","TBJT 1.5BSP 115-475L@7b FM",{"$f":"_xlfn.XLOOKUP(C1059,DataSource!A:A,DataSource!AH:AH)","v":"1720 1.5 in BSP 115-475 7 BLACK (Std) PG"}]
[null,null,"17204021","TBJT 1.5BSP 115-475L@7b SPANISH FM",{"$f":"_xlfn.XLOOKUP(C1060,DataSource!A:A,DataSource!AH:AH)","v":"1720 1.5 in BSP 115-475 7 BLACK (Std) PG"}]
[null,null,"17204025","TBJT 1.5BSP M 115-475L@7b FM",{"$f":"_xlfn.XLOOKUP(C1061,DataSource!A:A,DataSource!AH:AH)","v":"1720 1.5 in BSP 115-475 7 BLACK (Std) PG"}]
[null,null,"17207021","TBJT NPG 1.5BSP 115-475L@7b SPANISH FM",{"$f":"_xlfn.XLOOKUP(C1062,DataSource!A:A,DataSource!AH:AH)","v":"1720 1.5 in BSP 115-475 7 BLACK (Std) NPG"}]
[null,null,"17204015","TBJT 1.5BSP M 115-475L@5b",{"$f":"_xlfn.XLOOKUP(C1063,DataSource!A:A,DataSource!AH:AH)","v":"1720 1.5 in BSP 115-475 5 BLACK (Std) PG"}]
[null,null,"17204700","TBJT 1.5BSP100-450L@6b DUTCH SER# BLU EN",{"$f":"_xlfn.XLOOKUP(C1064,DataSource!A:A,DataSource!AH:AH)","v":"1720 1.5 in BSP 100-450 6 BLUE PG"}]
[null,null,"17204029","TBJT ZT 1.5BSP 100-450L@6b",{"$f":"_xlfn.XLOOKUP(C1065,DataSource!A:A,DataSource!AH:AH)","v":"1720 1.5 in BSP 100-450 6 BLACK (Std) PG ZT"}]
[null,null,"17204030","TBJT 1.5BSP100-450L@6b",{"$f":"_xlfn.XLOOKUP(C1066,DataSource!A:A,DataSource!AH:AH)","v":"1720 1.5 in BSP 100-450 6 BLACK (Std) PG"}]
[null,null,"17204701","TBJT 1.5BSP 100-450L@6b EN",{"$f":"_xlfn.XLOOKUP(C1067,DataSource!A:A,DataSource!AH:AH)","v":"1720 1.5 in BSP 100-450 6 BLACK (Std) PG"}]
[null,null,"17204017","TBJT 1.5BIM 115-475L@7b FM",{"$f":"_xlfn.XLOOKUP(C1068,DataSource!A:A,DataSource!AH:AH)","v":"1720 1.5 in BIM 115-475 7 BLACK (Std) PG"}]
[null,null,"17204028","TBJT ZT 1.5BIM 100-450L@6b",{"$f":"_xlfn.XLOOKUP(C1069,DataSource!A:A,DataSource!AH:AH)","v":"1720 1.5 in BIM 100-450 6 BLACK (Std) PG ZT"}]
[null,null,"17204035","TBJT 1.5ABX 30-125G@75P",{"$f":"_xlfn.XLOOKUP(C1070,DataSource!A:A,DataSource!AH:AH)","v":"1720 1.5 in ABX 30-125 75 BLACK (Std) PG"}]
[null,null,"17144003","TBJT TIP 1.5NPSH 30-125G@100P",{"$f":"_xlfn.XLOOKUP(C1071,DataSource!A:A,DataSource!AH:AH)","v":"1714 1.5 in NPSH 30-125 100 (Std) BLACK (Std)"}]
[null,null,"17144002","TBJT TIP 1.5NH 30-125G@75P",{"$f":"_xlfn.XLOOKUP(C1072,DataSource!A:A,DataSource!AH:AH)","v":"1714 1.5 in NH 30-125 75 BLACK (Std)"}]
[null,null,"17144008","TBJT TIP 1.5NH 30-125G@100P SUMMERFIELD",{"$f":"_xlfn.XLOOKUP(C1073,DataSource!A:A,DataSource!AH:AH)","v":"1714 1.5 in NH 30-125 100 (Std) BLACK (Std) ETCH"}]
[null,null,"17144001","TBJT TIP 1.5NH 30-125G@100P",{"$f":"_xlfn.XLOOKUP(C1074,DataSource!A:A,DataSource!AH:AH)","v":"1714 1.5 in NH 30-125 100 (Std) BLACK (Std)"}]
[null,null,"17144004","TBJT TIP 1.5BSP 115-475L@7b",{"$f":"_xlfn.XLOOKUP(C1075,DataSource!A:A,DataSource!AH:AH)","v":"1714 1.5 in BSP 115-475 7 BLACK (Std)"}]
[null,null,"17144005","TBJT TIP 1.5BSP 115-475L@6b",{"$f":"_xlfn.XLOOKUP(C1076,DataSource!A:A,DataSource!AH:AH)","v":"1714 1.5 in BSP 115-475 6 BLACK (Std)"}]
[null,null,"17114001","TBJT TIP 1.5NH 13-23-30G@100P",{"$f":"_xlfn.XLOOKUP(C1077,DataSource!A:A,DataSource!AH:AH)","v":"1711 1.5 in NH 13-30 100 (Std) BLACK (Std)"}]
[null,null,"17114702","TBJT TIP 1.5BSP 70-115L@6b",{"$f":"_xlfn.XLOOKUP(C1078,DataSource!A:A,DataSource!AH:AH)","v":"1711 1.5 in BSP 70-115 6 BLACK (Std)"}]
[null,null,"17114701","TBJT TIP 1.5BSP 50-115L@6b DUTCH BLU",{"$f":"_xlfn.XLOOKUP(C1079,DataSource!A:A,DataSource!AH:AH)","v":"1711 1.5 in BSP 50-115 6 BLUE"}]
[null,null,"17044005","TBJT 52MM 50-115L@7b GERMAN YLWBMPR",{"$f":"_xlfn.XLOOKUP(C1080,DataSource!A:A,DataSource!AH:AH)","v":"1704 2 in STORZ 50-115 7 YELLOW PG"}]
[null,null,"17044008","TBJT 52MM 50-115L@7b GERMAN",{"$f":"_xlfn.XLOOKUP(C1081,DataSource!A:A,DataSource!AH:AH)","v":"1704 2 in STORZ 50-115 7 BLACK (Std) PG"}]
[null,null,"17044010","TBJT 1.0 BSPX25MM STZ 50-115L@7b YLWBMPR",{"$f":"_xlfn.XLOOKUP(C1082,DataSource!A:A,DataSource!AH:AH)","v":"1704 1 in STORZ 50-115 7 YELLOW PG"}]
[null,null,"17044004","TBJT 1.0 NH 70-115L@7b",{"$f":"_xlfn.XLOOKUP(C1083,DataSource!A:A,DataSource!AH:AH)","v":"1704 1 in NH 70-115 7 BLACK (Std) PG"}]
[null,null,"17044007","TBJT 1.0 NH 50-90-115L@7b/700kPa",{"$f":"_xlfn.XLOOKUP(C1084,DataSource!A:A,DataSource!AH:AH)","v":"1704 1 in NH 50-115 7 BLACK (Std) PG"}]
[null,null,"17044009","TBJT 1.0 NH 18-30G@100P ORGBMPR",{"$f":"_xlfn.XLOOKUP(C1085,DataSource!A:A,DataSource!AH:AH)","v":"1704 1 in NH 18-30 100 (Std) ORANGE PG"}]
[null,null,"17044003","TBJT 1.0 NH 18-30G@100P",{"$f":"_xlfn.XLOOKUP(C1086,DataSource!A:A,DataSource!AH:AH)","v":"1704 1 in NH 18-30 100 (Std) BLACK (Std) PG"}]
[null,null,"17044002","TBJT 1.0 NH 13-23-30G@100P",{"$f":"_xlfn.XLOOKUP(C1087,DataSource!A:A,DataSource!AH:AH)","v":"1704 1 in NH 13-30 100 (Std) BLACK (Std) PG"}]
[null,null,"17047002","TBJT NPG 1.0 NH 13-23-30G@100P",{"$f":"_xlfn.XLOOKUP(C1088,DataSource!A:A,DataSource!AH:AH)","v":"1704 1 in NH 13-30 100 (Std) BLACK (Std) NPG"}]
[null,null,"17044001","TBJT 1.0 BSP 70-115L@7b",{"$f":"_xlfn.XLOOKUP(C1089,DataSource!A:A,DataSource!AH:AH)","v":"1704 1 in BSP 70-115 7 BLACK (Std) PG"}]
[null,null,"17044702","TBJT 1.0 BSP 70-115L@6b GERMAN EN",{"$f":"_xlfn.XLOOKUP(C1090,DataSource!A:A,DataSource!AH:AH)","v":"1704 1 in BSP 70-115 6 BLACK (Std) PG"}]
[null,null,"17044006","TBJT 1.0 BSP 50-90-115L@7b",{"$f":"_xlfn.XLOOKUP(C1091,DataSource!A:A,DataSource!AH:AH)","v":"1704 1 in BSP 50-115 7 BLACK (Std) PG"}]
[null,null,"17044701","TBJT 1.0 BSP 50-115L@6b DUTCH BLU EN",{"$f":"_xlfn.XLOOKUP(C1092,DataSource!A:A,DataSource!AH:AH)","v":"1704 1 in BSP 50-115 6 BLUE PG"}]
[null,null,"17044703","TBJT 1.0 BSP 50-115L@6b ENGLISH EN",{"$f":"_xlfn.XLOOKUP(C1093,DataSource!A:A,DataSource!AH:AH)","v":"1704 1 in BSP 50-115 6 BLACK (Std) PG"}]
[null,null,"17034005","TBJT TIP 1.0 W/1.5NPSH 13-60G@100P",{"$f":"_xlfn.XLOOKUP(C1094,DataSource!A:A,DataSource!AH:AH)","v":"1703 1.5 in NPSH 13-60 100 (Std) BLACK (Std)"}]
[null,null,"17034003","TBJT TIP 1.0 W/1.5NH 50-230L@7b",{"$f":"_xlfn.XLOOKUP(C1095,DataSource!A:A,DataSource!AH:AH)","v":"1703 1.5 in NH 50-230 7 BLACK (Std)"}]
[null,null,"17034001","TBJT TIP 1.0 W/1.5NH 13-60G@100P#",{"$f":"_xlfn.XLOOKUP(C1096,DataSource!A:A,DataSource!AH:AH)","v":"1703 1.5 in NH 13-60 100 (Std) BLACK (Std)"}]
[null,null,"17034004","TBJT TIP 1.0 W/1.5BSP 50-230L@6b GERMAN",{"$f":"_xlfn.XLOOKUP(C1097,DataSource!A:A,DataSource!AH:AH)","v":"1703 1.5 in BSP 50-30 6 BLACK (Std)"}]
[null,null,"17034002","TBJT TIP 1.0 W/1.5BSP 50-230L@7b",{"$f":"_xlfn.XLOOKUP(C1098,DataSource!A:A,DataSource!AH:AH)","v":"1703 1.5 in BSP 50-230 7 BLACK (Std)"}]
[null,null,"17024009","TBJT 2.5BIM 50-230L@7b FM",{"$f":"_xlfn.XLOOKUP(C1099,DataSource!A:A,DataSource!AH:AH)","v":"1702 2.5 in BIM 50-230 7 BLACK (Std) PG"}]
[null,null,"17024010","TBJT 52MM 50-230L@7b FM",{"$f":"_xlfn.XLOOKUP(C1100,DataSource!A:A,DataSource!AH:AH)","v":"1702 2 in STORZ 50-230 7 BLACK (Std) PG"}]
[null,null,"17024701","TBJT 52MM 50-230L@6b GERMAN EN",{"$f":"_xlfn.XLOOKUP(C1101,DataSource!A:A,DataSource!AH:AH)","v":"1702 2 in STORZ 50-230 6 BLACK (Std) PG"}]
[null,null,"17027701","TBJT NPG 52MM 50-230L@6b GERMAN EN",{"$f":"_xlfn.XLOOKUP(C1102,DataSource!A:A,DataSource!AH:AH)","v":"1702 2 in STORZ 50-230 6 BLACK (Std) NPG"}]
[null,null,"17024021","TBJT 1.5 NH 13-60G@100P FM",{"$f":"_xlfn.XLOOKUP(C1103,DataSource!A:A,DataSource!AH:AH)","v":"1702 1.5 in NH 13-60 100 (Std) BLACK (Std) PG"}]
[null,null,"17024003","TBJT 1.0 BSPX25MMSTZ 50-230L@7b FM",{"$f":"_xlfn.XLOOKUP(C1104,DataSource!A:A,DataSource!AH:AH)","v":"1702 1 in STORZ 50-230 7 BLACK (Std) PG"}]
[null,null,"17024704","TBJT 1.0BSPX25MMSTZ 50-230L@6b GERMAN EN",{"$f":"_xlfn.XLOOKUP(C1105,DataSource!A:A,DataSource!AH:AH)","v":"1702 1 in STORZ 50-230 6 BLACK (Std) PG"}]
[null,null,"17024008","TBJT 1.0 NPSH 13-60G@100P FM",{"$f":"_xlfn.XLOOKUP(C1106,DataSource!A:A,DataSource!AH:AH)","v":"1702 1 in NPSH 13-60 100 (Std) BLACK (Std) PG"}]
[null,null,"17027008","TBJT NPG 1.0 NPSH 13-60G@100P FM",{"$f":"_xlfn.XLOOKUP(C1107,DataSource!A:A,DataSource!AH:AH)","v":"1702 1 in NPSH 13-60 100 (Std) BLACK (Std) NPG"}]
[null,null,"17024004","TBJT 1.0 NH 50-230L@7b FM",{"$f":"_xlfn.XLOOKUP(C1108,DataSource!A:A,DataSource!AH:AH)","v":"1702 1 in NH 50-230 7 BLACK (Std) PG"}]
[null,null,"17024013","TBJT 1.0 NH 13-60G@100P YLWBMPR BCFD",{"$f":"_xlfn.XLOOKUP(C1109,DataSource!A:A,DataSource!AH:AH)","v":"1702 1 in NH 13-60 100 (Std) YELLOW PG ETCH"}]
[null,null,"17024012","TBJT 1.0 NH 13-60G@100P ORGBMPR BCFD",{"$f":"_xlfn.XLOOKUP(C1110,DataSource!A:A,DataSource!AH:AH)","v":"1702 1 in NH 13-60 100 (Std) ORANGE PG ETCH"}]
[null,null,"17024011","TBJT 1.0 NH 13-60G@100P UNIONVILLE E-210",{"$f":"_xlfn.XLOOKUP(C1111,DataSource!A:A,DataSource!AH:AH)","v":"1702 1 in NH 13-60 100 (Std) BLACK (Std) PG ETCH"}]
[null,null,"17024017","TBJT 1.0 NH 13-60G@100P MT. PLEASANT",{"$f":"_xlfn.XLOOKUP(C1112,DataSource!A:A,DataSource!AH:AH)","v":"1702 1 in NH 13-60 100 (Std) BLACK (Std) PG ETCH"}]
[null,null,"17024018","TBJT 1.0 NH 13-60G@100P RED BANKS",{"$f":"_xlfn.XLOOKUP(C1113,DataSource!A:A,DataSource!AH:AH)","v":"1702 1 in NH 13-60 100 (Std) BLACK (Std) PG ETCH"}]
[null,null,"17024019","TBJT 1.0 NH 13-60G@100P VICTORIA",{"$f":"_xlfn.XLOOKUP(C1114,DataSource!A:A,DataSource!AH:AH)","v":"1702 1 in NH 13-60 100 (Std) BLACK (Std) PG ETCH"}]
[null,null,"17024020","TBJT 1.0 NH 13-60G@100P WATSON",{"$f":"_xlfn.XLOOKUP(C1115,DataSource!A:A,DataSource!AH:AH)","v":"1702 1 in NH 13-60 100 (Std) BLACK (Std) PG ETCH"}]
[null,null,"17024001","TBJT 1.0 NH 13-60G@100P FM",{"$f":"_xlfn.XLOOKUP(C1116,DataSource!A:A,DataSource!AH:AH)","v":"1702 1 in NH 13-60 100 (Std) BLACK (Std) PG"}]
[null,null,"17027001","TBJT NPG 1.0 NH 13-60G@100P",{"$f":"_xlfn.XLOOKUP(C1117,DataSource!A:A,DataSource!AH:AH)","v":"1702 1 in NH 13-60 100 (Std) BLACK (Std) NPG"}]
[null,null,"17024002","TBJT 1.0 BSP 50-230L@7b FM",{"$f":"_xlfn.XLOOKUP(C1118,DataSource!A:A,DataSource!AH:AH)","v":"1702 1 in BSP 50-230 7 BLACK (Std) PG"}]
[null,null,"17027002","TBJT NPG 1.0 BSP 50-230L@7b FM",{"$f":"_xlfn.XLOOKUP(C1119,DataSource!A:A,DataSource!AH:AH)","v":"1702 1 in BSP 50-230 7 BLACK (Std) NPG"}]
[null,null,"17024702","TBJT 1.0 BSP 50-230L@6b EN",{"$f":"_xlfn.XLOOKUP(C1120,DataSource!A:A,DataSource!AH:AH)","v":"1702 1 in BSP 50-230 6 BLACK (Std) PG"}]
[null,null,"16164034","PROVENGER 75MM STORZ 115-550L@7b FM",{"$f":"_xlfn.XLOOKUP(C1121,DataSource!A:A,DataSource!AH:AH)","v":"1616 3 in STORZ 115-550 7 BLACK (Std) PG"}]
[null,null,"16164026","PROVENGER 65MM 30-150G@100P FM",{"$f":"_xlfn.XLOOKUP(C1122,DataSource!A:A,DataSource!AH:AH)","v":"1616 2.5 in STORZ 30-150 100 (Std) BLACK (Std) PG"}]
[null,null,"16164031","PROVENGER 2.5AFD 30-150G@100P FM",{"$f":"_xlfn.XLOOKUP(C1123,DataSource!A:A,DataSource!AH:AH)","v":"1616 2.5 in QST 30-150 100 (Std) BLACK (Std) PG"}]
[null,null,"16164014","PROVENGER 2.5NH 30-150G@75P FM",{"$f":"_xlfn.XLOOKUP(C1124,DataSource!A:A,DataSource!AH:AH)","v":"1616 2.5 in NH 30-150 75 BLACK (Std) PG"}]
[null,null,"16164012","PROVENGER 2.5NH 30-150G@100P FM",{"$f":"_xlfn.XLOOKUP(C1125,DataSource!A:A,DataSource!AH:AH)","v":"1616 2.5 in NH 30-150 100 (Std) BLACK (Std) PG"}]
[null,null,"16164013","PROVENGER 2.5NH 285-750L@7b FM",{"$f":"_xlfn.XLOOKUP(C1126,DataSource!A:A,DataSource!AH:AH)","v":"1616 2.5 in NH 285-750 7 BLACK (Std) PG"}]
[null,null,"16164020","PROVENGER 2.5NH 115-550L@7b FM",{"$f":"_xlfn.XLOOKUP(C1127,DataSource!A:A,DataSource!AH:AH)","v":"1616 2.5 in NH 115-550 7 BLACK (Std) PG"}]
[null,null,"16165002","PROVENGER JIM 65MM PG 285-750L@5b CCCF",{"$f":"_xlfn.XLOOKUP(C1128,DataSource!A:A,DataSource!AH:AH)","v":"1616 2.5 in JIM 285-750 5 BLACK (Std) PG ETCH"}]
[null,null,"16165000","PROV JIM 65MM 115-550L@7b W/638  CCCF",{"$f":"_xlfn.XLOOKUP(C1129,DataSource!A:A,DataSource!AH:AH)","v":"1616 2.5 in JIM 115-550 7 BLACK (Std) PG ETCH"}]
[null,null,"16165001","PROVENGER JIM 65MM PG 115-550L@5b CCCF",{"$f":"_xlfn.XLOOKUP(C1130,DataSource!A:A,DataSource!AH:AH)","v":"1616 2.5 in JIM 115-550 5 BLACK (Std) PG ETCH"}]
[null,null,"16164010","PROVENGER 2.5BIM 30-150G@100P FM",{"$f":"_xlfn.XLOOKUP(C1131,DataSource!A:A,DataSource!AH:AH)","v":"1616 2.5 in BIM 30-150 100 (Std) BLACK (Std) PG"}]
[null,null,"16164017","PROVENGER 2.5BIM 285-750L@7b FM",{"$f":"_xlfn.XLOOKUP(C1132,DataSource!A:A,DataSource!AH:AH)","v":"1616 2.5 in BIM 285-750 7 BLACK (Std) PG"}]
[null,null,"16164025","PROVENGER ZT 2.5BIM 115-550L@7b",{"$f":"_xlfn.XLOOKUP(C1133,DataSource!A:A,DataSource!AH:AH)","v":"1616 2.5 in BIM 115-550 7 BLACK (Std) PG ZT"}]
[null,null,"16164011","PROVENGER 2.5BIM 115-550L@7b FM",{"$f":"_xlfn.XLOOKUP(C1134,DataSource!A:A,DataSource!AH:AH)","v":"1616 2.5 in BIM 115-550 7 BLACK (Std) PG"}]
[null,null,"16164018","PROVENGER 2.5BIM 115-550L@6b EN",{"$f":"_xlfn.XLOOKUP(C1135,DataSource!A:A,DataSource!AH:AH)","v":"1616 2.5 in BIM 115-550 6 BLACK (Std) PG"}]
[null,null,"16164028","PROVENGER 2.5BAF 30-150G@100P FM",{"$f":"_xlfn.XLOOKUP(C1136,DataSource!A:A,DataSource!AH:AH)","v":"1616 2.5 in BAT 30-150 100 (Std) BLACK (Std) PG"}]
[null,null,"16164021","PROVENGER 52MM 30-150G@100P FM",{"$f":"_xlfn.XLOOKUP(C1137,DataSource!A:A,DataSource!AH:AH)","v":"1616 2 in STORZ 30-150 100 (Std) BLACK (Std) PG"}]
[null,null,"16164033","PROVENGER 52MM 115-550L@7b",{"$f":"_xlfn.XLOOKUP(C1138,DataSource!A:A,DataSource!AH:AH)","v":"1616 2 in STORZ 115-550 7 BLACK (Std) PG"}]
[null,null,"16164019","PROVENGER 38MM 30-150G@100P FM",{"$f":"_xlfn.XLOOKUP(C1139,DataSource!A:A,DataSource!AH:AH)","v":"1616 1.5 in STORZ 30-150 100 (Std) BLACK (Std) PG"}]
[null,null,"16164024","PROVENGER 38MM 115-550L@6b EN",{"$f":"_xlfn.XLOOKUP(C1140,DataSource!A:A,DataSource!AH:AH)","v":"1616 1.5 in STORZ 115-550 6 BLACK (Std) PG"}]
[null,null,"16164023","PROVENGER 1.5NPSH 30-150G@87P EN",{"$f":"_xlfn.XLOOKUP(C1141,DataSource!A:A,DataSource!AH:AH)","v":"1616 1.5 in NPSH 30-150 87 (CE) BLACK (Std) PG ETCH"}]
[null,null,"16164008","PROVENGER 1.5NPSH 30-150G@75P FM",{"$f":"_xlfn.XLOOKUP(C1142,DataSource!A:A,DataSource!AH:AH)","v":"1616 1.5 in NPSH 30-150 75 BLACK (Std) PG"}]
[null,null,"16164009","PROVENGER 1.5NPSH 30-150G@100P FM",{"$f":"_xlfn.XLOOKUP(C1143,DataSource!A:A,DataSource!AH:AH)","v":"1616 1.5 in NPSH 30-150 100 (Std) BLACK (Std) PG"}]
[null,null,"16164004","PROVENGER 1.5NH 30-150G@75P FM#",{"$f":"_xlfn.XLOOKUP(C1144,DataSource!A:A,DataSource!AH:AH)","v":"1616 1.5 in NH 30-150 75 BLACK (Std) PG"}]
[null,null,"16164006","PROVENGER 1.5NH 30-150G@100P FM#",{"$f":"_xlfn.XLOOKUP(C1145,DataSource!A:A,DataSource!AH:AH)","v":"1616 1.5 in NH 30-150 100 (Std) BLACK (Std) PG"}]
[null,null,"16164022","PROVENGER 1.5NH 30-150G@100P MTLTTH",{"$f":"_xlfn.XLOOKUP(C1146,DataSource!A:A,DataSource!AH:AH)","v":"1616 1.5 in NH 30-150 100 (Std) BLACK (Std) PG"}]
[null,null,"16164007","PROVENGER 1.5NH 115-550L@7b FM",{"$f":"_xlfn.XLOOKUP(C1147,DataSource!A:A,DataSource!AH:AH)","v":"1616 1.5 in NH 115-550 7 BLACK (Std) PG"}]
[null,null,"16165003","PROVENGER 1.5 NH PG 115-550L@5b CCCF",{"$f":"_xlfn.XLOOKUP(C1148,DataSource!A:A,DataSource!AH:AH)","v":"1616 1.5 in NH 115-550 5 BLACK (Std) PG ETCH"}]
[null,null,"16164003","PROVENGER 1.5BSP 115-550L@7b FM",{"$f":"_xlfn.XLOOKUP(C1149,DataSource!A:A,DataSource!AH:AH)","v":"1616 1.5 in BSP 115-550 7 BLACK (Std) PG"}]
[null,null,"16164029","PROVENGER 1.5BSP 115-550L@6b EN",{"$f":"_xlfn.XLOOKUP(C1150,DataSource!A:A,DataSource!AH:AH)","v":"1616 1.5 in BSP 115-550 6 BLACK (Std) PG"}]
[null,null,"16164032","PROVENGER 1.5BSP 115-550L@5b",{"$f":"_xlfn.XLOOKUP(C1151,DataSource!A:A,DataSource!AH:AH)","v":"1616 1.5 in BSP 115-550 5 BLACK (Std) PG"}]
[null,null,"16164016","PROVENGER 1.5BIM 115-550L@6b FM/EN",{"$f":"_xlfn.XLOOKUP(C1152,DataSource!A:A,DataSource!AH:AH)","v":"1616 1.5 in BIM 115-550 6 BLACK (Std) PG"}]
[null,null,"16164035","PROVENGER 1.5ABX 30-150G@100P FM",{"$f":"_xlfn.XLOOKUP(C1153,DataSource!A:A,DataSource!AH:AH)","v":"1616 1.5 in ABX 30-150 100 (Std) BLACK (Std) PG"}]
[null,null,"16024010","PROVENGER 1.0\"NPSH 5-40G@75P",{"$f":"_xlfn.XLOOKUP(C1154,DataSource!A:A,DataSource!AH:AH)","v":"1602 1 in NPSH 5-40 75 BLACK (Std) PG"}]
[null,null,"16024007","PROVENGER 1.0\"NPSH 5-40G@100P",{"$f":"_xlfn.XLOOKUP(C1155,DataSource!A:A,DataSource!AH:AH)","v":"1602 1 in NPSH 5-40 100 (Std) BLACK (Std) PG"}]
[null,null,"16024005","PROVENGER 1.0\"NH 5-40G@75P",{"$f":"_xlfn.XLOOKUP(C1156,DataSource!A:A,DataSource!AH:AH)","v":"1602 1 in NH 5-40 75 BLACK (Std) PG"}]
[null,null,"16024006","PROVENGER 1.0\"NH 5-40G@100P#",{"$f":"_xlfn.XLOOKUP(C1157,DataSource!A:A,DataSource!AH:AH)","v":"1602 1 in NH 5-40 100 (Std) BLACK (Std) PG"}]
[null,null,"16024009","PROVENGER 1.0\"NH 12-53G@87P",{"$f":"_xlfn.XLOOKUP(C1158,DataSource!A:A,DataSource!AH:AH)","v":"1602 1 in NH 12-53 87 (CE) BLACK (Std) PG"}]
[null,null,"16024004","PROVENGER 1.0\"BSP 45-200LPM@6b EN",{"$f":"_xlfn.XLOOKUP(C1159,DataSource!A:A,DataSource!AH:AH)","v":"1602 1 in BSP 45-200 6 BLACK (Std) PG"}]
[null,null,"16024003","PROVENGER 1.0\"BSP 19-150LPM@7b",{"$f":"_xlfn.XLOOKUP(C1160,DataSource!A:A,DataSource!AH:AH)","v":"1602 1 in BSP 19-50 7 BLACK (Std) PG"}]
[null,null,"16024002","PROVENGER 1.0\"BSP 19-150LPM@6b EN",{"$f":"_xlfn.XLOOKUP(C1161,DataSource!A:A,DataSource!AH:AH)","v":"1602 1 in BSP 19-150 6 BLACK (Std) PG"}]
[null,null,"15284016","SBJT 75MM 1-1/8D",{"$f":"_xlfn.XLOOKUP(C1162,DataSource!A:A,DataSource!AH:AH)","v":"1528 3 in STORZ 135 1-1/8\" bore size(s) 100 (Std) BLACK (Std) PG"}]
[null,null,"15284014","SBJT 2.5NPSH 1-1/8D",{"$f":"_xlfn.XLOOKUP(C1163,DataSource!A:A,DataSource!AH:AH)","v":"1528 2.5 in NPSH 135 1-1/8\" bore size(s) 100 (Std) BLACK (Std) PG"}]
[null,null,"15284008","SBJT 2.5NH 1-1/8D",{"$f":"_xlfn.XLOOKUP(C1164,DataSource!A:A,DataSource!AH:AH)","v":"1528 2.5 in NH 135 1-1/8\" bore size(s) 100 (Std) BLACK (Std) PG"}]
[null,null,"15284007","SBJT 2.5JIM 1-1/8D",{"$f":"_xlfn.XLOOKUP(C1165,DataSource!A:A,DataSource!AH:AH)","v":"1528 2.5 in JIM 135 1-1/8\" bore size(s) 100 (Std) BLACK (Std) PG"}]
[null,null,"15284006","SBJT 2.5BSP 1-1/8D",{"$f":"_xlfn.XLOOKUP(C1166,DataSource!A:A,DataSource!AH:AH)","v":"1528 2.5 in BSP 135 1-1/8\" bore size(s) 100 (Std) BLACK (Std) PG"}]
[null,null,"15284005","SBJT 2.5BIM 1-1/8D",{"$f":"_xlfn.XLOOKUP(C1167,DataSource!A:A,DataSource!AH:AH)","v":"1528 2.5 in BIM 135 1-1/8\" bore size(s) 100 (Std) BLACK (Std) PG"}]
[null,null,"15284004","SBJT 2.5BAF 1-1/8D",{"$f":"_xlfn.XLOOKUP(C1168,DataSource!A:A,DataSource!AH:AH)","v":"1528 2.5 in BAT 135 1-1/8\" bore size(s) 100 (Std) BLACK (Std) PG"}]
[null,null,"15284015","SBJT 2.5AEA 1-1/8D",{"$f":"_xlfn.XLOOKUP(C1169,DataSource!A:A,DataSource!AH:AH)","v":"1528 2.5 in AEA 135 1-1/8\" bore size(s) 100 (Std) BLACK (Std) PG"}]
[null,null,"15284017","SBJT 2.5AEA 1-1/8D SPC AMA",{"$f":"_xlfn.XLOOKUP(C1170,DataSource!A:A,DataSource!AH:AH)","v":"1528 2.5 in AEA 135 1-1/8\" bore size(s) 100 (Std) BLACK (Std) PG"}]
[null,null,"15284013","SBJT 52MM 1-1/8D",{"$f":"_xlfn.XLOOKUP(C1171,DataSource!A:A,DataSource!AH:AH)","v":"1528 2 in STORZ 135 1-1/8\" bore size(s) 100 (Std) BLACK (Std) PG"}]
[null,null,"15284003","SBJT 1.5NPSH 1-1/8D",{"$f":"_xlfn.XLOOKUP(C1172,DataSource!A:A,DataSource!AH:AH)","v":"1528 1.5 in NPSH 135 1-1/8\" bore size(s) 100 (Std) BLACK (Std) PG"}]
[null,null,"15284012","SBJT ZT 1.5NH 1-1/8D",{"$f":"_xlfn.XLOOKUP(C1173,DataSource!A:A,DataSource!AH:AH)","v":"1528 1.5 in NH 135 1-1/8\" bore size(s) 100 (Std) BLACK (Std) PG ZT"}]
[null,null,"15284002","SBJT 1.5NH 1-1/8D",{"$f":"_xlfn.XLOOKUP(C1174,DataSource!A:A,DataSource!AH:AH)","v":"1528 1.5 in NH 135 1-1/8\" bore size(s) 100 (Std) BLACK (Std) PG"}]
[null,null,"15284001","SBJT 1.5BSP 1-1/8D",{"$f":"_xlfn.XLOOKUP(C1175,DataSource!A:A,DataSource!AH:AH)","v":"1528 1.5 in BSP 135 1-1/8\" bore size(s) 100 (Std) BLACK (Std) PG"}]
[null,null,"15234028","SBJT ZT 1.5NH 15/16D",{"$f":"_xlfn.XLOOKUP(C1176,DataSource!A:A,DataSource!AH:AH)","v":"1523 2.5 in NH 135 15/16\" bore size(s) 100 (Std) BLACK (Std) PG ZT"}]
[null,null,"15234023","SBJT 2.5NH 1D",{"$f":"_xlfn.XLOOKUP(C1177,DataSource!A:A,DataSource!AH:AH)","v":"1523 2.5 in NH 135 1\" bore size(s) 100 (Std) BLACK (Std) PG"}]
[null,null,"15234010","SBJT 65MM JIM 3/4D",{"$f":"_xlfn.XLOOKUP(C1178,DataSource!A:A,DataSource!AH:AH)","v":"1523 2.5 in JIM 135 3/4\" bore size(s) 100 (Std) BLACK (Std) PG"}]
[null,null,"15234022","SBJT ZT 65MM JIM 1D",{"$f":"_xlfn.XLOOKUP(C1179,DataSource!A:A,DataSource!AH:AH)","v":"1523 2.5 in JIM 135 1\" bore size(s) 100 (Std) BLACK (Std) PG ZT"}]
[null,null,"15234019","SBJT 65MM JIM 1D",{"$f":"_xlfn.XLOOKUP(C1180,DataSource!A:A,DataSource!AH:AH)","v":"1523 2.5 in JIM 135 1\" bore size(s) 100 (Std) BLACK (Std) PG"}]
[null,null,"15234009","SBJT 2.5BIM 7/8D",{"$f":"_xlfn.XLOOKUP(C1181,DataSource!A:A,DataSource!AH:AH)","v":"1523 2.5 in BIM 135 7/8\" bore size(s) 100 (Std) BLACK (Std) PG"}]
[null,null,"15234029","SBJT 2.5BIM 3/4D",{"$f":"_xlfn.XLOOKUP(C1182,DataSource!A:A,DataSource!AH:AH)","v":"1523 2.5 in BIM 135 3/4\" bore size(s) 100 (Std) BLACK (Std) PG"}]
[null,null,"15234025","SBJT 2.5BIM 1D",{"$f":"_xlfn.XLOOKUP(C1183,DataSource!A:A,DataSource!AH:AH)","v":"1523 2.5 in BIM 135 1\" bore size(s) 100 (Std) BLACK (Std) PG"}]
[null,null,"15234027","SBJT 38MM 15/16D",{"$f":"_xlfn.XLOOKUP(C1184,DataSource!A:A,DataSource!AH:AH)","v":"1523 1.5 in STORZ 135 15/16\" bore size(s) 100 (Std) BLACK (Std) PG"}]
[null,null,"15234007","SBJT 1.5NPSH 7/8D",{"$f":"_xlfn.XLOOKUP(C1185,DataSource!A:A,DataSource!AH:AH)","v":"1523 1.5 in NPSH 135 7/8\" bore size(s) 100 (Std) BLACK (Std) PG"}]
[null,null,"15234021","SBJT 1.5NPSH 3/4D",{"$f":"_xlfn.XLOOKUP(C1186,DataSource!A:A,DataSource!AH:AH)","v":"1523 1.5 in NPSH 135 3/4\" bore size(s) 100 (Std) BLACK (Std) PG"}]
[null,null,"15234008","SBJT 1.5NPSH 15/16D",{"$f":"_xlfn.XLOOKUP(C1187,DataSource!A:A,DataSource!AH:AH)","v":"1523 1.5 in NPSH 135 15/16\" bore size(s) 100 (Std) BLACK (Std) PG"}]
[null,null,"15234006","SBJT 1.5NPSH 1D",{"$f":"_xlfn.XLOOKUP(C1188,DataSource!A:A,DataSource!AH:AH)","v":"1523 1.5 in NPSH 135 1\" bore size(s) 100 (Std) BLACK (Std) PG"}]
[null,null,"15234004","SBJT 1.5NH 7/8D",{"$f":"_xlfn.XLOOKUP(C1189,DataSource!A:A,DataSource!AH:AH)","v":"1523 1.5 in NH 135 7/8\" bore size(s) 100 (Std) BLACK (Std) PG"}]
[null,null,"15234003","SBJT 1.5NH 3/4D",{"$f":"_xlfn.XLOOKUP(C1190,DataSource!A:A,DataSource!AH:AH)","v":"1523 1.5 in NH 135 3/4\" bore size(s) 100 (Std) BLACK (Std) PG"}]
[null,null,"15234024","SBJT 1.5NH 15/16D LENOLA",{"$f":"_xlfn.XLOOKUP(C1191,DataSource!A:A,DataSource!AH:AH)","v":"1523 1.5 in NH 135 15/16\" bore size(s) 100 (Std) BLACK (Std) PG ETCH"}]
[null,null,"15234005","SBJT 1.5NH 15/16D",{"$f":"_xlfn.XLOOKUP(C1192,DataSource!A:A,DataSource!AH:AH)","v":"1523 1.5 in NH 135 15/16\" bore size(s) 100 (Std) BLACK (Std) PG"}]
[null,null,"15234002","SBJT 1.5NH 1D",{"$f":"_xlfn.XLOOKUP(C1193,DataSource!A:A,DataSource!AH:AH)","v":"1523 1.5 in NH 135 1\" bore size(s) 100 (Std) BLACK (Std) PG"}]
[null,null,"15234001","SBJT 1.5BSP 3/4D",{"$f":"_xlfn.XLOOKUP(C1194,DataSource!A:A,DataSource!AH:AH)","v":"1523 1.5 in BSP 135 3/4\" bore size(s) 100 (Std) BLACK (Std) PG"}]
[null,null,"15234026","SBJT 1.5BSP 15/16D",{"$f":"_xlfn.XLOOKUP(C1195,DataSource!A:A,DataSource!AH:AH)","v":"1523 1.5 in BSP 135 15/16\" bore size(s) 100 (Std) BLACK (Std) PG"}]
[null,null,"15234020","SBJT 1.5BSP 1D",{"$f":"_xlfn.XLOOKUP(C1196,DataSource!A:A,DataSource!AH:AH)","v":"1523 1.5 in BSP 135 1\" bore size(s) 100 (Std) BLACK (Std) PG"}]
[null,null,"15204009","SBJT 2.5BIM 5/8 TIP 95G/360L",{"$f":"_xlfn.XLOOKUP(C1197,DataSource!A:A,DataSource!AH:AH)","v":"1520 2.5 in BIM 95 5/8\" bore size(s) 100 (Std) BLACK (Std) PG"}]
[null,null,"15204008","SBJT 52MM 1/2 TIP 95G/360L",{"$f":"_xlfn.XLOOKUP(C1198,DataSource!A:A,DataSource!AH:AH)","v":"1520 2 in STORZ 95 1/2\" bore size(s) 100 (Std) BLACK (Std) PG"}]
[null,null,"15204017","SBJT 38MM 1/2 TIP 95G/360L",{"$f":"_xlfn.XLOOKUP(C1199,DataSource!A:A,DataSource!AH:AH)","v":"1520 1.5 in STORZ 95 1/2\" bore size(s) 100 (Std) BLACK (Std) PG"}]
[null,null,"15204018","SBJT ZT 1.5NPSH 5/8 TIP 95G/360L",{"$f":"_xlfn.XLOOKUP(C1200,DataSource!A:A,DataSource!AH:AH)","v":"1520 1.5 in NPSH 95 5/8\" bore size(s) 100 (Std) BLACK (Std) PG ZT"}]
[null,null,"15204004","SBJT 1.5NPSH 5/8 TIP 95G/360L",{"$f":"_xlfn.XLOOKUP(C1201,DataSource!A:A,DataSource!AH:AH)","v":"1520 1.5 in NPSH 95 5/8\" bore size(s) 100 (Std) BLACK (Std) PG"}]
[null,null,"15204003","SBJT 1.5NPSH 1/2 TIP 95G/360L",{"$f":"_xlfn.XLOOKUP(C1202,DataSource!A:A,DataSource!AH:AH)","v":"1520 1.5 in NPSH 95 1/2\" bore size(s) 100 (Std) BLACK (Std) PG"}]
[null,null,"15204002","SBJT 1.5NH 5/8 TIP 95G/360L",{"$f":"_xlfn.XLOOKUP(C1203,DataSource!A:A,DataSource!AH:AH)","v":"1520 1.5 in NH 95 5/8\" bore size(s) 100 (Std) BLACK (Std) PG"}]
[null,null,"15204001","SBJT 1.5NH 1/2 TIP 95G/360L",{"$f":"_xlfn.XLOOKUP(C1204,DataSource!A:A,DataSource!AH:AH)","v":"1520 1.5 in NH 95 1/2\" bore size(s) 100 (Std) BLACK (Std) PG"}]
[null,null,"15204007","SBJT 1.5BSP 5/8 TIP 95G/360L",{"$f":"_xlfn.XLOOKUP(C1205,DataSource!A:A,DataSource!AH:AH)","v":"1520 1.5 in BSP 95 5/8\" bore size(s) 100 (Std) BLACK (Std) PG"}]
[null,null,"15204005","SBJT 1.5BSP 1/2 TIP 95G/360L",{"$f":"_xlfn.XLOOKUP(C1206,DataSource!A:A,DataSource!AH:AH)","v":"1520 1.5 in BSP 95 1/2\" bore size(s) 100 (Std) BLACK (Std) PG"}]
[null,null,"15204006","SBJT 1.5BSP M 1/2 TIP 95G/360L",{"$f":"_xlfn.XLOOKUP(C1207,DataSource!A:A,DataSource!AH:AH)","v":"1520 1.5 in BSP 95 1/2\" bore size(s) 100 (Std) BLACK (Std) PG"}]
[null,null,"14994029","TIP 1.5ABT 7/8D",{"$f":"_xlfn.XLOOKUP(C1208,DataSource!A:A,DataSource!AH:AH)","v":"1499 1.5 in PCT 7/8\" bore size(s) "}]
[null,null,"14994022","TIP 1.5ABT 1-1/8D",{"$f":"_xlfn.XLOOKUP(C1209,DataSource!A:A,DataSource!AH:AH)","v":"1499 1.5 in PCT 1-1/8\" bore size(s) "}]
[null,null,"14994039","TIP 1.5ABQ 1D",{"$f":"_xlfn.XLOOKUP(C1210,DataSource!A:A,DataSource!AH:AH)","v":"1499 1.5 in NYCORP 1\" bore size(s) "}]
[null,null,"14994027","TIP 1.5NPSH 7/8D KITTERY FIRE DEPT",{"$f":"_xlfn.XLOOKUP(C1211,DataSource!A:A,DataSource!AH:AH)","v":"1499 1.5 in NPSH 7/8\" bore size(s) ETCH"}]
[null,null,"14994002","TIP 1.5NPSH 7/8D",{"$f":"_xlfn.XLOOKUP(C1212,DataSource!A:A,DataSource!AH:AH)","v":"1499 1.5 in NPSH 7/8\" bore size(s) "}]
[null,null,"14994004","TIP 1.5NPSH 15/16D",{"$f":"_xlfn.XLOOKUP(C1213,DataSource!A:A,DataSource!AH:AH)","v":"1499 1.5 in NPSH 15/16\" bore size(s) "}]
[null,null,"14994016","TIP 1.5NPSH 1-3/8D",{"$f":"_xlfn.XLOOKUP(C1214,DataSource!A:A,DataSource!AH:AH)","v":"1499 1.5 in NPSH 1-3/8\" bore size(s) "}]
[null,null,"14994012","TIP 1.5NPSH 1-3/16D",{"$f":"_xlfn.XLOOKUP(C1215,DataSource!A:A,DataSource!AH:AH)","v":"1499 1.5 in NPSH 1-3/16\" bore size(s) "}]
[null,null,"14994010","TIP 1.5NPSH 1-1/8D",{"$f":"_xlfn.XLOOKUP(C1216,DataSource!A:A,DataSource!AH:AH)","v":"1499 1.5 in NPSH 1-1/8\" bore size(s) "}]
[null,null,"14994014","TIP 1.5NPSH 1-1/4D",{"$f":"_xlfn.XLOOKUP(C1217,DataSource!A:A,DataSource!AH:AH)","v":"1499 1.5 in NPSH 1-1/4\" bore size(s) "}]
[null,null,"14994008","TIP 1.5NPSH 1-1/16D",{"$f":"_xlfn.XLOOKUP(C1218,DataSource!A:A,DataSource!AH:AH)","v":"1499 1.5 in NPSH 1-1/16\" bore size(s) "}]
[null,null,"14994025","TIP 1.5NPSH 1D KITTERY FIRE DEPT",{"$f":"_xlfn.XLOOKUP(C1219,DataSource!A:A,DataSource!AH:AH)","v":"1499 1.5 in NPSH 1\" bore size(s) ETCH"}]
[null,null,"14994006","TIP 1.5NPSH 1D",{"$f":"_xlfn.XLOOKUP(C1220,DataSource!A:A,DataSource!AH:AH)","v":"1499 1.5 in NPSH 1\" bore size(s) "}]
[null,null,"14994020","TIP 1.5NH 7/8D CLEVELAND",{"$f":"_xlfn.XLOOKUP(C1221,DataSource!A:A,DataSource!AH:AH)","v":"1499 1.5 in NH 7/8\" bore size(s) ETCH"}]
[null,null,"14994033","TIP 1.5NH 7/8D WFD, E-31",{"$f":"_xlfn.XLOOKUP(C1222,DataSource!A:A,DataSource!AH:AH)","v":"1499 1.5 in NH 7/8\" bore size(s) ETCH"}]
[null,null,"14994034","TIP 1.5NH 7/8D SUMMERFIELD FD",{"$f":"_xlfn.XLOOKUP(C1223,DataSource!A:A,DataSource!AH:AH)","v":"1499 1.5 in NH 7/8\" bore size(s) ETCH"}]
[null,null,"14994049","TIP 1.5NH 7/8D SPC ETCH GPM/PSI",{"$f":"_xlfn.XLOOKUP(C1224,DataSource!A:A,DataSource!AH:AH)","v":"1499 1.5 in NH 7/8\" bore size(s) ETCH"}]
[null,null,"14994051","TIP 1.5NH 7/8D OCEAN VIEW FIRE CO",{"$f":"_xlfn.XLOOKUP(C1225,DataSource!A:A,DataSource!AH:AH)","v":"1499 1.5 in NH 7/8\" bore size(s) ETCH"}]
[null,null,"14994001","TIP 1.5NH 7/8D",{"$f":"_xlfn.XLOOKUP(C1226,DataSource!A:A,DataSource!AH:AH)","v":"1499 1.5 in NH 7/8\" bore size(s) "}]
[null,null,"14994017","TIP 1.5NH 15/16D DURHAM FIRE RESCUE",{"$f":"_xlfn.XLOOKUP(C1227,DataSource!A:A,DataSource!AH:AH)","v":"1499 1.5 in NH 15/16\" bore size(s) ETCH"}]
[null,null,"14994030","TIP 1.5NH 15/16D SPEC ETCH GPM/PSI",{"$f":"_xlfn.XLOOKUP(C1228,DataSource!A:A,DataSource!AH:AH)","v":"1499 1.5 in NH 15/16\" bore size(s) ETCH"}]
[null,null,"14994032","TIP 1.5NH 15/16D D.F.D.",{"$f":"_xlfn.XLOOKUP(C1229,DataSource!A:A,DataSource!AH:AH)","v":"1499 1.5 in NH 15/16\" bore size(s) ETCH"}]
[null,null,"14994037","TIP 1.5NH 15/16D ETCH SPC LOGO",{"$f":"_xlfn.XLOOKUP(C1230,DataSource!A:A,DataSource!AH:AH)","v":"1499 1.5 in NH 15/16\" bore size(s) ETCH"}]
[null,null,"14994040","TIP 1.5NH 15/16D  ETCH ENG80INE",{"$f":"_xlfn.XLOOKUP(C1231,DataSource!A:A,DataSource!AH:AH)","v":"1499 1.5 in NH 15/16\" bore size(s) ETCH"}]
[null,null,"14994043","TIP 1.5NH 15/16D CREEDMOOR FD",{"$f":"_xlfn.XLOOKUP(C1232,DataSource!A:A,DataSource!AH:AH)","v":"1499 1.5 in NH 15/16\" bore size(s) ETCH"}]
[null,null,"14994044","TIP 1.5NH 15/16D SEQ ETCH SB15-20-001",{"$f":"_xlfn.XLOOKUP(C1233,DataSource!A:A,DataSource!AH:AH)","v":"1499 1.5 in NH 15/16\" bore size(s) ETCH"}]
[null,null,"14994003","TIP 1.5NH 15/16D",{"$f":"_xlfn.XLOOKUP(C1234,DataSource!A:A,DataSource!AH:AH)","v":"1499 1.5 in NH 15/16\" bore size(s) "}]
[null,null,"14994015","TIP 1.5NH 1-3/8D#",{"$f":"_xlfn.XLOOKUP(C1235,DataSource!A:A,DataSource!AH:AH)","v":"1499 1.5 in NH 1-3/8\" bore size(s) "}]
[null,null,"14994018","TIP 1.5NH 1-3/16D DURHAM FIRE RESCUE",{"$f":"_xlfn.XLOOKUP(C1236,DataSource!A:A,DataSource!AH:AH)","v":"1499 1.5 in NH 1-3/16\" bore size(s) ETCH"}]
[null,null,"14994023","TIP 1.5NH 1-3/16D SPEC ETCH GPM/PSI",{"$f":"_xlfn.XLOOKUP(C1237,DataSource!A:A,DataSource!AH:AH)","v":"1499 1.5 in NH 1-3/16\" bore size(s) ETCH"}]
[null,null,"14994036","TIP 1.5NH 1-3/16D CHARLOTTE FD",{"$f":"_xlfn.XLOOKUP(C1238,DataSource!A:A,DataSource!AH:AH)","v":"1499 1.5 in NH 1-3/16\" bore size(s) ETCH"}]
[null,null,"14994041","TIP 1.5NH 1-3/16D ETCH ENG80INE",{"$f":"_xlfn.XLOOKUP(C1239,DataSource!A:A,DataSource!AH:AH)","v":"1499 1.5 in NH 1-3/16\" bore size(s) ETCH"}]
[null,null,"14994042","TIP 1.5NH 1-3/16D CREEDMOOR FD",{"$f":"_xlfn.XLOOKUP(C1240,DataSource!A:A,DataSource!AH:AH)","v":"1499 1.5 in NH 1-3/16\" bore size(s) ETCH"}]
[null,null,"14994011","TIP 1.5NH 1-3/16D",{"$f":"_xlfn.XLOOKUP(C1241,DataSource!A:A,DataSource!AH:AH)","v":"1499 1.5 in NH 1-3/16\" bore size(s) "}]
[null,null,"14994019","TIP 1.5NH 1-1/8D DURHAM FIRE RESCUE",{"$f":"_xlfn.XLOOKUP(C1242,DataSource!A:A,DataSource!AH:AH)","v":"1499 1.5 in NH 1-1/8\" bore size(s) ETCH"}]
[null,null,"14994024","TIP 1.5NH 1-1/8D RICHMOND FD",{"$f":"_xlfn.XLOOKUP(C1243,DataSource!A:A,DataSource!AH:AH)","v":"1499 1.5 in NH 1-1/8\" bore size(s) ETCH"}]
[null,null,"14994028","TIP 1.5NH 1-1/8D ENO FD",{"$f":"_xlfn.XLOOKUP(C1244,DataSource!A:A,DataSource!AH:AH)","v":"1499 1.5 in NH 1-1/8\" bore size(s) ETCH"}]
[null,null,"14994035","TIP 1.5NH 1-1/8D SUMMERFIELD FD",{"$f":"_xlfn.XLOOKUP(C1245,DataSource!A:A,DataSource!AH:AH)","v":"1499 1.5 in NH 1-1/8\" bore size(s) ETCH"}]
[null,null,"14994009","TIP 1.5NH 1-1/8D",{"$f":"_xlfn.XLOOKUP(C1246,DataSource!A:A,DataSource!AH:AH)","v":"1499 1.5 in NH 1-1/8\" bore size(s) "}]
[null,null,"14994013","TIP 1.5NH 1-1/4D",{"$f":"_xlfn.XLOOKUP(C1247,DataSource!A:A,DataSource!AH:AH)","v":"1499 1.5 in NH 1-1/4\" bore size(s) "}]
[null,null,"14994031","TIP 1.5NH 1-1/16D D.F.D.",{"$f":"_xlfn.XLOOKUP(C1248,DataSource!A:A,DataSource!AH:AH)","v":"1499 1.5 in NH 1-1/16\" bore size(s) ETCH"}]
[null,null,"14994007","TIP 1.5NH 1-1/16D",{"$f":"_xlfn.XLOOKUP(C1249,DataSource!A:A,DataSource!AH:AH)","v":"1499 1.5 in NH 1-1/16\" bore size(s) "}]
[null,null,"14994005","TIP 1.5NH 1D#",{"$f":"_xlfn.XLOOKUP(C1250,DataSource!A:A,DataSource!AH:AH)","v":"1499 1.5 in NH 1\" bore size(s) "}]
[null,null,"14994021","TIP 1.5ABU 1-1/16D",{"$f":"_xlfn.XLOOKUP(C1251,DataSource!A:A,DataSource!AH:AH)","v":"1499 1.5 in FDNY 1-1/16\" bore size(s) "}]
[null,null,"14994026","TIP 1.5BSP 7/8D (22MM)",{"$f":"_xlfn.XLOOKUP(C1252,DataSource!A:A,DataSource!AH:AH)","v":"1499 1.5 in BSP 7/8\" bore size(s) "}]
[null,null,"14994038","TIP 1.5 ABX 15/16D",{"$f":"_xlfn.XLOOKUP(C1253,DataSource!A:A,DataSource!AH:AH)","v":"1499 1.5 in ABX 15/16\" bore size(s) "}]
[null,null,"14464004","SH/O TIP 2.5AEF X 1.5NH 1-3/8",{"$f":"_xlfn.XLOOKUP(C1254,DataSource!A:A,DataSource!AH:AH)","v":"1446 2.5 in NYCORP 1.5 in NH 1-3/8\" bore size(s) PG"}]
[null,null,"14464012","SH/O TIP 2.5AEF X 1.5NH 1-1/8",{"$f":"_xlfn.XLOOKUP(C1255,DataSource!A:A,DataSource!AH:AH)","v":"1446 2.5 in NYCORP 1.5 in NH 1-1/8\" bore size(s) PG"}]
[null,null,"14464014","SH/O TIP 2.5NPSH X 1.5NPSH 1-1/8",{"$f":"_xlfn.XLOOKUP(C1256,DataSource!A:A,DataSource!AH:AH)","v":"1446 2.5 in NPSH 1.5 in NPSH 1-1/8\" bore size(s) PG"}]
[null,null,"14467014","SH/O NPG TIP 2.5NPSH X 1.5NPSH 1-1/8",{"$f":"_xlfn.XLOOKUP(C1257,DataSource!A:A,DataSource!AH:AH)","v":"1446 2.5 in NPSH 1.5 in NPSH 1-1/8\" bore size(s) NPG"}]
[null,null,"14464007","SH/O TIP 2.5NH X 1.5NPSH 1-1/8",{"$f":"_xlfn.XLOOKUP(C1258,DataSource!A:A,DataSource!AH:AH)","v":"1446 2.5 in NH 1.5 in NPSH 1-1/8\" bore size(s) PG"}]
[null,null,"14464018","SH/O TIP 2.5NH X 1.5NH 7/8\" D",{"$f":"_xlfn.XLOOKUP(C1259,DataSource!A:A,DataSource!AH:AH)","v":"1446 2.5 in NH 1.5 in NH 7/8\" bore size(s) PG"}]
[null,null,"14464002","SH/O TIP 2.5NH X 1.5NH 15/16",{"$f":"_xlfn.XLOOKUP(C1260,DataSource!A:A,DataSource!AH:AH)","v":"1446 2.5 in NH 1.5 in NH 15/16\" bore size(s) PG"}]
[null,null,"14464001","SH/O TIP 2.5NH X 1.5NH 1-3/8",{"$f":"_xlfn.XLOOKUP(C1261,DataSource!A:A,DataSource!AH:AH)","v":"1446 2.5 in NH 1.5 in NH 1-3/8\" bore size(s) PG"}]
[null,null,"14464008","SH/O TIP 2.5NH X 1.5NH 1-3/16",{"$f":"_xlfn.XLOOKUP(C1262,DataSource!A:A,DataSource!AH:AH)","v":"1446 2.5 in NH 1.5 in NH 1-3/16\" bore size(s) PG"}]
[null,null,"14464005","SH/O TIP 2.5NH X 1.5NH 1-1/8",{"$f":"_xlfn.XLOOKUP(C1263,DataSource!A:A,DataSource!AH:AH)","v":"1446 2.5 in NH 1.5 in NH 1-1/8\" bore size(s) PG"}]
[null,null,"14464003","SH/O TIP 2.5NH X 1.5NH 1-1/4",{"$f":"_xlfn.XLOOKUP(C1264,DataSource!A:A,DataSource!AH:AH)","v":"1446 2.5 in NH 1.5 in NH 1-1/4\" bore size(s) PG"}]
[null,null,"14464017","SH/O TIP 2.5NH X 1.5NH 1\" D",{"$f":"_xlfn.XLOOKUP(C1265,DataSource!A:A,DataSource!AH:AH)","v":"1446 2.5 in NH 1.5 in NH 1\" bore size(s) PG"}]
[null,null,"14465000","NOZ SH/O PG  2.5JIMX1.5NH  7/8  CCCF",{"$f":"_xlfn.XLOOKUP(C1266,DataSource!A:A,DataSource!AH:AH)","v":"1446 2.5 in JIM 1.5 in NH 7/8\" bore size(s) PGETCH"}]
[null,null,"14464006","SH/O TIP 2.5AII X 1.5NPSH 1-3/8",{"$f":"_xlfn.XLOOKUP(C1267,DataSource!A:A,DataSource!AH:AH)","v":"1446 2.5 in CSA 1.5 in NPSH 1-3/8\" bore size(s) PG"}]
[null,null,"14464016","SH/O TIP 2.5AII X 1.5NPSH 1-1/8 D",{"$f":"_xlfn.XLOOKUP(C1268,DataSource!A:A,DataSource!AH:AH)","v":"1446 2.5 in CSA 1.5 in NPSH 1-1/8\" bore size(s) PG"}]
[null,null,"14464011","SH/O TIP 2.5AII X 1.5NPSH 1-1/4 D",{"$f":"_xlfn.XLOOKUP(C1269,DataSource!A:A,DataSource!AH:AH)","v":"1446 2.5 in CSA 1.5 in NPSH 1-1/4\" bore size(s) PG"}]
[null,null,"14464015","SH/O TIP 2.5BAF X 1.5NPSH 1-3/8",{"$f":"_xlfn.XLOOKUP(C1270,DataSource!A:A,DataSource!AH:AH)","v":"1446 2.5 in BAT 1.5 in NPSH 1-3/8\" bore size(s) PG"}]
[null,null,"14464010","SH/O TIP 2.5BAF X 1.5NPSH 1-1/8",{"$f":"_xlfn.XLOOKUP(C1271,DataSource!A:A,DataSource!AH:AH)","v":"1446 2.5 in BAT 1.5 in NPSH 1-1/8\" bore size(s) PG"}]
[null,null,"14464013","SH/O TIP 2.5AJZ X 1.5NH 1-3/8",{"$f":"_xlfn.XLOOKUP(C1272,DataSource!A:A,DataSource!AH:AH)","v":"1446 2.5 in AJZ 1.5 in NH 1-3/8\" bore size(s) PG"}]
[null,null,"14464009","SH/O TIP 2.5AHB X 1.5NH 1-1/4",{"$f":"_xlfn.XLOOKUP(C1273,DataSource!A:A,DataSource!AH:AH)","v":"1446 2.5 in AHB 1.5 in NH 1-1/4\" bore size(s) PG"}]
[null,null,"14454007","SH/O TIP 1.5NPSH X 1.5NPSH 7/8",{"$f":"_xlfn.XLOOKUP(C1274,DataSource!A:A,DataSource!AH:AH)","v":"1445 1.5 in NPSH 1.5 in NPSH 7/8\" bore size(s) PG"}]
[null,null,"14454006","SH/O TIP 1.5NPSH X 1.5NPSH 15/16",{"$f":"_xlfn.XLOOKUP(C1275,DataSource!A:A,DataSource!AH:AH)","v":"1445 1.5 in NPSH 1.5 in NPSH 15/16\" bore size(s) PG"}]
[null,null,"14454004","SH/O TIP 1.5NPSH X 1.5NPSH 1-3/8",{"$f":"_xlfn.XLOOKUP(C1276,DataSource!A:A,DataSource!AH:AH)","v":"1445 1.5 in NPSH 1.5 in NPSH 1-3/8\" bore size(s) PG"}]
[null,null,"14454002","SH/O TIP 1.5NH X 1.5NH 7/8",{"$f":"_xlfn.XLOOKUP(C1277,DataSource!A:A,DataSource!AH:AH)","v":"1445 1.5 in NH 1.5 in NH 7/8\" bore size(s) PG"}]
[null,null,"14457002","SH/O NPG TIP 1.5NH X 1.5NH 7/8",{"$f":"_xlfn.XLOOKUP(C1278,DataSource!A:A,DataSource!AH:AH)","v":"1445 1.5 in NH 1.5 in NH 7/8\" bore size(s) NPG"}]
[null,null,"14454009","SH/O TIP 1.5NH X 1.5NH 1-1/16 SEQ ETCH",{"$f":"_xlfn.XLOOKUP(C1279,DataSource!A:A,DataSource!AH:AH)","v":"1445 1.5 in NH 1.5 in NH 15/16\" bore size(s) PGETCH"}]
[null,null,"14454003","SH/O TIP 1.5NH X 1.5NH 15/16",{"$f":"_xlfn.XLOOKUP(C1280,DataSource!A:A,DataSource!AH:AH)","v":"1445 1.5 in NH 1.5 in NH 15/16\" bore size(s) PG"}]
[null,null,"14454001","SH/O TIP 1.5NH X 1.5NH 1-3/8",{"$f":"_xlfn.XLOOKUP(C1281,DataSource!A:A,DataSource!AH:AH)","v":"1445 1.5 in NH 1.5 in NH 1-3/8\" bore size(s) PG"}]
[null,null,"14457001","SH/O NPG TIP 1.5NH X 1.5NH 1-3/8",{"$f":"_xlfn.XLOOKUP(C1282,DataSource!A:A,DataSource!AH:AH)","v":"1445 1.5 in NH 1.5 in NH 1-3/8\" bore size(s) NPG"}]
[null,null,"14454005","SH/O TIP 1.5NH X 1.5NH 1-1/8",{"$f":"_xlfn.XLOOKUP(C1283,DataSource!A:A,DataSource!AH:AH)","v":"1445 1.5 in NH 1.5 in NH 1-1/8\" bore size(s) PG"}]
[null,null,"14454008","SH/O TIP 1.5NH X 1.5NH 1",{"$f":"_xlfn.XLOOKUP(C1284,DataSource!A:A,DataSource!AH:AH)","v":"1445 1.5 in NH 1.5 in NH 1\" bore size(s) PG"}]
[null,null,"14434006","SH/O TIP 2.5AEF X 1.5NPSH 1-1/8&1/2",{"$f":"_xlfn.XLOOKUP(C1285,DataSource!A:A,DataSource!AH:AH)","v":"1443 2.5 in NYCORP 1.5 in NPSH 1-1/8\"; 1/2\" bore size(s) PG"}]
[null,null,"14434007","SH/O TIP 2.5AEFX1.5NPSH 1-1/8&1/2 MTLHDL",{"$f":"_xlfn.XLOOKUP(C1286,DataSource!A:A,DataSource!AH:AH)","v":"1443 2.5 in NYCORP 1.5 in NPSH 1-1/8\"; 1/2\" bore size(s) PG"}]
[null,null,"14437005","SH/O NPG TIP2.5AEFX1.5NPSH1-1/8&1/2MTLHD",{"$f":"_xlfn.XLOOKUP(C1287,DataSource!A:A,DataSource!AH:AH)","v":"1443 2.5 in NYCORP 1.5 in NPSH 1-1/8\"; 1/2\" bore size(s) NPG"}]
[null,null,"14434002","SH/O TIP 2.5AEF X 1.5NH 1-1/8&1/2",{"$f":"_xlfn.XLOOKUP(C1288,DataSource!A:A,DataSource!AH:AH)","v":"1443 2.5 in NYCORP 1.5 in NH 1-1/8\"; 1/2\" bore size(s) PG"}]
[null,null,"14434004","SH/O TIP 2.5AEF X 1.5NH 1-1/8&1/2 MTLHDL",{"$f":"_xlfn.XLOOKUP(C1289,DataSource!A:A,DataSource!AH:AH)","v":"1443 2.5 in NYCORP 1.5 in NH 1-1/8\"; 1/2\" bore size(s) PG"}]
[null,null,"14437002","SH/O NPG TIP 2.5AEF X 1.5NH 1-1/8&1/2",{"$f":"_xlfn.XLOOKUP(C1290,DataSource!A:A,DataSource!AH:AH)","v":"1443 2.5 in NYCORP 1.5 in NH 1-1/8\"; 1/2\" bore size(s) NPG"}]
[null,null,"14434005","SH/O TIP 2.5NPSH X 1.5NPSH 1-1/8&1/2",{"$f":"_xlfn.XLOOKUP(C1291,DataSource!A:A,DataSource!AH:AH)","v":"1443 2.5 in NPSH 1.5 in NPSH 1-1/8\"; 1/2\" bore size(s) PG"}]
[null,null,"14434008","SH/O TIP 2.5NH X 1.5NPSH 1-1/8&1/2",{"$f":"_xlfn.XLOOKUP(C1292,DataSource!A:A,DataSource!AH:AH)","v":"1443 2.5 in NH 1.5 in NPSH 1-1/8\"; 1/2\" bore size(s) PG"}]
[null,null,"14434001","SH/O TIP 2.5NH X 1.5NH 1-1/8&1/2",{"$f":"_xlfn.XLOOKUP(C1293,DataSource!A:A,DataSource!AH:AH)","v":"1443 2.5 in NH 1.5 in NH 1-1/8\"; 1/2\" bore size(s) PG"}]
[null,null,"14437001","SH/O NPG TIP 2.5NH X 1.5NH 1-1/8&1/2",{"$f":"_xlfn.XLOOKUP(C1294,DataSource!A:A,DataSource!AH:AH)","v":"1443 2.5 in NH 1.5 in NH 1-1/8\"; 1/2\" bore size(s) NPG"}]
[null,null,"14437004","SH/O NPG 2.5NH X 1.5NH 1-1/8&1/2 MTLHDL",{"$f":"_xlfn.XLOOKUP(C1295,DataSource!A:A,DataSource!AH:AH)","v":"1443 2.5 in NH 1.5 in NH 1-1/8\"; 1/2\" bore size(s) NPG"}]
[null,null,"14430022","SH/O TIP PG 2.5 FB X1.5 ABU 1 1/8&1/2",{"$f":"_xlfn.XLOOKUP(C1296,DataSource!A:A,DataSource!AH:AH)","v":"1443 2.5 in FDNY 1.5 in FDNY 1-1/8\"; 1/2\" bore size(s) PG"}]
[null,null,"14434003","SH/O TIP 2.5AFB X 1.5ABU 1-1/8&1/2",{"$f":"_xlfn.XLOOKUP(C1297,DataSource!A:A,DataSource!AH:AH)","v":"1443 2.5 in FDNY 1.5 in FDNY 1-1/8\"; 1/2\" bore size(s) PG"}]
[null,null,"14437003","SH/O NPG TIP 2.5AFB X 1.5ABU 1-1/8&1/2",{"$f":"_xlfn.XLOOKUP(C1298,DataSource!A:A,DataSource!AH:AH)","v":"1443 2.5 in FDNY 1.5 in FDNY 1-1/8\"; 1/2\" bore size(s) NPG"}]
[null,null,"14420003","SH/O TIPS 2.5FDNY X 1.5FDNY    1 1/8&1/2",{"$f":"_xlfn.XLOOKUP(C1299,DataSource!A:A,DataSource!AH:AH)","v":"1442 2.5 in FDNY 1.5 in FDNY 1-1/8\"; 1/2\" bore size(s) NPG"}]
[null,null,"14414006","SH/O TIP 1.5ABQ X 1.5ABQ 15/16&1/2",{"$f":"_xlfn.XLOOKUP(C1300,DataSource!A:A,DataSource!AH:AH)","v":"1441 1.5 in NYCORP 1.5 in NYCORP 15/16\"; 1/2\" bore size(s) PG"}]
[null,null,"14414004","SH/O TIP 1.5NPSH X 1.5NPSH 15/16&1/2",{"$f":"_xlfn.XLOOKUP(C1301,DataSource!A:A,DataSource!AH:AH)","v":"1441 1.5 in NPSH 1.5 in NPSH 15/16\"; 1/2\" bore size(s) PG"}]
[null,null,"14414007","SH/O TIP 1.5NPSHX1.5NPSH15/16&1/2 MTLHDL",{"$f":"_xlfn.XLOOKUP(C1302,DataSource!A:A,DataSource!AH:AH)","v":"1441 1.5 in NPSH 1.5 in NPSH 15/16\"; 1/2\" bore size(s) PG"}]
[null,null,"14414001","SH/O TIP 1.5NH X 1.5NH 15/16&1/2",{"$f":"_xlfn.XLOOKUP(C1303,DataSource!A:A,DataSource!AH:AH)","v":"1441 1.5 in NH 1.5 in NH 15/16\"; 1/2\" bore size(s) PG"}]
[null,null,"14414005","SH/O TIP 1.5NH X 1.5NH 15/16&1/2 MTL HDL",{"$f":"_xlfn.XLOOKUP(C1304,DataSource!A:A,DataSource!AH:AH)","v":"1441 1.5 in NH 1.5 in NH 15/16\"; 1/2\" bore size(s) PG"}]
[null,null,"14417001","SH/O NPG MTLHDL TIP 1.5NHXNH 15/16&1/2",{"$f":"_xlfn.XLOOKUP(C1305,DataSource!A:A,DataSource!AH:AH)","v":"1441 1.5 in NH 1.5 in NH 15/16\"; 1/2\" bore size(s) NPG"}]
[null,null,"14417002","SH/O NPG TIP 1.5NHX1.5NH 15/16&1/2",{"$f":"_xlfn.XLOOKUP(C1306,DataSource!A:A,DataSource!AH:AH)","v":"1441 1.5 in NH 1.5 in NH 15/16\"; 1/2\" bore size(s) NPG"}]
[null,null,"14410010","SH/O TIP PG 1.5 ABU X1.5ABU 15/16&1/2",{"$f":"_xlfn.XLOOKUP(C1307,DataSource!A:A,DataSource!AH:AH)","v":"1441 1.5 in FDNY 1.5 in FDNY 15/16\"; 1/2\" bore size(s) PG"}]
[null,null,"14414002","SH/O TIP 1.5ABU X 1.5ABU 15/16&1/2",{"$f":"_xlfn.XLOOKUP(C1308,DataSource!A:A,DataSource!AH:AH)","v":"1441 1.5 in FDNY 1.5 in FDNY 15/16\"; 1/2\" bore size(s) PG"}]
[null,null,"14417003","SH/O NPG TIP 1.5ABU X 1.5ABU 15/16&1/2",{"$f":"_xlfn.XLOOKUP(C1309,DataSource!A:A,DataSource!AH:AH)","v":"1441 1.5 in FDNY 1.5 in FDNY 15/16\"; 1/2\" bore size(s) NPG"}]
[null,null,"14400004","SH/O TIPS 1.5FDNY X 1.5FDNY ABUABU",{"$f":"_xlfn.XLOOKUP(C1310,DataSource!A:A,DataSource!AH:AH)","v":"1440 1.5 in FDNY 1.5 in FDNY 15/16\"; 1/2\" bore size(s) PG"}]
[null,null,"14204002","TIP TRIPLE STK 1.5NPSH 1,1-1/8,1-1/4",{"$f":"_xlfn.XLOOKUP(C1311,DataSource!A:A,DataSource!AH:AH)","v":"1420 1.5 in NPSH 1.5 in NH 1-1/4\"; 1-1/8\"; 1\" bore size(s) "}]
[null,null,"14204004","TIP TRI STK 1.5NH 1,1-1/8,1-1/4 DURHAM",{"$f":"_xlfn.XLOOKUP(C1312,DataSource!A:A,DataSource!AH:AH)","v":"1420 1.5 in NH 1.5 in NH 1-1/4\"; 1-1/8\"; 1\" bore size(s) ETCH"}]
[null,null,"14204006","TIP TRISTK 1.5NH 1,1-1/8,1-1/4UNIONVILLE",{"$f":"_xlfn.XLOOKUP(C1313,DataSource!A:A,DataSource!AH:AH)","v":"1420 1.5 in NH 1.5 in NH 1-1/4\"; 1-1/8\"; 1\" bore size(s) ETCH"}]
[null,null,"14204007","TIP TRI STK 1.5NH 1,1-1/8,1-1/4 SACO FD",{"$f":"_xlfn.XLOOKUP(C1314,DataSource!A:A,DataSource!AH:AH)","v":"1420 1.5 in NH 1.5 in NH 1-1/4\"; 1-1/8\"; 1\" bore size(s) ETCH"}]
[null,null,"14204009","TIP TRIPLE STK 1.5NH 1,1-1/8,1-1/4 BDVFD",{"$f":"_xlfn.XLOOKUP(C1315,DataSource!A:A,DataSource!AH:AH)","v":"1420 1.5 in NH 1.5 in NH 1-1/4\"; 1-1/8\"; 1\" bore size(s) ETCH"}]
[null,null,"14204010","TIP TRI STK 1.5NH 1,1-1/8,1-1/4 D.C.F.D",{"$f":"_xlfn.XLOOKUP(C1316,DataSource!A:A,DataSource!AH:AH)","v":"1420 1.5 in NH 1.5 in NH 1-1/4\"; 1-1/8\"; 1\" bore size(s) ETCH"}]
[null,null,"14204001","TIP TRIPLE STK 1.5NH 1,1-1/8,1-1/4#",{"$f":"_xlfn.XLOOKUP(C1317,DataSource!A:A,DataSource!AH:AH)","v":"1420 1.5 in NH 1.5 in NH 1-1/4\"; 1-1/8\"; 1\" bore size(s) "}]
[null,null,"14204003","TIP TRIPLE STK 1.5BSP 1,1-1/8,1-1/4",{"$f":"_xlfn.XLOOKUP(C1318,DataSource!A:A,DataSource!AH:AH)","v":"1420 1.5 in BSP 1.5 in NH 1-1/4\"; 1-1/8\"; 1\" bore size(s) ETCH"}]
[null,null,"14174005","TIP PLAIN 1.5NPSH 7/8D",{"$f":"_xlfn.XLOOKUP(C1319,DataSource!A:A,DataSource!AH:AH)","v":"1417 1.5 in NPSH 7/8\" bore size(s) "}]
[null,null,"14174019","TIP PLAIN 1.5NPSH 3/8D",{"$f":"_xlfn.XLOOKUP(C1320,DataSource!A:A,DataSource!AH:AH)","v":"1417 1.5 in NPSH 3/8\" bore size(s) "}]
[null,null,"14174007","TIP PLAIN 1.5NPSH 15/16D",{"$f":"_xlfn.XLOOKUP(C1321,DataSource!A:A,DataSource!AH:AH)","v":"1417 1.5 in NPSH 15/16\" bore size(s) "}]
[null,null,"14174010","TIP PLAIN 1.5NPSH 1-1/8D",{"$f":"_xlfn.XLOOKUP(C1322,DataSource!A:A,DataSource!AH:AH)","v":"1417 1.5 in NPSH 1-1/8\" bore size(s) "}]
[null,null,"14174012","TIP PLAIN 1.5NPSH 1/2D",{"$f":"_xlfn.XLOOKUP(C1323,DataSource!A:A,DataSource!AH:AH)","v":"1417 1.5 in NPSH 1/2\" bore size(s) "}]
[null,null,"14174018","TIP PLAIN 1.5NPSH 1D",{"$f":"_xlfn.XLOOKUP(C1324,DataSource!A:A,DataSource!AH:AH)","v":"1417 1.5 in NPSH 1\" bore size(s) "}]
[null,null,"14174013","TIP PLAIN 1.5NH 7/8D RICHMOND FD",{"$f":"_xlfn.XLOOKUP(C1325,DataSource!A:A,DataSource!AH:AH)","v":"1417 1.5 in NH 7/8\" bore size(s) ETCH"}]
[null,null,"14174004","TIP PLAIN 1.5NH 7/8D#",{"$f":"_xlfn.XLOOKUP(C1326,DataSource!A:A,DataSource!AH:AH)","v":"1417 1.5 in NH 7/8\" bore size(s) "}]
[null,null,"14174001","TIP PLAIN 1.5NH 3/8D",{"$f":"_xlfn.XLOOKUP(C1327,DataSource!A:A,DataSource!AH:AH)","v":"1417 1.5 in NH 3/8\" bore size(s) "}]
[null,null,"14174003","TIP PLAIN 1.5NH 3/4D",{"$f":"_xlfn.XLOOKUP(C1328,DataSource!A:A,DataSource!AH:AH)","v":"1417 1.5 in NH 3/4\" bore size(s) "}]
[null,null,"14174006","TIP PLAIN 1.5NH 15/16D#",{"$f":"_xlfn.XLOOKUP(C1329,DataSource!A:A,DataSource!AH:AH)","v":"1417 1.5 in NH 15/16\" bore size(s) "}]
[null,null,"14174014","TIP PLAIN 1.5NH 1-1/8D ETCH N1594",{"$f":"_xlfn.XLOOKUP(C1330,DataSource!A:A,DataSource!AH:AH)","v":"1417 1.5 in NH 1-1/8\" bore size(s) ETCH"}]
[null,null,"14174015","TIP PLAIN 1.5NH 1-1/8D ETCH N1595",{"$f":"_xlfn.XLOOKUP(C1331,DataSource!A:A,DataSource!AH:AH)","v":"1417 1.5 in NH 1-1/8\" bore size(s) ETCH"}]
[null,null,"14174016","TIP PLAIN 1.5NH 1-1/8D ETCH N1597",{"$f":"_xlfn.XLOOKUP(C1332,DataSource!A:A,DataSource!AH:AH)","v":"1417 1.5 in NH 1-1/8\" bore size(s) ETCH"}]
[null,null,"14174017","TIP PLAIN 1.5NH 1-1/8D ETCH N1598",{"$f":"_xlfn.XLOOKUP(C1333,DataSource!A:A,DataSource!AH:AH)","v":"1417 1.5 in NH 1-1/8\" bore size(s) ETCH"}]
[null,null,"14174009","TIP PLAIN 1.5NH 1-1/8D#",{"$f":"_xlfn.XLOOKUP(C1334,DataSource!A:A,DataSource!AH:AH)","v":"1417 1.5 in NH 1-1/8\" bore size(s) "}]
[null,null,"14174002","TIP PLAIN 1.5NH 1/2D",{"$f":"_xlfn.XLOOKUP(C1335,DataSource!A:A,DataSource!AH:AH)","v":"1417 1.5 in NH 1/2\" bore size(s) "}]
[null,null,"14174011","TIP PLAIN 1.5NH 1D FINLEYFIRE.COM",{"$f":"_xlfn.XLOOKUP(C1336,DataSource!A:A,DataSource!AH:AH)","v":"1417 1.5 in NH 1\" bore size(s) ETCH"}]
[null,null,"14174008","TIP PLAIN 1.5NH 1D",{"$f":"_xlfn.XLOOKUP(C1337,DataSource!A:A,DataSource!AH:AH)","v":"1417 1.5 in NH 1\" bore size(s) "}]
[null,null,"14174020","TIP PLAIN 1.5BSP 3/4D",{"$f":"_xlfn.XLOOKUP(C1338,DataSource!A:A,DataSource!AH:AH)","v":"1417 1.5 in BSP 3/4\" bore size(s) "}]
[null,null,"11250002","SHUTOFF 1.5 NPSH F X 1.5 NPSH M CS",{"$f":"_xlfn.XLOOKUP(C1339,DataSource!A:A,DataSource!AH:AH)","v":"1125 1.5 in NPSH 1.5 in NPSH NPG"}]
[null,null,"11250001","SHUTOFF 1.5 NH F X 1.5 NH M CS #",{"$f":"_xlfn.XLOOKUP(C1340,DataSource!A:A,DataSource!AH:AH)","v":"1125 1.5 in NH 1.5 in NH NPG"}]
[null,null,"07530009","SHUTOFF 1.0NPSHX1.5NPSH 1HR W/BMPR",{"$f":"_xlfn.XLOOKUP(C1341,DataSource!A:A,DataSource!AH:AH)","v":"0753 1 in NPSH 1.5 in NPSH PG"}]
[null,null,"07530007","SHUTOFF 1.0NPSHX1.5\"NH IHR W/BMPR",{"$f":"_xlfn.XLOOKUP(C1342,DataSource!A:A,DataSource!AH:AH)","v":"0753 1 in NPSH 1.5 in NH PG"}]
[null,null,"07530006","SHUTOFF 1.0NHX1.5NPSH IHR W/BUMPER",{"$f":"_xlfn.XLOOKUP(C1343,DataSource!A:A,DataSource!AH:AH)","v":"0753 1 in NH 1.5 in NPSH PG"}]
[null,null,"07530003","SHUTOFF 1\"NHX1.5NH IHR W/BUMPER",{"$f":"_xlfn.XLOOKUP(C1344,DataSource!A:A,DataSource!AH:AH)","v":"0753 1 in NH 1.5 in NH PG"}]
[null,null,"07530010","SHUTOFF 1.0BSPX1.5NH IHR W/BMPR",{"$f":"_xlfn.XLOOKUP(C1345,DataSource!A:A,DataSource!AH:AH)","v":"0753 1 in BSP 1.5 in NH PG"}]
[null,null,"07530001","SHUTOFF 1\"BSPX1.5BSP W/BMP IHR #",{"$f":"_xlfn.XLOOKUP(C1346,DataSource!A:A,DataSource!AH:AH)","v":"0753 1 in BSP 1.5 in BSP PG"}]
[null,null,"07533000","SHUTOFF 1\"BSPX1.5BSP W/BMP IHR L/LATCH",{"$f":"_xlfn.XLOOKUP(C1347,DataSource!A:A,DataSource!AH:AH)","v":"0753 1 in BSP 1.5 in BSP PG"}]
[null,null,"04890530","PLAIN DELUGE TIP 2.5AFD 1 3/8D POLISH",{"$f":"_xlfn.XLOOKUP(C1348,DataSource!A:A,DataSource!AH:AH)","v":"0489 2.5 in QST 1-3/8\" bore size(s) "}]
[null,null,"04890607","PLAIN DELUGE TIP 2.5AFD 1 3/4DSCH POLISH",{"$f":"_xlfn.XLOOKUP(C1349,DataSource!A:A,DataSource!AH:AH)","v":"0489 2.5 in QST 1-3/4\" bore size(s) "}]
[null,null,"04890528","PLAIN DELUGE TIP 2.5AEF 2\"DSCH POLISH",{"$f":"_xlfn.XLOOKUP(C1350,DataSource!A:A,DataSource!AH:AH)","v":"0489 2.5 in NYCORP 2\" bore size(s) "}]
[null,null,"04890527","PLAIN DELUGE TIP 2.5AEF 1 3/4DSCH POLISH",{"$f":"_xlfn.XLOOKUP(C1351,DataSource!A:A,DataSource!AH:AH)","v":"0489 2.5 in NYCORP 1-3/4\" bore size(s) "}]
[null,null,"04890505","PLAIN DELUGE TIP 2.5NH 2 1/4D POLISH",{"$f":"_xlfn.XLOOKUP(C1352,DataSource!A:A,DataSource!AH:AH)","v":"0489 2.5 in NH 2-1/4\" bore size(s) "}]
[null,null,"04890638","PLAIN DELUGE TIP 2.5NH 2\"D DCFD",{"$f":"_xlfn.XLOOKUP(C1353,DataSource!A:A,DataSource!AH:AH)","v":"0489 2.5 in NH 2\" bore size(s) ETCH"}]
[null,null,"04890133","PLAIN DELUGE TIP 2.5\"NH W/2 DSCH CF/NC",{"$f":"_xlfn.XLOOKUP(C1354,DataSource!A:A,DataSource!AH:AH)","v":"0489 2.5 in NH 2\" bore size(s) "}]
[null,null,"04890504","PLAIN DELUGE TIP 2.5NH 2DSCH POLISH",{"$f":"_xlfn.XLOOKUP(C1355,DataSource!A:A,DataSource!AH:AH)","v":"0489 2.5 in NH 2\" bore size(s) "}]
[null,null,"04890634","PLAIN DELUGE TIP 2.5 NH 15/16DSCH POLISH",{"$f":"_xlfn.XLOOKUP(C1356,DataSource!A:A,DataSource!AH:AH)","v":"0489 2.5 in NH 15/16\" bore size(s) "}]
[null,null,"04890501","PLAIN DELUGE TIP 2.5NH 1 3/8D POLISH",{"$f":"_xlfn.XLOOKUP(C1357,DataSource!A:A,DataSource!AH:AH)","v":"0489 2.5 in NH 1-3/8\" bore size(s) "}]
[null,null,"04890637","PLAIN DELUGE TIP 2.5NH 1.75D DCFD",{"$f":"_xlfn.XLOOKUP(C1358,DataSource!A:A,DataSource!AH:AH)","v":"0489 2.5 in NH 1-3/4\" bore size(s) ETCH"}]
[null,null,"04890132","PLAIN DELUGE TIP 2.5\"NH, 1 3/4D CF/NC",{"$f":"_xlfn.XLOOKUP(C1359,DataSource!A:A,DataSource!AH:AH)","v":"0489 2.5 in NH 1-3/4\" bore size(s) "}]
[null,null,"04890503","PLAIN DELUGE TIP 2.5NH 1 3/4D POL ALUM",{"$f":"_xlfn.XLOOKUP(C1360,DataSource!A:A,DataSource!AH:AH)","v":"0489 2.5 in NH 1-3/4\" bore size(s) "}]
[null,null,"04890506","PLAIN DELUGE TIP 2.5NH 1 1/8D POLISH",{"$f":"_xlfn.XLOOKUP(C1361,DataSource!A:A,DataSource!AH:AH)","v":"0489 2.5 in NH 1-1/8\" bore size(s) "}]
[null,null,"04890502","PLAIN DELUGE TIP 2.5NH 1 1/4DSCH POLISH",{"$f":"_xlfn.XLOOKUP(C1362,DataSource!A:A,DataSource!AH:AH)","v":"0489 2.5 in NH 1-1/4\" bore size(s) "}]
[null,null,"04890500","PLAIN DELUGE TIP 2.5NH 1 1/2D POLISH#",{"$f":"_xlfn.XLOOKUP(C1363,DataSource!A:A,DataSource!AH:AH)","v":"0489 2.5 in NH 1-1/2\" bore size(s) "}]
[null,null,"04890511","PLAIN DELUGE TIP 2.5AFB 1 3/4DFDNYPOLISH",{"$f":"_xlfn.XLOOKUP(C1364,DataSource!A:A,DataSource!AH:AH)","v":"0489 2.5 in FDNY 1-3/4\" bore size(s) "}]
[null,null,"04890509","PLAIN DELUGE TIP 2.5AII 2 1/4D POLISH",{"$f":"_xlfn.XLOOKUP(C1365,DataSource!A:A,DataSource!AH:AH)","v":"0489 2.5 in CSA 2-1/4\" bore size(s) "}]
[null,null,"04890544","PLAIN DELUGE TIP 2.5AII 2\"DSCH POLISH",{"$f":"_xlfn.XLOOKUP(C1366,DataSource!A:A,DataSource!AH:AH)","v":"0489 2.5 in CSA 2\" bore size(s) "}]
[null,null,"04890598","PLAIN DELUGE TIP 2.5BAF 1 3/8D POLISH",{"$f":"_xlfn.XLOOKUP(C1367,DataSource!A:A,DataSource!AH:AH)","v":"0489 2.5 in BAT 1-3/8\" bore size(s) "}]
[null,null,"04890540","PLAIN DELUGE TIP 2.5AKB 1 1/2DSCH POLISH",{"$f":"_xlfn.XLOOKUP(C1368,DataSource!A:A,DataSource!AH:AH)","v":"0489 2.5 in AKB 1-1/2\" bore size(s) "}]
[null,null,"04890641","PLAIN DELUGE 5IP 2.5AEA1 3/8D POLISH",{"$f":"_xlfn.XLOOKUP(C1369,DataSource!A:A,DataSource!AH:AH)","v":"0489 2.5 in AEA 1-3/8\" bore size(s) "}]
[null,null,"04394010","TIP DUAL STK 1.5ABQ 15/16 &1/2D",{"$f":"_xlfn.XLOOKUP(C1370,DataSource!A:A,DataSource!AH:AH)","v":"0439 1.5 in NYCORP 1 in NH 15/16\"; 1/2\" bore size(s) "}]
[null,null,"04394008","TIP DUAL STK 1.5NPSH 15/16&1/2D",{"$f":"_xlfn.XLOOKUP(C1371,DataSource!A:A,DataSource!AH:AH)","v":"0439 1.5 in NPSH 1 in NH 15/16\"; 1/2\" bore size(s) "}]
[null,null,"04394004","TIP DUAL STK 1.5NPSH 1-1/8&1/2D",{"$f":"_xlfn.XLOOKUP(C1372,DataSource!A:A,DataSource!AH:AH)","v":"0439 1.5 in NPSH 1 in NH 1-1/8\"; 1/2\" bore size(s) "}]
[null,null,"04394005","TIP DUAL STK 1.5NH 15/16&1/2D#",{"$f":"_xlfn.XLOOKUP(C1373,DataSource!A:A,DataSource!AH:AH)","v":"0439 1.5 in NH 1 in NH 15/16\"; 1/2\" bore size(s) "}]
[null,null,"04394009","TIP DUAL STK 1.5NH 1-1/8&1/2D UNIONVILLE",{"$f":"_xlfn.XLOOKUP(C1374,DataSource!A:A,DataSource!AH:AH)","v":"0439 1.5 in NH 1 in NH 1-1/8\"; 1/2\" bore size(s) ETCH"}]
[null,null,"04394002","TIP DUAL STK 1.5NH 1-1/8&1/2D#",{"$f":"_xlfn.XLOOKUP(C1375,DataSource!A:A,DataSource!AH:AH)","v":"0439 1.5 in NH 1 in NH 1-1/8\"; 1/2\" bore size(s) "}]
[null,null,"04394006","TIP DUAL STK 1.5NH 1-1/16&15/16D",{"$f":"_xlfn.XLOOKUP(C1376,DataSource!A:A,DataSource!AH:AH)","v":"0439 1.5 in NH 1 in NH 1-1/16\"; 15/16\" bore size(s) "}]
[null,null,"04394001","TIP DUAL STK 1.5ABU FDNY 1/2&15/16D",{"$f":"_xlfn.XLOOKUP(C1377,DataSource!A:A,DataSource!AH:AH)","v":"0439 1.5 in FDNY 1 in NH 15/16\"; 1/2\" bore size(s) "}]
[null,null,"04394003","TIP DUAL STK 1.5ABU FDNY 1-1/8&1/2D",{"$f":"_xlfn.XLOOKUP(C1378,DataSource!A:A,DataSource!AH:AH)","v":"0439 1.5 in FDNY 1 in NH 1-1/8\"; 1/2\" bore size(s) "}]
[null,null,"04164005","TIP 1.5NSPH X 1.5NPSH 7/8D",{"$f":"_xlfn.XLOOKUP(C1379,DataSource!A:A,DataSource!AH:AH)","v":"0416 1.5 in NPSH 1.5 in NPSH 7/8\" bore size(s) "}]
[null,null,"04164008","TIP 1.5NPSH X 1.5NPSH 1-1/8D",{"$f":"_xlfn.XLOOKUP(C1380,DataSource!A:A,DataSource!AH:AH)","v":"0416 1.5 in NPSH 1.5 in NPSH 1-1/8\" bore size(s) "}]
[null,null,"04164010","TIP 1.5NPSH X 1.5NPSH 1D",{"$f":"_xlfn.XLOOKUP(C1381,DataSource!A:A,DataSource!AH:AH)","v":"0416 1.5 in NPSH 1.5 in NPSH 1\" bore size(s) "}]
[null,null,"04164004","TIP 1.5NH X 1.5NH 7/8D",{"$f":"_xlfn.XLOOKUP(C1382,DataSource!A:A,DataSource!AH:AH)","v":"0416 1.5 in NH 1.5 in NH 7/8\" bore size(s) "}]
[null,null,"04164003","TIP 1.5NH X 1.5NH 3/4D",{"$f":"_xlfn.XLOOKUP(C1383,DataSource!A:A,DataSource!AH:AH)","v":"0416 1.5 in NH 1.5 in NH 3/4\" bore size(s) "}]
[null,null,"04164002","TIP 1.5NH X 1.5NH 1-1/8D",{"$f":"_xlfn.XLOOKUP(C1384,DataSource!A:A,DataSource!AH:AH)","v":"0416 1.5 in NH 1.5 in NH 1-1/8\" bore size(s) "}]
[null,null,"04164001","TIP 1.5NH X 1.5NH 1-1/4D",{"$f":"_xlfn.XLOOKUP(C1385,DataSource!A:A,DataSource!AH:AH)","v":"0416 1.5 in NH 1.5 in NH 1-1/4\" bore size(s) "}]
[null,null,"04164006","TIP 1.5NH X 1.5NH 1D",{"$f":"_xlfn.XLOOKUP(C1386,DataSource!A:A,DataSource!AH:AH)","v":"0416 1.5 in NH 1.5 in NH 1\" bore size(s) "}]
[null,null,"04164009","TIP 1.5NH X 1.5ABE 1-1/4D",{"$f":"_xlfn.XLOOKUP(C1387,DataSource!A:A,DataSource!AH:AH)","v":"0416 1.5 in NH 1.5 in ABE 1-1/4\" bore size(s) "}]
[null,null,"04164012","TIP 1.5BSP X 1.5BSP 1D",{"$f":"_xlfn.XLOOKUP(C1388,DataSource!A:A,DataSource!AH:AH)","v":"0416 1.5 in BSP 1.5 in BSP 1\" bore size(s) "}]
[null,null,"04164011","TIP 1.5ABE X 1.5NH 1-1/4D",{"$f":"_xlfn.XLOOKUP(C1389,DataSource!A:A,DataSource!AH:AH)","v":"0416 1.5 in ABE 1.5 in NH 1-1/4\" bore size(s) "}]
[null,null,"04160036","TIP 1.5 ABE X 1.5 ABE 1 1/4 DSCH PY",{"$f":"_xlfn.XLOOKUP(C1390,DataSource!A:A,DataSource!AH:AH)","v":"0416 1.5 in ABE 1.5 in ABE 1-1/4\" bore size(s) "}]
[null,null,"04164007","TIP 1.5ABE X 1.5ABE 1-1/4D",{"$f":"_xlfn.XLOOKUP(C1391,DataSource!A:A,DataSource!AH:AH)","v":"0416 1.5 in ABE 1.5 in ABE 1-1/4\" bore size(s) "}]